### VMAX

displays the system velocity maximum for a drive and motor combination. This variable is based on drive and motor hardware parameters and is set equal to the MINIMUM of the five following values:

1.) MSPEED
2.) (VBUS * 0.707 / MBEMF) * 1000
3.) 24,000
4.) 180,000,000 / MENCRES (encoder-feedback systems only)
5.) 192,000 / MRESPOLES (resolver system, MRESPOLES>8)

Note that 24,000 is the highest value VMAX can take. VMAX is used to limit VLIM and VOSPD.

Firmware Versions: all
Type: variable (R) Range: 10 to 24,000
Units: rotary: RPM
linear: mm/sec
Default: 10
Opmodes: 0,1,4,8 Drive Status: dis EEPROM: yes