### UVMODE

defines how the drive will respond to an under-voltage (UV) fault:
0 = latch fault immediately, display flashing "u".
1 = display steady "u". Warning only, with no fault latch.
2 = display steady "u" - after UVTIME elapses, latch fault relay.
3 = fault only if UV exsists + drive is enabled

If UVMODE= 1 or 2, and the drive is disabled, the UV fault is ignored.
Firmware Versions: 3.1.0
Type: switch mode (R/W) Range: 0 - 3
Units: n/a Default: 0
Opmodes: all Drive Status: en/dis EEPROM: yes