### VOSPDSENS

sets over speed condition detection sensitivity.
If an over-speed condition is detected it is not latched as fault immediatly but only after VOSPDSENS number of the background cycles are completed. This feature controls the sensitivity of detection of the over-speed fault.

Firmware Versions: 4.1.8
Type: variable (R/W) Range: 1 to 40
Units: n/a Default: 20
Opmodes: all Drive Status: en/dis EEPROM: yes