### ECHO

enables/disables serial port character echo. If echo is enabled, characters received via the serial port are echoed back to the serial port and displayed on the MotionLink monitor or terminal.
0 = serial port echo disabled
1 = serial port echo enabled
Note that ECHO = 1 is needed for proper operation of MotionLink.

Firmware Versions: all
Type: switch (R/W) Range: 0, 1
Units: n/a Default: 1
Opmodes: all Drive Status: en/dis EEPROM: yes