### REMOTE

indicates the state of the external hardware enable input line. When REMOTE is set to 1, the software is ready (READY = 1), and Dip Switch 8 is set to OFF (DIPEN = 1), the drive is Enabled (ACTIVE = 1).
0 = remote enable input off
1 = remote enable input on

Firmware Versions: all
Type: switch (R) Range: 0, 1
Units: n/a Default: hardware defined
Opmodes: all Drive Status: en/dis EEPROM: no