{"text_format":"1","workbook":"xlsx","n_sheets":10,"sheets":["Main","Inertia","Drives","Motor","LinMotor","Hilfe","Help","Changes","Calc","Graphic"],"not_rendered":{"charts":5,"images":68,"macros":1,"external_links":0,"defined_names":202,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Main","index":0,"n_rows":197,"n_cols":22,"rows_kept":197,"cut":false,"hidden":false,"merged":[[4,20,7,20],[13,12,13,13],[9,7,9,10],[10,7,10,10],[22,16,23,17],[21,14,21,15],[21,8,21,9],[20,8,20,9],[58,7,59,7],[1,12,5,17],[8,1,8,10],[8,14,8,16],[19,11,19,17],[58,6,59,6],[58,8,59,8],[56,7,57,7],[56,8,57,8],[58,1,59,1],[58,2,59,2],[54,1,55,1],[56,1,57,1],[56,2,57,2],[54,2,55,2],[51,1,52,1],[60,6,61,6],[60,8,61,8],[22,13,23,13],[22,12,23,12],[24,10,25,10],[51,8,52,8],[26,8,27,8],[26,11,27,15],[26,9,27,9],[49,8,50,8],[26,10,27,10],[45,8,46,8],[54,7,55,7],[54,8,55,8],[47,8,48,8],[75,8,76,8],[75,6,76,7],[82,1,83,1],[82,2,83,2],[73,8,74,8],[75,3,76,3],[73,1,74,1],[73,2,74,2],[75,1,76,1],[90,0,92,0],[70,4,70,5],[68,4,69,5],[77,1,78,1],[77,2,78,2],[77,3,78,3],[80,1,81,1],[80,2,81,2],[80,3,81,3],[80,4,81,5],[71,4,72,5],[93,1,94,1],[91,10,92,10],[90,10,90,16],[77,4,78,5],[77,6,78,7],[77,8,78,8],[82,3,83,3],[82,4,83,5],[84,1,85,1],[84,2,85,2],[84,6,85,7],[84,8,85,8],[86,6,87,7],[86,8,87,8],[86,1,87,1],[86,2,87,2],[86,3,87,3],[86,4,87,5],[84,3,85,3],[84,4,85,5],[82,6,83,7],[82,8,83,8],[80,6,81,7],[80,8,81,8],[49,2,50,2],[51,2,52,2],[58,3,59,3],[58,4,59,4],[56,3,57,3],[56,4,57,4],[51,3,52,3],[54,4,55,4],[51,5,52,5],[49,3,50,3],[58,5,59,5],[56,5,57,5],[54,3,55,3],[54,5,55,5],[91,11,92,11],[91,5,92,5],[91,1,92,1],[91,2,92,2],[91,3,92,3],[91,4,92,4],[73,6,74,7],[73,3,74,3],[51,4,52,4],[75,2,76,2],[70,6,70,7],[68,8,69,8],[65,1,66,2],[75,4,76,5],[73,4,74,5],[71,1,72,1],[71,2,72,2],[65,3,66,3],[60,1,61,1],[60,2,61,2],[64,1,64,2],[60,3,61,3],[71,3,72,3],[71,8,72,8],[0,0,0,18],[9,2,9,3],[9,5,9,6],[29,1,29,2],[28,1,28,2],[22,3,23,3],[24,3,25,3],[20,16,20,17],[21,16,21,17],[22,14,23,15],[10,2,10,3],[20,4,20,5],[22,4,23,5],[26,6,27,6],[20,14,20,15],[20,6,20,7],[24,12,25,12],[24,11,25,11],[24,8,25,9],[22,6,23,7],[22,11,23,11],[22,8,23,9],[21,6,21,7],[1,1,5,11],[39,3,40,3],[24,4,25,5],[47,6,48,6],[45,6,46,6],[45,2,46,2],[26,4,27,5],[45,3,46,3],[49,7,50,7],[45,7,46,7],[47,7,48,7],[39,1,40,2],[45,1,46,1],[43,6,43,7],[47,1,48,1],[47,2,48,2],[47,3,48,3],[49,5,50,5],[47,4,48,4],[42,6,42,7],[42,4,42,5],[49,6,50,6],[47,5,48,5],[45,4,46,4],[49,1,50,1],[99,17,99,18],[100,17,100,18],[101,17,101,18],[102,17,102,18],[98,17,98,18],[10,5,10,6],[21,4,21,5],[31,4,31,7],[24,6,25,7],[19,4,19,9],[96,17,96,18],[97,17,97,18],[51,7,52,7],[51,6,52,6],[49,4,50,4],[43,4,43,5],[45,5,46,5],[60,7,61,7],[54,6,55,6],[56,6,57,6],[68,6,69,7],[60,5,61,5],[60,4,61,4],[71,6,72,7],[107,17,107,18],[108,17,108,18],[109,17,109,18],[110,17,110,18],[103,17,103,18],[104,17,104,18],[105,17,105,18],[106,17,106,18],[115,17,115,18],[116,17,116,18],[117,17,117,18],[118,17,118,18],[111,17,111,18],[112,17,112,18],[113,17,113,18],[114,17,114,18],[123,17,123,18],[124,17,124,18],[125,17,125,18],[126,17,126,18],[119,17,119,18],[120,17,120,18],[121,17,121,18],[122,17,122,18],[131,17,131,18],[132,17,132,18],[133,17,133,18],[134,17,134,18],[127,17,127,18],[128,17,128,18],[129,17,129,18],[130,17,130,18],[139,17,139,18],[140,17,140,18],[141,17,141,18],[142,17,142,18],[135,17,135,18],[136,17,136,18],[137,17,137,18],[138,17,138,18],[147,17,147,18],[148,17,148,18],[149,17,149,18],[150,17,150,18],[143,17,143,18],[144,17,144,18],[145,17,145,18],[146,17,146,18],[155,17,155,18],[174,17,174,18],[167,17,167,18],[168,17,168,18],[169,17,169,18],[170,17,170,18],[156,17,156,18],[157,17,157,18],[158,17,158,18],[151,17,151,18],[152,17,152,18],[153,17,153,18],[154,17,154,18],[163,17,163,18],[164,17,164,18],[165,17,165,18],[166,17,166,18],[159,17,159,18],[160,17,160,18],[161,17,161,18],[162,17,162,18],[171,17,171,18],[172,17,172,18],[173,17,173,18],[185,17,185,18],[186,17,186,18],[190,17,190,18],[183,17,183,18],[184,17,184,18],[175,17,175,18],[176,17,176,18],[196,17,196,18],[191,17,191,18],[192,17,192,18],[193,17,193,18],[194,17,194,18],[195,17,195,18],[187,17,187,18],[188,17,188,18],[189,17,189,18],[181,17,181,18],[182,17,182,18],[177,17,177,18],[178,17,178,18],[179,17,179,18],[180,17,180,18]]}
[]
[]
[{"$f":"MID(MID(CELL(\"Dateiname\"),FIND(\"[\",CELL(\"Dateiname\"))+1,FIND(\"]\",CELL(\"Dateiname\"))-FIND(\"[\",CELL(\"Dateiname\"))-1),1,(LEN(MID(CELL(\"Dateiname\"),FIND(\"[\",CELL(\"Dateiname\"))+1,FIND(\"]\",CELL(\"Dateiname\"))-FIND(\"[\",CELL(\"Dateiname\"))-1)))-(IF((MID(RIGHT(MID(CELL(\"Dateiname\"),FIND(\"[\",CELL(\"Dateiname\"))+1,FIND(\"]\",CELL(\"Dateiname\"))-FIND(\"[\",CELL(\"Dateiname\"))-1),5),1,1))=\".\",5,4)))","v":"AnyDim_V2.35"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Änderungshistorie"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ver 1.7 nach 1.8           26.06.2004 Hinzufügen von ca. 300 Linearmotoren ver. Baureihen H. Goergen"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ver 2.0 nach 2.1    14.11.07  H Krug","Berechnung erweitert dass 10 Fremdlinearmotoren   berechnet werden können in Reiter \"LinMotor\".  "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Reiter \"LinMotor\": Bei den L1S  25..75  Polpitch auf 48mm gesetzt  bei L1S 80..200  Polpitch auf 66mm. Gesetzt"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Im Reiter \"Main\"  bei Linmot auswahl  in Spalte \"R\"  Fehler im Induktivitätsscheck   L>Lmax und Umot> Umot  auf  Wert \"5\" in Berechnungsvorschrift  geändert "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Alle Platinum IC Linearmotoren auf UDC max = 330Vdc geändert "]
[null,{"$f":"IF(deutsch,\"Allgemeines\",\"General\")","v":"Allgemeines"},null,null,null,null,null,null,null,null,null,null,null,null,"Sprache/Language"]
[null,{"$f":"IF(deutsch,\"Bearbeiter:\",\"Author:\")","v":"Bearbeiter:"},null,null,"                                                                                                                                                                                                                                                                                                                              ","Kunde:"]
[null,{"$f":"IF(deutsch,\"Datum:\",\"Date:\")","v":"Datum:"},null,null,null,"Anwendung:"]
[]
[]
[null,{"$f":"IF(deutsch,\"Motorart\",\"Motor type\")","v":"Motorart"},{"$f":"D91","v":""},"                ","Drive",null,"Uac max =",{"$f":"Drives!B2","v":480},{"$f":"IF(Drives!G2=\"\",\"\",\"P br int =\")","v":"P br int ="},{"$f":"IF(Drives!G2=\"\",\"\",Drives!G2)","v":200},null,{"$f":"IF(deutsch,\"AC-Spg. [V]\",\"AC-Voltage [V]\")","v":"AC-Spg. [V]"},{"$f":"MIN(ROUND((UAC_V*SQRT(2)-5)/10,0)*10,640)","v":560},null,{"$f":"IF(deutsch,\"Eingabeänderung\",\"Input changes\")","v":"Eingabeänderung"}]
[null,null,null,null,null,null,"I cont =",{"$f":"Drives!C2","v":24},{"$f":"IF(Drives!E2=\"\",\"\",\"L min =\")","v":"L min ="},{"$f":"IF(Drives!E2=\"\",\"\",Drives!E2/H14*UAC_V)","v":1.4166666666666665}]
[null,null,null,null,null,null,"I peak =",{"$f":"Drives!D2","v":48},{"$f":"IF(Drives!F2=\"\",\"\",\"L max =\")","v":"L max ="},{"$f":"IF(Drives!F2=\"\",\"\",Drives!F2/H14*UAC_V)","v":13.333333333333334}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF((Calc!B2-Drives!B2)>0,\"       AC Spannung inkonsistent\",\"\")","v":""}]
[null,{"$f":"IF(deutsch,\"Motorlinien\",\"Motor lines\")","v":"Motorlinien"}]
[]
[null,null,null,null,{"$f":"IF(deutsch,\"Mechanische Daten (Abtrieb)\",\"Mech. data (gear output side)\")","v":"Mechanische Daten (Abtrieb)"},null,null,null,null,null,null,{"$f":"IF(deutsch,\"Getriebe\",\"Gear\")","v":"Getriebe"}]
[null,null,null,null,{"$f":"IF(deutsch,\"Massenträgheit\",\"Inertia\")","v":"Massenträgheit"},null,{"$f":"IF(deutsch,\"Lastmoment\",\"Load\")","v":"Lastmoment"},null,{"$f":"IF(deutsch,\"Tr.-Reibung\",\"Dry friction\")","v":"Tr.-Reibung"},null,null,{"$f":"IF(deutsch,\"Faktor\",\"Ratio\")","v":"Faktor"},{"$f":"IF(deutsch,\"Trägheit\",\"Inertia\")","v":"Trägheit"},{"$f":"IF(deutsch,\"Wirkungsgr.\",\"Efficiency\")","v":"Wirkungsgr."},{"$f":"IF(deutsch,\"Eingangsdrehzahl\",\"Input speed\")","v":"Eingangsdrehzahl"},null,{"$f":"IF(deutsch,\"Mittl. Drehz.\",\"Avg.-Speed\")","v":"Mittl. Drehz."}]
[null,null,null,null,"[10-3kgm2]",null,"[Nm]",null,"[Nm]",null,null,"i","[10-3kgm2]","h","[1/min]",null,"[1/min]"]
[null,null,null,{"$f":"IF(Calc!A31,\"\",\"1.\")","v":""},112.5,null,7.5,null,1.5,null,null,1,0,1,{"$f":"IF(move1,gear*MAX(ABS(speed1),ABS(speed2)),gear*MAX(ABS(speed1),ABS(speed2),ABS(speed6)))","v":127.32395447351627},null,{"$f":"IF(move1,(((ABS(speed2+speed1)/2*time1+ABS(speed2)*time2+ABS(speed2+speed1)/2*time3+speed1*time4)/time))*gear,(((ABS(speed2+speed1)/2*time1+ABS(speed2)*time2+ABS(speed2+speed1)/2*time3+speed1*time4+ABS(speed6+speed1)/2*time5+ABS(speed6)*time6+ABS(speed6+speed1)/2*time7+speed1*time8)/time))*gear)","v":22.185980958664175}]
[]
[null,null,null,{"$f":"IF(Calc!A31,\"\",\"2.\")","v":""},112.5,null,7.5,null,1.5]
[]
[null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(L23>0,\"\",IF(deutsch,\"Fehler: Getriebefaktor <= 0\",\"Error: Gear ratio <= 0\"))","v":""}]
[]
[]
[]
[]
[null,null,null,null,{"$f":"IF(deutsch,\"Mechanische Daten\",\"Mechanical data\")","v":"Mechanische Daten"}]
[null,null,null,null,{"$f":"IF(deutsch,\"Gewicht\",\"Weight\")","v":"Gewicht"},{"$f":"IF(deutsch,\"Last\",\"Load\")","v":"Last"},{"$f":"IF(deutsch,\"Tr.Reibung\",\"Dry Fric.\")","v":"Tr.Reibung"},{"$f":"IF(deutsch,\"Wirkungsgr\",\"Efficiency\")","v":"Wirkungsgr"}]
[null,null,null,null,"[kg]","[N]","[N]","h"]
[null,null,null,{"$f":"IF(Calc!A31,\"\",\"1.\")","v":""},5,0,0,1]
[null,null,null,{"$f":"IF(Calc!A31,\"\",\"2.\")","v":""},5,0,0]
[]
[]
[null,{"$f":"IF(deutsch,\"Bewegungsprofil\",\"Motion profile\")","v":"Bewegungsprofil"}]
[null,{"$f":"IF(deutsch,\"Einheiten / Umdrehung\",\"Units / turn\")","v":"Einheiten / Umdrehung"},null,{"$f":"Inertia!H9 * PI()","v":942.47779607693792}]
[]
[]
[null,null,null,{"$f":"IF(deutsch,\"Bewegungszeit\",\"Cylce time\")","v":"Bewegungszeit"},{"$f":"IF(deutsch,\"Geschwindigkeit\",\"Speed\")","v":"Geschwindigkeit"},null,{"$f":"IF(deutsch,\"Beschleunigung\",\"Acceleration\")","v":"Beschleunigung"},null,"Position",null,null,null,null,null,null,null,"M0 [Nm]",{"$f":"Calc!A108","v":42}]
[null,null,null,"t [ms]",{"$f":"IF(deutsch,\"Abtrieb\",\"Gear output side\")","v":"Abtrieb"},null,{"$f":"IF(deutsch,\"Abtrieb\",\"Gear output side\")","v":"Abtrieb"},null,{"$f":"IF(deutsch,\"Abtrieb\",\"Gear outp.\")","v":"Abtrieb"},null,null,null,null,null,null,null,"I0 [A]",{"$f":"Calc!A109","v":13.6}]
[null,null,null,{"$f":"IF(Calc!A31,time1+time2+time3+time4,time1+time2+time3+time4+time5+time6+time7+time8)","v":2481},{"$f":"IF(deutsch,\"[Einheiten/s]\",\"[Units/s]\")","v":"[Einheiten/s]"},"[1/min]",{"$f":"IF(deutsch,\"[Einheiten/s2]\",\"[Units/s2]\")","v":"[Einheiten/s2]"},"[rad/s2]",{"$f":"IF(deutsch,\"[Einheiten]\",\"[Units]\")","v":"[Einheiten]"},null,null,null,null,null,null,null,"Mn [Nm]",{"$f":"Calc!A110","v":33.799999999999997}]
[null,{"$f":"IF(deutsch,\"Beschleunigung\",\"Acceleration\")","v":"Beschleunigung"},"t1 [ ms ]",81,2000,{"$f":"E46/$D$40*60","v":127.32395447351627},{"$f":"(E48-E46)/D46*Calc!B30*1000","v":-38009.481481481482},{"$f":"G46/ULU*2*PI()","v":-253.39654320987654},{"$f":"E46*D46/1000+((E48+E46)/2-E46)*D46/1000","v":82.62},null,null,null,null,null,null,null,"In [A]",{"$f":"Calc!A111","v":10.903225806451612}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nn [min-1]",{"$f":"Calc!A112","v":1500}]
[null,{"$f":"IF(deutsch,\"Geschwindigkeit\",\"Speed\")","v":"Geschwindigkeit"},"t2 [ ms ]",2000,40,{"$f":"E48/$D$40*60","v":2.5464790894703255},0,0,{"$f":"I46+E48*D48/1000","v":162.62},null,null,null,null,null,null,null,"Mmax[Nm]",{"$f":"Calc!A113","v":112}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nmax[min-1]",{"$f":"Calc!A114","v":6000}]
[null,{"$f":"IF(deutsch,\"Verzögerung\",\"Deceleration\")","v":"Verzögerung"},"t3 [ ms ]",100,{"$f":"E46","v":2000},{"$f":"E50/$D$40*60","v":127.32395447351627},{"$f":"(E50-E48)/D50*Calc!B30*1000","v":30787.68},{"$f":"G50/ULU*2*PI()","v":205.25120000000001},{"$f":"I48+((E50+E48)/2-E48)*D50/1000+E48*D50/1000","v":264.62},null,null,null,null,null,null,null,"RU-V [W]",{"$f":"Calc!A115","v":0.68}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LU-V [mH]",{"$f":"Calc!A116","v":12.4}]
[null,"Pause","t4 [ ms ]",300,{"$f":"E46","v":2000},{"$f":"E52/$D$40*60","v":127.32395447351627},0,0,{"$f":"I50+E52*D52/1000","v":864.62},null,null,null,null,null,null,null,"KE [V/103]",{"$f":"Calc!A117","v":200}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Calc!A71,\"J [kgcm2]\",\"J[10-3kgm2\")","v":"J[10-3kgm2"},{"$f":"IF(Calc!A71,10*Calc!A107,Calc!A107)","v":9.1999999999999993}]
[null,{"$f":"IF(deutsch,IF(move1,\"\",\"2. Fahrsatz\"),IF(move1,\"\",\"2. Motion task\"))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UDCmax [V]",{"$f":"Calc!A118","v":640}]
[null,{"$f":"IF(deutsch,\"Beschleunigung\",\"Acceleration\")","v":"Beschleunigung"},"t5 [ ms ]",1,{"$f":"E46","v":2000},{"$f":"E55/$D$40*60","v":127.32395447351627},{"$f":"(E57-E55)/D55*AccType*1000","v":-3141600},{"$f":"G55/ULU*2*PI()","v":-20944},{"$f":"I52+E55*D55/1000+((E57+E55)/2-E55)*D55/1000","v":865.62}]
[]
[null,{"$f":"IF(deutsch,\"Geschwindigkeit\",\"Speed\")","v":"Geschwindigkeit"},"t6 [ ms ]",0,0,{"$f":"E57/$D$40*60","v":0},0,0,{"$f":"I55+E57*D57/1000","v":865.62}]
[]
[null,{"$f":"IF(deutsch,\"Verzögerung\",\"Deceleration\")","v":"Verzögerung"},"t7 [ ms ]",1,{"$f":"E55","v":2000},{"$f":"E59/$D$40*60","v":127.32395447351627},{"$f":"(E59-E57)/D59*AccType*1000","v":3141600},{"$f":"G59/ULU*2*PI()","v":20944},{"$f":"I57+((E59+E57)/2-E57)*D59/1000+E57*D59/1000","v":866.62}]
[]
[null,"Pause","t8 [ ms ]",0,{"$f":"E55","v":2000},{"$f":"E61/$D$40*60","v":127.32395447351627},0,0,{"$f":"I59+E61*D61/1000","v":866.62}]
[]
[]
[]
[null,{"$f":"IF(deutsch,\"Bewegungsprofil\",\"Motion profile\")","v":"Bewegungsprofil"}]
[]
[]
[]
[null,null,null,{"$f":"IF(deutsch,\"Bewegungszeit\",\"Cycle time\")","v":"Bewegungszeit"},{"$f":"IF(deutsch,\"Geschwindigkeit\",\"Speed\")","v":"Geschwindigkeit"},null,{"$f":"IF(deutsch,\"Beschleunigung\",\"Acceleration\")","v":"Beschleunigung"},null,"Position"]
[null,null,null,"t [ms]"]
[null,{"$f":"IF(deutsch,IF(move1,\"\",\"1. Fahrsatz\"),IF(move1,\"\",\"1. Motion task\"))","v":""},null,{"$f":"IF(Calc!A31,Ltime1+Ltime2+Ltime3+Ltime4,Ltime1+Ltime2+Ltime3+Ltime4+Ltime5+Ltime6+Ltime7+Ltime8)","v":130},"[m/s]",null,"[m/s2]",null,"[mm]",null,null,null,null,null,null,null,"Fn [N]",{"$f":"Calc!A108","v":42}]
[null,{"$f":"IF(deutsch,\"Beschleunigung\",\"Acceleration\")","v":"Beschleunigung"},"t1 [ ms ]",50,0,null,{"$f":"(E74-E72)/D72*AccType*1000","v":31.416},null,{"$f":"E72*D72+((E74+E72)/2-E72)*D72","v":25},null,null,null,null,null,null,null,"In [A]",{"$f":"Calc!A109","v":13.6}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fmax [N]",{"$f":"Calc!A110","v":33.799999999999997}]
[null,{"$f":"IF(deutsch,\"Geschwindigkeit\",\"Const. speed\")","v":"Geschwindigkeit"},"t2 [ ms ]",0,1,null,0,null,{"$f":"I72+E74*D74","v":25},null,null,null,null,null,null,null,"Imax [A]",{"$f":"Calc!A111","v":10.903225806451612}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"vmax [m/s]",{"$f":"Calc!A112","v":1500}]
[null,{"$f":"IF(deutsch,\"Verzögerung\",\"Deceleration\")","v":"Verzögerung"},"t3 [ ms ]",30,{"$f":"Lspeed1","v":0},null,{"$f":"(E76-E74)/D76*AccType*1000","v":-52.36},null,{"$f":"I74+((E76+E74)/2-E74)*D76+E74*D76","v":40},null,null,null,null,null,null,null,"RU-V [W]",{"$f":"Calc!A113","v":112}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LU-V [mH]",{"$f":"Calc!A114","v":6000}]
[null,"Pause","t4 [ ms ]",50,{"$f":"Lspeed1","v":0},null,0,null,{"$f":"I76+E78*D78","v":40},null,null,null,null,null,null,null,"KE [V/m/s]",{"$f":"Calc!A115","v":0.68}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"G [kg]",{"$f":"Calc!A107","v":9.1999999999999993}]
[null,{"$f":"IF(deutsch,IF(move1,\"\",\"2. Fahrsatz\"),IF(move1,\"\",\"2. Motion task\"))","v":""},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"UDCmax [V]",{"$f":"Calc!A117","v":200}]
[null,{"$f":"IF(deutsch,\"Beschleunigung\",\"Acceleration\")","v":"Beschleunigung"},"t5 [ ms ]",1,{"$f":"Lspeed1","v":0},null,{"$f":"(E83-E81)/D81*AccType*1000","v":0},null,{"$f":"I78+E81*D81+((E83+E81)/2-E81)*D81","v":40}]
[]
[null,{"$f":"IF(deutsch,\"Geschwindigkeit\",\"Speed\")","v":"Geschwindigkeit"},"t6 [ ms ]",0,0,null,0,null,{"$f":"I81+E83*D83","v":40}]
[]
[null,{"$f":"IF(deutsch,\"Verzögerung\",\"Deceleration\")","v":"Verzögerung"},"t7 [ ms ]",1,{"$f":"Lspeed1","v":0},null,{"$f":"(E85-E83)/D85*AccType*1000","v":0},null,{"$f":"I83+((E85+E83)/2-E83)*D85+E83*D85","v":40}]
[]
[null,"Pause","t8 [ ms ]",0,{"$f":"Lspeed1","v":0},null,0,null,{"$f":"I85+E87*D87","v":40}]
[]
[]
[]
[{"$f":"IF(deutsch,\"Motorkennlinie\",\"Motor curves\")","v":"Motorkennlinie"},null,null,{"$f":"IF(Calc!A140=0,\"\",Calc!A140)","v":""},{"$f":"IF(Calc!B140=0,\"\",Calc!B140)","v":""},{"$f":"IF(deutsch,\"Motordaten\",\"Motor data\")","v":"Motordaten"},null,null,null,null,{"$f":"IF(deutsch,\"Reglerdaten\",\"Drive data\")","v":"Reglerdaten"}]
[null,{"$f":"IF(deutsch,\"Typ\",\"Type\")","v":"Typ"},"Jext/Jmot","Trms","Tpk","n","T (t1)","T (t2)","T (t3)","T (t4)","Irms","Ipeak","Irms","Ipeak","P","PbrRMS","PbrPEAK"]
[null,null,null,null,null,null,"[Nm]","[Nm]","[Nm]","[Nm]",null,null,"[A]","[A]","[W]","[W]","[W]"]
["t","Filter\n (Maximum)",{"$f":"IF(jjbar<500,jjbar,IF(deutsch,\"alle\",\"all\"))","v":15},{"$f":"IF(mrmsbar<20,mrmsbar/10,IF(deutsch,\"alle\",\"all\"))","v":1},{"$f":"IF(mpkbar<20,mpkbar/10,IF(deutsch,\"alle\",\"all\"))","v":0.8},{"$f":"IF(nbar<20,nbar/10,IF(deutsch,\"alle\",\"all\"))","v":0.6},null,null,null,null,{"$f":"IF(irmsbar<20,irmsbar/10,IF(deutsch,\"alle\",\"all\"))","v":"alle"},{"$f":"IF(ipkbar<20,ipkbar/10,IF(deutsch,\"alle\",\"all\"))","v":"alle"}]
[]
[null,{"$f":"Calc!A70","v":"AKM73M"}]
[122,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A97,1),INDEX(LinMotor!$B$1:$B$1341,A97,1))","v":"AKM73M"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A97,1),INDEX(LinMotor!$R$1:$R$1355,A97,1))","v":12.228260869565219},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A97,1),INDEX(LinMotor!$S$1:$S$1355,A97,1))","v":0.24060955724718877},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A97,1),INDEX(LinMotor!$T$1:$T$1355,A97,1))","v":0.27659884857142858},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A97,1),INDEX(LinMotor!$U$1:$U$1355,A97,1))","v":6.710375985464169E-2},{"$f":"IF(A97<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A97,1),INDEX(LinMotor!$V$1:$V$1355,A97,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A97,1),INDEX(LinMotor!$V$1:$V$1355,A97,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A97,1),INDEX(LinMotor!$V$1:$V$1355,A97,1))/1000,\"0.0k\")),\"\")","v":-24.838359308641976},{"$f":"IF(A97<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A97,1),INDEX(LinMotor!$W$1:$W$1355,A97,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A97,1),INDEX(LinMotor!$X$1:$X$1355,A97,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A97,1),INDEX(LinMotor!$W$1:$W$1355,A97,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A97,1),INDEX(LinMotor!$X$1:$X$1355,A97,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A97,1),INDEX(LinMotor!$W$1:$W$1355,A97,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A97,1),INDEX(LinMotor!$X$1:$X$1355,A97,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A97<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A97,1),INDEX(LinMotor!$X$1:$X$1355,A97,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A97,1),INDEX(LinMotor!$Z$1:$Z$1355,A97,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A97,1),INDEX(LinMotor!$X$1:$X$1355,A97,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A97,1),INDEX(LinMotor!$Z$1:$Z$1355,A97,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A97,1),INDEX(LinMotor!$X$1:$X$1355,A97,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A97,1),INDEX(LinMotor!$Z$1:$Z$1355,A97,1)))/1000,\"0.0k\")),\"\")","v":30.979071040000001},{"$f":"IF(A97<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A97,1),INDEX(LinMotor!$Y$1:$Y$1355,A97,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A97,1),INDEX(LinMotor!$AB$1:$AB$445,A97,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A97,1),INDEX(LinMotor!$Y$1:$Y$1355,A97,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A97,1),INDEX(LinMotor!$AB$1:$AB$445,A97,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A97,1),INDEX(LinMotor!$Y$1:$Y$1355,A97,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A97,1),INDEX(LinMotor!$AB$1:$AB$445,A97,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A97,1),INDEX(LinMotor!$AD$1:$AD$1355,A97,1))","v":0.13595169123777476},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A97,1),INDEX(LinMotor!$AE$1:$AE$1355,A97,1))","v":0.20898579669841269},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A97,1),INDEX(LinMotor!$AF$1:$AF$1355,A97,1))","v":3.262840589706594},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A97,1),INDEX(LinMotor!$AG$1:$AG$1355,A97,1))","v":10.03131824152381},{"$f":"IF(A97<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A97,1),INDEX(LinMotor!$AI$1:$AI$1355,A97,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A97,1),INDEX(LinMotor!$AI$1:$AI$1355,A97,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A97,1),INDEX(LinMotor!$AI$1:$AI$1355,A97,1))/1000,\"0.0k\")),\"\")","v":23.408926749031853},{"$f":"IF(A97<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A97,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A97,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A97,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A97,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A97,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A97,1))/1000,\"0.0k\")),\"\")","v":2.7298553180953018},{"$f":"IF(A97<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A97,1),INDEX(LinMotor!$AK$1:$AK$1355,A97,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A97,1),INDEX(LinMotor!$AK$1:$AK$1355,A97,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A97,1),INDEX(LinMotor!$AK$1:$AK$1355,A97,1))/1000,\"0.0k\")),\"\")","v":167.22891467146775},{"$f":"IF(T97=1,\"L<Lmin\",IF(T97=2,\"Udc>Umot\",IF(T97=3,\"L<Lmin & Udc>Umot\",IF(T97=4,\"L>Lmax\",IF(T97=5,\"L>Lmax & Udc>Umot\",\"\")))))","v":""}]
[123,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A98,1),INDEX(LinMotor!$B$1:$B$1341,A98,1))","v":"AKM73P"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A98,1),INDEX(LinMotor!$R$1:$R$1355,A98,1))","v":12.228260869565219},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A98,1),INDEX(LinMotor!$S$1:$S$1355,A98,1))","v":0.24292879268287892},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A98,1),INDEX(LinMotor!$T$1:$T$1355,A98,1))","v":0.27909073009009011},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A98,1),INDEX(LinMotor!$U$1:$U$1355,A98,1))","v":4.5847258101006025E-2},{"$f":"IF(A98<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A98,1),INDEX(LinMotor!$V$1:$V$1355,A98,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A98,1),INDEX(LinMotor!$V$1:$V$1355,A98,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A98,1),INDEX(LinMotor!$V$1:$V$1355,A98,1))/1000,\"0.0k\")),\"\")","v":-24.838359308641976},{"$f":"IF(A98<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A98,1),INDEX(LinMotor!$W$1:$W$1355,A98,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A98,1),INDEX(LinMotor!$X$1:$X$1355,A98,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A98,1),INDEX(LinMotor!$W$1:$W$1355,A98,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A98,1),INDEX(LinMotor!$X$1:$X$1355,A98,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A98,1),INDEX(LinMotor!$W$1:$W$1355,A98,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A98,1),INDEX(LinMotor!$X$1:$X$1355,A98,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A98<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A98,1),INDEX(LinMotor!$X$1:$X$1355,A98,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A98,1),INDEX(LinMotor!$Z$1:$Z$1355,A98,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A98,1),INDEX(LinMotor!$X$1:$X$1355,A98,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A98,1),INDEX(LinMotor!$Z$1:$Z$1355,A98,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A98,1),INDEX(LinMotor!$X$1:$X$1355,A98,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A98,1),INDEX(LinMotor!$Z$1:$Z$1355,A98,1)))/1000,\"0.0k\")),\"\")","v":30.979071040000001},{"$f":"IF(A98<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A98,1),INDEX(LinMotor!$Y$1:$Y$1355,A98,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A98,1),INDEX(LinMotor!$AB$1:$AB$445,A98,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A98,1),INDEX(LinMotor!$Y$1:$Y$1355,A98,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A98,1),INDEX(LinMotor!$AB$1:$AB$445,A98,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A98,1),INDEX(LinMotor!$Y$1:$Y$1355,A98,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A98,1),INDEX(LinMotor!$AB$1:$AB$445,A98,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A98,1),INDEX(LinMotor!$AD$1:$AD$1355,A98,1))","v":0.19680506773850667},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A98,1),INDEX(LinMotor!$AE$1:$AE$1355,A98,1))","v":0.30252999062500002},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A98,1),INDEX(LinMotor!$AF$1:$AF$1355,A98,1))","v":4.7233216257241599},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A98,1),INDEX(LinMotor!$AG$1:$AG$1355,A98,1))","v":14.52143955},{"$f":"IF(A98<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A98,1),INDEX(LinMotor!$AI$1:$AI$1355,A98,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A98,1),INDEX(LinMotor!$AI$1:$AI$1355,A98,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A98,1),INDEX(LinMotor!$AI$1:$AI$1355,A98,1))/1000,\"0.0k\")),\"\")","v":23.408926749031853},{"$f":"IF(A98<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A98,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A98,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A98,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A98,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A98,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A98,1))/1000,\"0.0k\")),\"\")","v":2.7298553180953018},{"$f":"IF(A98<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A98,1),INDEX(LinMotor!$AK$1:$AK$1355,A98,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A98,1),INDEX(LinMotor!$AK$1:$AK$1355,A98,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A98,1),INDEX(LinMotor!$AK$1:$AK$1355,A98,1))/1000,\"0.0k\")),\"\")","v":167.22891467146775},{"$f":"IF(T98=1,\"L<Lmin\",IF(T98=2,\"Udc>Umot\",IF(T98=3,\"L<Lmin & Udc>Umot\",IF(T98=4,\"L>Lmax\",IF(T98=5,\"L>Lmax & Udc>Umot\",\"\")))))","v":""}]
[124,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A99,1),INDEX(LinMotor!$B$1:$B$1341,A99,1))","v":"AKM73Q"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A99,1),INDEX(LinMotor!$R$1:$R$1355,A99,1))","v":12.228260869565219},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A99,1),INDEX(LinMotor!$S$1:$S$1355,A99,1))","v":0.24351261231621935},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A99,1),INDEX(LinMotor!$T$1:$T$1355,A99,1))","v":0.27909073009009011},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A99,1),INDEX(LinMotor!$U$1:$U$1355,A99,1))","v":3.6521452442360464E-2},{"$f":"IF(A99<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A99,1),INDEX(LinMotor!$V$1:$V$1355,A99,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A99,1),INDEX(LinMotor!$V$1:$V$1355,A99,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A99,1),INDEX(LinMotor!$V$1:$V$1355,A99,1))/1000,\"0.0k\")),\"\")","v":-24.838359308641976},{"$f":"IF(A99<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A99,1),INDEX(LinMotor!$W$1:$W$1355,A99,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A99,1),INDEX(LinMotor!$X$1:$X$1355,A99,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A99,1),INDEX(LinMotor!$W$1:$W$1355,A99,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A99,1),INDEX(LinMotor!$X$1:$X$1355,A99,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A99,1),INDEX(LinMotor!$W$1:$W$1355,A99,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A99,1),INDEX(LinMotor!$X$1:$X$1355,A99,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A99<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A99,1),INDEX(LinMotor!$X$1:$X$1355,A99,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A99,1),INDEX(LinMotor!$Z$1:$Z$1355,A99,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A99,1),INDEX(LinMotor!$X$1:$X$1355,A99,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A99,1),INDEX(LinMotor!$Z$1:$Z$1355,A99,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A99,1),INDEX(LinMotor!$X$1:$X$1355,A99,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A99,1),INDEX(LinMotor!$Z$1:$Z$1355,A99,1)))/1000,\"0.0k\")),\"\")","v":30.979071040000001},{"$f":"IF(A99<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A99,1),INDEX(LinMotor!$Y$1:$Y$1355,A99,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A99,1),INDEX(LinMotor!$AB$1:$AB$445,A99,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A99,1),INDEX(LinMotor!$Y$1:$Y$1355,A99,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A99,1),INDEX(LinMotor!$AB$1:$AB$445,A99,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A99,1),INDEX(LinMotor!$Y$1:$Y$1355,A99,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A99,1),INDEX(LinMotor!$AB$1:$AB$445,A99,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A99,1),INDEX(LinMotor!$AD$1:$AD$1355,A99,1))","v":0.24786373189877783},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A99,1),INDEX(LinMotor!$AE$1:$AE$1355,A99,1))","v":0.381017691004016},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A99,1),INDEX(LinMotor!$AF$1:$AF$1355,A99,1))","v":5.9487295655706678},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A99,1),INDEX(LinMotor!$AG$1:$AG$1355,A99,1))","v":18.288849168192769},{"$f":"IF(A99<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A99,1),INDEX(LinMotor!$AI$1:$AI$1355,A99,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A99,1),INDEX(LinMotor!$AI$1:$AI$1355,A99,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A99,1),INDEX(LinMotor!$AI$1:$AI$1355,A99,1))/1000,\"0.0k\")),\"\")","v":23.408926749031853},{"$f":"IF(A99<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A99,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A99,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A99,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A99,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A99,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A99,1))/1000,\"0.0k\")),\"\")","v":2.7298553180953018},{"$f":"IF(A99<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A99,1),INDEX(LinMotor!$AK$1:$AK$1355,A99,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A99,1),INDEX(LinMotor!$AK$1:$AK$1355,A99,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A99,1),INDEX(LinMotor!$AK$1:$AK$1355,A99,1))/1000,\"0.0k\")),\"\")","v":167.22891467146775},""]
[126,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A100,1),INDEX(LinMotor!$B$1:$B$1341,A100,1))","v":"AKM74P"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A100,1),INDEX(LinMotor!$R$1:$R$1355,A100,1))","v":9.375},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A100,1),INDEX(LinMotor!$S$1:$S$1355,A100,1))","v":0.1935172334780032},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A100,1),INDEX(LinMotor!$T$1:$T$1355,A100,1))","v":0.22220967887323945},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A100,1),INDEX(LinMotor!$U$1:$U$1355,A100,1))","v":6.0636438643938945E-2},{"$f":"IF(A100<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A100,1),INDEX(LinMotor!$V$1:$V$1355,A100,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A100,1),INDEX(LinMotor!$V$1:$V$1355,A100,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A100,1),INDEX(LinMotor!$V$1:$V$1355,A100,1))/1000,\"0.0k\")),\"\")","v":-25.547869629629631},{"$f":"IF(A100<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A100,1),INDEX(LinMotor!$W$1:$W$1355,A100,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A100,1),INDEX(LinMotor!$X$1:$X$1355,A100,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A100,1),INDEX(LinMotor!$W$1:$W$1355,A100,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A100,1),INDEX(LinMotor!$X$1:$X$1355,A100,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A100,1),INDEX(LinMotor!$W$1:$W$1355,A100,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A100,1),INDEX(LinMotor!$X$1:$X$1355,A100,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A100<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A100,1),INDEX(LinMotor!$X$1:$X$1355,A100,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A100,1),INDEX(LinMotor!$Z$1:$Z$1355,A100,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A100,1),INDEX(LinMotor!$X$1:$X$1355,A100,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A100,1),INDEX(LinMotor!$Z$1:$Z$1355,A100,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A100,1),INDEX(LinMotor!$X$1:$X$1355,A100,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A100,1),INDEX(LinMotor!$Z$1:$Z$1355,A100,1)))/1000,\"0.0k\")),\"\")","v":31.553774400000002},{"$f":"IF(A100<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A100,1),INDEX(LinMotor!$Y$1:$Y$1355,A100,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A100,1),INDEX(LinMotor!$AB$1:$AB$445,A100,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A100,1),INDEX(LinMotor!$Y$1:$Y$1355,A100,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A100,1),INDEX(LinMotor!$AB$1:$AB$445,A100,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A100,1),INDEX(LinMotor!$Y$1:$Y$1355,A100,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A100,1),INDEX(LinMotor!$AB$1:$AB$445,A100,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A100,1),INDEX(LinMotor!$AD$1:$AD$1355,A100,1))","v":0.14871776488503011},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A100,1),INDEX(LinMotor!$AE$1:$AE$1355,A100,1))","v":0.23164477238095241},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A100,1),INDEX(LinMotor!$AF$1:$AF$1355,A100,1))","v":3.5692263572407228},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A100,1),INDEX(LinMotor!$AG$1:$AG$1355,A100,1))","v":11.118949074285716},{"$f":"IF(A100<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A100,1),INDEX(LinMotor!$AI$1:$AI$1355,A100,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A100,1),INDEX(LinMotor!$AI$1:$AI$1355,A100,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A100,1),INDEX(LinMotor!$AI$1:$AI$1355,A100,1))/1000,\"0.0k\")),\"\")","v":23.53081290472625},{"$f":"IF(A100<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A100,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A100,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A100,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A100,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A100,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A100,1))/1000,\"0.0k\")),\"\")","v":2.8281671606915895},{"$f":"IF(A100<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A100,1),INDEX(LinMotor!$AK$1:$AK$1355,A100,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A100,1),INDEX(LinMotor!$AK$1:$AK$1355,A100,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A100,1),INDEX(LinMotor!$AK$1:$AK$1355,A100,1))/1000,\"0.0k\")),\"\")","v":173.25142532532922},""]
[127,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A101,1),INDEX(LinMotor!$B$1:$B$1341,A101,1))","v":"AKM74Q"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A101,1),INDEX(LinMotor!$R$1:$R$1355,A101,1))","v":9.375},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A101,1),INDEX(LinMotor!$S$1:$S$1355,A101,1))","v":0.1947252225410695},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A101,1),INDEX(LinMotor!$T$1:$T$1355,A101,1))","v":0.22378563404255319},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A101,1),INDEX(LinMotor!$U$1:$U$1355,A101,1))","v":4.2689751962398194E-2},{"$f":"IF(A101<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A101,1),INDEX(LinMotor!$V$1:$V$1355,A101,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A101,1),INDEX(LinMotor!$V$1:$V$1355,A101,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A101,1),INDEX(LinMotor!$V$1:$V$1355,A101,1))/1000,\"0.0k\")),\"\")","v":-25.547869629629631},{"$f":"IF(A101<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A101,1),INDEX(LinMotor!$W$1:$W$1355,A101,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A101,1),INDEX(LinMotor!$X$1:$X$1355,A101,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A101,1),INDEX(LinMotor!$W$1:$W$1355,A101,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A101,1),INDEX(LinMotor!$X$1:$X$1355,A101,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A101,1),INDEX(LinMotor!$W$1:$W$1355,A101,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A101,1),INDEX(LinMotor!$X$1:$X$1355,A101,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A101<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A101,1),INDEX(LinMotor!$X$1:$X$1355,A101,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A101,1),INDEX(LinMotor!$Z$1:$Z$1355,A101,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A101,1),INDEX(LinMotor!$X$1:$X$1355,A101,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A101,1),INDEX(LinMotor!$Z$1:$Z$1355,A101,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A101,1),INDEX(LinMotor!$X$1:$X$1355,A101,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A101,1),INDEX(LinMotor!$Z$1:$Z$1355,A101,1)))/1000,\"0.0k\")),\"\")","v":31.553774400000002},{"$f":"IF(A101<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A101,1),INDEX(LinMotor!$Y$1:$Y$1355,A101,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A101,1),INDEX(LinMotor!$AB$1:$AB$445,A101,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A101,1),INDEX(LinMotor!$Y$1:$Y$1355,A101,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A101,1),INDEX(LinMotor!$AB$1:$AB$445,A101,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A101,1),INDEX(LinMotor!$Y$1:$Y$1355,A101,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A101,1),INDEX(LinMotor!$AB$1:$AB$445,A101,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A101,1),INDEX(LinMotor!$AD$1:$AD$1355,A101,1))","v":0.21101845017470489},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A101,1),INDEX(LinMotor!$AE$1:$AE$1355,A101,1))","v":0.32868515000000004},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A101,1),INDEX(LinMotor!$AF$1:$AF$1355,A101,1))","v":5.0644428041929173},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A101,1),INDEX(LinMotor!$AG$1:$AG$1355,A101,1))","v":15.776887200000001},{"$f":"IF(A101<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A101,1),INDEX(LinMotor!$AI$1:$AI$1355,A101,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A101,1),INDEX(LinMotor!$AI$1:$AI$1355,A101,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A101,1),INDEX(LinMotor!$AI$1:$AI$1355,A101,1))/1000,\"0.0k\")),\"\")","v":23.53081290472625},{"$f":"IF(A101<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A101,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A101,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A101,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A101,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A101,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A101,1))/1000,\"0.0k\")),\"\")","v":2.8281671606915895},{"$f":"IF(A101<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A101,1),INDEX(LinMotor!$AK$1:$AK$1355,A101,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A101,1),INDEX(LinMotor!$AK$1:$AK$1355,A101,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A101,1),INDEX(LinMotor!$AK$1:$AK$1355,A101,1))/1000,\"0.0k\")),\"\")","v":173.25142532532922},""]
[128,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A102,1),INDEX(LinMotor!$B$1:$B$1341,A102,1))","v":"AKM82T"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A102,1),INDEX(LinMotor!$R$1:$R$1355,A102,1))","v":6.5406976744186052},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A102,1),INDEX(LinMotor!$S$1:$S$1355,A102,1))","v":0.13682838014370946},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A102,1),INDEX(LinMotor!$T$1:$T$1355,A102,1))","v":0.15533847923809524},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A102,1),INDEX(LinMotor!$U$1:$U$1355,A102,1))","v":3.5858645594119727E-2},{"$f":"IF(A102<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A102,1),INDEX(LinMotor!$V$1:$V$1355,A102,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A102,1),INDEX(LinMotor!$V$1:$V$1355,A102,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A102,1),INDEX(LinMotor!$V$1:$V$1355,A102,1))/1000,\"0.0k\")),\"\")","v":-26.865531654320982},{"$f":"IF(A102<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A102,1),INDEX(LinMotor!$W$1:$W$1355,A102,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A102,1),INDEX(LinMotor!$X$1:$X$1355,A102,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A102,1),INDEX(LinMotor!$W$1:$W$1355,A102,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A102,1),INDEX(LinMotor!$X$1:$X$1355,A102,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A102,1),INDEX(LinMotor!$W$1:$W$1355,A102,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A102,1),INDEX(LinMotor!$X$1:$X$1355,A102,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A102<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A102,1),INDEX(LinMotor!$X$1:$X$1355,A102,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A102,1),INDEX(LinMotor!$Z$1:$Z$1355,A102,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A102,1),INDEX(LinMotor!$X$1:$X$1355,A102,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A102,1),INDEX(LinMotor!$Z$1:$Z$1355,A102,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A102,1),INDEX(LinMotor!$X$1:$X$1355,A102,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A102,1),INDEX(LinMotor!$Z$1:$Z$1355,A102,1)))/1000,\"0.0k\")),\"\")","v":32.621080640000002},{"$f":"IF(A102<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A102,1),INDEX(LinMotor!$Y$1:$Y$1355,A102,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A102,1),INDEX(LinMotor!$AB$1:$AB$445,A102,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A102,1),INDEX(LinMotor!$Y$1:$Y$1355,A102,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A102,1),INDEX(LinMotor!$AB$1:$AB$445,A102,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A102,1),INDEX(LinMotor!$Y$1:$Y$1355,A102,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A102,1),INDEX(LinMotor!$AB$1:$AB$445,A102,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A102,1),INDEX(LinMotor!$AD$1:$AD$1355,A102,1))","v":0.27276629654872014},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A102,1),INDEX(LinMotor!$AE$1:$AE$1355,A102,1))","v":0.43494774186666668},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A102,1),INDEX(LinMotor!$AF$1:$AF$1355,A102,1))","v":6.5463911171692839},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A102,1),INDEX(LinMotor!$AG$1:$AG$1355,A102,1))","v":20.8774916096},{"$f":"IF(A102<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A102,1),INDEX(LinMotor!$AI$1:$AI$1355,A102,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A102,1),INDEX(LinMotor!$AI$1:$AI$1355,A102,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A102,1),INDEX(LinMotor!$AI$1:$AI$1355,A102,1))/1000,\"0.0k\")),\"\")","v":23.762779560452554},{"$f":"IF(A102<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A102,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A102,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A102,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A102,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A102,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A102,1))/1000,\"0.0k\")),\"\")","v":3.0107462969418366},{"$f":"IF(A102<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A102,1),INDEX(LinMotor!$AK$1:$AK$1355,A102,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A102,1),INDEX(LinMotor!$AK$1:$AK$1355,A102,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A102,1),INDEX(LinMotor!$AK$1:$AK$1355,A102,1))/1000,\"0.0k\")),\"\")","v":184.43608796821474},""]
[129,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A103,1),INDEX(LinMotor!$B$1:$B$1341,A103,1))","v":"AKM83T"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A103,1),INDEX(LinMotor!$R$1:$R$1355,A103,1))","v":3.3682634730538923},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A103,1),INDEX(LinMotor!$S$1:$S$1355,A103,1))","v":8.1603030715410682E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A103,1),INDEX(LinMotor!$T$1:$T$1355,A103,1))","v":7.8829276491228076E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A103,1),INDEX(LinMotor!$U$1:$U$1355,A103,1))","v":4.57880287441833E-2},{"$f":"IF(A103<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A103,1),INDEX(LinMotor!$V$1:$V$1355,A103,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A103,1),INDEX(LinMotor!$V$1:$V$1355,A103,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A103,1),INDEX(LinMotor!$V$1:$V$1355,A103,1))/1000,\"0.0k\")),\"\")","v":-30.970555654320989},{"$f":"IF(A103<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A103,1),INDEX(LinMotor!$W$1:$W$1355,A103,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A103,1),INDEX(LinMotor!$X$1:$X$1355,A103,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A103,1),INDEX(LinMotor!$W$1:$W$1355,A103,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A103,1),INDEX(LinMotor!$X$1:$X$1355,A103,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A103,1),INDEX(LinMotor!$W$1:$W$1355,A103,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A103,1),INDEX(LinMotor!$X$1:$X$1355,A103,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A103<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A103,1),INDEX(LinMotor!$X$1:$X$1355,A103,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A103,1),INDEX(LinMotor!$Z$1:$Z$1355,A103,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A103,1),INDEX(LinMotor!$X$1:$X$1355,A103,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A103,1),INDEX(LinMotor!$Z$1:$Z$1355,A103,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A103,1),INDEX(LinMotor!$X$1:$X$1355,A103,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A103,1),INDEX(LinMotor!$Z$1:$Z$1355,A103,1)))/1000,\"0.0k\")),\"\")","v":35.946150080000002},{"$f":"IF(A103<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A103,1),INDEX(LinMotor!$Y$1:$Y$1355,A103,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A103,1),INDEX(LinMotor!$AB$1:$AB$445,A103,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A103,1),INDEX(LinMotor!$Y$1:$Y$1355,A103,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A103,1),INDEX(LinMotor!$AB$1:$AB$445,A103,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A103,1),INDEX(LinMotor!$Y$1:$Y$1355,A103,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A103,1),INDEX(LinMotor!$AB$1:$AB$445,A103,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A103,1),INDEX(LinMotor!$AD$1:$AD$1355,A103,1))","v":0.20982664504999282},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A103,1),INDEX(LinMotor!$AE$1:$AE$1355,A103,1))","v":0.35715726041025642},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A103,1),INDEX(LinMotor!$AF$1:$AF$1355,A103,1))","v":5.0358394811998277},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A103,1),INDEX(LinMotor!$AG$1:$AG$1355,A103,1))","v":17.143548499692308},{"$f":"IF(A103<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A103,1),INDEX(LinMotor!$AI$1:$AI$1355,A103,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A103,1),INDEX(LinMotor!$AI$1:$AI$1355,A103,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A103,1),INDEX(LinMotor!$AI$1:$AI$1355,A103,1))/1000,\"0.0k\")),\"\")","v":24.530071017231084},{"$f":"IF(A103<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A103,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A103,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A103,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A103,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A103,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A103,1))/1000,\"0.0k\")),\"\")","v":3.579550529106073},{"$f":"IF(A103<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A103,1),INDEX(LinMotor!$AK$1:$AK$1355,A103,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A103,1),INDEX(LinMotor!$AK$1:$AK$1355,A103,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A103,1),INDEX(LinMotor!$AK$1:$AK$1355,A103,1))/1000,\"0.0k\")),\"\")","v":219.28061389412758},""]
[130,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A104,1),INDEX(LinMotor!$B$1:$B$1341,A104,1))","v":"AKM84T"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A104,1),INDEX(LinMotor!$R$1:$R$1355,A104,1))","v":2.2727272727272729},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A104,1),INDEX(LinMotor!$S$1:$S$1355,A104,1))","v":6.0946488756377468E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A104,1),INDEX(LinMotor!$T$1:$T$1355,A104,1))","v":5.8758524550898202E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A104,1),INDEX(LinMotor!$U$1:$U$1355,A104,1))","v":5.7828361975168191E-2},{"$f":"IF(A104<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A104,1),INDEX(LinMotor!$V$1:$V$1355,A104,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A104,1),INDEX(LinMotor!$V$1:$V$1355,A104,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A104,1),INDEX(LinMotor!$V$1:$V$1355,A104,1))/1000,\"0.0k\")),\"\")","v":-35.050239999999995},{"$f":"IF(A104<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A104,1),INDEX(LinMotor!$W$1:$W$1355,A104,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A104,1),INDEX(LinMotor!$X$1:$X$1355,A104,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A104,1),INDEX(LinMotor!$W$1:$W$1355,A104,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A104,1),INDEX(LinMotor!$X$1:$X$1355,A104,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A104,1),INDEX(LinMotor!$W$1:$W$1355,A104,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A104,1),INDEX(LinMotor!$X$1:$X$1355,A104,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A104<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A104,1),INDEX(LinMotor!$X$1:$X$1355,A104,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A104,1),INDEX(LinMotor!$Z$1:$Z$1355,A104,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A104,1),INDEX(LinMotor!$X$1:$X$1355,A104,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A104,1),INDEX(LinMotor!$Z$1:$Z$1355,A104,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A104,1),INDEX(LinMotor!$X$1:$X$1355,A104,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A104,1),INDEX(LinMotor!$Z$1:$Z$1355,A104,1)))/1000,\"0.0k\")),\"\")","v":39.2506944},{"$f":"IF(A104<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A104,1),INDEX(LinMotor!$Y$1:$Y$1355,A104,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A104,1),INDEX(LinMotor!$AB$1:$AB$445,A104,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A104,1),INDEX(LinMotor!$Y$1:$Y$1355,A104,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A104,1),INDEX(LinMotor!$AB$1:$AB$445,A104,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A104,1),INDEX(LinMotor!$Y$1:$Y$1355,A104,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A104,1),INDEX(LinMotor!$AB$1:$AB$445,A104,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A104,1),INDEX(LinMotor!$AD$1:$AD$1355,A104,1))","v":0.16926849097058047},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A104,1),INDEX(LinMotor!$AE$1:$AE$1355,A104,1))","v":0.30437459777777776},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A104,1),INDEX(LinMotor!$AF$1:$AF$1355,A104,1))","v":4.0624437832939311},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A104,1),INDEX(LinMotor!$AG$1:$AG$1355,A104,1))","v":14.609980693333332},{"$f":"IF(A104<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A104,1),INDEX(LinMotor!$AI$1:$AI$1355,A104,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A104,1),INDEX(LinMotor!$AI$1:$AI$1355,A104,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A104,1),INDEX(LinMotor!$AI$1:$AI$1355,A104,1))/1000,\"0.0k\")),\"\")","v":25.35480827682192},{"$f":"IF(A104<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A104,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A104,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A104,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A104,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A104,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A104,1))/1000,\"0.0k\")),\"\")","v":4.1448436240347268},{"$f":"IF(A104<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A104,1),INDEX(LinMotor!$AK$1:$AK$1355,A104,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A104,1),INDEX(LinMotor!$AK$1:$AK$1355,A104,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A104,1),INDEX(LinMotor!$AK$1:$AK$1355,A104,1))/1000,\"0.0k\")),\"\")","v":253.91005015383104},""]
[173,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A105,1),INDEX(LinMotor!$B$1:$B$1341,A105,1))","v":"DBL7N02600"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A105,1),INDEX(LinMotor!$R$1:$R$1355,A105,1))","v":11.550308008213552},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A105,1),INDEX(LinMotor!$S$1:$S$1355,A105,1))","v":0.38860420301662824},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A105,1),INDEX(LinMotor!$T$1:$T$1355,A105,1))","v":0.2673710585483316},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A105,1),INDEX(LinMotor!$U$1:$U$1355,A105,1))","v":3.1104735669480223E-2},{"$f":"IF(A105<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A105,1),INDEX(LinMotor!$V$1:$V$1355,A105,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A105,1),INDEX(LinMotor!$V$1:$V$1355,A105,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A105,1),INDEX(LinMotor!$V$1:$V$1355,A105,1))/1000,\"0.0k\")),\"\")","v":-24.975193441975311},{"$f":"IF(A105<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A105,1),INDEX(LinMotor!$W$1:$W$1355,A105,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A105,1),INDEX(LinMotor!$X$1:$X$1355,A105,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A105,1),INDEX(LinMotor!$W$1:$W$1355,A105,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A105,1),INDEX(LinMotor!$X$1:$X$1355,A105,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A105,1),INDEX(LinMotor!$W$1:$W$1355,A105,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A105,1),INDEX(LinMotor!$X$1:$X$1355,A105,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A105<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A105,1),INDEX(LinMotor!$X$1:$X$1355,A105,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A105,1),INDEX(LinMotor!$Z$1:$Z$1355,A105,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A105,1),INDEX(LinMotor!$X$1:$X$1355,A105,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A105,1),INDEX(LinMotor!$Z$1:$Z$1355,A105,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A105,1),INDEX(LinMotor!$X$1:$X$1355,A105,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A105,1),INDEX(LinMotor!$Z$1:$Z$1355,A105,1)))/1000,\"0.0k\")),\"\")","v":31.089906687999999},{"$f":"IF(A105<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A105,1),INDEX(LinMotor!$Y$1:$Y$1355,A105,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A105,1),INDEX(LinMotor!$AB$1:$AB$445,A105,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A105,1),INDEX(LinMotor!$Y$1:$Y$1355,A105,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A105,1),INDEX(LinMotor!$AB$1:$AB$445,A105,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A105,1),INDEX(LinMotor!$Y$1:$Y$1355,A105,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A105,1),INDEX(LinMotor!$AB$1:$AB$445,A105,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A105,1),INDEX(LinMotor!$AD$1:$AD$1355,A105,1))","v":0.27479154568605424},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A105,1),INDEX(LinMotor!$AE$1:$AE$1355,A105,1))","v":0.42350033148717947},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A105,1),INDEX(LinMotor!$AF$1:$AF$1355,A105,1))","v":6.5949970964653017},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A105,1),INDEX(LinMotor!$AG$1:$AG$1355,A105,1))","v":20.328015911384615},{"$f":"IF(A105<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A105,1),INDEX(LinMotor!$AI$1:$AI$1355,A105,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A105,1),INDEX(LinMotor!$AI$1:$AI$1355,A105,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A105,1),INDEX(LinMotor!$AI$1:$AI$1355,A105,1))/1000,\"0.0k\")),\"\")","v":23.432266585280207},{"$f":"IF(A105<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A105,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A105,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A105,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A105,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A105,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A105,1))/1000,\"0.0k\")),\"\")","v":2.7488154591674427},{"$f":"IF(A105<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A105,1),INDEX(LinMotor!$AK$1:$AK$1355,A105,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A105,1),INDEX(LinMotor!$AK$1:$AK$1355,A105,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A105,1),INDEX(LinMotor!$AK$1:$AK$1355,A105,1))/1000,\"0.0k\")),\"\")","v":168.39039886899815},""]
[174,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A106,1),INDEX(LinMotor!$B$1:$B$1341,A106,1))","v":"DBL7N03200"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A106,1),INDEX(LinMotor!$R$1:$R$1355,A106,1))","v":9.8597721297107803},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A106,1),INDEX(LinMotor!$S$1:$S$1355,A106,1))","v":0.31683880991444852},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A106,1),INDEX(LinMotor!$T$1:$T$1355,A106,1))","v":0.21876862605790645},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A106,1),INDEX(LinMotor!$U$1:$U$1355,A106,1))","v":3.2213303383261414E-2},{"$f":"IF(A106<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A106,1),INDEX(LinMotor!$V$1:$V$1355,A106,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A106,1),INDEX(LinMotor!$V$1:$V$1355,A106,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A106,1),INDEX(LinMotor!$V$1:$V$1355,A106,1))/1000,\"0.0k\")),\"\")","v":-25.398365669135799},{"$f":"IF(A106<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A106,1),INDEX(LinMotor!$W$1:$W$1355,A106,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A106,1),INDEX(LinMotor!$X$1:$X$1355,A106,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A106,1),INDEX(LinMotor!$W$1:$W$1355,A106,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A106,1),INDEX(LinMotor!$X$1:$X$1355,A106,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A106,1),INDEX(LinMotor!$W$1:$W$1355,A106,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A106,1),INDEX(LinMotor!$X$1:$X$1355,A106,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A106<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A106,1),INDEX(LinMotor!$X$1:$X$1355,A106,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A106,1),INDEX(LinMotor!$Z$1:$Z$1355,A106,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A106,1),INDEX(LinMotor!$X$1:$X$1355,A106,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A106,1),INDEX(LinMotor!$Z$1:$Z$1355,A106,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A106,1),INDEX(LinMotor!$X$1:$X$1355,A106,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A106,1),INDEX(LinMotor!$Z$1:$Z$1355,A106,1)))/1000,\"0.0k\")),\"\")","v":31.432676191999999},{"$f":"IF(A106<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A106,1),INDEX(LinMotor!$Y$1:$Y$1355,A106,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A106,1),INDEX(LinMotor!$AB$1:$AB$445,A106,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A106,1),INDEX(LinMotor!$Y$1:$Y$1355,A106,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A106,1),INDEX(LinMotor!$AB$1:$AB$445,A106,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A106,1),INDEX(LinMotor!$Y$1:$Y$1355,A106,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A106,1),INDEX(LinMotor!$AB$1:$AB$445,A106,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A106,1),INDEX(LinMotor!$AD$1:$AD$1355,A106,1))","v":0.26348317129820747},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A106,1),INDEX(LinMotor!$AE$1:$AE$1355,A106,1))","v":0.40927963791666661},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A106,1),INDEX(LinMotor!$AF$1:$AF$1355,A106,1))","v":6.3235961111569798},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A106,1),INDEX(LinMotor!$AG$1:$AG$1355,A106,1))","v":19.645422619999998},{"$f":"IF(A106<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A106,1),INDEX(LinMotor!$AI$1:$AI$1355,A106,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A106,1),INDEX(LinMotor!$AI$1:$AI$1355,A106,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A106,1),INDEX(LinMotor!$AI$1:$AI$1355,A106,1))/1000,\"0.0k\")),\"\")","v":23.50495211097995},{"$f":"IF(A106<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A106,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A106,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A106,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A106,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A106,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A106,1))/1000,\"0.0k\")),\"\")","v":2.8074514510016568},{"$f":"IF(A106<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A106,1),INDEX(LinMotor!$AK$1:$AK$1355,A106,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A106,1),INDEX(LinMotor!$AK$1:$AK$1355,A106,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A106,1),INDEX(LinMotor!$AK$1:$AK$1355,A106,1))/1000,\"0.0k\")),\"\")","v":171.9823962946941},""]
[175,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A107,1),INDEX(LinMotor!$B$1:$B$1341,A107,1))","v":"DBL7N04000"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A107,1),INDEX(LinMotor!$R$1:$R$1355,A107,1))","v":8.0703012912482066},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A107,1),INDEX(LinMotor!$S$1:$S$1355,A107,1))","v":0.25480387227307189},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A107,1),INDEX(LinMotor!$T$1:$T$1355,A107,1))","v":0.19878040144332462},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A107,1),INDEX(LinMotor!$U$1:$U$1355,A107,1))","v":3.4113881900241054E-2},{"$f":"IF(A107<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A107,1),INDEX(LinMotor!$V$1:$V$1355,A107,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A107,1),INDEX(LinMotor!$V$1:$V$1355,A107,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A107,1),INDEX(LinMotor!$V$1:$V$1355,A107,1))/1000,\"0.0k\")),\"\")","v":-26.039458923456792},{"$f":"IF(A107<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A107,1),INDEX(LinMotor!$W$1:$W$1355,A107,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A107,1),INDEX(LinMotor!$X$1:$X$1355,A107,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A107,1),INDEX(LinMotor!$W$1:$W$1355,A107,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A107,1),INDEX(LinMotor!$X$1:$X$1355,A107,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A107,1),INDEX(LinMotor!$W$1:$W$1355,A107,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A107,1),INDEX(LinMotor!$X$1:$X$1355,A107,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A107<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A107,1),INDEX(LinMotor!$X$1:$X$1355,A107,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A107,1),INDEX(LinMotor!$Z$1:$Z$1355,A107,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A107,1),INDEX(LinMotor!$X$1:$X$1355,A107,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A107,1),INDEX(LinMotor!$Z$1:$Z$1355,A107,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A107,1),INDEX(LinMotor!$X$1:$X$1355,A107,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A107,1),INDEX(LinMotor!$Z$1:$Z$1355,A107,1)))/1000,\"0.0k\")),\"\")","v":31.951961728000001},{"$f":"IF(A107<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A107,1),INDEX(LinMotor!$Y$1:$Y$1355,A107,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A107,1),INDEX(LinMotor!$AB$1:$AB$445,A107,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A107,1),INDEX(LinMotor!$Y$1:$Y$1355,A107,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A107,1),INDEX(LinMotor!$AB$1:$AB$445,A107,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A107,1),INDEX(LinMotor!$Y$1:$Y$1355,A107,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A107,1),INDEX(LinMotor!$AB$1:$AB$445,A107,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A107,1),INDEX(LinMotor!$AD$1:$AD$1355,A107,1))","v":0.24779073831484708},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A107,1),INDEX(LinMotor!$AE$1:$AE$1355,A107,1))","v":0.38941453355999994},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A107,1),INDEX(LinMotor!$AF$1:$AF$1355,A107,1))","v":5.9469777195563296},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A107,1),INDEX(LinMotor!$AG$1:$AG$1355,A107,1))","v":18.691897610879998},{"$f":"IF(A107<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A107,1),INDEX(LinMotor!$AI$1:$AI$1355,A107,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A107,1),INDEX(LinMotor!$AI$1:$AI$1355,A107,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A107,1),INDEX(LinMotor!$AI$1:$AI$1355,A107,1))/1000,\"0.0k\")),\"\")","v":23.616509499740783},{"$f":"IF(A107<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A107,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A107,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A107,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A107,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A107,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A107,1))/1000,\"0.0k\")),\"\")","v":2.8962832230618742},{"$f":"IF(A107<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A107,1),INDEX(LinMotor!$AK$1:$AK$1355,A107,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A107,1),INDEX(LinMotor!$AK$1:$AK$1355,A107,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A107,1),INDEX(LinMotor!$AK$1:$AK$1355,A107,1))/1000,\"0.0k\")),\"\")","v":177.42416484979037},""]
[177,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A108,1),INDEX(LinMotor!$B$1:$B$1341,A108,1))","v":"DBL8N06800"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A108,1),INDEX(LinMotor!$R$1:$R$1355,A108,1))","v":9.9031690140845079},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A108,1),INDEX(LinMotor!$S$1:$S$1355,A108,1))","v":0.14906846547452951},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A108,1),INDEX(LinMotor!$T$1:$T$1355,A108,1))","v":0.12132206035521235},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A108,1),INDEX(LinMotor!$U$1:$U$1355,A108,1))","v":3.6699273820539204E-2},{"$f":"IF(A108<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A108,1),INDEX(LinMotor!$V$1:$V$1355,A108,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A108,1),INDEX(LinMotor!$V$1:$V$1355,A108,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A108,1),INDEX(LinMotor!$V$1:$V$1355,A108,1))/1000,\"0.0k\")),\"\")","v":-25.385695841975306},{"$f":"IF(A108<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A108,1),INDEX(LinMotor!$W$1:$W$1355,A108,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A108,1),INDEX(LinMotor!$X$1:$X$1355,A108,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A108,1),INDEX(LinMotor!$W$1:$W$1355,A108,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A108,1),INDEX(LinMotor!$X$1:$X$1355,A108,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A108,1),INDEX(LinMotor!$W$1:$W$1355,A108,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A108,1),INDEX(LinMotor!$X$1:$X$1355,A108,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A108<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A108,1),INDEX(LinMotor!$X$1:$X$1355,A108,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A108,1),INDEX(LinMotor!$Z$1:$Z$1355,A108,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A108,1),INDEX(LinMotor!$X$1:$X$1355,A108,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A108,1),INDEX(LinMotor!$Z$1:$Z$1355,A108,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A108,1),INDEX(LinMotor!$X$1:$X$1355,A108,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A108,1),INDEX(LinMotor!$Z$1:$Z$1355,A108,1)))/1000,\"0.0k\")),\"\")","v":31.422413632000001},{"$f":"IF(A108<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A108,1),INDEX(LinMotor!$Y$1:$Y$1355,A108,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A108,1),INDEX(LinMotor!$AB$1:$AB$445,A108,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A108,1),INDEX(LinMotor!$Y$1:$Y$1355,A108,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A108,1),INDEX(LinMotor!$AB$1:$AB$445,A108,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A108,1),INDEX(LinMotor!$Y$1:$Y$1355,A108,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A108,1),INDEX(LinMotor!$AB$1:$AB$445,A108,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A108,1),INDEX(LinMotor!$AD$1:$AD$1355,A108,1))","v":0.22936400370318685},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A108,1),INDEX(LinMotor!$AE$1:$AE$1355,A108,1))","v":0.35619770354901958},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A108,1),INDEX(LinMotor!$AF$1:$AF$1355,A108,1))","v":5.5047360888764842},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A108,1),INDEX(LinMotor!$AG$1:$AG$1355,A108,1))","v":17.09748977035294},{"$f":"IF(A108<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A108,1),INDEX(LinMotor!$AI$1:$AI$1355,A108,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A108,1),INDEX(LinMotor!$AI$1:$AI$1355,A108,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A108,1),INDEX(LinMotor!$AI$1:$AI$1355,A108,1))/1000,\"0.0k\")),\"\")","v":23.502764860391657},{"$f":"IF(A108<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A108,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A108,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A108,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A108,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A108,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A108,1))/1000,\"0.0k\")),\"\")","v":2.8056958823838656},{"$f":"IF(A108<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A108,1),INDEX(LinMotor!$AK$1:$AK$1355,A108,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A108,1),INDEX(LinMotor!$AK$1:$AK$1355,A108,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A108,1),INDEX(LinMotor!$AK$1:$AK$1355,A108,1))/1000,\"0.0k\")),\"\")","v":171.8748514615894},""]
[178,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A109,1),INDEX(LinMotor!$B$1:$B$1341,A109,1))","v":"DBL8L09300"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A109,1),INDEX(LinMotor!$R$1:$R$1355,A109,1))","v":7.3529411764705879},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A109,1),INDEX(LinMotor!$S$1:$S$1355,A109,1))","v":0.1098917238839454},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A109,1),INDEX(LinMotor!$T$1:$T$1355,A109,1))","v":0.10079149215085374},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A109,1),INDEX(LinMotor!$U$1:$U$1355,A109,1))","v":5.3539686746006634E-2},{"$f":"IF(A109<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A109,1),INDEX(LinMotor!$V$1:$V$1355,A109,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A109,1),INDEX(LinMotor!$V$1:$V$1355,A109,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A109,1),INDEX(LinMotor!$V$1:$V$1355,A109,1))/1000,\"0.0k\")),\"\")","v":-26.384078222222222},{"$f":"IF(A109<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A109,1),INDEX(LinMotor!$W$1:$W$1355,A109,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A109,1),INDEX(LinMotor!$X$1:$X$1355,A109,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A109,1),INDEX(LinMotor!$W$1:$W$1355,A109,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A109,1),INDEX(LinMotor!$X$1:$X$1355,A109,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A109,1),INDEX(LinMotor!$W$1:$W$1355,A109,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A109,1),INDEX(LinMotor!$X$1:$X$1355,A109,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A109<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A109,1),INDEX(LinMotor!$X$1:$X$1355,A109,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A109,1),INDEX(LinMotor!$Z$1:$Z$1355,A109,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A109,1),INDEX(LinMotor!$X$1:$X$1355,A109,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A109,1),INDEX(LinMotor!$Z$1:$Z$1355,A109,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A109,1),INDEX(LinMotor!$X$1:$X$1355,A109,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A109,1),INDEX(LinMotor!$Z$1:$Z$1355,A109,1)))/1000,\"0.0k\")),\"\")","v":32.231103360000006},{"$f":"IF(A109<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A109,1),INDEX(LinMotor!$Y$1:$Y$1355,A109,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A109,1),INDEX(LinMotor!$AB$1:$AB$445,A109,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A109,1),INDEX(LinMotor!$Y$1:$Y$1355,A109,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A109,1),INDEX(LinMotor!$AB$1:$AB$445,A109,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A109,1),INDEX(LinMotor!$Y$1:$Y$1355,A109,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A109,1),INDEX(LinMotor!$AB$1:$AB$445,A109,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A109,1),INDEX(LinMotor!$AD$1:$AD$1355,A109,1))","v":0.15525284549499827},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A109,1),INDEX(LinMotor!$AE$1:$AE$1355,A109,1))","v":0.24548779440860222},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A109,1),INDEX(LinMotor!$AF$1:$AF$1355,A109,1))","v":3.7260682918799586},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A109,1),INDEX(LinMotor!$AG$1:$AG$1355,A109,1))","v":11.783414131612906},{"$f":"IF(A109<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A109,1),INDEX(LinMotor!$AI$1:$AI$1355,A109,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A109,1),INDEX(LinMotor!$AI$1:$AI$1355,A109,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A109,1),INDEX(LinMotor!$AI$1:$AI$1355,A109,1))/1000,\"0.0k\")),\"\")","v":23.67718711491467},{"$f":"IF(A109<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A109,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A109,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A109,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A109,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A109,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A109,1))/1000,\"0.0k\")),\"\")","v":2.9440346894657852},{"$f":"IF(A109<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A109,1),INDEX(LinMotor!$AK$1:$AK$1355,A109,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A109,1),INDEX(LinMotor!$AK$1:$AK$1355,A109,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A109,1),INDEX(LinMotor!$AK$1:$AK$1355,A109,1))/1000,\"0.0k\")),\"\")","v":180.34938431023735},""]
[179,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A110,1),INDEX(LinMotor!$B$1:$B$1341,A110,1))","v":"DBL8L11500"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A110,1),INDEX(LinMotor!$R$1:$R$1355,A110,1))","v":5.9210526315789478},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A110,1),INDEX(LinMotor!$S$1:$S$1355,A110,1))","v":8.9511354924322106E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A110,1),INDEX(LinMotor!$T$1:$T$1355,A110,1))","v":8.3381016023858862E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A110,1),INDEX(LinMotor!$U$1:$U$1355,A110,1))","v":5.3477692665472809E-2},{"$f":"IF(A110<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A110,1),INDEX(LinMotor!$V$1:$V$1355,A110,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A110,1),INDEX(LinMotor!$V$1:$V$1355,A110,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A110,1),INDEX(LinMotor!$V$1:$V$1355,A110,1))/1000,\"0.0k\")),\"\")","v":-27.321645432098769},{"$f":"IF(A110<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A110,1),INDEX(LinMotor!$W$1:$W$1355,A110,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A110,1),INDEX(LinMotor!$X$1:$X$1355,A110,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A110,1),INDEX(LinMotor!$W$1:$W$1355,A110,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A110,1),INDEX(LinMotor!$X$1:$X$1355,A110,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A110,1),INDEX(LinMotor!$W$1:$W$1355,A110,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A110,1),INDEX(LinMotor!$X$1:$X$1355,A110,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A110<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A110,1),INDEX(LinMotor!$X$1:$X$1355,A110,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A110,1),INDEX(LinMotor!$Z$1:$Z$1355,A110,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A110,1),INDEX(LinMotor!$X$1:$X$1355,A110,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A110,1),INDEX(LinMotor!$Z$1:$Z$1355,A110,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A110,1),INDEX(LinMotor!$X$1:$X$1355,A110,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A110,1),INDEX(LinMotor!$Z$1:$Z$1355,A110,1)))/1000,\"0.0k\")),\"\")","v":32.990532799999997},{"$f":"IF(A110<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A110,1),INDEX(LinMotor!$Y$1:$Y$1355,A110,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A110,1),INDEX(LinMotor!$AB$1:$AB$445,A110,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A110,1),INDEX(LinMotor!$Y$1:$Y$1355,A110,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A110,1),INDEX(LinMotor!$AB$1:$AB$445,A110,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A110,1),INDEX(LinMotor!$Y$1:$Y$1355,A110,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A110,1),INDEX(LinMotor!$AB$1:$AB$445,A110,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A110,1),INDEX(LinMotor!$AD$1:$AD$1355,A110,1))","v":0.15991041536104877},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A110,1),INDEX(LinMotor!$AE$1:$AE$1355,A110,1))","v":0.25699146927536232},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A110,1),INDEX(LinMotor!$AF$1:$AF$1355,A110,1))","v":3.8378499686651706},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A110,1),INDEX(LinMotor!$AG$1:$AG$1355,A110,1))","v":12.335590525217391},{"$f":"IF(A110<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A110,1),INDEX(LinMotor!$AI$1:$AI$1355,A110,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A110,1),INDEX(LinMotor!$AI$1:$AI$1355,A110,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A110,1),INDEX(LinMotor!$AI$1:$AI$1355,A110,1))/1000,\"0.0k\")),\"\")","v":23.844742792175253},{"$f":"IF(A110<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A110,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A110,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A110,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A110,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A110,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A110,1))/1000,\"0.0k\")),\"\")","v":3.0739467671823091},{"$f":"IF(A110<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A110,1),INDEX(LinMotor!$AK$1:$AK$1355,A110,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A110,1),INDEX(LinMotor!$AK$1:$AK$1355,A110,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A110,1),INDEX(LinMotor!$AK$1:$AK$1355,A110,1))/1000,\"0.0k\")),\"\")","v":188.30770195998292},""]
[38,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A111,1),INDEX(LinMotor!$B$1:$B$1341,A111,1))","v":"AKM32C"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A111,1),INDEX(LinMotor!$R$1:$R$1355,A111,1))","v":1906.7796610169489},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A111,1),INDEX(LinMotor!$S$1:$S$1355,A111,1))","v":4.9584031437502301},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A111,1),INDEX(LinMotor!$T$1:$T$1355,A111,1))","v":4.2056170261271681},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A111,1),INDEX(LinMotor!$U$1:$U$1355,A111,1))","v":0.22739684467508217},{"$f":"IF(A111<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A111,1),INDEX(LinMotor!$V$1:$V$1355,A111,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A111,1),INDEX(LinMotor!$V$1:$V$1355,A111,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A111,1),INDEX(LinMotor!$V$1:$V$1355,A111,1))/1000,\"0.0k\")),\"\")","v":-22.52206150716049},{"$f":"IF(A111<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A111,1),INDEX(LinMotor!$W$1:$W$1355,A111,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A111,1),INDEX(LinMotor!$X$1:$X$1355,A111,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A111,1),INDEX(LinMotor!$W$1:$W$1355,A111,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A111,1),INDEX(LinMotor!$X$1:$X$1355,A111,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A111,1),INDEX(LinMotor!$W$1:$W$1355,A111,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A111,1),INDEX(LinMotor!$X$1:$X$1355,A111,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A111<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A111,1),INDEX(LinMotor!$X$1:$X$1355,A111,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A111,1),INDEX(LinMotor!$Z$1:$Z$1355,A111,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A111,1),INDEX(LinMotor!$X$1:$X$1355,A111,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A111,1),INDEX(LinMotor!$Z$1:$Z$1355,A111,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A111,1),INDEX(LinMotor!$X$1:$X$1355,A111,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A111,1),INDEX(LinMotor!$Z$1:$Z$1355,A111,1)))/1000,\"0.0k\")),\"\")","v":29.102869820800002},{"$f":"IF(A111<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A111,1),INDEX(LinMotor!$Y$1:$Y$1355,A111,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A111,1),INDEX(LinMotor!$AB$1:$AB$445,A111,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A111,1),INDEX(LinMotor!$Y$1:$Y$1355,A111,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A111,1),INDEX(LinMotor!$AB$1:$AB$445,A111,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A111,1),INDEX(LinMotor!$Y$1:$Y$1355,A111,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A111,1),INDEX(LinMotor!$AB$1:$AB$445,A111,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A111,1),INDEX(LinMotor!$AD$1:$AD$1355,A111,1))","v":0.29735017877218817},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A111,1),INDEX(LinMotor!$AE$1:$AE$1355,A111,1))","v":0.43654304731200005},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A111,1),INDEX(LinMotor!$AF$1:$AF$1355,A111,1))","v":7.136404290532516},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A111,1),INDEX(LinMotor!$AG$1:$AG$1355,A111,1))","v":20.954066270976003},{"$f":"IF(A111<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A111,1),INDEX(LinMotor!$AI$1:$AI$1355,A111,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A111,1),INDEX(LinMotor!$AI$1:$AI$1355,A111,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A111,1),INDEX(LinMotor!$AI$1:$AI$1355,A111,1))/1000,\"0.0k\")),\"\")","v":23.026196873630557},{"$f":"IF(A111<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A111,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A111,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A111,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A111,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A111,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A111,1))/1000,\"0.0k\")),\"\")","v":2.4089022633907784},{"$f":"IF(A111<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A111,1),INDEX(LinMotor!$AK$1:$AK$1355,A111,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A111,1),INDEX(LinMotor!$AK$1:$AK$1355,A111,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A111,1),INDEX(LinMotor!$AK$1:$AK$1355,A111,1))/1000,\"0.0k\")),\"\")","v":147.56756828327212},""]
[39,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A112,1),INDEX(LinMotor!$B$1:$B$1341,A112,1))","v":"AKM32D"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A112,1),INDEX(LinMotor!$R$1:$R$1355,A112,1))","v":1906.7796610169489},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A112,1),INDEX(LinMotor!$S$1:$S$1355,A112,1))","v":4.8624128009550569},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A112,1),INDEX(LinMotor!$T$1:$T$1355,A112,1))","v":4.0989957494084512},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A112,1),INDEX(LinMotor!$U$1:$U$1355,A112,1))","v":8.3132797597950614E-2},{"$f":"IF(A112<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A112,1),INDEX(LinMotor!$V$1:$V$1355,A112,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A112,1),INDEX(LinMotor!$V$1:$V$1355,A112,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A112,1),INDEX(LinMotor!$V$1:$V$1355,A112,1))/1000,\"0.0k\")),\"\")","v":-22.52206150716049},{"$f":"IF(A112<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A112,1),INDEX(LinMotor!$W$1:$W$1355,A112,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A112,1),INDEX(LinMotor!$X$1:$X$1355,A112,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A112,1),INDEX(LinMotor!$W$1:$W$1355,A112,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A112,1),INDEX(LinMotor!$X$1:$X$1355,A112,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A112,1),INDEX(LinMotor!$W$1:$W$1355,A112,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A112,1),INDEX(LinMotor!$X$1:$X$1355,A112,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A112<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A112,1),INDEX(LinMotor!$X$1:$X$1355,A112,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A112,1),INDEX(LinMotor!$Z$1:$Z$1355,A112,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A112,1),INDEX(LinMotor!$X$1:$X$1355,A112,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A112,1),INDEX(LinMotor!$Z$1:$Z$1355,A112,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A112,1),INDEX(LinMotor!$X$1:$X$1355,A112,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A112,1),INDEX(LinMotor!$Z$1:$Z$1355,A112,1)))/1000,\"0.0k\")),\"\")","v":29.102869820800002},{"$f":"IF(A112<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A112,1),INDEX(LinMotor!$Y$1:$Y$1355,A112,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A112,1),INDEX(LinMotor!$AB$1:$AB$445,A112,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A112,1),INDEX(LinMotor!$Y$1:$Y$1355,A112,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A112,1),INDEX(LinMotor!$AB$1:$AB$445,A112,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A112,1),INDEX(LinMotor!$Y$1:$Y$1355,A112,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A112,1),INDEX(LinMotor!$AB$1:$AB$445,A112,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A112,1),INDEX(LinMotor!$AD$1:$AD$1355,A112,1))","v":0.45145077523282923},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A112,1),INDEX(LinMotor!$AE$1:$AE$1355,A112,1))","v":0.66277981720163404},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A112,1),INDEX(LinMotor!$AF$1:$AF$1355,A112,1))","v":10.834818605587902},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A112,1),INDEX(LinMotor!$AG$1:$AG$1355,A112,1))","v":31.813431225678436},{"$f":"IF(A112<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A112,1),INDEX(LinMotor!$AI$1:$AI$1355,A112,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A112,1),INDEX(LinMotor!$AI$1:$AI$1355,A112,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A112,1),INDEX(LinMotor!$AI$1:$AI$1355,A112,1))/1000,\"0.0k\")),\"\")","v":23.026196873630557},{"$f":"IF(A112<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A112,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A112,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A112,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A112,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A112,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A112,1))/1000,\"0.0k\")),\"\")","v":2.4089022633907784},{"$f":"IF(A112<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A112,1),INDEX(LinMotor!$AK$1:$AK$1355,A112,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A112,1),INDEX(LinMotor!$AK$1:$AK$1355,A112,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A112,1),INDEX(LinMotor!$AK$1:$AK$1355,A112,1))/1000,\"0.0k\")),\"\")","v":147.56756828327212},""]
[40,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A113,1),INDEX(LinMotor!$B$1:$B$1341,A113,1))","v":"AKM32E"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A113,1),INDEX(LinMotor!$R$1:$R$1355,A113,1))","v":1906.7796610169489},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A113,1),INDEX(LinMotor!$S$1:$S$1355,A113,1))","v":4.8634233379023435},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A113,1),INDEX(LinMotor!$T$1:$T$1355,A113,1))","v":4.09323063583685},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A113,1),INDEX(LinMotor!$U$1:$U$1355,A113,1))","v":6.1176682226196488E-2},{"$f":"IF(A113<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A113,1),INDEX(LinMotor!$V$1:$V$1355,A113,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A113,1),INDEX(LinMotor!$V$1:$V$1355,A113,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A113,1),INDEX(LinMotor!$V$1:$V$1355,A113,1))/1000,\"0.0k\")),\"\")","v":-22.52206150716049},{"$f":"IF(A113<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A113,1),INDEX(LinMotor!$W$1:$W$1355,A113,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A113,1),INDEX(LinMotor!$X$1:$X$1355,A113,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A113,1),INDEX(LinMotor!$W$1:$W$1355,A113,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A113,1),INDEX(LinMotor!$X$1:$X$1355,A113,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A113,1),INDEX(LinMotor!$W$1:$W$1355,A113,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A113,1),INDEX(LinMotor!$X$1:$X$1355,A113,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A113<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A113,1),INDEX(LinMotor!$X$1:$X$1355,A113,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A113,1),INDEX(LinMotor!$Z$1:$Z$1355,A113,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A113,1),INDEX(LinMotor!$X$1:$X$1355,A113,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A113,1),INDEX(LinMotor!$Z$1:$Z$1355,A113,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A113,1),INDEX(LinMotor!$X$1:$X$1355,A113,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A113,1),INDEX(LinMotor!$Z$1:$Z$1355,A113,1)))/1000,\"0.0k\")),\"\")","v":29.102869820800002},{"$f":"IF(A113<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A113,1),INDEX(LinMotor!$Y$1:$Y$1355,A113,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A113,1),INDEX(LinMotor!$AB$1:$AB$445,A113,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A113,1),INDEX(LinMotor!$Y$1:$Y$1355,A113,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A113,1),INDEX(LinMotor!$AB$1:$AB$445,A113,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A113,1),INDEX(LinMotor!$Y$1:$Y$1355,A113,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A113,1),INDEX(LinMotor!$AB$1:$AB$445,A113,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A113,1),INDEX(LinMotor!$AD$1:$AD$1355,A113,1))","v":0.57089290859039388},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A113,1),INDEX(LinMotor!$AE$1:$AE$1355,A113,1))","v":0.83813411861372555},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A113,1),INDEX(LinMotor!$AF$1:$AF$1355,A113,1))","v":13.701429806169454},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A113,1),INDEX(LinMotor!$AG$1:$AG$1355,A113,1))","v":40.230437693458825},{"$f":"IF(A113<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A113,1),INDEX(LinMotor!$AI$1:$AI$1355,A113,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A113,1),INDEX(LinMotor!$AI$1:$AI$1355,A113,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A113,1),INDEX(LinMotor!$AI$1:$AI$1355,A113,1))/1000,\"0.0k\")),\"\")","v":23.026196873630557},{"$f":"IF(A113<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A113,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A113,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A113,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A113,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A113,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A113,1))/1000,\"0.0k\")),\"\")","v":2.4089022633907784},{"$f":"IF(A113<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A113,1),INDEX(LinMotor!$AK$1:$AK$1355,A113,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A113,1),INDEX(LinMotor!$AK$1:$AK$1355,A113,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A113,1),INDEX(LinMotor!$AK$1:$AK$1355,A113,1))/1000,\"0.0k\")),\"\")","v":147.56756828327212},""]
[41,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A114,1),INDEX(LinMotor!$B$1:$B$1341,A114,1))","v":"AKM32H"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A114,1),INDEX(LinMotor!$R$1:$R$1355,A114,1))","v":1906.7796610169489},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A114,1),INDEX(LinMotor!$S$1:$S$1355,A114,1))","v":4.724478881578662},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A114,1),INDEX(LinMotor!$T$1:$T$1355,A114,1))","v":4.0086597549311298},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A114,1),INDEX(LinMotor!$U$1:$U$1355,A114,1))","v":2.7558205413893894E-2},{"$f":"IF(A114<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A114,1),INDEX(LinMotor!$V$1:$V$1355,A114,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A114,1),INDEX(LinMotor!$V$1:$V$1355,A114,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A114,1),INDEX(LinMotor!$V$1:$V$1355,A114,1))/1000,\"0.0k\")),\"\")","v":-22.52206150716049},{"$f":"IF(A114<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A114,1),INDEX(LinMotor!$W$1:$W$1355,A114,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A114,1),INDEX(LinMotor!$X$1:$X$1355,A114,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A114,1),INDEX(LinMotor!$W$1:$W$1355,A114,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A114,1),INDEX(LinMotor!$X$1:$X$1355,A114,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A114,1),INDEX(LinMotor!$W$1:$W$1355,A114,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A114,1),INDEX(LinMotor!$X$1:$X$1355,A114,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A114<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A114,1),INDEX(LinMotor!$X$1:$X$1355,A114,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A114,1),INDEX(LinMotor!$Z$1:$Z$1355,A114,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A114,1),INDEX(LinMotor!$X$1:$X$1355,A114,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A114,1),INDEX(LinMotor!$Z$1:$Z$1355,A114,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A114,1),INDEX(LinMotor!$X$1:$X$1355,A114,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A114,1),INDEX(LinMotor!$Z$1:$Z$1355,A114,1)))/1000,\"0.0k\")),\"\")","v":29.102869820800002},{"$f":"IF(A114<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A114,1),INDEX(LinMotor!$Y$1:$Y$1355,A114,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A114,1),INDEX(LinMotor!$AB$1:$AB$445,A114,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A114,1),INDEX(LinMotor!$Y$1:$Y$1355,A114,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A114,1),INDEX(LinMotor!$AB$1:$AB$445,A114,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A114,1),INDEX(LinMotor!$Y$1:$Y$1355,A114,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A114,1),INDEX(LinMotor!$AB$1:$AB$445,A114,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A114,1),INDEX(LinMotor!$AD$1:$AD$1355,A114,1))","v":1.0816309413009491},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A114,1),INDEX(LinMotor!$AE$1:$AE$1355,A114,1))","v":1.5879542064920635},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A114,1),INDEX(LinMotor!$AF$1:$AF$1355,A114,1))","v":25.959142591222776},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A114,1),INDEX(LinMotor!$AG$1:$AG$1355,A114,1))","v":76.221801911619053},{"$f":"IF(A114<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A114,1),INDEX(LinMotor!$AI$1:$AI$1355,A114,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A114,1),INDEX(LinMotor!$AI$1:$AI$1355,A114,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A114,1),INDEX(LinMotor!$AI$1:$AI$1355,A114,1))/1000,\"0.0k\")),\"\")","v":23.026196873630557},{"$f":"IF(A114<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A114,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A114,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A114,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A114,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A114,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A114,1))/1000,\"0.0k\")),\"\")","v":2.4089022633907784},{"$f":"IF(A114<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A114,1),INDEX(LinMotor!$AK$1:$AK$1355,A114,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A114,1),INDEX(LinMotor!$AK$1:$AK$1355,A114,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A114,1),INDEX(LinMotor!$AK$1:$AK$1355,A114,1))/1000,\"0.0k\")),\"\")","v":147.56756828327212},""]
[42,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A115,1),INDEX(LinMotor!$B$1:$B$1341,A115,1))","v":"AKM33C"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A115,1),INDEX(LinMotor!$R$1:$R$1355,A115,1))","v":1323.5294117647059},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A115,1),INDEX(LinMotor!$S$1:$S$1355,A115,1))","v":3.6601583308087662},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A115,1),INDEX(LinMotor!$T$1:$T$1355,A115,1))","v":2.9823981918032789},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A115,1),INDEX(LinMotor!$U$1:$U$1355,A115,1))","v":0.16794711874012208},{"$f":"IF(A115<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A115,1),INDEX(LinMotor!$V$1:$V$1355,A115,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A115,1),INDEX(LinMotor!$V$1:$V$1355,A115,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A115,1),INDEX(LinMotor!$V$1:$V$1355,A115,1))/1000,\"0.0k\")),\"\")","v":-22.528649817283949},{"$f":"IF(A115<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A115,1),INDEX(LinMotor!$W$1:$W$1355,A115,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A115,1),INDEX(LinMotor!$X$1:$X$1355,A115,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A115,1),INDEX(LinMotor!$W$1:$W$1355,A115,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A115,1),INDEX(LinMotor!$X$1:$X$1355,A115,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A115,1),INDEX(LinMotor!$W$1:$W$1355,A115,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A115,1),INDEX(LinMotor!$X$1:$X$1355,A115,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A115<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A115,1),INDEX(LinMotor!$X$1:$X$1355,A115,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A115,1),INDEX(LinMotor!$Z$1:$Z$1355,A115,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A115,1),INDEX(LinMotor!$X$1:$X$1355,A115,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A115,1),INDEX(LinMotor!$Z$1:$Z$1355,A115,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A115,1),INDEX(LinMotor!$X$1:$X$1355,A115,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A115,1),INDEX(LinMotor!$Z$1:$Z$1355,A115,1)))/1000,\"0.0k\")),\"\")","v":29.108206352},{"$f":"IF(A115<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A115,1),INDEX(LinMotor!$Y$1:$Y$1355,A115,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A115,1),INDEX(LinMotor!$AB$1:$AB$445,A115,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A115,1),INDEX(LinMotor!$Y$1:$Y$1355,A115,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A115,1),INDEX(LinMotor!$AB$1:$AB$445,A115,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A115,1),INDEX(LinMotor!$Y$1:$Y$1355,A115,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A115,1),INDEX(LinMotor!$AB$1:$AB$445,A115,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A115,1),INDEX(LinMotor!$AD$1:$AD$1355,A115,1))","v":0.22402869430002928},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A115,1),INDEX(LinMotor!$AE$1:$AE$1355,A115,1))","v":0.32894421384870848},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A115,1),INDEX(LinMotor!$AF$1:$AF$1355,A115,1))","v":5.3766886632007029},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A115,1),INDEX(LinMotor!$AG$1:$AG$1355,A115,1))","v":15.789322264738006},{"$f":"IF(A115<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A115,1),INDEX(LinMotor!$AI$1:$AI$1355,A115,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A115,1),INDEX(LinMotor!$AI$1:$AI$1355,A115,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A115,1),INDEX(LinMotor!$AI$1:$AI$1355,A115,1))/1000,\"0.0k\")),\"\")","v":23.027251796103748},{"$f":"IF(A115<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A115,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A115,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A115,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A115,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A115,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A115,1))/1000,\"0.0k\")),\"\")","v":2.4098151590720303},{"$f":"IF(A115<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A115,1),INDEX(LinMotor!$AK$1:$AK$1355,A115,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A115,1),INDEX(LinMotor!$AK$1:$AK$1355,A115,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A115,1),INDEX(LinMotor!$AK$1:$AK$1355,A115,1))/1000,\"0.0k\")),\"\")","v":147.62349159648659},""]
[43,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A116,1),INDEX(LinMotor!$B$1:$B$1341,A116,1))","v":"AKM33E"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A116,1),INDEX(LinMotor!$R$1:$R$1355,A116,1))","v":1323.5294117647059},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A116,1),INDEX(LinMotor!$S$1:$S$1355,A116,1))","v":3.5555609605773557},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A116,1),INDEX(LinMotor!$T$1:$T$1355,A116,1))","v":2.9225106779116463},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A116,1),INDEX(LinMotor!$U$1:$U$1355,A116,1))","v":6.4233802498316672E-2},{"$f":"IF(A116<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A116,1),INDEX(LinMotor!$V$1:$V$1355,A116,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A116,1),INDEX(LinMotor!$V$1:$V$1355,A116,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A116,1),INDEX(LinMotor!$V$1:$V$1355,A116,1))/1000,\"0.0k\")),\"\")","v":-22.528649817283949},{"$f":"IF(A116<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A116,1),INDEX(LinMotor!$W$1:$W$1355,A116,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A116,1),INDEX(LinMotor!$X$1:$X$1355,A116,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A116,1),INDEX(LinMotor!$W$1:$W$1355,A116,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A116,1),INDEX(LinMotor!$X$1:$X$1355,A116,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A116,1),INDEX(LinMotor!$W$1:$W$1355,A116,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A116,1),INDEX(LinMotor!$X$1:$X$1355,A116,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A116<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A116,1),INDEX(LinMotor!$X$1:$X$1355,A116,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A116,1),INDEX(LinMotor!$Z$1:$Z$1355,A116,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A116,1),INDEX(LinMotor!$X$1:$X$1355,A116,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A116,1),INDEX(LinMotor!$Z$1:$Z$1355,A116,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A116,1),INDEX(LinMotor!$X$1:$X$1355,A116,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A116,1),INDEX(LinMotor!$Z$1:$Z$1355,A116,1)))/1000,\"0.0k\")),\"\")","v":29.108206352},{"$f":"IF(A116<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A116,1),INDEX(LinMotor!$Y$1:$Y$1355,A116,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A116,1),INDEX(LinMotor!$AB$1:$AB$445,A116,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A116,1),INDEX(LinMotor!$Y$1:$Y$1355,A116,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A116,1),INDEX(LinMotor!$AB$1:$AB$445,A116,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A116,1),INDEX(LinMotor!$Y$1:$Y$1355,A116,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A116,1),INDEX(LinMotor!$AB$1:$AB$445,A116,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A116,1),INDEX(LinMotor!$AD$1:$AD$1355,A116,1))","v":0.38191886104575251},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A116,1),INDEX(LinMotor!$AE$1:$AE$1355,A116,1))","v":0.5607763768530466},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A116,1),INDEX(LinMotor!$AF$1:$AF$1355,A116,1))","v":9.1660526650980607},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A116,1),INDEX(LinMotor!$AG$1:$AG$1355,A116,1))","v":26.917266088946239},{"$f":"IF(A116<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A116,1),INDEX(LinMotor!$AI$1:$AI$1355,A116,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A116,1),INDEX(LinMotor!$AI$1:$AI$1355,A116,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A116,1),INDEX(LinMotor!$AI$1:$AI$1355,A116,1))/1000,\"0.0k\")),\"\")","v":23.027251796103748},{"$f":"IF(A116<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A116,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A116,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A116,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A116,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A116,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A116,1))/1000,\"0.0k\")),\"\")","v":2.4098151590720303},{"$f":"IF(A116<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A116,1),INDEX(LinMotor!$AK$1:$AK$1355,A116,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A116,1),INDEX(LinMotor!$AK$1:$AK$1355,A116,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A116,1),INDEX(LinMotor!$AK$1:$AK$1355,A116,1))/1000,\"0.0k\")),\"\")","v":147.62349159648659},""]
[44,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A117,1),INDEX(LinMotor!$B$1:$B$1341,A117,1))","v":"AKM33H"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A117,1),INDEX(LinMotor!$R$1:$R$1355,A117,1))","v":1323.5294117647059},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A117,1),INDEX(LinMotor!$S$1:$S$1355,A117,1))","v":3.4446537246952871},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A117,1),INDEX(LinMotor!$T$1:$T$1355,A117,1))","v":2.8481610911937376},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A117,1),INDEX(LinMotor!$U$1:$U$1355,A117,1))","v":2.5576114969695425E-2},{"$f":"IF(A117<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A117,1),INDEX(LinMotor!$V$1:$V$1355,A117,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A117,1),INDEX(LinMotor!$V$1:$V$1355,A117,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A117,1),INDEX(LinMotor!$V$1:$V$1355,A117,1))/1000,\"0.0k\")),\"\")","v":-22.528649817283949},{"$f":"IF(A117<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A117,1),INDEX(LinMotor!$W$1:$W$1355,A117,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A117,1),INDEX(LinMotor!$X$1:$X$1355,A117,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A117,1),INDEX(LinMotor!$W$1:$W$1355,A117,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A117,1),INDEX(LinMotor!$X$1:$X$1355,A117,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A117,1),INDEX(LinMotor!$W$1:$W$1355,A117,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A117,1),INDEX(LinMotor!$X$1:$X$1355,A117,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A117<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A117,1),INDEX(LinMotor!$X$1:$X$1355,A117,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A117,1),INDEX(LinMotor!$Z$1:$Z$1355,A117,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A117,1),INDEX(LinMotor!$X$1:$X$1355,A117,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A117,1),INDEX(LinMotor!$Z$1:$Z$1355,A117,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A117,1),INDEX(LinMotor!$X$1:$X$1355,A117,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A117,1),INDEX(LinMotor!$Z$1:$Z$1355,A117,1)))/1000,\"0.0k\")),\"\")","v":29.108206352},{"$f":"IF(A117<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A117,1),INDEX(LinMotor!$Y$1:$Y$1355,A117,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A117,1),INDEX(LinMotor!$AB$1:$AB$445,A117,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A117,1),INDEX(LinMotor!$Y$1:$Y$1355,A117,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A117,1),INDEX(LinMotor!$AB$1:$AB$445,A117,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A117,1),INDEX(LinMotor!$Y$1:$Y$1355,A117,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A117,1),INDEX(LinMotor!$AB$1:$AB$445,A117,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A117,1),INDEX(LinMotor!$AD$1:$AD$1355,A117,1))","v":0.80593391438215845},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A117,1),INDEX(LinMotor!$AE$1:$AE$1355,A117,1))","v":1.1833631343912037},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A117,1),INDEX(LinMotor!$AF$1:$AF$1355,A117,1))","v":19.342413945171803},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A117,1),INDEX(LinMotor!$AG$1:$AG$1355,A117,1))","v":56.801430450777772},{"$f":"IF(A117<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A117,1),INDEX(LinMotor!$AI$1:$AI$1355,A117,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A117,1),INDEX(LinMotor!$AI$1:$AI$1355,A117,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A117,1),INDEX(LinMotor!$AI$1:$AI$1355,A117,1))/1000,\"0.0k\")),\"\")","v":23.027251796103748},{"$f":"IF(A117<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A117,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A117,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A117,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A117,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A117,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A117,1))/1000,\"0.0k\")),\"\")","v":2.4098151590720303},{"$f":"IF(A117<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A117,1),INDEX(LinMotor!$AK$1:$AK$1355,A117,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A117,1),INDEX(LinMotor!$AK$1:$AK$1355,A117,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A117,1),INDEX(LinMotor!$AK$1:$AK$1355,A117,1))/1000,\"0.0k\")),\"\")","v":147.62349159648659},""]
[45,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A118,1),INDEX(LinMotor!$B$1:$B$1341,A118,1))","v":"AKM41C"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A118,1),INDEX(LinMotor!$R$1:$R$1355,A118,1))","v":1388.8888888888889},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A118,1),INDEX(LinMotor!$S$1:$S$1355,A118,1))","v":5.0865784087832777},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A118,1),INDEX(LinMotor!$T$1:$T$1355,A118,1))","v":4.7561087168627454},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A118,1),INDEX(LinMotor!$U$1:$U$1355,A118,1))","v":0.32184655974625809},{"$f":"IF(A118<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A118,1),INDEX(LinMotor!$V$1:$V$1355,A118,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A118,1),INDEX(LinMotor!$V$1:$V$1355,A118,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A118,1),INDEX(LinMotor!$V$1:$V$1355,A118,1))/1000,\"0.0k\")),\"\")","v":-22.52763623111111},{"$f":"IF(A118<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A118,1),INDEX(LinMotor!$W$1:$W$1355,A118,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A118,1),INDEX(LinMotor!$X$1:$X$1355,A118,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A118,1),INDEX(LinMotor!$W$1:$W$1355,A118,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A118,1),INDEX(LinMotor!$X$1:$X$1355,A118,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A118,1),INDEX(LinMotor!$W$1:$W$1355,A118,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A118,1),INDEX(LinMotor!$X$1:$X$1355,A118,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A118<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A118,1),INDEX(LinMotor!$X$1:$X$1355,A118,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A118,1),INDEX(LinMotor!$Z$1:$Z$1355,A118,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A118,1),INDEX(LinMotor!$X$1:$X$1355,A118,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A118,1),INDEX(LinMotor!$Z$1:$Z$1355,A118,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A118,1),INDEX(LinMotor!$X$1:$X$1355,A118,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A118,1),INDEX(LinMotor!$Z$1:$Z$1355,A118,1)))/1000,\"0.0k\")),\"\")","v":29.107385347200001},{"$f":"IF(A118<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A118,1),INDEX(LinMotor!$Y$1:$Y$1355,A118,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A118,1),INDEX(LinMotor!$AB$1:$AB$445,A118,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A118,1),INDEX(LinMotor!$Y$1:$Y$1355,A118,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A118,1),INDEX(LinMotor!$AB$1:$AB$445,A118,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A118,1),INDEX(LinMotor!$Y$1:$Y$1355,A118,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A118,1),INDEX(LinMotor!$AB$1:$AB$445,A118,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A118,1),INDEX(LinMotor!$AD$1:$AD$1355,A118,1))","v":0.30922228644673383},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A118,1),INDEX(LinMotor!$AE$1:$AE$1355,A118,1))","v":0.45402545520205129},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A118,1),INDEX(LinMotor!$AF$1:$AF$1355,A118,1))","v":7.4213348747216115},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A118,1),INDEX(LinMotor!$AG$1:$AG$1355,A118,1))","v":21.793221849698462},{"$f":"IF(A118<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A118,1),INDEX(LinMotor!$AI$1:$AI$1355,A118,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A118,1),INDEX(LinMotor!$AI$1:$AI$1355,A118,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A118,1),INDEX(LinMotor!$AI$1:$AI$1355,A118,1))/1000,\"0.0k\")),\"\")","v":23.027089487625755},{"$f":"IF(A118<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A118,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A118,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A118,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A118,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A118,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A118,1))/1000,\"0.0k\")),\"\")","v":2.4096747135826071},{"$f":"IF(A118<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A118,1),INDEX(LinMotor!$AK$1:$AK$1355,A118,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A118,1),INDEX(LinMotor!$AK$1:$AK$1355,A118,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A118,1),INDEX(LinMotor!$AK$1:$AK$1355,A118,1))/1000,\"0.0k\")),\"\")","v":147.61488800983821},""]
[46,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A119,1),INDEX(LinMotor!$B$1:$B$1341,A119,1))","v":"AKM41E"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A119,1),INDEX(LinMotor!$R$1:$R$1355,A119,1))","v":1388.8888888888889},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A119,1),INDEX(LinMotor!$S$1:$S$1355,A119,1))","v":4.9109142440019413},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A119,1),INDEX(LinMotor!$T$1:$T$1355,A119,1))","v":4.6349339724840766},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A119,1),INDEX(LinMotor!$U$1:$U$1355,A119,1))","v":9.8826916207097631E-2},{"$f":"IF(A119<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A119,1),INDEX(LinMotor!$V$1:$V$1355,A119,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A119,1),INDEX(LinMotor!$V$1:$V$1355,A119,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A119,1),INDEX(LinMotor!$V$1:$V$1355,A119,1))/1000,\"0.0k\")),\"\")","v":-22.52763623111111},{"$f":"IF(A119<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A119,1),INDEX(LinMotor!$W$1:$W$1355,A119,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A119,1),INDEX(LinMotor!$X$1:$X$1355,A119,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A119,1),INDEX(LinMotor!$W$1:$W$1355,A119,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A119,1),INDEX(LinMotor!$X$1:$X$1355,A119,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A119,1),INDEX(LinMotor!$W$1:$W$1355,A119,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A119,1),INDEX(LinMotor!$X$1:$X$1355,A119,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A119<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A119,1),INDEX(LinMotor!$X$1:$X$1355,A119,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A119,1),INDEX(LinMotor!$Z$1:$Z$1355,A119,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A119,1),INDEX(LinMotor!$X$1:$X$1355,A119,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A119,1),INDEX(LinMotor!$Z$1:$Z$1355,A119,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A119,1),INDEX(LinMotor!$X$1:$X$1355,A119,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A119,1),INDEX(LinMotor!$Z$1:$Z$1355,A119,1)))/1000,\"0.0k\")),\"\")","v":29.107385347200001},{"$f":"IF(A119<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A119,1),INDEX(LinMotor!$Y$1:$Y$1355,A119,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A119,1),INDEX(LinMotor!$AB$1:$AB$445,A119,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A119,1),INDEX(LinMotor!$Y$1:$Y$1355,A119,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A119,1),INDEX(LinMotor!$AB$1:$AB$445,A119,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A119,1),INDEX(LinMotor!$Y$1:$Y$1355,A119,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A119,1),INDEX(LinMotor!$AB$1:$AB$445,A119,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A119,1),INDEX(LinMotor!$AD$1:$AD$1355,A119,1))","v":0.5827013620397814},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A119,1),INDEX(LinMotor!$AE$1:$AE$1355,A119,1))","v":0.85556980445049513},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A119,1),INDEX(LinMotor!$AF$1:$AF$1355,A119,1))","v":13.984832688954754},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A119,1),INDEX(LinMotor!$AG$1:$AG$1355,A119,1))","v":41.067350613623766},{"$f":"IF(A119<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A119,1),INDEX(LinMotor!$AI$1:$AI$1355,A119,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A119,1),INDEX(LinMotor!$AI$1:$AI$1355,A119,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A119,1),INDEX(LinMotor!$AI$1:$AI$1355,A119,1))/1000,\"0.0k\")),\"\")","v":23.027089487625755},{"$f":"IF(A119<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A119,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A119,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A119,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A119,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A119,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A119,1))/1000,\"0.0k\")),\"\")","v":2.4096747135826071},{"$f":"IF(A119<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A119,1),INDEX(LinMotor!$AK$1:$AK$1355,A119,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A119,1),INDEX(LinMotor!$AK$1:$AK$1355,A119,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A119,1),INDEX(LinMotor!$AK$1:$AK$1355,A119,1))/1000,\"0.0k\")),\"\")","v":147.61488800983821},""]
[47,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A120,1),INDEX(LinMotor!$B$1:$B$1341,A120,1))","v":"AKM41H"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A120,1),INDEX(LinMotor!$R$1:$R$1355,A120,1))","v":1388.8888888888889},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A120,1),INDEX(LinMotor!$S$1:$S$1355,A120,1))","v":4.8154813136817607},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A120,1),INDEX(LinMotor!$T$1:$T$1355,A120,1))","v":4.5766329162264148},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A120,1),INDEX(LinMotor!$U$1:$U$1355,A120,1))","v":4.6820686894613987E-2},{"$f":"IF(A120<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A120,1),INDEX(LinMotor!$V$1:$V$1355,A120,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A120,1),INDEX(LinMotor!$V$1:$V$1355,A120,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A120,1),INDEX(LinMotor!$V$1:$V$1355,A120,1))/1000,\"0.0k\")),\"\")","v":-22.52763623111111},{"$f":"IF(A120<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A120,1),INDEX(LinMotor!$W$1:$W$1355,A120,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A120,1),INDEX(LinMotor!$X$1:$X$1355,A120,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A120,1),INDEX(LinMotor!$W$1:$W$1355,A120,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A120,1),INDEX(LinMotor!$X$1:$X$1355,A120,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A120,1),INDEX(LinMotor!$W$1:$W$1355,A120,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A120,1),INDEX(LinMotor!$X$1:$X$1355,A120,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A120<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A120,1),INDEX(LinMotor!$X$1:$X$1355,A120,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A120,1),INDEX(LinMotor!$Z$1:$Z$1355,A120,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A120,1),INDEX(LinMotor!$X$1:$X$1355,A120,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A120,1),INDEX(LinMotor!$Z$1:$Z$1355,A120,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A120,1),INDEX(LinMotor!$X$1:$X$1355,A120,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A120,1),INDEX(LinMotor!$Z$1:$Z$1355,A120,1)))/1000,\"0.0k\")),\"\")","v":29.107385347200001},{"$f":"IF(A120<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A120,1),INDEX(LinMotor!$Y$1:$Y$1355,A120,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A120,1),INDEX(LinMotor!$AB$1:$AB$445,A120,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A120,1),INDEX(LinMotor!$Y$1:$Y$1355,A120,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A120,1),INDEX(LinMotor!$AB$1:$AB$445,A120,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A120,1),INDEX(LinMotor!$Y$1:$Y$1355,A120,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A120,1),INDEX(LinMotor!$AB$1:$AB$445,A120,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A120,1),INDEX(LinMotor!$AD$1:$AD$1355,A120,1))","v":1.1227248862875159},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A120,1),INDEX(LinMotor!$AE$1:$AE$1355,A120,1))","v":1.6484765164271844},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A120,1),INDEX(LinMotor!$AF$1:$AF$1355,A120,1))","v":26.945397270900383},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A120,1),INDEX(LinMotor!$AG$1:$AG$1355,A120,1))","v":79.126872788504855},{"$f":"IF(A120<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A120,1),INDEX(LinMotor!$AI$1:$AI$1355,A120,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A120,1),INDEX(LinMotor!$AI$1:$AI$1355,A120,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A120,1),INDEX(LinMotor!$AI$1:$AI$1355,A120,1))/1000,\"0.0k\")),\"\")","v":23.027089487625755},{"$f":"IF(A120<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A120,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A120,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A120,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A120,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A120,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A120,1))/1000,\"0.0k\")),\"\")","v":2.4096747135826071},{"$f":"IF(A120<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A120,1),INDEX(LinMotor!$AK$1:$AK$1355,A120,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A120,1),INDEX(LinMotor!$AK$1:$AK$1355,A120,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A120,1),INDEX(LinMotor!$AK$1:$AK$1355,A120,1))/1000,\"0.0k\")),\"\")","v":147.61488800983821},""]
[48,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A121,1),INDEX(LinMotor!$B$1:$B$1341,A121,1))","v":"AKM42C"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A121,1),INDEX(LinMotor!$R$1:$R$1355,A121,1))","v":750},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A121,1),INDEX(LinMotor!$S$1:$S$1355,A121,1))","v":2.9624526787672174},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A121,1),INDEX(LinMotor!$T$1:$T$1355,A121,1))","v":2.5771281132743362},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A121,1),INDEX(LinMotor!$U$1:$U$1355,A121,1))","v":0.21287120469470461},{"$f":"IF(A121<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A121,1),INDEX(LinMotor!$V$1:$V$1355,A121,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A121,1),INDEX(LinMotor!$V$1:$V$1355,A121,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A121,1),INDEX(LinMotor!$V$1:$V$1355,A121,1))/1000,\"0.0k\")),\"\")","v":-22.545120592592593},{"$f":"IF(A121<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A121,1),INDEX(LinMotor!$W$1:$W$1355,A121,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A121,1),INDEX(LinMotor!$X$1:$X$1355,A121,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A121,1),INDEX(LinMotor!$W$1:$W$1355,A121,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A121,1),INDEX(LinMotor!$X$1:$X$1355,A121,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A121,1),INDEX(LinMotor!$W$1:$W$1355,A121,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A121,1),INDEX(LinMotor!$X$1:$X$1355,A121,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A121<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A121,1),INDEX(LinMotor!$X$1:$X$1355,A121,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A121,1),INDEX(LinMotor!$Z$1:$Z$1355,A121,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A121,1),INDEX(LinMotor!$X$1:$X$1355,A121,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A121,1),INDEX(LinMotor!$Z$1:$Z$1355,A121,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A121,1),INDEX(LinMotor!$X$1:$X$1355,A121,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A121,1),INDEX(LinMotor!$Z$1:$Z$1355,A121,1)))/1000,\"0.0k\")),\"\")","v":29.121547680000003},{"$f":"IF(A121<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A121,1),INDEX(LinMotor!$Y$1:$Y$1355,A121,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A121,1),INDEX(LinMotor!$AB$1:$AB$445,A121,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A121,1),INDEX(LinMotor!$Y$1:$Y$1355,A121,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A121,1),INDEX(LinMotor!$AB$1:$AB$445,A121,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A121,1),INDEX(LinMotor!$Y$1:$Y$1355,A121,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A121,1),INDEX(LinMotor!$AB$1:$AB$445,A121,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A121,1),INDEX(LinMotor!$AD$1:$AD$1355,A121,1))","v":0.17261899563494731},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A121,1),INDEX(LinMotor!$AE$1:$AE$1355,A121,1))","v":0.25354581313432834},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A121,1),INDEX(LinMotor!$AF$1:$AF$1355,A121,1))","v":4.1428558952387355},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A121,1),INDEX(LinMotor!$AG$1:$AG$1355,A121,1))","v":12.17019903044776},{"$f":"IF(A121<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A121,1),INDEX(LinMotor!$AI$1:$AI$1355,A121,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A121,1),INDEX(LinMotor!$AI$1:$AI$1355,A121,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A121,1),INDEX(LinMotor!$AI$1:$AI$1355,A121,1))/1000,\"0.0k\")),\"\")","v":23.029889956690972},{"$f":"IF(A121<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A121,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A121,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A121,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A121,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A121,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A121,1))/1000,\"0.0k\")),\"\")","v":2.4120973982751583},{"$f":"IF(A121<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A121,1),INDEX(LinMotor!$AK$1:$AK$1355,A121,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A121,1),INDEX(LinMotor!$AK$1:$AK$1355,A121,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A121,1),INDEX(LinMotor!$AK$1:$AK$1355,A121,1))/1000,\"0.0k\")),\"\")","v":147.76329987952266},""]
[49,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A122,1),INDEX(LinMotor!$B$1:$B$1341,A122,1))","v":"AKM42E"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A122,1),INDEX(LinMotor!$R$1:$R$1355,A122,1))","v":750},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A122,1),INDEX(LinMotor!$S$1:$S$1355,A122,1))","v":2.9018956372137579},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A122,1),INDEX(LinMotor!$T$1:$T$1355,A122,1))","v":2.5771281132743362},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A122,1),INDEX(LinMotor!$U$1:$U$1355,A122,1))","v":8.5201507422024356E-2},{"$f":"IF(A122<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A122,1),INDEX(LinMotor!$V$1:$V$1355,A122,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A122,1),INDEX(LinMotor!$V$1:$V$1355,A122,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A122,1),INDEX(LinMotor!$V$1:$V$1355,A122,1))/1000,\"0.0k\")),\"\")","v":-22.545120592592593},{"$f":"IF(A122<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A122,1),INDEX(LinMotor!$W$1:$W$1355,A122,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A122,1),INDEX(LinMotor!$X$1:$X$1355,A122,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A122,1),INDEX(LinMotor!$W$1:$W$1355,A122,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A122,1),INDEX(LinMotor!$X$1:$X$1355,A122,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A122,1),INDEX(LinMotor!$W$1:$W$1355,A122,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A122,1),INDEX(LinMotor!$X$1:$X$1355,A122,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A122<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A122,1),INDEX(LinMotor!$X$1:$X$1355,A122,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A122,1),INDEX(LinMotor!$Z$1:$Z$1355,A122,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A122,1),INDEX(LinMotor!$X$1:$X$1355,A122,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A122,1),INDEX(LinMotor!$Z$1:$Z$1355,A122,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A122,1),INDEX(LinMotor!$X$1:$X$1355,A122,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A122,1),INDEX(LinMotor!$Z$1:$Z$1355,A122,1)))/1000,\"0.0k\")),\"\")","v":29.121547680000003},{"$f":"IF(A122<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A122,1),INDEX(LinMotor!$Y$1:$Y$1355,A122,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A122,1),INDEX(LinMotor!$AB$1:$AB$445,A122,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A122,1),INDEX(LinMotor!$Y$1:$Y$1355,A122,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A122,1),INDEX(LinMotor!$AB$1:$AB$445,A122,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A122,1),INDEX(LinMotor!$Y$1:$Y$1355,A122,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A122,1),INDEX(LinMotor!$AB$1:$AB$445,A122,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A122,1),INDEX(LinMotor!$AD$1:$AD$1355,A122,1))","v":0.33092517981060604},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A122,1),INDEX(LinMotor!$AE$1:$AE$1355,A122,1))","v":0.48606871736842111},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A122,1),INDEX(LinMotor!$AF$1:$AF$1355,A122,1))","v":7.9422043154545454},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A122,1),INDEX(LinMotor!$AG$1:$AG$1355,A122,1))","v":23.331298433684214},{"$f":"IF(A122<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A122,1),INDEX(LinMotor!$AI$1:$AI$1355,A122,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A122,1),INDEX(LinMotor!$AI$1:$AI$1355,A122,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A122,1),INDEX(LinMotor!$AI$1:$AI$1355,A122,1))/1000,\"0.0k\")),\"\")","v":23.029889956690972},{"$f":"IF(A122<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A122,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A122,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A122,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A122,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A122,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A122,1))/1000,\"0.0k\")),\"\")","v":2.4120973982751583},{"$f":"IF(A122<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A122,1),INDEX(LinMotor!$AK$1:$AK$1355,A122,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A122,1),INDEX(LinMotor!$AK$1:$AK$1355,A122,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A122,1),INDEX(LinMotor!$AK$1:$AK$1355,A122,1))/1000,\"0.0k\")),\"\")","v":147.76329987952266},""]
[50,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A123,1),INDEX(LinMotor!$B$1:$B$1341,A123,1))","v":"AKM42G"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A123,1),INDEX(LinMotor!$R$1:$R$1355,A123,1))","v":750},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A123,1),INDEX(LinMotor!$S$1:$S$1355,A123,1))","v":2.8117650806901184},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A123,1),INDEX(LinMotor!$T$1:$T$1355,A123,1))","v":2.5323084939130438},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A123,1),INDEX(LinMotor!$U$1:$U$1355,A123,1))","v":4.6112993760136507E-2},{"$f":"IF(A123<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A123,1),INDEX(LinMotor!$V$1:$V$1355,A123,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A123,1),INDEX(LinMotor!$V$1:$V$1355,A123,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A123,1),INDEX(LinMotor!$V$1:$V$1355,A123,1))/1000,\"0.0k\")),\"\")","v":-22.545120592592593},{"$f":"IF(A123<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A123,1),INDEX(LinMotor!$W$1:$W$1355,A123,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A123,1),INDEX(LinMotor!$X$1:$X$1355,A123,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A123,1),INDEX(LinMotor!$W$1:$W$1355,A123,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A123,1),INDEX(LinMotor!$X$1:$X$1355,A123,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A123,1),INDEX(LinMotor!$W$1:$W$1355,A123,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A123,1),INDEX(LinMotor!$X$1:$X$1355,A123,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A123<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A123,1),INDEX(LinMotor!$X$1:$X$1355,A123,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A123,1),INDEX(LinMotor!$Z$1:$Z$1355,A123,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A123,1),INDEX(LinMotor!$X$1:$X$1355,A123,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A123,1),INDEX(LinMotor!$Z$1:$Z$1355,A123,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A123,1),INDEX(LinMotor!$X$1:$X$1355,A123,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A123,1),INDEX(LinMotor!$Z$1:$Z$1355,A123,1)))/1000,\"0.0k\")),\"\")","v":29.121547680000003},{"$f":"IF(A123<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A123,1),INDEX(LinMotor!$Y$1:$Y$1355,A123,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A123,1),INDEX(LinMotor!$AB$1:$AB$445,A123,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A123,1),INDEX(LinMotor!$Y$1:$Y$1355,A123,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A123,1),INDEX(LinMotor!$AB$1:$AB$445,A123,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A123,1),INDEX(LinMotor!$Y$1:$Y$1355,A123,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A123,1),INDEX(LinMotor!$AB$1:$AB$445,A123,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A123,1),INDEX(LinMotor!$AD$1:$AD$1355,A123,1))","v":0.56165792185551466},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A123,1),INDEX(LinMotor!$AE$1:$AE$1355,A123,1))","v":0.82497302209631751},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A123,1),INDEX(LinMotor!$AF$1:$AF$1355,A123,1))","v":13.479790124532352},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A123,1),INDEX(LinMotor!$AG$1:$AG$1355,A123,1))","v":39.598705060623239},{"$f":"IF(A123<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A123,1),INDEX(LinMotor!$AI$1:$AI$1355,A123,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A123,1),INDEX(LinMotor!$AI$1:$AI$1355,A123,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A123,1),INDEX(LinMotor!$AI$1:$AI$1355,A123,1))/1000,\"0.0k\")),\"\")","v":23.029889956690972},{"$f":"IF(A123<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A123,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A123,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A123,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A123,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A123,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A123,1))/1000,\"0.0k\")),\"\")","v":2.4120973982751583},{"$f":"IF(A123<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A123,1),INDEX(LinMotor!$AK$1:$AK$1355,A123,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A123,1),INDEX(LinMotor!$AK$1:$AK$1355,A123,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A123,1),INDEX(LinMotor!$AK$1:$AK$1355,A123,1))/1000,\"0.0k\")),\"\")","v":147.76329987952266},""]
[51,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A124,1),INDEX(LinMotor!$B$1:$B$1341,A124,1))","v":"AKM42H"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A124,1),INDEX(LinMotor!$R$1:$R$1355,A124,1))","v":750},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A124,1),INDEX(LinMotor!$S$1:$S$1355,A124,1))","v":2.8035583296034061},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A124,1),INDEX(LinMotor!$T$1:$T$1355,A124,1))","v":2.5323084939130438},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A124,1),INDEX(LinMotor!$U$1:$U$1355,A124,1))","v":3.7025451580734392E-2},{"$f":"IF(A124<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A124,1),INDEX(LinMotor!$V$1:$V$1355,A124,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A124,1),INDEX(LinMotor!$V$1:$V$1355,A124,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A124,1),INDEX(LinMotor!$V$1:$V$1355,A124,1))/1000,\"0.0k\")),\"\")","v":-22.545120592592593},{"$f":"IF(A124<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A124,1),INDEX(LinMotor!$W$1:$W$1355,A124,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A124,1),INDEX(LinMotor!$X$1:$X$1355,A124,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A124,1),INDEX(LinMotor!$W$1:$W$1355,A124,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A124,1),INDEX(LinMotor!$X$1:$X$1355,A124,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A124,1),INDEX(LinMotor!$W$1:$W$1355,A124,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A124,1),INDEX(LinMotor!$X$1:$X$1355,A124,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A124<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A124,1),INDEX(LinMotor!$X$1:$X$1355,A124,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A124,1),INDEX(LinMotor!$Z$1:$Z$1355,A124,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A124,1),INDEX(LinMotor!$X$1:$X$1355,A124,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A124,1),INDEX(LinMotor!$Z$1:$Z$1355,A124,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A124,1),INDEX(LinMotor!$X$1:$X$1355,A124,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A124,1),INDEX(LinMotor!$Z$1:$Z$1355,A124,1)))/1000,\"0.0k\")),\"\")","v":29.121547680000003},{"$f":"IF(A124<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A124,1),INDEX(LinMotor!$Y$1:$Y$1355,A124,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A124,1),INDEX(LinMotor!$AB$1:$AB$445,A124,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A124,1),INDEX(LinMotor!$Y$1:$Y$1355,A124,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A124,1),INDEX(LinMotor!$AB$1:$AB$445,A124,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A124,1),INDEX(LinMotor!$Y$1:$Y$1355,A124,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A124,1),INDEX(LinMotor!$AB$1:$AB$445,A124,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A124,1),INDEX(LinMotor!$AD$1:$AD$1355,A124,1))","v":0.70008914694560975},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A124,1),INDEX(LinMotor!$AE$1:$AE$1355,A124,1))","v":1.0283032372881358},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A124,1),INDEX(LinMotor!$AF$1:$AF$1355,A124,1))","v":16.802139526694635},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A124,1),INDEX(LinMotor!$AG$1:$AG$1355,A124,1))","v":49.358555389830514},{"$f":"IF(A124<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A124,1),INDEX(LinMotor!$AI$1:$AI$1355,A124,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A124,1),INDEX(LinMotor!$AI$1:$AI$1355,A124,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A124,1),INDEX(LinMotor!$AI$1:$AI$1355,A124,1))/1000,\"0.0k\")),\"\")","v":23.029889956690972},{"$f":"IF(A124<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A124,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A124,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A124,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A124,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A124,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A124,1))/1000,\"0.0k\")),\"\")","v":2.4120973982751583},{"$f":"IF(A124<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A124,1),INDEX(LinMotor!$AK$1:$AK$1355,A124,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A124,1),INDEX(LinMotor!$AK$1:$AK$1355,A124,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A124,1),INDEX(LinMotor!$AK$1:$AK$1355,A124,1))/1000,\"0.0k\")),\"\")","v":147.76329987952266},""]
[52,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A125,1),INDEX(LinMotor!$B$1:$B$1341,A125,1))","v":"AKM42J"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A125,1),INDEX(LinMotor!$R$1:$R$1355,A125,1))","v":750},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A125,1),INDEX(LinMotor!$S$1:$S$1355,A125,1))","v":2.7880413546225484},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A125,1),INDEX(LinMotor!$T$1:$T$1355,A125,1))","v":2.5104782482758625},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A125,1),INDEX(LinMotor!$U$1:$U$1355,A125,1))","v":2.6073705548603249E-2},{"$f":"IF(A125<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A125,1),INDEX(LinMotor!$V$1:$V$1355,A125,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A125,1),INDEX(LinMotor!$V$1:$V$1355,A125,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A125,1),INDEX(LinMotor!$V$1:$V$1355,A125,1))/1000,\"0.0k\")),\"\")","v":-22.545120592592593},{"$f":"IF(A125<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A125,1),INDEX(LinMotor!$W$1:$W$1355,A125,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A125,1),INDEX(LinMotor!$X$1:$X$1355,A125,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A125,1),INDEX(LinMotor!$W$1:$W$1355,A125,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A125,1),INDEX(LinMotor!$X$1:$X$1355,A125,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A125,1),INDEX(LinMotor!$W$1:$W$1355,A125,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A125,1),INDEX(LinMotor!$X$1:$X$1355,A125,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A125<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A125,1),INDEX(LinMotor!$X$1:$X$1355,A125,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A125,1),INDEX(LinMotor!$Z$1:$Z$1355,A125,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A125,1),INDEX(LinMotor!$X$1:$X$1355,A125,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A125,1),INDEX(LinMotor!$Z$1:$Z$1355,A125,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A125,1),INDEX(LinMotor!$X$1:$X$1355,A125,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A125,1),INDEX(LinMotor!$Z$1:$Z$1355,A125,1)))/1000,\"0.0k\")),\"\")","v":29.121547680000003},{"$f":"IF(A125<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A125,1),INDEX(LinMotor!$Y$1:$Y$1355,A125,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A125,1),INDEX(LinMotor!$AB$1:$AB$445,A125,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A125,1),INDEX(LinMotor!$Y$1:$Y$1355,A125,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A125,1),INDEX(LinMotor!$AB$1:$AB$445,A125,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A125,1),INDEX(LinMotor!$Y$1:$Y$1355,A125,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A125,1),INDEX(LinMotor!$AB$1:$AB$445,A125,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A125,1),INDEX(LinMotor!$AD$1:$AD$1355,A125,1))","v":0.9746184865905736},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A125,1),INDEX(LinMotor!$AE$1:$AE$1355,A125,1))","v":1.4315367539325843},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A125,1),INDEX(LinMotor!$AF$1:$AF$1355,A125,1))","v":23.390843678173766},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A125,1),INDEX(LinMotor!$AG$1:$AG$1355,A125,1))","v":68.713764188764046},{"$f":"IF(A125<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A125,1),INDEX(LinMotor!$AI$1:$AI$1355,A125,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A125,1),INDEX(LinMotor!$AI$1:$AI$1355,A125,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A125,1),INDEX(LinMotor!$AI$1:$AI$1355,A125,1))/1000,\"0.0k\")),\"\")","v":23.029889956690972},{"$f":"IF(A125<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A125,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A125,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A125,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A125,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A125,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A125,1))/1000,\"0.0k\")),\"\")","v":2.4120973982751583},{"$f":"IF(A125<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A125,1),INDEX(LinMotor!$AK$1:$AK$1355,A125,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A125,1),INDEX(LinMotor!$AK$1:$AK$1355,A125,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A125,1),INDEX(LinMotor!$AK$1:$AK$1355,A125,1))/1000,\"0.0k\")),\"\")","v":147.76329987952266},""]
[53,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A126,1),INDEX(LinMotor!$B$1:$B$1341,A126,1))","v":"AKM43E"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A126,1),INDEX(LinMotor!$R$1:$R$1355,A126,1))","v":535.71428571428578},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A126,1),INDEX(LinMotor!$S$1:$S$1355,A126,1))","v":2.1125391671651603},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A126,1),INDEX(LinMotor!$T$1:$T$1355,A126,1))","v":1.8323184120754719},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A126,1),INDEX(LinMotor!$U$1:$U$1355,A126,1))","v":8.2386516264141604E-2},{"$f":"IF(A126<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A126,1),INDEX(LinMotor!$V$1:$V$1355,A126,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A126,1),INDEX(LinMotor!$V$1:$V$1355,A126,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A126,1),INDEX(LinMotor!$V$1:$V$1355,A126,1))/1000,\"0.0k\")),\"\")","v":-22.560324385185183},{"$f":"IF(A126<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A126,1),INDEX(LinMotor!$W$1:$W$1355,A126,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A126,1),INDEX(LinMotor!$X$1:$X$1355,A126,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A126,1),INDEX(LinMotor!$W$1:$W$1355,A126,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A126,1),INDEX(LinMotor!$X$1:$X$1355,A126,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A126,1),INDEX(LinMotor!$W$1:$W$1355,A126,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A126,1),INDEX(LinMotor!$X$1:$X$1355,A126,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A126<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A126,1),INDEX(LinMotor!$X$1:$X$1355,A126,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A126,1),INDEX(LinMotor!$Z$1:$Z$1355,A126,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A126,1),INDEX(LinMotor!$X$1:$X$1355,A126,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A126,1),INDEX(LinMotor!$Z$1:$Z$1355,A126,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A126,1),INDEX(LinMotor!$X$1:$X$1355,A126,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A126,1),INDEX(LinMotor!$Z$1:$Z$1355,A126,1)))/1000,\"0.0k\")),\"\")","v":29.133862752000002},{"$f":"IF(A126<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A126,1),INDEX(LinMotor!$Y$1:$Y$1355,A126,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A126,1),INDEX(LinMotor!$AB$1:$AB$445,A126,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A126,1),INDEX(LinMotor!$Y$1:$Y$1355,A126,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A126,1),INDEX(LinMotor!$AB$1:$AB$445,A126,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A126,1),INDEX(LinMotor!$Y$1:$Y$1355,A126,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A126,1),INDEX(LinMotor!$AB$1:$AB$445,A126,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A126,1),INDEX(LinMotor!$AD$1:$AD$1355,A126,1))","v":0.24258420616354884},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A126,1),INDEX(LinMotor!$AE$1:$AE$1355,A126,1))","v":0.35642491664680848},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A126,1),INDEX(LinMotor!$AF$1:$AF$1355,A126,1))","v":5.8220209479251723},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A126,1),INDEX(LinMotor!$AG$1:$AG$1355,A126,1))","v":17.108395999046806},{"$f":"IF(A126<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A126,1),INDEX(LinMotor!$AI$1:$AI$1355,A126,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A126,1),INDEX(LinMotor!$AI$1:$AI$1355,A126,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A126,1),INDEX(LinMotor!$AI$1:$AI$1355,A126,1))/1000,\"0.0k\")),\"\")","v":23.032326264912953},{"$f":"IF(A126<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A126,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A126,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A126,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A126,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A126,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A126,1))/1000,\"0.0k\")),\"\")","v":2.414204080616507},{"$f":"IF(A126<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A126,1),INDEX(LinMotor!$AK$1:$AK$1355,A126,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A126,1),INDEX(LinMotor!$AK$1:$AK$1355,A126,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A126,1),INDEX(LinMotor!$AK$1:$AK$1355,A126,1))/1000,\"0.0k\")),\"\")","v":147.89235367924826},""]
[54,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A127,1),INDEX(LinMotor!$B$1:$B$1341,A127,1))","v":"AKM43G"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A127,1),INDEX(LinMotor!$R$1:$R$1355,A127,1))","v":535.71428571428578},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A127,1),INDEX(LinMotor!$S$1:$S$1355,A127,1))","v":2.0689048915774868},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A127,1),INDEX(LinMotor!$T$1:$T$1355,A127,1))","v":1.8095566926708075},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A127,1),INDEX(LinMotor!$U$1:$U$1355,A127,1))","v":4.3990370629987764E-2},{"$f":"IF(A127<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A127,1),INDEX(LinMotor!$V$1:$V$1355,A127,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A127,1),INDEX(LinMotor!$V$1:$V$1355,A127,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A127,1),INDEX(LinMotor!$V$1:$V$1355,A127,1))/1000,\"0.0k\")),\"\")","v":-22.560324385185183},{"$f":"IF(A127<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A127,1),INDEX(LinMotor!$W$1:$W$1355,A127,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A127,1),INDEX(LinMotor!$X$1:$X$1355,A127,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A127,1),INDEX(LinMotor!$W$1:$W$1355,A127,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A127,1),INDEX(LinMotor!$X$1:$X$1355,A127,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A127,1),INDEX(LinMotor!$W$1:$W$1355,A127,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A127,1),INDEX(LinMotor!$X$1:$X$1355,A127,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A127<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A127,1),INDEX(LinMotor!$X$1:$X$1355,A127,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A127,1),INDEX(LinMotor!$Z$1:$Z$1355,A127,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A127,1),INDEX(LinMotor!$X$1:$X$1355,A127,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A127,1),INDEX(LinMotor!$Z$1:$Z$1355,A127,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A127,1),INDEX(LinMotor!$X$1:$X$1355,A127,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A127,1),INDEX(LinMotor!$Z$1:$Z$1355,A127,1)))/1000,\"0.0k\")),\"\")","v":29.133862752000002},{"$f":"IF(A127<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A127,1),INDEX(LinMotor!$Y$1:$Y$1355,A127,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A127,1),INDEX(LinMotor!$AB$1:$AB$445,A127,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A127,1),INDEX(LinMotor!$Y$1:$Y$1355,A127,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A127,1),INDEX(LinMotor!$AB$1:$AB$445,A127,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A127,1),INDEX(LinMotor!$Y$1:$Y$1355,A127,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A127,1),INDEX(LinMotor!$AB$1:$AB$445,A127,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A127,1),INDEX(LinMotor!$AD$1:$AD$1355,A127,1))","v":0.41912061404570283},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A127,1),INDEX(LinMotor!$AE$1:$AE$1355,A127,1))","v":0.61580690799583337},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A127,1),INDEX(LinMotor!$AF$1:$AF$1355,A127,1))","v":10.058894737096868},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A127,1),INDEX(LinMotor!$AG$1:$AG$1355,A127,1))","v":29.558731583800004},{"$f":"IF(A127<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A127,1),INDEX(LinMotor!$AI$1:$AI$1355,A127,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A127,1),INDEX(LinMotor!$AI$1:$AI$1355,A127,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A127,1),INDEX(LinMotor!$AI$1:$AI$1355,A127,1))/1000,\"0.0k\")),\"\")","v":23.032326264912953},{"$f":"IF(A127<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A127,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A127,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A127,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A127,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A127,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A127,1))/1000,\"0.0k\")),\"\")","v":2.414204080616507},{"$f":"IF(A127<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A127,1),INDEX(LinMotor!$AK$1:$AK$1355,A127,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A127,1),INDEX(LinMotor!$AK$1:$AK$1355,A127,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A127,1),INDEX(LinMotor!$AK$1:$AK$1355,A127,1))/1000,\"0.0k\")),\"\")","v":147.89235367924826},""]
[55,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A128,1),INDEX(LinMotor!$B$1:$B$1341,A128,1))","v":"AKM43H"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A128,1),INDEX(LinMotor!$R$1:$R$1355,A128,1))","v":535.71428571428578},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A128,1),INDEX(LinMotor!$S$1:$S$1355,A128,1))","v":2.0604517166797773},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A128,1),INDEX(LinMotor!$T$1:$T$1355,A128,1))","v":1.8095566926708075},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A128,1),INDEX(LinMotor!$U$1:$U$1355,A128,1))","v":3.3186907400500509E-2},{"$f":"IF(A128<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A128,1),INDEX(LinMotor!$V$1:$V$1355,A128,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A128,1),INDEX(LinMotor!$V$1:$V$1355,A128,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A128,1),INDEX(LinMotor!$V$1:$V$1355,A128,1))/1000,\"0.0k\")),\"\")","v":-22.560324385185183},{"$f":"IF(A128<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A128,1),INDEX(LinMotor!$W$1:$W$1355,A128,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A128,1),INDEX(LinMotor!$X$1:$X$1355,A128,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A128,1),INDEX(LinMotor!$W$1:$W$1355,A128,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A128,1),INDEX(LinMotor!$X$1:$X$1355,A128,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A128,1),INDEX(LinMotor!$W$1:$W$1355,A128,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A128,1),INDEX(LinMotor!$X$1:$X$1355,A128,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A128<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A128,1),INDEX(LinMotor!$X$1:$X$1355,A128,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A128,1),INDEX(LinMotor!$Z$1:$Z$1355,A128,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A128,1),INDEX(LinMotor!$X$1:$X$1355,A128,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A128,1),INDEX(LinMotor!$Z$1:$Z$1355,A128,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A128,1),INDEX(LinMotor!$X$1:$X$1355,A128,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A128,1),INDEX(LinMotor!$Z$1:$Z$1355,A128,1)))/1000,\"0.0k\")),\"\")","v":29.133862752000002},{"$f":"IF(A128<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A128,1),INDEX(LinMotor!$Y$1:$Y$1355,A128,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A128,1),INDEX(LinMotor!$AB$1:$AB$445,A128,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A128,1),INDEX(LinMotor!$Y$1:$Y$1355,A128,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A128,1),INDEX(LinMotor!$AB$1:$AB$445,A128,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A128,1),INDEX(LinMotor!$Y$1:$Y$1355,A128,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A128,1),INDEX(LinMotor!$AB$1:$AB$445,A128,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A128,1),INDEX(LinMotor!$AD$1:$AD$1355,A128,1))","v":0.46280497567734608},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A128,1),INDEX(LinMotor!$AE$1:$AE$1355,A128,1))","v":0.67999160987551877},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A128,1),INDEX(LinMotor!$AF$1:$AF$1355,A128,1))","v":11.107319416256306},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A128,1),INDEX(LinMotor!$AG$1:$AG$1355,A128,1))","v":32.639597274024901},{"$f":"IF(A128<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A128,1),INDEX(LinMotor!$AI$1:$AI$1355,A128,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A128,1),INDEX(LinMotor!$AI$1:$AI$1355,A128,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A128,1),INDEX(LinMotor!$AI$1:$AI$1355,A128,1))/1000,\"0.0k\")),\"\")","v":23.032326264912953},{"$f":"IF(A128<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A128,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A128,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A128,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A128,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A128,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A128,1))/1000,\"0.0k\")),\"\")","v":2.414204080616507},{"$f":"IF(A128<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A128,1),INDEX(LinMotor!$AK$1:$AK$1355,A128,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A128,1),INDEX(LinMotor!$AK$1:$AK$1355,A128,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A128,1),INDEX(LinMotor!$AK$1:$AK$1355,A128,1))/1000,\"0.0k\")),\"\")","v":147.89235367924826},""]
[56,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A129,1),INDEX(LinMotor!$B$1:$B$1341,A129,1))","v":"AKM43K"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A129,1),INDEX(LinMotor!$R$1:$R$1355,A129,1))","v":535.71428571428578},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A129,1),INDEX(LinMotor!$S$1:$S$1355,A129,1))","v":2.0268160116444611},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A129,1),INDEX(LinMotor!$T$1:$T$1355,A129,1))","v":1.7764550458536588},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A129,1),INDEX(LinMotor!$U$1:$U$1355,A129,1))","v":2.1978502778268481E-2},{"$f":"IF(A129<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A129,1),INDEX(LinMotor!$V$1:$V$1355,A129,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A129,1),INDEX(LinMotor!$V$1:$V$1355,A129,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A129,1),INDEX(LinMotor!$V$1:$V$1355,A129,1))/1000,\"0.0k\")),\"\")","v":-22.560324385185183},{"$f":"IF(A129<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A129,1),INDEX(LinMotor!$W$1:$W$1355,A129,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A129,1),INDEX(LinMotor!$X$1:$X$1355,A129,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A129,1),INDEX(LinMotor!$W$1:$W$1355,A129,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A129,1),INDEX(LinMotor!$X$1:$X$1355,A129,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A129,1),INDEX(LinMotor!$W$1:$W$1355,A129,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A129,1),INDEX(LinMotor!$X$1:$X$1355,A129,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A129<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A129,1),INDEX(LinMotor!$X$1:$X$1355,A129,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A129,1),INDEX(LinMotor!$Z$1:$Z$1355,A129,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A129,1),INDEX(LinMotor!$X$1:$X$1355,A129,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A129,1),INDEX(LinMotor!$Z$1:$Z$1355,A129,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A129,1),INDEX(LinMotor!$X$1:$X$1355,A129,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A129,1),INDEX(LinMotor!$Z$1:$Z$1355,A129,1)))/1000,\"0.0k\")),\"\")","v":29.133862752000002},{"$f":"IF(A129<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A129,1),INDEX(LinMotor!$Y$1:$Y$1355,A129,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A129,1),INDEX(LinMotor!$AB$1:$AB$445,A129,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A129,1),INDEX(LinMotor!$Y$1:$Y$1355,A129,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A129,1),INDEX(LinMotor!$AB$1:$AB$445,A129,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A129,1),INDEX(LinMotor!$Y$1:$Y$1355,A129,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A129,1),INDEX(LinMotor!$AB$1:$AB$445,A129,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A129,1),INDEX(LinMotor!$AD$1:$AD$1355,A129,1))","v":0.80933151302124562},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A129,1),INDEX(LinMotor!$AE$1:$AE$1355,A129,1))","v":1.1891372551836734},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A129,1),INDEX(LinMotor!$AF$1:$AF$1355,A129,1))","v":19.423956312509894},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A129,1),INDEX(LinMotor!$AG$1:$AG$1355,A129,1))","v":57.078588248816324},{"$f":"IF(A129<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A129,1),INDEX(LinMotor!$AI$1:$AI$1355,A129,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A129,1),INDEX(LinMotor!$AI$1:$AI$1355,A129,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A129,1),INDEX(LinMotor!$AI$1:$AI$1355,A129,1))/1000,\"0.0k\")),\"\")","v":23.032326264912953},{"$f":"IF(A129<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A129,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A129,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A129,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A129,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A129,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A129,1))/1000,\"0.0k\")),\"\")","v":2.414204080616507},{"$f":"IF(A129<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A129,1),INDEX(LinMotor!$AK$1:$AK$1355,A129,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A129,1),INDEX(LinMotor!$AK$1:$AK$1355,A129,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A129,1),INDEX(LinMotor!$AK$1:$AK$1355,A129,1))/1000,\"0.0k\")),\"\")","v":147.89235367924826},""]
[57,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A130,1),INDEX(LinMotor!$B$1:$B$1341,A130,1))","v":"AKM43L"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A130,1),INDEX(LinMotor!$R$1:$R$1355,A130,1))","v":535.71428571428578},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A130,1),INDEX(LinMotor!$S$1:$S$1355,A130,1))","v":2.099659930958667},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A130,1),INDEX(LinMotor!$T$1:$T$1355,A130,1))","v":1.8208664220000002},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A130,1),INDEX(LinMotor!$U$1:$U$1355,A130,1))","v":2.1220659078919377E-2},{"$f":"IF(A130<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A130,1),INDEX(LinMotor!$V$1:$V$1355,A130,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A130,1),INDEX(LinMotor!$V$1:$V$1355,A130,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A130,1),INDEX(LinMotor!$V$1:$V$1355,A130,1))/1000,\"0.0k\")),\"\")","v":-22.560324385185183},{"$f":"IF(A130<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A130,1),INDEX(LinMotor!$W$1:$W$1355,A130,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A130,1),INDEX(LinMotor!$X$1:$X$1355,A130,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A130,1),INDEX(LinMotor!$W$1:$W$1355,A130,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A130,1),INDEX(LinMotor!$X$1:$X$1355,A130,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A130,1),INDEX(LinMotor!$W$1:$W$1355,A130,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A130,1),INDEX(LinMotor!$X$1:$X$1355,A130,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A130<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A130,1),INDEX(LinMotor!$X$1:$X$1355,A130,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A130,1),INDEX(LinMotor!$Z$1:$Z$1355,A130,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A130,1),INDEX(LinMotor!$X$1:$X$1355,A130,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A130,1),INDEX(LinMotor!$Z$1:$Z$1355,A130,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A130,1),INDEX(LinMotor!$X$1:$X$1355,A130,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A130,1),INDEX(LinMotor!$Z$1:$Z$1355,A130,1)))/1000,\"0.0k\")),\"\")","v":29.133862752000002},{"$f":"IF(A130<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A130,1),INDEX(LinMotor!$Y$1:$Y$1355,A130,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A130,1),INDEX(LinMotor!$AB$1:$AB$445,A130,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A130,1),INDEX(LinMotor!$Y$1:$Y$1355,A130,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A130,1),INDEX(LinMotor!$AB$1:$AB$445,A130,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A130,1),INDEX(LinMotor!$Y$1:$Y$1355,A130,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A130,1),INDEX(LinMotor!$AB$1:$AB$445,A130,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A130,1),INDEX(LinMotor!$AD$1:$AD$1355,A130,1))","v":0.97815612743582525},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A130,1),INDEX(LinMotor!$AE$1:$AE$1355,A130,1))","v":1.4371884373784356},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A130,1),INDEX(LinMotor!$AF$1:$AF$1355,A130,1))","v":23.475747058459806},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A130,1),INDEX(LinMotor!$AG$1:$AG$1355,A130,1))","v":68.985044994164909},{"$f":"IF(A130<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A130,1),INDEX(LinMotor!$AI$1:$AI$1355,A130,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A130,1),INDEX(LinMotor!$AI$1:$AI$1355,A130,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A130,1),INDEX(LinMotor!$AI$1:$AI$1355,A130,1))/1000,\"0.0k\")),\"\")","v":23.032326264912953},{"$f":"IF(A130<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A130,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A130,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A130,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A130,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A130,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A130,1))/1000,\"0.0k\")),\"\")","v":2.414204080616507},{"$f":"IF(A130<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A130,1),INDEX(LinMotor!$AK$1:$AK$1355,A130,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A130,1),INDEX(LinMotor!$AK$1:$AK$1355,A130,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A130,1),INDEX(LinMotor!$AK$1:$AK$1355,A130,1))/1000,\"0.0k\")),\"\")","v":147.89235367924826},""]
[58,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A131,1),INDEX(LinMotor!$B$1:$B$1341,A131,1))","v":"AKM44E"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A131,1),INDEX(LinMotor!$R$1:$R$1355,A131,1))","v":416.66666666666663},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A131,1),INDEX(LinMotor!$S$1:$S$1355,A131,1))","v":1.7246052054937293},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A131,1),INDEX(LinMotor!$T$1:$T$1355,A131,1))","v":1.4646320514572866},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A131,1),INDEX(LinMotor!$U$1:$U$1355,A131,1))","v":8.0292549158861914E-2},{"$f":"IF(A131<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A131,1),INDEX(LinMotor!$V$1:$V$1355,A131,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A131,1),INDEX(LinMotor!$V$1:$V$1355,A131,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A131,1),INDEX(LinMotor!$V$1:$V$1355,A131,1))/1000,\"0.0k\")),\"\")","v":-22.575528177777777},{"$f":"IF(A131<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A131,1),INDEX(LinMotor!$W$1:$W$1355,A131,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A131,1),INDEX(LinMotor!$X$1:$X$1355,A131,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A131,1),INDEX(LinMotor!$W$1:$W$1355,A131,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A131,1),INDEX(LinMotor!$X$1:$X$1355,A131,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A131,1),INDEX(LinMotor!$W$1:$W$1355,A131,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A131,1),INDEX(LinMotor!$X$1:$X$1355,A131,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A131<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A131,1),INDEX(LinMotor!$X$1:$X$1355,A131,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A131,1),INDEX(LinMotor!$Z$1:$Z$1355,A131,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A131,1),INDEX(LinMotor!$X$1:$X$1355,A131,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A131,1),INDEX(LinMotor!$Z$1:$Z$1355,A131,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A131,1),INDEX(LinMotor!$X$1:$X$1355,A131,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A131,1),INDEX(LinMotor!$Z$1:$Z$1355,A131,1)))/1000,\"0.0k\")),\"\")","v":29.146177824000002},{"$f":"IF(A131<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A131,1),INDEX(LinMotor!$Y$1:$Y$1355,A131,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A131,1),INDEX(LinMotor!$AB$1:$AB$445,A131,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A131,1),INDEX(LinMotor!$Y$1:$Y$1355,A131,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A131,1),INDEX(LinMotor!$AB$1:$AB$445,A131,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A131,1),INDEX(LinMotor!$Y$1:$Y$1355,A131,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A131,1),INDEX(LinMotor!$AB$1:$AB$445,A131,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A131,1),INDEX(LinMotor!$AD$1:$AD$1355,A131,1))","v":0.20800451799394415},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A131,1),INDEX(LinMotor!$AE$1:$AE$1355,A131,1))","v":0.30571439413194446},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A131,1),INDEX(LinMotor!$AF$1:$AF$1355,A131,1))","v":4.9921084318546596},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A131,1),INDEX(LinMotor!$AG$1:$AG$1355,A131,1))","v":14.674290918333334},{"$f":"IF(A131<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A131,1),INDEX(LinMotor!$AI$1:$AI$1355,A131,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A131,1),INDEX(LinMotor!$AI$1:$AI$1355,A131,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A131,1),INDEX(LinMotor!$AI$1:$AI$1355,A131,1))/1000,\"0.0k\")),\"\")","v":23.034763612537809},{"$f":"IF(A131<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A131,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A131,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A131,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A131,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A131,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A131,1))/1000,\"0.0k\")),\"\")","v":2.4163107629578562},{"$f":"IF(A131<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A131,1),INDEX(LinMotor!$AK$1:$AK$1355,A131,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A131,1),INDEX(LinMotor!$AK$1:$AK$1355,A131,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A131,1),INDEX(LinMotor!$AK$1:$AK$1355,A131,1))/1000,\"0.0k\")),\"\")","v":148.02140747897386},""]
[59,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A132,1),INDEX(LinMotor!$B$1:$B$1341,A132,1))","v":"AKM44G"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A132,1),INDEX(LinMotor!$R$1:$R$1355,A132,1))","v":416.66666666666663},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A132,1),INDEX(LinMotor!$S$1:$S$1355,A132,1))","v":1.6896646659488996},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A132,1),INDEX(LinMotor!$T$1:$T$1355,A132,1))","v":1.4357723066009853},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A132,1),INDEX(LinMotor!$U$1:$U$1355,A132,1))","v":4.3156360932052426E-2},{"$f":"IF(A132<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A132,1),INDEX(LinMotor!$V$1:$V$1355,A132,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A132,1),INDEX(LinMotor!$V$1:$V$1355,A132,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A132,1),INDEX(LinMotor!$V$1:$V$1355,A132,1))/1000,\"0.0k\")),\"\")","v":-22.575528177777777},{"$f":"IF(A132<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A132,1),INDEX(LinMotor!$W$1:$W$1355,A132,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A132,1),INDEX(LinMotor!$X$1:$X$1355,A132,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A132,1),INDEX(LinMotor!$W$1:$W$1355,A132,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A132,1),INDEX(LinMotor!$X$1:$X$1355,A132,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A132,1),INDEX(LinMotor!$W$1:$W$1355,A132,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A132,1),INDEX(LinMotor!$X$1:$X$1355,A132,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A132<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A132,1),INDEX(LinMotor!$X$1:$X$1355,A132,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A132,1),INDEX(LinMotor!$Z$1:$Z$1355,A132,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A132,1),INDEX(LinMotor!$X$1:$X$1355,A132,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A132,1),INDEX(LinMotor!$Z$1:$Z$1355,A132,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A132,1),INDEX(LinMotor!$X$1:$X$1355,A132,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A132,1),INDEX(LinMotor!$Z$1:$Z$1355,A132,1)))/1000,\"0.0k\")),\"\")","v":29.146177824000002},{"$f":"IF(A132<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A132,1),INDEX(LinMotor!$Y$1:$Y$1355,A132,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A132,1),INDEX(LinMotor!$AB$1:$AB$445,A132,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A132,1),INDEX(LinMotor!$Y$1:$Y$1355,A132,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A132,1),INDEX(LinMotor!$AB$1:$AB$445,A132,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A132,1),INDEX(LinMotor!$Y$1:$Y$1355,A132,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A132,1),INDEX(LinMotor!$AB$1:$AB$445,A132,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A132,1),INDEX(LinMotor!$AD$1:$AD$1355,A132,1))","v":0.35130953074276278},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A132,1),INDEX(LinMotor!$AE$1:$AE$1355,A132,1))","v":0.51633676700680275},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A132,1),INDEX(LinMotor!$AF$1:$AF$1355,A132,1))","v":8.4314287378263071},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A132,1),INDEX(LinMotor!$AG$1:$AG$1355,A132,1))","v":24.784164816326534},{"$f":"IF(A132<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A132,1),INDEX(LinMotor!$AI$1:$AI$1355,A132,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A132,1),INDEX(LinMotor!$AI$1:$AI$1355,A132,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A132,1),INDEX(LinMotor!$AI$1:$AI$1355,A132,1))/1000,\"0.0k\")),\"\")","v":23.034763612537809},{"$f":"IF(A132<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A132,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A132,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A132,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A132,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A132,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A132,1))/1000,\"0.0k\")),\"\")","v":2.4163107629578562},{"$f":"IF(A132<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A132,1),INDEX(LinMotor!$AK$1:$AK$1355,A132,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A132,1),INDEX(LinMotor!$AK$1:$AK$1355,A132,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A132,1),INDEX(LinMotor!$AK$1:$AK$1355,A132,1))/1000,\"0.0k\")),\"\")","v":148.02140747897386},""]
[60,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A133,1),INDEX(LinMotor!$B$1:$B$1341,A133,1))","v":"AKM44H"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A133,1),INDEX(LinMotor!$R$1:$R$1355,A133,1))","v":416.66666666666663},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A133,1),INDEX(LinMotor!$S$1:$S$1355,A133,1))","v":1.6868538930719319},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A133,1),INDEX(LinMotor!$T$1:$T$1355,A133,1))","v":1.4428800902970298},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A133,1),INDEX(LinMotor!$U$1:$U$1355,A133,1))","v":3.805691760442087E-2},{"$f":"IF(A133<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A133,1),INDEX(LinMotor!$V$1:$V$1355,A133,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A133,1),INDEX(LinMotor!$V$1:$V$1355,A133,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A133,1),INDEX(LinMotor!$V$1:$V$1355,A133,1))/1000,\"0.0k\")),\"\")","v":-22.575528177777777},{"$f":"IF(A133<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A133,1),INDEX(LinMotor!$W$1:$W$1355,A133,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A133,1),INDEX(LinMotor!$X$1:$X$1355,A133,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A133,1),INDEX(LinMotor!$W$1:$W$1355,A133,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A133,1),INDEX(LinMotor!$X$1:$X$1355,A133,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A133,1),INDEX(LinMotor!$W$1:$W$1355,A133,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A133,1),INDEX(LinMotor!$X$1:$X$1355,A133,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A133<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A133,1),INDEX(LinMotor!$X$1:$X$1355,A133,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A133,1),INDEX(LinMotor!$Z$1:$Z$1355,A133,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A133,1),INDEX(LinMotor!$X$1:$X$1355,A133,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A133,1),INDEX(LinMotor!$Z$1:$Z$1355,A133,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A133,1),INDEX(LinMotor!$X$1:$X$1355,A133,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A133,1),INDEX(LinMotor!$Z$1:$Z$1355,A133,1)))/1000,\"0.0k\")),\"\")","v":29.146177824000002},{"$f":"IF(A133<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A133,1),INDEX(LinMotor!$Y$1:$Y$1355,A133,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A133,1),INDEX(LinMotor!$AB$1:$AB$445,A133,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A133,1),INDEX(LinMotor!$Y$1:$Y$1355,A133,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A133,1),INDEX(LinMotor!$AB$1:$AB$445,A133,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A133,1),INDEX(LinMotor!$Y$1:$Y$1355,A133,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A133,1),INDEX(LinMotor!$AB$1:$AB$445,A133,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A133,1),INDEX(LinMotor!$AD$1:$AD$1355,A133,1))","v":0.39279864951774851},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A133,1),INDEX(LinMotor!$AE$1:$AE$1355,A133,1))","v":0.57731535022071312},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A133,1),INDEX(LinMotor!$AF$1:$AF$1355,A133,1))","v":9.4271675884259647},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A133,1),INDEX(LinMotor!$AG$1:$AG$1355,A133,1))","v":27.71113681059423},{"$f":"IF(A133<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A133,1),INDEX(LinMotor!$AI$1:$AI$1355,A133,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A133,1),INDEX(LinMotor!$AI$1:$AI$1355,A133,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A133,1),INDEX(LinMotor!$AI$1:$AI$1355,A133,1))/1000,\"0.0k\")),\"\")","v":23.034763612537809},{"$f":"IF(A133<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A133,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A133,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A133,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A133,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A133,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A133,1))/1000,\"0.0k\")),\"\")","v":2.4163107629578562},{"$f":"IF(A133<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A133,1),INDEX(LinMotor!$AK$1:$AK$1355,A133,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A133,1),INDEX(LinMotor!$AK$1:$AK$1355,A133,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A133,1),INDEX(LinMotor!$AK$1:$AK$1355,A133,1))/1000,\"0.0k\")),\"\")","v":148.02140747897386},""]
[61,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A134,1),INDEX(LinMotor!$B$1:$B$1341,A134,1))","v":"AKM44J"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A134,1),INDEX(LinMotor!$R$1:$R$1355,A134,1))","v":416.66666666666663},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A134,1),INDEX(LinMotor!$S$1:$S$1355,A134,1))","v":1.6558765895884324},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A134,1),INDEX(LinMotor!$T$1:$T$1355,A134,1))","v":1.4287342070588238},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A134,1),INDEX(LinMotor!$U$1:$U$1355,A134,1))","v":2.391712460930492E-2},{"$f":"IF(A134<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A134,1),INDEX(LinMotor!$V$1:$V$1355,A134,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A134,1),INDEX(LinMotor!$V$1:$V$1355,A134,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A134,1),INDEX(LinMotor!$V$1:$V$1355,A134,1))/1000,\"0.0k\")),\"\")","v":-22.575528177777777},{"$f":"IF(A134<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A134,1),INDEX(LinMotor!$W$1:$W$1355,A134,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A134,1),INDEX(LinMotor!$X$1:$X$1355,A134,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A134,1),INDEX(LinMotor!$W$1:$W$1355,A134,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A134,1),INDEX(LinMotor!$X$1:$X$1355,A134,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A134,1),INDEX(LinMotor!$W$1:$W$1355,A134,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A134,1),INDEX(LinMotor!$X$1:$X$1355,A134,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A134<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A134,1),INDEX(LinMotor!$X$1:$X$1355,A134,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A134,1),INDEX(LinMotor!$Z$1:$Z$1355,A134,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A134,1),INDEX(LinMotor!$X$1:$X$1355,A134,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A134,1),INDEX(LinMotor!$Z$1:$Z$1355,A134,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A134,1),INDEX(LinMotor!$X$1:$X$1355,A134,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A134,1),INDEX(LinMotor!$Z$1:$Z$1355,A134,1)))/1000,\"0.0k\")),\"\")","v":29.146177824000002},{"$f":"IF(A134<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A134,1),INDEX(LinMotor!$Y$1:$Y$1355,A134,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A134,1),INDEX(LinMotor!$AB$1:$AB$445,A134,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A134,1),INDEX(LinMotor!$Y$1:$Y$1355,A134,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A134,1),INDEX(LinMotor!$AB$1:$AB$445,A134,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A134,1),INDEX(LinMotor!$Y$1:$Y$1355,A134,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A134,1),INDEX(LinMotor!$AB$1:$AB$445,A134,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A134,1),INDEX(LinMotor!$AD$1:$AD$1355,A134,1))","v":0.6059386786251173},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A134,1),INDEX(LinMotor!$AE$1:$AE$1355,A134,1))","v":0.89057765573333347},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A134,1),INDEX(LinMotor!$AF$1:$AF$1355,A134,1))","v":14.542528287002815},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A134,1),INDEX(LinMotor!$AG$1:$AG$1355,A134,1))","v":42.747727475200008},{"$f":"IF(A134<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A134,1),INDEX(LinMotor!$AI$1:$AI$1355,A134,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A134,1),INDEX(LinMotor!$AI$1:$AI$1355,A134,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A134,1),INDEX(LinMotor!$AI$1:$AI$1355,A134,1))/1000,\"0.0k\")),\"\")","v":23.034763612537809},{"$f":"IF(A134<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A134,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A134,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A134,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A134,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A134,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A134,1))/1000,\"0.0k\")),\"\")","v":2.4163107629578562},{"$f":"IF(A134<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A134,1),INDEX(LinMotor!$AK$1:$AK$1355,A134,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A134,1),INDEX(LinMotor!$AK$1:$AK$1355,A134,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A134,1),INDEX(LinMotor!$AK$1:$AK$1355,A134,1))/1000,\"0.0k\")),\"\")","v":148.02140747897386},""]
[62,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A135,1),INDEX(LinMotor!$B$1:$B$1341,A135,1))","v":"AKM44K"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A135,1),INDEX(LinMotor!$R$1:$R$1355,A135,1))","v":416.66666666666663},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A135,1),INDEX(LinMotor!$S$1:$S$1355,A135,1))","v":1.6897285492874883},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A135,1),INDEX(LinMotor!$T$1:$T$1355,A135,1))","v":1.4500585982089553},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A135,1),INDEX(LinMotor!$U$1:$U$1355,A135,1))","v":2.1220659078919377E-2},{"$f":"IF(A135<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A135,1),INDEX(LinMotor!$V$1:$V$1355,A135,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A135,1),INDEX(LinMotor!$V$1:$V$1355,A135,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A135,1),INDEX(LinMotor!$V$1:$V$1355,A135,1))/1000,\"0.0k\")),\"\")","v":-22.575528177777777},{"$f":"IF(A135<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A135,1),INDEX(LinMotor!$W$1:$W$1355,A135,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A135,1),INDEX(LinMotor!$X$1:$X$1355,A135,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A135,1),INDEX(LinMotor!$W$1:$W$1355,A135,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A135,1),INDEX(LinMotor!$X$1:$X$1355,A135,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A135,1),INDEX(LinMotor!$W$1:$W$1355,A135,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A135,1),INDEX(LinMotor!$X$1:$X$1355,A135,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A135<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A135,1),INDEX(LinMotor!$X$1:$X$1355,A135,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A135,1),INDEX(LinMotor!$Z$1:$Z$1355,A135,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A135,1),INDEX(LinMotor!$X$1:$X$1355,A135,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A135,1),INDEX(LinMotor!$Z$1:$Z$1355,A135,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A135,1),INDEX(LinMotor!$X$1:$X$1355,A135,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A135,1),INDEX(LinMotor!$Z$1:$Z$1355,A135,1)))/1000,\"0.0k\")),\"\")","v":29.146177824000002},{"$f":"IF(A135<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A135,1),INDEX(LinMotor!$Y$1:$Y$1355,A135,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A135,1),INDEX(LinMotor!$AB$1:$AB$445,A135,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A135,1),INDEX(LinMotor!$Y$1:$Y$1355,A135,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A135,1),INDEX(LinMotor!$AB$1:$AB$445,A135,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A135,1),INDEX(LinMotor!$Y$1:$Y$1355,A135,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A135,1),INDEX(LinMotor!$AB$1:$AB$445,A135,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A135,1),INDEX(LinMotor!$AD$1:$AD$1355,A135,1))","v":0.70964525210038099},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A135,1),INDEX(LinMotor!$AE$1:$AE$1355,A135,1))","v":1.0430002693537417},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A135,1),INDEX(LinMotor!$AF$1:$AF$1355,A135,1))","v":17.031486050409143},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A135,1),INDEX(LinMotor!$AG$1:$AG$1355,A135,1))","v":50.064012928979601},{"$f":"IF(A135<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A135,1),INDEX(LinMotor!$AI$1:$AI$1355,A135,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A135,1),INDEX(LinMotor!$AI$1:$AI$1355,A135,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A135,1),INDEX(LinMotor!$AI$1:$AI$1355,A135,1))/1000,\"0.0k\")),\"\")","v":23.034763612537809},{"$f":"IF(A135<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A135,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A135,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A135,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A135,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A135,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A135,1))/1000,\"0.0k\")),\"\")","v":2.4163107629578562},{"$f":"IF(A135<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A135,1),INDEX(LinMotor!$AK$1:$AK$1355,A135,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A135,1),INDEX(LinMotor!$AK$1:$AK$1355,A135,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A135,1),INDEX(LinMotor!$AK$1:$AK$1355,A135,1))/1000,\"0.0k\")),\"\")","v":148.02140747897386},""]
[63,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A136,1),INDEX(LinMotor!$B$1:$B$1341,A136,1))","v":"AKM51E"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A136,1),INDEX(LinMotor!$R$1:$R$1355,A136,1))","v":330.88235294117646},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A136,1),INDEX(LinMotor!$S$1:$S$1355,A136,1))","v":2.1127839462662545},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A136,1),INDEX(LinMotor!$T$1:$T$1355,A136,1))","v":2.5138401213793107},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A136,1),INDEX(LinMotor!$U$1:$U$1355,A136,1))","v":8.9471681683010534E-2},{"$f":"IF(A136<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A136,1),INDEX(LinMotor!$V$1:$V$1355,A136,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A136,1),INDEX(LinMotor!$V$1:$V$1355,A136,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A136,1),INDEX(LinMotor!$V$1:$V$1355,A136,1))/1000,\"0.0k\")),\"\")","v":-22.593265935802467},{"$f":"IF(A136<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A136,1),INDEX(LinMotor!$W$1:$W$1355,A136,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A136,1),INDEX(LinMotor!$X$1:$X$1355,A136,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A136,1),INDEX(LinMotor!$W$1:$W$1355,A136,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A136,1),INDEX(LinMotor!$X$1:$X$1355,A136,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A136,1),INDEX(LinMotor!$W$1:$W$1355,A136,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A136,1),INDEX(LinMotor!$X$1:$X$1355,A136,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A136<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A136,1),INDEX(LinMotor!$X$1:$X$1355,A136,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A136,1),INDEX(LinMotor!$Z$1:$Z$1355,A136,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A136,1),INDEX(LinMotor!$X$1:$X$1355,A136,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A136,1),INDEX(LinMotor!$Z$1:$Z$1355,A136,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A136,1),INDEX(LinMotor!$X$1:$X$1355,A136,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A136,1),INDEX(LinMotor!$Z$1:$Z$1355,A136,1)))/1000,\"0.0k\")),\"\")","v":29.160545408000001},{"$f":"IF(A136<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A136,1),INDEX(LinMotor!$Y$1:$Y$1355,A136,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A136,1),INDEX(LinMotor!$AB$1:$AB$445,A136,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A136,1),INDEX(LinMotor!$Y$1:$Y$1355,A136,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A136,1),INDEX(LinMotor!$AB$1:$AB$445,A136,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A136,1),INDEX(LinMotor!$Y$1:$Y$1355,A136,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A136,1),INDEX(LinMotor!$AB$1:$AB$445,A136,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A136,1),INDEX(LinMotor!$AD$1:$AD$1355,A136,1))","v":0.24176071056245785},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A136,1),INDEX(LinMotor!$AE$1:$AE$1355,A136,1))","v":0.35545877602836878},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A136,1),INDEX(LinMotor!$AF$1:$AF$1355,A136,1))","v":5.8022570534989883},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A136,1),INDEX(LinMotor!$AG$1:$AG$1355,A136,1))","v":17.062021249361703},{"$f":"IF(A136<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A136,1),INDEX(LinMotor!$AI$1:$AI$1355,A136,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A136,1),INDEX(LinMotor!$AI$1:$AI$1355,A136,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A136,1),INDEX(LinMotor!$AI$1:$AI$1355,A136,1))/1000,\"0.0k\")),\"\")","v":23.037608498016418},{"$f":"IF(A136<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A136,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A136,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A136,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A136,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A136,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A136,1))/1000,\"0.0k\")),\"\")","v":2.4187685590227637},{"$f":"IF(A136<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A136,1),INDEX(LinMotor!$AK$1:$AK$1355,A136,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A136,1),INDEX(LinMotor!$AK$1:$AK$1355,A136,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A136,1),INDEX(LinMotor!$AK$1:$AK$1355,A136,1))/1000,\"0.0k\")),\"\")","v":148.17197024532041},""]
[64,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A137,1),INDEX(LinMotor!$B$1:$B$1341,A137,1))","v":"AKM51G"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A137,1),INDEX(LinMotor!$R$1:$R$1355,A137,1))","v":330.88235294117646},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A137,1),INDEX(LinMotor!$S$1:$S$1355,A137,1))","v":2.0918643091876739},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A137,1),INDEX(LinMotor!$T$1:$T$1355,A137,1))","v":2.4923543083760684},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A137,1),INDEX(LinMotor!$U$1:$U$1355,A137,1))","v":4.8055897886198344E-2},{"$f":"IF(A137<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A137,1),INDEX(LinMotor!$V$1:$V$1355,A137,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A137,1),INDEX(LinMotor!$V$1:$V$1355,A137,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A137,1),INDEX(LinMotor!$V$1:$V$1355,A137,1))/1000,\"0.0k\")),\"\")","v":-22.593265935802467},{"$f":"IF(A137<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A137,1),INDEX(LinMotor!$W$1:$W$1355,A137,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A137,1),INDEX(LinMotor!$X$1:$X$1355,A137,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A137,1),INDEX(LinMotor!$W$1:$W$1355,A137,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A137,1),INDEX(LinMotor!$X$1:$X$1355,A137,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A137,1),INDEX(LinMotor!$W$1:$W$1355,A137,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A137,1),INDEX(LinMotor!$X$1:$X$1355,A137,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A137<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A137,1),INDEX(LinMotor!$X$1:$X$1355,A137,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A137,1),INDEX(LinMotor!$Z$1:$Z$1355,A137,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A137,1),INDEX(LinMotor!$X$1:$X$1355,A137,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A137,1),INDEX(LinMotor!$Z$1:$Z$1355,A137,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A137,1),INDEX(LinMotor!$X$1:$X$1355,A137,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A137,1),INDEX(LinMotor!$Z$1:$Z$1355,A137,1)))/1000,\"0.0k\")),\"\")","v":29.160545408000001},{"$f":"IF(A137<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A137,1),INDEX(LinMotor!$Y$1:$Y$1355,A137,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A137,1),INDEX(LinMotor!$AB$1:$AB$445,A137,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A137,1),INDEX(LinMotor!$Y$1:$Y$1355,A137,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A137,1),INDEX(LinMotor!$AB$1:$AB$445,A137,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A137,1),INDEX(LinMotor!$Y$1:$Y$1355,A137,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A137,1),INDEX(LinMotor!$AB$1:$AB$445,A137,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A137,1),INDEX(LinMotor!$AD$1:$AD$1355,A137,1))","v":0.42101991532055821},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A137,1),INDEX(LinMotor!$AE$1:$AE$1355,A137,1))","v":0.61902210427508775},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A137,1),INDEX(LinMotor!$AF$1:$AF$1355,A137,1))","v":10.104477967693397},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A137,1),INDEX(LinMotor!$AG$1:$AG$1355,A137,1))","v":29.71306100520421},{"$f":"IF(A137<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A137,1),INDEX(LinMotor!$AI$1:$AI$1355,A137,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A137,1),INDEX(LinMotor!$AI$1:$AI$1355,A137,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A137,1),INDEX(LinMotor!$AI$1:$AI$1355,A137,1))/1000,\"0.0k\")),\"\")","v":23.037608498016418},{"$f":"IF(A137<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A137,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A137,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A137,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A137,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A137,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A137,1))/1000,\"0.0k\")),\"\")","v":2.4187685590227637},{"$f":"IF(A137<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A137,1),INDEX(LinMotor!$AK$1:$AK$1355,A137,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A137,1),INDEX(LinMotor!$AK$1:$AK$1355,A137,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A137,1),INDEX(LinMotor!$AK$1:$AK$1355,A137,1))/1000,\"0.0k\")),\"\")","v":148.17197024532041},""]
[65,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A138,1),INDEX(LinMotor!$B$1:$B$1341,A138,1))","v":"AKM51H"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A138,1),INDEX(LinMotor!$R$1:$R$1355,A138,1))","v":330.88235294117646},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A138,1),INDEX(LinMotor!$S$1:$S$1355,A138,1))","v":2.0748169501117042},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A138,1),INDEX(LinMotor!$T$1:$T$1355,A138,1))","v":2.4923543083760684},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A138,1),INDEX(LinMotor!$U$1:$U$1355,A138,1))","v":3.8246419096000149E-2},{"$f":"IF(A138<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A138,1),INDEX(LinMotor!$V$1:$V$1355,A138,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A138,1),INDEX(LinMotor!$V$1:$V$1355,A138,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A138,1),INDEX(LinMotor!$V$1:$V$1355,A138,1))/1000,\"0.0k\")),\"\")","v":-22.593265935802467},{"$f":"IF(A138<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A138,1),INDEX(LinMotor!$W$1:$W$1355,A138,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A138,1),INDEX(LinMotor!$X$1:$X$1355,A138,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A138,1),INDEX(LinMotor!$W$1:$W$1355,A138,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A138,1),INDEX(LinMotor!$X$1:$X$1355,A138,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A138,1),INDEX(LinMotor!$W$1:$W$1355,A138,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A138,1),INDEX(LinMotor!$X$1:$X$1355,A138,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A138<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A138,1),INDEX(LinMotor!$X$1:$X$1355,A138,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A138,1),INDEX(LinMotor!$Z$1:$Z$1355,A138,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A138,1),INDEX(LinMotor!$X$1:$X$1355,A138,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A138,1),INDEX(LinMotor!$Z$1:$Z$1355,A138,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A138,1),INDEX(LinMotor!$X$1:$X$1355,A138,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A138,1),INDEX(LinMotor!$Z$1:$Z$1355,A138,1)))/1000,\"0.0k\")),\"\")","v":29.160545408000001},{"$f":"IF(A138<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A138,1),INDEX(LinMotor!$Y$1:$Y$1355,A138,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A138,1),INDEX(LinMotor!$AB$1:$AB$445,A138,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A138,1),INDEX(LinMotor!$Y$1:$Y$1355,A138,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A138,1),INDEX(LinMotor!$AB$1:$AB$445,A138,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A138,1),INDEX(LinMotor!$Y$1:$Y$1355,A138,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A138,1),INDEX(LinMotor!$AB$1:$AB$445,A138,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A138,1),INDEX(LinMotor!$AD$1:$AD$1355,A138,1))","v":0.51756705544591475},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A138,1),INDEX(LinMotor!$AE$1:$AE$1355,A138,1))","v":0.76097456701461386},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A138,1),INDEX(LinMotor!$AF$1:$AF$1355,A138,1))","v":12.421609330701953},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A138,1),INDEX(LinMotor!$AG$1:$AG$1355,A138,1))","v":36.526779216701463},{"$f":"IF(A138<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A138,1),INDEX(LinMotor!$AI$1:$AI$1355,A138,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A138,1),INDEX(LinMotor!$AI$1:$AI$1355,A138,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A138,1),INDEX(LinMotor!$AI$1:$AI$1355,A138,1))/1000,\"0.0k\")),\"\")","v":23.037608498016418},{"$f":"IF(A138<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A138,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A138,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A138,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A138,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A138,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A138,1))/1000,\"0.0k\")),\"\")","v":2.4187685590227637},{"$f":"IF(A138<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A138,1),INDEX(LinMotor!$AK$1:$AK$1355,A138,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A138,1),INDEX(LinMotor!$AK$1:$AK$1355,A138,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A138,1),INDEX(LinMotor!$AK$1:$AK$1355,A138,1))/1000,\"0.0k\")),\"\")","v":148.17197024532041},""]
[66,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A139,1),INDEX(LinMotor!$B$1:$B$1341,A139,1))","v":"AKM51I"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A139,1),INDEX(LinMotor!$R$1:$R$1355,A139,1))","v":330.88235294117646},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A139,1),INDEX(LinMotor!$S$1:$S$1355,A139,1))","v":2.0576283344644888},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A139,1),INDEX(LinMotor!$T$1:$T$1355,A139,1))","v":2.471232661694915},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A139,1),INDEX(LinMotor!$U$1:$U$1355,A139,1))","v":3.0510858440553359E-2},{"$f":"IF(A139<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A139,1),INDEX(LinMotor!$V$1:$V$1355,A139,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A139,1),INDEX(LinMotor!$V$1:$V$1355,A139,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A139,1),INDEX(LinMotor!$V$1:$V$1355,A139,1))/1000,\"0.0k\")),\"\")","v":-22.593265935802467},{"$f":"IF(A139<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A139,1),INDEX(LinMotor!$W$1:$W$1355,A139,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A139,1),INDEX(LinMotor!$X$1:$X$1355,A139,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A139,1),INDEX(LinMotor!$W$1:$W$1355,A139,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A139,1),INDEX(LinMotor!$X$1:$X$1355,A139,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A139,1),INDEX(LinMotor!$W$1:$W$1355,A139,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A139,1),INDEX(LinMotor!$X$1:$X$1355,A139,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A139<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A139,1),INDEX(LinMotor!$X$1:$X$1355,A139,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A139,1),INDEX(LinMotor!$Z$1:$Z$1355,A139,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A139,1),INDEX(LinMotor!$X$1:$X$1355,A139,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A139,1),INDEX(LinMotor!$Z$1:$Z$1355,A139,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A139,1),INDEX(LinMotor!$X$1:$X$1355,A139,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A139,1),INDEX(LinMotor!$Z$1:$Z$1355,A139,1)))/1000,\"0.0k\")),\"\")","v":29.160545408000001},{"$f":"IF(A139<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A139,1),INDEX(LinMotor!$Y$1:$Y$1355,A139,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A139,1),INDEX(LinMotor!$AB$1:$AB$445,A139,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A139,1),INDEX(LinMotor!$Y$1:$Y$1355,A139,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A139,1),INDEX(LinMotor!$AB$1:$AB$445,A139,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A139,1),INDEX(LinMotor!$Y$1:$Y$1355,A139,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A139,1),INDEX(LinMotor!$AB$1:$AB$445,A139,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A139,1),INDEX(LinMotor!$AD$1:$AD$1355,A139,1))","v":0.64160098229449569},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A139,1),INDEX(LinMotor!$AE$1:$AE$1355,A139,1))","v":0.94334062525879914},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A139,1),INDEX(LinMotor!$AF$1:$AF$1355,A139,1))","v":15.398423575067897},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A139,1),INDEX(LinMotor!$AG$1:$AG$1355,A139,1))","v":45.28035001242236},{"$f":"IF(A139<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A139,1),INDEX(LinMotor!$AI$1:$AI$1355,A139,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A139,1),INDEX(LinMotor!$AI$1:$AI$1355,A139,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A139,1),INDEX(LinMotor!$AI$1:$AI$1355,A139,1))/1000,\"0.0k\")),\"\")","v":23.037608498016418},{"$f":"IF(A139<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A139,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A139,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A139,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A139,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A139,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A139,1))/1000,\"0.0k\")),\"\")","v":2.4187685590227637},{"$f":"IF(A139<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A139,1),INDEX(LinMotor!$AK$1:$AK$1355,A139,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A139,1),INDEX(LinMotor!$AK$1:$AK$1355,A139,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A139,1),INDEX(LinMotor!$AK$1:$AK$1355,A139,1))/1000,\"0.0k\")),\"\")","v":148.17197024532041},""]
[67,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A140,1),INDEX(LinMotor!$B$1:$B$1341,A140,1))","v":"AKM51K"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A140,1),INDEX(LinMotor!$R$1:$R$1355,A140,1))","v":330.88235294117646},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A140,1),INDEX(LinMotor!$S$1:$S$1355,A140,1))","v":2.0280501566751941},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A140,1),INDEX(LinMotor!$T$1:$T$1355,A140,1))","v":2.4504660006722689},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A140,1),INDEX(LinMotor!$U$1:$U$1355,A140,1))","v":2.4457783006820041E-2},{"$f":"IF(A140<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A140,1),INDEX(LinMotor!$V$1:$V$1355,A140,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A140,1),INDEX(LinMotor!$V$1:$V$1355,A140,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A140,1),INDEX(LinMotor!$V$1:$V$1355,A140,1))/1000,\"0.0k\")),\"\")","v":-22.593265935802467},{"$f":"IF(A140<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A140,1),INDEX(LinMotor!$W$1:$W$1355,A140,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A140,1),INDEX(LinMotor!$X$1:$X$1355,A140,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A140,1),INDEX(LinMotor!$W$1:$W$1355,A140,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A140,1),INDEX(LinMotor!$X$1:$X$1355,A140,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A140,1),INDEX(LinMotor!$W$1:$W$1355,A140,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A140,1),INDEX(LinMotor!$X$1:$X$1355,A140,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A140<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A140,1),INDEX(LinMotor!$X$1:$X$1355,A140,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A140,1),INDEX(LinMotor!$Z$1:$Z$1355,A140,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A140,1),INDEX(LinMotor!$X$1:$X$1355,A140,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A140,1),INDEX(LinMotor!$Z$1:$Z$1355,A140,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A140,1),INDEX(LinMotor!$X$1:$X$1355,A140,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A140,1),INDEX(LinMotor!$Z$1:$Z$1355,A140,1)))/1000,\"0.0k\")),\"\")","v":29.160545408000001},{"$f":"IF(A140<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A140,1),INDEX(LinMotor!$Y$1:$Y$1355,A140,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A140,1),INDEX(LinMotor!$AB$1:$AB$445,A140,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A140,1),INDEX(LinMotor!$Y$1:$Y$1355,A140,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A140,1),INDEX(LinMotor!$AB$1:$AB$445,A140,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A140,1),INDEX(LinMotor!$Y$1:$Y$1355,A140,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A140,1),INDEX(LinMotor!$AB$1:$AB$445,A140,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A140,1),INDEX(LinMotor!$AD$1:$AD$1355,A140,1))","v":0.79265218498325696},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A140,1),INDEX(LinMotor!$AE$1:$AE$1355,A140,1))","v":1.1654299610340135},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A140,1),INDEX(LinMotor!$AF$1:$AF$1355,A140,1))","v":19.023652439598166},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A140,1),INDEX(LinMotor!$AG$1:$AG$1355,A140,1))","v":55.940638129632653},{"$f":"IF(A140<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A140,1),INDEX(LinMotor!$AI$1:$AI$1355,A140,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A140,1),INDEX(LinMotor!$AI$1:$AI$1355,A140,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A140,1),INDEX(LinMotor!$AI$1:$AI$1355,A140,1))/1000,\"0.0k\")),\"\")","v":23.037608498016418},{"$f":"IF(A140<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A140,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A140,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A140,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A140,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A140,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A140,1))/1000,\"0.0k\")),\"\")","v":2.4187685590227637},{"$f":"IF(A140<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A140,1),INDEX(LinMotor!$AK$1:$AK$1355,A140,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A140,1),INDEX(LinMotor!$AK$1:$AK$1355,A140,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A140,1),INDEX(LinMotor!$AK$1:$AK$1355,A140,1))/1000,\"0.0k\")),\"\")","v":148.17197024532041},""]
[68,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A141,1),INDEX(LinMotor!$B$1:$B$1341,A141,1))","v":"AKM51L"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A141,1),INDEX(LinMotor!$R$1:$R$1355,A141,1))","v":330.88235294117646},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A141,1),INDEX(LinMotor!$S$1:$S$1355,A141,1))","v":2.0323728469506221},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A141,1),INDEX(LinMotor!$T$1:$T$1355,A141,1))","v":2.4300454506666669},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A141,1),INDEX(LinMotor!$U$1:$U$1355,A141,1))","v":2.1220659078919377E-2},{"$f":"IF(A141<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A141,1),INDEX(LinMotor!$V$1:$V$1355,A141,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A141,1),INDEX(LinMotor!$V$1:$V$1355,A141,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A141,1),INDEX(LinMotor!$V$1:$V$1355,A141,1))/1000,\"0.0k\")),\"\")","v":-22.593265935802467},{"$f":"IF(A141<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A141,1),INDEX(LinMotor!$W$1:$W$1355,A141,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A141,1),INDEX(LinMotor!$X$1:$X$1355,A141,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A141,1),INDEX(LinMotor!$W$1:$W$1355,A141,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A141,1),INDEX(LinMotor!$X$1:$X$1355,A141,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A141,1),INDEX(LinMotor!$W$1:$W$1355,A141,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A141,1),INDEX(LinMotor!$X$1:$X$1355,A141,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A141<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A141,1),INDEX(LinMotor!$X$1:$X$1355,A141,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A141,1),INDEX(LinMotor!$Z$1:$Z$1355,A141,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A141,1),INDEX(LinMotor!$X$1:$X$1355,A141,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A141,1),INDEX(LinMotor!$Z$1:$Z$1355,A141,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A141,1),INDEX(LinMotor!$X$1:$X$1355,A141,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A141,1),INDEX(LinMotor!$Z$1:$Z$1355,A141,1)))/1000,\"0.0k\")),\"\")","v":29.160545408000001},{"$f":"IF(A141<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A141,1),INDEX(LinMotor!$Y$1:$Y$1355,A141,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A141,1),INDEX(LinMotor!$AB$1:$AB$445,A141,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A141,1),INDEX(LinMotor!$Y$1:$Y$1355,A141,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A141,1),INDEX(LinMotor!$AB$1:$AB$445,A141,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A141,1),INDEX(LinMotor!$Y$1:$Y$1355,A141,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A141,1),INDEX(LinMotor!$AB$1:$AB$445,A141,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A141,1),INDEX(LinMotor!$AD$1:$AD$1355,A141,1))","v":1.005516009797975},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A141,1),INDEX(LinMotor!$AE$1:$AE$1355,A141,1))","v":1.4784018846080438},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A141,1),INDEX(LinMotor!$AF$1:$AF$1355,A141,1))","v":24.132384235151399},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A141,1),INDEX(LinMotor!$AG$1:$AG$1355,A141,1))","v":70.963290461186105},{"$f":"IF(A141<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A141,1),INDEX(LinMotor!$AI$1:$AI$1355,A141,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A141,1),INDEX(LinMotor!$AI$1:$AI$1355,A141,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A141,1),INDEX(LinMotor!$AI$1:$AI$1355,A141,1))/1000,\"0.0k\")),\"\")","v":23.037608498016418},{"$f":"IF(A141<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A141,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A141,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A141,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A141,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A141,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A141,1))/1000,\"0.0k\")),\"\")","v":2.4187685590227637},{"$f":"IF(A141<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A141,1),INDEX(LinMotor!$AK$1:$AK$1355,A141,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A141,1),INDEX(LinMotor!$AK$1:$AK$1355,A141,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A141,1),INDEX(LinMotor!$AK$1:$AK$1355,A141,1))/1000,\"0.0k\")),\"\")","v":148.17197024532041},""]
[69,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A142,1),INDEX(LinMotor!$B$1:$B$1341,A142,1))","v":"AKM52E"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A142,1),INDEX(LinMotor!$R$1:$R$1355,A142,1))","v":181.45161290322579},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A142,1),INDEX(LinMotor!$S$1:$S$1355,A142,1))","v":1.1911691219007017},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A142,1),INDEX(LinMotor!$T$1:$T$1355,A142,1))","v":1.3717378283568076},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A142,1),INDEX(LinMotor!$U$1:$U$1355,A142,1))","v":8.7969671225590462E-2},{"$f":"IF(A142<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A142,1),INDEX(LinMotor!$V$1:$V$1355,A142,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A142,1),INDEX(LinMotor!$V$1:$V$1355,A142,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A142,1),INDEX(LinMotor!$V$1:$V$1355,A142,1))/1000,\"0.0k\")),\"\")","v":-22.664216967901236},{"$f":"IF(A142<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A142,1),INDEX(LinMotor!$W$1:$W$1355,A142,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A142,1),INDEX(LinMotor!$X$1:$X$1355,A142,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A142,1),INDEX(LinMotor!$W$1:$W$1355,A142,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A142,1),INDEX(LinMotor!$X$1:$X$1355,A142,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A142,1),INDEX(LinMotor!$W$1:$W$1355,A142,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A142,1),INDEX(LinMotor!$X$1:$X$1355,A142,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A142<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A142,1),INDEX(LinMotor!$X$1:$X$1355,A142,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A142,1),INDEX(LinMotor!$Z$1:$Z$1355,A142,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A142,1),INDEX(LinMotor!$X$1:$X$1355,A142,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A142,1),INDEX(LinMotor!$Z$1:$Z$1355,A142,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A142,1),INDEX(LinMotor!$X$1:$X$1355,A142,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A142,1),INDEX(LinMotor!$Z$1:$Z$1355,A142,1)))/1000,\"0.0k\")),\"\")","v":29.218015744000002},{"$f":"IF(A142<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A142,1),INDEX(LinMotor!$Y$1:$Y$1355,A142,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A142,1),INDEX(LinMotor!$AB$1:$AB$445,A142,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A142,1),INDEX(LinMotor!$Y$1:$Y$1355,A142,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A142,1),INDEX(LinMotor!$AB$1:$AB$445,A142,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A142,1),INDEX(LinMotor!$Y$1:$Y$1355,A142,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A142,1),INDEX(LinMotor!$AB$1:$AB$445,A142,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A142,1),INDEX(LinMotor!$AD$1:$AD$1355,A142,1))","v":0.14820769756627192},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A142,1),INDEX(LinMotor!$AE$1:$AE$1355,A142,1))","v":0.21823008361950444},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A142,1),INDEX(LinMotor!$AF$1:$AF$1355,A142,1))","v":3.5569847415905258},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A142,1),INDEX(LinMotor!$AG$1:$AG$1355,A142,1))","v":10.475044013736213},{"$f":"IF(A142<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A142,1),INDEX(LinMotor!$AI$1:$AI$1355,A142,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A142,1),INDEX(LinMotor!$AI$1:$AI$1355,A142,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A142,1),INDEX(LinMotor!$AI$1:$AI$1355,A142,1))/1000,\"0.0k\")),\"\")","v":23.049002172390853},{"$f":"IF(A142<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A142,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A142,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A142,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A142,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A142,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A142,1))/1000,\"0.0k\")),\"\")","v":2.4285997432823918},{"$f":"IF(A142<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A142,1),INDEX(LinMotor!$AK$1:$AK$1355,A142,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A142,1),INDEX(LinMotor!$AK$1:$AK$1355,A142,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A142,1),INDEX(LinMotor!$AK$1:$AK$1355,A142,1))/1000,\"0.0k\")),\"\")","v":148.77422131070654},""]
[70,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A143,1),INDEX(LinMotor!$B$1:$B$1341,A143,1))","v":"AKM52G"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A143,1),INDEX(LinMotor!$R$1:$R$1355,A143,1))","v":181.45161290322579},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A143,1),INDEX(LinMotor!$S$1:$S$1355,A143,1))","v":1.1786261983973787},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A143,1),INDEX(LinMotor!$T$1:$T$1355,A143,1))","v":1.3589774764651164},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A143,1),INDEX(LinMotor!$U$1:$U$1355,A143,1))","v":5.3969614209498813E-2},{"$f":"IF(A143<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A143,1),INDEX(LinMotor!$V$1:$V$1355,A143,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A143,1),INDEX(LinMotor!$V$1:$V$1355,A143,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A143,1),INDEX(LinMotor!$V$1:$V$1355,A143,1))/1000,\"0.0k\")),\"\")","v":-22.664216967901236},{"$f":"IF(A143<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A143,1),INDEX(LinMotor!$W$1:$W$1355,A143,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A143,1),INDEX(LinMotor!$X$1:$X$1355,A143,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A143,1),INDEX(LinMotor!$W$1:$W$1355,A143,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A143,1),INDEX(LinMotor!$X$1:$X$1355,A143,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A143,1),INDEX(LinMotor!$W$1:$W$1355,A143,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A143,1),INDEX(LinMotor!$X$1:$X$1355,A143,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A143<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A143,1),INDEX(LinMotor!$X$1:$X$1355,A143,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A143,1),INDEX(LinMotor!$Z$1:$Z$1355,A143,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A143,1),INDEX(LinMotor!$X$1:$X$1355,A143,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A143,1),INDEX(LinMotor!$Z$1:$Z$1355,A143,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A143,1),INDEX(LinMotor!$X$1:$X$1355,A143,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A143,1),INDEX(LinMotor!$Z$1:$Z$1355,A143,1)))/1000,\"0.0k\")),\"\")","v":29.218015744000002},{"$f":"IF(A143<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A143,1),INDEX(LinMotor!$Y$1:$Y$1355,A143,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A143,1),INDEX(LinMotor!$AB$1:$AB$445,A143,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A143,1),INDEX(LinMotor!$Y$1:$Y$1355,A143,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A143,1),INDEX(LinMotor!$AB$1:$AB$445,A143,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A143,1),INDEX(LinMotor!$Y$1:$Y$1355,A143,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A143,1),INDEX(LinMotor!$AB$1:$AB$445,A143,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A143,1),INDEX(LinMotor!$AD$1:$AD$1355,A143,1))","v":0.23146218407569638},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A143,1),INDEX(LinMotor!$AE$1:$AE$1355,A143,1))","v":0.34081908440015818},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A143,1),INDEX(LinMotor!$AF$1:$AF$1355,A143,1))","v":5.5550924178167129},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A143,1),INDEX(LinMotor!$AG$1:$AG$1355,A143,1))","v":16.359316051207593},{"$f":"IF(A143<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A143,1),INDEX(LinMotor!$AI$1:$AI$1355,A143,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A143,1),INDEX(LinMotor!$AI$1:$AI$1355,A143,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A143,1),INDEX(LinMotor!$AI$1:$AI$1355,A143,1))/1000,\"0.0k\")),\"\")","v":23.049002172390853},{"$f":"IF(A143<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A143,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A143,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A143,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A143,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A143,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A143,1))/1000,\"0.0k\")),\"\")","v":2.4285997432823918},{"$f":"IF(A143<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A143,1),INDEX(LinMotor!$AK$1:$AK$1355,A143,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A143,1),INDEX(LinMotor!$AK$1:$AK$1355,A143,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A143,1),INDEX(LinMotor!$AK$1:$AK$1355,A143,1))/1000,\"0.0k\")),\"\")","v":148.77422131070654},""]
[71,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A144,1),INDEX(LinMotor!$B$1:$B$1341,A144,1))","v":"AKM52H"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A144,1),INDEX(LinMotor!$R$1:$R$1355,A144,1))","v":181.45161290322579},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A144,1),INDEX(LinMotor!$S$1:$S$1355,A144,1))","v":1.1719317133604101},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A144,1),INDEX(LinMotor!$T$1:$T$1355,A144,1))","v":1.3526859140740741},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A144,1),INDEX(LinMotor!$U$1:$U$1355,A144,1))","v":4.2813735161864576E-2},{"$f":"IF(A144<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A144,1),INDEX(LinMotor!$V$1:$V$1355,A144,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A144,1),INDEX(LinMotor!$V$1:$V$1355,A144,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A144,1),INDEX(LinMotor!$V$1:$V$1355,A144,1))/1000,\"0.0k\")),\"\")","v":-22.664216967901236},{"$f":"IF(A144<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A144,1),INDEX(LinMotor!$W$1:$W$1355,A144,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A144,1),INDEX(LinMotor!$X$1:$X$1355,A144,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A144,1),INDEX(LinMotor!$W$1:$W$1355,A144,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A144,1),INDEX(LinMotor!$X$1:$X$1355,A144,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A144,1),INDEX(LinMotor!$W$1:$W$1355,A144,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A144,1),INDEX(LinMotor!$X$1:$X$1355,A144,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A144<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A144,1),INDEX(LinMotor!$X$1:$X$1355,A144,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A144,1),INDEX(LinMotor!$Z$1:$Z$1355,A144,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A144,1),INDEX(LinMotor!$X$1:$X$1355,A144,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A144,1),INDEX(LinMotor!$Z$1:$Z$1355,A144,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A144,1),INDEX(LinMotor!$X$1:$X$1355,A144,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A144,1),INDEX(LinMotor!$Z$1:$Z$1355,A144,1)))/1000,\"0.0k\")),\"\")","v":29.218015744000002},{"$f":"IF(A144<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A144,1),INDEX(LinMotor!$Y$1:$Y$1355,A144,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A144,1),INDEX(LinMotor!$AB$1:$AB$445,A144,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A144,1),INDEX(LinMotor!$Y$1:$Y$1355,A144,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A144,1),INDEX(LinMotor!$AB$1:$AB$445,A144,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A144,1),INDEX(LinMotor!$Y$1:$Y$1355,A144,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A144,1),INDEX(LinMotor!$AB$1:$AB$445,A144,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A144,1),INDEX(LinMotor!$AD$1:$AD$1355,A144,1))","v":0.28762178828981727},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A144,1),INDEX(LinMotor!$AE$1:$AE$1355,A144,1))","v":0.42351192238993712},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A144,1),INDEX(LinMotor!$AF$1:$AF$1355,A144,1))","v":6.9029229189556149},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A144,1),INDEX(LinMotor!$AG$1:$AG$1355,A144,1))","v":20.328572274716983},{"$f":"IF(A144<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A144,1),INDEX(LinMotor!$AI$1:$AI$1355,A144,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A144,1),INDEX(LinMotor!$AI$1:$AI$1355,A144,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A144,1),INDEX(LinMotor!$AI$1:$AI$1355,A144,1))/1000,\"0.0k\")),\"\")","v":23.049002172390853},{"$f":"IF(A144<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A144,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A144,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A144,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A144,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A144,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A144,1))/1000,\"0.0k\")),\"\")","v":2.4285997432823918},{"$f":"IF(A144<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A144,1),INDEX(LinMotor!$AK$1:$AK$1355,A144,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A144,1),INDEX(LinMotor!$AK$1:$AK$1355,A144,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A144,1),INDEX(LinMotor!$AK$1:$AK$1355,A144,1))/1000,\"0.0k\")),\"\")","v":148.77422131070654},""]
[72,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A145,1),INDEX(LinMotor!$B$1:$B$1341,A145,1))","v":"AKM52I"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A145,1),INDEX(LinMotor!$R$1:$R$1355,A145,1))","v":181.45161290322579},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A145,1),INDEX(LinMotor!$S$1:$S$1355,A145,1))","v":1.165398841895005},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A145,1),INDEX(LinMotor!$T$1:$T$1355,A145,1))","v":1.3402759515596332},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A145,1),INDEX(LinMotor!$U$1:$U$1355,A145,1))","v":3.4383006011958574E-2},{"$f":"IF(A145<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A145,1),INDEX(LinMotor!$V$1:$V$1355,A145,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A145,1),INDEX(LinMotor!$V$1:$V$1355,A145,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A145,1),INDEX(LinMotor!$V$1:$V$1355,A145,1))/1000,\"0.0k\")),\"\")","v":-22.664216967901236},{"$f":"IF(A145<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A145,1),INDEX(LinMotor!$W$1:$W$1355,A145,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A145,1),INDEX(LinMotor!$X$1:$X$1355,A145,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A145,1),INDEX(LinMotor!$W$1:$W$1355,A145,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A145,1),INDEX(LinMotor!$X$1:$X$1355,A145,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A145,1),INDEX(LinMotor!$W$1:$W$1355,A145,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A145,1),INDEX(LinMotor!$X$1:$X$1355,A145,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A145<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A145,1),INDEX(LinMotor!$X$1:$X$1355,A145,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A145,1),INDEX(LinMotor!$Z$1:$Z$1355,A145,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A145,1),INDEX(LinMotor!$X$1:$X$1355,A145,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A145,1),INDEX(LinMotor!$Z$1:$Z$1355,A145,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A145,1),INDEX(LinMotor!$X$1:$X$1355,A145,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A145,1),INDEX(LinMotor!$Z$1:$Z$1355,A145,1)))/1000,\"0.0k\")),\"\")","v":29.218015744000002},{"$f":"IF(A145<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A145,1),INDEX(LinMotor!$Y$1:$Y$1355,A145,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A145,1),INDEX(LinMotor!$AB$1:$AB$445,A145,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A145,1),INDEX(LinMotor!$Y$1:$Y$1355,A145,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A145,1),INDEX(LinMotor!$AB$1:$AB$445,A145,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A145,1),INDEX(LinMotor!$Y$1:$Y$1355,A145,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A145,1),INDEX(LinMotor!$AB$1:$AB$445,A145,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A145,1),INDEX(LinMotor!$AD$1:$AD$1355,A145,1))","v":0.35863139982042674},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A145,1),INDEX(LinMotor!$AE$1:$AE$1355,A145,1))","v":0.52807081991402904},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A145,1),INDEX(LinMotor!$AF$1:$AF$1355,A145,1))","v":8.6071535956902423},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A145,1),INDEX(LinMotor!$AG$1:$AG$1355,A145,1))","v":25.347399355873392},{"$f":"IF(A145<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A145,1),INDEX(LinMotor!$AI$1:$AI$1355,A145,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A145,1),INDEX(LinMotor!$AI$1:$AI$1355,A145,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A145,1),INDEX(LinMotor!$AI$1:$AI$1355,A145,1))/1000,\"0.0k\")),\"\")","v":23.049002172390853},{"$f":"IF(A145<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A145,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A145,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A145,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A145,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A145,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A145,1))/1000,\"0.0k\")),\"\")","v":2.4285997432823918},{"$f":"IF(A145<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A145,1),INDEX(LinMotor!$AK$1:$AK$1355,A145,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A145,1),INDEX(LinMotor!$AK$1:$AK$1355,A145,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A145,1),INDEX(LinMotor!$AK$1:$AK$1355,A145,1))/1000,\"0.0k\")),\"\")","v":148.77422131070654},""]
[73,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A146,1),INDEX(LinMotor!$B$1:$B$1341,A146,1))","v":"AKM52K"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A146,1),INDEX(LinMotor!$R$1:$R$1355,A146,1))","v":181.45161290322579},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A146,1),INDEX(LinMotor!$S$1:$S$1355,A146,1))","v":1.1562104330290355},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A146,1),INDEX(LinMotor!$T$1:$T$1355,A146,1))","v":1.3341559700456622},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A146,1),INDEX(LinMotor!$U$1:$U$1355,A146,1))","v":2.7160553142436449E-2},{"$f":"IF(A146<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A146,1),INDEX(LinMotor!$V$1:$V$1355,A146,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A146,1),INDEX(LinMotor!$V$1:$V$1355,A146,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A146,1),INDEX(LinMotor!$V$1:$V$1355,A146,1))/1000,\"0.0k\")),\"\")","v":-22.664216967901236},{"$f":"IF(A146<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A146,1),INDEX(LinMotor!$W$1:$W$1355,A146,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A146,1),INDEX(LinMotor!$X$1:$X$1355,A146,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A146,1),INDEX(LinMotor!$W$1:$W$1355,A146,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A146,1),INDEX(LinMotor!$X$1:$X$1355,A146,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A146,1),INDEX(LinMotor!$W$1:$W$1355,A146,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A146,1),INDEX(LinMotor!$X$1:$X$1355,A146,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A146<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A146,1),INDEX(LinMotor!$X$1:$X$1355,A146,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A146,1),INDEX(LinMotor!$Z$1:$Z$1355,A146,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A146,1),INDEX(LinMotor!$X$1:$X$1355,A146,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A146,1),INDEX(LinMotor!$Z$1:$Z$1355,A146,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A146,1),INDEX(LinMotor!$X$1:$X$1355,A146,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A146,1),INDEX(LinMotor!$Z$1:$Z$1355,A146,1)))/1000,\"0.0k\")),\"\")","v":29.218015744000002},{"$f":"IF(A146<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A146,1),INDEX(LinMotor!$Y$1:$Y$1355,A146,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A146,1),INDEX(LinMotor!$AB$1:$AB$445,A146,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A146,1),INDEX(LinMotor!$Y$1:$Y$1355,A146,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A146,1),INDEX(LinMotor!$AB$1:$AB$445,A146,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A146,1),INDEX(LinMotor!$Y$1:$Y$1355,A146,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A146,1),INDEX(LinMotor!$AB$1:$AB$445,A146,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A146,1),INDEX(LinMotor!$AD$1:$AD$1355,A146,1))","v":0.44704384532298297},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A146,1),INDEX(LinMotor!$AE$1:$AE$1355,A146,1))","v":0.65825471516279088},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A146,1),INDEX(LinMotor!$AF$1:$AF$1355,A146,1))","v":10.729052287751591},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A146,1),INDEX(LinMotor!$AG$1:$AG$1355,A146,1))","v":31.596226327813962},{"$f":"IF(A146<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A146,1),INDEX(LinMotor!$AI$1:$AI$1355,A146,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A146,1),INDEX(LinMotor!$AI$1:$AI$1355,A146,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A146,1),INDEX(LinMotor!$AI$1:$AI$1355,A146,1))/1000,\"0.0k\")),\"\")","v":23.04900217239085},{"$f":"IF(A146<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A146,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A146,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A146,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A146,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A146,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A146,1))/1000,\"0.0k\")),\"\")","v":2.4285997432823918},{"$f":"IF(A146<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A146,1),INDEX(LinMotor!$AK$1:$AK$1355,A146,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A146,1),INDEX(LinMotor!$AK$1:$AK$1355,A146,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A146,1),INDEX(LinMotor!$AK$1:$AK$1355,A146,1))/1000,\"0.0k\")),\"\")","v":148.77422131070654},""]
[74,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A147,1),INDEX(LinMotor!$B$1:$B$1341,A147,1))","v":"AKM52L"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A147,1),INDEX(LinMotor!$R$1:$R$1355,A147,1))","v":181.45161290322579},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A147,1),INDEX(LinMotor!$S$1:$S$1355,A147,1))","v":1.1469886474963402},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A147,1),INDEX(LinMotor!$T$1:$T$1355,A147,1))","v":1.3280916247272729},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A147,1),INDEX(LinMotor!$U$1:$U$1355,A147,1))","v":2.1647742669108148E-2},{"$f":"IF(A147<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A147,1),INDEX(LinMotor!$V$1:$V$1355,A147,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A147,1),INDEX(LinMotor!$V$1:$V$1355,A147,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A147,1),INDEX(LinMotor!$V$1:$V$1355,A147,1))/1000,\"0.0k\")),\"\")","v":-22.664216967901236},{"$f":"IF(A147<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A147,1),INDEX(LinMotor!$W$1:$W$1355,A147,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A147,1),INDEX(LinMotor!$X$1:$X$1355,A147,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A147,1),INDEX(LinMotor!$W$1:$W$1355,A147,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A147,1),INDEX(LinMotor!$X$1:$X$1355,A147,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A147,1),INDEX(LinMotor!$W$1:$W$1355,A147,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A147,1),INDEX(LinMotor!$X$1:$X$1355,A147,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A147<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A147,1),INDEX(LinMotor!$X$1:$X$1355,A147,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A147,1),INDEX(LinMotor!$Z$1:$Z$1355,A147,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A147,1),INDEX(LinMotor!$X$1:$X$1355,A147,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A147,1),INDEX(LinMotor!$Z$1:$Z$1355,A147,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A147,1),INDEX(LinMotor!$X$1:$X$1355,A147,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A147,1),INDEX(LinMotor!$Z$1:$Z$1355,A147,1)))/1000,\"0.0k\")),\"\")","v":29.218015744000002},{"$f":"IF(A147<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A147,1),INDEX(LinMotor!$Y$1:$Y$1355,A147,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A147,1),INDEX(LinMotor!$AB$1:$AB$445,A147,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A147,1),INDEX(LinMotor!$Y$1:$Y$1355,A147,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A147,1),INDEX(LinMotor!$AB$1:$AB$445,A147,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A147,1),INDEX(LinMotor!$Y$1:$Y$1355,A147,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A147,1),INDEX(LinMotor!$AB$1:$AB$445,A147,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A147,1),INDEX(LinMotor!$AD$1:$AD$1355,A147,1))","v":0.5531010902682687},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A147,1),INDEX(LinMotor!$AE$1:$AE$1355,A147,1))","v":0.81441989290272987},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A147,1),INDEX(LinMotor!$AF$1:$AF$1355,A147,1))","v":13.274426166438449},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A147,1),INDEX(LinMotor!$AG$1:$AG$1355,A147,1))","v":39.092154859331032},{"$f":"IF(A147<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A147,1),INDEX(LinMotor!$AI$1:$AI$1355,A147,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A147,1),INDEX(LinMotor!$AI$1:$AI$1355,A147,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A147,1),INDEX(LinMotor!$AI$1:$AI$1355,A147,1))/1000,\"0.0k\")),\"\")","v":23.049002172390853},{"$f":"IF(A147<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A147,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A147,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A147,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A147,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A147,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A147,1))/1000,\"0.0k\")),\"\")","v":2.4285997432823918},{"$f":"IF(A147<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A147,1),INDEX(LinMotor!$AK$1:$AK$1355,A147,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A147,1),INDEX(LinMotor!$AK$1:$AK$1355,A147,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A147,1),INDEX(LinMotor!$AK$1:$AK$1355,A147,1))/1000,\"0.0k\")),\"\")","v":148.77422131070654},""]
[75,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A148,1),INDEX(LinMotor!$B$1:$B$1341,A148,1))","v":"AKM52M"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A148,1),INDEX(LinMotor!$R$1:$R$1355,A148,1))","v":181.45161290322579},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A148,1),INDEX(LinMotor!$S$1:$S$1355,A148,1))","v":1.1559145941260422},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A148,1),INDEX(LinMotor!$T$1:$T$1355,A148,1))","v":1.3341559700456622},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A148,1),INDEX(LinMotor!$U$1:$U$1355,A148,1))","v":2.1220659078919377E-2},{"$f":"IF(A148<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A148,1),INDEX(LinMotor!$V$1:$V$1355,A148,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A148,1),INDEX(LinMotor!$V$1:$V$1355,A148,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A148,1),INDEX(LinMotor!$V$1:$V$1355,A148,1))/1000,\"0.0k\")),\"\")","v":-22.664216967901236},{"$f":"IF(A148<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A148,1),INDEX(LinMotor!$W$1:$W$1355,A148,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A148,1),INDEX(LinMotor!$X$1:$X$1355,A148,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A148,1),INDEX(LinMotor!$W$1:$W$1355,A148,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A148,1),INDEX(LinMotor!$X$1:$X$1355,A148,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A148,1),INDEX(LinMotor!$W$1:$W$1355,A148,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A148,1),INDEX(LinMotor!$X$1:$X$1355,A148,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A148<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A148,1),INDEX(LinMotor!$X$1:$X$1355,A148,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A148,1),INDEX(LinMotor!$Z$1:$Z$1355,A148,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A148,1),INDEX(LinMotor!$X$1:$X$1355,A148,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A148,1),INDEX(LinMotor!$Z$1:$Z$1355,A148,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A148,1),INDEX(LinMotor!$X$1:$X$1355,A148,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A148,1),INDEX(LinMotor!$Z$1:$Z$1355,A148,1)))/1000,\"0.0k\")),\"\")","v":29.218015744000002},{"$f":"IF(A148<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A148,1),INDEX(LinMotor!$Y$1:$Y$1355,A148,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A148,1),INDEX(LinMotor!$AB$1:$AB$445,A148,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A148,1),INDEX(LinMotor!$Y$1:$Y$1355,A148,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A148,1),INDEX(LinMotor!$AB$1:$AB$445,A148,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A148,1),INDEX(LinMotor!$Y$1:$Y$1355,A148,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A148,1),INDEX(LinMotor!$AB$1:$AB$445,A148,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A148,1),INDEX(LinMotor!$AD$1:$AD$1355,A148,1))","v":0.6297069219065673},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A148,1),INDEX(LinMotor!$AE$1:$AE$1355,A148,1))","v":0.92721900737984508},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A148,1),INDEX(LinMotor!$AF$1:$AF$1355,A148,1))","v":15.112966125757614},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A148,1),INDEX(LinMotor!$AG$1:$AG$1355,A148,1))","v":44.506512354232562},{"$f":"IF(A148<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A148,1),INDEX(LinMotor!$AI$1:$AI$1355,A148,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A148,1),INDEX(LinMotor!$AI$1:$AI$1355,A148,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A148,1),INDEX(LinMotor!$AI$1:$AI$1355,A148,1))/1000,\"0.0k\")),\"\")","v":23.049002172390853},{"$f":"IF(A148<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A148,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A148,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A148,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A148,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A148,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A148,1))/1000,\"0.0k\")),\"\")","v":2.4285997432823918},{"$f":"IF(A148<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A148,1),INDEX(LinMotor!$AK$1:$AK$1355,A148,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A148,1),INDEX(LinMotor!$AK$1:$AK$1355,A148,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A148,1),INDEX(LinMotor!$AK$1:$AK$1355,A148,1))/1000,\"0.0k\")),\"\")","v":148.77422131070654},""]
[76,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A149,1),INDEX(LinMotor!$B$1:$B$1341,A149,1))","v":"AKM53G"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A149,1),INDEX(LinMotor!$R$1:$R$1355,A149,1))","v":123.62637362637362},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A149,1),INDEX(LinMotor!$S$1:$S$1355,A149,1))","v":0.87206785109646634},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A149,1),INDEX(LinMotor!$T$1:$T$1355,A149,1))","v":0.98577571016835019},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A149,1),INDEX(LinMotor!$U$1:$U$1355,A149,1))","v":6.1812271595071577E-2},{"$f":"IF(A149<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A149,1),INDEX(LinMotor!$V$1:$V$1355,A149,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A149,1),INDEX(LinMotor!$V$1:$V$1355,A149,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A149,1),INDEX(LinMotor!$V$1:$V$1355,A149,1))/1000,\"0.0k\")),\"\")","v":-22.737701965432098},{"$f":"IF(A149<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A149,1),INDEX(LinMotor!$W$1:$W$1355,A149,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A149,1),INDEX(LinMotor!$X$1:$X$1355,A149,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A149,1),INDEX(LinMotor!$W$1:$W$1355,A149,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A149,1),INDEX(LinMotor!$X$1:$X$1355,A149,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A149,1),INDEX(LinMotor!$W$1:$W$1355,A149,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A149,1),INDEX(LinMotor!$X$1:$X$1355,A149,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A149<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A149,1),INDEX(LinMotor!$X$1:$X$1355,A149,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A149,1),INDEX(LinMotor!$Z$1:$Z$1355,A149,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A149,1),INDEX(LinMotor!$X$1:$X$1355,A149,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A149,1),INDEX(LinMotor!$Z$1:$Z$1355,A149,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A149,1),INDEX(LinMotor!$X$1:$X$1355,A149,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A149,1),INDEX(LinMotor!$Z$1:$Z$1355,A149,1)))/1000,\"0.0k\")),\"\")","v":29.277538591999999},{"$f":"IF(A149<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A149,1),INDEX(LinMotor!$Y$1:$Y$1355,A149,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A149,1),INDEX(LinMotor!$AB$1:$AB$445,A149,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A149,1),INDEX(LinMotor!$Y$1:$Y$1355,A149,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A149,1),INDEX(LinMotor!$AB$1:$AB$445,A149,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A149,1),INDEX(LinMotor!$Y$1:$Y$1355,A149,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A149,1),INDEX(LinMotor!$AB$1:$AB$445,A149,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A149,1),INDEX(LinMotor!$AD$1:$AD$1355,A149,1))","v":0.1730620689625417},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A149,1),INDEX(LinMotor!$AE$1:$AE$1355,A149,1))","v":0.25521538575263153},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A149,1),INDEX(LinMotor!$AF$1:$AF$1355,A149,1))","v":4.1534896551010005},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A149,1),INDEX(LinMotor!$AG$1:$AG$1355,A149,1))","v":12.250338516126314},{"$f":"IF(A149<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A149,1),INDEX(LinMotor!$AI$1:$AI$1355,A149,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A149,1),INDEX(LinMotor!$AI$1:$AI$1355,A149,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A149,1),INDEX(LinMotor!$AI$1:$AI$1355,A149,1))/1000,\"0.0k\")),\"\")","v":23.060826574487265},{"$f":"IF(A149<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A149,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A149,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A149,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A149,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A149,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A149,1))/1000,\"0.0k\")),\"\")","v":2.4387820412655792},{"$f":"IF(A149<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A149,1),INDEX(LinMotor!$AK$1:$AK$1355,A149,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A149,1),INDEX(LinMotor!$AK$1:$AK$1355,A149,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A149,1),INDEX(LinMotor!$AK$1:$AK$1355,A149,1))/1000,\"0.0k\")),\"\")","v":149.39798134271362},""]
[77,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A150,1),INDEX(LinMotor!$B$1:$B$1341,A150,1))","v":"AKM53H"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A150,1),INDEX(LinMotor!$R$1:$R$1355,A150,1))","v":123.62637362637362},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A150,1),INDEX(LinMotor!$S$1:$S$1355,A150,1))","v":0.86391845885031904},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A150,1),INDEX(LinMotor!$T$1:$T$1355,A150,1))","v":0.97591795306666662},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A150,1),INDEX(LinMotor!$U$1:$U$1355,A150,1))","v":4.442470055860244E-2},{"$f":"IF(A150<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A150,1),INDEX(LinMotor!$V$1:$V$1355,A150,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A150,1),INDEX(LinMotor!$V$1:$V$1355,A150,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A150,1),INDEX(LinMotor!$V$1:$V$1355,A150,1))/1000,\"0.0k\")),\"\")","v":-22.737701965432098},{"$f":"IF(A150<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A150,1),INDEX(LinMotor!$W$1:$W$1355,A150,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A150,1),INDEX(LinMotor!$X$1:$X$1355,A150,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A150,1),INDEX(LinMotor!$W$1:$W$1355,A150,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A150,1),INDEX(LinMotor!$X$1:$X$1355,A150,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A150,1),INDEX(LinMotor!$W$1:$W$1355,A150,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A150,1),INDEX(LinMotor!$X$1:$X$1355,A150,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A150<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A150,1),INDEX(LinMotor!$X$1:$X$1355,A150,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A150,1),INDEX(LinMotor!$Z$1:$Z$1355,A150,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A150,1),INDEX(LinMotor!$X$1:$X$1355,A150,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A150,1),INDEX(LinMotor!$Z$1:$Z$1355,A150,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A150,1),INDEX(LinMotor!$X$1:$X$1355,A150,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A150,1),INDEX(LinMotor!$Z$1:$Z$1355,A150,1)))/1000,\"0.0k\")),\"\")","v":29.277538591999999},{"$f":"IF(A150<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A150,1),INDEX(LinMotor!$Y$1:$Y$1355,A150,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A150,1),INDEX(LinMotor!$AB$1:$AB$445,A150,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A150,1),INDEX(LinMotor!$Y$1:$Y$1355,A150,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A150,1),INDEX(LinMotor!$AB$1:$AB$445,A150,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A150,1),INDEX(LinMotor!$Y$1:$Y$1355,A150,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A150,1),INDEX(LinMotor!$AB$1:$AB$445,A150,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A150,1),INDEX(LinMotor!$AD$1:$AD$1355,A150,1))","v":0.23716848294786305},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A150,1),INDEX(LinMotor!$AE$1:$AE$1355,A150,1))","v":0.3497533932580365},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A150,1),INDEX(LinMotor!$AF$1:$AF$1355,A150,1))","v":5.692043590748713},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A150,1),INDEX(LinMotor!$AG$1:$AG$1355,A150,1))","v":16.788162876385751},{"$f":"IF(A150<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A150,1),INDEX(LinMotor!$AI$1:$AI$1355,A150,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A150,1),INDEX(LinMotor!$AI$1:$AI$1355,A150,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A150,1),INDEX(LinMotor!$AI$1:$AI$1355,A150,1))/1000,\"0.0k\")),\"\")","v":23.060826574487265},{"$f":"IF(A150<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A150,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A150,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A150,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A150,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A150,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A150,1))/1000,\"0.0k\")),\"\")","v":2.4387820412655792},{"$f":"IF(A150<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A150,1),INDEX(LinMotor!$AK$1:$AK$1355,A150,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A150,1),INDEX(LinMotor!$AK$1:$AK$1355,A150,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A150,1),INDEX(LinMotor!$AK$1:$AK$1355,A150,1))/1000,\"0.0k\")),\"\")","v":149.39798134271362},""]
[1185,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A151,1),INDEX(LinMotor!$B$1:$B$1341,A151,1))","v":"KBMS-60S01-A (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A151,1),INDEX(LinMotor!$R$1:$R$1355,A151,1))","v":4.39453125},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A151,1),INDEX(LinMotor!$S$1:$S$1355,A151,1))","v":0.19364710659197532},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A151,1),INDEX(LinMotor!$T$1:$T$1355,A151,1))","v":0.27043457259842518},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A151,1),INDEX(LinMotor!$U$1:$U$1355,A151,1))","v":0.12952589468312947},{"$f":"IF(A151<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A151,1),INDEX(LinMotor!$V$1:$V$1355,A151,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A151,1),INDEX(LinMotor!$V$1:$V$1355,A151,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A151,1),INDEX(LinMotor!$V$1:$V$1355,A151,1))/1000,\"0.0k\")),\"\")","v":-28.994062617283944},{"$f":"IF(A151<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A151,1),INDEX(LinMotor!$W$1:$W$1355,A151,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A151,1),INDEX(LinMotor!$X$1:$X$1355,A151,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A151,1),INDEX(LinMotor!$W$1:$W$1355,A151,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A151,1),INDEX(LinMotor!$X$1:$X$1355,A151,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A151,1),INDEX(LinMotor!$W$1:$W$1355,A151,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A151,1),INDEX(LinMotor!$X$1:$X$1355,A151,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A151<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A151,1),INDEX(LinMotor!$X$1:$X$1355,A151,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A151,1),INDEX(LinMotor!$Z$1:$Z$1355,A151,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A151,1),INDEX(LinMotor!$X$1:$X$1355,A151,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A151,1),INDEX(LinMotor!$Z$1:$Z$1355,A151,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A151,1),INDEX(LinMotor!$X$1:$X$1355,A151,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A151,1),INDEX(LinMotor!$Z$1:$Z$1355,A151,1)))/1000,\"0.0k\")),\"\")","v":34.345190719999998},{"$f":"IF(A151<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A151,1),INDEX(LinMotor!$Y$1:$Y$1355,A151,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A151,1),INDEX(LinMotor!$AB$1:$AB$445,A151,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A151,1),INDEX(LinMotor!$Y$1:$Y$1355,A151,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A151,1),INDEX(LinMotor!$AB$1:$AB$445,A151,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A151,1),INDEX(LinMotor!$Y$1:$Y$1355,A151,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A151,1),INDEX(LinMotor!$AB$1:$AB$445,A151,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A151,1),INDEX(LinMotor!$AD$1:$AD$1355,A151,1))","v":0.1099008313581336},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A151,1),INDEX(LinMotor!$AE$1:$AE$1355,A151,1))","v":0.18153129354320985},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A151,1),INDEX(LinMotor!$AF$1:$AF$1355,A151,1))","v":2.6376199525952062},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A151,1),INDEX(LinMotor!$AG$1:$AG$1355,A151,1))","v":8.7135020900740727},{"$f":"IF(A151<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A151,1),INDEX(LinMotor!$AI$1:$AI$1355,A151,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A151,1),INDEX(LinMotor!$AI$1:$AI$1355,A151,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A151,1),INDEX(LinMotor!$AI$1:$AI$1355,A151,1))/1000,\"0.0k\")),\"\")","v":24.152421342923351},{"$f":"IF(A151<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A151,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A151,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A151,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A151,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A151,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A151,1))/1000,\"0.0k\")),\"\")","v":3.3056818247307},{"$f":"IF(A151<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A151,1),INDEX(LinMotor!$AK$1:$AK$1355,A151,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A151,1),INDEX(LinMotor!$AK$1:$AK$1355,A151,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A151,1),INDEX(LinMotor!$AK$1:$AK$1355,A151,1))/1000,\"0.0k\")),\"\")","v":202.50361992979919},""]
[1186,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A152,1),INDEX(LinMotor!$B$1:$B$1341,A152,1))","v":"KBMS-60S02-A (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A152,1),INDEX(LinMotor!$R$1:$R$1355,A152,1))","v":2.6785714285714284},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A152,1),INDEX(LinMotor!$S$1:$S$1355,A152,1))","v":0.10013707798134101},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A152,1),INDEX(LinMotor!$T$1:$T$1355,A152,1))","v":0.14788749176470589},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A152,1),INDEX(LinMotor!$U$1:$U$1355,A152,1))","v":0.21802046998889771},{"$f":"IF(A152<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A152,1),INDEX(LinMotor!$V$1:$V$1355,A152,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A152,1),INDEX(LinMotor!$V$1:$V$1355,A152,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A152,1),INDEX(LinMotor!$V$1:$V$1355,A152,1))/1000,\"0.0k\")),\"\")","v":-33.149765925925927},{"$f":"IF(A152<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A152,1),INDEX(LinMotor!$W$1:$W$1355,A152,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A152,1),INDEX(LinMotor!$X$1:$X$1355,A152,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A152,1),INDEX(LinMotor!$W$1:$W$1355,A152,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A152,1),INDEX(LinMotor!$X$1:$X$1355,A152,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A152,1),INDEX(LinMotor!$W$1:$W$1355,A152,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A152,1),INDEX(LinMotor!$X$1:$X$1355,A152,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A152<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A152,1),INDEX(LinMotor!$X$1:$X$1355,A152,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A152,1),INDEX(LinMotor!$Z$1:$Z$1355,A152,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A152,1),INDEX(LinMotor!$X$1:$X$1355,A152,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A152,1),INDEX(LinMotor!$Z$1:$Z$1355,A152,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A152,1),INDEX(LinMotor!$X$1:$X$1355,A152,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A152,1),INDEX(LinMotor!$Z$1:$Z$1355,A152,1)))/1000,\"0.0k\")),\"\")","v":37.711310400000002},{"$f":"IF(A152<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A152,1),INDEX(LinMotor!$Y$1:$Y$1355,A152,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A152,1),INDEX(LinMotor!$AB$1:$AB$445,A152,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A152,1),INDEX(LinMotor!$Y$1:$Y$1355,A152,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A152,1),INDEX(LinMotor!$AB$1:$AB$445,A152,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A152,1),INDEX(LinMotor!$Y$1:$Y$1355,A152,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A152,1),INDEX(LinMotor!$AB$1:$AB$445,A152,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A152,1),INDEX(LinMotor!$AD$1:$AD$1355,A152,1))","v":6.7988472955146151E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A152,1),INDEX(LinMotor!$AE$1:$AE$1355,A152,1))","v":0.11930275666666666},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A152,1),INDEX(LinMotor!$AF$1:$AF$1355,A152,1))","v":1.6317233509235076},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A152,1),INDEX(LinMotor!$AG$1:$AG$1355,A152,1))","v":5.7265323199999996},{"$f":"IF(A152<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A152,1),INDEX(LinMotor!$AI$1:$AI$1355,A152,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A152,1),INDEX(LinMotor!$AI$1:$AI$1355,A152,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A152,1),INDEX(LinMotor!$AI$1:$AI$1355,A152,1))/1000,\"0.0k\")),\"\")","v":24.963283009110185},{"$f":"IF(A152<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A152,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A152,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A152,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A152,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A152,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A152,1))/1000,\"0.0k\")),\"\")","v":3.8815083313660983},{"$f":"IF(A152<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A152,1),INDEX(LinMotor!$AK$1:$AK$1355,A152,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A152,1),INDEX(LinMotor!$AK$1:$AK$1355,A152,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A152,1),INDEX(LinMotor!$AK$1:$AK$1355,A152,1))/1000,\"0.0k\")),\"\")","v":237.77832518813062},""]
[1187,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A153,1),INDEX(LinMotor!$B$1:$B$1341,A153,1))","v":"KBMS-60S03-A (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A153,1),INDEX(LinMotor!$R$1:$R$1355,A153,1))","v":2.1266540642722118},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A153,1),INDEX(LinMotor!$S$1:$S$1355,A153,1))","v":7.2057038255803937E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A153,1),INDEX(LinMotor!$T$1:$T$1355,A153,1))","v":0.10165025058524174},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A153,1),INDEX(LinMotor!$U$1:$U$1355,A153,1))","v":0.27264230079982071},{"$f":"IF(A153<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A153,1),INDEX(LinMotor!$V$1:$V$1355,A153,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A153,1),INDEX(LinMotor!$V$1:$V$1355,A153,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A153,1),INDEX(LinMotor!$V$1:$V$1355,A153,1))/1000,\"0.0k\")),\"\")","v":-35.911788246913581},{"$f":"IF(A153<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A153,1),INDEX(LinMotor!$W$1:$W$1355,A153,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A153,1),INDEX(LinMotor!$X$1:$X$1355,A153,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A153,1),INDEX(LinMotor!$W$1:$W$1355,A153,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A153,1),INDEX(LinMotor!$X$1:$X$1355,A153,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A153,1),INDEX(LinMotor!$W$1:$W$1355,A153,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A153,1),INDEX(LinMotor!$X$1:$X$1355,A153,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A153<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A153,1),INDEX(LinMotor!$X$1:$X$1355,A153,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A153,1),INDEX(LinMotor!$Z$1:$Z$1355,A153,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A153,1),INDEX(LinMotor!$X$1:$X$1355,A153,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A153,1),INDEX(LinMotor!$Z$1:$Z$1355,A153,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A153,1),INDEX(LinMotor!$X$1:$X$1355,A153,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A153,1),INDEX(LinMotor!$Z$1:$Z$1355,A153,1)))/1000,\"0.0k\")),\"\")","v":39.948548480000007},{"$f":"IF(A153<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A153,1),INDEX(LinMotor!$Y$1:$Y$1355,A153,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A153,1),INDEX(LinMotor!$AB$1:$AB$445,A153,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A153,1),INDEX(LinMotor!$Y$1:$Y$1355,A153,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A153,1),INDEX(LinMotor!$AB$1:$AB$445,A153,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A153,1),INDEX(LinMotor!$Y$1:$Y$1355,A153,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A153,1),INDEX(LinMotor!$AB$1:$AB$445,A153,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A153,1),INDEX(LinMotor!$AD$1:$AD$1355,A153,1))","v":5.5615150297258283E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A153,1),INDEX(LinMotor!$AE$1:$AE$1355,A153,1))","v":0.10106031609523809},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A153,1),INDEX(LinMotor!$AF$1:$AF$1355,A153,1))","v":1.3347636071341988},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A153,1),INDEX(LinMotor!$AG$1:$AG$1355,A153,1))","v":4.8508951725714287},{"$f":"IF(A153<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A153,1),INDEX(LinMotor!$AI$1:$AI$1355,A153,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A153,1),INDEX(LinMotor!$AI$1:$AI$1355,A153,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A153,1),INDEX(LinMotor!$AI$1:$AI$1355,A153,1))/1000,\"0.0k\")),\"\")","v":25.53634490980976},{"$f":"IF(A153<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A153,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A153,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A153,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A153,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A153,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A153,1))/1000,\"0.0k\")),\"\")","v":4.2642222900445041},{"$f":"IF(A153<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A153,1),INDEX(LinMotor!$AK$1:$AK$1355,A153,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A153,1),INDEX(LinMotor!$AK$1:$AK$1355,A153,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A153,1),INDEX(LinMotor!$AK$1:$AK$1355,A153,1))/1000,\"0.0k\")),\"\")","v":261.22309880494851},""]
[1188,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A154,1),INDEX(LinMotor!$B$1:$B$1341,A154,1))","v":"KBMS-88H01-A (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A154,1),INDEX(LinMotor!$R$1:$R$1355,A154,1))","v":0.77054794520547942},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A154,1),INDEX(LinMotor!$S$1:$S$1355,A154,1))","v":6.644291623879843E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A154,1),INDEX(LinMotor!$T$1:$T$1355,A154,1))","v":0.14372706864674659},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A154,1),INDEX(LinMotor!$U$1:$U$1355,A154,1))","v":0.24323891384701504},{"$f":"IF(A154<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A154,1),INDEX(LinMotor!$V$1:$V$1355,A154,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A154,1),INDEX(LinMotor!$V$1:$V$1355,A154,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A154,1),INDEX(LinMotor!$V$1:$V$1355,A154,1))/1000,\"0.0k\")),\"\")","v":-59.503006419753092},{"$f":"IF(A154<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A154,1),INDEX(LinMotor!$W$1:$W$1355,A154,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A154,1),INDEX(LinMotor!$X$1:$X$1355,A154,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A154,1),INDEX(LinMotor!$W$1:$W$1355,A154,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A154,1),INDEX(LinMotor!$X$1:$X$1355,A154,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A154,1),INDEX(LinMotor!$W$1:$W$1355,A154,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A154,1),INDEX(LinMotor!$X$1:$X$1355,A154,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A154<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A154,1),INDEX(LinMotor!$X$1:$X$1355,A154,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A154,1),INDEX(LinMotor!$Z$1:$Z$1355,A154,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A154,1),INDEX(LinMotor!$X$1:$X$1355,A154,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A154,1),INDEX(LinMotor!$Z$1:$Z$1355,A154,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A154,1),INDEX(LinMotor!$X$1:$X$1355,A154,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A154,1),INDEX(LinMotor!$Z$1:$Z$1355,A154,1)))/1000,\"0.0k\")),\"\")","v":59.0574352},{"$f":"IF(A154<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A154,1),INDEX(LinMotor!$Y$1:$Y$1355,A154,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A154,1),INDEX(LinMotor!$AB$1:$AB$445,A154,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A154,1),INDEX(LinMotor!$Y$1:$Y$1355,A154,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A154,1),INDEX(LinMotor!$AB$1:$AB$445,A154,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A154,1),INDEX(LinMotor!$Y$1:$Y$1355,A154,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A154,1),INDEX(LinMotor!$AB$1:$AB$445,A154,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A154,1),INDEX(LinMotor!$AD$1:$AD$1355,A154,1))","v":4.6552447403057966E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A154,1),INDEX(LinMotor!$AE$1:$AE$1355,A154,1))","v":0.10279990946502059},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A154,1),INDEX(LinMotor!$AF$1:$AF$1355,A154,1))","v":1.1172587376733911},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A154,1),INDEX(LinMotor!$AG$1:$AG$1355,A154,1))","v":4.9343956543209879},{"$f":"IF(A154<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A154,1),INDEX(LinMotor!$AI$1:$AI$1355,A154,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A154,1),INDEX(LinMotor!$AI$1:$AI$1355,A154,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A154,1),INDEX(LinMotor!$AI$1:$AI$1355,A154,1))/1000,\"0.0k\")),\"\")","v":31.299252364547094},{"$f":"IF(A154<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A154,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A154,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A154,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A154,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A154,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A154,1))/1000,\"0.0k\")),\"\")","v":7.5330910563710658},{"$f":"IF(A154<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A154,1),INDEX(LinMotor!$AK$1:$AK$1355,A154,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A154,1),INDEX(LinMotor!$AK$1:$AK$1355,A154,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A154,1),INDEX(LinMotor!$AK$1:$AK$1355,A154,1))/1000,\"0.0k\")),\"\")","v":461.47157804584231},""]
[1189,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A155,1),INDEX(LinMotor!$B$1:$B$1341,A155,1))","v":"KBMS-88H01-A (480 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A155,1),INDEX(LinMotor!$R$1:$R$1355,A155,1))","v":0.77054794520547942},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A155,1),INDEX(LinMotor!$S$1:$S$1355,A155,1))","v":6.6463644417627463E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A155,1),INDEX(LinMotor!$T$1:$T$1355,A155,1))","v":0.14372706864674659},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A155,1),INDEX(LinMotor!$U$1:$U$1355,A155,1))","v":0.24323891384701504},{"$f":"IF(A155<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A155,1),INDEX(LinMotor!$V$1:$V$1355,A155,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A155,1),INDEX(LinMotor!$V$1:$V$1355,A155,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A155,1),INDEX(LinMotor!$V$1:$V$1355,A155,1))/1000,\"0.0k\")),\"\")","v":-59.503006419753092},{"$f":"IF(A155<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A155,1),INDEX(LinMotor!$W$1:$W$1355,A155,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A155,1),INDEX(LinMotor!$X$1:$X$1355,A155,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A155,1),INDEX(LinMotor!$W$1:$W$1355,A155,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A155,1),INDEX(LinMotor!$X$1:$X$1355,A155,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A155,1),INDEX(LinMotor!$W$1:$W$1355,A155,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A155,1),INDEX(LinMotor!$X$1:$X$1355,A155,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A155<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A155,1),INDEX(LinMotor!$X$1:$X$1355,A155,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A155,1),INDEX(LinMotor!$Z$1:$Z$1355,A155,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A155,1),INDEX(LinMotor!$X$1:$X$1355,A155,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A155,1),INDEX(LinMotor!$Z$1:$Z$1355,A155,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A155,1),INDEX(LinMotor!$X$1:$X$1355,A155,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A155,1),INDEX(LinMotor!$Z$1:$Z$1355,A155,1)))/1000,\"0.0k\")),\"\")","v":59.0574352},{"$f":"IF(A155<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A155,1),INDEX(LinMotor!$Y$1:$Y$1355,A155,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A155,1),INDEX(LinMotor!$AB$1:$AB$445,A155,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A155,1),INDEX(LinMotor!$Y$1:$Y$1355,A155,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A155,1),INDEX(LinMotor!$AB$1:$AB$445,A155,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A155,1),INDEX(LinMotor!$Y$1:$Y$1355,A155,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A155,1),INDEX(LinMotor!$AB$1:$AB$445,A155,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A155,1),INDEX(LinMotor!$AD$1:$AD$1355,A155,1))","v":4.6552447403057966E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A155,1),INDEX(LinMotor!$AE$1:$AE$1355,A155,1))","v":0.10279990946502059},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A155,1),INDEX(LinMotor!$AF$1:$AF$1355,A155,1))","v":1.1172587376733911},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A155,1),INDEX(LinMotor!$AG$1:$AG$1355,A155,1))","v":4.9343956543209879},{"$f":"IF(A155<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A155,1),INDEX(LinMotor!$AI$1:$AI$1355,A155,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A155,1),INDEX(LinMotor!$AI$1:$AI$1355,A155,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A155,1),INDEX(LinMotor!$AI$1:$AI$1355,A155,1))/1000,\"0.0k\")),\"\")","v":31.299252364547094},{"$f":"IF(A155<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A155,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A155,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A155,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A155,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A155,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A155,1))/1000,\"0.0k\")),\"\")","v":7.5330910563710658},{"$f":"IF(A155<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A155,1),INDEX(LinMotor!$AK$1:$AK$1355,A155,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A155,1),INDEX(LinMotor!$AK$1:$AK$1355,A155,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A155,1),INDEX(LinMotor!$AK$1:$AK$1355,A155,1))/1000,\"0.0k\")),\"\")","v":461.47157804584231},""]
[1192,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A156,1),INDEX(LinMotor!$B$1:$B$1341,A156,1))","v":"KBMS-88H02-A (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A156,1),INDEX(LinMotor!$R$1:$R$1355,A156,1))","v":0.45546558704453444},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A156,1),INDEX(LinMotor!$S$1:$S$1355,A156,1))","v":4.3979424496109483E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A156,1),INDEX(LinMotor!$T$1:$T$1355,A156,1))","v":0.10785305105697163},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A156,1),INDEX(LinMotor!$U$1:$U$1355,A156,1))","v":0.51232944803983316},{"$f":"IF(A156<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A156,1),INDEX(LinMotor!$V$1:$V$1355,A156,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A156,1),INDEX(LinMotor!$V$1:$V$1355,A156,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A156,1),INDEX(LinMotor!$V$1:$V$1355,A156,1))/1000,\"0.0k\")),\"\")","v":-85.096057283950614},{"$f":"IF(A156<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A156,1),INDEX(LinMotor!$W$1:$W$1355,A156,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A156,1),INDEX(LinMotor!$X$1:$X$1355,A156,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A156,1),INDEX(LinMotor!$W$1:$W$1355,A156,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A156,1),INDEX(LinMotor!$X$1:$X$1355,A156,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A156,1),INDEX(LinMotor!$W$1:$W$1355,A156,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A156,1),INDEX(LinMotor!$X$1:$X$1355,A156,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A156<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A156,1),INDEX(LinMotor!$X$1:$X$1355,A156,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A156,1),INDEX(LinMotor!$Z$1:$Z$1355,A156,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A156,1),INDEX(LinMotor!$X$1:$X$1355,A156,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A156,1),INDEX(LinMotor!$Z$1:$Z$1355,A156,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A156,1),INDEX(LinMotor!$X$1:$X$1355,A156,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A156,1),INDEX(LinMotor!$Z$1:$Z$1355,A156,1)))/1000,\"0.0k\")),\"\")","v":79.787806400000008},{"$f":"IF(A156<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A156,1),INDEX(LinMotor!$Y$1:$Y$1355,A156,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A156,1),INDEX(LinMotor!$AB$1:$AB$445,A156,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A156,1),INDEX(LinMotor!$Y$1:$Y$1355,A156,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A156,1),INDEX(LinMotor!$AB$1:$AB$445,A156,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A156,1),INDEX(LinMotor!$Y$1:$Y$1355,A156,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A156,1),INDEX(LinMotor!$AB$1:$AB$445,A156,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A156,1),INDEX(LinMotor!$AD$1:$AD$1355,A156,1))","v":2.7042897955173954E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A156,1),INDEX(LinMotor!$AE$1:$AE$1355,A156,1))","v":6.9071475068141722E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A156,1),INDEX(LinMotor!$AF$1:$AF$1355,A156,1))","v":0.64902955092417491},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A156,1),INDEX(LinMotor!$AG$1:$AG$1355,A156,1))","v":3.3154308032708029},{"$f":"IF(A156<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A156,1),INDEX(LinMotor!$AI$1:$AI$1355,A156,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A156,1),INDEX(LinMotor!$AI$1:$AI$1355,A156,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A156,1),INDEX(LinMotor!$AI$1:$AI$1355,A156,1))/1000,\"0.0k\")),\"\")","v":38.699843242509104},{"$f":"IF(A156<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A156,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A156,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A156,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A156,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A156,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A156,1))/1000,\"0.0k\")),\"\")","v":11.079339664308581},{"$f":"IF(A156<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A156,1),INDEX(LinMotor!$AK$1:$AK$1355,A156,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A156,1),INDEX(LinMotor!$AK$1:$AK$1355,A156,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A156,1),INDEX(LinMotor!$AK$1:$AK$1355,A156,1))/1000,\"0.0k\")),\"\")","v":678.71214091727381},""]
[1193,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A157,1),INDEX(LinMotor!$B$1:$B$1341,A157,1))","v":"KBMS-88H02-A (480 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A157,1),INDEX(LinMotor!$R$1:$R$1355,A157,1))","v":0.45546558704453444},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A157,1),INDEX(LinMotor!$S$1:$S$1355,A157,1))","v":4.3936070001107289E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A157,1),INDEX(LinMotor!$T$1:$T$1355,A157,1))","v":0.10785305105697163},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A157,1),INDEX(LinMotor!$U$1:$U$1355,A157,1))","v":0.51232944803983316},{"$f":"IF(A157<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A157,1),INDEX(LinMotor!$V$1:$V$1355,A157,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A157,1),INDEX(LinMotor!$V$1:$V$1355,A157,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A157,1),INDEX(LinMotor!$V$1:$V$1355,A157,1))/1000,\"0.0k\")),\"\")","v":-85.096057283950614},{"$f":"IF(A157<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A157,1),INDEX(LinMotor!$W$1:$W$1355,A157,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A157,1),INDEX(LinMotor!$X$1:$X$1355,A157,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A157,1),INDEX(LinMotor!$W$1:$W$1355,A157,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A157,1),INDEX(LinMotor!$X$1:$X$1355,A157,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A157,1),INDEX(LinMotor!$W$1:$W$1355,A157,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A157,1),INDEX(LinMotor!$X$1:$X$1355,A157,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A157<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A157,1),INDEX(LinMotor!$X$1:$X$1355,A157,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A157,1),INDEX(LinMotor!$Z$1:$Z$1355,A157,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A157,1),INDEX(LinMotor!$X$1:$X$1355,A157,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A157,1),INDEX(LinMotor!$Z$1:$Z$1355,A157,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A157,1),INDEX(LinMotor!$X$1:$X$1355,A157,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A157,1),INDEX(LinMotor!$Z$1:$Z$1355,A157,1)))/1000,\"0.0k\")),\"\")","v":79.787806400000008},{"$f":"IF(A157<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A157,1),INDEX(LinMotor!$Y$1:$Y$1355,A157,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A157,1),INDEX(LinMotor!$AB$1:$AB$445,A157,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A157,1),INDEX(LinMotor!$Y$1:$Y$1355,A157,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A157,1),INDEX(LinMotor!$AB$1:$AB$445,A157,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A157,1),INDEX(LinMotor!$Y$1:$Y$1355,A157,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A157,1),INDEX(LinMotor!$AB$1:$AB$445,A157,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A157,1),INDEX(LinMotor!$AD$1:$AD$1355,A157,1))","v":2.7042897955173954E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A157,1),INDEX(LinMotor!$AE$1:$AE$1355,A157,1))","v":6.9071475068141722E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A157,1),INDEX(LinMotor!$AF$1:$AF$1355,A157,1))","v":0.64902955092417491},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A157,1),INDEX(LinMotor!$AG$1:$AG$1355,A157,1))","v":3.3154308032708029},{"$f":"IF(A157<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A157,1),INDEX(LinMotor!$AI$1:$AI$1355,A157,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A157,1),INDEX(LinMotor!$AI$1:$AI$1355,A157,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A157,1),INDEX(LinMotor!$AI$1:$AI$1355,A157,1))/1000,\"0.0k\")),\"\")","v":38.699843242509104},{"$f":"IF(A157<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A157,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A157,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A157,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A157,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A157,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A157,1))/1000,\"0.0k\")),\"\")","v":11.079339664308581},{"$f":"IF(A157<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A157,1),INDEX(LinMotor!$AK$1:$AK$1355,A157,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A157,1),INDEX(LinMotor!$AK$1:$AK$1355,A157,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A157,1),INDEX(LinMotor!$AK$1:$AK$1355,A157,1))/1000,\"0.0k\")),\"\")","v":678.71214091727381},""]
[1196,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A158,1),INDEX(LinMotor!$B$1:$B$1341,A158,1))","v":"KBMS-88H03-A (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A158,1),INDEX(LinMotor!$R$1:$R$1355,A158,1))","v":0.35714285714285715},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A158,1),INDEX(LinMotor!$S$1:$S$1355,A158,1))","v":3.5936063205761037E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A158,1),INDEX(LinMotor!$T$1:$T$1355,A158,1))","v":8.5272518518518525E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A158,1),INDEX(LinMotor!$U$1:$U$1355,A158,1))","v":0.59363818298226667},{"$f":"IF(A158<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A158,1),INDEX(LinMotor!$V$1:$V$1355,A158,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A158,1),INDEX(LinMotor!$V$1:$V$1355,A158,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A158,1),INDEX(LinMotor!$V$1:$V$1355,A158,1))/1000,\"0.0k\")),\"\")","v":-102.32702222222223},{"$f":"IF(A158<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A158,1),INDEX(LinMotor!$W$1:$W$1355,A158,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A158,1),INDEX(LinMotor!$X$1:$X$1355,A158,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A158,1),INDEX(LinMotor!$W$1:$W$1355,A158,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A158,1),INDEX(LinMotor!$X$1:$X$1355,A158,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A158,1),INDEX(LinMotor!$W$1:$W$1355,A158,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A158,1),INDEX(LinMotor!$X$1:$X$1355,A158,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A158<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A158,1),INDEX(LinMotor!$X$1:$X$1355,A158,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A158,1),INDEX(LinMotor!$Z$1:$Z$1355,A158,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A158,1),INDEX(LinMotor!$X$1:$X$1355,A158,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A158,1),INDEX(LinMotor!$Z$1:$Z$1355,A158,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A158,1),INDEX(LinMotor!$X$1:$X$1355,A158,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A158,1),INDEX(LinMotor!$Z$1:$Z$1355,A158,1)))/1000,\"0.0k\")),\"\")","v":93.744888000000003},{"$f":"IF(A158<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A158,1),INDEX(LinMotor!$Y$1:$Y$1355,A158,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A158,1),INDEX(LinMotor!$AB$1:$AB$445,A158,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A158,1),INDEX(LinMotor!$Y$1:$Y$1355,A158,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A158,1),INDEX(LinMotor!$AB$1:$AB$445,A158,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A158,1),INDEX(LinMotor!$Y$1:$Y$1355,A158,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A158,1),INDEX(LinMotor!$AB$1:$AB$445,A158,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A158,1),INDEX(LinMotor!$AD$1:$AD$1355,A158,1))","v":2.6589826021676453E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A158,1),INDEX(LinMotor!$AE$1:$AE$1355,A158,1))","v":7.1720845036486305E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A158,1),INDEX(LinMotor!$AF$1:$AF$1355,A158,1))","v":0.63815582452023489},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A158,1),INDEX(LinMotor!$AG$1:$AG$1355,A158,1))","v":3.4426005617513429},{"$f":"IF(A158<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A158,1),INDEX(LinMotor!$AI$1:$AI$1355,A158,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A158,1),INDEX(LinMotor!$AI$1:$AI$1355,A158,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A158,1),INDEX(LinMotor!$AI$1:$AI$1355,A158,1))/1000,\"0.0k\")),\"\")","v":44.066210284047393},{"$f":"IF(A158<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A158,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A158,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A158,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A158,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A158,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A158,1))/1000,\"0.0k\")),\"\")","v":13.466912984504134},{"$f":"IF(A158<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A158,1),INDEX(LinMotor!$AK$1:$AK$1355,A158,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A158,1),INDEX(LinMotor!$AK$1:$AK$1355,A158,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A158,1),INDEX(LinMotor!$AK$1:$AK$1355,A158,1))/1000,\"0.0k\")),\"\")","v":824.97311393962366},""]
[1197,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A159,1),INDEX(LinMotor!$B$1:$B$1341,A159,1))","v":"KBMS-88H03-A (480 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A159,1),INDEX(LinMotor!$R$1:$R$1355,A159,1))","v":0.35714285714285715},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A159,1),INDEX(LinMotor!$S$1:$S$1355,A159,1))","v":3.5881404238794525E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A159,1),INDEX(LinMotor!$T$1:$T$1355,A159,1))","v":8.5272518518518525E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A159,1),INDEX(LinMotor!$U$1:$U$1355,A159,1))","v":0.59363818298226667},{"$f":"IF(A159<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A159,1),INDEX(LinMotor!$V$1:$V$1355,A159,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A159,1),INDEX(LinMotor!$V$1:$V$1355,A159,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A159,1),INDEX(LinMotor!$V$1:$V$1355,A159,1))/1000,\"0.0k\")),\"\")","v":-102.32702222222223},{"$f":"IF(A159<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A159,1),INDEX(LinMotor!$W$1:$W$1355,A159,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A159,1),INDEX(LinMotor!$X$1:$X$1355,A159,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A159,1),INDEX(LinMotor!$W$1:$W$1355,A159,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A159,1),INDEX(LinMotor!$X$1:$X$1355,A159,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A159,1),INDEX(LinMotor!$W$1:$W$1355,A159,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A159,1),INDEX(LinMotor!$X$1:$X$1355,A159,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A159<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A159,1),INDEX(LinMotor!$X$1:$X$1355,A159,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A159,1),INDEX(LinMotor!$Z$1:$Z$1355,A159,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A159,1),INDEX(LinMotor!$X$1:$X$1355,A159,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A159,1),INDEX(LinMotor!$Z$1:$Z$1355,A159,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A159,1),INDEX(LinMotor!$X$1:$X$1355,A159,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A159,1),INDEX(LinMotor!$Z$1:$Z$1355,A159,1)))/1000,\"0.0k\")),\"\")","v":93.744888000000003},{"$f":"IF(A159<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A159,1),INDEX(LinMotor!$Y$1:$Y$1355,A159,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A159,1),INDEX(LinMotor!$AB$1:$AB$445,A159,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A159,1),INDEX(LinMotor!$Y$1:$Y$1355,A159,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A159,1),INDEX(LinMotor!$AB$1:$AB$445,A159,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A159,1),INDEX(LinMotor!$Y$1:$Y$1355,A159,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A159,1),INDEX(LinMotor!$AB$1:$AB$445,A159,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A159,1),INDEX(LinMotor!$AD$1:$AD$1355,A159,1))","v":2.6589826021676453E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A159,1),INDEX(LinMotor!$AE$1:$AE$1355,A159,1))","v":7.1720845036486305E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A159,1),INDEX(LinMotor!$AF$1:$AF$1355,A159,1))","v":0.63815582452023489},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A159,1),INDEX(LinMotor!$AG$1:$AG$1355,A159,1))","v":3.4426005617513429},{"$f":"IF(A159<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A159,1),INDEX(LinMotor!$AI$1:$AI$1355,A159,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A159,1),INDEX(LinMotor!$AI$1:$AI$1355,A159,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A159,1),INDEX(LinMotor!$AI$1:$AI$1355,A159,1))/1000,\"0.0k\")),\"\")","v":44.066210284047393},{"$f":"IF(A159<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A159,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A159,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A159,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A159,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A159,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A159,1))/1000,\"0.0k\")),\"\")","v":13.466912984504134},{"$f":"IF(A159<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A159,1),INDEX(LinMotor!$AK$1:$AK$1355,A159,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A159,1),INDEX(LinMotor!$AK$1:$AK$1355,A159,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A159,1),INDEX(LinMotor!$AK$1:$AK$1355,A159,1))/1000,\"0.0k\")),\"\")","v":824.97311393962366},""]
[1198,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A160,1),INDEX(LinMotor!$B$1:$B$1341,A160,1))","v":"KBMS-88H03-B (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A160,1),INDEX(LinMotor!$R$1:$R$1355,A160,1))","v":0.35714285714285715},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A160,1),INDEX(LinMotor!$S$1:$S$1355,A160,1))","v":3.5408028164731389E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A160,1),INDEX(LinMotor!$T$1:$T$1355,A160,1))","v":8.5272518518518525E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A160,1),INDEX(LinMotor!$U$1:$U$1355,A160,1))","v":0.30696311074720145},{"$f":"IF(A160<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A160,1),INDEX(LinMotor!$V$1:$V$1355,A160,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A160,1),INDEX(LinMotor!$V$1:$V$1355,A160,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A160,1),INDEX(LinMotor!$V$1:$V$1355,A160,1))/1000,\"0.0k\")),\"\")","v":-102.32702222222223},{"$f":"IF(A160<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A160,1),INDEX(LinMotor!$W$1:$W$1355,A160,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A160,1),INDEX(LinMotor!$X$1:$X$1355,A160,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A160,1),INDEX(LinMotor!$W$1:$W$1355,A160,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A160,1),INDEX(LinMotor!$X$1:$X$1355,A160,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A160,1),INDEX(LinMotor!$W$1:$W$1355,A160,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A160,1),INDEX(LinMotor!$X$1:$X$1355,A160,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A160<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A160,1),INDEX(LinMotor!$X$1:$X$1355,A160,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A160,1),INDEX(LinMotor!$Z$1:$Z$1355,A160,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A160,1),INDEX(LinMotor!$X$1:$X$1355,A160,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A160,1),INDEX(LinMotor!$Z$1:$Z$1355,A160,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A160,1),INDEX(LinMotor!$X$1:$X$1355,A160,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A160,1),INDEX(LinMotor!$Z$1:$Z$1355,A160,1)))/1000,\"0.0k\")),\"\")","v":93.744888000000003},{"$f":"IF(A160<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A160,1),INDEX(LinMotor!$Y$1:$Y$1355,A160,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A160,1),INDEX(LinMotor!$AB$1:$AB$445,A160,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A160,1),INDEX(LinMotor!$Y$1:$Y$1355,A160,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A160,1),INDEX(LinMotor!$AB$1:$AB$445,A160,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A160,1),INDEX(LinMotor!$Y$1:$Y$1355,A160,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A160,1),INDEX(LinMotor!$AB$1:$AB$445,A160,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A160,1),INDEX(LinMotor!$AD$1:$AD$1355,A160,1))","v":5.148148281088738E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A160,1),INDEX(LinMotor!$AE$1:$AE$1355,A160,1))","v":0.13886121134896365},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A160,1),INDEX(LinMotor!$AF$1:$AF$1355,A160,1))","v":1.2355555874612971},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A160,1),INDEX(LinMotor!$AG$1:$AG$1355,A160,1))","v":6.6653381447502547},{"$f":"IF(A160<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A160,1),INDEX(LinMotor!$AI$1:$AI$1355,A160,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A160,1),INDEX(LinMotor!$AI$1:$AI$1355,A160,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A160,1),INDEX(LinMotor!$AI$1:$AI$1355,A160,1))/1000,\"0.0k\")),\"\")","v":44.066210284047393},{"$f":"IF(A160<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A160,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A160,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A160,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A160,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A160,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A160,1))/1000,\"0.0k\")),\"\")","v":13.466912984504134},{"$f":"IF(A160<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A160,1),INDEX(LinMotor!$AK$1:$AK$1355,A160,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A160,1),INDEX(LinMotor!$AK$1:$AK$1355,A160,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A160,1),INDEX(LinMotor!$AK$1:$AK$1355,A160,1))/1000,\"0.0k\")),\"\")","v":824.97311393962366},""]
[1199,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A161,1),INDEX(LinMotor!$B$1:$B$1341,A161,1))","v":"KBMS-88H03-B (480 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A161,1),INDEX(LinMotor!$R$1:$R$1355,A161,1))","v":0.35714285714285715},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A161,1),INDEX(LinMotor!$S$1:$S$1355,A161,1))","v":3.543396135521016E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A161,1),INDEX(LinMotor!$T$1:$T$1355,A161,1))","v":8.5272518518518525E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A161,1),INDEX(LinMotor!$U$1:$U$1355,A161,1))","v":0.30696311074720145},{"$f":"IF(A161<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A161,1),INDEX(LinMotor!$V$1:$V$1355,A161,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A161,1),INDEX(LinMotor!$V$1:$V$1355,A161,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A161,1),INDEX(LinMotor!$V$1:$V$1355,A161,1))/1000,\"0.0k\")),\"\")","v":-102.32702222222223},{"$f":"IF(A161<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A161,1),INDEX(LinMotor!$W$1:$W$1355,A161,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A161,1),INDEX(LinMotor!$X$1:$X$1355,A161,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A161,1),INDEX(LinMotor!$W$1:$W$1355,A161,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A161,1),INDEX(LinMotor!$X$1:$X$1355,A161,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A161,1),INDEX(LinMotor!$W$1:$W$1355,A161,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A161,1),INDEX(LinMotor!$X$1:$X$1355,A161,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A161<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A161,1),INDEX(LinMotor!$X$1:$X$1355,A161,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A161,1),INDEX(LinMotor!$Z$1:$Z$1355,A161,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A161,1),INDEX(LinMotor!$X$1:$X$1355,A161,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A161,1),INDEX(LinMotor!$Z$1:$Z$1355,A161,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A161,1),INDEX(LinMotor!$X$1:$X$1355,A161,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A161,1),INDEX(LinMotor!$Z$1:$Z$1355,A161,1)))/1000,\"0.0k\")),\"\")","v":93.744888000000003},{"$f":"IF(A161<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A161,1),INDEX(LinMotor!$Y$1:$Y$1355,A161,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A161,1),INDEX(LinMotor!$AB$1:$AB$445,A161,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A161,1),INDEX(LinMotor!$Y$1:$Y$1355,A161,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A161,1),INDEX(LinMotor!$AB$1:$AB$445,A161,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A161,1),INDEX(LinMotor!$Y$1:$Y$1355,A161,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A161,1),INDEX(LinMotor!$AB$1:$AB$445,A161,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A161,1),INDEX(LinMotor!$AD$1:$AD$1355,A161,1))","v":5.148148281088738E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A161,1),INDEX(LinMotor!$AE$1:$AE$1355,A161,1))","v":0.13886121134896365},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A161,1),INDEX(LinMotor!$AF$1:$AF$1355,A161,1))","v":1.2355555874612971},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A161,1),INDEX(LinMotor!$AG$1:$AG$1355,A161,1))","v":6.6653381447502547},{"$f":"IF(A161<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A161,1),INDEX(LinMotor!$AI$1:$AI$1355,A161,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A161,1),INDEX(LinMotor!$AI$1:$AI$1355,A161,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A161,1),INDEX(LinMotor!$AI$1:$AI$1355,A161,1))/1000,\"0.0k\")),\"\")","v":44.066210284047393},{"$f":"IF(A161<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A161,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A161,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A161,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A161,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A161,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A161,1))/1000,\"0.0k\")),\"\")","v":13.466912984504134},{"$f":"IF(A161<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A161,1),INDEX(LinMotor!$AK$1:$AK$1355,A161,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A161,1),INDEX(LinMotor!$AK$1:$AK$1355,A161,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A161,1),INDEX(LinMotor!$AK$1:$AK$1355,A161,1))/1000,\"0.0k\")),\"\")","v":824.97311393962366},""]
[1200,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A162,1),INDEX(LinMotor!$B$1:$B$1341,A162,1))","v":"KBMS-88S01-A (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A162,1),INDEX(LinMotor!$R$1:$R$1355,A162,1))","v":0.77054794520547942},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A162,1),INDEX(LinMotor!$S$1:$S$1355,A162,1))","v":6.6543217853561709E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A162,1),INDEX(LinMotor!$T$1:$T$1355,A162,1))","v":0.14372706864674659},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A162,1),INDEX(LinMotor!$U$1:$U$1355,A162,1))","v":0.39176601376466541},{"$f":"IF(A162<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A162,1),INDEX(LinMotor!$V$1:$V$1355,A162,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A162,1),INDEX(LinMotor!$V$1:$V$1355,A162,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A162,1),INDEX(LinMotor!$V$1:$V$1355,A162,1))/1000,\"0.0k\")),\"\")","v":-59.503006419753092},{"$f":"IF(A162<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A162,1),INDEX(LinMotor!$W$1:$W$1355,A162,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A162,1),INDEX(LinMotor!$X$1:$X$1355,A162,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A162,1),INDEX(LinMotor!$W$1:$W$1355,A162,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A162,1),INDEX(LinMotor!$X$1:$X$1355,A162,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A162,1),INDEX(LinMotor!$W$1:$W$1355,A162,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A162,1),INDEX(LinMotor!$X$1:$X$1355,A162,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A162<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A162,1),INDEX(LinMotor!$X$1:$X$1355,A162,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A162,1),INDEX(LinMotor!$Z$1:$Z$1355,A162,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A162,1),INDEX(LinMotor!$X$1:$X$1355,A162,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A162,1),INDEX(LinMotor!$Z$1:$Z$1355,A162,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A162,1),INDEX(LinMotor!$X$1:$X$1355,A162,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A162,1),INDEX(LinMotor!$Z$1:$Z$1355,A162,1)))/1000,\"0.0k\")),\"\")","v":59.0574352},{"$f":"IF(A162<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A162,1),INDEX(LinMotor!$Y$1:$Y$1355,A162,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A162,1),INDEX(LinMotor!$AB$1:$AB$445,A162,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A162,1),INDEX(LinMotor!$Y$1:$Y$1355,A162,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A162,1),INDEX(LinMotor!$AB$1:$AB$445,A162,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A162,1),INDEX(LinMotor!$Y$1:$Y$1355,A162,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A162,1),INDEX(LinMotor!$AB$1:$AB$445,A162,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A162,1),INDEX(LinMotor!$AD$1:$AD$1355,A162,1))","v":4.6552447403057966E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A162,1),INDEX(LinMotor!$AE$1:$AE$1355,A162,1))","v":0.10279990946502059},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A162,1),INDEX(LinMotor!$AF$1:$AF$1355,A162,1))","v":1.1172587376733911},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A162,1),INDEX(LinMotor!$AG$1:$AG$1355,A162,1))","v":4.9343956543209879},{"$f":"IF(A162<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A162,1),INDEX(LinMotor!$AI$1:$AI$1355,A162,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A162,1),INDEX(LinMotor!$AI$1:$AI$1355,A162,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A162,1),INDEX(LinMotor!$AI$1:$AI$1355,A162,1))/1000,\"0.0k\")),\"\")","v":31.299252364547087},{"$f":"IF(A162<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A162,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A162,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A162,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A162,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A162,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A162,1))/1000,\"0.0k\")),\"\")","v":7.5330910563710658},{"$f":"IF(A162<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A162,1),INDEX(LinMotor!$AK$1:$AK$1355,A162,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A162,1),INDEX(LinMotor!$AK$1:$AK$1355,A162,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A162,1),INDEX(LinMotor!$AK$1:$AK$1355,A162,1))/1000,\"0.0k\")),\"\")","v":461.47157804584231},{"$f":"IF(T162=1,\"L<Lmin\",IF(T162=2,\"Udc>Umot\",IF(T162=3,\"L<Lmin & Udc>Umot\",IF(T162=4,\"L>Lmax\",IF(T162=5,\"L>Lmax & Udc>Umot\",\"\")))))","v":""}]
[1202,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A163,1),INDEX(LinMotor!$B$1:$B$1341,A163,1))","v":"KBMS-88S02-A (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A163,1),INDEX(LinMotor!$R$1:$R$1355,A163,1))","v":0.45546558704453444},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A163,1),INDEX(LinMotor!$S$1:$S$1355,A163,1))","v":4.424673796574459E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A163,1),INDEX(LinMotor!$T$1:$T$1355,A163,1))","v":0.10785305105697163},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A163,1),INDEX(LinMotor!$U$1:$U$1355,A163,1))","v":0.82677892515270301},{"$f":"IF(A163<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A163,1),INDEX(LinMotor!$V$1:$V$1355,A163,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A163,1),INDEX(LinMotor!$V$1:$V$1355,A163,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A163,1),INDEX(LinMotor!$V$1:$V$1355,A163,1))/1000,\"0.0k\")),\"\")","v":-85.096057283950614},{"$f":"IF(A163<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A163,1),INDEX(LinMotor!$W$1:$W$1355,A163,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A163,1),INDEX(LinMotor!$X$1:$X$1355,A163,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A163,1),INDEX(LinMotor!$W$1:$W$1355,A163,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A163,1),INDEX(LinMotor!$X$1:$X$1355,A163,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A163,1),INDEX(LinMotor!$W$1:$W$1355,A163,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A163,1),INDEX(LinMotor!$X$1:$X$1355,A163,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A163<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A163,1),INDEX(LinMotor!$X$1:$X$1355,A163,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A163,1),INDEX(LinMotor!$Z$1:$Z$1355,A163,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A163,1),INDEX(LinMotor!$X$1:$X$1355,A163,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A163,1),INDEX(LinMotor!$Z$1:$Z$1355,A163,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A163,1),INDEX(LinMotor!$X$1:$X$1355,A163,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A163,1),INDEX(LinMotor!$Z$1:$Z$1355,A163,1)))/1000,\"0.0k\")),\"\")","v":79.787806400000008},{"$f":"IF(A163<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A163,1),INDEX(LinMotor!$Y$1:$Y$1355,A163,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A163,1),INDEX(LinMotor!$AB$1:$AB$445,A163,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A163,1),INDEX(LinMotor!$Y$1:$Y$1355,A163,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A163,1),INDEX(LinMotor!$AB$1:$AB$445,A163,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A163,1),INDEX(LinMotor!$Y$1:$Y$1355,A163,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A163,1),INDEX(LinMotor!$AB$1:$AB$445,A163,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A163,1),INDEX(LinMotor!$AD$1:$AD$1355,A163,1))","v":2.7042897955173954E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A163,1),INDEX(LinMotor!$AE$1:$AE$1355,A163,1))","v":6.9071475068141722E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A163,1),INDEX(LinMotor!$AF$1:$AF$1355,A163,1))","v":0.64902955092417491},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A163,1),INDEX(LinMotor!$AG$1:$AG$1355,A163,1))","v":3.3154308032708029},{"$f":"IF(A163<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A163,1),INDEX(LinMotor!$AI$1:$AI$1355,A163,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A163,1),INDEX(LinMotor!$AI$1:$AI$1355,A163,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A163,1),INDEX(LinMotor!$AI$1:$AI$1355,A163,1))/1000,\"0.0k\")),\"\")","v":38.699843242509104},{"$f":"IF(A163<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A163,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A163,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A163,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A163,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A163,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A163,1))/1000,\"0.0k\")),\"\")","v":11.079339664308581},{"$f":"IF(A163<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A163,1),INDEX(LinMotor!$AK$1:$AK$1355,A163,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A163,1),INDEX(LinMotor!$AK$1:$AK$1355,A163,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A163,1),INDEX(LinMotor!$AK$1:$AK$1355,A163,1))/1000,\"0.0k\")),\"\")","v":678.71214091727381},""]
[1204,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A164,1),INDEX(LinMotor!$B$1:$B$1341,A164,1))","v":"KBMS-88S03-A (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A164,1),INDEX(LinMotor!$R$1:$R$1355,A164,1))","v":0.35714285714285715},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A164,1),INDEX(LinMotor!$S$1:$S$1355,A164,1))","v":3.6172623750920674E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A164,1),INDEX(LinMotor!$T$1:$T$1355,A164,1))","v":8.5272518518518525E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A164,1),INDEX(LinMotor!$U$1:$U$1355,A164,1))","v":0.9645754126781535},{"$f":"IF(A164<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A164,1),INDEX(LinMotor!$V$1:$V$1355,A164,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A164,1),INDEX(LinMotor!$V$1:$V$1355,A164,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A164,1),INDEX(LinMotor!$V$1:$V$1355,A164,1))/1000,\"0.0k\")),\"\")","v":-102.32702222222223},{"$f":"IF(A164<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A164,1),INDEX(LinMotor!$W$1:$W$1355,A164,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A164,1),INDEX(LinMotor!$X$1:$X$1355,A164,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A164,1),INDEX(LinMotor!$W$1:$W$1355,A164,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A164,1),INDEX(LinMotor!$X$1:$X$1355,A164,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A164,1),INDEX(LinMotor!$W$1:$W$1355,A164,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A164,1),INDEX(LinMotor!$X$1:$X$1355,A164,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A164<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A164,1),INDEX(LinMotor!$X$1:$X$1355,A164,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A164,1),INDEX(LinMotor!$Z$1:$Z$1355,A164,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A164,1),INDEX(LinMotor!$X$1:$X$1355,A164,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A164,1),INDEX(LinMotor!$Z$1:$Z$1355,A164,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A164,1),INDEX(LinMotor!$X$1:$X$1355,A164,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A164,1),INDEX(LinMotor!$Z$1:$Z$1355,A164,1)))/1000,\"0.0k\")),\"\")","v":93.744888000000003},{"$f":"IF(A164<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A164,1),INDEX(LinMotor!$Y$1:$Y$1355,A164,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A164,1),INDEX(LinMotor!$AB$1:$AB$445,A164,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A164,1),INDEX(LinMotor!$Y$1:$Y$1355,A164,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A164,1),INDEX(LinMotor!$AB$1:$AB$445,A164,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A164,1),INDEX(LinMotor!$Y$1:$Y$1355,A164,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A164,1),INDEX(LinMotor!$AB$1:$AB$445,A164,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A164,1),INDEX(LinMotor!$AD$1:$AD$1355,A164,1))","v":2.6589826021676453E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A164,1),INDEX(LinMotor!$AE$1:$AE$1355,A164,1))","v":7.1720845036486305E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A164,1),INDEX(LinMotor!$AF$1:$AF$1355,A164,1))","v":0.63815582452023489},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A164,1),INDEX(LinMotor!$AG$1:$AG$1355,A164,1))","v":3.4426005617513429},{"$f":"IF(A164<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A164,1),INDEX(LinMotor!$AI$1:$AI$1355,A164,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A164,1),INDEX(LinMotor!$AI$1:$AI$1355,A164,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A164,1),INDEX(LinMotor!$AI$1:$AI$1355,A164,1))/1000,\"0.0k\")),\"\")","v":44.066210284047393},{"$f":"IF(A164<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A164,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A164,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A164,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A164,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A164,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A164,1))/1000,\"0.0k\")),\"\")","v":13.466912984504134},{"$f":"IF(A164<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A164,1),INDEX(LinMotor!$AK$1:$AK$1355,A164,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A164,1),INDEX(LinMotor!$AK$1:$AK$1355,A164,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A164,1),INDEX(LinMotor!$AK$1:$AK$1355,A164,1))/1000,\"0.0k\")),\"\")","v":824.97311393962366},""]
[1205,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A165,1),INDEX(LinMotor!$B$1:$B$1341,A165,1))","v":"KBMS-88S03-B (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A165,1),INDEX(LinMotor!$R$1:$R$1355,A165,1))","v":0.35714285714285715},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A165,1),INDEX(LinMotor!$S$1:$S$1355,A165,1))","v":3.5456535324261747E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A165,1),INDEX(LinMotor!$T$1:$T$1355,A165,1))","v":8.5272518518518525E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A165,1),INDEX(LinMotor!$U$1:$U$1355,A165,1))","v":0.49930962538633827},{"$f":"IF(A165<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A165,1),INDEX(LinMotor!$V$1:$V$1355,A165,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A165,1),INDEX(LinMotor!$V$1:$V$1355,A165,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A165,1),INDEX(LinMotor!$V$1:$V$1355,A165,1))/1000,\"0.0k\")),\"\")","v":-102.32702222222223},{"$f":"IF(A165<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A165,1),INDEX(LinMotor!$W$1:$W$1355,A165,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A165,1),INDEX(LinMotor!$X$1:$X$1355,A165,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A165,1),INDEX(LinMotor!$W$1:$W$1355,A165,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A165,1),INDEX(LinMotor!$X$1:$X$1355,A165,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A165,1),INDEX(LinMotor!$W$1:$W$1355,A165,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A165,1),INDEX(LinMotor!$X$1:$X$1355,A165,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A165<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A165,1),INDEX(LinMotor!$X$1:$X$1355,A165,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A165,1),INDEX(LinMotor!$Z$1:$Z$1355,A165,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A165,1),INDEX(LinMotor!$X$1:$X$1355,A165,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A165,1),INDEX(LinMotor!$Z$1:$Z$1355,A165,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A165,1),INDEX(LinMotor!$X$1:$X$1355,A165,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A165,1),INDEX(LinMotor!$Z$1:$Z$1355,A165,1)))/1000,\"0.0k\")),\"\")","v":93.744888000000003},{"$f":"IF(A165<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A165,1),INDEX(LinMotor!$Y$1:$Y$1355,A165,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A165,1),INDEX(LinMotor!$AB$1:$AB$445,A165,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A165,1),INDEX(LinMotor!$Y$1:$Y$1355,A165,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A165,1),INDEX(LinMotor!$AB$1:$AB$445,A165,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A165,1),INDEX(LinMotor!$Y$1:$Y$1355,A165,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A165,1),INDEX(LinMotor!$AB$1:$AB$445,A165,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A165,1),INDEX(LinMotor!$AD$1:$AD$1355,A165,1))","v":5.148148281088738E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A165,1),INDEX(LinMotor!$AE$1:$AE$1355,A165,1))","v":0.13886121134896365},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A165,1),INDEX(LinMotor!$AF$1:$AF$1355,A165,1))","v":1.2355555874612971},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A165,1),INDEX(LinMotor!$AG$1:$AG$1355,A165,1))","v":6.6653381447502547},{"$f":"IF(A165<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A165,1),INDEX(LinMotor!$AI$1:$AI$1355,A165,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A165,1),INDEX(LinMotor!$AI$1:$AI$1355,A165,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A165,1),INDEX(LinMotor!$AI$1:$AI$1355,A165,1))/1000,\"0.0k\")),\"\")","v":44.066210284047393},{"$f":"IF(A165<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A165,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A165,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A165,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A165,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A165,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A165,1))/1000,\"0.0k\")),\"\")","v":13.466912984504134},{"$f":"IF(A165<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A165,1),INDEX(LinMotor!$AK$1:$AK$1355,A165,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A165,1),INDEX(LinMotor!$AK$1:$AK$1355,A165,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A165,1),INDEX(LinMotor!$AK$1:$AK$1355,A165,1))/1000,\"0.0k\")),\"\")","v":824.97311393962366},""]
[1210,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A166,1),INDEX(LinMotor!$B$1:$B$1341,A166,1))","v":"KBMS-163H03-A (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A166,1),INDEX(LinMotor!$R$1:$R$1355,A166,1))","v":6.1475409836065573E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A166,1),INDEX(LinMotor!$S$1:$S$1355,A166,1))","v":5.7376916515100566E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A166,1),INDEX(LinMotor!$T$1:$T$1355,A166,1))","v":0.1237208104796909},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A166,1),INDEX(LinMotor!$U$1:$U$1355,A166,1))","v":0.7225686176357452},{"$f":"IF(A166<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A166,1),INDEX(LinMotor!$V$1:$V$1355,A166,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A166,1),INDEX(LinMotor!$V$1:$V$1355,A166,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A166,1),INDEX(LinMotor!$V$1:$V$1355,A166,1))/1000,\"0.0k\")),\"\")","v":-486.22278518518522},{"$f":"IF(A166<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A166,1),INDEX(LinMotor!$W$1:$W$1355,A166,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A166,1),INDEX(LinMotor!$X$1:$X$1355,A166,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A166,1),INDEX(LinMotor!$W$1:$W$1355,A166,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A166,1),INDEX(LinMotor!$X$1:$X$1355,A166,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A166,1),INDEX(LinMotor!$W$1:$W$1355,A166,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A166,1),INDEX(LinMotor!$X$1:$X$1355,A166,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A166<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A166,1),INDEX(LinMotor!$X$1:$X$1355,A166,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A166,1),INDEX(LinMotor!$Z$1:$Z$1355,A166,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A166,1),INDEX(LinMotor!$X$1:$X$1355,A166,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A166,1),INDEX(LinMotor!$Z$1:$Z$1355,A166,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A166,1),INDEX(LinMotor!$X$1:$X$1355,A166,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A166,1),INDEX(LinMotor!$Z$1:$Z$1355,A166,1)))/1000,\"0.0k\")),\"\")","v":404.70045600000003},{"$f":"IF(A166<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A166,1),INDEX(LinMotor!$Y$1:$Y$1355,A166,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A166,1),INDEX(LinMotor!$AB$1:$AB$445,A166,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A166,1),INDEX(LinMotor!$Y$1:$Y$1355,A166,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A166,1),INDEX(LinMotor!$AB$1:$AB$445,A166,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A166,1),INDEX(LinMotor!$Y$1:$Y$1355,A166,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A166,1),INDEX(LinMotor!$AB$1:$AB$445,A166,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A166,1),INDEX(LinMotor!$AD$1:$AD$1355,A166,1))","v":8.9703858824012397E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A166,1),INDEX(LinMotor!$AE$1:$AE$1355,A166,1))","v":0.28436665921436588},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A166,1),INDEX(LinMotor!$AF$1:$AF$1355,A166,1))","v":2.1528926117762976},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A166,1),INDEX(LinMotor!$AG$1:$AG$1355,A166,1))","v":13.649599642289562},{"$f":"IF(A166<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A166,1),INDEX(LinMotor!$AI$1:$AI$1355,A166,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A166,1),INDEX(LinMotor!$AI$1:$AI$1355,A166,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A166,1),INDEX(LinMotor!$AI$1:$AI$1355,A166,1))/1000,\"0.0k\")),\"\")","v":178.16115732580599},{"$f":"IF(A166<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A166,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A166,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A166,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A166,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A166,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A166,1))/1000,\"0.0k\")),\"\")","v":66.660642103566872},{"$f":"IF(A166<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A166,1),INDEX(LinMotor!$AK$1:$AK$1355,A166,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A166,1),INDEX(LinMotor!$AK$1:$AK$1355,A166,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A166,1),INDEX(LinMotor!$AK$1:$AK$1355,A166,1))/1000,\"0.0k\")),\"\")","v":"4.1k"},""]
[1211,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A167,1),INDEX(LinMotor!$B$1:$B$1341,A167,1))","v":"KBMS-163H03-A (480 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A167,1),INDEX(LinMotor!$R$1:$R$1355,A167,1))","v":6.1475409836065573E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A167,1),INDEX(LinMotor!$S$1:$S$1355,A167,1))","v":5.7374157967056492E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A167,1),INDEX(LinMotor!$T$1:$T$1355,A167,1))","v":0.1237208104796909},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A167,1),INDEX(LinMotor!$U$1:$U$1355,A167,1))","v":0.7225686176357452},{"$f":"IF(A167<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A167,1),INDEX(LinMotor!$V$1:$V$1355,A167,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A167,1),INDEX(LinMotor!$V$1:$V$1355,A167,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A167,1),INDEX(LinMotor!$V$1:$V$1355,A167,1))/1000,\"0.0k\")),\"\")","v":-486.22278518518522},{"$f":"IF(A167<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A167,1),INDEX(LinMotor!$W$1:$W$1355,A167,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A167,1),INDEX(LinMotor!$X$1:$X$1355,A167,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A167,1),INDEX(LinMotor!$W$1:$W$1355,A167,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A167,1),INDEX(LinMotor!$X$1:$X$1355,A167,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A167,1),INDEX(LinMotor!$W$1:$W$1355,A167,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A167,1),INDEX(LinMotor!$X$1:$X$1355,A167,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A167<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A167,1),INDEX(LinMotor!$X$1:$X$1355,A167,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A167,1),INDEX(LinMotor!$Z$1:$Z$1355,A167,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A167,1),INDEX(LinMotor!$X$1:$X$1355,A167,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A167,1),INDEX(LinMotor!$Z$1:$Z$1355,A167,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A167,1),INDEX(LinMotor!$X$1:$X$1355,A167,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A167,1),INDEX(LinMotor!$Z$1:$Z$1355,A167,1)))/1000,\"0.0k\")),\"\")","v":404.70045600000003},{"$f":"IF(A167<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A167,1),INDEX(LinMotor!$Y$1:$Y$1355,A167,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A167,1),INDEX(LinMotor!$AB$1:$AB$445,A167,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A167,1),INDEX(LinMotor!$Y$1:$Y$1355,A167,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A167,1),INDEX(LinMotor!$AB$1:$AB$445,A167,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A167,1),INDEX(LinMotor!$Y$1:$Y$1355,A167,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A167,1),INDEX(LinMotor!$AB$1:$AB$445,A167,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A167,1),INDEX(LinMotor!$AD$1:$AD$1355,A167,1))","v":8.9703858824012397E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A167,1),INDEX(LinMotor!$AE$1:$AE$1355,A167,1))","v":0.28436665921436588},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A167,1),INDEX(LinMotor!$AF$1:$AF$1355,A167,1))","v":2.1528926117762976},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A167,1),INDEX(LinMotor!$AG$1:$AG$1355,A167,1))","v":13.649599642289562},{"$f":"IF(A167<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A167,1),INDEX(LinMotor!$AI$1:$AI$1355,A167,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A167,1),INDEX(LinMotor!$AI$1:$AI$1355,A167,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A167,1),INDEX(LinMotor!$AI$1:$AI$1355,A167,1))/1000,\"0.0k\")),\"\")","v":178.16115732580599},{"$f":"IF(A167<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A167,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A167,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A167,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A167,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A167,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A167,1))/1000,\"0.0k\")),\"\")","v":66.660642103566872},{"$f":"IF(A167<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A167,1),INDEX(LinMotor!$AK$1:$AK$1355,A167,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A167,1),INDEX(LinMotor!$AK$1:$AK$1355,A167,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A167,1),INDEX(LinMotor!$AK$1:$AK$1355,A167,1))/1000,\"0.0k\")),\"\")","v":"4.1k"},""]
[1214,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A168,1),INDEX(LinMotor!$B$1:$B$1341,A168,1))","v":"KBMS-163S03-A (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A168,1),INDEX(LinMotor!$R$1:$R$1355,A168,1))","v":6.1475409836065573E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A168,1),INDEX(LinMotor!$S$1:$S$1355,A168,1))","v":5.7704307216404765E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A168,1),INDEX(LinMotor!$T$1:$T$1355,A168,1))","v":0.1237208104796909},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A168,1),INDEX(LinMotor!$U$1:$U$1355,A168,1))","v":1.1574904952137843},{"$f":"IF(A168<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A168,1),INDEX(LinMotor!$V$1:$V$1355,A168,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A168,1),INDEX(LinMotor!$V$1:$V$1355,A168,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A168,1),INDEX(LinMotor!$V$1:$V$1355,A168,1))/1000,\"0.0k\")),\"\")","v":-486.22278518518522},{"$f":"IF(A168<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A168,1),INDEX(LinMotor!$W$1:$W$1355,A168,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A168,1),INDEX(LinMotor!$X$1:$X$1355,A168,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A168,1),INDEX(LinMotor!$W$1:$W$1355,A168,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A168,1),INDEX(LinMotor!$X$1:$X$1355,A168,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A168,1),INDEX(LinMotor!$W$1:$W$1355,A168,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A168,1),INDEX(LinMotor!$X$1:$X$1355,A168,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A168<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A168,1),INDEX(LinMotor!$X$1:$X$1355,A168,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A168,1),INDEX(LinMotor!$Z$1:$Z$1355,A168,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A168,1),INDEX(LinMotor!$X$1:$X$1355,A168,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A168,1),INDEX(LinMotor!$Z$1:$Z$1355,A168,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A168,1),INDEX(LinMotor!$X$1:$X$1355,A168,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A168,1),INDEX(LinMotor!$Z$1:$Z$1355,A168,1)))/1000,\"0.0k\")),\"\")","v":404.70045600000003},{"$f":"IF(A168<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A168,1),INDEX(LinMotor!$Y$1:$Y$1355,A168,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A168,1),INDEX(LinMotor!$AB$1:$AB$445,A168,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A168,1),INDEX(LinMotor!$Y$1:$Y$1355,A168,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A168,1),INDEX(LinMotor!$AB$1:$AB$445,A168,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A168,1),INDEX(LinMotor!$Y$1:$Y$1355,A168,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A168,1),INDEX(LinMotor!$AB$1:$AB$445,A168,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A168,1),INDEX(LinMotor!$AD$1:$AD$1355,A168,1))","v":8.9703858824012397E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A168,1),INDEX(LinMotor!$AE$1:$AE$1355,A168,1))","v":0.28436665921436588},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A168,1),INDEX(LinMotor!$AF$1:$AF$1355,A168,1))","v":2.1528926117762976},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A168,1),INDEX(LinMotor!$AG$1:$AG$1355,A168,1))","v":13.649599642289562},{"$f":"IF(A168<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A168,1),INDEX(LinMotor!$AI$1:$AI$1355,A168,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A168,1),INDEX(LinMotor!$AI$1:$AI$1355,A168,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A168,1),INDEX(LinMotor!$AI$1:$AI$1355,A168,1))/1000,\"0.0k\")),\"\")","v":178.16115732580599},{"$f":"IF(A168<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A168,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A168,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A168,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A168,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A168,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A168,1))/1000,\"0.0k\")),\"\")","v":66.660642103566872},{"$f":"IF(A168<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A168,1),INDEX(LinMotor!$AK$1:$AK$1355,A168,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A168,1),INDEX(LinMotor!$AK$1:$AK$1355,A168,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A168,1),INDEX(LinMotor!$AK$1:$AK$1355,A168,1))/1000,\"0.0k\")),\"\")","v":"4.1k"},""]
[1215,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A169,1),INDEX(LinMotor!$B$1:$B$1341,A169,1))","v":"KBMS-260H01-A (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A169,1),INDEX(LinMotor!$R$1:$R$1355,A169,1))","v":2.0642201834862386E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A169,1),INDEX(LinMotor!$S$1:$S$1355,A169,1))","v":0.11648469711972388},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A169,1),INDEX(LinMotor!$T$1:$T$1355,A169,1))","v":0.21612538829764988},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A169,1),INDEX(LinMotor!$U$1:$U$1355,A169,1))","v":1.2257414592844313},{"$f":"IF(A169<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A169,1),INDEX(LinMotor!$V$1:$V$1355,A169,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A169,1),INDEX(LinMotor!$V$1:$V$1355,A169,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A169,1),INDEX(LinMotor!$V$1:$V$1355,A169,1))/1000,\"0.0k\")),\"\")","v":"-1.4k"},{"$f":"IF(A169<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A169,1),INDEX(LinMotor!$W$1:$W$1355,A169,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A169,1),INDEX(LinMotor!$X$1:$X$1355,A169,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A169,1),INDEX(LinMotor!$W$1:$W$1355,A169,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A169,1),INDEX(LinMotor!$X$1:$X$1355,A169,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A169,1),INDEX(LinMotor!$W$1:$W$1355,A169,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A169,1),INDEX(LinMotor!$X$1:$X$1355,A169,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A169<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A169,1),INDEX(LinMotor!$X$1:$X$1355,A169,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A169,1),INDEX(LinMotor!$Z$1:$Z$1355,A169,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A169,1),INDEX(LinMotor!$X$1:$X$1355,A169,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A169,1),INDEX(LinMotor!$Z$1:$Z$1355,A169,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A169,1),INDEX(LinMotor!$X$1:$X$1355,A169,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A169,1),INDEX(LinMotor!$Z$1:$Z$1355,A169,1)))/1000,\"0.0k\")),\"\")","v":"1.1k"},{"$f":"IF(A169<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A169,1),INDEX(LinMotor!$Y$1:$Y$1355,A169,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A169,1),INDEX(LinMotor!$AB$1:$AB$445,A169,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A169,1),INDEX(LinMotor!$Y$1:$Y$1355,A169,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A169,1),INDEX(LinMotor!$AB$1:$AB$445,A169,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A169,1),INDEX(LinMotor!$Y$1:$Y$1355,A169,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A169,1),INDEX(LinMotor!$AB$1:$AB$445,A169,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A169,1),INDEX(LinMotor!$AD$1:$AD$1355,A169,1))","v":0.15584325409062308},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A169,1),INDEX(LinMotor!$AE$1:$AE$1355,A169,1))","v":0.5009538344345611},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A169,1),INDEX(LinMotor!$AF$1:$AF$1355,A169,1))","v":3.7402380981749541},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A169,1),INDEX(LinMotor!$AG$1:$AG$1355,A169,1))","v":24.045784052858934},{"$f":"IF(A169<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A169,1),INDEX(LinMotor!$AI$1:$AI$1355,A169,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A169,1),INDEX(LinMotor!$AI$1:$AI$1355,A169,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A169,1),INDEX(LinMotor!$AI$1:$AI$1355,A169,1))/1000,\"0.0k\")),\"\")","v":507.17010034806481},{"$f":"IF(A169<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A169,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A169,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A169,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A169,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A169,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A169,1))/1000,\"0.0k\")),\"\")","v":193.76381003162436},{"$f":"IF(A169<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A169,1),INDEX(LinMotor!$AK$1:$AK$1355,A169,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A169,1),INDEX(LinMotor!$AK$1:$AK$1355,A169,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A169,1),INDEX(LinMotor!$AK$1:$AK$1355,A169,1))/1000,\"0.0k\")),\"\")","v":"11.9k"},""]
[1216,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A170,1),INDEX(LinMotor!$B$1:$B$1341,A170,1))","v":"KBMS-260H01-A (480 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A170,1),INDEX(LinMotor!$R$1:$R$1355,A170,1))","v":2.0642201834862386E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A170,1),INDEX(LinMotor!$S$1:$S$1355,A170,1))","v":0.11619180949076607},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A170,1),INDEX(LinMotor!$T$1:$T$1355,A170,1))","v":0.21612538829764988},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A170,1),INDEX(LinMotor!$U$1:$U$1355,A170,1))","v":1.2257414592844313},{"$f":"IF(A170<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A170,1),INDEX(LinMotor!$V$1:$V$1355,A170,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A170,1),INDEX(LinMotor!$V$1:$V$1355,A170,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A170,1),INDEX(LinMotor!$V$1:$V$1355,A170,1))/1000,\"0.0k\")),\"\")","v":"-1.4k"},{"$f":"IF(A170<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A170,1),INDEX(LinMotor!$W$1:$W$1355,A170,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A170,1),INDEX(LinMotor!$X$1:$X$1355,A170,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A170,1),INDEX(LinMotor!$W$1:$W$1355,A170,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A170,1),INDEX(LinMotor!$X$1:$X$1355,A170,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A170,1),INDEX(LinMotor!$W$1:$W$1355,A170,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A170,1),INDEX(LinMotor!$X$1:$X$1355,A170,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A170<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A170,1),INDEX(LinMotor!$X$1:$X$1355,A170,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A170,1),INDEX(LinMotor!$Z$1:$Z$1355,A170,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A170,1),INDEX(LinMotor!$X$1:$X$1355,A170,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A170,1),INDEX(LinMotor!$Z$1:$Z$1355,A170,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A170,1),INDEX(LinMotor!$X$1:$X$1355,A170,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A170,1),INDEX(LinMotor!$Z$1:$Z$1355,A170,1)))/1000,\"0.0k\")),\"\")","v":"1.1k"},{"$f":"IF(A170<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A170,1),INDEX(LinMotor!$Y$1:$Y$1355,A170,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A170,1),INDEX(LinMotor!$AB$1:$AB$445,A170,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A170,1),INDEX(LinMotor!$Y$1:$Y$1355,A170,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A170,1),INDEX(LinMotor!$AB$1:$AB$445,A170,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A170,1),INDEX(LinMotor!$Y$1:$Y$1355,A170,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A170,1),INDEX(LinMotor!$AB$1:$AB$445,A170,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A170,1),INDEX(LinMotor!$AD$1:$AD$1355,A170,1))","v":0.15584325409062308},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A170,1),INDEX(LinMotor!$AE$1:$AE$1355,A170,1))","v":0.5009538344345611},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A170,1),INDEX(LinMotor!$AF$1:$AF$1355,A170,1))","v":3.7402380981749541},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A170,1),INDEX(LinMotor!$AG$1:$AG$1355,A170,1))","v":24.045784052858934},{"$f":"IF(A170<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A170,1),INDEX(LinMotor!$AI$1:$AI$1355,A170,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A170,1),INDEX(LinMotor!$AI$1:$AI$1355,A170,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A170,1),INDEX(LinMotor!$AI$1:$AI$1355,A170,1))/1000,\"0.0k\")),\"\")","v":507.17010034806481},{"$f":"IF(A170<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A170,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A170,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A170,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A170,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A170,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A170,1))/1000,\"0.0k\")),\"\")","v":193.76381003162436},{"$f":"IF(A170<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A170,1),INDEX(LinMotor!$AK$1:$AK$1355,A170,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A170,1),INDEX(LinMotor!$AK$1:$AK$1355,A170,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A170,1),INDEX(LinMotor!$AK$1:$AK$1355,A170,1))/1000,\"0.0k\")),\"\")","v":"11.9k"},""]
[1217,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A171,1),INDEX(LinMotor!$B$1:$B$1341,A171,1))","v":"KBMS-260H02-A (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A171,1),INDEX(LinMotor!$R$1:$R$1355,A171,1))","v":1.4312977099236641E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A171,1),INDEX(LinMotor!$S$1:$S$1355,A171,1))","v":0.12056049201267173},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A171,1),INDEX(LinMotor!$T$1:$T$1355,A171,1))","v":0.20677588961510529},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A171,1),INDEX(LinMotor!$U$1:$U$1355,A171,1))","v":1.861020380109677},{"$f":"IF(A171<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A171,1),INDEX(LinMotor!$V$1:$V$1355,A171,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A171,1),INDEX(LinMotor!$V$1:$V$1355,A171,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A171,1),INDEX(LinMotor!$V$1:$V$1355,A171,1))/1000,\"0.0k\")),\"\")","v":"-2.0k"},{"$f":"IF(A171<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A171,1),INDEX(LinMotor!$W$1:$W$1355,A171,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A171,1),INDEX(LinMotor!$X$1:$X$1355,A171,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A171,1),INDEX(LinMotor!$W$1:$W$1355,A171,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A171,1),INDEX(LinMotor!$X$1:$X$1355,A171,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A171,1),INDEX(LinMotor!$W$1:$W$1355,A171,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A171,1),INDEX(LinMotor!$X$1:$X$1355,A171,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A171<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A171,1),INDEX(LinMotor!$X$1:$X$1355,A171,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A171,1),INDEX(LinMotor!$Z$1:$Z$1355,A171,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A171,1),INDEX(LinMotor!$X$1:$X$1355,A171,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A171,1),INDEX(LinMotor!$Z$1:$Z$1355,A171,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A171,1),INDEX(LinMotor!$X$1:$X$1355,A171,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A171,1),INDEX(LinMotor!$Z$1:$Z$1355,A171,1)))/1000,\"0.0k\")),\"\")","v":"1.6k"},{"$f":"IF(A171<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A171,1),INDEX(LinMotor!$Y$1:$Y$1355,A171,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A171,1),INDEX(LinMotor!$AB$1:$AB$445,A171,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A171,1),INDEX(LinMotor!$Y$1:$Y$1355,A171,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A171,1),INDEX(LinMotor!$AB$1:$AB$445,A171,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A171,1),INDEX(LinMotor!$Y$1:$Y$1355,A171,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A171,1),INDEX(LinMotor!$AB$1:$AB$445,A171,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A171,1),INDEX(LinMotor!$AD$1:$AD$1355,A171,1))","v":0.14929364122143376},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A171,1),INDEX(LinMotor!$AE$1:$AE$1355,A171,1))","v":0.48072433298659578},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A171,1),INDEX(LinMotor!$AF$1:$AF$1355,A171,1))","v":3.5830473893144106},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A171,1),INDEX(LinMotor!$AG$1:$AG$1355,A171,1))","v":23.074767983356598},{"$f":"IF(A171<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A171,1),INDEX(LinMotor!$AI$1:$AI$1355,A171,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A171,1),INDEX(LinMotor!$AI$1:$AI$1355,A171,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A171,1),INDEX(LinMotor!$AI$1:$AI$1355,A171,1))/1000,\"0.0k\")),\"\")","v":726.59752623167151},{"$f":"IF(A171<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A171,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A171,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A171,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A171,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A171,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A171,1))/1000,\"0.0k\")),\"\")","v":278.38221740914327},{"$f":"IF(A171<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A171,1),INDEX(LinMotor!$AK$1:$AK$1355,A171,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A171,1),INDEX(LinMotor!$AK$1:$AK$1355,A171,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A171,1),INDEX(LinMotor!$AK$1:$AK$1355,A171,1))/1000,\"0.0k\")),\"\")","v":"17.1k"},""]
[1218,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A172,1),INDEX(LinMotor!$B$1:$B$1341,A172,1))","v":"KBMS-260H02-A (480 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A172,1),INDEX(LinMotor!$R$1:$R$1355,A172,1))","v":1.4312977099236641E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A172,1),INDEX(LinMotor!$S$1:$S$1355,A172,1))","v":0.11991558544967441},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A172,1),INDEX(LinMotor!$T$1:$T$1355,A172,1))","v":0.20677588961510529},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A172,1),INDEX(LinMotor!$U$1:$U$1355,A172,1))","v":1.861020380109677},{"$f":"IF(A172<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A172,1),INDEX(LinMotor!$V$1:$V$1355,A172,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A172,1),INDEX(LinMotor!$V$1:$V$1355,A172,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A172,1),INDEX(LinMotor!$V$1:$V$1355,A172,1))/1000,\"0.0k\")),\"\")","v":"-2.0k"},{"$f":"IF(A172<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A172,1),INDEX(LinMotor!$W$1:$W$1355,A172,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A172,1),INDEX(LinMotor!$X$1:$X$1355,A172,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A172,1),INDEX(LinMotor!$W$1:$W$1355,A172,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A172,1),INDEX(LinMotor!$X$1:$X$1355,A172,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A172,1),INDEX(LinMotor!$W$1:$W$1355,A172,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A172,1),INDEX(LinMotor!$X$1:$X$1355,A172,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A172<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A172,1),INDEX(LinMotor!$X$1:$X$1355,A172,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A172,1),INDEX(LinMotor!$Z$1:$Z$1355,A172,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A172,1),INDEX(LinMotor!$X$1:$X$1355,A172,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A172,1),INDEX(LinMotor!$Z$1:$Z$1355,A172,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A172,1),INDEX(LinMotor!$X$1:$X$1355,A172,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A172,1),INDEX(LinMotor!$Z$1:$Z$1355,A172,1)))/1000,\"0.0k\")),\"\")","v":"1.6k"},{"$f":"IF(A172<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A172,1),INDEX(LinMotor!$Y$1:$Y$1355,A172,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A172,1),INDEX(LinMotor!$AB$1:$AB$445,A172,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A172,1),INDEX(LinMotor!$Y$1:$Y$1355,A172,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A172,1),INDEX(LinMotor!$AB$1:$AB$445,A172,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A172,1),INDEX(LinMotor!$Y$1:$Y$1355,A172,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A172,1),INDEX(LinMotor!$AB$1:$AB$445,A172,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A172,1),INDEX(LinMotor!$AD$1:$AD$1355,A172,1))","v":0.14929364122143376},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A172,1),INDEX(LinMotor!$AE$1:$AE$1355,A172,1))","v":0.48072433298659578},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A172,1),INDEX(LinMotor!$AF$1:$AF$1355,A172,1))","v":3.5830473893144106},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A172,1),INDEX(LinMotor!$AG$1:$AG$1355,A172,1))","v":23.074767983356598},{"$f":"IF(A172<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A172,1),INDEX(LinMotor!$AI$1:$AI$1355,A172,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A172,1),INDEX(LinMotor!$AI$1:$AI$1355,A172,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A172,1),INDEX(LinMotor!$AI$1:$AI$1355,A172,1))/1000,\"0.0k\")),\"\")","v":726.59752623167151},{"$f":"IF(A172<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A172,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A172,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A172,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A172,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A172,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A172,1))/1000,\"0.0k\")),\"\")","v":278.38221740914327},{"$f":"IF(A172<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A172,1),INDEX(LinMotor!$AK$1:$AK$1355,A172,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A172,1),INDEX(LinMotor!$AK$1:$AK$1355,A172,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A172,1),INDEX(LinMotor!$AK$1:$AK$1355,A172,1))/1000,\"0.0k\")),\"\")","v":"17.1k"},""]
[1219,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A173,1),INDEX(LinMotor!$B$1:$B$1341,A173,1))","v":"KBMS-260H03-A (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A173,1),INDEX(LinMotor!$R$1:$R$1355,A173,1))","v":1.1029411764705883E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A173,1),INDEX(LinMotor!$S$1:$S$1355,A173,1))","v":0.11894211192678691},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A173,1),INDEX(LinMotor!$T$1:$T$1355,A173,1))","v":0.20349296377238929},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A173,1),INDEX(LinMotor!$U$1:$U$1355,A173,1))","v":2.5118360625240439},{"$f":"IF(A173<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A173,1),INDEX(LinMotor!$V$1:$V$1355,A173,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A173,1),INDEX(LinMotor!$V$1:$V$1355,A173,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A173,1),INDEX(LinMotor!$V$1:$V$1355,A173,1))/1000,\"0.0k\")),\"\")","v":"-2.6k"},{"$f":"IF(A173<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A173,1),INDEX(LinMotor!$W$1:$W$1355,A173,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A173,1),INDEX(LinMotor!$X$1:$X$1355,A173,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A173,1),INDEX(LinMotor!$W$1:$W$1355,A173,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A173,1),INDEX(LinMotor!$X$1:$X$1355,A173,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A173,1),INDEX(LinMotor!$W$1:$W$1355,A173,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A173,1),INDEX(LinMotor!$X$1:$X$1355,A173,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A173<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A173,1),INDEX(LinMotor!$X$1:$X$1355,A173,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A173,1),INDEX(LinMotor!$Z$1:$Z$1355,A173,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A173,1),INDEX(LinMotor!$X$1:$X$1355,A173,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A173,1),INDEX(LinMotor!$Z$1:$Z$1355,A173,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A173,1),INDEX(LinMotor!$X$1:$X$1355,A173,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A173,1),INDEX(LinMotor!$Z$1:$Z$1355,A173,1)))/1000,\"0.0k\")),\"\")","v":"2.1k"},{"$f":"IF(A173<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A173,1),INDEX(LinMotor!$Y$1:$Y$1355,A173,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A173,1),INDEX(LinMotor!$AB$1:$AB$445,A173,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A173,1),INDEX(LinMotor!$Y$1:$Y$1355,A173,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A173,1),INDEX(LinMotor!$AB$1:$AB$445,A173,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A173,1),INDEX(LinMotor!$Y$1:$Y$1355,A173,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A173,1),INDEX(LinMotor!$AB$1:$AB$445,A173,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A173,1),INDEX(LinMotor!$AD$1:$AD$1355,A173,1))","v":0.14436614692751623},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A173,1),INDEX(LinMotor!$AE$1:$AE$1355,A173,1))","v":0.46524740871581988},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A173,1),INDEX(LinMotor!$AF$1:$AF$1355,A173,1))","v":3.4647875262603893},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A173,1),INDEX(LinMotor!$AG$1:$AG$1355,A173,1))","v":22.331875618359355},{"$f":"IF(A173<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A173,1),INDEX(LinMotor!$AI$1:$AI$1355,A173,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A173,1),INDEX(LinMotor!$AI$1:$AI$1355,A173,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A173,1),INDEX(LinMotor!$AI$1:$AI$1355,A173,1))/1000,\"0.0k\")),\"\")","v":939.70816053716703},{"$f":"IF(A173<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A173,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A173,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A173,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A173,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A173,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A173,1))/1000,\"0.0k\")),\"\")","v":360.54282872175503},{"$f":"IF(A173<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A173,1),INDEX(LinMotor!$AK$1:$AK$1355,A173,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A173,1),INDEX(LinMotor!$AK$1:$AK$1355,A173,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A173,1),INDEX(LinMotor!$AK$1:$AK$1355,A173,1))/1000,\"0.0k\")),\"\")","v":"22.1k"},""]
[1220,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A174,1),INDEX(LinMotor!$B$1:$B$1341,A174,1))","v":"KBMS-260H03-A (480 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A174,1),INDEX(LinMotor!$R$1:$R$1355,A174,1))","v":1.1029411764705883E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A174,1),INDEX(LinMotor!$S$1:$S$1355,A174,1))","v":0.1198472002070924},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A174,1),INDEX(LinMotor!$T$1:$T$1355,A174,1))","v":0.20349296377238929},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A174,1),INDEX(LinMotor!$U$1:$U$1355,A174,1))","v":2.5118360625240439},{"$f":"IF(A174<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A174,1),INDEX(LinMotor!$V$1:$V$1355,A174,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A174,1),INDEX(LinMotor!$V$1:$V$1355,A174,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A174,1),INDEX(LinMotor!$V$1:$V$1355,A174,1))/1000,\"0.0k\")),\"\")","v":"-2.6k"},{"$f":"IF(A174<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A174,1),INDEX(LinMotor!$W$1:$W$1355,A174,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A174,1),INDEX(LinMotor!$X$1:$X$1355,A174,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A174,1),INDEX(LinMotor!$W$1:$W$1355,A174,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A174,1),INDEX(LinMotor!$X$1:$X$1355,A174,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A174,1),INDEX(LinMotor!$W$1:$W$1355,A174,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A174,1),INDEX(LinMotor!$X$1:$X$1355,A174,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A174<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A174,1),INDEX(LinMotor!$X$1:$X$1355,A174,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A174,1),INDEX(LinMotor!$Z$1:$Z$1355,A174,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A174,1),INDEX(LinMotor!$X$1:$X$1355,A174,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A174,1),INDEX(LinMotor!$Z$1:$Z$1355,A174,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A174,1),INDEX(LinMotor!$X$1:$X$1355,A174,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A174,1),INDEX(LinMotor!$Z$1:$Z$1355,A174,1)))/1000,\"0.0k\")),\"\")","v":"2.1k"},{"$f":"IF(A174<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A174,1),INDEX(LinMotor!$Y$1:$Y$1355,A174,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A174,1),INDEX(LinMotor!$AB$1:$AB$445,A174,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A174,1),INDEX(LinMotor!$Y$1:$Y$1355,A174,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A174,1),INDEX(LinMotor!$AB$1:$AB$445,A174,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A174,1),INDEX(LinMotor!$Y$1:$Y$1355,A174,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A174,1),INDEX(LinMotor!$AB$1:$AB$445,A174,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A174,1),INDEX(LinMotor!$AD$1:$AD$1355,A174,1))","v":0.14436614692751623},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A174,1),INDEX(LinMotor!$AE$1:$AE$1355,A174,1))","v":0.46524740871581988},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A174,1),INDEX(LinMotor!$AF$1:$AF$1355,A174,1))","v":3.4647875262603893},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A174,1),INDEX(LinMotor!$AG$1:$AG$1355,A174,1))","v":22.331875618359355},{"$f":"IF(A174<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A174,1),INDEX(LinMotor!$AI$1:$AI$1355,A174,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A174,1),INDEX(LinMotor!$AI$1:$AI$1355,A174,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A174,1),INDEX(LinMotor!$AI$1:$AI$1355,A174,1))/1000,\"0.0k\")),\"\")","v":939.70816053716703},{"$f":"IF(A174<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A174,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A174,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A174,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A174,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A174,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A174,1))/1000,\"0.0k\")),\"\")","v":360.54282872175503},{"$f":"IF(A174<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A174,1),INDEX(LinMotor!$AK$1:$AK$1355,A174,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A174,1),INDEX(LinMotor!$AK$1:$AK$1355,A174,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A174,1),INDEX(LinMotor!$AK$1:$AK$1355,A174,1))/1000,\"0.0k\")),\"\")","v":"22.1k"},""]
[1221,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A175,1),INDEX(LinMotor!$B$1:$B$1341,A175,1))","v":"KBMS-260S01-A (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A175,1),INDEX(LinMotor!$R$1:$R$1355,A175,1))","v":2.0642201834862386E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A175,1),INDEX(LinMotor!$S$1:$S$1355,A175,1))","v":0.11814409859723583},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A175,1),INDEX(LinMotor!$T$1:$T$1355,A175,1))","v":0.21612538829764988},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A175,1),INDEX(LinMotor!$U$1:$U$1355,A175,1))","v":1.9003575294554667},{"$f":"IF(A175<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A175,1),INDEX(LinMotor!$V$1:$V$1355,A175,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A175,1),INDEX(LinMotor!$V$1:$V$1355,A175,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A175,1),INDEX(LinMotor!$V$1:$V$1355,A175,1))/1000,\"0.0k\")),\"\")","v":"-1.4k"},{"$f":"IF(A175<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A175,1),INDEX(LinMotor!$W$1:$W$1355,A175,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A175,1),INDEX(LinMotor!$X$1:$X$1355,A175,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A175,1),INDEX(LinMotor!$W$1:$W$1355,A175,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A175,1),INDEX(LinMotor!$X$1:$X$1355,A175,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A175,1),INDEX(LinMotor!$W$1:$W$1355,A175,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A175,1),INDEX(LinMotor!$X$1:$X$1355,A175,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A175<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A175,1),INDEX(LinMotor!$X$1:$X$1355,A175,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A175,1),INDEX(LinMotor!$Z$1:$Z$1355,A175,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A175,1),INDEX(LinMotor!$X$1:$X$1355,A175,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A175,1),INDEX(LinMotor!$Z$1:$Z$1355,A175,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A175,1),INDEX(LinMotor!$X$1:$X$1355,A175,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A175,1),INDEX(LinMotor!$Z$1:$Z$1355,A175,1)))/1000,\"0.0k\")),\"\")","v":"1.1k"},{"$f":"IF(A175<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A175,1),INDEX(LinMotor!$Y$1:$Y$1355,A175,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A175,1),INDEX(LinMotor!$AB$1:$AB$445,A175,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A175,1),INDEX(LinMotor!$Y$1:$Y$1355,A175,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A175,1),INDEX(LinMotor!$AB$1:$AB$445,A175,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A175,1),INDEX(LinMotor!$Y$1:$Y$1355,A175,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A175,1),INDEX(LinMotor!$AB$1:$AB$445,A175,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A175,1),INDEX(LinMotor!$AD$1:$AD$1355,A175,1))","v":0.15584325409062308},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A175,1),INDEX(LinMotor!$AE$1:$AE$1355,A175,1))","v":0.5009538344345611},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A175,1),INDEX(LinMotor!$AF$1:$AF$1355,A175,1))","v":3.7402380981749541},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A175,1),INDEX(LinMotor!$AG$1:$AG$1355,A175,1))","v":24.045784052858934},{"$f":"IF(A175<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A175,1),INDEX(LinMotor!$AI$1:$AI$1355,A175,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A175,1),INDEX(LinMotor!$AI$1:$AI$1355,A175,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A175,1),INDEX(LinMotor!$AI$1:$AI$1355,A175,1))/1000,\"0.0k\")),\"\")","v":507.17010034806481},{"$f":"IF(A175<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A175,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A175,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A175,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A175,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A175,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A175,1))/1000,\"0.0k\")),\"\")","v":193.76381003162436},{"$f":"IF(A175<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A175,1),INDEX(LinMotor!$AK$1:$AK$1355,A175,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A175,1),INDEX(LinMotor!$AK$1:$AK$1355,A175,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A175,1),INDEX(LinMotor!$AK$1:$AK$1355,A175,1))/1000,\"0.0k\")),\"\")","v":"11.9k"},""]
[1222,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A176,1),INDEX(LinMotor!$B$1:$B$1341,A176,1))","v":"KBMS-260S02-A (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A176,1),INDEX(LinMotor!$R$1:$R$1355,A176,1))","v":1.4312977099236641E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A176,1),INDEX(LinMotor!$S$1:$S$1355,A176,1))","v":0.12366375094283437},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A176,1),INDEX(LinMotor!$T$1:$T$1355,A176,1))","v":0.20677588961510529},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A176,1),INDEX(LinMotor!$U$1:$U$1355,A176,1))","v":2.8937262380344606},{"$f":"IF(A176<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A176,1),INDEX(LinMotor!$V$1:$V$1355,A176,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A176,1),INDEX(LinMotor!$V$1:$V$1355,A176,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A176,1),INDEX(LinMotor!$V$1:$V$1355,A176,1))/1000,\"0.0k\")),\"\")","v":"-2.0k"},{"$f":"IF(A176<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A176,1),INDEX(LinMotor!$W$1:$W$1355,A176,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A176,1),INDEX(LinMotor!$X$1:$X$1355,A176,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A176,1),INDEX(LinMotor!$W$1:$W$1355,A176,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A176,1),INDEX(LinMotor!$X$1:$X$1355,A176,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A176,1),INDEX(LinMotor!$W$1:$W$1355,A176,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A176,1),INDEX(LinMotor!$X$1:$X$1355,A176,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A176<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A176,1),INDEX(LinMotor!$X$1:$X$1355,A176,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A176,1),INDEX(LinMotor!$Z$1:$Z$1355,A176,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A176,1),INDEX(LinMotor!$X$1:$X$1355,A176,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A176,1),INDEX(LinMotor!$Z$1:$Z$1355,A176,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A176,1),INDEX(LinMotor!$X$1:$X$1355,A176,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A176,1),INDEX(LinMotor!$Z$1:$Z$1355,A176,1)))/1000,\"0.0k\")),\"\")","v":"1.6k"},{"$f":"IF(A176<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A176,1),INDEX(LinMotor!$Y$1:$Y$1355,A176,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A176,1),INDEX(LinMotor!$AB$1:$AB$445,A176,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A176,1),INDEX(LinMotor!$Y$1:$Y$1355,A176,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A176,1),INDEX(LinMotor!$AB$1:$AB$445,A176,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A176,1),INDEX(LinMotor!$Y$1:$Y$1355,A176,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A176,1),INDEX(LinMotor!$AB$1:$AB$445,A176,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A176,1),INDEX(LinMotor!$AD$1:$AD$1355,A176,1))","v":0.14929364122143376},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A176,1),INDEX(LinMotor!$AE$1:$AE$1355,A176,1))","v":0.48072433298659578},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A176,1),INDEX(LinMotor!$AF$1:$AF$1355,A176,1))","v":3.5830473893144106},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A176,1),INDEX(LinMotor!$AG$1:$AG$1355,A176,1))","v":23.074767983356598},{"$f":"IF(A176<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A176,1),INDEX(LinMotor!$AI$1:$AI$1355,A176,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A176,1),INDEX(LinMotor!$AI$1:$AI$1355,A176,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A176,1),INDEX(LinMotor!$AI$1:$AI$1355,A176,1))/1000,\"0.0k\")),\"\")","v":726.59752623167151},{"$f":"IF(A176<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A176,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A176,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A176,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A176,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A176,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A176,1))/1000,\"0.0k\")),\"\")","v":278.38221740914327},{"$f":"IF(A176<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A176,1),INDEX(LinMotor!$AK$1:$AK$1355,A176,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A176,1),INDEX(LinMotor!$AK$1:$AK$1355,A176,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A176,1),INDEX(LinMotor!$AK$1:$AK$1355,A176,1))/1000,\"0.0k\")),\"\")","v":"17.1k"},""]
[1223,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A177,1),INDEX(LinMotor!$B$1:$B$1341,A177,1))","v":"KBMS-260S03-A (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A177,1),INDEX(LinMotor!$R$1:$R$1355,A177,1))","v":1.1029411764705883E-2},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A177,1),INDEX(LinMotor!$S$1:$S$1355,A177,1))","v":0.12272990911982505},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A177,1),INDEX(LinMotor!$T$1:$T$1355,A177,1))","v":0.20349296377238929},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A177,1),INDEX(LinMotor!$U$1:$U$1355,A177,1))","v":3.858301650712614},{"$f":"IF(A177<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A177,1),INDEX(LinMotor!$V$1:$V$1355,A177,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A177,1),INDEX(LinMotor!$V$1:$V$1355,A177,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A177,1),INDEX(LinMotor!$V$1:$V$1355,A177,1))/1000,\"0.0k\")),\"\")","v":"-2.6k"},{"$f":"IF(A177<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A177,1),INDEX(LinMotor!$W$1:$W$1355,A177,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A177,1),INDEX(LinMotor!$X$1:$X$1355,A177,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A177,1),INDEX(LinMotor!$W$1:$W$1355,A177,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A177,1),INDEX(LinMotor!$X$1:$X$1355,A177,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A177,1),INDEX(LinMotor!$W$1:$W$1355,A177,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A177,1),INDEX(LinMotor!$X$1:$X$1355,A177,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A177<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A177,1),INDEX(LinMotor!$X$1:$X$1355,A177,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A177,1),INDEX(LinMotor!$Z$1:$Z$1355,A177,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A177,1),INDEX(LinMotor!$X$1:$X$1355,A177,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A177,1),INDEX(LinMotor!$Z$1:$Z$1355,A177,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A177,1),INDEX(LinMotor!$X$1:$X$1355,A177,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A177,1),INDEX(LinMotor!$Z$1:$Z$1355,A177,1)))/1000,\"0.0k\")),\"\")","v":"2.1k"},{"$f":"IF(A177<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A177,1),INDEX(LinMotor!$Y$1:$Y$1355,A177,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A177,1),INDEX(LinMotor!$AB$1:$AB$445,A177,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A177,1),INDEX(LinMotor!$Y$1:$Y$1355,A177,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A177,1),INDEX(LinMotor!$AB$1:$AB$445,A177,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A177,1),INDEX(LinMotor!$Y$1:$Y$1355,A177,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A177,1),INDEX(LinMotor!$AB$1:$AB$445,A177,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A177,1),INDEX(LinMotor!$AD$1:$AD$1355,A177,1))","v":0.14436614692751623},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A177,1),INDEX(LinMotor!$AE$1:$AE$1355,A177,1))","v":0.46524740871581988},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A177,1),INDEX(LinMotor!$AF$1:$AF$1355,A177,1))","v":3.4647875262603893},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A177,1),INDEX(LinMotor!$AG$1:$AG$1355,A177,1))","v":22.331875618359355},{"$f":"IF(A177<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A177,1),INDEX(LinMotor!$AI$1:$AI$1355,A177,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A177,1),INDEX(LinMotor!$AI$1:$AI$1355,A177,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A177,1),INDEX(LinMotor!$AI$1:$AI$1355,A177,1))/1000,\"0.0k\")),\"\")","v":939.70816053716703},{"$f":"IF(A177<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A177,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A177,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A177,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A177,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A177,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A177,1))/1000,\"0.0k\")),\"\")","v":360.54282872175503},{"$f":"IF(A177<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A177,1),INDEX(LinMotor!$AK$1:$AK$1355,A177,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A177,1),INDEX(LinMotor!$AK$1:$AK$1355,A177,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A177,1),INDEX(LinMotor!$AK$1:$AK$1355,A177,1))/1000,\"0.0k\")),\"\")","v":"22.1k"},""]
[935,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A178,1),INDEX(LinMotor!$B$1:$B$1341,A178,1))","v":"KBMS-17H04-C (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A178,1),INDEX(LinMotor!$R$1:$R$1355,A178,1))","v":468.75},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A178,1),INDEX(LinMotor!$S$1:$S$1355,A178,1))","v":1.6299898271998137},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A178,1),INDEX(LinMotor!$T$1:$T$1355,A178,1))","v":1.2295367210126582},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A178,1),INDEX(LinMotor!$U$1:$U$1355,A178,1))","v":3.8285017766954817E-2},{"$f":"IF(A178<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A178,1),INDEX(LinMotor!$V$1:$V$1355,A178,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A178,1),INDEX(LinMotor!$V$1:$V$1355,A178,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A178,1),INDEX(LinMotor!$V$1:$V$1355,A178,1))/1000,\"0.0k\")),\"\")","v":-22.56792628148148},{"$f":"IF(A178<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A178,1),INDEX(LinMotor!$W$1:$W$1355,A178,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A178,1),INDEX(LinMotor!$X$1:$X$1355,A178,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A178,1),INDEX(LinMotor!$W$1:$W$1355,A178,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A178,1),INDEX(LinMotor!$X$1:$X$1355,A178,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A178,1),INDEX(LinMotor!$W$1:$W$1355,A178,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A178,1),INDEX(LinMotor!$X$1:$X$1355,A178,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A178<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A178,1),INDEX(LinMotor!$X$1:$X$1355,A178,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A178,1),INDEX(LinMotor!$Z$1:$Z$1355,A178,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A178,1),INDEX(LinMotor!$X$1:$X$1355,A178,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A178,1),INDEX(LinMotor!$Z$1:$Z$1355,A178,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A178,1),INDEX(LinMotor!$X$1:$X$1355,A178,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A178,1),INDEX(LinMotor!$Z$1:$Z$1355,A178,1)))/1000,\"0.0k\")),\"\")","v":29.140020287999999},{"$f":"IF(A178<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A178,1),INDEX(LinMotor!$Y$1:$Y$1355,A178,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A178,1),INDEX(LinMotor!$AB$1:$AB$445,A178,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A178,1),INDEX(LinMotor!$Y$1:$Y$1355,A178,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A178,1),INDEX(LinMotor!$AB$1:$AB$445,A178,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A178,1),INDEX(LinMotor!$Y$1:$Y$1355,A178,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A178,1),INDEX(LinMotor!$AB$1:$AB$445,A178,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A178,1),INDEX(LinMotor!$AD$1:$AD$1355,A178,1))","v":0.41989057695977666},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A178,1),INDEX(LinMotor!$AE$1:$AE$1355,A178,1))","v":0.61703594872131151},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A178,1),INDEX(LinMotor!$AF$1:$AF$1355,A178,1))","v":10.077373847034639},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A178,1),INDEX(LinMotor!$AG$1:$AG$1355,A178,1))","v":29.617725538622953},{"$f":"IF(A178<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A178,1),INDEX(LinMotor!$AI$1:$AI$1355,A178,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A178,1),INDEX(LinMotor!$AI$1:$AI$1355,A178,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A178,1),INDEX(LinMotor!$AI$1:$AI$1355,A178,1))/1000,\"0.0k\")),\"\")","v":23.03354480882064},{"$f":"IF(A178<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A178,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A178,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A178,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A178,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A178,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A178,1))/1000,\"0.0k\")),\"\")","v":2.4152574217871821},{"$f":"IF(A178<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A178,1),INDEX(LinMotor!$AK$1:$AK$1355,A178,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A178,1),INDEX(LinMotor!$AK$1:$AK$1355,A178,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A178,1),INDEX(LinMotor!$AK$1:$AK$1355,A178,1))/1000,\"0.0k\")),\"\")","v":147.95688057911107},""]
[937,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A179,1),INDEX(LinMotor!$B$1:$B$1341,A179,1))","v":"KBMS-17H04-D (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A179,1),INDEX(LinMotor!$R$1:$R$1355,A179,1))","v":468.75},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A179,1),INDEX(LinMotor!$S$1:$S$1355,A179,1))","v":1.635935833534969},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A179,1),INDEX(LinMotor!$T$1:$T$1355,A179,1))","v":1.2141675119999999},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A179,1),INDEX(LinMotor!$U$1:$U$1355,A179,1))","v":2.4221713157362448E-2},{"$f":"IF(A179<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A179,1),INDEX(LinMotor!$V$1:$V$1355,A179,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A179,1),INDEX(LinMotor!$V$1:$V$1355,A179,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A179,1),INDEX(LinMotor!$V$1:$V$1355,A179,1))/1000,\"0.0k\")),\"\")","v":-22.56792628148148},{"$f":"IF(A179<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A179,1),INDEX(LinMotor!$W$1:$W$1355,A179,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A179,1),INDEX(LinMotor!$X$1:$X$1355,A179,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A179,1),INDEX(LinMotor!$W$1:$W$1355,A179,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A179,1),INDEX(LinMotor!$X$1:$X$1355,A179,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A179,1),INDEX(LinMotor!$W$1:$W$1355,A179,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A179,1),INDEX(LinMotor!$X$1:$X$1355,A179,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A179<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A179,1),INDEX(LinMotor!$X$1:$X$1355,A179,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A179,1),INDEX(LinMotor!$Z$1:$Z$1355,A179,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A179,1),INDEX(LinMotor!$X$1:$X$1355,A179,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A179,1),INDEX(LinMotor!$Z$1:$Z$1355,A179,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A179,1),INDEX(LinMotor!$X$1:$X$1355,A179,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A179,1),INDEX(LinMotor!$Z$1:$Z$1355,A179,1)))/1000,\"0.0k\")),\"\")","v":29.140020287999999},{"$f":"IF(A179<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A179,1),INDEX(LinMotor!$Y$1:$Y$1355,A179,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A179,1),INDEX(LinMotor!$AB$1:$AB$445,A179,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A179,1),INDEX(LinMotor!$Y$1:$Y$1355,A179,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A179,1),INDEX(LinMotor!$AB$1:$AB$445,A179,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A179,1),INDEX(LinMotor!$Y$1:$Y$1355,A179,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A179,1),INDEX(LinMotor!$AB$1:$AB$445,A179,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A179,1),INDEX(LinMotor!$AD$1:$AD$1355,A179,1))","v":0.65064406882038406},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A179,1),INDEX(LinMotor!$AE$1:$AE$1355,A179,1))","v":0.95613191225041183},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A179,1),INDEX(LinMotor!$AF$1:$AF$1355,A179,1))","v":15.615457651689217},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A179,1),INDEX(LinMotor!$AG$1:$AG$1355,A179,1))","v":45.89433178801977},{"$f":"IF(A179<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A179,1),INDEX(LinMotor!$AI$1:$AI$1355,A179,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A179,1),INDEX(LinMotor!$AI$1:$AI$1355,A179,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A179,1),INDEX(LinMotor!$AI$1:$AI$1355,A179,1))/1000,\"0.0k\")),\"\")","v":23.03354480882064},{"$f":"IF(A179<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A179,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A179,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A179,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A179,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A179,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A179,1))/1000,\"0.0k\")),\"\")","v":2.4152574217871821},{"$f":"IF(A179<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A179,1),INDEX(LinMotor!$AK$1:$AK$1355,A179,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A179,1),INDEX(LinMotor!$AK$1:$AK$1355,A179,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A179,1),INDEX(LinMotor!$AK$1:$AK$1355,A179,1))/1000,\"0.0k\")),\"\")","v":147.95688057911107},""]
[961,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A180,1),INDEX(LinMotor!$B$1:$B$1341,A180,1))","v":"KBMS-25H02-C (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A180,1),INDEX(LinMotor!$R$1:$R$1355,A180,1))","v":165.92920353982299},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A180,1),INDEX(LinMotor!$S$1:$S$1355,A180,1))","v":1.1357261545140895},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A180,1),INDEX(LinMotor!$T$1:$T$1355,A180,1))","v":0.98417240113131321},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A180,1),INDEX(LinMotor!$U$1:$U$1355,A180,1))","v":4.3980640578071252E-2},{"$f":"IF(A180<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A180,1),INDEX(LinMotor!$V$1:$V$1355,A180,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A180,1),INDEX(LinMotor!$V$1:$V$1355,A180,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A180,1),INDEX(LinMotor!$V$1:$V$1355,A180,1))/1000,\"0.0k\")),\"\")","v":-22.678913967407407},{"$f":"IF(A180<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A180,1),INDEX(LinMotor!$W$1:$W$1355,A180,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A180,1),INDEX(LinMotor!$X$1:$X$1355,A180,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A180,1),INDEX(LinMotor!$W$1:$W$1355,A180,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A180,1),INDEX(LinMotor!$X$1:$X$1355,A180,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A180,1),INDEX(LinMotor!$W$1:$W$1355,A180,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A180,1),INDEX(LinMotor!$X$1:$X$1355,A180,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A180<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A180,1),INDEX(LinMotor!$X$1:$X$1355,A180,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A180,1),INDEX(LinMotor!$Z$1:$Z$1355,A180,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A180,1),INDEX(LinMotor!$X$1:$X$1355,A180,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A180,1),INDEX(LinMotor!$Z$1:$Z$1355,A180,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A180,1),INDEX(LinMotor!$X$1:$X$1355,A180,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A180,1),INDEX(LinMotor!$Z$1:$Z$1355,A180,1)))/1000,\"0.0k\")),\"\")","v":29.229920313600001},{"$f":"IF(A180<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A180,1),INDEX(LinMotor!$Y$1:$Y$1355,A180,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A180,1),INDEX(LinMotor!$AB$1:$AB$445,A180,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A180,1),INDEX(LinMotor!$Y$1:$Y$1355,A180,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A180,1),INDEX(LinMotor!$AB$1:$AB$445,A180,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A180,1),INDEX(LinMotor!$Y$1:$Y$1355,A180,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A180,1),INDEX(LinMotor!$AB$1:$AB$445,A180,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A180,1),INDEX(LinMotor!$AD$1:$AD$1355,A180,1))","v":0.30712519642412928},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A180,1),INDEX(LinMotor!$AE$1:$AE$1355,A180,1))","v":0.45236781437714285},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A180,1),INDEX(LinMotor!$AF$1:$AF$1355,A180,1))","v":7.3710047141791026},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A180,1),INDEX(LinMotor!$AG$1:$AG$1355,A180,1))","v":21.713655090102858},{"$f":"IF(A180<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A180,1),INDEX(LinMotor!$AI$1:$AI$1355,A180,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A180,1),INDEX(LinMotor!$AI$1:$AI$1355,A180,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A180,1),INDEX(LinMotor!$AI$1:$AI$1355,A180,1))/1000,\"0.0k\")),\"\")","v":23.051365115686874},{"$f":"IF(A180<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A180,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A180,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A180,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A180,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A180,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A180,1))/1000,\"0.0k\")),\"\")","v":2.4306362028790298},{"$f":"IF(A180<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A180,1),INDEX(LinMotor!$AK$1:$AK$1355,A180,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A180,1),INDEX(LinMotor!$AK$1:$AK$1355,A180,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A180,1),INDEX(LinMotor!$AK$1:$AK$1355,A180,1))/1000,\"0.0k\")),\"\")","v":148.89897331710799},""]
[962,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A181,1),INDEX(LinMotor!$B$1:$B$1341,A181,1))","v":"KBMS-25H02-C (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A181,1),INDEX(LinMotor!$R$1:$R$1355,A181,1))","v":165.92920353982299},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A181,1),INDEX(LinMotor!$S$1:$S$1355,A181,1))","v":1.135952146924025},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A181,1),INDEX(LinMotor!$T$1:$T$1355,A181,1))","v":0.98417240113131321},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A181,1),INDEX(LinMotor!$U$1:$U$1355,A181,1))","v":4.1993701845190599E-2},{"$f":"IF(A181<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A181,1),INDEX(LinMotor!$V$1:$V$1355,A181,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A181,1),INDEX(LinMotor!$V$1:$V$1355,A181,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A181,1),INDEX(LinMotor!$V$1:$V$1355,A181,1))/1000,\"0.0k\")),\"\")","v":-22.678913967407407},{"$f":"IF(A181<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A181,1),INDEX(LinMotor!$W$1:$W$1355,A181,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A181,1),INDEX(LinMotor!$X$1:$X$1355,A181,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A181,1),INDEX(LinMotor!$W$1:$W$1355,A181,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A181,1),INDEX(LinMotor!$X$1:$X$1355,A181,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A181,1),INDEX(LinMotor!$W$1:$W$1355,A181,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A181,1),INDEX(LinMotor!$X$1:$X$1355,A181,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A181<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A181,1),INDEX(LinMotor!$X$1:$X$1355,A181,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A181,1),INDEX(LinMotor!$Z$1:$Z$1355,A181,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A181,1),INDEX(LinMotor!$X$1:$X$1355,A181,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A181,1),INDEX(LinMotor!$Z$1:$Z$1355,A181,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A181,1),INDEX(LinMotor!$X$1:$X$1355,A181,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A181,1),INDEX(LinMotor!$Z$1:$Z$1355,A181,1)))/1000,\"0.0k\")),\"\")","v":29.229920313600001},{"$f":"IF(A181<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A181,1),INDEX(LinMotor!$Y$1:$Y$1355,A181,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A181,1),INDEX(LinMotor!$AB$1:$AB$445,A181,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A181,1),INDEX(LinMotor!$Y$1:$Y$1355,A181,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A181,1),INDEX(LinMotor!$AB$1:$AB$445,A181,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A181,1),INDEX(LinMotor!$Y$1:$Y$1355,A181,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A181,1),INDEX(LinMotor!$AB$1:$AB$445,A181,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A181,1),INDEX(LinMotor!$AD$1:$AD$1355,A181,1))","v":0.30712519642412928},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A181,1),INDEX(LinMotor!$AE$1:$AE$1355,A181,1))","v":0.45236781437714285},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A181,1),INDEX(LinMotor!$AF$1:$AF$1355,A181,1))","v":7.3710047141791026},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A181,1),INDEX(LinMotor!$AG$1:$AG$1355,A181,1))","v":21.713655090102858},{"$f":"IF(A181<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A181,1),INDEX(LinMotor!$AI$1:$AI$1355,A181,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A181,1),INDEX(LinMotor!$AI$1:$AI$1355,A181,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A181,1),INDEX(LinMotor!$AI$1:$AI$1355,A181,1))/1000,\"0.0k\")),\"\")","v":23.051365115686874},{"$f":"IF(A181<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A181,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A181,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A181,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A181,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A181,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A181,1))/1000,\"0.0k\")),\"\")","v":2.4306362028790298},{"$f":"IF(A181<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A181,1),INDEX(LinMotor!$AK$1:$AK$1355,A181,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A181,1),INDEX(LinMotor!$AK$1:$AK$1355,A181,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A181,1),INDEX(LinMotor!$AK$1:$AK$1355,A181,1))/1000,\"0.0k\")),\"\")","v":148.89897331710799},""]
[963,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A182,1),INDEX(LinMotor!$B$1:$B$1341,A182,1))","v":"KBMS-25H02-C (480 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A182,1),INDEX(LinMotor!$R$1:$R$1355,A182,1))","v":165.92920353982299},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A182,1),INDEX(LinMotor!$S$1:$S$1355,A182,1))","v":1.1362528186967695},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A182,1),INDEX(LinMotor!$T$1:$T$1355,A182,1))","v":0.98417240113131321},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A182,1),INDEX(LinMotor!$U$1:$U$1355,A182,1))","v":4.1993701845190599E-2},{"$f":"IF(A182<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A182,1),INDEX(LinMotor!$V$1:$V$1355,A182,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A182,1),INDEX(LinMotor!$V$1:$V$1355,A182,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A182,1),INDEX(LinMotor!$V$1:$V$1355,A182,1))/1000,\"0.0k\")),\"\")","v":-22.678913967407407},{"$f":"IF(A182<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A182,1),INDEX(LinMotor!$W$1:$W$1355,A182,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A182,1),INDEX(LinMotor!$X$1:$X$1355,A182,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A182,1),INDEX(LinMotor!$W$1:$W$1355,A182,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A182,1),INDEX(LinMotor!$X$1:$X$1355,A182,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A182,1),INDEX(LinMotor!$W$1:$W$1355,A182,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A182,1),INDEX(LinMotor!$X$1:$X$1355,A182,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A182<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A182,1),INDEX(LinMotor!$X$1:$X$1355,A182,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A182,1),INDEX(LinMotor!$Z$1:$Z$1355,A182,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A182,1),INDEX(LinMotor!$X$1:$X$1355,A182,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A182,1),INDEX(LinMotor!$Z$1:$Z$1355,A182,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A182,1),INDEX(LinMotor!$X$1:$X$1355,A182,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A182,1),INDEX(LinMotor!$Z$1:$Z$1355,A182,1)))/1000,\"0.0k\")),\"\")","v":29.229920313600001},{"$f":"IF(A182<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A182,1),INDEX(LinMotor!$Y$1:$Y$1355,A182,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A182,1),INDEX(LinMotor!$AB$1:$AB$445,A182,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A182,1),INDEX(LinMotor!$Y$1:$Y$1355,A182,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A182,1),INDEX(LinMotor!$AB$1:$AB$445,A182,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A182,1),INDEX(LinMotor!$Y$1:$Y$1355,A182,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A182,1),INDEX(LinMotor!$AB$1:$AB$445,A182,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A182,1),INDEX(LinMotor!$AD$1:$AD$1355,A182,1))","v":0.30712519642412928},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A182,1),INDEX(LinMotor!$AE$1:$AE$1355,A182,1))","v":0.45236781437714285},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A182,1),INDEX(LinMotor!$AF$1:$AF$1355,A182,1))","v":7.3710047141791026},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A182,1),INDEX(LinMotor!$AG$1:$AG$1355,A182,1))","v":21.713655090102858},{"$f":"IF(A182<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A182,1),INDEX(LinMotor!$AI$1:$AI$1355,A182,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A182,1),INDEX(LinMotor!$AI$1:$AI$1355,A182,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A182,1),INDEX(LinMotor!$AI$1:$AI$1355,A182,1))/1000,\"0.0k\")),\"\")","v":23.051365115686874},{"$f":"IF(A182<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A182,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A182,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A182,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A182,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A182,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A182,1))/1000,\"0.0k\")),\"\")","v":2.4306362028790298},{"$f":"IF(A182<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A182,1),INDEX(LinMotor!$AK$1:$AK$1355,A182,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A182,1),INDEX(LinMotor!$AK$1:$AK$1355,A182,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A182,1),INDEX(LinMotor!$AK$1:$AK$1355,A182,1))/1000,\"0.0k\")),\"\")","v":148.89897331710799},""]
[965,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A183,1),INDEX(LinMotor!$B$1:$B$1341,A183,1))","v":"KBMS-25H02-D (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A183,1),INDEX(LinMotor!$R$1:$R$1355,A183,1))","v":165.92920353982299},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A183,1),INDEX(LinMotor!$S$1:$S$1355,A183,1))","v":1.1528956015256069},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A183,1),INDEX(LinMotor!$T$1:$T$1355,A183,1))","v":0.98086980918120803},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A183,1),INDEX(LinMotor!$U$1:$U$1355,A183,1))","v":3.5397262850574443E-2},{"$f":"IF(A183<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A183,1),INDEX(LinMotor!$V$1:$V$1355,A183,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A183,1),INDEX(LinMotor!$V$1:$V$1355,A183,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A183,1),INDEX(LinMotor!$V$1:$V$1355,A183,1))/1000,\"0.0k\")),\"\")","v":-22.678913967407407},{"$f":"IF(A183<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A183,1),INDEX(LinMotor!$W$1:$W$1355,A183,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A183,1),INDEX(LinMotor!$X$1:$X$1355,A183,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A183,1),INDEX(LinMotor!$W$1:$W$1355,A183,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A183,1),INDEX(LinMotor!$X$1:$X$1355,A183,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A183,1),INDEX(LinMotor!$W$1:$W$1355,A183,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A183,1),INDEX(LinMotor!$X$1:$X$1355,A183,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A183<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A183,1),INDEX(LinMotor!$X$1:$X$1355,A183,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A183,1),INDEX(LinMotor!$Z$1:$Z$1355,A183,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A183,1),INDEX(LinMotor!$X$1:$X$1355,A183,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A183,1),INDEX(LinMotor!$Z$1:$Z$1355,A183,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A183,1),INDEX(LinMotor!$X$1:$X$1355,A183,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A183,1),INDEX(LinMotor!$Z$1:$Z$1355,A183,1)))/1000,\"0.0k\")),\"\")","v":29.229920313600001},{"$f":"IF(A183<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A183,1),INDEX(LinMotor!$Y$1:$Y$1355,A183,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A183,1),INDEX(LinMotor!$AB$1:$AB$445,A183,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A183,1),INDEX(LinMotor!$Y$1:$Y$1355,A183,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A183,1),INDEX(LinMotor!$AB$1:$AB$445,A183,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A183,1),INDEX(LinMotor!$Y$1:$Y$1355,A183,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A183,1),INDEX(LinMotor!$AB$1:$AB$445,A183,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A183,1),INDEX(LinMotor!$AD$1:$AD$1355,A183,1))","v":0.38370094145438255},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A183,1),INDEX(LinMotor!$AE$1:$AE$1355,A183,1))","v":0.56515700529002333},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A183,1),INDEX(LinMotor!$AF$1:$AF$1355,A183,1))","v":9.2088225949051807},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A183,1),INDEX(LinMotor!$AG$1:$AG$1355,A183,1))","v":27.127536253921118},{"$f":"IF(A183<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A183,1),INDEX(LinMotor!$AI$1:$AI$1355,A183,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A183,1),INDEX(LinMotor!$AI$1:$AI$1355,A183,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A183,1),INDEX(LinMotor!$AI$1:$AI$1355,A183,1))/1000,\"0.0k\")),\"\")","v":23.051365115686874},{"$f":"IF(A183<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A183,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A183,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A183,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A183,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A183,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A183,1))/1000,\"0.0k\")),\"\")","v":2.4306362028790298},{"$f":"IF(A183<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A183,1),INDEX(LinMotor!$AK$1:$AK$1355,A183,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A183,1),INDEX(LinMotor!$AK$1:$AK$1355,A183,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A183,1),INDEX(LinMotor!$AK$1:$AK$1355,A183,1))/1000,\"0.0k\")),\"\")","v":148.89897331710799},""]
[966,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A184,1),INDEX(LinMotor!$B$1:$B$1341,A184,1))","v":"KBMS-25H02-D (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A184,1),INDEX(LinMotor!$R$1:$R$1355,A184,1))","v":165.92920353982299},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A184,1),INDEX(LinMotor!$S$1:$S$1355,A184,1))","v":1.1534863312899279},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A184,1),INDEX(LinMotor!$T$1:$T$1355,A184,1))","v":0.98086980918120803},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A184,1),INDEX(LinMotor!$U$1:$U$1355,A184,1))","v":3.355852279662868E-2},{"$f":"IF(A184<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A184,1),INDEX(LinMotor!$V$1:$V$1355,A184,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A184,1),INDEX(LinMotor!$V$1:$V$1355,A184,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A184,1),INDEX(LinMotor!$V$1:$V$1355,A184,1))/1000,\"0.0k\")),\"\")","v":-22.678913967407407},{"$f":"IF(A184<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A184,1),INDEX(LinMotor!$W$1:$W$1355,A184,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A184,1),INDEX(LinMotor!$X$1:$X$1355,A184,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A184,1),INDEX(LinMotor!$W$1:$W$1355,A184,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A184,1),INDEX(LinMotor!$X$1:$X$1355,A184,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A184,1),INDEX(LinMotor!$W$1:$W$1355,A184,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A184,1),INDEX(LinMotor!$X$1:$X$1355,A184,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A184<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A184,1),INDEX(LinMotor!$X$1:$X$1355,A184,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A184,1),INDEX(LinMotor!$Z$1:$Z$1355,A184,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A184,1),INDEX(LinMotor!$X$1:$X$1355,A184,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A184,1),INDEX(LinMotor!$Z$1:$Z$1355,A184,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A184,1),INDEX(LinMotor!$X$1:$X$1355,A184,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A184,1),INDEX(LinMotor!$Z$1:$Z$1355,A184,1)))/1000,\"0.0k\")),\"\")","v":29.229920313600001},{"$f":"IF(A184<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A184,1),INDEX(LinMotor!$Y$1:$Y$1355,A184,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A184,1),INDEX(LinMotor!$AB$1:$AB$445,A184,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A184,1),INDEX(LinMotor!$Y$1:$Y$1355,A184,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A184,1),INDEX(LinMotor!$AB$1:$AB$445,A184,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A184,1),INDEX(LinMotor!$Y$1:$Y$1355,A184,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A184,1),INDEX(LinMotor!$AB$1:$AB$445,A184,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A184,1),INDEX(LinMotor!$AD$1:$AD$1355,A184,1))","v":0.38370094145438255},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A184,1),INDEX(LinMotor!$AE$1:$AE$1355,A184,1))","v":0.56515700529002333},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A184,1),INDEX(LinMotor!$AF$1:$AF$1355,A184,1))","v":9.2088225949051807},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A184,1),INDEX(LinMotor!$AG$1:$AG$1355,A184,1))","v":27.127536253921118},{"$f":"IF(A184<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A184,1),INDEX(LinMotor!$AI$1:$AI$1355,A184,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A184,1),INDEX(LinMotor!$AI$1:$AI$1355,A184,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A184,1),INDEX(LinMotor!$AI$1:$AI$1355,A184,1))/1000,\"0.0k\")),\"\")","v":23.051365115686874},{"$f":"IF(A184<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A184,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A184,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A184,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A184,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A184,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A184,1))/1000,\"0.0k\")),\"\")","v":2.4306362028790298},{"$f":"IF(A184<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A184,1),INDEX(LinMotor!$AK$1:$AK$1355,A184,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A184,1),INDEX(LinMotor!$AK$1:$AK$1355,A184,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A184,1),INDEX(LinMotor!$AK$1:$AK$1355,A184,1))/1000,\"0.0k\")),\"\")","v":148.89897331710799},""]
[967,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A185,1),INDEX(LinMotor!$B$1:$B$1341,A185,1))","v":"KBMS-25H02-D (480 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A185,1),INDEX(LinMotor!$R$1:$R$1355,A185,1))","v":165.92920353982299},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A185,1),INDEX(LinMotor!$S$1:$S$1355,A185,1))","v":1.1539595682556307},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A185,1),INDEX(LinMotor!$T$1:$T$1355,A185,1))","v":0.98086980918120803},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A185,1),INDEX(LinMotor!$U$1:$U$1355,A185,1))","v":3.355852279662868E-2},{"$f":"IF(A185<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A185,1),INDEX(LinMotor!$V$1:$V$1355,A185,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A185,1),INDEX(LinMotor!$V$1:$V$1355,A185,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A185,1),INDEX(LinMotor!$V$1:$V$1355,A185,1))/1000,\"0.0k\")),\"\")","v":-22.678913967407407},{"$f":"IF(A185<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A185,1),INDEX(LinMotor!$W$1:$W$1355,A185,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A185,1),INDEX(LinMotor!$X$1:$X$1355,A185,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A185,1),INDEX(LinMotor!$W$1:$W$1355,A185,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A185,1),INDEX(LinMotor!$X$1:$X$1355,A185,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A185,1),INDEX(LinMotor!$W$1:$W$1355,A185,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A185,1),INDEX(LinMotor!$X$1:$X$1355,A185,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A185<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A185,1),INDEX(LinMotor!$X$1:$X$1355,A185,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A185,1),INDEX(LinMotor!$Z$1:$Z$1355,A185,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A185,1),INDEX(LinMotor!$X$1:$X$1355,A185,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A185,1),INDEX(LinMotor!$Z$1:$Z$1355,A185,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A185,1),INDEX(LinMotor!$X$1:$X$1355,A185,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A185,1),INDEX(LinMotor!$Z$1:$Z$1355,A185,1)))/1000,\"0.0k\")),\"\")","v":29.229920313600001},{"$f":"IF(A185<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A185,1),INDEX(LinMotor!$Y$1:$Y$1355,A185,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A185,1),INDEX(LinMotor!$AB$1:$AB$445,A185,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A185,1),INDEX(LinMotor!$Y$1:$Y$1355,A185,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A185,1),INDEX(LinMotor!$AB$1:$AB$445,A185,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A185,1),INDEX(LinMotor!$Y$1:$Y$1355,A185,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A185,1),INDEX(LinMotor!$AB$1:$AB$445,A185,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A185,1),INDEX(LinMotor!$AD$1:$AD$1355,A185,1))","v":0.38370094145438255},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A185,1),INDEX(LinMotor!$AE$1:$AE$1355,A185,1))","v":0.56515700529002333},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A185,1),INDEX(LinMotor!$AF$1:$AF$1355,A185,1))","v":9.2088225949051807},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A185,1),INDEX(LinMotor!$AG$1:$AG$1355,A185,1))","v":27.127536253921118},{"$f":"IF(A185<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A185,1),INDEX(LinMotor!$AI$1:$AI$1355,A185,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A185,1),INDEX(LinMotor!$AI$1:$AI$1355,A185,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A185,1),INDEX(LinMotor!$AI$1:$AI$1355,A185,1))/1000,\"0.0k\")),\"\")","v":23.051365115686874},{"$f":"IF(A185<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A185,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A185,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A185,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A185,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A185,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A185,1))/1000,\"0.0k\")),\"\")","v":2.4306362028790298},{"$f":"IF(A185<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A185,1),INDEX(LinMotor!$AK$1:$AK$1355,A185,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A185,1),INDEX(LinMotor!$AK$1:$AK$1355,A185,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A185,1),INDEX(LinMotor!$AK$1:$AK$1355,A185,1))/1000,\"0.0k\")),\"\")","v":148.89897331710799},""]
[969,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A186,1),INDEX(LinMotor!$B$1:$B$1341,A186,1))","v":"KBMS-25H02-E (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A186,1),INDEX(LinMotor!$R$1:$R$1355,A186,1))","v":165.92920353982299},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A186,1),INDEX(LinMotor!$S$1:$S$1355,A186,1))","v":1.1230154534126859},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A186,1),INDEX(LinMotor!$T$1:$T$1355,A186,1))","v":0.98086980918120803},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A186,1),INDEX(LinMotor!$U$1:$U$1355,A186,1))","v":2.8420525552124168E-2},{"$f":"IF(A186<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A186,1),INDEX(LinMotor!$V$1:$V$1355,A186,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A186,1),INDEX(LinMotor!$V$1:$V$1355,A186,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A186,1),INDEX(LinMotor!$V$1:$V$1355,A186,1))/1000,\"0.0k\")),\"\")","v":-22.678913967407407},{"$f":"IF(A186<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A186,1),INDEX(LinMotor!$W$1:$W$1355,A186,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A186,1),INDEX(LinMotor!$X$1:$X$1355,A186,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A186,1),INDEX(LinMotor!$W$1:$W$1355,A186,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A186,1),INDEX(LinMotor!$X$1:$X$1355,A186,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A186,1),INDEX(LinMotor!$W$1:$W$1355,A186,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A186,1),INDEX(LinMotor!$X$1:$X$1355,A186,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A186<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A186,1),INDEX(LinMotor!$X$1:$X$1355,A186,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A186,1),INDEX(LinMotor!$Z$1:$Z$1355,A186,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A186,1),INDEX(LinMotor!$X$1:$X$1355,A186,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A186,1),INDEX(LinMotor!$Z$1:$Z$1355,A186,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A186,1),INDEX(LinMotor!$X$1:$X$1355,A186,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A186,1),INDEX(LinMotor!$Z$1:$Z$1355,A186,1)))/1000,\"0.0k\")),\"\")","v":29.229920313600001},{"$f":"IF(A186<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A186,1),INDEX(LinMotor!$Y$1:$Y$1355,A186,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A186,1),INDEX(LinMotor!$AB$1:$AB$445,A186,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A186,1),INDEX(LinMotor!$Y$1:$Y$1355,A186,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A186,1),INDEX(LinMotor!$AB$1:$AB$445,A186,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A186,1),INDEX(LinMotor!$Y$1:$Y$1355,A186,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A186,1),INDEX(LinMotor!$AB$1:$AB$445,A186,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A186,1),INDEX(LinMotor!$AD$1:$AD$1355,A186,1))","v":0.47650454204004417},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A186,1),INDEX(LinMotor!$AE$1:$AE$1355,A186,1))","v":0.70184836911186432},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A186,1),INDEX(LinMotor!$AF$1:$AF$1355,A186,1))","v":11.43610900896106},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A186,1),INDEX(LinMotor!$AG$1:$AG$1355,A186,1))","v":33.688721717369489},{"$f":"IF(A186<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A186,1),INDEX(LinMotor!$AI$1:$AI$1355,A186,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A186,1),INDEX(LinMotor!$AI$1:$AI$1355,A186,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A186,1),INDEX(LinMotor!$AI$1:$AI$1355,A186,1))/1000,\"0.0k\")),\"\")","v":23.051365115686874},{"$f":"IF(A186<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A186,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A186,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A186,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A186,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A186,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A186,1))/1000,\"0.0k\")),\"\")","v":2.4306362028790298},{"$f":"IF(A186<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A186,1),INDEX(LinMotor!$AK$1:$AK$1355,A186,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A186,1),INDEX(LinMotor!$AK$1:$AK$1355,A186,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A186,1),INDEX(LinMotor!$AK$1:$AK$1355,A186,1))/1000,\"0.0k\")),\"\")","v":148.89897331710799},""]
[970,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A187,1),INDEX(LinMotor!$B$1:$B$1341,A187,1))","v":"KBMS-25H02-E (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A187,1),INDEX(LinMotor!$R$1:$R$1355,A187,1))","v":165.92920353982299},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A187,1),INDEX(LinMotor!$S$1:$S$1355,A187,1))","v":1.1239604884112133},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A187,1),INDEX(LinMotor!$T$1:$T$1355,A187,1))","v":0.98086980918120803},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A187,1),INDEX(LinMotor!$U$1:$U$1355,A187,1))","v":2.6538022225695151E-2},{"$f":"IF(A187<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A187,1),INDEX(LinMotor!$V$1:$V$1355,A187,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A187,1),INDEX(LinMotor!$V$1:$V$1355,A187,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A187,1),INDEX(LinMotor!$V$1:$V$1355,A187,1))/1000,\"0.0k\")),\"\")","v":-22.678913967407407},{"$f":"IF(A187<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A187,1),INDEX(LinMotor!$W$1:$W$1355,A187,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A187,1),INDEX(LinMotor!$X$1:$X$1355,A187,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A187,1),INDEX(LinMotor!$W$1:$W$1355,A187,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A187,1),INDEX(LinMotor!$X$1:$X$1355,A187,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A187,1),INDEX(LinMotor!$W$1:$W$1355,A187,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A187,1),INDEX(LinMotor!$X$1:$X$1355,A187,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A187<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A187,1),INDEX(LinMotor!$X$1:$X$1355,A187,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A187,1),INDEX(LinMotor!$Z$1:$Z$1355,A187,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A187,1),INDEX(LinMotor!$X$1:$X$1355,A187,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A187,1),INDEX(LinMotor!$Z$1:$Z$1355,A187,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A187,1),INDEX(LinMotor!$X$1:$X$1355,A187,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A187,1),INDEX(LinMotor!$Z$1:$Z$1355,A187,1)))/1000,\"0.0k\")),\"\")","v":29.229920313600001},{"$f":"IF(A187<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A187,1),INDEX(LinMotor!$Y$1:$Y$1355,A187,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A187,1),INDEX(LinMotor!$AB$1:$AB$445,A187,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A187,1),INDEX(LinMotor!$Y$1:$Y$1355,A187,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A187,1),INDEX(LinMotor!$AB$1:$AB$445,A187,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A187,1),INDEX(LinMotor!$Y$1:$Y$1355,A187,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A187,1),INDEX(LinMotor!$AB$1:$AB$445,A187,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A187,1),INDEX(LinMotor!$AD$1:$AD$1355,A187,1))","v":0.47650454204004417},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A187,1),INDEX(LinMotor!$AE$1:$AE$1355,A187,1))","v":0.70184836911186432},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A187,1),INDEX(LinMotor!$AF$1:$AF$1355,A187,1))","v":11.43610900896106},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A187,1),INDEX(LinMotor!$AG$1:$AG$1355,A187,1))","v":33.688721717369489},{"$f":"IF(A187<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A187,1),INDEX(LinMotor!$AI$1:$AI$1355,A187,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A187,1),INDEX(LinMotor!$AI$1:$AI$1355,A187,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A187,1),INDEX(LinMotor!$AI$1:$AI$1355,A187,1))/1000,\"0.0k\")),\"\")","v":23.051365115686874},{"$f":"IF(A187<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A187,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A187,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A187,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A187,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A187,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A187,1))/1000,\"0.0k\")),\"\")","v":2.4306362028790298},{"$f":"IF(A187<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A187,1),INDEX(LinMotor!$AK$1:$AK$1355,A187,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A187,1),INDEX(LinMotor!$AK$1:$AK$1355,A187,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A187,1),INDEX(LinMotor!$AK$1:$AK$1355,A187,1))/1000,\"0.0k\")),\"\")","v":148.89897331710799},""]
[972,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A188,1),INDEX(LinMotor!$B$1:$B$1341,A188,1))","v":"KBMS-25H02-F (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A188,1),INDEX(LinMotor!$R$1:$R$1355,A188,1))","v":165.92920353982299},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A188,1),INDEX(LinMotor!$S$1:$S$1355,A188,1))","v":1.1131881166355215},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A188,1),INDEX(LinMotor!$T$1:$T$1355,A188,1))","v":0.9710936981262458},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A188,1),INDEX(LinMotor!$U$1:$U$1355,A188,1))","v":2.288352884139401E-2},{"$f":"IF(A188<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A188,1),INDEX(LinMotor!$V$1:$V$1355,A188,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A188,1),INDEX(LinMotor!$V$1:$V$1355,A188,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A188,1),INDEX(LinMotor!$V$1:$V$1355,A188,1))/1000,\"0.0k\")),\"\")","v":-22.678913967407407},{"$f":"IF(A188<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A188,1),INDEX(LinMotor!$W$1:$W$1355,A188,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A188,1),INDEX(LinMotor!$X$1:$X$1355,A188,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A188,1),INDEX(LinMotor!$W$1:$W$1355,A188,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A188,1),INDEX(LinMotor!$X$1:$X$1355,A188,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A188,1),INDEX(LinMotor!$W$1:$W$1355,A188,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A188,1),INDEX(LinMotor!$X$1:$X$1355,A188,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A188<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A188,1),INDEX(LinMotor!$X$1:$X$1355,A188,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A188,1),INDEX(LinMotor!$Z$1:$Z$1355,A188,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A188,1),INDEX(LinMotor!$X$1:$X$1355,A188,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A188,1),INDEX(LinMotor!$Z$1:$Z$1355,A188,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A188,1),INDEX(LinMotor!$X$1:$X$1355,A188,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A188,1),INDEX(LinMotor!$Z$1:$Z$1355,A188,1)))/1000,\"0.0k\")),\"\")","v":29.229920313600001},{"$f":"IF(A188<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A188,1),INDEX(LinMotor!$Y$1:$Y$1355,A188,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A188,1),INDEX(LinMotor!$AB$1:$AB$445,A188,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A188,1),INDEX(LinMotor!$Y$1:$Y$1355,A188,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A188,1),INDEX(LinMotor!$AB$1:$AB$445,A188,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A188,1),INDEX(LinMotor!$Y$1:$Y$1355,A188,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A188,1),INDEX(LinMotor!$AB$1:$AB$445,A188,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A188,1),INDEX(LinMotor!$AD$1:$AD$1355,A188,1))","v":0.58983170421879261},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A188,1),INDEX(LinMotor!$AE$1:$AE$1355,A188,1))","v":0.86876909480044795},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A188,1),INDEX(LinMotor!$AF$1:$AF$1355,A188,1))","v":14.155960901251023},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A188,1),INDEX(LinMotor!$AG$1:$AG$1355,A188,1))","v":41.700916550421503},{"$f":"IF(A188<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A188,1),INDEX(LinMotor!$AI$1:$AI$1355,A188,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A188,1),INDEX(LinMotor!$AI$1:$AI$1355,A188,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A188,1),INDEX(LinMotor!$AI$1:$AI$1355,A188,1))/1000,\"0.0k\")),\"\")","v":23.051365115686874},{"$f":"IF(A188<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A188,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A188,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A188,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A188,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A188,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A188,1))/1000,\"0.0k\")),\"\")","v":2.4306362028790298},{"$f":"IF(A188<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A188,1),INDEX(LinMotor!$AK$1:$AK$1355,A188,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A188,1),INDEX(LinMotor!$AK$1:$AK$1355,A188,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A188,1),INDEX(LinMotor!$AK$1:$AK$1355,A188,1))/1000,\"0.0k\")),\"\")","v":148.89897331710799},""]
[974,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A189,1),INDEX(LinMotor!$B$1:$B$1341,A189,1))","v":"KBMS-25H02-G (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A189,1),INDEX(LinMotor!$R$1:$R$1355,A189,1))","v":165.92920353982299},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A189,1),INDEX(LinMotor!$S$1:$S$1355,A189,1))","v":1.137679798860562},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A189,1),INDEX(LinMotor!$T$1:$T$1355,A189,1))","v":0.97433067711999999},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A189,1),INDEX(LinMotor!$U$1:$U$1355,A189,1))","v":2.0158954159834749E-2},{"$f":"IF(A189<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A189,1),INDEX(LinMotor!$V$1:$V$1355,A189,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A189,1),INDEX(LinMotor!$V$1:$V$1355,A189,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A189,1),INDEX(LinMotor!$V$1:$V$1355,A189,1))/1000,\"0.0k\")),\"\")","v":-22.678913967407407},{"$f":"IF(A189<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A189,1),INDEX(LinMotor!$W$1:$W$1355,A189,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A189,1),INDEX(LinMotor!$X$1:$X$1355,A189,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A189,1),INDEX(LinMotor!$W$1:$W$1355,A189,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A189,1),INDEX(LinMotor!$X$1:$X$1355,A189,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A189,1),INDEX(LinMotor!$W$1:$W$1355,A189,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A189,1),INDEX(LinMotor!$X$1:$X$1355,A189,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A189<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A189,1),INDEX(LinMotor!$X$1:$X$1355,A189,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A189,1),INDEX(LinMotor!$Z$1:$Z$1355,A189,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A189,1),INDEX(LinMotor!$X$1:$X$1355,A189,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A189,1),INDEX(LinMotor!$Z$1:$Z$1355,A189,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A189,1),INDEX(LinMotor!$X$1:$X$1355,A189,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A189,1),INDEX(LinMotor!$Z$1:$Z$1355,A189,1)))/1000,\"0.0k\")),\"\")","v":29.229920313600001},{"$f":"IF(A189<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A189,1),INDEX(LinMotor!$Y$1:$Y$1355,A189,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A189,1),INDEX(LinMotor!$AB$1:$AB$445,A189,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A189,1),INDEX(LinMotor!$Y$1:$Y$1355,A189,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A189,1),INDEX(LinMotor!$AB$1:$AB$445,A189,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A189,1),INDEX(LinMotor!$Y$1:$Y$1355,A189,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A189,1),INDEX(LinMotor!$AB$1:$AB$445,A189,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A189,1),INDEX(LinMotor!$AD$1:$AD$1355,A189,1))","v":0.67975980259424318},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A189,1),INDEX(LinMotor!$AE$1:$AE$1355,A189,1))","v":1.0012251022750571},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A189,1),INDEX(LinMotor!$AF$1:$AF$1355,A189,1))","v":16.314235262261835},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A189,1),INDEX(LinMotor!$AG$1:$AG$1355,A189,1))","v":48.058804909202742},{"$f":"IF(A189<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A189,1),INDEX(LinMotor!$AI$1:$AI$1355,A189,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A189,1),INDEX(LinMotor!$AI$1:$AI$1355,A189,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A189,1),INDEX(LinMotor!$AI$1:$AI$1355,A189,1))/1000,\"0.0k\")),\"\")","v":23.051365115686874},{"$f":"IF(A189<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A189,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A189,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A189,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A189,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A189,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A189,1))/1000,\"0.0k\")),\"\")","v":2.4306362028790298},{"$f":"IF(A189<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A189,1),INDEX(LinMotor!$AK$1:$AK$1355,A189,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A189,1),INDEX(LinMotor!$AK$1:$AK$1355,A189,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A189,1),INDEX(LinMotor!$AK$1:$AK$1355,A189,1))/1000,\"0.0k\")),\"\")","v":148.89897331710799},""]
[980,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A190,1),INDEX(LinMotor!$B$1:$B$1341,A190,1))","v":"KBMS-25H03-B (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A190,1),INDEX(LinMotor!$R$1:$R$1355,A190,1))","v":120.83780880773362},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A190,1),INDEX(LinMotor!$S$1:$S$1355,A190,1))","v":0.83999415631331464},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A190,1),INDEX(LinMotor!$T$1:$T$1355,A190,1))","v":0.69224229000472814},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A190,1),INDEX(LinMotor!$U$1:$U$1355,A190,1))","v":5.3073761764700404E-2},{"$f":"IF(A190<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A190,1),INDEX(LinMotor!$V$1:$V$1355,A190,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A190,1),INDEX(LinMotor!$V$1:$V$1355,A190,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A190,1),INDEX(LinMotor!$V$1:$V$1355,A190,1))/1000,\"0.0k\")),\"\")","v":-22.743023292839506},{"$f":"IF(A190<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A190,1),INDEX(LinMotor!$W$1:$W$1355,A190,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A190,1),INDEX(LinMotor!$X$1:$X$1355,A190,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A190,1),INDEX(LinMotor!$W$1:$W$1355,A190,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A190,1),INDEX(LinMotor!$X$1:$X$1355,A190,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A190,1),INDEX(LinMotor!$W$1:$W$1355,A190,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A190,1),INDEX(LinMotor!$X$1:$X$1355,A190,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A190<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A190,1),INDEX(LinMotor!$X$1:$X$1355,A190,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A190,1),INDEX(LinMotor!$Z$1:$Z$1355,A190,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A190,1),INDEX(LinMotor!$X$1:$X$1355,A190,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A190,1),INDEX(LinMotor!$Z$1:$Z$1355,A190,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A190,1),INDEX(LinMotor!$X$1:$X$1355,A190,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A190,1),INDEX(LinMotor!$Z$1:$Z$1355,A190,1)))/1000,\"0.0k\")),\"\")","v":29.281848867200001},{"$f":"IF(A190<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A190,1),INDEX(LinMotor!$Y$1:$Y$1355,A190,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A190,1),INDEX(LinMotor!$AB$1:$AB$445,A190,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A190,1),INDEX(LinMotor!$Y$1:$Y$1355,A190,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A190,1),INDEX(LinMotor!$AB$1:$AB$445,A190,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A190,1),INDEX(LinMotor!$Y$1:$Y$1355,A190,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A190,1),INDEX(LinMotor!$AB$1:$AB$445,A190,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A190,1),INDEX(LinMotor!$AD$1:$AD$1355,A190,1))","v":0.25397280465277899},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A190,1),INDEX(LinMotor!$AE$1:$AE$1355,A190,1))","v":0.3745760157385698},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A190,1),INDEX(LinMotor!$AF$1:$AF$1355,A190,1))","v":6.0953473116666963},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A190,1),INDEX(LinMotor!$AG$1:$AG$1355,A190,1))","v":17.97964875545135},{"$f":"IF(A190<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A190,1),INDEX(LinMotor!$AI$1:$AI$1355,A190,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A190,1),INDEX(LinMotor!$AI$1:$AI$1355,A190,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A190,1),INDEX(LinMotor!$AI$1:$AI$1355,A190,1))/1000,\"0.0k\")),\"\")","v":23.061683764075173},{"$f":"IF(A190<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A190,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A190,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A190,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A190,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A190,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A190,1))/1000,\"0.0k\")),\"\")","v":2.4395193800850512},{"$f":"IF(A190<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A190,1),INDEX(LinMotor!$AK$1:$AK$1355,A190,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A190,1),INDEX(LinMotor!$AK$1:$AK$1355,A190,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A190,1),INDEX(LinMotor!$AK$1:$AK$1355,A190,1))/1000,\"0.0k\")),\"\")","v":149.44315017261758},""]
[981,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A191,1),INDEX(LinMotor!$B$1:$B$1341,A191,1))","v":"KBMS-25H03-B (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A191,1),INDEX(LinMotor!$R$1:$R$1355,A191,1))","v":120.83780880773362},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A191,1),INDEX(LinMotor!$S$1:$S$1355,A191,1))","v":0.84147331584759455},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A191,1),INDEX(LinMotor!$T$1:$T$1355,A191,1))","v":0.69224229000472814},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A191,1),INDEX(LinMotor!$U$1:$U$1355,A191,1))","v":4.1728832911881453E-2},{"$f":"IF(A191<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A191,1),INDEX(LinMotor!$V$1:$V$1355,A191,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A191,1),INDEX(LinMotor!$V$1:$V$1355,A191,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A191,1),INDEX(LinMotor!$V$1:$V$1355,A191,1))/1000,\"0.0k\")),\"\")","v":-22.743023292839506},{"$f":"IF(A191<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A191,1),INDEX(LinMotor!$W$1:$W$1355,A191,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A191,1),INDEX(LinMotor!$X$1:$X$1355,A191,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A191,1),INDEX(LinMotor!$W$1:$W$1355,A191,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A191,1),INDEX(LinMotor!$X$1:$X$1355,A191,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A191,1),INDEX(LinMotor!$W$1:$W$1355,A191,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A191,1),INDEX(LinMotor!$X$1:$X$1355,A191,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A191<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A191,1),INDEX(LinMotor!$X$1:$X$1355,A191,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A191,1),INDEX(LinMotor!$Z$1:$Z$1355,A191,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A191,1),INDEX(LinMotor!$X$1:$X$1355,A191,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A191,1),INDEX(LinMotor!$Z$1:$Z$1355,A191,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A191,1),INDEX(LinMotor!$X$1:$X$1355,A191,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A191,1),INDEX(LinMotor!$Z$1:$Z$1355,A191,1)))/1000,\"0.0k\")),\"\")","v":29.281848867200001},{"$f":"IF(A191<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A191,1),INDEX(LinMotor!$Y$1:$Y$1355,A191,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A191,1),INDEX(LinMotor!$AB$1:$AB$445,A191,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A191,1),INDEX(LinMotor!$Y$1:$Y$1355,A191,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A191,1),INDEX(LinMotor!$AB$1:$AB$445,A191,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A191,1),INDEX(LinMotor!$Y$1:$Y$1355,A191,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A191,1),INDEX(LinMotor!$AB$1:$AB$445,A191,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A191,1),INDEX(LinMotor!$AD$1:$AD$1355,A191,1))","v":0.25397280465277899},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A191,1),INDEX(LinMotor!$AE$1:$AE$1355,A191,1))","v":0.3745760157385698},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A191,1),INDEX(LinMotor!$AF$1:$AF$1355,A191,1))","v":6.0953473116666963},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A191,1),INDEX(LinMotor!$AG$1:$AG$1355,A191,1))","v":17.97964875545135},{"$f":"IF(A191<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A191,1),INDEX(LinMotor!$AI$1:$AI$1355,A191,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A191,1),INDEX(LinMotor!$AI$1:$AI$1355,A191,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A191,1),INDEX(LinMotor!$AI$1:$AI$1355,A191,1))/1000,\"0.0k\")),\"\")","v":23.061683764075173},{"$f":"IF(A191<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A191,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A191,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A191,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A191,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A191,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A191,1))/1000,\"0.0k\")),\"\")","v":2.4395193800850512},{"$f":"IF(A191<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A191,1),INDEX(LinMotor!$AK$1:$AK$1355,A191,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A191,1),INDEX(LinMotor!$AK$1:$AK$1355,A191,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A191,1),INDEX(LinMotor!$AK$1:$AK$1355,A191,1))/1000,\"0.0k\")),\"\")","v":149.44315017261758},""]
[982,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A192,1),INDEX(LinMotor!$B$1:$B$1341,A192,1))","v":"KBMS-25H03-B (480 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A192,1),INDEX(LinMotor!$R$1:$R$1355,A192,1))","v":120.83780880773362},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A192,1),INDEX(LinMotor!$S$1:$S$1355,A192,1))","v":0.84039404596885292},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A192,1),INDEX(LinMotor!$T$1:$T$1355,A192,1))","v":0.69224229000472814},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A192,1),INDEX(LinMotor!$U$1:$U$1355,A192,1))","v":4.1728832911881453E-2},{"$f":"IF(A192<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A192,1),INDEX(LinMotor!$V$1:$V$1355,A192,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A192,1),INDEX(LinMotor!$V$1:$V$1355,A192,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A192,1),INDEX(LinMotor!$V$1:$V$1355,A192,1))/1000,\"0.0k\")),\"\")","v":-22.743023292839506},{"$f":"IF(A192<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A192,1),INDEX(LinMotor!$W$1:$W$1355,A192,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A192,1),INDEX(LinMotor!$X$1:$X$1355,A192,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A192,1),INDEX(LinMotor!$W$1:$W$1355,A192,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A192,1),INDEX(LinMotor!$X$1:$X$1355,A192,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A192,1),INDEX(LinMotor!$W$1:$W$1355,A192,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A192,1),INDEX(LinMotor!$X$1:$X$1355,A192,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A192<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A192,1),INDEX(LinMotor!$X$1:$X$1355,A192,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A192,1),INDEX(LinMotor!$Z$1:$Z$1355,A192,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A192,1),INDEX(LinMotor!$X$1:$X$1355,A192,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A192,1),INDEX(LinMotor!$Z$1:$Z$1355,A192,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A192,1),INDEX(LinMotor!$X$1:$X$1355,A192,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A192,1),INDEX(LinMotor!$Z$1:$Z$1355,A192,1)))/1000,\"0.0k\")),\"\")","v":29.281848867200001},{"$f":"IF(A192<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A192,1),INDEX(LinMotor!$Y$1:$Y$1355,A192,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A192,1),INDEX(LinMotor!$AB$1:$AB$445,A192,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A192,1),INDEX(LinMotor!$Y$1:$Y$1355,A192,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A192,1),INDEX(LinMotor!$AB$1:$AB$445,A192,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A192,1),INDEX(LinMotor!$Y$1:$Y$1355,A192,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A192,1),INDEX(LinMotor!$AB$1:$AB$445,A192,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A192,1),INDEX(LinMotor!$AD$1:$AD$1355,A192,1))","v":0.25397280465277899},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A192,1),INDEX(LinMotor!$AE$1:$AE$1355,A192,1))","v":0.3745760157385698},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A192,1),INDEX(LinMotor!$AF$1:$AF$1355,A192,1))","v":6.0953473116666963},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A192,1),INDEX(LinMotor!$AG$1:$AG$1355,A192,1))","v":17.97964875545135},{"$f":"IF(A192<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A192,1),INDEX(LinMotor!$AI$1:$AI$1355,A192,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A192,1),INDEX(LinMotor!$AI$1:$AI$1355,A192,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A192,1),INDEX(LinMotor!$AI$1:$AI$1355,A192,1))/1000,\"0.0k\")),\"\")","v":23.061683764075173},{"$f":"IF(A192<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A192,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A192,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A192,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A192,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A192,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A192,1))/1000,\"0.0k\")),\"\")","v":2.4395193800850512},{"$f":"IF(A192<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A192,1),INDEX(LinMotor!$AK$1:$AK$1355,A192,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A192,1),INDEX(LinMotor!$AK$1:$AK$1355,A192,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A192,1),INDEX(LinMotor!$AK$1:$AK$1355,A192,1))/1000,\"0.0k\")),\"\")","v":149.44315017261758},""]
[984,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A193,1),INDEX(LinMotor!$B$1:$B$1341,A193,1))","v":"KBMS-25H03-C (240 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A193,1),INDEX(LinMotor!$R$1:$R$1355,A193,1))","v":120.83780880773362},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A193,1),INDEX(LinMotor!$S$1:$S$1355,A193,1))","v":0.83573615043191363},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A193,1),INDEX(LinMotor!$T$1:$T$1355,A193,1))","v":0.6906096430943397},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A193,1),INDEX(LinMotor!$U$1:$U$1355,A193,1))","v":4.7579953091747486E-2},{"$f":"IF(A193<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A193,1),INDEX(LinMotor!$V$1:$V$1355,A193,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A193,1),INDEX(LinMotor!$V$1:$V$1355,A193,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A193,1),INDEX(LinMotor!$V$1:$V$1355,A193,1))/1000,\"0.0k\")),\"\")","v":-22.743023292839506},{"$f":"IF(A193<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A193,1),INDEX(LinMotor!$W$1:$W$1355,A193,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A193,1),INDEX(LinMotor!$X$1:$X$1355,A193,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A193,1),INDEX(LinMotor!$W$1:$W$1355,A193,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A193,1),INDEX(LinMotor!$X$1:$X$1355,A193,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A193,1),INDEX(LinMotor!$W$1:$W$1355,A193,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A193,1),INDEX(LinMotor!$X$1:$X$1355,A193,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A193<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A193,1),INDEX(LinMotor!$X$1:$X$1355,A193,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A193,1),INDEX(LinMotor!$Z$1:$Z$1355,A193,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A193,1),INDEX(LinMotor!$X$1:$X$1355,A193,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A193,1),INDEX(LinMotor!$Z$1:$Z$1355,A193,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A193,1),INDEX(LinMotor!$X$1:$X$1355,A193,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A193,1),INDEX(LinMotor!$Z$1:$Z$1355,A193,1)))/1000,\"0.0k\")),\"\")","v":29.281848867200001},{"$f":"IF(A193<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A193,1),INDEX(LinMotor!$Y$1:$Y$1355,A193,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A193,1),INDEX(LinMotor!$AB$1:$AB$445,A193,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A193,1),INDEX(LinMotor!$Y$1:$Y$1355,A193,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A193,1),INDEX(LinMotor!$AB$1:$AB$445,A193,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A193,1),INDEX(LinMotor!$Y$1:$Y$1355,A193,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A193,1),INDEX(LinMotor!$AB$1:$AB$445,A193,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A193,1),INDEX(LinMotor!$AD$1:$AD$1355,A193,1))","v":0.28501741539570941},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A193,1),INDEX(LinMotor!$AE$1:$AE$1355,A193,1))","v":0.42036267631484586},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A193,1),INDEX(LinMotor!$AF$1:$AF$1355,A193,1))","v":6.8404179694970253},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A193,1),INDEX(LinMotor!$AG$1:$AG$1355,A193,1))","v":20.177408463112602},{"$f":"IF(A193<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A193,1),INDEX(LinMotor!$AI$1:$AI$1355,A193,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A193,1),INDEX(LinMotor!$AI$1:$AI$1355,A193,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A193,1),INDEX(LinMotor!$AI$1:$AI$1355,A193,1))/1000,\"0.0k\")),\"\")","v":23.061683764075173},{"$f":"IF(A193<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A193,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A193,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A193,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A193,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A193,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A193,1))/1000,\"0.0k\")),\"\")","v":2.4395193800850512},{"$f":"IF(A193<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A193,1),INDEX(LinMotor!$AK$1:$AK$1355,A193,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A193,1),INDEX(LinMotor!$AK$1:$AK$1355,A193,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A193,1),INDEX(LinMotor!$AK$1:$AK$1355,A193,1))/1000,\"0.0k\")),\"\")","v":149.44315017261758},""]
[985,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A194,1),INDEX(LinMotor!$B$1:$B$1341,A194,1))","v":"KBMS-25H03-C (400 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A194,1),INDEX(LinMotor!$R$1:$R$1355,A194,1))","v":120.83780880773362},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A194,1),INDEX(LinMotor!$S$1:$S$1355,A194,1))","v":0.83601701767205261},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A194,1),INDEX(LinMotor!$T$1:$T$1355,A194,1))","v":0.6906096430943397},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A194,1),INDEX(LinMotor!$U$1:$U$1355,A194,1))","v":3.7269014177351609E-2},{"$f":"IF(A194<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A194,1),INDEX(LinMotor!$V$1:$V$1355,A194,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A194,1),INDEX(LinMotor!$V$1:$V$1355,A194,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A194,1),INDEX(LinMotor!$V$1:$V$1355,A194,1))/1000,\"0.0k\")),\"\")","v":-22.743023292839506},{"$f":"IF(A194<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A194,1),INDEX(LinMotor!$W$1:$W$1355,A194,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A194,1),INDEX(LinMotor!$X$1:$X$1355,A194,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A194,1),INDEX(LinMotor!$W$1:$W$1355,A194,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A194,1),INDEX(LinMotor!$X$1:$X$1355,A194,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A194,1),INDEX(LinMotor!$W$1:$W$1355,A194,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A194,1),INDEX(LinMotor!$X$1:$X$1355,A194,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A194<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A194,1),INDEX(LinMotor!$X$1:$X$1355,A194,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A194,1),INDEX(LinMotor!$Z$1:$Z$1355,A194,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A194,1),INDEX(LinMotor!$X$1:$X$1355,A194,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A194,1),INDEX(LinMotor!$Z$1:$Z$1355,A194,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A194,1),INDEX(LinMotor!$X$1:$X$1355,A194,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A194,1),INDEX(LinMotor!$Z$1:$Z$1355,A194,1)))/1000,\"0.0k\")),\"\")","v":29.281848867200001},{"$f":"IF(A194<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A194,1),INDEX(LinMotor!$Y$1:$Y$1355,A194,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A194,1),INDEX(LinMotor!$AB$1:$AB$445,A194,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A194,1),INDEX(LinMotor!$Y$1:$Y$1355,A194,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A194,1),INDEX(LinMotor!$AB$1:$AB$445,A194,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A194,1),INDEX(LinMotor!$Y$1:$Y$1355,A194,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A194,1),INDEX(LinMotor!$AB$1:$AB$445,A194,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A194,1),INDEX(LinMotor!$AD$1:$AD$1355,A194,1))","v":0.28501741539570941},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A194,1),INDEX(LinMotor!$AE$1:$AE$1355,A194,1))","v":0.42036267631484586},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A194,1),INDEX(LinMotor!$AF$1:$AF$1355,A194,1))","v":6.8404179694970253},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A194,1),INDEX(LinMotor!$AG$1:$AG$1355,A194,1))","v":20.177408463112602},{"$f":"IF(A194<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A194,1),INDEX(LinMotor!$AI$1:$AI$1355,A194,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A194,1),INDEX(LinMotor!$AI$1:$AI$1355,A194,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A194,1),INDEX(LinMotor!$AI$1:$AI$1355,A194,1))/1000,\"0.0k\")),\"\")","v":23.061683764075173},{"$f":"IF(A194<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A194,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A194,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A194,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A194,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A194,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A194,1))/1000,\"0.0k\")),\"\")","v":2.4395193800850512},{"$f":"IF(A194<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A194,1),INDEX(LinMotor!$AK$1:$AK$1355,A194,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A194,1),INDEX(LinMotor!$AK$1:$AK$1355,A194,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A194,1),INDEX(LinMotor!$AK$1:$AK$1355,A194,1))/1000,\"0.0k\")),\"\")","v":149.44315017261758},""]
[986,{"$f":"IF(Calc!$A$90,INDEX(Motor!$B$1:$B$1223,A195,1),INDEX(LinMotor!$B$1:$B$1341,A195,1))","v":"KBMS-25H03-C (480 V)"},{"$f":"IF(Calc!$A$90,INDEX(Motor!$T$1:$T$1223,A195,1),INDEX(LinMotor!$R$1:$R$1355,A195,1))","v":120.83780880773362},{"$f":"IF(Calc!$A$90,INDEX(Motor!$U$1:$U$1223,A195,1),INDEX(LinMotor!$S$1:$S$1355,A195,1))","v":0.83640043944381948},{"$f":"IF(Calc!$A$90,INDEX(Motor!$V$1:$V$1223,A195,1),INDEX(LinMotor!$T$1:$T$1355,A195,1))","v":0.6906096430943397},{"$f":"IF(Calc!$A$90,INDEX(Motor!$W$1:$W$1223,A195,1),INDEX(LinMotor!$U$1:$U$1355,A195,1))","v":3.7269014177351609E-2},{"$f":"IF(A195<>2,IF(ABS(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A195,1),INDEX(LinMotor!$V$1:$V$1355,A195,1)))<1000,IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A195,1),INDEX(LinMotor!$V$1:$V$1355,A195,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1223,A195,1),INDEX(LinMotor!$V$1:$V$1355,A195,1))/1000,\"0.0k\")),\"\")","v":-22.743023292839506},{"$f":"IF(A195<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A195,1),INDEX(LinMotor!$W$1:$W$1355,A195,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,A195,1),INDEX(LinMotor!$X$1:$X$1355,A195,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A195,1),INDEX(LinMotor!$W$1:$W$1355,A195,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A195,1),INDEX(LinMotor!$X$1:$X$1355,A195,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1223,A195,1),INDEX(LinMotor!$W$1:$W$1355,A195,1)),IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A195,1),INDEX(LinMotor!$X$1:$X$1355,A195,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(A195<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A195,1),INDEX(LinMotor!$X$1:$X$1355,A195,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A195,1),INDEX(LinMotor!$Z$1:$Z$1355,A195,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A195,1),INDEX(LinMotor!$X$1:$X$1355,A195,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A195,1),INDEX(LinMotor!$Z$1:$Z$1355,A195,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1223,A195,1),INDEX(LinMotor!$X$1:$X$1355,A195,1)),IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1223,A195,1),INDEX(LinMotor!$Z$1:$Z$1355,A195,1)))/1000,\"0.0k\")),\"\")","v":29.281848867200001},{"$f":"IF(A195<>2,IF(ABS(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A195,1),INDEX(LinMotor!$Y$1:$Y$1355,A195,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A195,1),INDEX(LinMotor!$AB$1:$AB$445,A195,1))))<1000,IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A195,1),INDEX(LinMotor!$Y$1:$Y$1355,A195,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A195,1),INDEX(LinMotor!$AB$1:$AB$445,A195,1))),TEXT(IF(move1,IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1223,A195,1),INDEX(LinMotor!$Y$1:$Y$1355,A195,1)),IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1223,A195,1),INDEX(LinMotor!$AB$1:$AB$445,A195,1)))/1000,\"0.0k\")),\"\")","v":9},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AF$1:$AF$1223,A195,1),INDEX(LinMotor!$AD$1:$AD$1355,A195,1))","v":0.28501741539570941},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AG$1:$AG$1223,A195,1),INDEX(LinMotor!$AE$1:$AE$1355,A195,1))","v":0.42036267631484586},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AH$1:$AH$1223,A195,1),INDEX(LinMotor!$AF$1:$AF$1355,A195,1))","v":6.8404179694970253},{"$f":"IF(Calc!$A$90,INDEX(Motor!$AI$1:$AI$1223,A195,1),INDEX(LinMotor!$AG$1:$AG$1355,A195,1))","v":20.177408463112602},{"$f":"IF(A195<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A195,1),INDEX(LinMotor!$AI$1:$AI$1355,A195,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A195,1),INDEX(LinMotor!$AI$1:$AI$1355,A195,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AK$1:$AK$1223,A195,1),INDEX(LinMotor!$AI$1:$AI$1355,A195,1))/1000,\"0.0k\")),\"\")","v":23.061683764075173},{"$f":"IF(A195<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A195,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A195,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A195,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A195,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AL$1:$AL$1223,A195,1),INDEX(LinMotor!$AJ$1:$AJ$1355,A195,1))/1000,\"0.0k\")),\"\")","v":2.4395193800850512},{"$f":"IF(A195<>2,IF(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A195,1),INDEX(LinMotor!$AK$1:$AK$1355,A195,1))<1000,IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A195,1),INDEX(LinMotor!$AK$1:$AK$1355,A195,1)),TEXT(IF(Calc!$A$90,INDEX(Motor!$AM$1:$AM$1223,A195,1),INDEX(LinMotor!$AK$1:$AK$1355,A195,1))/1000,\"0.0k\")),\"\")","v":149.44315017261758},""]
[1," ...",null,null,"Auswahl einschränken",null,null,null,null,null,null,null,null,null,null,null,null,""]
[121,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5]

{"sheet":"Inertia","index":1,"n_rows":54,"n_cols":13,"rows_kept":54,"cut":false,"hidden":false,"merged":[[53,10,54,10],[53,11,54,11],[48,11,49,11],[8,6,9,6],[13,6,14,6],[13,7,14,7],[13,10,14,10],[13,11,14,11],[33,10,34,10],[33,11,34,11],[33,7,34,7],[48,10,49,10],[6,12,7,12],[8,7,9,7],[8,8,9,8],[8,9,9,9],[8,11,9,11],[8,12,9,12],[8,10,9,10],[26,12,27,12],[28,6,29,6],[28,7,29,7],[28,8,29,8],[28,9,29,9],[28,11,29,11],[28,12,29,12],[28,10,29,10],[0,2,0,13],[13,8,14,8],[33,8,34,8],[53,8,54,8],[13,12,14,12],[33,12,34,12],[53,12,54,12],[53,6,54,6],[53,7,54,7],[33,6,34,6],[46,12,47,12],[48,6,49,6],[48,7,49,7],[48,8,49,8],[48,9,49,9],[48,12,49,12]]}
[]
[]
[null,null,{"$f":"IF(deutsch,\"Massenträgheit 1\",\"Inertia 1\")","v":"Massenträgheit 1"}]
[]
[]
[]
[null,null,null,null,null,null,"Gewicht","Durchmesser",null,null,"Last","Reibung"]
[null,null,null,null,null,null,"G [kg]","D [mm]",null,null,"F Last [N]","F Reibung [N]"]
[null,null,null,null,null,null,5,300,null,null,{"$f":"G9*10","v":50},{"$f":"G9*10*0.2","v":10}]
[]
[]
[null,null,null,null,null,null,{"$f":"IF(deutsch,\"Massenträgheit\",\"Inertia\")","v":"Massenträgheit"},{"$f":"IF(deutsch,\"Lastmoment\",\"Load\")","v":"Lastmoment"},{"$f":"IF(deutsch,\"Reibmoment\",\"Friction\")","v":"Reibmoment"},null,{"$f":"IF(deutsch,\"Sum. Massenträgheit\",\"Sum inertia\")","v":"Sum. Massenträgheit"},{"$f":"IF(deutsch,\"Sum. Lastmoment\",\"Sum load\")","v":"Sum. Lastmoment"},{"$f":"IF(deutsch,\"Sum. Reibmoment\",\"Sum friction\")","v":"Sum. Reibmoment"}]
[null,null,null,null,null,null,"[10-3kgm2]",{"$f":"IF(deutsch,\"T Last [Nm]\",\"T Load [Nm]\")","v":"T Last [Nm]"},{"$f":"IF(deutsch,\"T Reibung [Nm]\",\"T Friction [Nm]\")","v":"T Reibung [Nm]"},null,"[10-3kgm2]",{"$f":"IF(deutsch,\"T Last [Nm]\",\"T Load [Nm]\")","v":"T Last [Nm]"},{"$f":"IF(deutsch,\"T Reibung [Nm]\",\"T Friction [Nm]\")","v":"T Reibung [Nm]"}]
[null,null,null,null,null,null,{"$f":"Calc!A72*(1000*G9*(H9/2000)^2)","v":112.5},{"$f":"H9*K9/2000","v":7.5},{"$f":"H9*L9/2000","v":1.5},null,{"$f":"G14+G34+G54","v":112.5},{"$f":"H14+H34+H54","v":7.5},{"$f":"I14+I34+I54","v":1.5}]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"IF(deutsch,\"Massenträgheit 2\",\"Inertia 2\")","v":"Massenträgheit 2"}]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,5,50,null,null,{"$f":"G29*10","v":50},{"$f":"G29*10*0.2","v":10}]
[]
[]
[null,null,null,null,null,null,{"$f":"IF(deutsch,\"Massenträgheit\",\"Inertia\")","v":"Massenträgheit"},{"$f":"IF(deutsch,\"Lastmoment\",\"Load\")","v":"Lastmoment"},{"$f":"IF(deutsch,\"Reibmoment\",\"Friction\")","v":"Reibmoment"},null,{"$f":"IF(deutsch,\"Sum. Massenträgheit\",\"Sum inertia\")","v":"Sum. Massenträgheit"},{"$f":"IF(deutsch,\"Sum. Lastmoment\",\"Sum load\")","v":"Sum. Lastmoment"},{"$f":"IF(deutsch,\"Sum. Reibmoment\",\"Sum friction\")","v":"Sum. Reibmoment"}]
[null,null,null,null,null,null,"[10-3kgm2]",{"$f":"IF(deutsch,\"T Last [Nm]\",\"T Load [Nm]\")","v":"T Last [Nm]"},{"$f":"IF(deutsch,\"T Reibung [Nm]\",\"T Friction [Nm]\")","v":"T Reibung [Nm]"},null,"[10-3kgm2]",{"$f":"IF(deutsch,\"T Last [Nm]\",\"T Load [Nm]\")","v":"T Last [Nm]"},{"$f":"IF(deutsch,\"T Reibung [Nm]\",\"T Friction [Nm]\")","v":"T Reibung [Nm]"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"G14+G34+G54","v":112.5},{"$f":"H14+H34+H54","v":7.5},{"$f":"I14+I34+I54","v":1.5}]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,{"$f":"IF(deutsch,\"Massenträgheit 3\",\"Inertia 3\")","v":"Massenträgheit 3"}]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,5,50,null,null,{"$f":"G49*10","v":50},{"$f":"G49*10*0.2","v":10}]
[]
[]
[null,null,null,null,null,null,{"$f":"IF(deutsch,\"Massenträgheit\",\"Inertia\")","v":"Massenträgheit"},{"$f":"IF(deutsch,\"Lastmoment\",\"Load\")","v":"Lastmoment"},{"$f":"IF(deutsch,\"Reibmoment\",\"Friction\")","v":"Reibmoment"},null,{"$f":"IF(deutsch,\"Sum. Massenträgheit\",\"Sum inertia\")","v":"Sum. Massenträgheit"},{"$f":"IF(deutsch,\"Sum. Lastmoment\",\"Sum load\")","v":"Sum. Lastmoment"},{"$f":"IF(deutsch,\"Sum. Reibmoment\",\"Sum friction\")","v":"Sum. Reibmoment"}]
[null,null,null,null,null,null,"[10-3kgm2]",{"$f":"IF(deutsch,\"T Last [Nm]\",\"T Load [Nm]\")","v":"T Last [Nm]"},{"$f":"IF(deutsch,\"T Reibung [Nm]\",\"T Friction [Nm]\")","v":"T Reibung [Nm]"},null,"[10-3kgm2]",{"$f":"IF(deutsch,\"T Last [Nm]\",\"T Load [Nm]\")","v":"T Last [Nm]"},{"$f":"IF(deutsch,\"T Reibung [Nm]\",\"T Friction [Nm]\")","v":"T Reibung [Nm]"}]
[null,null,null,null,null,null,null,null,null,null,{"$f":"G14+G34+G54","v":112.5},{"$f":"H14+H34+H54","v":7.5},{"$f":"I14+I34+I54","v":1.5}]

{"sheet":"Drives","index":2,"n_rows":69,"n_cols":23,"rows_kept":69,"cut":false,"hidden":true,"merged":[]}
["Selected"]
["S724",480,24,48,1.7,16,200]
[]
[]
[]
[]
[]
[]
["Drives","AC-\nVoltage\n[V]","Icont\n[Arms]","Ipeak\n[Arms]","Lmin \nbei UAC\n[mH]","Lmax \nbei UAC\n[mH]","Brake \nPower\n[W]","AKM","DBL","DBK","6SMx7","6SM45100","AKMH","ACC","Goldline BH","DDR","KBM","Sonstige","IC/ICD","IL",null,"ICH","Sonstige"]
["DMC30515(P)",230,3.5,10,4,null,50,null,null,null,null,null,null,1]
["DMC31025(P)",230,7,17,3,null,50,null,null,null,null,null,null,1]
["DMC32050(P)",230,14,35,2,null,100,null,null,null,null,null,null,1]
["DMC34080",230,28,56,1,null,"external",null,null,null,null,null,null,1]
["DMC50412(P)",400,3,8,10,null,40,null,null,null,null,null,null,1]
["DMC50720(P)",400,5,14,8,null,40,null,null,null,null,null,null,1]
["DMC51540(P)",400,10,28,6,null,80,null,null,null,null,null,null,1]
["DMC53080",400,21,56,3,null,"external",null,null,null,null,null,null,1]
["SAM-DA-400-07",400,6.5,10,null,null,"external",null,null,null,null,null,null,1]
["SAM-DA-400-14",400,15,28,null,null,"external",null,null,null,null,null,null,1]
["SAM-DA-400-28",400,20,38,null,null,"external",null,null,null,null,null,null,1]
["SAM-DA-400-50",400,34,62,null,null,"external",null,null,null,null,null,null,1]
["Servostar 303",230,3,9,5.9,null,40,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 306",230,6,15,3.6,null,80,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 310",230,10,20,2.7,null,80,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 341",480,1.5,4.5,35.6,null,40,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 343",480,3,7.5,17.8,null,80,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 346",480,6,12,10.7,null,80,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 403M/A",230,3,9,6.9,43.1,40,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 406M/A",230,6,12,4.3,23,40,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 443M/403A",400,3,9,12,75,40,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 446M/406A",400,6,12,7.5,40,40,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 601",480,1.5,3,30,180,80,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 603",480,3,6,14.4,90,80,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 606",480,6,12,9,48,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 610",480,10,20,4.8,30,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 610/30",480,10,30,4.8,30,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 614",480,14,28,3,18,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 620",480,20,40,2.4,14.4,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 640",480,40,80,1.3,null,"external",1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar 670",480,70,140,0.8,null,"external",1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["Servostar S20260",230,1.5,4.5,2.5,150,"external",1,null,null,null,null,1,null,null,1,1,1,null,null,null,null,1]
["Servostar S20360",230,3,9,5,300,"external",1,null,null,null,null,1,null,null,1,1,1,null,null,null,null,1]
["Servostar S20330",50,3,9,0.2,15,"external",1,null,null,null,null,1,null,null,1,1,1,null,null,null,null,1]
["Servostar S20630",50,6,18,0.4,30,"external",1,null,null,null,null,1,null,null,1,1,1,null,null,null,null,1]
["ST1/140-310",230,30,100,0.2,0.2,"external",null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1]
["ST1/25-310",230,10,17,1.2,1.2,"external",null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1]
["ST1/80-310",230,20,56,0.4,0.4,"external",null,null,null,null,null,null,null,null,null,null,1,null,null,null,null,1]
["S701",480,1.5,4.5,17.8,180,20,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S703",480,3,9,8.9,80,50,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S706",480,6,18,4.4000000000000004,48,50,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S712",480,12,24,2.7,30,100,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S712P",480,12,30,2.7,30,100,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S724",480,24,48,1.7,16,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S724P",480,24,72,1.7,16,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S748",480,48,96,0.85,8,0,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S772",480,72,140,0.57999999999999996,5.5,0,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["S 131xx   5A 230V",230,5,10,null,null,66,1,1,1,1,1,1,null,1,1,null,1,1,1,null,1,1]
["S 132xx   10A 480V",480,10,20,null,null,200,1,1,1,1,1,1,null,1,1,null,1,1,1,null,1,1]
["S 132xx   15A 480V",480,15,30,null,null,200,1,1,1,1,1,1,null,1,1,null,1,1,1,null,1,1]
["S 132xx   20A 480V",480,20,40,null,null,200,1,1,1,1,1,1,null,1,1,null,1,1,1,null,1,1]
["AKD-B00306",230,3,9,2.5,250,"external",1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B00606",230,6,18,1.3,125,"external",1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B01206",230,12,30,1,100,100,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B02406",230,24,48,0.6,60,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B00307",480,3,9,6.3,600,80,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B00607",480,6,18,3.2,300,100,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B01207",480,12,30,2.5,250,100,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B02407",480,24,48,1.2,120,200,1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]
["AKD-B04807",480,48,96,0.6,60,"external",1,1,1,1,1,1,null,1,1,1,1,1,1,null,1,1]

{"sheet":"Motor","index":3,"n_rows":1223,"n_cols":52,"rows_kept":1223,"cut":false,"hidden":true,"merged":[[0,0,1,0]]}
["Motor\nLinie","Typ","M0","I0","Mn","In","nn","Mmax","nmax","RU-V","LU-V","KE","J","UDCmax","Poles","Nmax","Nmax","Nmax","MnStrich","Jext/Jmot","Trms","Tpk","n","T (t1)","T (t2)","T (t3)","T (t4)","T (t5)","T (t6)","T (t7)","T (t8)","Irms","Ipeak","Irms","Ipeak","Ipeak","P","PbrRMS","PbrPEAK","Koeff","Koeff","Koeff","nmax","Koeff","Koeff","Koeff","nmax","Inenn","Koeff","Koeff","Koeff","nmax"]
[null,"Kein Motor","[Nm]","[A]","[Nm]","[A] ","[min-1]","[Nm]","[min-1] ","[W]","[mH]","[V/1000]","[10-3kgm2]","[V]",null,"bei Mmax","bei Mn","bei M0",null," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," ","trapez"," "," "," ","A","B","C","theo","A","B","C","theo","nmax","A","B","C","theo"]
["Other","power_rotor_test",4.8,4.87,3.01,3.0404040404040402,5000,16.100000000000001,6000,2.61,10.8,63.9,0.21,640,10,{"$f":"IFERROR(IF(AQ3<I3,IF(AQ3<0,0,AQ3),I3),0)","v":3593.2633044796335},{"$f":"IFERROR(IF(AU3<I3,IF(AU3<0,0,AU3),I3),0)","v":5878.3105151918489},{"$f":"IFERROR(IF(UAC_V*0.98/L3*1000<I3,IF(UAC_V*0.98/L3*1000<0,0,UAC_V*0.98/L3*1000),I3),0)","v":6000},{"$f":"IFERROR(C3+(E3-C3)/G3*Q3,0)","v":2.6955648355613175},{"$f":"IFERROR(IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M3,(inertia/gear^2+gear_inertia)/M3),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M3,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M3)),0)","v":535.71428571428578},{"$f":"IFERROR(IF((C3+(E3-C3)/G3*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X3^2*time1+Y3^2*time2+Z3^2*time3+AA3^2*time4)/time)/(C3+(E3-C3)/G3*mspeed),SQRT((((X3-Y3)*2/PI()+Y3)^2*time1+Y3^2*time2+((Z3-Y3)*2/PI()+Y3)^2*time3+AA3^2*time4)/time)/(C3+(E3-C3)/G3*mspeed)),IF(AccType=1,SQRT((X3^2*time1+Y3^2*time2+Z3^2*time3+AA3^2*time4+AB3^2*time5+AC3^2*time6+AD3^2*time7+AE3^2*time8)/time)/(C3+(E3-C3)/G3*mspeed),SQRT((((X3-Y3)*2/PI()+Y3)^2*time1+Y3^2*time2+((Z3-Y3)*2/PI()+Y3)^2*time3+AA3^2*time4+((AB3-AC3)*2/PI()+AC3)^2*time5+AC3^2*time6+((AD3-AC3)*2/PI()+AC3)^2*time7+AE3^2*time8)/time)/(C3+(E3-C3)/G3*mspeed)))),0)","v":2.0689048915774868},{"$f":"IFERROR(IF(move1,MAX(ABS(X3),ABS(Z3))/H3,MAX(ABS(X3),ABS(Z3),ABS(AB3),ABS(AD3))/H3),0)","v":1.8095566926708075},{"$f":"IFERROR(IF(AZ3>0,speed/(MIN(AZ3,I3)),\"NA\"),0)","v":4.3990370629987764E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M3+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M3+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.560324385185183},{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M3+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M3+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.133862752000002},{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M3+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M3+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2354.5982399999998},{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M3+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M3+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2366.5982399999998},{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},{"$f":"AH3/Irms","v":0.41912061404570283},{"$f":"AI3/Ipeak","v":0.61580690799583337},{"$f":"IFERROR(IF(move1,IF(AccType=1,SQRT((X3^2*time1+Y3^2*time2+Z3^2*time3+AA3^2*time4)/time)/(C3/D3),SQRT((((X3-Y3)*2/PI()+Y3)^2*time1+Y3^2*time2+((Z3-AA3)*2/PI()+AA3)^2*time3+AA3^2*time4)/time)/(C3/D3)),IF(AccType=1,SQRT((X3^2*time1+Y3^2*time2+Z3^2*time3+AA3^2*time4+AB3^2*time5+AC3^2*time6+AD3^2*time7+AE3^2*time8)/time)/(C3/D3),SQRT((((X3-Y3)*2/PI()+Y3)^2*time1+Y3^2*time2+((Z3-AA3)*2/PI()+AA3)^2*time3+AA3^2*time4+((AB3-AC3)*2/PI()+AC3)^2*time5+AC3^2*time6+((AD3-AE3)*2/PI()+AE3)^2*time7+AE3^2*time8)/time)/(C3/D3))),0)","v":10.058894737096868},{"$f":"IFERROR(IF(move1,MAX(ABS(X3),ABS(Z3))/(C3/D3),MAX(ABS(X3),ABS(Z3),ABS(AB3),ABS(AD3))/(C3/D3)),0)","v":29.558731583800004},{"$f":"IFERROR(IF(move1,IF(AccType=1,MAX(ABS(X3),ABS(Z3))/(C3/D3),MAX(ABS((X3-Y3)*2/PI()+Y3),ABS((Z3-Y3)*2/PI()+Y3))/(C3/D3)),IF(AccType=1,MAX(ABS(X3),ABS(Z3),ABS(AB3),ABS(AD3))/(C3/D3),MAX(ABS((X3-Y3)*2/PI()+Y3),ABS((Z3-Y3)*2/PI()+Y3),ABS((AB3-AC3)*2/PI()+AC3),ABS((AD3-AC3)*2/PI()+AC3))/(C3/D3))),0)","v":22.13578867592172},{"$f":"IFERROR(IF((C3+(E3-C3)/G3*mspeed)<0,\"NA\",U3*(C3+(E3-C3)/G3*mspeed)*mspeed/9.55),0)","v":23.032326264912953},{"$f":"IF(move1,IF(speed1>speed2,AM3/2*time1/time,AM3/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z3*-speed/30*PI(),((Z3-AA3)*2/PI()+AA3)*-speed/30*PI()),IF(AccType=1,X3*-speed/30*PI(),((X3-Y3)*2/PI()+Y3)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z3*-speed/30*PI(),((Z3-AA3)*2/PI()+AA3)*-speed/30*PI()),IF(AccType=1,X3*-speed/30*PI(),((X3-Y3)*2/PI()+Y3)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD3*-speed/30*PI(),((AD3-AE3)*2/PI()+AE3)*-speed/30*PI()),IF(AccType=1,AB3*-speed/30*PI(),((AB3-AC3)*2/PI()+AC3)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD3*-speed/30*PI(),((AD3-AE3)*2/PI()+AE3)*-speed/30*PI()),IF(AccType=1,AB3*-speed/30*PI(),((AB3-AC3)*2/PI()+AC3)*-speed/30*PI()),0)/2*time7/time)))","v":2.414204080616507},{"$f":"IF(move1,MAX(IF(AccType=1,Z3*-speed/30*PI(),((Z3-AA3)*2/PI()+AA3)*-speed/30*PI()),IF(AccType=1,X3*-speed/30*PI(),((X3-Y3)*2/PI()+Y3)*-speed/30*PI()),0),MAX(IF(AccType=1,Z3*-speed/30*PI(),((Z3-AA3)*2/PI()+AA3)*-speed/30*PI()),IF(AccType=1,X3*-speed/30*PI(),((X3-Y3)*2/PI()+Y3)*-speed/30*PI()),IF(AccType=1,AD3*-speed/30*PI(),((AD3-AE3)*2/PI()+AE3)*-speed/30*PI()),IF(AccType=1,AB3*-speed/30*PI(),((AB3-AC3)*2/PI()+AC3)*-speed/30*PI()),0))","v":147.89235367924826},{"$f":"IFERROR((L3^2)/1000000+((K3/1000)^2*(D3/C3*H3)^2*PI()*PI()*(O3/2)^2)/1200,0)","v":1.0482521026179489E-2},{"$f":"IFERROR(SQRT(3)*L3*J3*D3/C3*H3/1000,0)","v":4.7186263950285383},{"$f":"IFERROR(0.75*J3^2*(D3/C3*H3)^2-(UAC_V*0.98)^2,0)","v":-152300.76892347808},{"$f":"IFERROR(-AO3/2/AN3+SQRT((AO3/2/AN3)^2-AP3/AN3),0)","v":3593.2633044796335},{"$f":"IFERROR((L3^2)/1000000+((K3/1000)^2*AV3^2*PI()*PI()*(O3/2)^2)/1200,0)","v":4.2984541698830063E-3},{"$f":"IFERROR(SQRT(3)*L3*J3*AV3/1000,0)","v":0.8653955981903696},{"$f":"IFERROR(0.75*J3^2*AV3^2-(UAC_V*0.98)^2,0)","v":-153618.14701047906},{"$f":"IFERROR(-AS3/2/AR3+SQRT((AS3/2/AR3)^2-AT3/AR3),0)","v":5878.3105151918489},{"$f":"IFERROR(D3+(F3-D3)*((0.85*UAC_V-D3*J3)/L3*1000)/G3,0)","v":2.9957991208169323},{"$f":"(L3^2)/1000000+((K3/1000)^2*AJ3^2*PI()*PI()*(O3/2)^2)/1200","v":1.5834783443362054E-2},{"$f":"SQRT(3)*L3*J3*AJ3/1000","v":6.3943586702806448},{"$f":"0.75*J3^2*AJ3^2-(UAC_V*0.98)^2","v":-151160.5882966959},{"$f":"IFERROR(IF(((AX3/2/AW3)^2-AY3/AW3)>0,-AX3/2/AW3+SQRT((AX3/2/AW3)^2-AY3/AW3),-9999),0)","v":2894.3596666748904}]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IFERROR(IF(AQ4<I4,IF(AQ4<0,0,AQ4),I4),0)","v":0},{"$f":"IFERROR(IF(AU4<I4,IF(AU4<0,0,AU4),I4),0)","v":0},0,{"$f":"IFERROR(C4+(E4-C4)/G4*Q4,0)","v":0},0,0,0,"NA",-22.507111111111108,9,29.090760000000003,9,-2350.1999999999998,7.5,2362.1999999999998,9,0,0,0,0,0,0,2.4068306924217855,147.44066538020863,{"$f":"IFERROR((L4^2)/1000000+((K4/1000)^2*(D4/C4*H4)^2*PI()*PI()*(O4/2)^2)/1200,0)","v":0},{"$f":"IFERROR(SQRT(3)*L4*J4*D4/C4*H4/1000,0)","v":0},0,{"$f":"IFERROR(-AO4/2/AN4+SQRT((AO4/2/AN4)^2-AP4/AN4),0)","v":0},{"$f":"IFERROR((L4^2)/1000000+((K4/1000)^2*AV4^2*PI()*PI()*(O4/2)^2)/1200,0)","v":0},{"$f":"IFERROR(SQRT(3)*L4*J4*AV4/1000,0)","v":0},-153664,{"$f":"IFERROR(-AS4/2/AR4+SQRT((AS4/2/AR4)^2-AT4/AR4),0)","v":0},0,0,0,-153664,{"$f":"IFERROR(IF(((AX4/2/AW4)^2-AY4/AW4)>0,-AX4/2/AW4+SQRT((AX4/2/AW4)^2-AY4/AW4),-9999),0)","v":0}]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",-22.507111111111108,9,29.090760000000003,9,-2350.1999999999998,7.5,2362.1999999999998,9,0,0,0,0,0,0,2.4068306924217855,147.44066538020863,0,0,0,0,0,0,-153664,0,0,0,0,-153664,0]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",-22.507111111111108,9,29.090760000000003,9,-2350.1999999999998,7.5,2362.1999999999998,9,0,0,0,0,0,0,2.4068306924217855,147.44066538020863,0,0,0,0,0,0,-153664,0,0,0,0,-153664,0]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",-22.507111111111108,9,29.090760000000003,9,-2350.1999999999998,7.5,2362.1999999999998,9,0,0,0,0,0,0,2.4068306924217855,147.44066538020863,0,0,0,0,0,0,-153664,0,0,0,0,-153664,0]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",-22.507111111111108,9,29.090760000000003,9,-2350.1999999999998,7.5,2362.1999999999998,9,0,0,0,0,0,0,2.4068306924217855,147.44066538020863,0,0,0,0,0,0,-153664,0,0,0,0,-153664,0]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",-22.507111111111108,9,29.090760000000003,9,-2350.1999999999998,7.5,2362.1999999999998,9,0,0,0,0,0,0,2.4068306924217855,147.44066538020863,0,0,0,0,0,0,-153664,0,0,0,0,-153664,0]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",-22.507111111111108,9,29.090760000000003,9,-2350.1999999999998,7.5,2362.1999999999998,9,0,0,0,0,0,0,2.4068306924217855,147.44066538020863,0,0,0,0,0,0,-153664,0,0,0,0,-153664,0]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",-22.507111111111108,9,29.090760000000003,9,-2350.1999999999998,7.5,2362.1999999999998,9,0,0,0,0,0,0,2.4068306924217855,147.44066538020863,0,0,0,0,0,0,-153664,0,0,0,0,-153664,0]
["Other","",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"NA",-22.507111111111108,9,29.090760000000003,9,-2350.1999999999998,7.5,2362.1999999999998,9,0,0,0,0,0,0,2.4068306924217855,147.44066538020863,0,0,0,0,0,0,-153664,0,0,0,0,-153664,0]
["Leerzeile"]
["AKM","AKM11B",0.183,1.1599999999999999,0.16700000000000001,1.0569620253164558,8000,0.61,8000,20.2,12.5,10.199999999999999,1.7000000000000001E-3,320,6,{"$f":"IF(AQ14<I14,IF(AQ14<0,0,AQ14),I14)","v":8000},{"$f":"IF(AU14<I14,IF(AU14<0,0,AU14),I14)","v":8000},{"$f":"IF(UAC_V*0.98/L14*1000<I14,IF(UAC_V*0.98/L14*1000<0,0,UAC_V*0.98/L14*1000),I14)","v":8000},{"$f":"C14+(E14-C14)/G14*Q14","v":0.16700000000000001},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M14,(inertia/gear^2+gear_inertia)/M14),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M14,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M14))","v":66176.470588235286},{"$f":"IF((C14+(E14-C14)/G14*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X14^2*time1+Y14^2*time2+Z14^2*time3+AA14^2*time4)/time)/(C14+(E14-C14)/G14*mspeed),SQRT((((X14-Y14)*2/PI()+Y14)^2*time1+Y14^2*time2+((Z14-Y14)*2/PI()+Y14)^2*time3+AA14^2*time4)/time)/(C14+(E14-C14)/G14*mspeed)),IF(AccType=1,SQRT((X14^2*time1+Y14^2*time2+Z14^2*time3+AA14^2*time4+AB14^2*time5+AC14^2*time6+AD14^2*time7+AE14^2*time8)/time)/(C14+(E14-C14)/G14*mspeed),SQRT((((X14-Y14)*2/PI()+Y14)^2*time1+Y14^2*time2+((Z14-Y14)*2/PI()+Y14)^2*time3+AA14^2*time4+((AB14-AC14)*2/PI()+AC14)^2*time5+AC14^2*time6+((AD14-AC14)*2/PI()+AC14)^2*time7+AE14^2*time8)/time)/(C14+(E14-C14)/G14*mspeed))))","v":54.169813067090423},{"$f":"IF(move1,MAX(ABS(X14),ABS(Z14))/H14,MAX(ABS(X14),ABS(Z14),ABS(AB14),ABS(AD14))/H14)","v":47.690342503344262},{"$f":"IF(AZ14>0,speed/(MIN(AZ14,I14)),\"NA\")","v":"NA"},-22.50754188523457,9,29.091108927040001,9,-2350.2356047999997,7.5,2362.2356047999997,9,2.6175727954595343,3.841722034991621,{"$f":"IF(move1,IF(AccType=1,SQRT((X14^2*time1+Y14^2*time2+Z14^2*time3+AA14^2*time4)/time)/(C14/D14),SQRT((((X14-Y14)*2/PI()+Y14)^2*time1+Y14^2*time2+((Z14-AA14)*2/PI()+AA14)^2*time3+AA14^2*time4)/time)/(C14/D14)),IF(AccType=1,SQRT((X14^2*time1+Y14^2*time2+Z14^2*time3+AA14^2*time4+AB14^2*time5+AC14^2*time6+AD14^2*time7+AE14^2*time8)/time)/(C14/D14),SQRT((((X14-Y14)*2/PI()+Y14)^2*time1+Y14^2*time2+((Z14-AA14)*2/PI()+AA14)^2*time3+AA14^2*time4+((AB14-AC14)*2/PI()+AC14)^2*time5+AC14^2*time6+((AD14-AE14)*2/PI()+AE14)^2*time7+AE14^2*time8)/time)/(C14/D14)))","v":62.821747091028826},{"$f":"IF(move1,MAX(ABS(X14),ABS(Z14))/(C14/D14),MAX(ABS(X14),ABS(Z14),ABS(AB14),ABS(AD14))/(C14/D14))","v":184.40265767959781},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X14),ABS(Z14))/(C14/D14),MAX(ABS((X14-Y14)*2/PI()+Y14),ABS((Z14-Y14)*2/PI()+Y14))/(C14/D14)),IF(AccType=1,MAX(ABS(X14),ABS(Z14),ABS(AB14),ABS(AD14))/(C14/D14),MAX(ABS((X14-Y14)*2/PI()+Y14),ABS((Z14-Y14)*2/PI()+Y14),ABS((AB14-AC14)*2/PI()+AC14),ABS((AD14-AC14)*2/PI()+AC14))/(C14/D14)))","v":138.12492208974649},{"$f":"IF((C14+(E14-C14)/G14*mspeed)<0,\"NA\",U14*(C14+(E14-C14)/G14*mspeed)*mspeed/9.55)","v":23.02387267643433},2.4068903817547911,147.44432190453423,{"$f":"(L14^2)/1000000+((K14/1000)^2*(D14/C14*H14)^2*PI()*PI()*(O14/2)^2)/1200","v":2.7696369377741982E-4},{"$f":"SQRT(3)*L14*J14*D14/C14*H14/1000","v":1.3799040937804334},{"$f":"0.75*J14^2*(D14/C14*H14)^2-(UAC_V*0.98)^2","v":-149088.51146666668},{"$f":"-AO14/2/AN14+SQRT((AO14/2/AN14)^2-AP14/AN14)","v":20843.437367070565},{"$f":"(L14^2)/1000000+((K14/1000)^2*AV14^2*PI()*PI()*(O14/2)^2)/1200","v":1.1072511581782929E-4},{"$f":"SQRT(3)*L14*J14*AV14/1000","v":0.27131644565884899},{"$f":"0.75*J14^2*AV14^2-(UAC_V*0.98)^2","v":-153487.11463455172},{"$f":"-AS14/2/AR14+SQRT((AS14/2/AR14)^2-AT14/AR14)","v":36026.674718795148},{"$f":"D14+(F14-D14)*((0.85*UAC_V-D14*J14)/L14*1000)/G14","v":0.76026316703896801},{"$f":"(L14^2)/1000000+((K14/1000)^2*AJ14^2*PI()*PI()*(O14/2)^2)/1200","v":0.22076480877914417},{"$f":"SQRT(3)*L14*J14*AJ14/1000","v":49.292882442606356},5684927.5501264203,{"$f":"IF(((AX14/2/AW14)^2-AY14/AW14)>0,-AX14/2/AW14+SQRT((AX14/2/AW14)^2-AY14/AW14),-9999)","v":-9999}]
["AKM","AKM11C",0.185,1.45,0.17599999999999999,1.3643410852713178,6000,0.61,8000,13.1,8.3000000000000007,8.3000000000000007,1.7000000000000001E-3,320,6,{"$f":"IF(AQ15<I15,IF(AQ15<0,0,AQ15),I15)","v":8000},{"$f":"IF(AU15<I15,IF(AU15<0,0,AU15),I15)","v":8000},{"$f":"IF(UAC_V*0.98/L15*1000<I15,IF(UAC_V*0.98/L15*1000<0,0,UAC_V*0.98/L15*1000),I15)","v":8000},{"$f":"C15+(E15-C15)/G15*Q15","v":0.17299999999999999},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M15,(inertia/gear^2+gear_inertia)/M15),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M15,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M15))","v":66176.470588235286},{"$f":"IF((C15+(E15-C15)/G15*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X15^2*time1+Y15^2*time2+Z15^2*time3+AA15^2*time4)/time)/(C15+(E15-C15)/G15*mspeed),SQRT((((X15-Y15)*2/PI()+Y15)^2*time1+Y15^2*time2+((Z15-Y15)*2/PI()+Y15)^2*time3+AA15^2*time4)/time)/(C15+(E15-C15)/G15*mspeed)),IF(AccType=1,SQRT((X15^2*time1+Y15^2*time2+Z15^2*time3+AA15^2*time4+AB15^2*time5+AC15^2*time6+AD15^2*time7+AE15^2*time8)/time)/(C15+(E15-C15)/G15*mspeed),SQRT((((X15-Y15)*2/PI()+Y15)^2*time1+Y15^2*time2+((Z15-Y15)*2/PI()+Y15)^2*time3+AA15^2*time4+((AB15-AC15)*2/PI()+AC15)^2*time5+AC15^2*time6+((AD15-AC15)*2/PI()+AC15)^2*time7+AE15^2*time8)/time)/(C15+(E15-C15)/G15*mspeed))))","v":53.580839381721475},{"$f":"IF(move1,MAX(ABS(X15),ABS(Z15))/H15,MAX(ABS(X15),ABS(Z15),ABS(AB15),ABS(AD15))/H15)","v":47.690342503344262},{"$f":"IF(AZ15>0,speed/(MIN(AZ15,I15)),\"NA\")","v":"NA"},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M15+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M15+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.50754188523457},{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M15+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M15+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.091108927040001},{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M15+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M15+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2350.2356047999997},{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M15+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M15+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2362.2356047999997},{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},{"$f":"AH15/Irms","v":3.2365933889803702},{"$f":"AI15/Ipeak","v":4.7502373811045047},77.678241335528881,{"$f":"IF(move1,MAX(ABS(X15),ABS(Z15))/(C15/D15),MAX(ABS(X15),ABS(Z15),ABS(AB15),ABS(AD15))/(C15/D15))","v":228.01139429301622},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X15),ABS(Z15))/(C15/D15),MAX(ABS((X15-Y15)*2/PI()+Y15),ABS((Z15-Y15)*2/PI()+Y15))/(C15/D15)),IF(AccType=1,MAX(ABS(X15),ABS(Z15),ABS(AB15),ABS(AD15))/(C15/D15),MAX(ABS((X15-Y15)*2/PI()+Y15),ABS((Z15-Y15)*2/PI()+Y15),ABS((AB15-AC15)*2/PI()+AC15),ABS((AD15-AC15)*2/PI()+AC15))/(C15/D15)))","v":170.78959961097033},{"$f":"IF((C15+(E15-C15)/G15*mspeed)<0,\"NA\",U15*(C15+(E15-C15)/G15*mspeed)*mspeed/9.55)","v":23.02387267643433},{"$f":"IF(move1,IF(speed1>speed2,AM15/2*time1/time,AM15/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z15*-speed/30*PI(),((Z15-AA15)*2/PI()+AA15)*-speed/30*PI()),IF(AccType=1,X15*-speed/30*PI(),((X15-Y15)*2/PI()+Y15)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z15*-speed/30*PI(),((Z15-AA15)*2/PI()+AA15)*-speed/30*PI()),IF(AccType=1,X15*-speed/30*PI(),((X15-Y15)*2/PI()+Y15)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD15*-speed/30*PI(),((AD15-AE15)*2/PI()+AE15)*-speed/30*PI()),IF(AccType=1,AB15*-speed/30*PI(),((AB15-AC15)*2/PI()+AC15)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD15*-speed/30*PI(),((AD15-AE15)*2/PI()+AE15)*-speed/30*PI()),IF(AccType=1,AB15*-speed/30*PI(),((AB15-AC15)*2/PI()+AC15)*-speed/30*PI()),0)/2*time7/time)))","v":2.4068903817547911},{"$f":"IF(move1,MAX(IF(AccType=1,Z15*-speed/30*PI(),((Z15-AA15)*2/PI()+AA15)*-speed/30*PI()),IF(AccType=1,X15*-speed/30*PI(),((X15-Y15)*2/PI()+Y15)*-speed/30*PI()),0),MAX(IF(AccType=1,Z15*-speed/30*PI(),((Z15-AA15)*2/PI()+AA15)*-speed/30*PI()),IF(AccType=1,X15*-speed/30*PI(),((X15-Y15)*2/PI()+Y15)*-speed/30*PI()),IF(AccType=1,AD15*-speed/30*PI(),((AD15-AE15)*2/PI()+AE15)*-speed/30*PI()),IF(AccType=1,AB15*-speed/30*PI(),((AB15-AC15)*2/PI()+AC15)*-speed/30*PI()),0))","v":147.44432190453423},{"$f":"(L15^2)/1000000+((K15/1000)^2*(D15/C15*H15)^2*PI()*PI()*(O15/2)^2)/1200","v":1.8545533367685276E-4},{"$f":"SQRT(3)*L15*J15*D15/C15*H15/1000","v":0.90040132253789007},{"$f":"0.75*J15^2*(D15/C15*H15)^2-(UAC_V*0.98)^2","v":-150721.90919716947},{"$f":"-AO15/2/AN15+SQRT((AO15/2/AN15)^2-AP15/AN15)","v":26183.743692548192},{"$f":"(L15^2)/1000000+((K15/1000)^2*AV15^2*PI()*PI()*(O15/2)^2)/1200","v":7.300080895924574E-5},{"$f":"SQRT(3)*L15*J15*AV15/1000","v":0.16908888713191261},{"$f":"0.75*J15^2*AV15^2-(UAC_V*0.98)^2","v":-153560.24382438848},{"$f":"-AS15/2/AR15+SQRT((AS15/2/AR15)^2-AT15/AR15)","v":44720.873017402395},{"$f":"D15+(F15-D15)*((0.85*UAC_V-D15*J15)/L15*1000)/G15","v":0.89785261199838129},{"$f":"(L15^2)/1000000+((K15/1000)^2*AJ15^2*PI()*PI()*(O15/2)^2)/1200","v":0.14881308797693715},{"$f":"SQRT(3)*L15*J15*AJ15/1000","v":32.164102377168305},{"$f":"0.75*J15^2*AJ15^2-(UAC_V*0.98)^2","v":3600616.3082049778},{"$f":"IF(((AX15/2/AW15)^2-AY15/AW15)>0,-AX15/2/AW15+SQRT((AX15/2/AW15)^2-AY15/AW15),-9999)","v":-9999}]
["AKM","AKM11E",0.185,2.91,0.17599999999999999,2.75,6000,0.61,8000,3.3,2.04,4.0999999999999996,1.7000000000000001E-3,320,6,8000,8000,8000,0.17299999999999999,66176.470588235286,53.580839381721475,47.690342503344262,"NA",-22.50754188523457,9,29.091108927040001,9,-2350.2356047999997,7.5,2362.2356047999997,9,6.4955081116778466,9.5332350200097302,155.89219468026832,457.59528096046705,342.75705852960255,23.02387267643433,2.4068903817547911,147.44432190453423,4.517113027776887E-5,0.22485860890062109,-152912.04589534915,55746.480391174729,1.6988434110440788E-5,1.7835557632030628E-2,-153659.2690791784,94581.375405725877,0.76107642276422549,3.6207274555963197E-2,8.0323908195535516,805873.51157121034,-9999]
["AKM","AKM12C",0.31,1.51,0.27900000000000003,1.347826086956522,8000,1.08,8000,12.4,9.1,13.3,3.0999999999999999E-3,320,6,8000,8000,8000,0.27900000000000003,36290.322580645159,31.978857591851444,26.936478035851856,"NA",-22.50789664039506,9,29.091396278720005,9,-2350.2649264000001,7.5,2362.2649264000001,9,2.0114451451999895,2.9521511008647319,48.274683484799745,141.70325284150712,106.14121286939825,23.02392945179329,2.4069395376760885,147.44733315986113,3.4652747961446957E-4,1.5027023391151291,-150472.58963199999,18782.453134280287,1.8327133463476574E-4,0.29145252119030463,-153543.94718171153,28160.481931833176,1.0203140405361235,6.9234554304128088E-2,30.319218264141579,1145526.1692416989,-9999]
["AKM","AKM12E",0.31,2.72,0.27900000000000003,2.4910714285714288,8000,1.08,8000,3.9,2.7,7.2,3.0999999999999999E-3,320,6,8000,8000,8000,0.27900000000000003,36290.322580645159,31.978857591851444,26.936478035851856,"NA",-22.50789664039506,9,29.091396278720005,9,-2350.2649264000001,7.5,2362.2649264000001,9,3.6232654271152129,5.3177821154649472,86.958370250765114,255.25354154231746,191.19476755282332,23.02392945179329,2.4069395376760885,147.44733315986113,1.0029632443798256E-4,0.46088088535802108,-152639.64047796879,36781.370510379864,5.2914108329413184E-5,6.8617912927634389E-2,-153641.29350899623,53240.55458378102,1.4108465277777784,1.9777908755885289E-2,9.2989461673221445,263342.17198473762,-9999]
["AKM","AKM13C",0.40899999999999997,1.48,0.40699999999999997,1.464028776978417,8000,1.46,8000,13.5,10.3,17.899999999999999,4.5000000000000005E-3,320,6,8000,8000,8000,0.40699999999999997,24999.999999999996,24.231920418103758,19.925810705753424,"NA",-22.508251395555554,9,29.091683630399999,9,-2350.2942479999997,7.5,2362.2942479999997,9,1.4942814947213041,2.1931383339951096,35.862755873311301,105.27064003176527,78.851660947957768,23.023986227718769,2.4069886935973868,147.45034441518806,5.3959861099869843E-4,2.2112542977603922,-149848.85255659639,14740.975158050043,3.3679155117837174E-4,0.60451517763982621,-153378.86642115031,20461.781917602915,1.4443078855351468,4.9147084905286041E-2,33.003368812521856,696202.07235677761,-9999]
["AKM","AKM13D",0.40100000000000002,2.4,0.36499999999999999,2.1597633136094672,7000,1.44,8000,5.21,3.8,10.9,4.5000000000000005E-3,320,6,8000,8000,8000,0.35985714285714282,24999.999999999996,24.722049421606876,20.202558076666666,"NA",-22.508251395555554,9,29.091683630399999,9,-2350.2942479999997,7.5,2362.2942479999997,9,2.4715015084222416,3.6273919738653357,59.316036202133802,174.11481474553611,130.41853202553639,23.023986227718769,2.4069886935973868,147.45034441518806,1.9820386132351152E-4,0.84772347511949153,-152151.84805515388,25650.450355389203,1.20812818121878E-4,0.13464229441199974,-153625.85391077239,35106.651109486695,1.3688525052928715,1.8299351613946743E-2,12.828153740352095,192606.36525988852,-9999]
["AKM","AKM21C",0.48,1.58,0.39,1.3,8000,1.47,8000,13,19,19.5,1.1000000000000001E-2,640,6,8000,8000,8000,0.39,10227.272727272726,20.658313908304152,19.791168546394559,"NA",-22.509898473086416,9,29.093017763200002,9,-2350.4303840000002,7.5,2362.4303840000002,9,1.3592984845409297,1.995094100080556,32.623163628982311,95.764516803866684,71.730724132179432,23.024249837650856,2.4072169175176992,147.46432524349166,1.0059045097641352E-3,2.12457357423891,-150696.33867695314,11229.184450936471,4.0732639947914942E-4,0.44197727725695352,-153535.56876159666,18879.857825603656,1.0066102564102564,0.13787263356000873,31.495159070472681,498502.36743877549,-9999]
["AKM","AKM21E",0.5,3.11,0.41,2.5625,7000,1.49,8000,3.42,5.2,10.199999999999999,1.1000000000000001E-2,640,6,8000,8000,8000,0.39714285714285713,10227.272727272726,19.832983691213574,19.525515277315439,"NA",-22.509898473086416,9,29.093017763200002,9,-2350.4303840000002,7.5,2362.4303840000002,9,2.5685579464844293,3.7699702184813333,61.645390715626306,180.958570487104,135.54382909432587,23.024249837650856,2.4072169175176992,147.46432524349166,2.7595786227686131E-4,0.55996844974851034,-152910.52858344448,22546.76866254579,1.0472361604416847E-4,3.53109320052565E-2,-153661.00388812216,38137.13728738379,0.58441623949579791,3.6876882065862211E-2,8.1896747718904912,7501.8325387822406,-9999]
["AKM","AKM21G",0.5,4.87,0.46,4.5999999999999996,4000,1.51,8000,1.44,2.1800000000000002,6.6,1.1000000000000001E-2,640,6,8000,8000,8000,0.42000000000000004,10227.272727272726,19.830468208195683,19.266899180927155,5.823586290941854E-2,-22.509898473086416,9,29.093017763200002,9,-2350.4303840000002,7.5,2362.4303840000002,9,4.0221470094466794,5.9034581877826673,96.531528226720297,283.36599301356802,212.25030472326915,23.024249837650856,2.4072169175176992,147.46432524349166,1.1965319231905482E-4,0.24210455430495473,-153327.59839752526,34799.715036458612,4.4314436260121293E-5,2.4106898191171813E-2,-153660.6647007553,58614.180420837438,1.4644490909090857,1.5891420541782112E-2,3.4939394744222572,-83601.941626916436,2186.3495810401059]
["AKM","AKM22C",0.84,1.39,0.68,1.1147540983606559,8000,2.73,8000,19.399999999999999,35.5,39,1.6E-2,640,6,5763.9314293478628,8000,8000,0.68,7031.25,11.804952260007061,10.657158981391943,"NA",-22.51116545580247,9,29.094044019200002,9,-2350.5351040000005,7.5,2362.5351040000005,9,0.68334232714205445,1.0029940770507937,16.400215851409307,48.143715698438093,36.061011147537734,23.024452622831248,2.407392474379479,147.47507972680214,3.4247680647328856E-3,5.9200466032473704,-147903.48852981249,5763.9314293478628,1.6367350279500802E-3,1.4596560016616504,-153313.80347745121,9242.7143137434705,1.1138419052122743,0.12283013756357093,47.256860332849222,213398.92710690643,-9999]
["AKM","AKM22E",0.87,2.73,0.7,2.1875,8000,2.76,8000,5.09,9.6999999999999993,22.4,1.6E-2,640,6,8000,8000,8000,0.7,7031.25,11.39804073525578,10.541320296811596,0.1070925627823832,-22.51116545580247,9,29.094044019200002,9,-2350.5351040000005,7.5,2362.5351040000005,9,1.2958245469297607,1.9019813259678164,31.099789126314256,91.295103646455189,68.382626944127637,23.024452622831248,2.407392474379479,147.47507972680214,1.0241675324533163E-3,1.7103260263654887,-152206.52276164741,11384.348112731648,5.229136210754457E-4,0.34416487889442715,-153604.98300788004,16813.161841042562,1.7427701855468749,3.3070131105976577E-2,13.504304076284914,-62800.72443759696,1188.915001803105]
["AKM","AKM22G",0.88,4.82,0.74,4.1111111111111116,7000,2.79,8000,1.69,3.19,11.7,1.6E-2,640,6,8000,8000,8000,0.72,7031.25,11.268092821977886,10.427972766738351,3.9998407544551952E-2,-22.51116545580247,9,29.094044019200002,9,-2350.5351040000005,7.5,2362.5351040000005,9,2.2618675720509733,3.3199169548424248,54.28482172922336,159.35601383243639,119.36218274538162,23.024452622831248,2.407392474379479,147.47507972680214,3.1279553846056475E-4,0.52336148984493103,-153163.76760710659,21307.505706196975,1.397472729844393E-4,6.670184913189614E-2,-153655.87461341658,32921.320768341822,1.9476220377153717,1.0868771755853655E-2,4.0878970104875103,-123145.14915561267,3183.2255904612539]
["AKM","AKM23C",1.1299999999999999,1.41,0.99,1.2375,5500,3.77,8000,20.3,40.700000000000003,51.8,2.2000000000000002E-2,640,6,4482.2519846527784,6933.2810468905518,7567.5675675675675,0.95351648244278597,5113.6363636363631,8.7752055028079941,7.7175797152254644,"NA",-22.512685835061731,9,29.095275526400002,9,-2350.6607680000002,7.5,2362.6607680000002,9,0.51528567295858707,0.75634842352920362,12.36685615100609,36.304724329401772,27.193097452305878,23.024695974585331,2.4076031426136142,147.48798510677474,5.3966402831604329E-3,8.5677827238047595,-146824.609859505,4482.2519846527784,2.8661824958019252E-3,2.2246864581925778,-153202.87559095855,6933.2810468905518,1.2214688223938224,9.3353985259508318E-2,49.527351455353802,74880.459513697686,-9999]
["AKM","AKM23D",1.1599999999999999,2.19,0.92,1.7692307692307692,8000,3.84,8000,8.36,17.3,33.799999999999997,2.2000000000000002E-2,640,6,7355.6322364198932,8000,8000,0.92,5113.6363636363631,8.5488935589887056,7.5768946683333338,0.11993394070231927,-22.512685835061731,9,29.095275526400002,9,-2350.6607680000002,7.5,2362.6607680000002,9,0.77963894281646817,1.1443723671482759,18.711334627595235,54.929873623117246,41.143774923710787,23.024695974585331,2.4076031426136142,147.48798510677474,2.3068017093524447E-3,3.5481416950475198,-150909.08300476728,7355.6322364198932,1.2056704678633471E-3,0.8268375571638048,-153514.39469338945,10946.239697391107,1.689415950159308,3.8645049352726508E-2,20.136674066093967,-64931.628399718713,1061.6173680938184]
["AKM","AKM23E",1.1599999999999999,2.78,0.98,2.3333333333333299,6500,3.86,8000,5.44,11.1,27,2.2000000000000002E-2,640,6,8000,8000,8000,0.93846153846153846,5113.6363636363631,8.5485160402276854,7.5376361467357524,7.646670768587055E-2,-22.512685835061731,9,29.095275526400002,9,-2350.6607680000002,7.5,2362.6607680000002,9,0.98967865800446642,1.4526735984804597,23.752287792107193,69.728332727062067,52.228170907724184,23.024695974585331,2.4076031426136142,147.48798510677474,1.5094681578589752E-3,2.3534089599695966,-151764.6400093055,9277.7613684755124,7.6379201041790103E-4,0.49688921490987836,-153579.32959811599,13858.537267931832,1.9531530636277241,2.560706507806175E-2,13.287035881517815,-93120.336585479439,1665.0900545708087]
["AKM","AKM23F",1.18,4.3099999999999996,0.94,3.481481481481481,8000,3.88,8000,2.23,4.68,17.600000000000001,2.2000000000000002E-2,640,6,8000,8000,8000,0.94,5113.6363636363631,8.4039152829396127,7.498782352164949,3.9068198433671215E-2,-22.512685835061731,9,29.095275526400002,9,-2350.6607680000002,7.5,2362.6607680000002,9,1.508351852993272,2.2139943064757062,36.20044447183853,106.2717267108339,79.600037577813026,23.024695974585331,2.4076031426136142,147.48798510677474,6.3537671593085518E-4,0.96339668294950298,-152914.92558051547,14773.865409732598,3.1883476476783743E-4,0.16083089875936957,-153643.12369415374,21701.213746581634,2.3658724697495788,1.0582333574241178E-2,5.411173150120951,-130032.16013963238,3259.0178093234313]
["AKM","AKM24C",1.38,1.42,1.25,1.2886597938144331,4500,4.67,8000,20.399999999999999,43.8,62.4,2.7000000000000003E-2,640,6,3840.0447540841351,5762.6211930378486,6282.0512820512822,1.2135242766455734,4166.6666666666661,7.1853037113310751,6.2304714737473237,"NA",-22.513952817777778,9,29.096301782400001,9,-2350.765488,7.5,2362.765488,9,0.42493302164096675,0.62374318434492759,10.198392519383201,29.939672848556526,22.425404604290748,23.02489877566153,2.4077786994753927,147.49873959008517,7.1729116881755275E-3,10.595013709748901,-146456.67883037429,3840.0447540841351,4.1244357802756792E-3,2.8100999597647434,-153156.99251983495,5762.6211930378486,1.274519205803742,7.5308819874413416E-2,49.444236139607732,3300.7646124370804,-75.421317455592401]
["AKM","AKM24D",1.41,2.21,1.1000000000000001,1.7460317460317463,8000,4.76,8000,8.4,18.7,40.799999999999997,2.7000000000000003E-2,640,6,6289.9435632800632,8000,8000,1.1000000000000001,4166.6666666666661,7.0334472049565102,6.1126684416806727,9.0319153259290422E-2,-22.513952817777778,9,29.096301782400001,9,-2350.765488,7.5,2362.765488,9,0.6472683694938669,0.95010087084964556,15.534440867852807,45.604841800782985,34.158924663952611,23.02489877566153,2.4077786994753927,147.49873959008517,3.105442486655942E-3,4.4287400565669151,-150718.3573252114,6289.9435632800632,1.7441920949680955E-3,1.0406478136342563,-153501.36004901634,9087.6361214200861,1.7530879298941802,3.1867815264505384E-2,20.277026418056092,-91915.243458263532,1409.7115603817892]
["AKM","AKM24E",1.4,2.79,1.24,2.48,5500,4.79,8000,5.44,11.8,32.4,2.7000000000000003E-2,640,6,{"$f":"IF(AQ33<I33,IF(AQ33<0,0,AQ33),I33)","v":8000},{"$f":"IF(AU33<I33,IF(AU33<0,0,AU33),I33)","v":8000},{"$f":"IF(UAC_V*0.98/L33*1000<I33,IF(UAC_V*0.98/L33*1000<0,0,UAC_V*0.98/L33*1000),I33)","v":8000},{"$f":"C33+(E33-C33)/G33*Q33","v":1.1672727272727272},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M33,(inertia/gear^2+gear_inertia)/M33),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M33,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M33))","v":4166.6666666666661},{"$f":"IF((C33+(E33-C33)/G33*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X33^2*time1+Y33^2*time2+Z33^2*time3+AA33^2*time4)/time)/(C33+(E33-C33)/G33*mspeed),SQRT((((X33-Y33)*2/PI()+Y33)^2*time1+Y33^2*time2+((Z33-Y33)*2/PI()+Y33)^2*time3+AA33^2*time4)/time)/(C33+(E33-C33)/G33*mspeed)),IF(AccType=1,SQRT((X33^2*time1+Y33^2*time2+Z33^2*time3+AA33^2*time4+AB33^2*time5+AC33^2*time6+AD33^2*time7+AE33^2*time8)/time)/(C33+(E33-C33)/G33*mspeed),SQRT((((X33-Y33)*2/PI()+Y33)^2*time1+Y33^2*time2+((Z33-Y33)*2/PI()+Y33)^2*time3+AA33^2*time4+((AB33-AC33)*2/PI()+AC33)^2*time5+AC33^2*time6+((AD33-AC33)*2/PI()+AC33)^2*time7+AE33^2*time8)/time)/(C33+(E33-C33)/G33*mspeed))))","v":7.0826321864430666},{"$f":"IF(move1,MAX(ABS(X33),ABS(Z33))/H33,MAX(ABS(X33),ABS(Z33),ABS(AB33),ABS(AD33))/H33)","v":6.0743845057202508},{"$f":"IF(AZ33>0,speed/(MIN(AZ33,I33)),\"NA\")","v":6.2581686230597622E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M33+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M33+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.513952817777778},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M33+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M33+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.096301782400001},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M33+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M33+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2350.765488},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M33+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M33+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2362.765488},9,{"$f":"AH33/Irms","v":0.82297641847185632},{"$f":"AI33/Ipeak","v":1.2080161007871431},{"$f":"IF(move1,IF(AccType=1,SQRT((X33^2*time1+Y33^2*time2+Z33^2*time3+AA33^2*time4)/time)/(C33/D33),SQRT((((X33-Y33)*2/PI()+Y33)^2*time1+Y33^2*time2+((Z33-AA33)*2/PI()+AA33)^2*time3+AA33^2*time4)/time)/(C33/D33)),IF(AccType=1,SQRT((X33^2*time1+Y33^2*time2+Z33^2*time3+AA33^2*time4+AB33^2*time5+AC33^2*time6+AD33^2*time7+AE33^2*time8)/time)/(C33/D33),SQRT((((X33-Y33)*2/PI()+Y33)^2*time1+Y33^2*time2+((Z33-AA33)*2/PI()+AA33)^2*time3+AA33^2*time4+((AB33-AC33)*2/PI()+AC33)^2*time5+AC33^2*time6+((AD33-AE33)*2/PI()+AE33)^2*time7+AE33^2*time8)/time)/(C33/D33)))","v":19.751434043324551},{"$f":"IF(move1,MAX(ABS(X33),ABS(Z33))/(C33/D33),MAX(ABS(X33),ABS(Z33),ABS(AB33),ABS(AD33))/(C33/D33))","v":57.984772837782863},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X33),ABS(Z33))/(C33/D33),MAX(ABS((X33-Y33)*2/PI()+Y33),ABS((Z33-Y33)*2/PI()+Y33))/(C33/D33)),IF(AccType=1,MAX(ABS(X33),ABS(Z33),ABS(AB33),ABS(AD33))/(C33/D33),MAX(ABS((X33-Y33)*2/PI()+Y33),ABS((Z33-Y33)*2/PI()+Y33),ABS((AB33-AC33)*2/PI()+AC33),ABS((AD33-AC33)*2/PI()+AC33))/(C33/D33)))","v":43.431736824668128},{"$f":"IF((C33+(E33-C33)/G33*mspeed)<0,\"NA\",U33*(C33+(E33-C33)/G33*mspeed)*mspeed/9.55)","v":23.02489877566153},{"$f":"IF(move1,IF(speed1>speed2,AM33/2*time1/time,AM33/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z33*-speed/30*PI(),((Z33-AA33)*2/PI()+AA33)*-speed/30*PI()),IF(AccType=1,X33*-speed/30*PI(),((X33-Y33)*2/PI()+Y33)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z33*-speed/30*PI(),((Z33-AA33)*2/PI()+AA33)*-speed/30*PI()),IF(AccType=1,X33*-speed/30*PI(),((X33-Y33)*2/PI()+Y33)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD33*-speed/30*PI(),((AD33-AE33)*2/PI()+AE33)*-speed/30*PI()),IF(AccType=1,AB33*-speed/30*PI(),((AB33-AC33)*2/PI()+AC33)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD33*-speed/30*PI(),((AD33-AE33)*2/PI()+AE33)*-speed/30*PI()),IF(AccType=1,AB33*-speed/30*PI(),((AB33-AC33)*2/PI()+AC33)*-speed/30*PI()),0)/2*time7/time)))","v":2.4077786994753927},{"$f":"IF(move1,MAX(IF(AccType=1,Z33*-speed/30*PI(),((Z33-AA33)*2/PI()+AA33)*-speed/30*PI()),IF(AccType=1,X33*-speed/30*PI(),((X33-Y33)*2/PI()+Y33)*-speed/30*PI()),0),MAX(IF(AccType=1,Z33*-speed/30*PI(),((Z33-AA33)*2/PI()+AA33)*-speed/30*PI()),IF(AccType=1,X33*-speed/30*PI(),((X33-Y33)*2/PI()+Y33)*-speed/30*PI()),IF(AccType=1,AD33*-speed/30*PI(),((AD33-AE33)*2/PI()+AE33)*-speed/30*PI()),IF(AccType=1,AB33*-speed/30*PI(),((AB33-AC33)*2/PI()+AC33)*-speed/30*PI()),0))","v":147.49873959008517},{"$f":"(L33^2)/1000000+((K33/1000)^2*(D33/C33*H33)^2*PI()*PI()*(O33/2)^2)/1200","v":1.9889390263936883E-3},{"$f":"SQRT(3)*L33*J33*D33/C33*H33/1000","v":2.9141789597131709},{"$f":"0.75*J33^2*(D33/C33*H33)^2-(UAC_V*0.98)^2","v":-151641.52843287156},{"$f":"-AO33/2/AN33+SQRT((AO33/2/AN33)^2-AP33/AN33)","v":8029.7731506618638},{"$f":"(L33^2)/1000000+((K33/1000)^2*AV33^2*PI()*PI()*(O33/2)^2)/1200","v":1.1007821656355246E-3},{"$f":"SQRT(3)*L33*J33*AV33/1000","v":0.6792372104521891},{"$f":"0.75*J33^2*AV33^2-(UAC_V*0.98)^2","v":-153554.12650794876},{"$f":"-AS33/2/AR33+SQRT((AS33/2/AR33)^2-AT33/AR33)","v":11506.32425739811},{"$f":"D33+(F33-D33)*((0.85*UAC_V-D33*J33)/L33*1000)/G33","v":2.2249329741863075},{"$f":"(L33^2)/1000000+((K33/1000)^2*AJ33^2*PI()*PI()*(O33/2)^2)/1200","v":2.0491691895393949E-2},{"$f":"SQRT(3)*L33*J33*AJ33/1000","v":13.259029421625595},{"$f":"0.75*J33^2*AJ33^2-(UAC_V*0.98)^2","v":-111796.84436358472},{"$f":"IF(((AX33/2/AW33)^2-AY33/AW33)>0,-AX33/2/AW33+SQRT((AX33/2/AW33)^2-AY33/AW33),-9999)","v":2034.5241897822925}]
["AKM","AKM24F",1.42,3.89,1.1200000000000001,3.1111111111111116,8000,4.82,8000,2.77,6.16,23.4,2.7000000000000003E-2,640,6,{"$f":"IF(AQ34<I34,IF(AQ34<0,0,AQ34),I34)","v":8000},{"$f":"IF(AU34<I34,IF(AU34<0,0,AU34),I34)","v":8000},{"$f":"IF(UAC_V*0.98/L34*1000<I34,IF(UAC_V*0.98/L34*1000<0,0,UAC_V*0.98/L34*1000),I34)","v":8000},{"$f":"C34+(E34-C34)/G34*Q34","v":1.1200000000000001},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M34,(inertia/gear^2+gear_inertia)/M34),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M34,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M34))","v":4166.6666666666661},{"$f":"IF((C34+(E34-C34)/G34*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X34^2*time1+Y34^2*time2+Z34^2*time3+AA34^2*time4)/time)/(C34+(E34-C34)/G34*mspeed),SQRT((((X34-Y34)*2/PI()+Y34)^2*time1+Y34^2*time2+((Z34-Y34)*2/PI()+Y34)^2*time3+AA34^2*time4)/time)/(C34+(E34-C34)/G34*mspeed)),IF(AccType=1,SQRT((X34^2*time1+Y34^2*time2+Z34^2*time3+AA34^2*time4+AB34^2*time5+AC34^2*time6+AD34^2*time7+AE34^2*time8)/time)/(C34+(E34-C34)/G34*mspeed),SQRT((((X34-Y34)*2/PI()+Y34)^2*time1+Y34^2*time2+((Z34-Y34)*2/PI()+Y34)^2*time3+AA34^2*time4+((AB34-AC34)*2/PI()+AC34)^2*time5+AC34^2*time6+((AD34-AC34)*2/PI()+AC34)^2*time7+AE34^2*time8)/time)/(C34+(E34-C34)/G34*mspeed))))","v":6.9837494061907286},{"$f":"IF(move1,MAX(ABS(X34),ABS(Z34))/H34,MAX(ABS(X34),ABS(Z34),ABS(AB34),ABS(AD34))/H34)","v":6.0365771332780085},{"$f":"IF(AZ34>0,speed/(MIN(AZ34,I34)),\"NA\")","v":3.9202799027761838E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M34+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M34+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.513952817777778},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M34+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M34+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.096301782400001},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M34+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M34+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2350.765488},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M34+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M34+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2362.765488},9,{"$f":"AH34/Irms","v":1.1312861767372733},{"$f":"AI34/Ipeak","v":1.6605723875225353},{"$f":"IF(move1,IF(AccType=1,SQRT((X34^2*time1+Y34^2*time2+Z34^2*time3+AA34^2*time4)/time)/(C34/D34),SQRT((((X34-Y34)*2/PI()+Y34)^2*time1+Y34^2*time2+((Z34-AA34)*2/PI()+AA34)^2*time3+AA34^2*time4)/time)/(C34/D34)),IF(AccType=1,SQRT((X34^2*time1+Y34^2*time2+Z34^2*time3+AA34^2*time4+AB34^2*time5+AC34^2*time6+AD34^2*time7+AE34^2*time8)/time)/(C34/D34),SQRT((((X34-Y34)*2/PI()+Y34)^2*time1+Y34^2*time2+((Z34-AA34)*2/PI()+AA34)^2*time3+AA34^2*time4+((AB34-AC34)*2/PI()+AC34)^2*time5+AC34^2*time6+((AD34-AE34)*2/PI()+AE34)^2*time7+AE34^2*time8)/time)/(C34/D34)))","v":27.15086824169456},{"$f":"IF(move1,MAX(ABS(X34),ABS(Z34))/(C34/D34),MAX(ABS(X34),ABS(Z34),ABS(AB34),ABS(AD34))/(C34/D34))","v":79.707474601081699},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X34),ABS(Z34))/(C34/D34),MAX(ABS((X34-Y34)*2/PI()+Y34),ABS((Z34-Y34)*2/PI()+Y34))/(C34/D34)),IF(AccType=1,MAX(ABS(X34),ABS(Z34),ABS(AB34),ABS(AD34))/(C34/D34),MAX(ABS((X34-Y34)*2/PI()+Y34),ABS((Z34-Y34)*2/PI()+Y34),ABS((AB34-AC34)*2/PI()+AC34),ABS((AD34-AC34)*2/PI()+AC34))/(C34/D34)))","v":59.70246825865582},{"$f":"IF((C34+(E34-C34)/G34*mspeed)<0,\"NA\",U34*(C34+(E34-C34)/G34*mspeed)*mspeed/9.55)","v":23.02489877566153},{"$f":"IF(move1,IF(speed1>speed2,AM34/2*time1/time,AM34/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z34*-speed/30*PI(),((Z34-AA34)*2/PI()+AA34)*-speed/30*PI()),IF(AccType=1,X34*-speed/30*PI(),((X34-Y34)*2/PI()+Y34)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z34*-speed/30*PI(),((Z34-AA34)*2/PI()+AA34)*-speed/30*PI()),IF(AccType=1,X34*-speed/30*PI(),((X34-Y34)*2/PI()+Y34)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD34*-speed/30*PI(),((AD34-AE34)*2/PI()+AE34)*-speed/30*PI()),IF(AccType=1,AB34*-speed/30*PI(),((AB34-AC34)*2/PI()+AC34)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD34*-speed/30*PI(),((AD34-AE34)*2/PI()+AE34)*-speed/30*PI()),IF(AccType=1,AB34*-speed/30*PI(),((AB34-AC34)*2/PI()+AC34)*-speed/30*PI()),0)/2*time7/time)))","v":2.4077786994753927},{"$f":"IF(move1,MAX(IF(AccType=1,Z34*-speed/30*PI(),((Z34-AA34)*2/PI()+AA34)*-speed/30*PI()),IF(AccType=1,X34*-speed/30*PI(),((X34-Y34)*2/PI()+Y34)*-speed/30*PI()),0),MAX(IF(AccType=1,Z34*-speed/30*PI(),((Z34-AA34)*2/PI()+AA34)*-speed/30*PI()),IF(AccType=1,X34*-speed/30*PI(),((X34-Y34)*2/PI()+Y34)*-speed/30*PI()),IF(AccType=1,AD34*-speed/30*PI(),((AD34-AE34)*2/PI()+AE34)*-speed/30*PI()),IF(AccType=1,AB34*-speed/30*PI(),((AB34-AC34)*2/PI()+AC34)*-speed/30*PI()),0))","v":147.49873959008517},{"$f":"(L34^2)/1000000+((K34/1000)^2*(D34/C34*H34)^2*PI()*PI()*(O34/2)^2)/1200","v":1.0372700574643808E-3},{"$f":"SQRT(3)*L34*J34*D34/C34*H34/1000","v":1.4823970737534444},{"$f":"0.75*J34^2*(D34/C34*H34)^2-(UAC_V*0.98)^2","v":-152660.68479971474},{"$f":"-AO34/2/AN34+SQRT((AO34/2/AN34)^2-AP34/AN34)","v":11438.048463151006},{"$f":"(L34^2)/1000000+((K34/1000)^2*AV34^2*PI()*PI()*(O34/2)^2)/1200","v":5.6539968193243311E-4},{"$f":"SQRT(3)*L34*J34*AV34/1000","v":0.28293624844927967},{"$f":"0.75*J34^2*AV34^2-(UAC_V*0.98)^2","v":-153627.45016039952},{"$f":"-AS34/2/AR34+SQRT((AS34/2/AR34)^2-AT34/AR34)","v":16235.463035809296},{"$f":"D34+(F34-D34)*((0.85*UAC_V-D34*J34)/L34*1000)/G34","v":2.5201845043922133},{"$f":"(L34^2)/1000000+((K34/1000)^2*AJ34^2*PI()*PI()*(O34/2)^2)/1200","v":1.0559241058984715E-2},{"$f":"SQRT(3)*L34*J34*AJ34/1000","v":6.7026808405601539},{"$f":"0.75*J34^2*AJ34^2-(UAC_V*0.98)^2","v":-133152.124383441},{"$f":"IF(((AX34/2/AW34)^2-AY34/AW34)>0,-AX34/2/AW34+SQRT((AX34/2/AW34)^2-AY34/AW34),-9999)","v":3247.8281559270958}]
["AKM","AKM31C",1.1499999999999999,1.37,1,1.1764705882352942,5000,3.88,8000,21.4,37.5,54.5,3.3000000000000002E-2,640,8,3971.9845456902299,6551.876140705368,7192.660550458716,0.95344371577883902,3409.090909090909,8.6234419146696624,7.4993642498969075,"NA",-22.515473197037039,9,29.097533289600001,9,-2350.8911520000001,7.5,2362.8911520000001,9,0.4919699095785306,0.7221670399773914,11.807277829884734,34.664017918914787,25.963867202718095,23.025142146490033,2.4079893677095279,147.51164497005774,6.9240065303963795E-3,9.3373869206654927,-146325.66193870761,3971.9845456902299,3.214710360203368E-3,2.3217989899621063,-153210.27131135517,6551.876140705368,1.1493537441985968,0.12772002638314425,52.449370745134893,77876.820769346989,-9999]
["AKM","AKM31E",1.2,2.99,0.95,2.3170731707317072,6000,4,8000,4.58,8.6,26.1,3.3000000000000002E-2,640,8,8000,8000,8000,0.8666666666666667,3409.090909090909,8.2657163130753482,7.2743833224000003,7.3643675902406266E-2,-22.515473197037039,9,29.097533289600001,9,-2350.8911520000001,7.5,2362.8911520000001,9,1.0289772105144632,1.5104448704150002,24.695453052347116,72.501353779920009,54.304596944371148,23.025142146490033,2.4079893677095279,147.51164497005774,1.648006905577037E-3,2.0635573647038465,-152101.24071966668,9001.2816057330656,7.0574821812461144E-4,0.32875353531426443,-153624.33569421264,14522.768474199773,1.5878293271656851,2.9382972986037002E-2,11.243543574765658,-107269.61643338541,1728.9190539897538]
["AKM","AKM31H",1.23,5.85,0.97,4.6190476190476195,6000,4.0599999999999996,8000,1.25,2.4,13.7,3.3000000000000002E-2,640,8,8000,8000,8000,0.8833333333333333,3409.090909090909,8.0642044569725186,7.1668801205911343,3.2361699151094575E-2,-22.515473197037039,9,29.097533289600001,9,-2350.8911520000001,7.5,2362.8911520000001,9,1.9641134453086251,2.8831397314390244,47.138722687407004,138.39070710907316,103.65670678671056,23.025142146490033,2.4079893677095279,147.51164497005774,4.7031758128761428E-4,0.57275382175689737,-153227.04685873364,17451.154584906395,1.882610514162313E-4,2.5745322196281673E-2,-153663.11713248576,28501.332769555269,0.86797481462171522,8.3320278188734678E-3,3.0745999412349709,-141072.53961500069,3934.4026368655545]
["AKM","AKM32C",2,1.44,1.86,1.3285714285714287,3000,6.92,8000,23,46.5,89.8,5.9000000000000004E-2,640,8,2549.9677961600942,3963.1480481514882,4365.2561247216036,1.8150530910862641,1906.7796610169489,4.9584031437502301,4.2056170261271681,0.22739684467508217,-22.52206150716049,9,29.102869820800002,9,-2351.435696,7.5,2363.435696,9,0.29735017877218817,0.43654304731200005,7.136404290532516,20.954066270976003,15.694476774662029,23.026196873630557,2.4089022633907784,147.56756828327212,1.5127566349111322E-2,17.823926841575823,-143814.95510272001,2549.9677961600942,8.5546309272593515E-3,4.6973439603771325,-152979.94336455141,3963.1480481514882,1.3130690423162585,7.8151136875418539E-2,56.145071822492561,-55937.888461836483,559.91961830184641]
["AKM","AKM32D",2.04,2.23,1.65,1.793478260869565,5500,7.1,8000,9.57,20.100000000000001,59,5.9000000000000004E-2,640,8,4196.0645561115662,6243.9988305710021,6644.0677966101694,1.5972437192867834,1906.7796610169489,4.8624128009550569,4.0989957494084512,8.3132797597950614E-2,-22.52206150716049,9,29.102869820800002,9,-2351.435696,7.5,2363.435696,9,0.45145077523282923,0.66277981720163404,10.834818605587902,31.813431225678436,23.828079525800874,23.026196873630557,2.4089022633907784,147.56756828327212,6.6835556530417985E-3,7.5902769260358234,-149526.37404381559,4196.0645561115662,3.6535122545970329E-3,1.7616484818987503,-153441.11825813155,6243.9988305710021,1.80133578669525,3.3667216225579825E-2,23.303095643372917,-114664.12449266118,1531.573075277513]
["AKM","AKM32E",2.04,2.82,1.41,1.9315068493150684,7000,7.11,8000,6.3,12.8,47.1,5.9000000000000004E-2,640,8,5362.7875926700754,7954.7126438027281,8000,1.3240758620577544,1906.7796610169489,4.8634233379023435,4.09323063583685,6.1176682226196488E-2,-22.52206150716049,9,29.102869820800002,9,-2351.435696,7.5,2363.435696,9,0.57089290859039388,0.83813411861372555,13.701429806169454,40.230437693458825,30.132369624555363,23.026196873630557,2.4089022633907784,147.56756828327212,4.3011521417505635E-3,5.0513868062215588,-150788.45978582979,5362.7875926700754,2.3005305576245978E-3,1.0030413064270525,-153550.62016236866,7954.7126438027281,1.9516266244531142,2.1794456754519565E-2,15.486574642537594,-126636.30965433706,2081.2497481106425]
["AKM","AKM32H",2.1,5.5,1.45,3.7179487179487176,7000,7.26,8000,1.64,3.55,24.8,5.9000000000000004E-2,640,8,8000,8000,8000,1.3571428571428572,1906.7796610169489,4.724478881578662,4.0086597549311298,2.7558205413893894E-2,-22.52206150716049,9,29.102869820800002,9,-2351.435696,7.5,2363.435696,9,1.0816309413009491,1.5879542064920635,25.959142591222776,76.221801911619053,57.089697262328805,23.026196873630557,2.4089022633907784,147.56756828327212,1.2146311569246914E-3,1.3394798094697493,-152934.69533689797,10683.126162716704,6.2237037086327674E-4,0.1481056190856895,-153655.08380170201,15594.100040237134,2.1024001536098305,6.0202263100982483E-3,4.0217391260812105,-147089.47411621502,4620.1830838129954]
["AKM","AKM33C",2.71,1.47,2.54,1.3655913978494623,2000,9.76,8000,25.4,53.6,120,8.5000000000000006E-2,640,8,1873.5063782065949,2957.7518101405485,3266.6666666666665,2.4585910961380533,1323.5294117647059,3.6601583308087662,2.9823981918032789,0.16794711874012208,-22.528649817283949,9,29.108206352,9,-2351.9802399999999,7.5,2363.9802399999999,9,0.22402869430002928,0.32894421384870848,5.3766886632007029,15.789322264738006,11.825787517815487,23.027251796103748,2.4098151590720303,147.62349159648659,2.4996532743950292E-2,27.949461936413833,-140101.97877543324,1873.5063782065949,1.5077166172281713E-2,7.0654395782230379,-152797.32575636249,2957.7518101405485,1.3383311818996415,6.727230014931905E-2,62.431771972488555,-85995.143200958191,758.11931415468189]
["AKM","AKM33E",2.79,2.58,2.34,2.127272727272727,4500,9.9600000000000009,8000,8.36,18.5,70.599999999999994,8.5000000000000006E-2,640,8,3616.5730124494039,5232.7096112060781,5552.4079320113315,2.2667290388793919,1323.5294117647059,3.5555609605773557,2.9225106779116463,6.4233802498316672E-2,-22.528649817283949,9,29.108206352,9,-2351.9802399999999,7.5,2363.9802399999999,9,0.38191886104575251,0.5607763768530466,9.1660526650980607,26.917266088946239,20.160325059630441,23.027251796103748,2.4098151590720303,147.62349159648659,8.8049604370576146E-3,9.4155663249074024,-149217.4467204049,3616.5730124494039,5.1879717004030892E-3,2.173611893893757,-153427.02932245683,5232.7096112060781,2.1262307562880931,2.3289666261728195E-2,20.609579748003426,-132359.62103312596,1982.1955033232377]
["AKM","AKM33H",2.88,5.62,2.27,4.365384615384615,5500,10.220000000000001,8000,1.82,4.0999999999999996,33.4,8.5000000000000006E-2,640,8,{"$f":"IF(AQ44<I44,IF(AQ44<0,0,AQ44),I44)","v":8000},{"$f":"IF(AU44<I44,IF(AU44<0,0,AU44),I44)","v":8000},{"$f":"IF(UAC_V*0.98/L44*1000<I44,IF(UAC_V*0.98/L44*1000<0,0,UAC_V*0.98/L44*1000),I44)","v":8000},{"$f":"C44+(E44-C44)/G44*Q44","v":1.9927272727272727},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M44,(inertia/gear^2+gear_inertia)/M44),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M44,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M44))","v":1323.5294117647059},{"$f":"IF((C44+(E44-C44)/G44*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X44^2*time1+Y44^2*time2+Z44^2*time3+AA44^2*time4)/time)/(C44+(E44-C44)/G44*mspeed),SQRT((((X44-Y44)*2/PI()+Y44)^2*time1+Y44^2*time2+((Z44-Y44)*2/PI()+Y44)^2*time3+AA44^2*time4)/time)/(C44+(E44-C44)/G44*mspeed)),IF(AccType=1,SQRT((X44^2*time1+Y44^2*time2+Z44^2*time3+AA44^2*time4+AB44^2*time5+AC44^2*time6+AD44^2*time7+AE44^2*time8)/time)/(C44+(E44-C44)/G44*mspeed),SQRT((((X44-Y44)*2/PI()+Y44)^2*time1+Y44^2*time2+((Z44-Y44)*2/PI()+Y44)^2*time3+AA44^2*time4+((AB44-AC44)*2/PI()+AC44)^2*time5+AC44^2*time6+((AD44-AC44)*2/PI()+AC44)^2*time7+AE44^2*time8)/time)/(C44+(E44-C44)/G44*mspeed))))","v":3.4446537246952871},{"$f":"IF(move1,MAX(ABS(X44),ABS(Z44))/H44,MAX(ABS(X44),ABS(Z44),ABS(AB44),ABS(AD44))/H44)","v":2.8481610911937376},{"$f":"IF(AZ44>0,speed/(MIN(AZ44,I44)),\"NA\")","v":2.5576114969695425E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M44+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M44+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.528649817283949},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M44+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M44+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.108206352},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M44+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M44+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2351.9802399999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M44+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M44+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2363.9802399999999},9,{"$f":"AH44/Irms","v":0.80593391438215845},{"$f":"AI44/Ipeak","v":1.1833631343912037},{"$f":"IF(move1,IF(AccType=1,SQRT((X44^2*time1+Y44^2*time2+Z44^2*time3+AA44^2*time4)/time)/(C44/D44),SQRT((((X44-Y44)*2/PI()+Y44)^2*time1+Y44^2*time2+((Z44-AA44)*2/PI()+AA44)^2*time3+AA44^2*time4)/time)/(C44/D44)),IF(AccType=1,SQRT((X44^2*time1+Y44^2*time2+Z44^2*time3+AA44^2*time4+AB44^2*time5+AC44^2*time6+AD44^2*time7+AE44^2*time8)/time)/(C44/D44),SQRT((((X44-Y44)*2/PI()+Y44)^2*time1+Y44^2*time2+((Z44-AA44)*2/PI()+AA44)^2*time3+AA44^2*time4+((AB44-AC44)*2/PI()+AC44)^2*time5+AC44^2*time6+((AD44-AE44)*2/PI()+AE44)^2*time7+AE44^2*time8)/time)/(C44/D44)))","v":19.342413945171803},{"$f":"IF(move1,MAX(ABS(X44),ABS(Z44))/(C44/D44),MAX(ABS(X44),ABS(Z44),ABS(AB44),ABS(AD44))/(C44/D44))","v":56.801430450777772},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X44),ABS(Z44))/(C44/D44),MAX(ABS((X44-Y44)*2/PI()+Y44),ABS((Z44-Y44)*2/PI()+Y44))/(C44/D44)),IF(AccType=1,MAX(ABS(X44),ABS(Z44),ABS(AB44),ABS(AD44))/(C44/D44),MAX(ABS((X44-Y44)*2/PI()+Y44),ABS((Z44-Y44)*2/PI()+Y44),ABS((AB44-AC44)*2/PI()+AC44),ABS((AD44-AC44)*2/PI()+AC44))/(C44/D44)))","v":42.5427789715215},{"$f":"IF((C44+(E44-C44)/G44*mspeed)<0,\"NA\",U44*(C44+(E44-C44)/G44*mspeed)*mspeed/9.55)","v":23.027251796103748},{"$f":"IF(move1,IF(speed1>speed2,AM44/2*time1/time,AM44/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z44*-speed/30*PI(),((Z44-AA44)*2/PI()+AA44)*-speed/30*PI()),IF(AccType=1,X44*-speed/30*PI(),((X44-Y44)*2/PI()+Y44)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z44*-speed/30*PI(),((Z44-AA44)*2/PI()+AA44)*-speed/30*PI()),IF(AccType=1,X44*-speed/30*PI(),((X44-Y44)*2/PI()+Y44)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD44*-speed/30*PI(),((AD44-AE44)*2/PI()+AE44)*-speed/30*PI()),IF(AccType=1,AB44*-speed/30*PI(),((AB44-AC44)*2/PI()+AC44)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD44*-speed/30*PI(),((AD44-AE44)*2/PI()+AE44)*-speed/30*PI()),IF(AccType=1,AB44*-speed/30*PI(),((AB44-AC44)*2/PI()+AC44)*-speed/30*PI()),0)/2*time7/time)))","v":2.4098151590720303},{"$f":"IF(move1,MAX(IF(AccType=1,Z44*-speed/30*PI(),((Z44-AA44)*2/PI()+AA44)*-speed/30*PI()),IF(AccType=1,X44*-speed/30*PI(),((X44-Y44)*2/PI()+Y44)*-speed/30*PI()),0),MAX(IF(AccType=1,Z44*-speed/30*PI(),((Z44-AA44)*2/PI()+AA44)*-speed/30*PI()),IF(AccType=1,X44*-speed/30*PI(),((X44-Y44)*2/PI()+Y44)*-speed/30*PI()),IF(AccType=1,AD44*-speed/30*PI(),((AD44-AE44)*2/PI()+AE44)*-speed/30*PI()),IF(AccType=1,AB44*-speed/30*PI(),((AB44-AC44)*2/PI()+AC44)*-speed/30*PI()),0))","v":147.62349159648659},{"$f":"(L44^2)/1000000+((K44/1000)^2*(D44/C44*H44)^2*PI()*PI()*(O44/2)^2)/1200","v":1.9953836719841093E-3},{"$f":"SQRT(3)*L44*J44*D44/C44*H44/1000","v":2.0997771519020754},{"$f":"0.75*J44^2*(D44/C44*H44)^2-(UAC_V*0.98)^2","v":-152675.91686515068},{"$f":"-AO44/2/AN44+SQRT((AO44/2/AN44)^2-AP44/AN44)","v":8236.9120390292301},{"$f":"(L44^2)/1000000+((K44/1000)^2*AV44^2*PI()*PI()*(O44/2)^2)/1200","v":1.1406492925389608E-3},{"$f":"SQRT(3)*L44*J44*AV44/1000","v":0.35458437329888393},{"$f":"0.75*J44^2*AV44^2-(UAC_V*0.98)^2","v":-153635.82355099954},{"$f":"-AS44/2/AR44+SQRT((AS44/2/AR44)^2-AT44/AR44)","v":11451.278797234872},{"$f":"D44+(F44-D44)*((0.85*UAC_V-D44*J44)/L44*1000)/G44","v":3.367759810728193},{"$f":"(L44^2)/1000000+((K44/1000)^2*AJ44^2*PI()*PI()*(O44/2)^2)/1200","v":5.1192266111645792E-3},{"$f":"SQRT(3)*L44*J44*AJ44/1000","v":4.4792400491138764},{"$f":"0.75*J44^2*AJ44^2-(UAC_V*0.98)^2","v":-149167.69513571981},{"$f":"IF(((AX44/2/AW44)^2-AY44/AW44)>0,-AX44/2/AW44+SQRT((AX44/2/AW44)^2-AY44/AW44),-9999)","v":4978.2367112589072}]
["AKM","AKM41C",1.95,1.46,1.77,1.3208955223880596,3000,6.12,6000,21.7,66.099999999999994,86.3,8.1000000000000003E-2,640,10,2092.0798004298103,3907.1125587968236,4542.2943221320975,1.7155732464721907,1388.8888888888889,5.0865784087832777,4.7561087168627454,0.32184655974625809,-22.52763623111111,9,29.107385347200001,9,-2351.8964640000004,7.5,2363.8964640000004,9,0.30922228644673383,0.45402545520205129,7.4213348747216115,21.793221849698462,16.322619620849686,23.027089487625755,2.4096747135826071,147.61488800983821,2.6310255467470008E-2,14.862806492279299,-146248.84789152947,2092.0798004298103,8.9527737260189123E-3,4.1983706120499891,-153072.32943516294,3907.1125587968236,1.2943437067270829,0.24680194208135339,52.944520200997374,-59570.320640567079,395.60452214837318]
["AKM","AKM41E",2.02,2.85,1.58,2.2253521126760565,6000,6.28,6000,5.7,18.399999999999999,45.6,8.1000000000000003E-2,640,10,4228.3059995376043,6000,6000,1.58,1388.8888888888889,4.9109142440019413,4.6349339724840766,9.8826916207097631E-2,-22.52763623111111,9,29.107385347200001,9,-2351.8964640000004,7.5,2363.8964640000004,9,0.5827013620397814,0.85556980445049513,13.984832688954754,41.067350613623766,30.758496725509335,23.027089487625755,2.4096747135826071,147.61488800983821,7.5444890635392101E-3,3.9889028576125303,-151750.98998640574,4228.3059995376043,2.3895349628031692E-3,0.95029100418980694,-153555.42656963633,7819.9570241554629,2.1108447486821516,6.7939760351796052E-2,13.847310541858565,-130610.27081858512,1288.3530050325703]
["AKM","AKM41H",2.06,5.6,1.62,4.378378378378379,6000,6.36,6000,1.51,5,23.7,8.1000000000000003E-2,640,10,6000,6000,6000,1.62,1388.8888888888889,4.8154813136817607,4.5766329162264148,4.6820686894613987E-2,-22.52763623111111,9,29.107385347200001,9,-2351.8964640000004,7.5,2363.8964640000004,9,1.1227248862875159,1.6484765164271844,26.945397270900383,79.126872788504855,59.264199447958028,23.027089487625755,2.4096747135826071,147.61488800983821,2.0982671168294923E-3,1.0716768342488578,-153152.82335582544,8291.8710017186168,6.0061387704575574E-4,0.17056688113605942,-153651.05110428328,15853.115065100565,2.7517488121032443,1.8616102514550845E-2,3.6734856097338828,-147657.79705668523,2719.3952698750982]
["AKM","AKM42C",3.35,1.4,3.1,1.2916666666666667,1500,11.3,6000,27.52,97.4,154,0.15,640,10,1213.2377717553047,2221.1133216094113,2545.4545454545455,2.9798144463984317,750,2.9624526787672174,2.5771281132743362,0.21287120469470461,-22.545120592592593,9,29.121547680000003,9,-2353.3416000000002,7.5,2365.3416000000002,9,0.17261899563494731,0.25354581313432834,4.1428558952387355,12.17019903044776,9.1145328791686708,23.029889956690972,2.4120973982751583,147.76329987952266,6.7217052626439441E-2,34.66501958360795,-140996.77552357141,1213.2377717553047,2.6806036628906096E-2,9.2389662501458183,-152764.20136857676,2221.1133216094113,1.2586170274170276,0.18576458890421005,66.905865582717993,-106476.5015878233,598.12671542927376]
["AKM","AKM42E",3.42,2.74,2.81,2.2301587301587302,3500,11.3,6000,7.22,26.8,80.900000000000006,0.15,640,10,2605.4527999933289,4456.7540905431406,4845.4882571075404,2.64325142993391,750,2.9018956372137579,2.5771281132743362,8.5201507422024356E-2,-22.545120592592593,9,29.121547680000003,9,-2353.3416000000002,7.5,2365.3416000000002,9,0.33092517981060604,0.48606871736842111,7.9422043154545454,23.331298433684214,17.473328591873276,23.029889956690972,2.4120973982751583,147.76329987952266,1.8648948839048756E-2,9.1590250493864254,-150459.63883996295,2605.4527999933289,7.2360166525569326E-3,2.1887000770134901,-153481.01500780319,4456.7540905431406,2.1634153492035466,5.1634721630697905E-2,17.677546592610796,-141727.22668137326,1494.3861713954063]
["AKM","AKM42G",3.53,4.8,2.35,3.1756756756756759,6000,11.5,6000,2.38,9.1999999999999993,47.5,0.15,640,10,4611.8813339809085,6000,6000,2.35,750,2.8117650806901184,2.5323084939130438,4.6112993760136507E-2,-22.545120592592593,9,29.121547680000003,9,-2353.3416000000002,7.5,2365.3416000000002,9,0.56165792185551466,0.82497302209631751,13.479790124532352,39.598705060623239,29.65635141583008,23.029889956690972,2.4120973982751583,147.76329987952266,6.5118706479420224E-3,3.061932174934991,-152625.17134139588,4611.8813339809085,2.4053832099042707E-3,0.57319355097808511,-153627.5954740296,7873.5009021902615,2.9273193361782837,1.7562528151783927E-2,5.8069610537558107,-149927.62363658319,2761.1296532992515]
["AKM","AKM42H",3.54,6,2.72,4.6101694915254239,4500,11.5,6000,1.65,6,38.299999999999997,0.15,640,10,5733.2642819071716,6000,6000,2.4466666666666672,750,2.8035583296034061,2.5323084939130438,3.7025451580734392E-2,-22.545120592592593,9,29.121547680000003,9,-2353.3416000000002,7.5,2365.3416000000002,9,0.70008914694560975,1.0283032372881358,16.802139526694635,49.358555389830514,36.965720514788202,23.029889956690972,2.4120973982751583,147.76329987952266,4.2791318458289297E-3,2.133482939016313,-152888.25174159725,5733.2642819071716,1.5493707821875148E-3,0.36537533500883196,-153641.24793007097,9840.8814152015912,3.3380733922398744,1.1581737981847249E-2,4.0461550510939226,-150873.85031299334,3438.8224596230789]
["AKM","AKM42J",3.56,8.4,2.38,5.5348837209302326,6000,11.6,6000,0.8,3.1,27.5,0.15,640,10,6000,6000,6000,2.38,750,2.7880413546225484,2.5104782482758625,2.6073705548603249E-2,-22.545120592592593,9,29.121547680000003,9,-2353.3416000000002,7.5,2365.3416000000002,9,0.9746184865905736,1.4315367539325843,23.390843678173766,68.713764188764046,51.461267098677055,23.029889956690972,2.4120973982751583,147.76329987952266,2.2365728753251215E-3,1.0429670435868681,-153304.40322181542,8049.2713869042436,7.6973957769009462E-4,9.9561524321966896E-2,-153660.72314144619,14064.414068867505,2.6128124031007758,5.9891549510935832E-3,1.9609376432091883,-152392.83423452734,4883.2320452562954]
["AKM","AKM43E",4.7,2.76,3.92,2.2790697674418605,2500,15.9,6000,8.0399999999999991,32.6,111,0.21,640,10,1964.5935369188753,3260.1948071929796,3531.5315315315315,3.6828192201557899,535.71428571428578,2.1125391671651603,1.8323184120754719,8.2386516264141604E-2,-22.560324385185183,9,29.133862752000002,9,-2354.5982399999998,7.5,2366.5982399999998,9,0.24258420616354884,0.35642491664680848,5.8220209479251723,17.108395999046806,12.812046326995976,23.032326264912953,2.414204080616507,147.89235367924826,3.1371676619625963E-2,14.432713922141241,-149437.41061686614,1964.5935369188753,1.3387516750611651E-2,3.4148893900593018,-153427.38224278996,3260.1948071929796,2.2092099285145612,4.8190944842885095E-2,19.80423883773906,-145705.88223475748,1545.4465153654457]
["AKM","AKM43G",4.8,4.87,3.01,3.0404040404040402,5000,16.100000000000001,6000,2.61,10.8,63.9,0.21,640,10,3593.2633044796335,5878.3105151918489,6000,2.6955648355613175,535.71428571428578,2.0689048915774868,1.8095566926708075,4.3990370629987764E-2,-22.560324385185183,9,29.133862752000002,9,-2354.5982399999998,7.5,2366.5982399999998,9,0.41912061404570283,0.61580690799583337,10.058894737096868,29.558731583800004,22.13578867592172,23.032326264912953,2.414204080616507,147.89235367924826,1.0482521026179489E-2,4.7186263950285383,-152300.76892347808,3593.2633044796335,4.2984541698830063E-3,0.8653955981903696,-153618.14701047906,5878.3105151918489,2.9957991208169323,1.5834783443362054E-2,6.3943586702806448,-151160.5882966959,2894.3596666748904]
["AKM","AKM43H",4.82,5.4,2.58,2.898876404494382,6000,16.100000000000001,6000,2.1,6.8,57.4,0.21,640,10,4601.4978022115465,6000,6000,2.58,535.71428571428578,2.0604517166797773,1.8095566926708075,3.3186907400500509E-2,-22.560324385185183,9,29.133862752000002,9,-2354.5982399999998,7.5,2366.5982399999998,9,0.46280497567734608,0.67999160987551877,11.107319416256306,32.639597274024901,24.442971298571614,23.032326264912953,2.414204080616507,147.89235367924826,6.3880563466889549E-3,3.7658620941282166,-152587.91878983661,4601.4978022115465,3.3810832462372806E-3,0.6290968776981728,-153633.97027996503,6648.4761081421457,3.0131844340915315,8.975230764975627E-3,5.1032378740644821,-151687.90486717649,3836.5718425331802]
["AKM","AKM43K",4.9000000000000004,9.6,2.62,5.0384615384615383,6000,16.399999999999999,6000,0.7,2.9,33.200000000000003,0.21,640,10,6000,6000,6000,2.62,535.71428571428578,2.0268160116444611,1.7764550458536588,2.1978502778268481E-2,-22.560324385185183,9,29.133862752000002,9,-2354.5982399999998,7.5,2366.5982399999998,9,0.80933151302124562,1.1891372551836734,19.423956312509894,57.078588248816324,42.744715341175571,23.032326264912953,2.414204080616507,147.89235367924826,2.8874631334773106E-3,1.293349061081283,-153284.60173061225,7065.5132735969164,1.1089382256590395E-3,7.9222653826801812E-2,-153662.57648314355,11735.795425190268,1.9681248069199899,4.2617472938551735E-3,1.7205970751918895,-152992.53682157269,5793.1131960184939]
["AKM","AKM43L",4.7300000000000004,11.2,2.5299999999999998,5.8837209302325579,6000,16,6000,0.56999999999999995,2,27.5,0.21,640,10,6000,6000,6000,2.5299999999999998,535.71428571428578,2.099659930958667,1.8208664220000002,2.1220659078919377E-2,-22.560324385185183,9,29.133862752000002,9,-2354.5982399999998,7.5,2366.5982399999998,9,0.97815612743582525,1.4371884373784356,23.475747058459806,68.985044994164909,51.661160542717482,23.032326264912953,2.414204080616507,147.89235367924826,1.9367669538243369E-3,1.0285964981878799,-153314.24437815393,8635.6010682311571,7.5641724225031931E-4,1.224283308409202E-2,-153663.9504505911,14244.876896584557,0.45093479915433399,2.9513121221533159E-3,1.4025951570850106,-153013.66176043692,6966.7126309681898]
["AKM","AKM44E",5.76,2.9,4.8,2.3529411764705883,2000,19.899999999999999,6000,8.08,33.9,132,0.27,640,10,{"$f":"IF(AQ58<I58,IF(AQ58<0,0,AQ58),I58)","v":1689.7319035376775},{"$f":"IF(AU58<I58,IF(AU58<0,0,AU58),I58)","v":2761.7099024117206},{"$f":"IF(UAC_V*0.98/L58*1000<I58,IF(UAC_V*0.98/L58*1000<0,0,UAC_V*0.98/L58*1000),I58)","v":2969.6969696969695},{"$f":"C58+(E58-C58)/G58*Q58","v":4.4343792468423739},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M58,(inertia/gear^2+gear_inertia)/M58),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M58,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M58))","v":416.66666666666663},{"$f":"IF((C58+(E58-C58)/G58*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X58^2*time1+Y58^2*time2+Z58^2*time3+AA58^2*time4)/time)/(C58+(E58-C58)/G58*mspeed),SQRT((((X58-Y58)*2/PI()+Y58)^2*time1+Y58^2*time2+((Z58-Y58)*2/PI()+Y58)^2*time3+AA58^2*time4)/time)/(C58+(E58-C58)/G58*mspeed)),IF(AccType=1,SQRT((X58^2*time1+Y58^2*time2+Z58^2*time3+AA58^2*time4+AB58^2*time5+AC58^2*time6+AD58^2*time7+AE58^2*time8)/time)/(C58+(E58-C58)/G58*mspeed),SQRT((((X58-Y58)*2/PI()+Y58)^2*time1+Y58^2*time2+((Z58-Y58)*2/PI()+Y58)^2*time3+AA58^2*time4+((AB58-AC58)*2/PI()+AC58)^2*time5+AC58^2*time6+((AD58-AC58)*2/PI()+AC58)^2*time7+AE58^2*time8)/time)/(C58+(E58-C58)/G58*mspeed))))","v":1.7246052054937293},{"$f":"IF(move1,MAX(ABS(X58),ABS(Z58))/H58,MAX(ABS(X58),ABS(Z58),ABS(AB58),ABS(AD58))/H58)","v":1.4646320514572866},{"$f":"IF(AZ58>0,speed/(MIN(AZ58,I58)),\"NA\")","v":8.0292549158861914E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M58+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M58+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.575528177777777},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M58+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M58+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.146177824000002},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M58+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M58+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2355.8548799999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M58+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M58+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2367.8548799999999},9,{"$f":"AH58/Irms","v":0.20800451799394415},{"$f":"AI58/Ipeak","v":0.30571439413194446},{"$f":"IF(move1,IF(AccType=1,SQRT((X58^2*time1+Y58^2*time2+Z58^2*time3+AA58^2*time4)/time)/(C58/D58),SQRT((((X58-Y58)*2/PI()+Y58)^2*time1+Y58^2*time2+((Z58-AA58)*2/PI()+AA58)^2*time3+AA58^2*time4)/time)/(C58/D58)),IF(AccType=1,SQRT((X58^2*time1+Y58^2*time2+Z58^2*time3+AA58^2*time4+AB58^2*time5+AC58^2*time6+AD58^2*time7+AE58^2*time8)/time)/(C58/D58),SQRT((((X58-Y58)*2/PI()+Y58)^2*time1+Y58^2*time2+((Z58-AA58)*2/PI()+AA58)^2*time3+AA58^2*time4+((AB58-AC58)*2/PI()+AC58)^2*time5+AC58^2*time6+((AD58-AE58)*2/PI()+AE58)^2*time7+AE58^2*time8)/time)/(C58/D58)))","v":4.9921084318546596},{"$f":"IF(move1,MAX(ABS(X58),ABS(Z58))/(C58/D58),MAX(ABS(X58),ABS(Z58),ABS(AB58),ABS(AD58))/(C58/D58))","v":14.674290918333334},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X58),ABS(Z58))/(C58/D58),MAX(ABS((X58-Y58)*2/PI()+Y58),ABS((Z58-Y58)*2/PI()+Y58))/(C58/D58)),IF(AccType=1,MAX(ABS(X58),ABS(Z58),ABS(AB58),ABS(AD58))/(C58/D58),MAX(ABS((X58-Y58)*2/PI()+Y58),ABS((Z58-Y58)*2/PI()+Y58),ABS((AB58-AC58)*2/PI()+AC58),ABS((AD58-AC58)*2/PI()+AC58))/(C58/D58)))","v":10.988510400544431},{"$f":"IF((C58+(E58-C58)/G58*mspeed)<0,\"NA\",U58*(C58+(E58-C58)/G58*mspeed)*mspeed/9.55)","v":23.034763612537809},{"$f":"IF(move1,IF(speed1>speed2,AM58/2*time1/time,AM58/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z58*-speed/30*PI(),((Z58-AA58)*2/PI()+AA58)*-speed/30*PI()),IF(AccType=1,X58*-speed/30*PI(),((X58-Y58)*2/PI()+Y58)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z58*-speed/30*PI(),((Z58-AA58)*2/PI()+AA58)*-speed/30*PI()),IF(AccType=1,X58*-speed/30*PI(),((X58-Y58)*2/PI()+Y58)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD58*-speed/30*PI(),((AD58-AE58)*2/PI()+AE58)*-speed/30*PI()),IF(AccType=1,AB58*-speed/30*PI(),((AB58-AC58)*2/PI()+AC58)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD58*-speed/30*PI(),((AD58-AE58)*2/PI()+AE58)*-speed/30*PI()),IF(AccType=1,AB58*-speed/30*PI(),((AB58-AC58)*2/PI()+AC58)*-speed/30*PI()),0)/2*time7/time)))","v":2.4163107629578562},{"$f":"IF(move1,MAX(IF(AccType=1,Z58*-speed/30*PI(),((Z58-AA58)*2/PI()+AA58)*-speed/30*PI()),IF(AccType=1,X58*-speed/30*PI(),((X58-Y58)*2/PI()+Y58)*-speed/30*PI()),0),MAX(IF(AccType=1,Z58*-speed/30*PI(),((Z58-AA58)*2/PI()+AA58)*-speed/30*PI()),IF(AccType=1,X58*-speed/30*PI(),((X58-Y58)*2/PI()+Y58)*-speed/30*PI()),IF(AccType=1,AD58*-speed/30*PI(),((AD58-AE58)*2/PI()+AE58)*-speed/30*PI()),IF(AccType=1,AB58*-speed/30*PI(),((AB58-AC58)*2/PI()+AC58)*-speed/30*PI()),0))","v":148.02140747897386},{"$f":"(L58^2)/1000000+((K58/1000)^2*(D58/C58*H58)^2*PI()*PI()*(O58/2)^2)/1200","v":4.1144021928728083E-2},{"$f":"SQRT(3)*L58*J58*D58/C58*H58/1000","v":18.508640081405446},{"$f":"0.75*J58^2*(D58/C58*H58)^2-(UAC_V*0.98)^2","v":-148748.80030901331},{"$f":"-AO58/2/AN58+SQRT((AO58/2/AN58)^2-AP58/AN58)","v":1689.7319035376775},{"$f":"(L58^2)/1000000+((K58/1000)^2*AV58^2*PI()*PI()*(O58/2)^2)/1200","v":1.861389199383567E-2},{"$f":"SQRT(3)*L58*J58*AV58/1000","v":4.1454409990407406},{"$f":"0.75*J58^2*AV58^2-(UAC_V*0.98)^2","v":-153417.43375406726},{"$f":"-AS58/2/AR58+SQRT((AS58/2/AR58)^2-AT58/AR58)","v":2761.7099024117206},{"$f":"D58+(F58-D58)*((0.85*UAC_V-D58*J58)/L58*1000)/G58","v":2.2440101604278078},{"$f":"(L58^2)/1000000+((K58/1000)^2*AJ58^2*PI()*PI()*(O58/2)^2)/1200","v":4.5956219181390756E-2},{"$f":"SQRT(3)*L58*J58*AJ58/1000","v":20.299472050571374},{"$f":"0.75*J58^2*AJ58^2-(UAC_V*0.98)^2","v":-147751.6296267802},{"$f":"IF(((AX58/2/AW58)^2-AY58/AW58)>0,-AX58/2/AW58+SQRT((AX58/2/AW58)^2-AY58/AW58),-9999)","v":1585.7505560273207}]
["AKM","AKM44G",5.88,5,3.76,3.1596638655462184,4000,20.3,6000,2.65,11.5,76.599999999999994,0.27,640,10,{"$f":"IF(AQ59<I59,IF(AQ59<0,0,AQ59),I59)","v":3089.4733087080822},{"$f":"IF(AU59<I59,IF(AU59<0,0,AU59),I59)","v":4924.172358142112},{"$f":"IF(UAC_V*0.98/L59*1000<I59,IF(UAC_V*0.98/L59*1000<0,0,UAC_V*0.98/L59*1000),I59)","v":5117.493472584857},{"$f":"C59+(E59-C59)/G59*Q59","v":3.2701886501846809},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M59,(inertia/gear^2+gear_inertia)/M59),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M59,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M59))","v":416.66666666666663},{"$f":"IF((C59+(E59-C59)/G59*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X59^2*time1+Y59^2*time2+Z59^2*time3+AA59^2*time4)/time)/(C59+(E59-C59)/G59*mspeed),SQRT((((X59-Y59)*2/PI()+Y59)^2*time1+Y59^2*time2+((Z59-Y59)*2/PI()+Y59)^2*time3+AA59^2*time4)/time)/(C59+(E59-C59)/G59*mspeed)),IF(AccType=1,SQRT((X59^2*time1+Y59^2*time2+Z59^2*time3+AA59^2*time4+AB59^2*time5+AC59^2*time6+AD59^2*time7+AE59^2*time8)/time)/(C59+(E59-C59)/G59*mspeed),SQRT((((X59-Y59)*2/PI()+Y59)^2*time1+Y59^2*time2+((Z59-Y59)*2/PI()+Y59)^2*time3+AA59^2*time4+((AB59-AC59)*2/PI()+AC59)^2*time5+AC59^2*time6+((AD59-AC59)*2/PI()+AC59)^2*time7+AE59^2*time8)/time)/(C59+(E59-C59)/G59*mspeed))))","v":1.6896646659488996},{"$f":"IF(move1,MAX(ABS(X59),ABS(Z59))/H59,MAX(ABS(X59),ABS(Z59),ABS(AB59),ABS(AD59))/H59)","v":1.4357723066009853},{"$f":"IF(AZ59>0,speed/(MIN(AZ59,I59)),\"NA\")","v":4.3156360932052426E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M59+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M59+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.575528177777777},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M59+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M59+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.146177824000002},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M59+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M59+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2355.8548799999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M59+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M59+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2367.8548799999999},9,{"$f":"AH59/Irms","v":0.35130953074276278},{"$f":"AI59/Ipeak","v":0.51633676700680275},{"$f":"IF(move1,IF(AccType=1,SQRT((X59^2*time1+Y59^2*time2+Z59^2*time3+AA59^2*time4)/time)/(C59/D59),SQRT((((X59-Y59)*2/PI()+Y59)^2*time1+Y59^2*time2+((Z59-AA59)*2/PI()+AA59)^2*time3+AA59^2*time4)/time)/(C59/D59)),IF(AccType=1,SQRT((X59^2*time1+Y59^2*time2+Z59^2*time3+AA59^2*time4+AB59^2*time5+AC59^2*time6+AD59^2*time7+AE59^2*time8)/time)/(C59/D59),SQRT((((X59-Y59)*2/PI()+Y59)^2*time1+Y59^2*time2+((Z59-AA59)*2/PI()+AA59)^2*time3+AA59^2*time4+((AB59-AC59)*2/PI()+AC59)^2*time5+AC59^2*time6+((AD59-AE59)*2/PI()+AE59)^2*time7+AE59^2*time8)/time)/(C59/D59)))","v":8.4314287378263071},{"$f":"IF(move1,MAX(ABS(X59),ABS(Z59))/(C59/D59),MAX(ABS(X59),ABS(Z59),ABS(AB59),ABS(AD59))/(C59/D59))","v":24.784164816326534},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X59),ABS(Z59))/(C59/D59),MAX(ABS((X59-Y59)*2/PI()+Y59),ABS((Z59-Y59)*2/PI()+Y59))/(C59/D59)),IF(AccType=1,MAX(ABS(X59),ABS(Z59),ABS(AB59),ABS(AD59))/(C59/D59),MAX(ABS((X59-Y59)*2/PI()+Y59),ABS((Z59-Y59)*2/PI()+Y59),ABS((AB59-AC59)*2/PI()+AC59),ABS((AD59-AC59)*2/PI()+AC59))/(C59/D59)))","v":18.559060493530357},{"$f":"IF((C59+(E59-C59)/G59*mspeed)<0,\"NA\",U59*(C59+(E59-C59)/G59*mspeed)*mspeed/9.55)","v":23.034763612537809},{"$f":"IF(move1,IF(speed1>speed2,AM59/2*time1/time,AM59/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z59*-speed/30*PI(),((Z59-AA59)*2/PI()+AA59)*-speed/30*PI()),IF(AccType=1,X59*-speed/30*PI(),((X59-Y59)*2/PI()+Y59)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z59*-speed/30*PI(),((Z59-AA59)*2/PI()+AA59)*-speed/30*PI()),IF(AccType=1,X59*-speed/30*PI(),((X59-Y59)*2/PI()+Y59)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD59*-speed/30*PI(),((AD59-AE59)*2/PI()+AE59)*-speed/30*PI()),IF(AccType=1,AB59*-speed/30*PI(),((AB59-AC59)*2/PI()+AC59)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD59*-speed/30*PI(),((AD59-AE59)*2/PI()+AE59)*-speed/30*PI()),IF(AccType=1,AB59*-speed/30*PI(),((AB59-AC59)*2/PI()+AC59)*-speed/30*PI()),0)/2*time7/time)))","v":2.4163107629578562},{"$f":"IF(move1,MAX(IF(AccType=1,Z59*-speed/30*PI(),((Z59-AA59)*2/PI()+AA59)*-speed/30*PI()),IF(AccType=1,X59*-speed/30*PI(),((X59-Y59)*2/PI()+Y59)*-speed/30*PI()),0),MAX(IF(AccType=1,Z59*-speed/30*PI(),((Z59-AA59)*2/PI()+AA59)*-speed/30*PI()),IF(AccType=1,X59*-speed/30*PI(),((X59-Y59)*2/PI()+Y59)*-speed/30*PI()),IF(AccType=1,AD59*-speed/30*PI(),((AD59-AE59)*2/PI()+AE59)*-speed/30*PI()),IF(AccType=1,AB59*-speed/30*PI(),((AB59-AC59)*2/PI()+AC59)*-speed/30*PI()),0))","v":148.02140747897386},{"$f":"(L59^2)/1000000+((K59/1000)^2*(D59/C59*H59)^2*PI()*PI()*(O59/2)^2)/1200","v":1.3970294730039598E-2},{"$f":"SQRT(3)*L59*J59*D59/C59*H59/1000","v":6.0690957198951105},{"$f":"0.75*J59^2*(D59/C59*H59)^2-(UAC_V*0.98)^2","v":-152094.61158056973},{"$f":"-AO59/2/AN59+SQRT((AO59/2/AN59)^2-AP59/AN59)","v":3089.4733087080822},{"$f":"(L59^2)/1000000+((K59/1000)^2*AV59^2*PI()*PI()*(O59/2)^2)/1200","v":6.1184412778726577E-3},{"$f":"SQRT(3)*L59*J59*AV59/1000","v":1.0679288107199805},{"$f":"0.75*J59^2*AV59^2-(UAC_V*0.98)^2","v":-153615.4077425384},{"$f":"-AS59/2/AR59+SQRT((AS59/2/AR59)^2-AT59/AR59)","v":4924.172358142112},{"$f":"D59+(F59-D59)*((0.85*UAC_V-D59*J59)/L59*1000)/G59","v":3.0374352743708446},{"$f":"(L59^2)/1000000+((K59/1000)^2*AJ59^2*PI()*PI()*(O59/2)^2)/1200","v":1.5233819011115561E-2},{"$f":"SQRT(3)*L59*J59*AJ59/1000","v":6.5251613978972411},{"$f":"0.75*J59^2*AJ59^2-(UAC_V*0.98)^2","v":-151849.88428287875},{"$f":"IF(((AX59/2/AW59)^2-AY59/AW59)>0,-AX59/2/AW59+SQRT((AX59/2/AW59)^2-AY59/AW59),-9999)","v":2950.2940406393764}]
["AKM","AKM44H",5.89,5.6,3.19,3.0094339622641506,5000,20.2,6000,2.23,9.1,68,0.27,640,10,{"$f":"IF(AQ60<I60,IF(AQ60<0,0,AQ60),I60)","v":3512.9308366531741},{"$f":"IF(AU60<I60,IF(AU60<0,0,AU60),I60)","v":5579.8780376177438},{"$f":"IF(UAC_V*0.98/L60*1000<I60,IF(UAC_V*0.98/L60*1000<0,0,UAC_V*0.98/L60*1000),I60)","v":5764.7058823529414},{"$f":"C60+(E60-C60)/G60*Q60","v":2.8768658596864185},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M60,(inertia/gear^2+gear_inertia)/M60),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M60,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M60))","v":416.66666666666663},{"$f":"IF((C60+(E60-C60)/G60*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X60^2*time1+Y60^2*time2+Z60^2*time3+AA60^2*time4)/time)/(C60+(E60-C60)/G60*mspeed),SQRT((((X60-Y60)*2/PI()+Y60)^2*time1+Y60^2*time2+((Z60-Y60)*2/PI()+Y60)^2*time3+AA60^2*time4)/time)/(C60+(E60-C60)/G60*mspeed)),IF(AccType=1,SQRT((X60^2*time1+Y60^2*time2+Z60^2*time3+AA60^2*time4+AB60^2*time5+AC60^2*time6+AD60^2*time7+AE60^2*time8)/time)/(C60+(E60-C60)/G60*mspeed),SQRT((((X60-Y60)*2/PI()+Y60)^2*time1+Y60^2*time2+((Z60-Y60)*2/PI()+Y60)^2*time3+AA60^2*time4+((AB60-AC60)*2/PI()+AC60)^2*time5+AC60^2*time6+((AD60-AC60)*2/PI()+AC60)^2*time7+AE60^2*time8)/time)/(C60+(E60-C60)/G60*mspeed))))","v":1.6868538930719319},{"$f":"IF(move1,MAX(ABS(X60),ABS(Z60))/H60,MAX(ABS(X60),ABS(Z60),ABS(AB60),ABS(AD60))/H60)","v":1.4428800902970298},{"$f":"IF(AZ60>0,speed/(MIN(AZ60,I60)),\"NA\")","v":3.805691760442087E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M60+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M60+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.575528177777777},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M60+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M60+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.146177824000002},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M60+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M60+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2355.8548799999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M60+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M60+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2367.8548799999999},9,{"$f":"AH60/Irms","v":0.39279864951774851},{"$f":"AI60/Ipeak","v":0.57731535022071312},{"$f":"IF(move1,IF(AccType=1,SQRT((X60^2*time1+Y60^2*time2+Z60^2*time3+AA60^2*time4)/time)/(C60/D60),SQRT((((X60-Y60)*2/PI()+Y60)^2*time1+Y60^2*time2+((Z60-AA60)*2/PI()+AA60)^2*time3+AA60^2*time4)/time)/(C60/D60)),IF(AccType=1,SQRT((X60^2*time1+Y60^2*time2+Z60^2*time3+AA60^2*time4+AB60^2*time5+AC60^2*time6+AD60^2*time7+AE60^2*time8)/time)/(C60/D60),SQRT((((X60-Y60)*2/PI()+Y60)^2*time1+Y60^2*time2+((Z60-AA60)*2/PI()+AA60)^2*time3+AA60^2*time4+((AB60-AC60)*2/PI()+AC60)^2*time5+AC60^2*time6+((AD60-AE60)*2/PI()+AE60)^2*time7+AE60^2*time8)/time)/(C60/D60)))","v":9.4271675884259647},{"$f":"IF(move1,MAX(ABS(X60),ABS(Z60))/(C60/D60),MAX(ABS(X60),ABS(Z60),ABS(AB60),ABS(AD60))/(C60/D60))","v":27.71113681059423},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X60),ABS(Z60))/(C60/D60),MAX(ABS((X60-Y60)*2/PI()+Y60),ABS((Z60-Y60)*2/PI()+Y60))/(C60/D60)),IF(AccType=1,MAX(ABS(X60),ABS(Z60),ABS(AB60),ABS(AD60))/(C60/D60),MAX(ABS((X60-Y60)*2/PI()+Y60),ABS((Z60-Y60)*2/PI()+Y60),ABS((AB60-AC60)*2/PI()+AC60),ABS((AD60-AC60)*2/PI()+AC60))/(C60/D60)))","v":20.750857179319777},{"$f":"IF((C60+(E60-C60)/G60*mspeed)<0,\"NA\",U60*(C60+(E60-C60)/G60*mspeed)*mspeed/9.55)","v":23.034763612537809},{"$f":"IF(move1,IF(speed1>speed2,AM60/2*time1/time,AM60/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z60*-speed/30*PI(),((Z60-AA60)*2/PI()+AA60)*-speed/30*PI()),IF(AccType=1,X60*-speed/30*PI(),((X60-Y60)*2/PI()+Y60)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z60*-speed/30*PI(),((Z60-AA60)*2/PI()+AA60)*-speed/30*PI()),IF(AccType=1,X60*-speed/30*PI(),((X60-Y60)*2/PI()+Y60)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD60*-speed/30*PI(),((AD60-AE60)*2/PI()+AE60)*-speed/30*PI()),IF(AccType=1,AB60*-speed/30*PI(),((AB60-AC60)*2/PI()+AC60)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD60*-speed/30*PI(),((AD60-AE60)*2/PI()+AE60)*-speed/30*PI()),IF(AccType=1,AB60*-speed/30*PI(),((AB60-AC60)*2/PI()+AC60)*-speed/30*PI()),0)/2*time7/time)))","v":2.4163107629578562},{"$f":"IF(move1,MAX(IF(AccType=1,Z60*-speed/30*PI(),((Z60-AA60)*2/PI()+AA60)*-speed/30*PI()),IF(AccType=1,X60*-speed/30*PI(),((X60-Y60)*2/PI()+Y60)*-speed/30*PI()),0),MAX(IF(AccType=1,Z60*-speed/30*PI(),((Z60-AA60)*2/PI()+AA60)*-speed/30*PI()),IF(AccType=1,X60*-speed/30*PI(),((X60-Y60)*2/PI()+Y60)*-speed/30*PI()),IF(AccType=1,AD60*-speed/30*PI(),((AD60-AE60)*2/PI()+AE60)*-speed/30*PI()),IF(AccType=1,AB60*-speed/30*PI(),((AB60-AC60)*2/PI()+AC60)*-speed/30*PI()),0))","v":148.02140747897386},{"$f":"(L60^2)/1000000+((K60/1000)^2*(D60/C60*H60)^2*PI()*PI()*(O60/2)^2)/1200","v":1.0904431685355397E-2},{"$f":"SQRT(3)*L60*J60*D60/C60*H60/1000","v":5.0442720927141425},{"$f":"0.75*J60^2*(D60/C60*H60)^2-(UAC_V*0.98)^2","v":-152288.31439525654},{"$f":"-AO60/2/AN60+SQRT((AO60/2/AN60)^2-AP60/AN60)","v":3512.9308366531741},{"$f":"(L60^2)/1000000+((K60/1000)^2*AV60^2*PI()*PI()*(O60/2)^2)/1200","v":4.7881149340894581E-3},{"$f":"SQRT(3)*L60*J60*AV60/1000","v":0.81541333244629666},{"$f":"0.75*J60^2*AV60^2-(UAC_V*0.98)^2","v":-153628.05174617586},{"$f":"-AS60/2/AR60+SQRT((AS60/2/AR60)^2-AT60/AR60)","v":5579.8780376177438},{"$f":"D60+(F60-D60)*((0.85*UAC_V-D60*J60)/L60*1000)/G60","v":3.1045839289678132},{"$f":"(L60^2)/1000000+((K60/1000)^2*AJ60^2*PI()*PI()*(O60/2)^2)/1200","v":1.1955846691076466E-2},{"$f":"SQRT(3)*L60*J60*AJ60/1000","v":5.4501749641317945},{"$f":"0.75*J60^2*AJ60^2-(UAC_V*0.98)^2","v":-152058.00912956049},{"$f":"IF(((AX60/2/AW60)^2-AY60/AW60)>0,-AX60/2/AW60+SQRT((AX60/2/AW60)^2-AY60/AW60),-9999)","v":3345.6192063943117}]
["AKM","AKM44J",6,8.8000000000000007,2.75,3.985507246376812,6000,20.399999999999999,6000,0.88,3.8,44.2,0.27,640,10,{"$f":"IF(AQ61<I61,IF(AQ61<0,0,AQ61),I61)","v":5548.2706556938892},{"$f":"IF(AU61<I61,IF(AU61<0,0,AU61),I61)","v":6000},{"$f":"IF(UAC_V*0.98/L61*1000<I61,IF(UAC_V*0.98/L61*1000<0,0,UAC_V*0.98/L61*1000),I61)","v":6000},{"$f":"C61+(E61-C61)/G61*Q61","v":2.75},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M61,(inertia/gear^2+gear_inertia)/M61),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M61,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M61))","v":416.66666666666663},{"$f":"IF((C61+(E61-C61)/G61*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X61^2*time1+Y61^2*time2+Z61^2*time3+AA61^2*time4)/time)/(C61+(E61-C61)/G61*mspeed),SQRT((((X61-Y61)*2/PI()+Y61)^2*time1+Y61^2*time2+((Z61-Y61)*2/PI()+Y61)^2*time3+AA61^2*time4)/time)/(C61+(E61-C61)/G61*mspeed)),IF(AccType=1,SQRT((X61^2*time1+Y61^2*time2+Z61^2*time3+AA61^2*time4+AB61^2*time5+AC61^2*time6+AD61^2*time7+AE61^2*time8)/time)/(C61+(E61-C61)/G61*mspeed),SQRT((((X61-Y61)*2/PI()+Y61)^2*time1+Y61^2*time2+((Z61-Y61)*2/PI()+Y61)^2*time3+AA61^2*time4+((AB61-AC61)*2/PI()+AC61)^2*time5+AC61^2*time6+((AD61-AC61)*2/PI()+AC61)^2*time7+AE61^2*time8)/time)/(C61+(E61-C61)/G61*mspeed))))","v":1.6558765895884324},{"$f":"IF(move1,MAX(ABS(X61),ABS(Z61))/H61,MAX(ABS(X61),ABS(Z61),ABS(AB61),ABS(AD61))/H61)","v":1.4287342070588238},{"$f":"IF(AZ61>0,speed/(MIN(AZ61,I61)),\"NA\")","v":2.391712460930492E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M61+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M61+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.575528177777777},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M61+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M61+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.146177824000002},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M61+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M61+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2355.8548799999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M61+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M61+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2367.8548799999999},9,{"$f":"AH61/Irms","v":0.6059386786251173},{"$f":"AI61/Ipeak","v":0.89057765573333347},{"$f":"IF(move1,IF(AccType=1,SQRT((X61^2*time1+Y61^2*time2+Z61^2*time3+AA61^2*time4)/time)/(C61/D61),SQRT((((X61-Y61)*2/PI()+Y61)^2*time1+Y61^2*time2+((Z61-AA61)*2/PI()+AA61)^2*time3+AA61^2*time4)/time)/(C61/D61)),IF(AccType=1,SQRT((X61^2*time1+Y61^2*time2+Z61^2*time3+AA61^2*time4+AB61^2*time5+AC61^2*time6+AD61^2*time7+AE61^2*time8)/time)/(C61/D61),SQRT((((X61-Y61)*2/PI()+Y61)^2*time1+Y61^2*time2+((Z61-AA61)*2/PI()+AA61)^2*time3+AA61^2*time4+((AB61-AC61)*2/PI()+AC61)^2*time5+AC61^2*time6+((AD61-AE61)*2/PI()+AE61)^2*time7+AE61^2*time8)/time)/(C61/D61)))","v":14.542528287002815},{"$f":"IF(move1,MAX(ABS(X61),ABS(Z61))/(C61/D61),MAX(ABS(X61),ABS(Z61),ABS(AB61),ABS(AD61))/(C61/D61))","v":42.747727475200008},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X61),ABS(Z61))/(C61/D61),MAX(ABS((X61-Y61)*2/PI()+Y61),ABS((Z61-Y61)*2/PI()+Y61))/(C61/D61)),IF(AccType=1,MAX(ABS(X61),ABS(Z61),ABS(AB61),ABS(AD61))/(C61/D61),MAX(ABS((X61-Y61)*2/PI()+Y61),ABS((Z61-Y61)*2/PI()+Y61),ABS((AB61-AC61)*2/PI()+AC61),ABS((AD61-AC61)*2/PI()+AC61))/(C61/D61)))","v":32.010667539241155},{"$f":"IF((C61+(E61-C61)/G61*mspeed)<0,\"NA\",U61*(C61+(E61-C61)/G61*mspeed)*mspeed/9.55)","v":23.034763612537809},{"$f":"IF(move1,IF(speed1>speed2,AM61/2*time1/time,AM61/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z61*-speed/30*PI(),((Z61-AA61)*2/PI()+AA61)*-speed/30*PI()),IF(AccType=1,X61*-speed/30*PI(),((X61-Y61)*2/PI()+Y61)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z61*-speed/30*PI(),((Z61-AA61)*2/PI()+AA61)*-speed/30*PI()),IF(AccType=1,X61*-speed/30*PI(),((X61-Y61)*2/PI()+Y61)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD61*-speed/30*PI(),((AD61-AE61)*2/PI()+AE61)*-speed/30*PI()),IF(AccType=1,AB61*-speed/30*PI(),((AB61-AC61)*2/PI()+AC61)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD61*-speed/30*PI(),((AD61-AE61)*2/PI()+AE61)*-speed/30*PI()),IF(AccType=1,AB61*-speed/30*PI(),((AB61-AC61)*2/PI()+AC61)*-speed/30*PI()),0)/2*time7/time)))","v":2.4163107629578562},{"$f":"IF(move1,MAX(IF(AccType=1,Z61*-speed/30*PI(),((Z61-AA61)*2/PI()+AA61)*-speed/30*PI()),IF(AccType=1,X61*-speed/30*PI(),((X61-Y61)*2/PI()+Y61)*-speed/30*PI()),0),MAX(IF(AccType=1,Z61*-speed/30*PI(),((Z61-AA61)*2/PI()+AA61)*-speed/30*PI()),IF(AccType=1,X61*-speed/30*PI(),((X61-Y61)*2/PI()+Y61)*-speed/30*PI()),IF(AccType=1,AD61*-speed/30*PI(),((AD61-AE61)*2/PI()+AE61)*-speed/30*PI()),IF(AccType=1,AB61*-speed/30*PI(),((AB61-AC61)*2/PI()+AC61)*-speed/30*PI()),0))","v":148.02140747897386},{"$f":"(L61^2)/1000000+((K61/1000)^2*(D61/C61*H61)^2*PI()*PI()*(O61/2)^2)/1200","v":4.6116026851181118E-3},{"$f":"SQRT(3)*L61*J61*D61/C61*H61/1000","v":2.015705858479075},{"$f":"0.75*J61^2*(D61/C61*H61)^2-(UAC_V*0.98)^2","v":-153144.06412287999},{"$f":"-AO61/2/AN61+SQRT((AO61/2/AN61)^2-AP61/AN61)","v":5548.2706556938892},{"$f":"(L61^2)/1000000+((K61/1000)^2*AV61^2*PI()*PI()*(O61/2)^2)/1200","v":1.9763913890778607E-3},{"$f":"SQRT(3)*L61*J61*AV61/1000","v":0.18649048438731308},{"$f":"0.75*J61^2*AV61^2-(UAC_V*0.98)^2","v":-153659.54949980971},{"$f":"-AS61/2/AR61+SQRT((AS61/2/AR61)^2-AT61/AR61)","v":8770.4026799900403},{"$f":"D61+(F61-D61)*((0.85*UAC_V-D61*J61)/L61*1000)/G61","v":2.7681594858679279},{"$f":"(L61^2)/1000000+((K61/1000)^2*AJ61^2*PI()*PI()*(O61/2)^2)/1200","v":4.9960319478091252E-3},{"$f":"SQRT(3)*L61*J61*AJ61/1000","v":2.1565538132578332},{"$f":"0.75*J61^2*AJ61^2-(UAC_V*0.98)^2","v":-153068.86420867243},{"$f":"IF(((AX61/2/AW61)^2-AY61/AW61)>0,-AX61/2/AW61+SQRT((AX61/2/AW61)^2-AY61/AW61),-9999)","v":5323.5477321542694}]
["AKM","AKM44K",5.88,10.1,3.18,5.389830508474577,5000,20.100000000000001,6000,0.68,2.8,37.799999999999997,0.27,640,10,{"$f":"IF(AQ62<I62,IF(AQ62<0,0,AQ62),I62)","v":6000},{"$f":"IF(AU62<I62,IF(AU62<0,0,AU62),I62)","v":6000},{"$f":"IF(UAC_V*0.98/L62*1000<I62,IF(UAC_V*0.98/L62*1000<0,0,UAC_V*0.98/L62*1000),I62)","v":6000},{"$f":"C62+(E62-C62)/G62*Q62","v":2.6400000000000006},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M62,(inertia/gear^2+gear_inertia)/M62),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M62,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M62))","v":416.66666666666663},{"$f":"IF((C62+(E62-C62)/G62*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X62^2*time1+Y62^2*time2+Z62^2*time3+AA62^2*time4)/time)/(C62+(E62-C62)/G62*mspeed),SQRT((((X62-Y62)*2/PI()+Y62)^2*time1+Y62^2*time2+((Z62-Y62)*2/PI()+Y62)^2*time3+AA62^2*time4)/time)/(C62+(E62-C62)/G62*mspeed)),IF(AccType=1,SQRT((X62^2*time1+Y62^2*time2+Z62^2*time3+AA62^2*time4+AB62^2*time5+AC62^2*time6+AD62^2*time7+AE62^2*time8)/time)/(C62+(E62-C62)/G62*mspeed),SQRT((((X62-Y62)*2/PI()+Y62)^2*time1+Y62^2*time2+((Z62-Y62)*2/PI()+Y62)^2*time3+AA62^2*time4+((AB62-AC62)*2/PI()+AC62)^2*time5+AC62^2*time6+((AD62-AC62)*2/PI()+AC62)^2*time7+AE62^2*time8)/time)/(C62+(E62-C62)/G62*mspeed))))","v":1.6897285492874883},{"$f":"IF(move1,MAX(ABS(X62),ABS(Z62))/H62,MAX(ABS(X62),ABS(Z62),ABS(AB62),ABS(AD62))/H62)","v":1.4500585982089553},{"$f":"IF(AZ62>0,speed/(MIN(AZ62,I62)),\"NA\")","v":2.1220659078919377E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M62+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M62+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.575528177777777},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M62+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M62+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.146177824000002},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M62+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M62+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2355.8548799999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M62+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M62+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2367.8548799999999},9,{"$f":"AH62/Irms","v":0.70964525210038099},{"$f":"AI62/Ipeak","v":1.0430002693537417},{"$f":"IF(move1,IF(AccType=1,SQRT((X62^2*time1+Y62^2*time2+Z62^2*time3+AA62^2*time4)/time)/(C62/D62),SQRT((((X62-Y62)*2/PI()+Y62)^2*time1+Y62^2*time2+((Z62-AA62)*2/PI()+AA62)^2*time3+AA62^2*time4)/time)/(C62/D62)),IF(AccType=1,SQRT((X62^2*time1+Y62^2*time2+Z62^2*time3+AA62^2*time4+AB62^2*time5+AC62^2*time6+AD62^2*time7+AE62^2*time8)/time)/(C62/D62),SQRT((((X62-Y62)*2/PI()+Y62)^2*time1+Y62^2*time2+((Z62-AA62)*2/PI()+AA62)^2*time3+AA62^2*time4+((AB62-AC62)*2/PI()+AC62)^2*time5+AC62^2*time6+((AD62-AE62)*2/PI()+AE62)^2*time7+AE62^2*time8)/time)/(C62/D62)))","v":17.031486050409143},{"$f":"IF(move1,MAX(ABS(X62),ABS(Z62))/(C62/D62),MAX(ABS(X62),ABS(Z62),ABS(AB62),ABS(AD62))/(C62/D62))","v":50.064012928979601},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X62),ABS(Z62))/(C62/D62),MAX(ABS((X62-Y62)*2/PI()+Y62),ABS((Z62-Y62)*2/PI()+Y62))/(C62/D62)),IF(AccType=1,MAX(ABS(X62),ABS(Z62),ABS(AB62),ABS(AD62))/(C62/D62),MAX(ABS((X62-Y62)*2/PI()+Y62),ABS((Z62-Y62)*2/PI()+Y62),ABS((AB62-AC62)*2/PI()+AC62),ABS((AD62-AC62)*2/PI()+AC62))/(C62/D62)))","v":37.48930219693132},{"$f":"IF((C62+(E62-C62)/G62*mspeed)<0,\"NA\",U62*(C62+(E62-C62)/G62*mspeed)*mspeed/9.55)","v":23.034763612537809},{"$f":"IF(move1,IF(speed1>speed2,AM62/2*time1/time,AM62/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z62*-speed/30*PI(),((Z62-AA62)*2/PI()+AA62)*-speed/30*PI()),IF(AccType=1,X62*-speed/30*PI(),((X62-Y62)*2/PI()+Y62)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z62*-speed/30*PI(),((Z62-AA62)*2/PI()+AA62)*-speed/30*PI()),IF(AccType=1,X62*-speed/30*PI(),((X62-Y62)*2/PI()+Y62)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD62*-speed/30*PI(),((AD62-AE62)*2/PI()+AE62)*-speed/30*PI()),IF(AccType=1,AB62*-speed/30*PI(),((AB62-AC62)*2/PI()+AC62)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD62*-speed/30*PI(),((AD62-AE62)*2/PI()+AE62)*-speed/30*PI()),IF(AccType=1,AB62*-speed/30*PI(),((AB62-AC62)*2/PI()+AC62)*-speed/30*PI()),0)/2*time7/time)))","v":2.4163107629578562},{"$f":"IF(move1,MAX(IF(AccType=1,Z62*-speed/30*PI(),((Z62-AA62)*2/PI()+AA62)*-speed/30*PI()),IF(AccType=1,X62*-speed/30*PI(),((X62-Y62)*2/PI()+Y62)*-speed/30*PI()),0),MAX(IF(AccType=1,Z62*-speed/30*PI(),((Z62-AA62)*2/PI()+AA62)*-speed/30*PI()),IF(AccType=1,X62*-speed/30*PI(),((X62-Y62)*2/PI()+Y62)*-speed/30*PI()),IF(AccType=1,AD62*-speed/30*PI(),((AD62-AE62)*2/PI()+AE62)*-speed/30*PI()),IF(AccType=1,AB62*-speed/30*PI(),((AB62-AC62)*2/PI()+AC62)*-speed/30*PI()),0))","v":148.02140747897386},{"$f":"(L62^2)/1000000+((K62/1000)^2*(D62/C62*H62)^2*PI()*PI()*(O62/2)^2)/1200","v":3.3504036779351863E-3},{"$f":"SQRT(3)*L62*J62*D62/C62*H62/1000","v":1.5370976020004949},{"$f":"0.75*J62^2*(D62/C62*H62)^2-(UAC_V*0.98)^2","v":-153250.61063553728},{"$f":"-AO62/2/AN62+SQRT((AO62/2/AN62)^2-AP62/AN62)","v":6537.7039147085652},{"$f":"(L62^2)/1000000+((K62/1000)^2*AV62^2*PI()*PI()*(O62/2)^2)/1200","v":1.4340504687295611E-3},{"$f":"SQRT(3)*L62*J62*AV62/1000","v":8.0040989969482446E-2},{"$f":"0.75*J62^2*AV62^2-(UAC_V*0.98)^2","v":-153662.87906272302},{"$f":"-AS62/2/AR62+SQRT((AS62/2/AR62)^2-AT62/AR62)","v":10323.605961314859},{"$f":"D62+(F62-D62)*((0.85*UAC_V-D62*J62)/L62*1000)/G62","v":1.7978403013182707},{"$f":"(L62^2)/1000000+((K62/1000)^2*AJ62^2*PI()*PI()*(O62/2)^2)/1200","v":3.6944715525793165E-3},{"$f":"SQRT(3)*L62*J62*AJ62/1000","v":1.6690475004410676},{"$f":"0.75*J62^2*AJ62^2-(UAC_V*0.98)^2","v":-153176.590710169},{"$f":"IF(((AX62/2/AW62)^2-AY62/AW62)>0,-AX62/2/AW62+SQRT((AX62/2/AW62)^2-AY62/AW62),-9999)","v":6217.1002723472193}]
["AKM","AKM51E",4.7,2.75,3.98,2.3139534883720931,2500,11.6,6000,8.4700000000000006,36.6,110,0.34,640,10,2258.5574875784655,3240.0972804197768,3563.6363636363635,3.7668519832391043,330.88235294117646,2.1127839462662545,2.5138401213793107,8.9471681683010534E-2,-22.593265935802467,9,29.160545408000001,9,-2357.32096,7.5,2369.32096,9,0.24176071056245785,0.35545877602836878,5.8022570534989883,17.062021249361703,12.775564899623388,23.037608498016418,2.4187685590227637,148.17197024532041,2.4788384450708075E-2,10.952910728391561,-151185.3584003282,2258.5574875784655,1.3491695303351979E-2,3.6274251874339725,-153392.13608490847,3240.0972804197768,2.2478210887949261,5.7055300377193016E-2,20.61659005318602,-144882.10360700148,1423.0642822229793]
["AKM","AKM51G",4.75,4.84,2.62,2.6464646464646466,5000,11.7,6000,2.75,12.1,63.6,0.34,640,10,4073.9169398357917,5923.2849181810825,6000,2.226680624854859,330.88235294117646,2.0918643091876739,2.4923543083760684,4.8055897886198344E-2,-22.593265935802467,9,29.160545408000001,9,-2357.32096,7.5,2369.32096,9,0.42101991532055821,0.61902210427508775,10.104477967693397,29.71306100520421,22.248310073617827,23.037608498016418,2.4187685590227637,148.17197024532041,8.3235874802755263E-3,3.6115035874976238,-152857.87594917451,4073.9169398357917,4.2463609607813202E-3,0.78354975928116055,-153626.05461702528,5923.2849181810825,2.5865218092878473,1.8946230756332155E-2,6.73980707991619,-150856.49390139282,2649.4969415623741]
["AKM","AKM51H",4.79,6,1.95,1.9696969696969697,6000,11.7,6000,1.97,7.9,51.3,0.34,640,10,5096.7950638771163,6000,6000,1.9500000000000002,330.88235294117646,2.0748169501117042,2.4923543083760684,3.8246419096000149E-2,-22.593265935802467,9,29.160545408000001,9,-2357.32096,7.5,2369.32096,9,0.51756705544591475,0.76097456701461386,12.421609330701953,36.526779216701463,27.350231935424528,23.037608498016418,2.4187685590227637,148.17197024532041,5.3879227452663728E-3,2.5653452241739085,-153038.83175077688,5096.7950638771163,2.668900202503913E-3,0.29807042725673277,-153655.55998810602,7532.0259759123574,1.7028432472876922,1.2230882870616092E-2,4.7874608138757306,-151486.71268230723,3329.0424955582821]
["AKM","AKM51I",4.83,7.5,1.97,3.078125,6000,11.8,6000,1.3,5.15,41.4,0.34,640,10,6000,6000,6000,1.9699999999999998,330.88235294117646,2.0576283344644888,2.471232661694915,3.0510858440553359E-2,-22.593265935802467,9,29.160545408000001,9,-2357.32096,7.5,2369.32096,9,0.64160098229449569,0.94334062525879914,15.398423575067897,45.28035001242236,33.904661224296966,23.037608498016418,2.4187685590227637,148.17197024532041,3.5448626193285088E-3,1.7080495320925659,-153238.46013849773,6338.3182806986715,1.7282911421240667E-3,0.15111523095553978,-153660.66914440438,9385.5411321699066,1.621078024355878,7.9828663871031862E-3,3.1605577488565082,-152206.97572815922,4173.0702111050487]
["AKM","AKM51K",4.9000000000000004,9.4,2.35,4.5192307692307692,5500,11.9,6000,0.75,3.4,33.5,0.34,640,10,6000,6000,6000,2.1181818181818186,330.88235294117646,2.0280501566751941,2.4504660006722689,2.4457783006820041E-2,-22.593265935802467,9,29.160545408000001,9,-2357.32096,7.5,2369.32096,9,0.79265218498325696,1.1654299610340135,19.023652439598166,55.940638129632653,41.886787181102882,23.037608498016418,2.4187685590227637,148.17197024532041,2.3609718892966636E-3,0.99344867015983618,-153444.14251275509,7854.112910046093,1.1230500913428094E-3,2.5248077369383858E-2,-153663.85799389376,11686.082709542217,0.58017847823817981,5.2925801943293502E-3,1.8228198445328105,-152923.81907203773,5205.8665512737616]
["AKM","AKM51L",4.8899999999999997,11.9,2,4.8780487804878048,6000,12,6000,0.56000000000000005,2.1,26.6,0.34,640,10,6000,6000,6000,2,330.88235294117646,2.0323728469506221,2.4300454506666669,2.1220659078919377E-2,-22.593265935802467,9,29.160545408000001,9,-2357.32096,7.5,2369.32096,9,1.005516009797975,1.4784018846080438,24.132384235151399,70.963290461186105,53.13532960296979,23.037608498016418,2.4187685590227637,148.17197024532041,1.4808382485152808E-3,0.75344167624931879,-153463.42536339344,9928.8011751570084,7.1449670626565654E-4,-7.1360583845421488E-2,-153662.20074165909,14715.067982659411,-2.7658466898954721,3.2677008259763092E-3,1.3709249168218112,-152999.94496312577,6636.0981860972743]
["AKM","AKM52E",8.34,2.99,7.61,2.7275985663082438,1500,21.3,6000,8.59,44.7,179,0.62,640,10,1467.4777690348244,1993.0808844935777,2189.9441340782123,7.3700339695464594,181.45161290322579,1.1911691219007017,1.3717378283568076,8.7969671225590462E-2,-22.664216967901236,9,29.218015744000002,9,-2363.1852800000001,7.5,2375.1852800000001,9,0.14820769756627192,0.21823008361950444,3.5569847415905258,10.475044013736213,7.8411095750841344,23.049002172390853,2.4285997432823918,148.77422131070654,5.599858493683528E-2,20.337218904969554,-150436.86544748407,1467.4777690348244,3.4998043372753744E-2,7.1449450378431481,-153265.68035022472,1993.0808844935777,2.6828233043124219,5.7300723952407449E-2,20.882589196100707,-150261.46472072421,1447.3619453118702]
["AKM","AKM52G",8.43,4.72,7.06,3.94413407821229,2500,21.5,6000,3.47,18.5,115,0.62,640,10,2378.97044753505,3188.6544700785535,3408.695652173913,6.6826173503969519,181.45161290322579,1.1786261983973787,1.3589774764651164,5.3969614209498813E-2,-22.664216967901236,9,29.218015744000002,9,-2363.1852800000001,7.5,2375.1852800000001,9,0.23146218407569638,0.34081908440015818,5.5550924178167129,16.359316051207593,12.245790047539719,23.049002172390853,2.4285997432823918,148.77422131070654,2.3422829172479037E-2,8.3203352657985032,-152355.34255320812,2378.97044753505,1.4266281652134767E-2,2.658710606326216,-153530.37538585649,3188.6544700785535,3.8466540139324743,2.3777991377746707E-2,8.4639824024499344,-152309.76563121018,2359.178518105969]
["AKM","AKM52H",8.48,5.9,6.26,4.3472222222222223,3500,21.6,6000,2.35,11.9,92.7,0.62,640,10,2991.6337251016348,4010.3214669987456,4228.6947141316068,5.9363103837893672,181.45161290322579,1.1719317133604101,1.3526859140740741,4.2813735161864576E-2,-22.664216967901236,9,29.218015744000002,9,-2363.1852800000001,7.5,2375.1852800000001,9,0.28762178828981727,0.42351192238993712,6.9029229189556149,20.328572274716983,15.216982620984647,23.049002172390853,2.4285997432823918,148.77422131070654,1.5169448193407913E-2,5.6704579511558819,-152728.55812105065,2991.6337251016348,9.1415207144875006E-3,1.6372450645889931,-153586.01556675264,4010.3214669987456,4.3391580195544597,1.5335612470483283E-2,5.7416507031706878,-152704.92167268822,2973.9043788668869]
["AKM","AKM52I",8.5299999999999994,7.4,5.16,4.4482758620689662,4500,21.8,6000,1.57,7.8,74.900000000000006,0.62,640,10,3708.8615851093441,5039.5765133237928,5233.6448598130837,4.7559171444664043,181.45161290322579,1.165398841895005,1.3402759515596332,3.4383006011958574E-2,-22.664216967901236,9,29.218015744000002,9,-2363.1852800000001,7.5,2375.1852800000001,9,0.35863139982042674,0.52807081991402904,8.6071535956902423,25.347399355873392,18.97383300081524,23.049002172390853,2.4285997432823918,148.77422131070654,1.0084320072970766E-2,3.8519556629686509,-153002.79073167979,3708.8615851093441,5.8660622727808647E-3,0.92147288075491385,-153626.16083973259,5039.5765133237928,4.5241860974274779,1.0113589784137655E-2,3.8645343444571103,-152998.46528172461,3703.1071230139792]
["AKM","AKM52K",8.6,9.3000000000000007,3.9,4.193548387096774,5500,21.9,6000,0.93,5,60.1,0.62,640,10,4684.9500156406775,6000,6000,3.4727272727272736,181.45161290322579,1.1562104330290355,1.3341559700456622,2.7160553142436449E-2,-22.664216967901236,9,29.218015744000002,9,-2363.1852800000001,7.5,2375.1852800000001,9,0.44704384532298297,0.65825471516279088,10.729052287751591,31.596226327813962,23.651401604677442,23.04900217239085,2.4285997432823918,148.77422131070654,6.4950836773473523E-3,2.2926969860964403,-153300.18183019594,4684.9500156406775,3.7018759258363827E-3,0.40477745552472355,-153652.65972211448,6388.1295268584699,4.181174259908949,6.4875027819457191E-3,2.2896807370432768,-153301.13847154443,4687.8262679629142]
["AKM","AKM52L",8.67,11.6,3.27,4.3600000000000003,6000,22,6000,0.61,3.24,48.3,0.62,640,10,5865.7080684199218,6000,6000,3.2699999999999996,181.45161290322579,1.1469886474963402,1.3280916247272729,2.1647742669108148E-2,-22.664216967901236,9,29.218015744000002,9,-2363.1852800000001,7.5,2375.1852800000001,9,0.5531010902682687,0.81441989290272987,13.274426166438449,39.092154859331032,29.262489911853024,23.049002172390853,2.4285997432823918,148.77422131070654,4.203019468147929E-3,1.5021011053236613,-153422.20680244089,5865.7080684199218,2.3561492715612259E-3,0.16751796305978844,-153660.992757058,8040.2335985679183,3.2826440303657698,4.1811841221409069E-3,1.4933062064439016,-153425.02994288158,5881.6273095859842]
["AKM","AKM52M",8.6,13.1,5.2,7.8787878787878789,4500,21.9,6000,0.48,2.5,42.4,0.62,640,10,6000,6000,6000,4.0666666666666673,181.45161290322579,1.1559145941260422,1.3341559700456622,2.1220659078919377E-2,-22.664216967901236,9,29.218015744000002,9,-2363.1852800000001,7.5,2375.1852800000001,9,0.6297069219065673,0.92721900737984508,15.112966125757614,44.506512354232562,33.315415163577896,23.049002172390853,2.4285997432823918,148.77422131070654,3.2278798802450543E-3,1.1759386929587528,-153471.70072067497,6715.5887146937348,1.8179942433973262E-3,0.13987559391170173,-153661.2792277929,9155.2184771677403,3.9680233784384722,3.2241194528549676E-3,1.1743916398633261,-153472.20636183629,6719.6454058845411]
["AKM","AKM53G",11.4,4.7699999999999996,9.85,4.1213389121338908,2000,29.7,6000,3.75,21.3,154,0.91,640,10,1840.628281003542,2384.5262190629514,2545.4545454545455,9.5519921802262111,123.62637362637362,0.87206785109646634,0.98577571016835019,6.1812271595071577E-2,-22.737701965432098,9,29.277538591999999,9,-2369.2590399999999,7.5,2381.2590399999999,9,0.1730620689625417,0.25521538575263153,4.1534896551010005,12.250338516126314,9.1672211537252828,23.060826574487265,2.4387820412655792,149.39798134271362,3.8122472976757991E-2,12.43032812567473,-152035.21503086586,1840.628281003542,2.5277736447391071E-2,4.092678513113392,-153487.43125514736,2384.5262190629514,4.0916173874504151,3.1555586060667135E-2,9.1695985934277928,-152777.66231273621,2059.8491397890652]
["AKM","AKM53H",11.51,6.6,8.83,5.0457142857142854,3000,30,6000,2.1,11.4,112.4,0.91,640,10,2560.5408744092319,3317.2918497096894,3487.5444839857651,8.546552614259344,123.62637362637362,0.86391845885031904,0.97591795306666662,4.442470055860244E-2,-22.737701965432098,9,29.277538591999999,9,-2369.2590399999999,7.5,2381.2590399999999,9,0.23716848294786305,0.3497533932580365,5.692043590748713,16.788162876385751,12.562983598371124,23.060826574487265,2.4387820412655792,149.39798134271362,2.0541419198029605E-2,7.0329268443505155,-152685.23239641276,2560.5408744092319,1.3327897249651298E-2,2.0836981364684823,-153578.08341768559,3317.2918497096894,5.0966941196407385,1.6851247423914001E-2,5.1361656983753319,-153141.98204807661,2866.0621877587678]
["AKM","AKM53I",11.58,7.4,8.58,5.5,3250,30.1,6000,1.66,9.11,100.6,0.91,640,10,{"$f":"IF(AQ78<I78,IF(AQ78<0,0,AQ78),I78)","v":2885.6485411114072},{"$f":"IF(AU78<I78,IF(AU78<0,0,AU78),I78)","v":3726.2752390275537},{"$f":"IF(UAC_V*0.98/L78*1000<I78,IF(UAC_V*0.98/L78*1000<0,0,UAC_V*0.98/L78*1000),I78)","v":3896.62027833002},{"$f":"C78+(E78-C78)/G78*Q78","v":8.1403613178207195},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M78,(inertia/gear^2+gear_inertia)/M78),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M78,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M78))","v":123.62637362637362},{"$f":"IF((C78+(E78-C78)/G78*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X78^2*time1+Y78^2*time2+Z78^2*time3+AA78^2*time4)/time)/(C78+(E78-C78)/G78*mspeed),SQRT((((X78-Y78)*2/PI()+Y78)^2*time1+Y78^2*time2+((Z78-Y78)*2/PI()+Y78)^2*time3+AA78^2*time4)/time)/(C78+(E78-C78)/G78*mspeed)),IF(AccType=1,SQRT((X78^2*time1+Y78^2*time2+Z78^2*time3+AA78^2*time4+AB78^2*time5+AC78^2*time6+AD78^2*time7+AE78^2*time8)/time)/(C78+(E78-C78)/G78*mspeed),SQRT((((X78-Y78)*2/PI()+Y78)^2*time1+Y78^2*time2+((Z78-Y78)*2/PI()+Y78)^2*time3+AA78^2*time4+((AB78-AC78)*2/PI()+AC78)^2*time5+AC78^2*time6+((AD78-AC78)*2/PI()+AC78)^2*time7+AE78^2*time8)/time)/(C78+(E78-C78)/G78*mspeed))))","v":0.85873621970291025},{"$f":"IF(move1,MAX(ABS(X78),ABS(Z78))/H78,MAX(ABS(X78),ABS(Z78),ABS(AB78),ABS(AD78))/H78)","v":0.97267570073089693},{"$f":"IF(AZ78>0,speed/(MIN(AZ78,I78)),\"NA\")","v":3.9459947685750722E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M78+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M78+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.737701965432098},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M78+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M78+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.277538591999999},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M78+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M78+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2369.2590399999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M78+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M78+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2381.2590399999999},9,{"$f":"AH78/Irms","v":0.26430873981526776},{"$f":"AI78/Ipeak","v":0.38977724809441566},{"$f":"IF(move1,IF(AccType=1,SQRT((X78^2*time1+Y78^2*time2+Z78^2*time3+AA78^2*time4)/time)/(C78/D78),SQRT((((X78-Y78)*2/PI()+Y78)^2*time1+Y78^2*time2+((Z78-AA78)*2/PI()+AA78)^2*time3+AA78^2*time4)/time)/(C78/D78)),IF(AccType=1,SQRT((X78^2*time1+Y78^2*time2+Z78^2*time3+AA78^2*time4+AB78^2*time5+AC78^2*time6+AD78^2*time7+AE78^2*time8)/time)/(C78/D78),SQRT((((X78-Y78)*2/PI()+Y78)^2*time1+Y78^2*time2+((Z78-AA78)*2/PI()+AA78)^2*time3+AA78^2*time4+((AB78-AC78)*2/PI()+AC78)^2*time5+AC78^2*time6+((AD78-AE78)*2/PI()+AE78)^2*time7+AE78^2*time8)/time)/(C78/D78)))","v":6.3434097555664266},{"$f":"IF(move1,MAX(ABS(X78),ABS(Z78))/(C78/D78),MAX(ABS(X78),ABS(Z78),ABS(AB78),ABS(AD78))/(C78/D78))","v":18.709307908531951},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X78),ABS(Z78))/(C78/D78),MAX(ABS((X78-Y78)*2/PI()+Y78),ABS((Z78-Y78)*2/PI()+Y78))/(C78/D78)),IF(AccType=1,MAX(ABS(X78),ABS(Z78),ABS(AB78),ABS(AD78))/(C78/D78),MAX(ABS((X78-Y78)*2/PI()+Y78),ABS((Z78-Y78)*2/PI()+Y78),ABS((AB78-AC78)*2/PI()+AC78),ABS((AD78-AC78)*2/PI()+AC78))/(C78/D78)))","v":14.000622350547733},{"$f":"IF((C78+(E78-C78)/G78*mspeed)<0,\"NA\",U78*(C78+(E78-C78)/G78*mspeed)*mspeed/9.55)","v":23.060826574487265},{"$f":"IF(move1,IF(speed1>speed2,AM78/2*time1/time,AM78/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z78*-speed/30*PI(),((Z78-AA78)*2/PI()+AA78)*-speed/30*PI()),IF(AccType=1,X78*-speed/30*PI(),((X78-Y78)*2/PI()+Y78)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z78*-speed/30*PI(),((Z78-AA78)*2/PI()+AA78)*-speed/30*PI()),IF(AccType=1,X78*-speed/30*PI(),((X78-Y78)*2/PI()+Y78)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD78*-speed/30*PI(),((AD78-AE78)*2/PI()+AE78)*-speed/30*PI()),IF(AccType=1,AB78*-speed/30*PI(),((AB78-AC78)*2/PI()+AC78)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD78*-speed/30*PI(),((AD78-AE78)*2/PI()+AE78)*-speed/30*PI()),IF(AccType=1,AB78*-speed/30*PI(),((AB78-AC78)*2/PI()+AC78)*-speed/30*PI()),0)/2*time7/time)))","v":2.4387820412655792},{"$f":"IF(move1,MAX(IF(AccType=1,Z78*-speed/30*PI(),((Z78-AA78)*2/PI()+AA78)*-speed/30*PI()),IF(AccType=1,X78*-speed/30*PI(),((X78-Y78)*2/PI()+Y78)*-speed/30*PI()),0),MAX(IF(AccType=1,Z78*-speed/30*PI(),((Z78-AA78)*2/PI()+AA78)*-speed/30*PI()),IF(AccType=1,X78*-speed/30*PI(),((X78-Y78)*2/PI()+Y78)*-speed/30*PI()),IF(AccType=1,AD78*-speed/30*PI(),((AD78-AE78)*2/PI()+AE78)*-speed/30*PI()),IF(AccType=1,AB78*-speed/30*PI(),((AB78-AC78)*2/PI()+AC78)*-speed/30*PI()),0))","v":149.39798134271362},{"$f":"(L78^2)/1000000+((K78/1000)^2*(D78/C78*H78)^2*PI()*PI()*(O78/2)^2)/1200","v":1.6433923805160251E-2},{"$f":"SQRT(3)*L78*J78*D78/C78*H78/1000","v":5.563605810934404},{"$f":"0.75*J78^2*(D78/C78*H78)^2-(UAC_V*0.98)^2","v":-152899.36046100478},{"$f":"-AO78/2/AN78+SQRT((AO78/2/AN78)^2-AP78/AN78)","v":2885.6485411114072},{"$f":"(L78^2)/1000000+((K78/1000)^2*AV78^2*PI()*PI()*(O78/2)^2)/1200","v":1.0635727895110357E-2},{"$f":"SQRT(3)*L78*J78*AV78/1000","v":1.5895630008966293},{"$f":"0.75*J78^2*AV78^2-(UAC_V*0.98)^2","v":-153601.58348186675},{"$f":"-AS78/2/AR78+SQRT((AS78/2/AR78)^2-AT78/AR78)","v":3726.2752390275537},{"$f":"D78+(F78-D78)*((0.85*UAC_V-D78*J78)/L78*1000)/G78","v":5.4955485548248966},{"$f":"(L78^2)/1000000+((K78/1000)^2*AJ78^2*PI()*PI()*(O78/2)^2)/1200","v":1.3465312418542546E-2},{"$f":"SQRT(3)*L78*J78*AJ78/1000","v":4.0496178053814278},{"$f":"0.75*J78^2*AJ78^2-(UAC_V*0.98)^2","v":-153258.89078526697},{"$f":"IF(((AX78/2/AW78)^2-AY78/AW78)>0,-AX78/2/AW78+SQRT((AX78/2/AW78)^2-AY78/AW78),-9999)","v":3226.6630327919538}]
["AKM","AKM53K",11.6,9.4,7.65,6.1693548387096779,4000,30.3,6000,1,5.7,79.8,0.91,640,10,3679.2827027752969,4757.1998320791017,4912.2807017543864,6.9022651658218876,123.62637362637362,0.85735884742692936,0.96625539907590752,3.0957886486721251E-2,-22.737701965432098,9,29.277538591999999,9,-2369.2590399999999,7.5,2381.2590399999999,9,0.33516466619724516,0.49426879088505743,8.043951988733884,23.724901962482758,17.753911277980219,23.060826574487265,2.4387820412655792,149.39798134271362,1.0395518262749932E-2,3.393720029201643,-153211.84613332342,3679.2827027752969,6.6128839719463038E-3,0.83676617679151433,-153636.51204316312,4757.1998320791017,6.0539746543778801,8.4737390918954228E-3,2.4539039740492403,-153427.59897575021,4112.8115941677497]
["AKM","AKM53L",11.6,11.8,5.0599999999999996,5.1111111111111107,5500,30.3,6000,0.69,3.64,63.6,0.91,640,10,4634.4467310333521,6000,6000,4.4654545454545449,123.62637362637362,0.85769016390588371,0.96625539907590752,2.4590918939936316E-2,-22.737701965432098,9,29.277538591999999,9,-2369.2590399999999,7.5,2381.2590399999999,9,0.42073862352420144,0.62046507791954031,10.097726964580835,29.782323740137933,22.286824795762403,23.060826574487265,2.4387820412655792,149.39798134271362,6.6331405457381084E-3,2.3427906404115633,-153324.77118285472,4634.4467310333521,4.1260044331513949E-3,0.41456992272785331,-153653.3776316187,6052.445958464883,5.4541987167270189,5.3981465522971086E-3,1.6940063450737042,-153486.63993357474,5177.6818420046402]
["AKM","AKM53M",11.4,13.4,8.7200000000000006,10.258823529411766,3000,29.7,6000,0.51,2.7,54.7,0.91,640,10,5470.2336881088086,6000,6000,6.0400000000000009,123.62637362637362,0.87226903204868067,0.98577571016835019,2.1220659078919377E-2,-22.737701965432098,9,29.277538591999999,9,-2369.2590399999999,7.5,2381.2590399999999,9,0.48617017276688873,0.71695726815204674,11.668084146405329,34.413948871298246,25.752780599563689,23.060826574487265,2.4387820412655792,149.39798134271362,4.8189229196541833E-3,1.6868424673960098,-153426.25334884558,5470.2336881088086,3.0660131557956704E-3,0.33932461185993723,-153654.37953468863,7024.1007206573886,7.0225886654478993,3.9861996557911073E-3,1.2443491563525497,-153534.62514639305,6052.0498888571783]
["AKM","AKM53P",11.4,19.100000000000001,5.88,9.8000000000000007,5000,29.8,6000,0.27,1.3,38.4,0.91,640,10,6000,6000,6000,4.7759999999999998,123.62637362637362,0.87262742062984089,0.98246773798657716,2.1220659078919377E-2,-22.737701965432098,9,29.277538591999999,9,-2369.2590399999999,7.5,2381.2590399999999,9,0.69297390297369965,1.0219316284853801,16.631373671368792,49.052718167298245,36.707321600870635,23.060826574487265,2.4387820412655792,149.39798134271362,2.3407930957715564E-3,0.89660342984776231,-153527.70549343282,7909.3829082916436,1.4774443266862961E-3,5.1737475487673504E-2,-153663.54617540658,10180.854763169866,2.8810421874999967,1.9427806959828567E-3,0.65918651236105674,-153590.32940367318,8723.3659819453751]
["AKM","AKM53Q",11.57,21.1,4.99,9.0727272727272723,5500,30.1,6000,0.25,1.1299999999999999,35.5,0.91,640,10,6000,6000,6000,4.3918181818181816,123.62637362637362,0.85993118185457207,0.97267570073089693,2.1220659078919377E-2,-22.737701965432098,9,29.277538591999999,9,-2369.2590399999999,7.5,2381.2590399999999,9,0.75428845416831625,1.1123524637914146,18.102922900039591,53.392918261987901,39.955197083418582,23.060826574487265,2.4387820412655792,149.39798134271362,2.0513776781260016E-3,0.84380983120192254,-153522.75520110433,8447.7206864902091,1.2603107842633526E-3,7.3963400616641108E-3,-153663.98914781862,11039.052904442013,0.4811581888022296,1.6793927412455446E-3,0.61418932845231566,-153589.16791684492,9382.1078051357636]
["AKM","AKM54G",14.3,5,12.9,4.479166666666667,1500,38,6000,3.8,22.9,185,1.2,640,10,1542.9097861289117,1983.3635746177656,2118.9189189189192,12.448860663690086,93.75,0.69553018081192353,0.77202793263157898,6.9564670351728794E-2,-22.81118696296296,9,29.337061440000003,9,-2375.3328000000001,7.5,2387.3328000000001,9,0.14469229750708062,0.21370237062937061,3.472615140169935,10.25771379020979,7.6737676309644458,23.07267516827395,2.4489643392487652,150.02174137472068,5.3260513626125494E-2,16.178323522166078,-151752.10699789721,1542.9097861289117,3.6310189923463368E-2,5.3545629028155357,-153454.5672470401,1983.3635746177656,4.3975225225225225,4.057460575772473E-2,9.3438228618824386,-153026.25693444678,1830.2962384461594]
["AKM","AKM54H",14.19,5.5,12.6,4.9027237354085607,1800,37.5,6000,3.2,18.3,165.6,1.2,640,10,1750.9968557943478,2223.3202232072504,2367.1497584541066,12.226067136166929,93.75,0.70087489628804789,0.78232163840000013,6.1912962645045873E-2,-22.81118696296296,9,29.337061440000003,9,-2375.3328000000001,7.5,2387.3328000000001,9,0.16039533754660876,0.23689487596899228,3.8494881011186104,11.370954046511629,8.5065796219218281,23.07267516827395,2.4489643392487652,150.02174137472068,4.1970707427209458E-2,13.340819243414236,-152041.50135208221,1750.9968557943478,2.9045763662841409E-2,4.4552292222160901,-153483.04964032045,2223.3202232072504,4.8539926606807571,3.2406127581612897E-2,7.8077501887649845,-153108.26063208375,2056.4991406319728]
["AKM","AKM54I",14.42,7.7,11.71,6.262032085561497,2500,38,6000,1.66,9.84,120.3,1.2,640,10,2446.1462597271393,3107.539310903348,3258.5203657522861,11.051427386980771,93.75,0.68989396512532453,0.77202793263157898,4.4360885515287871E-2,-22.81118696296296,9,29.337061440000003,9,-2375.3328000000001,7.5,2387.3328000000001,9,0.22097182910547367,0.32636294077669908,5.3033238985313682,15.665421157281557,11.71925872185153,23.07267516827395,2.4489643392487652,150.02174137472068,2.2669314467464279E-2,7.0184854537385366,-152813.06661608067,2446.1462597271393,1.5221545731142351E-2,2.1221837406640667,-153586.20087373111,3107.539310903348,6.1354813465445117,1.720640779663344E-2,4.0535402044952553,-153380.1573036538,2870.185141584634]
["AKM","AKM54K",14.4,9.6999999999999993,10.050000000000001,6.7,3500,38.4,6000,1.02,6.2,96.6,1.2,640,10,3089.0347210568953,3921.7864051636343,4057.971014492754,9.5257797535823414,93.75,0.69102316507150663,0.76398597500000009,3.5238640646765733E-2,-22.81118696296296,9,29.337061440000003,9,-2375.3328000000001,7.5,2387.3328000000001,9,0.27875373037787715,0.41170355319444446,6.6900895290690521,19.761770553333335,14.783726501264978,23.07267516827395,2.4489643392487652,150.02174137472068,1.4619942021052778E-2,4.4144681937662735,-153141.91340799999,3089.0347210568953,9.6939187476629222E-3,1.1555436545243545,-153628.22674404088,3921.7864051636343,6.7709316770186341,1.1059026865865549E-2,2.5230266916948638,-153493.45874840315,3613.1914323772953]
["AKM","AKM54L",14.1,12.5,8.1300000000000008,7.1946902654867273,4500,37.5,6000,0.63,3.5,72.900000000000006,1.2,640,10,4191.1526245603,5261.5126690874258,5377.2290809327842,7.1197265256773496,93.75,0.70584785845637843,0.78232163840000013,2.6374077081862131E-2,-22.81118696296296,9,29.337061440000003,9,-2375.3328000000001,7.5,2387.3328000000001,9,0.36686167630341376,0.54183402482269516,8.8046802312819299,26.008033191489368,19.456538496948866,23.07267516827395,2.4489643392487652,150.02174137472068,8.0982157841559786E-3,2.6445444627398884,-153335.00696900464,4191.1526245603,5.4424147345853695E-3,0.56708012118711959,-153648.87226880097,5261.5126690874258,7.1287883079554319,6.2679210977589208E-3,1.5477267288774428,-153551.31307768493,4827.6174395910502]
["AKM","AKM54N",14.1,17.8,9.85,12.3125,3500,37.6,6000,0.33,1.8,51.3,1.2,640,10,5928.0329540318617,6000,6000,6.8142857142857149,93.75,0.70572280551536792,0.78024099574468087,2.1220659078919377E-2,-22.81118696296296,9,29.337061440000003,9,-2375.3328000000001,7.5,2387.3328000000001,9,0.52241102705606113,0.77157165134751793,12.537864649345467,37.035439264680861,27.706110819655184,23.07267516827395,2.4489643392487652,150.02174137472068,4.1326910200517528E-3,1.391812289492631,-153479.97932799999,5928.0329540318617,2.6700509077212534E-3,0.22250235441060048,-153659.29700518315,7544.5670948249599,7.5882683096630466,3.1430828506165036E-3,0.81239548173119736,-153601.30393599387,6862.6408556823471]
["AKM","AKM54P",14.36,19.600000000000001,9.23,12.472972972972974,4000,38,6000,0.3,1.5,47.3,1.2,640,10,6000,6000,6000,6.6650000000000009,93.75,0.69299424979345259,0.77202793263157898,2.1220659078919377E-2,-22.81118696296296,9,29.337061440000003,9,-2375.3328000000001,7.5,2387.3328000000001,9,0.56482391567248702,0.83421309805013955,13.555773976139688,40.042228706406696,29.955481777252302,23.07267516827395,2.4489643392487652,150.02174137472068,3.4818375157741363E-3,1.2747594815155212,-153482.4174005478,6458.8070869301846,2.260049635548665E-3,0.17238725785895609,-153660.67931217319,8207.5525919460797,7.0139414890577676,2.6524291040521098E-3,0.73623986876431169,-153603.43016502575,7472.3727413959696]
["AKM","AKM62G",11.9,4.9000000000000004,10.199999999999999,4.1295546558704448,2000,29.7,6000,3.94,31.7,159,1.7,640,10,1530.5459395571854,2232.2768881425513,2465.4088050314463,10.002564645078831,66.17647058823529,0.83666177166187705,0.99123525387205391,7.1202075215912541E-2,-22.937885234567901,9,29.439687039999999,9,-2385.8048000000003,7.5,2397.8048000000003,9,0.17054774684983212,0.25254633490196082,4.0931459243959711,12.122224075294119,9.0638919043932855,23.093160481295573,2.466520025426675,151.09718970576742,5.6183112435973279E-2,13.269652242253271,-151922.73511104845,1530.5459395571854,2.8793444999086145E-2,4.4737346727499423,-153466.08158377669,2232.2768881425513,4.1230276755022528,4.2255870410040502E-2,9.834871525038249,-152707.5040355009,1788.205667986786]
["AKM","AKM62H",11.9,5.4,10.199999999999999,4.6363636363636358,2000,29.6,6000,3.3,25.4,142.1,1.7,640,10,1737.6439516429318,2508.7794925097396,2758.6206896551726,9.7675374313667209,66.17647058823529,0.83666177166187705,0.99458402162162152,6.301852100698227E-2,-22.937885234567901,9,29.439687039999999,9,-2385.8048000000003,7.5,2397.8048000000003,9,0.18795057816103947,0.27831636907563023,4.5108138758649474,13.359185715630252,9.9887788334130061,23.093160481295573,2.466520025426675,151.09718970576742,4.4125730697427104E-2,10.90955797792377,-152190.44563881081,1737.6439516429318,2.2919810107046523E-2,3.6828166772736752,-153496.07627669995,2508.7794925097396,4.5343125839677558,3.3428226449461709E-2,8.1129919016525616,-152849.08194915464,2020.4211783930814]
["AKM","AKM62I",12.1,7.6,9.4,5.875,3000,30.1,6000,1.75,13.4,103.2,1.7,640,10,2410.7158486823732,3519.7778249145999,3798.4496124031007,8.9321999575768611,66.17647058823529,0.82288662291024528,0.97806269235880394,4.5118231484954807E-2,-22.937885234567901,9,29.439687039999999,9,-2385.8048000000003,7.5,2397.8048000000003,9,0.26015075434472623,0.38523006457300274,6.2436181042734296,18.491043099504132,13.825913034800617,23.093160481295573,2.466520025426675,151.09718970576742,2.3846702861050575E-2,5.9138879387393235,-152843.03092906906,2410.7158486823732,1.1883578476056731E-2,1.8079460263612812,-153587.27241371473,3519.7778249145999,5.7797238372093025,1.7707818971275675E-2,4.3248614010170074,-153224.93885823214,2822.0067649587263]
["AKM","AKM62K",12.2,9.6,9,7.03125,3500,30.2,6000,1.05,8.5,82.1,1.7,640,10,3066.9569154043065,4490.5075455142915,4774.6650426309388,8.0943931012440764,66.17647058823529,0.8161518306811556,0.97482407417218542,3.5488096985194721E-2,-22.937885234567901,9,29.439687039999999,9,-2385.8048000000003,7.5,2397.8048000000003,9,0.32591794245775885,0.48261782032786887,7.8220306189862123,23.165655375737707,17.321161110034943,23.093160481295573,2.466520025426675,151.09718970576742,1.5129851500929416E-2,3.5482272660728231,-153197.04336339692,3066.9569154043065,7.3975089640431133E-3,0.99302525796813423,-153627.42584638906,4490.5075455142915,6.6506977553506177,1.1197489308486628E-2,2.5862475054985086,-153415.91879426854,3587.7932402696752]
["AKM","AKM62L",12.2,12,7.42,7.42,5000,30.1,6000,0.74,5.4,65.5,1.7,640,10,3879.3877272231175,5702.7361861879999,5984.7328244274813,6.7481842060042725,66.17647058823529,0.81621385046628891,0.97806269235880394,2.815208394811412E-2,-22.937885234567901,9,29.439687039999999,9,-2385.8048000000003,7.5,2397.8048000000003,9,0.40739742807219859,0.60327227540983608,9.7775382737327661,28.957069219672132,21.651451387543677,23.093160481295573,2.466520025426675,151.09718970576742,9.5458445014414244E-3,2.4855445864428112,-153304.00163794679,3879.3877272231175,4.6158672263270223E-3,0.61867749659380999,-153641.69583096605,5702.7361861879999,7.369375267175573,7.1009859999020351E-3,1.8176935298345906,-153471.46985791024,4522.718627444473]
["AKM","AKM62M",12.2,13.4,5.7,6.2637362637362637,6000,30.2,6000,0.55000000000000004,4.4000000000000004,58.8,1.7,640,10,4307.3831595589945,6000,6000,5.6999999999999993,66.17647058823529,0.81640322488226447,0.97482407417218542,2.5281758371440196E-2,-22.937885234567901,9,29.439687039999999,9,-2385.8048000000003,7.5,2397.8048000000003,9,0.45492712801395507,0.67365404087431691,10.918251072334922,32.335393961967213,24.177454049423773,23.093160481295573,2.466520025426675,151.09718970576742,7.8373751697600261E-3,1.8580292799096325,-153414.37362868182,4307.3831595589945,3.634630380112316E-3,0.37371349636986484,-153653.90135928831,6450.7138541888753,6.6717250380005479,5.7843789762700628E-3,1.3542885587562734,-153531.38038112171,5036.1985350413406]
["AKM","AKM62P",12.3,18.8,8.1,12.272727272727272,4500,30.3,6000,0.3,2.2000000000000002,42.2,1.7,640,10,6000,6000,6000,6.6999999999999993,66.17647058823529,0.80953334826408951,0.97160683300330031,2.1220659078919377E-2,-22.937885234567901,9,29.439687039999999,9,-2385.8048000000003,7.5,2397.8048000000003,9,0.63306689771435942,0.93744260899728993,15.193605545144626,44.997245231869918,33.644829879722337,23.093160481295573,2.466520025426675,151.09718970576742,3.9153323484014315E-3,1.01552284900959,-153519.22468935157,6133.4267666518845,1.8339799036267734E-3,0.16023330087606663,-153660.39570220941,9109.8459205180425,7.30732538656709,2.9073642450630111E-3,0.73775586330832266,-153587.5917160096,7142.4548873810409]
["AKM","AKM62Q",12,21.8,6.5,10.833333333333334,5500,40.9,6000,0.27,1.6,35.5,1.7,640,10,5920.9407814656306,6000,6000,6,66.17647058823529,0.82990913276488232,0.71979674914425429,2.1220659078919377E-2,-22.937885234567901,9,29.439687039999999,9,-2385.8048000000003,7.5,2397.8048000000003,9,0.75244041645890214,1.1142103775555554,18.058569995013652,53.482098122666663,39.989027854382748,23.093160481295573,2.466520025426675,151.09718970576742,4.1662498293124628E-3,1.2335344989093444,-153362.15366792312,5920.9407814656306,1.2650944942092632E-3,5.0364871295226675E-2,-153663.49680217009,11001.185249100869,3.0337164319248799,2.1019942651195108E-3,0.66388612327531238,-153576.56798558272,8391.1901908322452]
["AKM","AKM63G",16.5,4.5,14.6,3.9459459459459456,1500,42.1,6000,5.16,43.5,238,2.4,640,10,1075.1638421990701,1495.1215460505139,1647.0588235294117,14.606179375002682,46.875,0.60423481747979857,0.70269270498812353,9.2121723816307788E-2,-23.115262814814812,9,29.583362880000003,9,-2400.4656,7.5,2412.4656,9,0.11310106971613783,0.16808728909090911,{"$f":"IF(move1,IF(AccType=1,SQRT((X99^2*time1+Y99^2*time2+Z99^2*time3+AA99^2*time4)/time)/(C99/D99),SQRT((((X99-Y99)*2/PI()+Y99)^2*time1+Y99^2*time2+((Z99-AA99)*2/PI()+AA99)^2*time3+AA99^2*time4)/time)/(C99/D99)),IF(AccType=1,SQRT((X99^2*time1+Y99^2*time2+Z99^2*time3+AA99^2*time4+AB99^2*time5+AC99^2*time6+AD99^2*time7+AE99^2*time8)/time)/(C99/D99),SQRT((((X99-Y99)*2/PI()+Y99)^2*time1+Y99^2*time2+((Z99-AA99)*2/PI()+AA99)^2*time3+AA99^2*time4+((AB99-AC99)*2/PI()+AC99)^2*time5+AC99^2*time6+((AD99-AE99)*2/PI()+AE99)^2*time7+AE99^2*time8)/time)/(C99/D99)))","v":2.714425673187308},8.0681898763636379,6.0283024885158891,23.121960184623759,2.4910979860757463,152.60281736923275,0.10793702977506395,24.422940501125932,-151031.41745497522,1075.1638421990701,6.2895321268656657E-2,8.5261836807535261,-153343.15486124766,1495.1215460505139,4.0083662654250887,7.0783273472849628E-2,12.822783871717677,-152938.31066741058,1382.1273549700643]
["AKM","AKM63H",16.600000000000001,5.6,14.6,4.8666666666666663,1500,58.9,6000,3.43,28.1,191.5,2.4,640,10,{"$f":"IF(AQ100<I100,IF(AQ100<0,0,AQ100),I100)","v":1113.7527104123913},{"$f":"IF(AU100<I100,IF(AU100<0,0,AU100),I100)","v":1883.2086348252308},{"$f":"IF(UAC_V*0.98/L100*1000<I100,IF(UAC_V*0.98/L100*1000<0,0,UAC_V*0.98/L100*1000),I100)","v":2046.9973890339427},{"$f":"C100+(E100-C100)/G100*Q100","v":14.089055153566358},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M100,(inertia/gear^2+gear_inertia)/M100),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M100,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M100))","v":46.875},{"$f":"IF((C100+(E100-C100)/G100*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X100^2*time1+Y100^2*time2+Z100^2*time3+AA100^2*time4)/time)/(C100+(E100-C100)/G100*mspeed),SQRT((((X100-Y100)*2/PI()+Y100)^2*time1+Y100^2*time2+((Z100-Y100)*2/PI()+Y100)^2*time3+AA100^2*time4)/time)/(C100+(E100-C100)/G100*mspeed)),IF(AccType=1,SQRT((X100^2*time1+Y100^2*time2+Z100^2*time3+AA100^2*time4+AB100^2*time5+AC100^2*time6+AD100^2*time7+AE100^2*time8)/time)/(C100+(E100-C100)/G100*mspeed),SQRT((((X100-Y100)*2/PI()+Y100)^2*time1+Y100^2*time2+((Z100-Y100)*2/PI()+Y100)^2*time3+AA100^2*time4+((AB100-AC100)*2/PI()+AC100)^2*time5+AC100^2*time6+((AD100-AC100)*2/PI()+AC100)^2*time7+AE100^2*time8)/time)/(C100+(E100-C100)/G100*mspeed))))","v":0.6006422843010093},{"$f":"IF(move1,MAX(ABS(X100),ABS(Z100))/H100,MAX(ABS(X100),ABS(Z100),ABS(AB100),ABS(AD100))/H100)","v":0.50226422546689309},{"$f":"IF(AZ100>0,speed/(MIN(AZ100,I100)),\"NA\")","v":7.3161653870713592E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M100+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M100+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-23.115262814814812},{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M100+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M100+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.583362880000003},{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M100+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M100+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2400.4656},{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M100+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M100+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2412.4656},{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},{"$f":"AH100/Irms","v":0.13990011836373673},{"$f":"AI100/Ipeak","v":0.20791520096385541},3.3576028407296814,{"$f":"IF(move1,MAX(ABS(X100),ABS(Z100))/(C100/D100),MAX(ABS(X100),ABS(Z100),ABS(AB100),ABS(AD100))/(C100/D100))","v":9.9799296462650595},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X100),ABS(Z100))/(C100/D100),MAX(ABS((X100-Y100)*2/PI()+Y100),ABS((Z100-Y100)*2/PI()+Y100))/(C100/D100)),IF(AccType=1,MAX(ABS(X100),ABS(Z100),ABS(AB100),ABS(AD100))/(C100/D100),MAX(ABS((X100-Y100)*2/PI()+Y100),ABS((Z100-Y100)*2/PI()+Y100),ABS((AB100-AC100)*2/PI()+AC100),ABS((AD100-AC100)*2/PI()+AC100))/(C100/D100)))","v":7.4566954476421428},{"$f":"IF((C100+(E100-C100)/G100*mspeed)<0,\"NA\",U100*(C100+(E100-C100)/G100*mspeed)*mspeed/9.55)","v":23.121960184623759},{"$f":"IF(move1,IF(speed1>speed2,AM100/2*time1/time,AM100/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z100*-speed/30*PI(),((Z100-AA100)*2/PI()+AA100)*-speed/30*PI()),IF(AccType=1,X100*-speed/30*PI(),((X100-Y100)*2/PI()+Y100)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z100*-speed/30*PI(),((Z100-AA100)*2/PI()+AA100)*-speed/30*PI()),IF(AccType=1,X100*-speed/30*PI(),((X100-Y100)*2/PI()+Y100)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD100*-speed/30*PI(),((AD100-AE100)*2/PI()+AE100)*-speed/30*PI()),IF(AccType=1,AB100*-speed/30*PI(),((AB100-AC100)*2/PI()+AC100)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD100*-speed/30*PI(),((AD100-AE100)*2/PI()+AE100)*-speed/30*PI()),IF(AccType=1,AB100*-speed/30*PI(),((AB100-AC100)*2/PI()+AC100)*-speed/30*PI()),0)/2*time7/time)))","v":2.4910979860757463},{"$f":"IF(move1,MAX(IF(AccType=1,Z100*-speed/30*PI(),((Z100-AA100)*2/PI()+AA100)*-speed/30*PI()),IF(AccType=1,X100*-speed/30*PI(),((X100-Y100)*2/PI()+Y100)*-speed/30*PI()),0),MAX(IF(AccType=1,Z100*-speed/30*PI(),((Z100-AA100)*2/PI()+AA100)*-speed/30*PI()),IF(AccType=1,X100*-speed/30*PI(),((X100-Y100)*2/PI()+Y100)*-speed/30*PI()),IF(AccType=1,AD100*-speed/30*PI(),((AD100-AE100)*2/PI()+AE100)*-speed/30*PI()),IF(AccType=1,AB100*-speed/30*PI(),((AB100-AC100)*2/PI()+AC100)*-speed/30*PI()),0))","v":152.60281736923275},{"$f":"(L100^2)/1000000+((K100/1000)^2*(D100/C100*H100)^2*PI()*PI()*(O100/2)^2)/1200","v":0.10077277925241421},{"$f":"SQRT(3)*L100*J100*D100/C100*H100/1000","v":22.605741624347555},{"$f":"0.75*J100^2*(D100/C100*H100)^2-(UAC_V*0.98)^2","v":-150180.30623709506},{"$f":"-AO100/2/AN100+SQRT((AO100/2/AN100)^2-AP100/AN100)","v":1113.7527104123913},{"$f":"(L100^2)/1000000+((K100/1000)^2*AV100^2*PI()*PI()*(O100/2)^2)/1200","v":4.0383456661222394E-2},{"$f":"SQRT(3)*L100*J100*AV100/1000","v":5.4393314200120653},{"$f":"0.75*J100^2*AV100^2-(UAC_V*0.98)^2","v":-153462.30576050875},{"$f":"-AS100/2/AR100+SQRT((AS100/2/AR100)^2-AT100/AR100)","v":1883.2086348252308},{"$f":"D100+(F100-D100)*((0.85*UAC_V-D100*J100)/L100*1000)/G100","v":4.7810357992457204},{"$f":"(L100^2)/1000000+((K100/1000)^2*AJ100^2*PI()*PI()*(O100/2)^2)/1200","v":4.5699676457772342E-2},{"$f":"SQRT(3)*L100*J100*AJ100/1000","v":8.4833997361449764},{"$f":"0.75*J100^2*AJ100^2-(UAC_V*0.98)^2","v":-153173.38331379159},{"$f":"IF(((AX100/2/AW100)^2-AY100/AW100)>0,-AX100/2/AW100+SQRT((AX100/2/AW100)^2-AY100/AW100),-9999)","v":1740.3099538798656}]
["AKM","AKM63I",16.8,7.9,14.1,6.558139534883721,2000,42.5,6000,1.5,14.6,138.19999999999999,2.4,640,10,1948.7143759031096,2660.8755000922361,2836.4688856729381,13.20781807487548,46.875,0.59349225390534988,0.69607912658823534,5.1746443624364986E-2,-23.115262814814812,9,29.583362880000003,9,-2400.4656,7.5,2412.4656,9,0.19500958250659481,0.28981717107142863,4.6802299801582752,13.911224211428575,10.394037425635531,23.121960184623759,2.4910979860757463,152.60281736923275,3.6604868140016109E-2,7.1757395807340005,-152990.00409060108,1948.7143759031096,2.0842638915594024E-2,2.2645202332964671,-153596.87623110908,2660.8755000922361,6.3069048059771813,2.3834379434313411E-2,3.7320220900885346,-153481.68922636571,2460.5353635078673]
["AKM","AKM63K",16.8,9.9,12.9,7.5438596491228074,3000,42.6,6000,1.0900000000000001,9.3000000000000007,110,2.4,640,10,2453.5864401508552,3363.3225025372976,3563.6363636363635,12.427680746701514,46.875,0.59345299839398979,0.6944451380281691,4.1092786154998014E-2,-23.115262814814812,9,29.583362880000003,9,-2400.4656,7.5,2412.4656,9,0.2443790970652264,0.36318860678571435,5.8650983295654333,17.433053125714288,13.02543930554326,23.121960184623759,2.4910979860757463,152.60281736923275,2.3307156305910369E-2,5.2133312737698443,-153102.4540708664,2453.5864401508552,1.3113588367529091E-2,1.5678280016797999,-153613.21312721382,3363.3225025372976,7.5495072461456676,1.5117235189859432E-2,2.7050306479058612,-153512.8183717746,3098.4502728353009]
["AKM","AKM63L",16.8,11.1,12.9,8.6,3000,42.6,6000,0.94,7.4,98.2,2.4,640,10,2753.5495828090484,3776.5259347924489,3991.8533604887984,11.890516284769816,46.875,0.59345299839398979,0.6944451380281691,3.6644777244259658E-2,-23.115262814814812,9,29.583362880000003,9,-2400.4656,7.5,2412.4656,9,0.27400080580040531,0.40721146821428572,6.5760193392097275,19.546150474285714,14.604280433487897,23.121960184623759,2.4910979860757463,152.60281736923275,1.8563315695493826E-2,4.5001114006895717,-153138.99485083291,2753.5495828090484,1.0419524396246145E-2,1.3275455257732454,-153618.31055529573,3776.5259347924489,8.3032756279701285,1.2044738252546015E-2,2.3349636956896114,-153522.65602587437,3474.5457347120687]
["AKM","AKM63M",17,13.8,11.3,9.112903225806452,4000,43,6000,0.57999999999999996,4.9000000000000004,79.900000000000006,2.4,640,10,3405.6891600084591,4708.5761617722201,4906.1326658322905,10.290278969474588,46.875,0.58655518179439914,0.68798518325581404,2.9614087817180876E-2,-23.115262814814812,9,29.583362880000003,9,-2400.4656,7.5,2412.4656,9,0.3366420075080338,0.50030687223529424,8.0794081801928108,24.014729867294122,17.943065054053175,23.121960184623759,2.4910979860757463,152.60281736923275,1.2399180047754694E-2,2.8017799355501998,-153356.59247685812,3405.6891600084591,6.7777971165028606E-3,0.71687067953979677,-153643.87536159938,4708.5761617722201,8.9311095724494329,7.9734492430186248E-3,1.4402305932966102,-153582.77111087437,4299.4386745773118]
["AKM","AKM63N",17,17.399999999999999,9.6,9.795918367346939,5000,43,6000,0.38,3.1,63.3,2.4,640,10,4310.2605344010881,6000,6000,8.120000000000001,46.875,0.58659736513061478,0.68798518325581404,2.3407290799480954E-2,-23.115262814814812,9,29.583362880000003,9,-2400.4656,7.5,2412.4656,9,0.42446166164056431,0.63082170847058827,10.187079879373544,30.279442006588237,22.623864633371394,23.121960184623759,2.4910979860757463,152.60281736923275,7.834427555449398E-3,1.8336511555129911,-153454.21906265744,4310.2605344010881,4.1811225452597182E-3,0.39122052060124202,-153654.45060534857,6015.5386358968235,9.3901751426637006,5.0182726120393236E-3,0.94257241908789935,-153608.56780912221,5439.4998363646428]
["AKM","AKM63Q",16.7,22.4,11.9,15.866666666666667,3500,51.9,6000,0.23,1.8,48.3,2.4,640,10,5134.1349563019303,6000,6000,8.4714285714285715,46.875,0.59706951278375064,0.57000699190751447,2.1220659078919377E-2,-23.115262814814812,9,29.583362880000003,9,-2400.4656,7.5,2412.4656,9,0.55624957241629469,0.82668079904191627,13.349989737991072,39.680678354011981,29.648178306792715,23.121960184623759,2.4910979860757463,152.60281736923275,5.5613939960747344E-3,1.3394746509512794,-153471.72857479981,5134.1349563019303,2.3924967303711369E-3,0.18200423141309269,-153660.45016050347,7976.1651824015753,9.4590144927536244,2.9184879476213382E-3,0.57047104745002597,-153629.12510062853,7158.2651905888733]
["AKM","AKM64K",20.8,9.1999999999999993,17.2,7.5438596491228074,2000,53.5,6000,1.34,11.8,147,3.2,640,10,1911.1360954584361,2521.7550490795084,2666.6666666666665,16.260840911656885,35.15625,0.48011100103674881,0.55602923065420562,5.2136791688784115E-2,-23.317980049382719,9,29.747563840000002,9,-2417.2208000000001,7.5,2429.2208000000001,9,0.18368919962176353,0.27411617320512821,4.4085407909223244,13.157576313846153,9.8229060670588684,23.155045327706091,2.5191870839604005,154.32353469890751,3.7640681324665193E-2,8.0734848541574209,-152909.90265988352,1911.1360954584361,2.3157428433020034E-2,2.5090947856108956,-153591.16510894557,2521.7550490795084,7.3541808807733622,2.4371501387050548E-2,3.3513728846184172,-153534.05761243284,2442.1133397225653]
["AKM","AKM64L",21,12.8,15.6,9.3975903614457827,3000,54.1,6000,0.71,6.2,107,3.2,640,10,2659.0242190585959,3508.5883769816028,3663.5514018691588,14.684540921433115,35.15625,0.47552980345295826,0.54986254787430688,3.7640958558771441E-2,-23.317980049382719,9,29.747563840000002,9,-2417.2208000000001,7.5,2429.2208000000001,9,0.25313360511023975,0.3777468424126984,6.0752065226457539,18.131848435809523,13.536493329677814,23.155045327706091,2.5191870839604005,154.32353469890751,2.0043443622275666E-2,4.339010427086941,-153252.89397575401,2659.0242190585959,1.2131511134601725E-2,1.2227472104991186,-153631.35280939855,3508.5883769816028,9.2925290395225772,1.2897285672019457E-2,1.7811845826261579,-153594.72280292198,3382.5906498825352]
["AKM","AKM64P",20.399999999999999,18.600000000000001,11.9,10.818181818181818,4500,52.9,6000,0.36,2.8,71,3.2,640,10,4058.0726763078769,5382.1452427566765,5521.1267605633802,10.233725652570723,35.15625,0.48959082902350498,0.56233580037807185,2.4903996322967956E-2,-23.317980049382719,9,29.747563840000002,9,-2417.2208000000001,7.5,2429.2208000000001,9,0.37865343962951764,0.56505789156862751,9.0876825511084238,27.122778795294121,20.248752659973018,23.155045327706091,2.5191870839604005,154.32353469890751,8.7911744302638373E-3,2.1353050426509146,-153437.87782061246,4058.0726763078769,5.2181170029784694E-3,0.46404951052371646,-153653.32047469664,5382.1452427566765,10.481968302745766,5.7019538271507282E-3,0.89643695622652031,-153624.14683512753,5112.5912814278126]
["AKM","AKM64Q",20,20.7,10.7,10.7,5000,53.2,6000,0.32,2.2999999999999998,64.400000000000006,3.2,640,10,4409.5635929286018,5959.9511279596954,6000,8.9144909019949665,35.15625,0.49938716872289929,0.55916473383458642,2.2665260048547718E-2,-23.317980049382719,9,29.747563840000002,9,-2417.2208000000001,7.5,2429.2208000000001,9,0.42983272711492665,0.64143184529999997,10.315985450758239,30.7887285744,22.985600196917755,23.155045327706091,2.5191870839604005,154.32353469890751,7.4451131528548041E-3,1.965388701719496,-153431.15592878079,4409.5635929286018,4.2638043904715556E-3,0.36931646416184166,-153655.77822453916,5959.9511279596954,10.346708074534165,4.7220397272852693E-3,0.82045038191971909,-153623.4236556995,5617.5818940879344]
["AKM","AKM65K",24.8,9.8000000000000007,20.2,7.9527559055118102,2000,64.5,6000,1.27,11.4,164,4,640,10,1757.6318587399739,2268.2367880064498,2390.2439024390242,19.583055387585162,28.125,0.40330788087775932,0.46374829147286822,5.6638364767005005E-2,-23.520697283950618,9,29.9117648,9,-2433.9760000000001,7.5,2445.9760000000001,9,0.16434520226069432,0.24624940779569895,3.9442848542566638,11.81997157419355,8.8171718096148357,23.18831233110085,2.5472761818450538,156.04425202858218,4.4255468722552524E-2,9.1948003961653946,-152878.15494566737,1757.6318587399739,2.8587133172281547E-2,2.8698750938934734,-153587.44416405275,2268.2367880064498,7.9552677069329736,2.8973432002552799E-2,3.1808083281648467,-153569.95681866707,2248.0160752749971]
["AKM","AKM65L",25,12.2,19.2,9.1428571428571423,2500,65.2,6000,0.9,7.6,133.19999999999999,4,640,10,2159.2982733589906,2812.4295435232948,2942.9429429429433,18.475163459025957,28.125,0.4000819342862299,0.4587693987730061,4.5905625703211821E-2,-23.520697283950618,9,29.9117648,9,-2433.9760000000001,7.5,2445.9760000000001,9,0.20295626284079862,0.30410294213333328,4.8709503081791672,14.596941222399998,10.888667358028833,23.18831233110085,2.5472761818450538,156.04425202858218,2.9765452640752227E-2,6.6065508090154328,-153048.99150062079,2159.2982733589906,1.8742963045082418E-2,1.9059937221749228,-153612.8112539768,2812.4295435232948,9.1793959673959673,1.9150345366793796E-2,2.2609038438878266,-153591.97293082345,2773.6024185072365]
["AKM","AKM65M",25,13.6,19.2,10.378378378378377,2500,65.2,6000,0.68,6.1,119,4,640,10,2435.7355566356487,3161.2328214022145,3294.1176470588234,17.66593985434686,28.125,0.4000819342862299,0.4587693987730061,4.0878793661214982E-2,-23.520697283950618,9,29.9117648,9,-2433.9760000000001,7.5,2445.9760000000001,9,0.22624632578974277,0.33900000106666667,5.4299118189538262,16.272000051199999,12.138186563048537,23.18831233110085,2.5472761818450538,156.04425202858218,2.3786231172236546E-2,4.9712201572687382,-153227.71319377102,2435.7355566356487,1.4928901732364403E-2,1.4041394334294648,-153629.19300281562,3161.2328214022145,10.018293127413125,1.5288264407211656E-2,1.7012585064878272,-153612.90402326995,3114.6700543249835]
["AKM","AKM65N",24.3,17.8,16,11.594202898550726,3500,63.7,6000,0.42,3.4,88.8,4,640,10,3313.4155964024908,4289.739450961998,4414.4144144144148,14.127189302004405,28.125,0.41165076183320948,0.4695724458398744,3.0425727829441123E-2,-23.520697283950618,9,29.9117648,9,-2433.9760000000001,7.5,2445.9760000000001,9,0.30464661999647641,0.45647240521262006,7.3115188799154343,21.910675450205762,16.344387014514037,23.18831233110085,2.5472761818450538,156.04425202858218,1.3060586687251463E-2,3.0142276167439537,-153375.95113634935,3313.4155964024908,8.1814992732512845E-3,0.72094817508400844,-153647.52132946427,4289.739450961998,11.160436050957792,8.5204105990482372E-3,1.0558239783085717,-153628.65751203574,4184.7463826424109]
["AKM","AKM65P",24.5,19.8,14.9,11.461538461538462,4000,64.099999999999994,6000,0.37,2.8,80.5,4,640,10,3645.9187093131204,4752.3299160556344,4869.5652173913049,13.094408201466479,28.125,0.40829370206802329,0.46664219656786277,2.7575000681803769E-2,-23.520697283950618,9,29.9117648,9,-2433.9760000000001,7.5,2445.9760000000001,9,0.33611023789292521,0.50361644816326534,8.0666457094302046,24.173589511836738,18.032420014132732,23.18831233110085,2.5472761818450538,156.04425202858218,1.0806273173548962E-2,2.6724855594309678,-153388.46359841953,3645.9187093131204,6.68192698962242E-3,0.57703096811029775,-153651.15463376575,4752.3299160556344,11.185126230291448,7.0044325988065414E-3,0.93027691989269501,-153630.61335798446,4617.3690417181015]
["AKM","AKM72K",29.7,9.3000000000000007,25.1,7.7708978328173384,1500,79.400000000000006,6000,1.22,20.7,208,6.5,640,10,1196.4723627929282,1745.5705577070012,1884.6153846153845,24.346916956365199,17.307692307692307,0.33837467762358259,0.38318504785894208,7.2248644855661237E-2,-24.15418864197531,9,30.424892800000002,9,-2486.3359999999998,7.5,2498.3359999999998,9,0.13081981635735002,0.19847888821548823,3.1396755925764004,9.5269866343434355,7.0891396131051607,23.293435258959583,2.6350546127345957,161.42149368381561,9.7725951898429461E-2,10.927751102046958,-152973.95894884726,1196.4723627929282,4.8473190300428938E-2,3.3796311562605754,-153597.99878217242,1745.5705577070012,7.6892771036754795,4.769178227848004E-2,3.1158555979311737,-153607.8993383231,1762.3023203810233]
["AKM","AKM72L",30,11.5,24.3,9.3461538461538467,1800,79.5,6000,0.92,13.6,168.5,6.5,640,10,1487.1406142257499,2166.7632357423913,2326.4094955489613,23.138583086815764,17.307692307692307,0.33500807066074284,0.38270305408805033,5.8406917746043584E-2,-24.15418864197531,9,30.424892800000002,9,-2486.3359999999998,7.5,2498.3359999999998,9,0.16014877518585269,0.24297657444444445,3.8435706044604645,11.662875573333334,8.6784789779787364,23.293435258959583,2.6350546127345957,161.42149368381561,6.3712498734618539E-2,8.1826141808697521,-153074.44497325001,1487.1406142257499,3.1583717479085685E-2,2.4596618729176156,-153610.7289794831,2166.7632357423913,9.1606660072535444,3.1256583328637642E-2,2.3301934422834729,-153616.18940486875,2179.946475298143]
["AKM","AKM72M",30,13,23.6,10.128755364806867,2000,79.8,6000,0.64,10.8,150,6.5,640,10,1675.4404289009753,2455.4908624892782,2613.3333333333335,22.142429240034311,17.307692307692307,0.33501634856452578,0.38126432080200506,5.1844350264029927E-2,-24.15418864197531,9,30.424892800000002,9,-2486.3359999999998,7.5,2498.3359999999998,9,0.18103774586226828,0.27466917111111117,4.3449059006944388,13.184120213333335,9.8104544968455301,23.293435258959583,2.6350546127345957,161.42149368381561,5.1178471248985856E-2,5.749854424870251,-153296.65748992001,1675.4404289009753,2.4815367482908909E-2,1.6337620951172052,-153634.34246018398,2455.4908624892782,9.8255519313304731,2.4808257601804582E-2,1.6312517408523863,-153634.43353064408,2455.8887096682311]
["AKM","AKM72P",29.4,18.7,20.100000000000001,12.721518987341772,3000,78.5,6000,0.33,5,102,6.5,640,10,2508.9146950967424,3677.8329089225444,3843.1372549019611,17.998717982340114,17.307692307692307,0.34184410816294319,0.38757825222929937,3.5137473387887766E-2,-24.15418864197531,9,30.424892800000002,9,-2486.3359999999998,7.5,2498.3359999999998,9,0.26573044329861978,0.40316432494331061,6.3775306391668751,19.35188759727891,14.399960682182996,23.293435258959583,2.6350546127345957,161.42149368381561,2.3219229332493312E-2,2.9109763151971055,-153460.3816054489,2508.9146950967424,1.1166319200085428E-2,0.70997639508877586,-153651.88767585583,3677.8329089225444,12.17780935302391,1.14699114545561E-2,0.83952966237049287,-153647.06396448481,3623.5944761300366]
["AKM","AKM72Q",29.5,23.5,16.3,12.538461538461538,4000,78.400000000000006,6000,0.26,3.2,81.2,6.5,640,10,3143.2868029635506,4683.8597869221139,4827.5862068965516,14.043262703157025,17.307692307692307,0.34073397737429351,0.38807261224489797,2.7986189287835538E-2,-24.15418864197531,9,30.424892800000002,9,-2486.3359999999998,7.5,2498.3359999999998,9,0.33280732942085822,0.50493289604519787,7.9873759061005973,24.236779010169496,18.034864198894649,23.293435258959583,2.6350546127345957,161.42149368381561,1.4806070480668291E-2,2.2837676329099583,-153466.2430400092,3143.2868029635506,6.9084549608468887E-3,0.44727678981160179,-153656.41456179536,4683.8597869221139,12.231686955286092,7.2782722716180862E-3,0.65948190082511082,-153647.50950423771,4549.5280963049454]
["AKM","AKM73L",42,12.1,34.4,9.8285714285714274,1400,113,6000,0.95,15.7,224.7,9.1999999999999993,640,10,1155.1332245243223,1634.5999570069121,1744.5482866043615,33.12645737624819,12.228260869565219,0.24060470145521329,0.27415107115044246,7.5602804373898908E-2,-24.838359308641976,9,30.979071040000001,9,-2542.8848000000003,7.5,2554.8848000000003,9,0.12095701941007901,0.18593589265079366,2.9029684658418962,8.9249228472380953,6.623975370196713,23.408926749031853,2.7298553180953018,167.22891467146775,0.10420401143845166,12.036544574152712,-152946.63939871386,1155.1332245243223,5.5286399950117832E-2,3.596764631245343,-153599.94428227114,1634.5999570069121,9.7280258031116311,5.2713887464530464E-2,2.449097156192074,-153634.30072198095,1684.1168198447617]
["AKM","AKM73M",42,13.6,33.799999999999997,10.903225806451612,1500,112,6000,0.68,12.4,200,9.1999999999999993,640,10,1319.0204936359687,1849.2330490204452,1960,31.890859332021563,12.228260869565219,0.24060955724718877,0.27659884857142858,6.710375985464169E-2,-24.838359308641976,9,30.979071040000001,9,-2542.8848000000003,7.5,2554.8848000000003,9,0.13595169123777476,0.20898579669841269,3.262840589706594,10.03131824152381,7.4451293417087019,23.408926749031853,2.7298553180953018,167.22891467146775,8.1583128435069471E-2,8.5429364631450539,-153207.86397866666,1319.0204936359687,4.3570310197541234E-2,2.5032347077150283,-153624.83634998807,1849.2330490204452,10.626788473118278,4.1752452972293588E-2,1.7537665512715368,-153644.77689302276,1897.4190827655843]
["AKM","AKM73P",41.6,19.5,28.5,13.380281690140846,2400,111,6000,0.35,5.9,137,9.1999999999999993,640,10,1949.5938214042462,2741.8714685510927,2861.3138686131388,26.633951567491952,12.228260869565219,0.24292879268287892,0.27909073009009011,4.5847258101006025E-2,-24.838359308641976,9,30.979071040000001,9,-2542.8848000000003,7.5,2554.8848000000003,9,0.19680506773850667,0.30252999062500002,4.7233216257241599,14.52143955,10.777645876094859,23.408926749031853,2.7298553180953018,167.22891467146775,3.8146201272721239E-2,4.3212908534742045,-153415.27131652832,1949.5938214042462,2.0034875223099741E-2,1.1044941576999445,-153647.75103435994,2741.8714685510927,13.298852956547069,1.9600400633011005E-2,0.89510328017014196,-153653.32801584832,2777.1334589520939]
["AKM","AKM73Q",41.5,24.5,25.2,14.823529411764707,3000,111,6000,0.27,3.7,109.2,9.1999999999999993,640,10,2459.043054556133,3472.2264023926659,3589.7435897435898,22.634236546999848,12.228260869565219,0.24351261231621935,0.27909073009009011,3.6521452442360464E-2,-24.838359308641976,9,30.979071040000001,9,-2542.8848000000003,7.5,2554.8848000000003,9,0.24786373189877783,0.381017691004016,5.9487295655706678,18.288849168192769,13.573774083306617,23.408926749031853,2.7298553180953018,167.22891467146775,2.4012346016058402E-2,3.3464781700042439,-153429.21479595368,2459.043054556133,1.2528998476934901E-2,0.74827866170581625,-153652.26126081031,3472.2264023926659,14.652655228758171,1.2443276633431149E-2,0.6931825902392833,-153653.92627652889,3486.2785009567665]
["AKM","AKM74L",53,12.9,43.5,10.507246376811596,1200,143,6000,0.85,16.399999999999999,266,12,640,10,1005.6070810134075,1388.0970127596702,1473.6842105263156,42.010898648985943,9.375,0.19174648627437191,0.22065576503496503,8.8415301713558575E-2,-25.547869629629631,9,31.553774400000002,9,-2601.5279999999998,7.5,2613.5279999999998,9,0.10272218895296954,0.1600014503773585,2.4653325348712691,7.6800696181132073,5.6852925574867061,23.53081290472625,2.8281671606915895,173.25142532532922,0.13775155055908794,13.630477426409692,-153007.55420433651,1005.6070810134075,7.6776160912389105E-2,4.0859414349808283,-153605.01236146019,1388.0970127596702,10.433522279430461,7.2543523827960213E-2,2.2264554393505458,-153646.48521742533,1440.0669568035983]
["AKM","AKM74P",52.5,18.5,39.6,13.943661971830988,1800,142,6000,0.43,7.7,183,12,640,10,1495.2537445531971,2043.9805006597128,2142.0765027322404,37.851473078605395,9.375,0.1935172334780032,0.22220967887323945,6.0636438643938945E-2,-25.547869629629631,9,31.553774400000002,9,-2601.5279999999998,7.5,2613.5279999999998,9,0.14871776488503011,0.23164477238095241,3.5692263572407228,11.118949074285716,8.2309772648441726,23.53081290472625,2.8281671606915895,173.25142532532922,6.4013003671322732E-2,6.81994609582918,-153316.78401303402,1495.2537445531971,3.5846825152916081E-2,1.8954659695410561,-153637.17931827102,2043.9805006597128,13.907075711708014,3.431492908985944E-2,1.1218416887199163,-153654.6049092646,2099.7927536801872]
["AKM","AKM74Q",52.2,26.1,31.5,15.75,2500,141,6000,0.26,3.8,129,12,640,10,2146.1751235428255,2950.5874587811127,3038.7596899224809,27.769135841292389,9.375,0.1947252225410695,0.22378563404255319,4.2689751962398194E-2,-25.547869629629631,9,31.553774400000002,9,-2601.5279999999998,7.5,2613.5279999999998,9,0.21101845017470489,0.32868515000000004,5.0644428041929173,15.776887200000001,11.679089362278892,23.53081290472625,2.8281671606915895,173.25142532532922,3.1398199050083078E-2,4.09555537805314,-153412.008325,2146.1751235428255,1.7345716186439309E-2,0.89498953750428889,-153651.96637413252,2950.5874587811127,15.406155348837208,1.7045989407263751E-2,0.67847315246020612,-153657.08446279357,2982.5414442713372]
["AKM","AKM82T",75,48,47.5,30.06,2500,210,4000,9.1999999999999998E-2,2.73,108.4,17.2,640,10,{"$f":"IF(AQ128<I128,IF(AQ128<0,0,AQ128),I128)","v":1944.1213567440589},{"$f":"IF(AU128<I128,IF(AU128<0,0,AU128),I128)","v":3451.5293548919362},{"$f":"IF(UAC_V*0.98/L128*1000<I128,IF(UAC_V*0.98/L128*1000<0,0,UAC_V*0.98/L128*1000),I128)","v":3616.2361623616234},{"$f":"C128+(E128-C128)/G128*Q128","v":37.033177096188702},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M128,(inertia/gear^2+gear_inertia)/M128),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M128,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M128))","v":6.5406976744186052},{"$f":"IF((C128+(E128-C128)/G128*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X128^2*time1+Y128^2*time2+Z128^2*time3+AA128^2*time4)/time)/(C128+(E128-C128)/G128*mspeed),SQRT((((X128-Y128)*2/PI()+Y128)^2*time1+Y128^2*time2+((Z128-Y128)*2/PI()+Y128)^2*time3+AA128^2*time4)/time)/(C128+(E128-C128)/G128*mspeed)),IF(AccType=1,SQRT((X128^2*time1+Y128^2*time2+Z128^2*time3+AA128^2*time4+AB128^2*time5+AC128^2*time6+AD128^2*time7+AE128^2*time8)/time)/(C128+(E128-C128)/G128*mspeed),SQRT((((X128-Y128)*2/PI()+Y128)^2*time1+Y128^2*time2+((Z128-Y128)*2/PI()+Y128)^2*time3+AA128^2*time4+((AB128-AC128)*2/PI()+AC128)^2*time5+AC128^2*time6+((AD128-AC128)*2/PI()+AC128)^2*time7+AE128^2*time8)/time)/(C128+(E128-C128)/G128*mspeed))))","v":0.13682838014370946},{"$f":"IF(move1,MAX(ABS(X128),ABS(Z128))/H128,MAX(ABS(X128),ABS(Z128),ABS(AB128),ABS(AD128))/H128)","v":0.15533847923809524},{"$f":"IF(AZ128>0,speed/(MIN(AZ128,I128)),\"NA\")","v":3.5858645594119727E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M128+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M128+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-26.865531654320982},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M128+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M128+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":32.621080640000002},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M128+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M128+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2710.4367999999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M128+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M128+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2722.4367999999999},9,{"$f":"AH128/Irms","v":0.27276629654872014},{"$f":"AI128/Ipeak","v":0.43494774186666668},{"$f":"IF(move1,IF(AccType=1,SQRT((X128^2*time1+Y128^2*time2+Z128^2*time3+AA128^2*time4)/time)/(C128/D128),SQRT((((X128-Y128)*2/PI()+Y128)^2*time1+Y128^2*time2+((Z128-AA128)*2/PI()+AA128)^2*time3+AA128^2*time4)/time)/(C128/D128)),IF(AccType=1,SQRT((X128^2*time1+Y128^2*time2+Z128^2*time3+AA128^2*time4+AB128^2*time5+AC128^2*time6+AD128^2*time7+AE128^2*time8)/time)/(C128/D128),SQRT((((X128-Y128)*2/PI()+Y128)^2*time1+Y128^2*time2+((Z128-AA128)*2/PI()+AA128)^2*time3+AA128^2*time4+((AB128-AC128)*2/PI()+AC128)^2*time5+AC128^2*time6+((AD128-AE128)*2/PI()+AE128)^2*time7+AE128^2*time8)/time)/(C128/D128)))","v":6.5463911171692839},{"$f":"IF(move1,MAX(ABS(X128),ABS(Z128))/(C128/D128),MAX(ABS(X128),ABS(Z128),ABS(AB128),ABS(AD128))/(C128/D128))","v":20.8774916096},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X128),ABS(Z128))/(C128/D128),MAX(ABS((X128-Y128)*2/PI()+Y128),ABS((Z128-Y128)*2/PI()+Y128))/(C128/D128)),IF(AccType=1,MAX(ABS(X128),ABS(Z128),ABS(AB128),ABS(AD128))/(C128/D128),MAX(ABS((X128-Y128)*2/PI()+Y128),ABS((Z128-Y128)*2/PI()+Y128),ABS((AB128-AC128)*2/PI()+AC128),ABS((AD128-AC128)*2/PI()+AC128))/(C128/D128)))","v":15.384094067272374},{"$f":"IF((C128+(E128-C128)/G128*mspeed)<0,\"NA\",U128*(C128+(E128-C128)/G128*mspeed)*mspeed/9.55)","v":23.762779560452554},{"$f":"IF(move1,IF(speed1>speed2,AM128/2*time1/time,AM128/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z128*-speed/30*PI(),((Z128-AA128)*2/PI()+AA128)*-speed/30*PI()),IF(AccType=1,X128*-speed/30*PI(),((X128-Y128)*2/PI()+Y128)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z128*-speed/30*PI(),((Z128-AA128)*2/PI()+AA128)*-speed/30*PI()),IF(AccType=1,X128*-speed/30*PI(),((X128-Y128)*2/PI()+Y128)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD128*-speed/30*PI(),((AD128-AE128)*2/PI()+AE128)*-speed/30*PI()),IF(AccType=1,AB128*-speed/30*PI(),((AB128-AC128)*2/PI()+AC128)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD128*-speed/30*PI(),((AD128-AE128)*2/PI()+AE128)*-speed/30*PI()),IF(AccType=1,AB128*-speed/30*PI(),((AB128-AC128)*2/PI()+AC128)*-speed/30*PI()),0)/2*time7/time)))","v":3.0107462969418366},{"$f":"IF(move1,MAX(IF(AccType=1,Z128*-speed/30*PI(),((Z128-AA128)*2/PI()+AA128)*-speed/30*PI()),IF(AccType=1,X128*-speed/30*PI(),((X128-Y128)*2/PI()+Y128)*-speed/30*PI()),0),MAX(IF(AccType=1,Z128*-speed/30*PI(),((Z128-AA128)*2/PI()+AA128)*-speed/30*PI()),IF(AccType=1,X128*-speed/30*PI(),((X128-Y128)*2/PI()+Y128)*-speed/30*PI()),IF(AccType=1,AD128*-speed/30*PI(),((AD128-AE128)*2/PI()+AE128)*-speed/30*PI()),IF(AccType=1,AB128*-speed/30*PI(),((AB128-AC128)*2/PI()+AC128)*-speed/30*PI()),0))","v":184.43608796821474},3.9431595960855534E-2,2.3215444618763579,{"$f":"0.75*J128^2*(D128/C128*H128)^2-(UAC_V*0.98)^2","v":-153549.33379072},{"$f":"-AO128/2/AN128+SQRT((AO128/2/AN128)^2-AP128/AN128)","v":1944.1213567440589},{"$f":"(L128^2)/1000000+((K128/1000)^2*AV128^2*PI()*PI()*(O128/2)^2)/1200","v":1.2769395705602656E-2},{"$f":"SQRT(3)*L128*J128*AV128/1000","v":0.44538738716261528},{"$f":"0.75*J128^2*AV128^2-(UAC_V*0.98)^2","v":-153659.77956444962},{"$f":"-AS128/2/AR128+SQRT((AS128/2/AR128)^2-AT128/AR128)","v":3451.5293548919362},{"$f":"D128+(F128-D128)*((0.85*UAC_V-D128*J128)/L128*1000)/G128","v":25.784586863468633},{"$f":"(L128^2)/1000000+((K128/1000)^2*AJ128^2*PI()*PI()*(O128/2)^2)/1200","v":1.2113243380982892E-2},{"$f":"SQRT(3)*L128*J128*AJ128/1000","v":0.26573555344390709},{"$f":"0.75*J128^2*AJ128^2-(UAC_V*0.98)^2","v":-153662.49761661649},{"$f":"IF(((AX128/2/AW128)^2-AY128/AW128)>0,-AX128/2/AW128+SQRT((AX128/2/AW128)^2-AY128/AW128),-9999)","v":3550.7184491763255}]
["AKM","AKM83T",130,62,70,33.33,2200,456,4000,6.0999999999999999E-2,2.36,140.1,33.4,640,10,{"$f":"IF(AQ129<I129,IF(AQ129<0,0,AQ129),I129)","v":1420.7849200607677},{"$f":"IF(AU129<I129,IF(AU129<0,0,AU129),I129)","v":2713.003657445568},{"$f":"IF(UAC_V*0.98/L129*1000<I129,IF(UAC_V*0.98/L129*1000<0,0,UAC_V*0.98/L129*1000),I129)","v":2798.0014275517487},{"$f":"C129+(E129-C129)/G129*Q129","v":56.00899116057542},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M129,(inertia/gear^2+gear_inertia)/M129),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M129,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M129))","v":3.3682634730538923},{"$f":"IF((C129+(E129-C129)/G129*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X129^2*time1+Y129^2*time2+Z129^2*time3+AA129^2*time4)/time)/(C129+(E129-C129)/G129*mspeed),SQRT((((X129-Y129)*2/PI()+Y129)^2*time1+Y129^2*time2+((Z129-Y129)*2/PI()+Y129)^2*time3+AA129^2*time4)/time)/(C129+(E129-C129)/G129*mspeed)),IF(AccType=1,SQRT((X129^2*time1+Y129^2*time2+Z129^2*time3+AA129^2*time4+AB129^2*time5+AC129^2*time6+AD129^2*time7+AE129^2*time8)/time)/(C129+(E129-C129)/G129*mspeed),SQRT((((X129-Y129)*2/PI()+Y129)^2*time1+Y129^2*time2+((Z129-Y129)*2/PI()+Y129)^2*time3+AA129^2*time4+((AB129-AC129)*2/PI()+AC129)^2*time5+AC129^2*time6+((AD129-AC129)*2/PI()+AC129)^2*time7+AE129^2*time8)/time)/(C129+(E129-C129)/G129*mspeed))))","v":8.1603030715410682E-2},{"$f":"IF(move1,MAX(ABS(X129),ABS(Z129))/H129,MAX(ABS(X129),ABS(Z129),ABS(AB129),ABS(AD129))/H129)","v":7.8829276491228076E-2},{"$f":"IF(AZ129>0,speed/(MIN(AZ129,I129)),\"NA\")","v":4.57880287441833E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M129+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M129+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-30.970555654320989},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M129+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M129+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":35.946150080000002},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M129+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M129+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-3049.7296000000001},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M129+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M129+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":3061.7296000000001},9,{"$f":"AH129/Irms","v":0.20982664504999282},{"$f":"AI129/Ipeak","v":0.35715726041025642},{"$f":"IF(move1,IF(AccType=1,SQRT((X129^2*time1+Y129^2*time2+Z129^2*time3+AA129^2*time4)/time)/(C129/D129),SQRT((((X129-Y129)*2/PI()+Y129)^2*time1+Y129^2*time2+((Z129-AA129)*2/PI()+AA129)^2*time3+AA129^2*time4)/time)/(C129/D129)),IF(AccType=1,SQRT((X129^2*time1+Y129^2*time2+Z129^2*time3+AA129^2*time4+AB129^2*time5+AC129^2*time6+AD129^2*time7+AE129^2*time8)/time)/(C129/D129),SQRT((((X129-Y129)*2/PI()+Y129)^2*time1+Y129^2*time2+((Z129-AA129)*2/PI()+AA129)^2*time3+AA129^2*time4+((AB129-AC129)*2/PI()+AC129)^2*time5+AC129^2*time6+((AD129-AE129)*2/PI()+AE129)^2*time7+AE129^2*time8)/time)/(C129/D129)))","v":5.0358394811998277},{"$f":"IF(move1,MAX(ABS(X129),ABS(Z129))/(C129/D129),MAX(ABS(X129),ABS(Z129),ABS(AB129),ABS(AD129))/(C129/D129))","v":17.143548499692308},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X129),ABS(Z129))/(C129/D129),MAX(ABS((X129-Y129)*2/PI()+Y129),ABS((Z129-Y129)*2/PI()+Y129))/(C129/D129)),IF(AccType=1,MAX(ABS(X129),ABS(Z129),ABS(AB129),ABS(AD129))/(C129/D129),MAX(ABS((X129-Y129)*2/PI()+Y129),ABS((Z129-Y129)*2/PI()+Y129),ABS((AB129-AC129)*2/PI()+AC129),ABS((AD129-AC129)*2/PI()+AC129))/(C129/D129)))","v":12.47366168974586},{"$f":"IF((C129+(E129-C129)/G129*mspeed)<0,\"NA\",U129*(C129+(E129-C129)/G129*mspeed)*mspeed/9.55)","v":24.530071017231084},{"$f":"IF(move1,IF(speed1>speed2,AM129/2*time1/time,AM129/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z129*-speed/30*PI(),((Z129-AA129)*2/PI()+AA129)*-speed/30*PI()),IF(AccType=1,X129*-speed/30*PI(),((X129-Y129)*2/PI()+Y129)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z129*-speed/30*PI(),((Z129-AA129)*2/PI()+AA129)*-speed/30*PI()),IF(AccType=1,X129*-speed/30*PI(),((X129-Y129)*2/PI()+Y129)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD129*-speed/30*PI(),((AD129-AE129)*2/PI()+AE129)*-speed/30*PI()),IF(AccType=1,AB129*-speed/30*PI(),((AB129-AC129)*2/PI()+AC129)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD129*-speed/30*PI(),((AD129-AE129)*2/PI()+AE129)*-speed/30*PI()),IF(AccType=1,AB129*-speed/30*PI(),((AB129-AC129)*2/PI()+AC129)*-speed/30*PI()),0)/2*time7/time)))","v":3.579550529106073},{"$f":"IF(move1,MAX(IF(AccType=1,Z129*-speed/30*PI(),((Z129-AA129)*2/PI()+AA129)*-speed/30*PI()),IF(AccType=1,X129*-speed/30*PI(),((X129-Y129)*2/PI()+Y129)*-speed/30*PI()),0),MAX(IF(AccType=1,Z129*-speed/30*PI(),((Z129-AA129)*2/PI()+AA129)*-speed/30*PI()),IF(AccType=1,X129*-speed/30*PI(),((X129-Y129)*2/PI()+Y129)*-speed/30*PI()),IF(AccType=1,AD129*-speed/30*PI(),((AD129-AE129)*2/PI()+AE129)*-speed/30*PI()),IF(AccType=1,AB129*-speed/30*PI(),((AB129-AC129)*2/PI()+AC129)*-speed/30*PI()),0))","v":219.28061389412758},7.3791778556152918E-2,3.2191541798645242,{"$f":"0.75*J129^2*(D129/C129*H129)^2-(UAC_V*0.98)^2","v":-153532.00809616284},{"$f":"-AO129/2/AN129+SQRT((AO129/2/AN129)^2-AP129/AN129)","v":1420.7849200607677},{"$f":"(L129^2)/1000000+((K129/1000)^2*AV129^2*PI()*PI()*(O129/2)^2)/1200","v":2.070915911787171E-2},{"$f":"SQRT(3)*L129*J129*AV129/1000","v":0.45481014115718527},{"$f":"0.75*J129^2*AV129^2-(UAC_V*0.98)^2","v":-153661.3653433983},{"$f":"-AS129/2/AR129+SQRT((AS129/2/AR129)^2-AT129/AR129)","v":2713.003657445568},{"$f":"D129+(F129-D129)*((0.85*UAC_V-D129*J129)/L129*1000)/G129","v":30.725682759068189},{"$f":"(L129^2)/1000000+((K129/1000)^2*AJ129^2*PI()*PI()*(O129/2)^2)/1200","v":1.9806194710532219E-2},{"$f":"SQRT(3)*L129*J129*AJ129/1000","v":0.18463862555457622},{"$f":"0.75*J129^2*AJ129^2-(UAC_V*0.98)^2","v":-153663.56578096753},{"$f":"IF(((AX129/2/AW129)^2-AY129/AW129)>0,-AX129/2/AW129+SQRT((AX129/2/AW129)^2-AY129/AW129),-9999)","v":2780.7258352368121}]
["AKM","AKM84T",180,67,105,39.18,1800,668,4000,5.8000000000000003E-2,2.5,177.4,49.5,640,10,{"$f":"IF(AQ130<I130,IF(AQ130<0,0,AQ130),I130)","v":1156.6040516921698},{"$f":"IF(AU130<I130,IF(AU130<0,0,AU130),I130)","v":2138.0879002078477},{"$f":"IF(UAC_V*0.98/L130*1000<I130,IF(UAC_V*0.98/L130*1000<0,0,UAC_V*0.98/L130*1000),I130)","v":2209.6956031567079},{"$f":"C130+(E130-C130)/G130*Q130","v":90.913004158006345},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M130,(inertia/gear^2+gear_inertia)/M130),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M130,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M130))","v":2.2727272727272729},{"$f":"IF((C130+(E130-C130)/G130*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X130^2*time1+Y130^2*time2+Z130^2*time3+AA130^2*time4)/time)/(C130+(E130-C130)/G130*mspeed),SQRT((((X130-Y130)*2/PI()+Y130)^2*time1+Y130^2*time2+((Z130-Y130)*2/PI()+Y130)^2*time3+AA130^2*time4)/time)/(C130+(E130-C130)/G130*mspeed)),IF(AccType=1,SQRT((X130^2*time1+Y130^2*time2+Z130^2*time3+AA130^2*time4+AB130^2*time5+AC130^2*time6+AD130^2*time7+AE130^2*time8)/time)/(C130+(E130-C130)/G130*mspeed),SQRT((((X130-Y130)*2/PI()+Y130)^2*time1+Y130^2*time2+((Z130-Y130)*2/PI()+Y130)^2*time3+AA130^2*time4+((AB130-AC130)*2/PI()+AC130)^2*time5+AC130^2*time6+((AD130-AC130)*2/PI()+AC130)^2*time7+AE130^2*time8)/time)/(C130+(E130-C130)/G130*mspeed))))","v":6.0946488756377468E-2},{"$f":"IF(move1,MAX(ABS(X130),ABS(Z130))/H130,MAX(ABS(X130),ABS(Z130),ABS(AB130),ABS(AD130))/H130)","v":5.8758524550898202E-2},{"$f":"IF(AZ130>0,speed/(MIN(AZ130,I130)),\"NA\")","v":5.7828361975168191E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M130+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M130+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-35.050239999999995},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M130+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M130+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":39.2506944},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M130+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M130+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-3386.9279999999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M130+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M130+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":3398.9279999999999},9,{"$f":"AH130/Irms","v":0.16926849097058047},{"$f":"AI130/Ipeak","v":0.30437459777777776},{"$f":"IF(move1,IF(AccType=1,SQRT((X130^2*time1+Y130^2*time2+Z130^2*time3+AA130^2*time4)/time)/(C130/D130),SQRT((((X130-Y130)*2/PI()+Y130)^2*time1+Y130^2*time2+((Z130-AA130)*2/PI()+AA130)^2*time3+AA130^2*time4)/time)/(C130/D130)),IF(AccType=1,SQRT((X130^2*time1+Y130^2*time2+Z130^2*time3+AA130^2*time4+AB130^2*time5+AC130^2*time6+AD130^2*time7+AE130^2*time8)/time)/(C130/D130),SQRT((((X130-Y130)*2/PI()+Y130)^2*time1+Y130^2*time2+((Z130-AA130)*2/PI()+AA130)^2*time3+AA130^2*time4+((AB130-AC130)*2/PI()+AC130)^2*time5+AC130^2*time6+((AD130-AE130)*2/PI()+AE130)^2*time7+AE130^2*time8)/time)/(C130/D130)))","v":4.0624437832939311},{"$f":"IF(move1,MAX(ABS(X130),ABS(Z130))/(C130/D130),MAX(ABS(X130),ABS(Z130),ABS(AB130),ABS(AD130))/(C130/D130))","v":14.609980693333332},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X130),ABS(Z130))/(C130/D130),MAX(ABS((X130-Y130)*2/PI()+Y130),ABS((Z130-Y130)*2/PI()+Y130))/(C130/D130)),IF(AccType=1,MAX(ABS(X130),ABS(Z130),ABS(AB130),ABS(AD130))/(C130/D130),MAX(ABS((X130-Y130)*2/PI()+Y130),ABS((Z130-Y130)*2/PI()+Y130),ABS((AB130-AC130)*2/PI()+AC130),ABS((AD130-AC130)*2/PI()+AC130))/(C130/D130)))","v":10.518326345853227},{"$f":"IF((C130+(E130-C130)/G130*mspeed)<0,\"NA\",U130*(C130+(E130-C130)/G130*mspeed)*mspeed/9.55)","v":25.35480827682192},{"$f":"IF(move1,IF(speed1>speed2,AM130/2*time1/time,AM130/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z130*-speed/30*PI(),((Z130-AA130)*2/PI()+AA130)*-speed/30*PI()),IF(AccType=1,X130*-speed/30*PI(),((X130-Y130)*2/PI()+Y130)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z130*-speed/30*PI(),((Z130-AA130)*2/PI()+AA130)*-speed/30*PI()),IF(AccType=1,X130*-speed/30*PI(),((X130-Y130)*2/PI()+Y130)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD130*-speed/30*PI(),((AD130-AE130)*2/PI()+AE130)*-speed/30*PI()),IF(AccType=1,AB130*-speed/30*PI(),((AB130-AC130)*2/PI()+AC130)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD130*-speed/30*PI(),((AD130-AE130)*2/PI()+AE130)*-speed/30*PI()),IF(AccType=1,AB130*-speed/30*PI(),((AB130-AC130)*2/PI()+AC130)*-speed/30*PI()),0)/2*time7/time)))","v":4.1448436240347268},{"$f":"IF(move1,MAX(IF(AccType=1,Z130*-speed/30*PI(),((Z130-AA130)*2/PI()+AA130)*-speed/30*PI()),IF(AccType=1,X130*-speed/30*PI(),((X130-Y130)*2/PI()+Y130)*-speed/30*PI()),0),MAX(IF(AccType=1,Z130*-speed/30*PI(),((Z130-AA130)*2/PI()+AA130)*-speed/30*PI()),IF(AccType=1,X130*-speed/30*PI(),((X130-Y130)*2/PI()+Y130)*-speed/30*PI()),IF(AccType=1,AD130*-speed/30*PI(),((AD130-AE130)*2/PI()+AE130)*-speed/30*PI()),IF(AccType=1,AB130*-speed/30*PI(),((AB130-AC130)*2/PI()+AC130)*-speed/30*PI()),0))","v":253.91005015383104},0.11092115221774389,4.4311963712577898,{"$f":"0.75*J130^2*(D130/C130*H130)^2-(UAC_V*0.98)^2","v":-153508.01789724297},{"$f":"-AO130/2/AN130+SQRT((AO130/2/AN130)^2-AP130/AN130)","v":1156.6040516921698},{"$f":"(L130^2)/1000000+((K130/1000)^2*AV130^2*PI()*PI()*(O130/2)^2)/1200","v":3.3298900800769318E-2},{"$f":"SQRT(3)*L130*J130*AV130/1000","v":0.67216794017383541},{"$f":"0.75*J130^2*AV130^2-(UAC_V*0.98)^2","v":-153660.41087679644},{"$f":"-AS130/2/AR130+SQRT((AS130/2/AR130)^2-AT130/AR130)","v":2138.0879002078477},{"$f":"D130+(F130-D130)*((0.85*UAC_V-D130*J130)/L130*1000)/G130","v":37.716862457722669},{"$f":"(L130^2)/1000000+((K130/1000)^2*AJ130^2*PI()*PI()*(O130/2)^2)/1200","v":3.1612937805915765E-2},{"$f":"SQRT(3)*L130*J130*AJ130/1000","v":0.1874514817316339},{"$f":"0.75*J130^2*AJ130^2-(UAC_V*0.98)^2","v":-153663.72086741787},{"$f":"IF(((AX130/2/AW130)^2-AY130/AW130)>0,-AX130/2/AW130+SQRT((AX130/2/AW130)^2-AY130/AW130),-9999)","v":2201.7561992883329}]
["DBK","DBK4N00100",1,1.1000000000000001,0.9,1.06,3000,4.6500000000000004,9000,38,70,56,7.9000000000000001E-2,670,6,2491.2904980772728,6065.6943382906311,7000,0.79781018872364573,1424.0506329113923,9.9193576102674452,6.2595644827526877,"NA",-22.527129438024691,9,29.1069748448,9,-2351.8545759999997,7.5,2363.8545759999997,9,0.45430100471091084,0.66703484019333337,10.90322411306186,32.017672329280003,23.980547523566987,23.027008335120275,2.4096044908378951,147.61058621651401,1.2625610012295903E-2,18.852888066161114,-125329.22732499999,2491.2904980772728,3.5200500609167793E-3,3.7926924379432614,-152517.27519700001,6065.6943382906311,1.0289999999999999,0.2117172559427962,88.387600826405745,469133.19227104925,-9999]
["DBK","DBK4H00100",1,1.9,0.9,1.85,3000,4.6109999999999998,9000,13,24,32,7.9000000000000001E-2,670,6,5099.7895395946744,9000,9000,0.70000000000000007,1424.0506329113923,9.9193576102674452,6.3125080990674478,"NA",-22.527129438024691,9,29.1069748448,9,-2351.8545759999997,7.5,2363.8545759999997,9,0.78470173540975507,1.1521510876066667,18.832841649834123,55.303252205120003,41.420945722524799,23.027008335120275,2.4096044908378951,147.61058621651401,4.2965096701362369E-3,6.3125187507325524,-143935.51050333251,5099.7895395946744,1.1524616446316363E-3,1.250687907383373,-153282.11029255981,11002.881984141832,1.7357812500000005,7.4175546695431402E-2,29.845163915409731,63800.308871502784,-9999]
["DBK","DBK4N00160",1.6,1.1000000000000001,1.4,1,3000,7.3010000000000002,9000,25,68,90,0.128,670,6,2385.7304848523891,4041.3391135013649,4355.5555555555547,1.3305773924332422,878.90625,6.2012812531381272,3.9880882281331322,0.26265593167124623,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.28396264830601559,0.41704082511666662,6.8151035593443741,20.017959605599998,14.992244045856102,23.028996904169631,2.4113249480833296,147.71598015295655,1.6723606596990688E-2,19.561321744687135,-141853.95961730956,2385.7304848523891,8.4315872723742715E-3,3.8357708509285762,-153209.89080182614,4041.3391135013649,0.98425925925925928,8.5032902984967115E-2,58.426488915513197,-48304.289907574494,484.7556788966088]
["DBK","DBK4H00160",1.6,1.9,1.4,1.7,3000,5.9639999999999995,9000,7.6,18,51,0.128,670,6,5716.5909722254291,7423.7875491527393,7686.2745098039222,1.1050808300564836,878.90625,6.2012812531381272,4.8821314811535883,5.8976407416606633E-2,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.49048093798311782,0.72034324338333322,11.771542511594827,34.576475682399995,25.895694261024175,23.028996904169631,2.4113249480833296,147.71598015295655,3.8039526276768109E-3,4.7546182040462526,-151491.14395749249,5716.5909722254291,2.6531380933376659E-3,0.98984902319721457,-153569.8245781695,7423.7875491527393,1.4744313725490197,1.8683780578393882E-2,17.384890301794155,-124614.17197179772,2158.8964138508081]
["DBK","DBK5N00210",2.1,1.5,1.9,1.5,3000,9.52,9000,22,60,83,0.41299999999999998,670,6,2167.5868758023034,4212.1578032448115,4722.8915662650606,1.8191894797836792,272.39709443099275,4.7261203526682092,3.0646563808403364,0.19001062036257105,-22.611763883456788,9,29.175528745600001,9,-2358.8498719999998,7.5,2370.8498719999998,9,0.29517447915257128,0.43415965395238093,7.0841874996617111,20.839663389714286,15.602957512442476,23.040576813103883,2.4213316892047381,148.32898570165321,1.9211003702672039E-2,21.50652846742123,-136878.88,2167.5868758023034,7.4885784673661788E-3,4.7440871619311551,-152847.25,4212.1578032448115,1.5,7.1763998577302784E-2,49.347860281957075,-65290.821221964099,670.08862047059017]
["DBK","DBK5H00210",2.1,4,1.9,3.94,3000,7.5919999999999996,9000,3.1,10,32,0.41299999999999998,670,6,7223.6886810512933,9000,9000,1.4999999999999996,272.39709443099275,4.7261203526682092,3.8429305513171763,4.3216078146326747E-2,-22.611763883456788,9,29.175528745600001,9,-2358.8498719999998,7.5,2370.8498719999998,9,0.78713194440685685,1.1577590772063491,18.891166665764565,55.572435705904759,41.607886699846603,23.040576813103883,2.4213316892047381,148.32898570165321,2.571942416235185E-3,2.4846727415646495,-152156.77377131974,7223.6886810512933,1.1306207631368501E-3,0.65209773008063743,-153560.18372813077,11369.343182885745,3.7952499999999998,1.3838814533788206E-2,7.1490437969626024,-141186.25898171644,2946.2172398523967]
["DBK","DBK5N00430",4.3,2.9,3.9,2.8,3000,19.37,9000,7.1,32,90,0.57799999999999996,670,6,2323.9912606137536,4028.4576843254813,4355.5555555555547,3.7628723087566023,194.63667820069205,2.308740112300077,1.507970841177078,5.9975566559336654E-2,-22.65357431308642,9,29.209395193600002,9,-2362.3056320000001,7.5,2374.3056320000001,9,0.27878084777360684,0.41040332394108531,6.6907403465665647,19.699359549172094,14.74663526668018,23.047291680507506,2.4271250656434473,148.68388365089859,2.1035382980776021E-2,14.458413748527679,-147211.97135420944,2323.9912606137536,8.6865182720819306E-3,3.0787312223737668,-153371.45105124632,4028.4576843254813,2.7816999999999998,2.4583401722419036E-2,16.321287852926758,-145442.2581117872,2122.930416131187]
["DBK","DBK5H00430",4.3,5,3.9,4.8,3000,19.574999999999999,9000,2.2000000000000002,10,53,0.57799999999999996,670,6,4446.2173840484475,7043.1016962036847,7396.2264150943402,3.3609197738395089,194.63667820069205,2.308740112300077,1.4921785539514689,3.0765561065939764E-2,-22.65357431308642,9,29.209395193600002,9,-2362.3056320000001,7.5,2374.3056320000001,9,0.48065663409242565,0.70759193782945751,11.535759218218216,33.96441301581396,25.425233218414103,23.047291680507506,2.4271250656434473,148.68388365089859,6.6440201286967655E-3,4.5968729133506345,-151783.32711093835,4446.2173840484475,2.9646897710913392E-3,0.92620839584476511,-153587.65058806218,7043.1016962036847,4.586163522012578,7.5940986904131525E-3,5.1348069819525675,-151317.41378231498,4138.5221027051348]
["DBK","DBK6N00350",3.5,2.8,3,2.7,3000,16.510000000000002,9000,12,56,77,0.8,670,6,1491.6249591235269,4218.2836931221545,5090.909090909091,2.7969527178129745,140.625,2.8386124081851341,1.7719540254391277,0.11774201698295869,-22.709828345679011,9,29.254960960000002,9,-2366.9551999999999,7.5,2378.9551999999999,9,0.33082157317250444,0.48758268266666671,7.9397177561401069,23.403968768000002,17.515766908535561,23.056338606661289,2.4349197903064397,149.16138270988338,4.6424911928584042E-2,21.138280609325626,-134823.263488,1491.6249591235269,7.5805818652126414E-3,4.2688817023665582,-152895.60098714792,4218.2836931221545,2.6673593073593076,7.7147918953243882E-2,28.032495154464321,-120529.37423743187,1081.3807826304217]
["DBK","DBK6N00700",7,5,6,4.5999999999999996,3000,31.97,9000,4.4000000000000004,34,84,1.135,670,6,1545.8604176493247,4017.7037399320911,4666.666666666667,5.6607654200226367,99.118942731277528,1.4201482424561513,0.917226153018455,5.9478237780362805E-2,-22.79471618765432,9,29.323720112000004,9,-2373.9714399999998,7.5,2385.9714399999998,9,0.2955516439455711,0.43636488261904766,7.0932394546937063,20.945514365714288,15.670344336688485,23.070017347425342,2.4466821000456376,149.8819330916846,5.1677898505634819E-2,14.618647379945928,-146092.25782244897,1545.8604176493247,8.7851164480323048E-3,2.8776984937272356,-153370.59195646259,4017.7037399320911,4.4952380952380953,2.8068412704837554E-2,10.031621315374863,-150098.47327752682,2140.6813521222589]
["DBK","DBK7N00650",6.5,4.5,5,3.8,3000,30.03,9000,4.1500000000000004,22,87,3.2360000000000002,670,6,2268.0670382625894,4229.3237883667971,4505.7471264367814,4.3853381058166008,34.765142150803456,1.5361259454322242,0.99084092185148198,4.5817001666309233E-2,-23.32710232493827,9,29.754952883200005,9,-2417.974784,7.5,2429.974784,9,0.28753206965831896,0.42915797427692315,6.9007696717996545,20.599582765292311,15.378240032309536,23.156538440986232,2.5204510933652089,154.40096697874282,2.3054147593009295E-2,13.001170867272332,-148081.0153283125,2268.0670382625894,8.0432219077528379E-3,2.2751791447337735,-153493.02496562849,4229.3237883667971,3.6382088122605363,1.6041657311168696E-2,9.6168891918222155,-150609.28478901484,2778.9674104131045]
["DBK","DBK7N01200",12,7.5,10,6.8,3000,55.545000000000002,9000,1.65,11.5,98,5.3109999999999999,670,6,2440.5311979995413,3817.2783683914708,4000,9.4551477544056866,21.182451515722086,0.83478646769663967,0.54335852233684401,3.6606746304554627E-2,-23.852900152098766,9,30.180849123200002,9,-2461.4335840000003,7.5,2473.4335840000003,9,0.26054923371289312,0.39297980629166668,6.2531816091094354,18.863030702,14.052592092102293,23.24321978819199,2.5933071910035306,158.86407755258665,2.1401953126759649E-2,9.7228958953793914,-151203.18407454222,2440.5311979995413,1.0046066435599733E-2,1.8820713057347005,-153571.79382549276,3817.2783683914708,6.7199404761904757,1.1537167875577899E-2,3.9357462229685414,-153260.78003093475,3478.1554584017913]
["DBK","DBK7N01950",19.5,11.8,15,10,3000,90.75,9000,0.9,7,100,6.9160000000000004,670,6,2496.1754565249098,3779.1399618785181,3920,13.831290057182223,16.266628108733372,0.51545962581256921,0.33620140274600552,3.4484890654672244E-2,-24.259601603950617,9,30.510277299199998,9,-2495.0487039999998,7.5,2507.0487039999998,9,0.25300180149300611,0.38463811125059832,6.0720432358321466,18.46262934002872,13.732699512092669,23.311097651983076,2.6496609436346152,162.31626669524644,2.0938182070613345E-2,8.5604612643929183,-151831.96257352072,2496.1754565249098,1.0350033040028486E-2,1.5313663943397477,-153605.37292415719,3779.1399618785181,9.8237199999999998,1.0684020193980499E-2,2.1407159952018753,-153549.43337569718,3692.1663968293769]
["DBL","DBL1X00010",0.1,0.6,0.09,0.59,6000,0.47599999999999998,14000,38.200000000000003,6.5,10,6.0000000000000001E-3,330,6,14000,14000,14000,7.6666666666666647E-2,18750,99.144132504130241,61.117629216806726,"NA",-22.508631490370373,9,29.091991507199999,9,-2350.325664,7.5,2362.325664,9,2.4776868085049641,3.6364989383999995,59.464483404119143,174.55194904319998,130.74575435835021,23.024047059696148,2.4070413606559211,147.45357076018124,1.2550962816545679E-4,1.8896535746511842,-144737.02341952,27255.179524613821,1.0093628016017811E-4,0.36202039643404915,-153336.35308141433,37224.070328739028,0.54715333333333327,5.3561718195205756E-2,86.507066559426534,18555017.411792632,-9999]
["DBL","DBL1X00020",0.2,0.93,0.18,0.89,6000,0.96399999999999997,14000,22,4.7,13,1.2E-2,330,6,14000,14000,14000,0.15333333333333329,9375,49.572590164720381,30.179691923651458,"NA",-22.510151869629631,9,29.093223014400003,9,-2350.4513280000001,7.5,2362.4513280000001,9,1.9202275706998846,2.81840597952,46.085461696797232,135.28348701696001,101.33160523624646,23.024290394108892,2.4072520288900559,147.46647614015379,2.0185615194266189E-4,2.2205300117023588,-146369.98589812001,21983.777538649909,1.6995976617751135E-4,0.37951681158975459,-153450.93341674667,28951.978058022927,0.76613333333333322,1.6958840472678618E-2,50.196285762963718,3573654.2017708807,-9999]
["DBL","DBL2H00040",0.4,0.93,0.34,0.7,6000,1.849,14000,26.5,20,26,8.0000000000000002E-3,560,6,8951.2474851728657,14000,14000,0.26,14062.5,24.790705523311139,15.734127641752297,"NA",-22.509138283456789,9,29.092402009599997,9,-2350.3675519999997,7.5,2362.3675519999997,9,0.96010702059888631,1.4091632223399999,23.04256849437327,67.639834672319992,50.664587415281552,23.024128170010936,2.4071115834006322,147.45787255350538,1.2231932568670474E-3,5.1302640408524161,-143930.41674228426,8951.2474851728657,6.8240363961226294E-4,0.55498697457336188,-153550.09077590751,14599.322344193133,0.46505352564102542,7.6678874986789283E-2,60.462257648422053,1198290.3638846793,-9999]
["DBL","DBL2H00060",0.6,1.5,0.52,1.27,6000,2.7879999999999998,14000,14.8,13.2,25,1.0999999999999999E-2,560,6,9150.9822731360764,14000,14000,0.41333333333333344,10227.272727272728,16.5262053131374,10.435085280918223,"NA",-22.509898473086416,9,29.093017763200002,9,-2350.4303840000002,7.5,2362.4303840000002,9,1.0323785958538705,1.5152613418333336,24.777086300492893,72.73254440800001,54.479030986465389,23.02424983765086,2.4072169175176992,147.46432524349166,1.2515769687817988E-3,4.4667858276393773,-145683.12974800001,9150.9822731360764,6.3822745245304118E-4,0.64900197793724268,-153495.51857305341,15008.045675454969,1.0127066666666666,3.8904620151693367E-2,34.913366357800584,333913.26017360087,-9999]
["DBL","DBL2M00080",0.8,0.83,0.72,0.83,4500,3.6480000000000001,12000,47.7,43,58,1.2999999999999999E-2,560,6,3509.3052937507009,6090.119886849744,6758.620689655173,0.69173120201156002,8653.8461538461543,12.394697650558456,7.9751722219298253,"NA",-22.510405266172842,9,29.093428265600004,9,-2350.472272,7.5,2362.472272,9,0.42843862664048654,0.62884232969916665,10.282527039371677,30.184431825560001,22.609068993350494,23.024330950855941,2.4072871402624116,147.46862703681589,5.3245764876220167E-3,18.136351949220067,-129219.3461633488,3509.3052937507009,3.4582874965192181E-3,3.977270164302646,-152488.41453924999,6090.119886849744,0.83,7.3326171093155867E-2,108.34021150591926,718630.99324816605,-9999]
["DBL","DBL2H00080",0.8,1.49,0.69,1.1000000000000001,6000,3.6720000000000002,12000,14.7,13,33,1.2999999999999999E-2,560,6,7781.4224821593198,11497.939247611541,11878.787878787878,0.58920444712712161,8653.8461538461543,12.394888711953769,7.9230469132897614,"NA",-22.510405266172842,9,29.093428265600004,9,-2350.472272,7.5,2362.472272,9,0.76912476348713854,1.1288856280141668,18.458994323691325,54.186510144680007,40.587364819388242,23.024330950855941,2.4072871402624116,147.46862703681589,1.6741209138648699E-3,5.7463338757192943,-146083.57001578531,7781.4224821593198,1.0983264716867133E-3,0.72548215329995791,-153543.17255400441,11497.939247611541,0.8634453030303032,2.1696695270323963E-2,34.102228273870551,113315.33270045382,-9999]
["DBL","DBL3N00065",0.65,0.67,0.6,0.65,3000,2.94,9000,79,82.8,59,0.05,670,6,2478.9176987966198,5755.3531869878843,6644.0677966101694,0.55407744688353522,2250,15.257164684931968,9.8983069931972789,"NA",-22.519780938271605,9,29.101022560000001,9,-2351.2471999999998,7.5,2363.2471999999998,9,0.42568688189807657,0.62492580497435901,10.216485165553838,29.996438638769231,22.467376357472133,23.025831753667905,2.4085862610395767,147.54821021331333,8.1415721461795734E-3,24.46518514764908,-110677.40963022485,2478.9176987966198,3.6872849294056448E-3,5.1471003974261205,-151761.33966524102,5755.3531869878843,0.63756271186440683,0.25964989980270808,181.38112475320088,2209099.0290675252,-9999]
["DBL","DBL3H00065",0.65,1.08,0.48,0.95,6000,3,9000,30.3,31,36.5,0.05,670,6,5273.5074700902906,9000,9000,0.39499999999999996,2250,15.263246120420904,9.7003408533333335,"NA",-22.519780938271605,9,29.101022560000001,9,-2351.2471999999998,7.5,2363.2471999999998,9,0.68618183947749645,1.0073430886153847,16.468364147459916,48.352468253538461,36.216069352343141,23.025831753667905,2.4085862610395767,147.54821021331333,3.0997023068686652E-3,9.5483377748366021,-136555.58298698225,5273.5074700902906,1.3895624332303433E-3,1.7194056346303639,-153109.23255087284,9896.4452574335537,0.89759872146118713,9.4633405582312813E-2,69.374111414969789,749463.66646962671,-9999]
["DBL","DBL3N00130",1.3,1,1.2,0.95,3000,5.76,9000,35.5,61,77.5,0.08,670,6,2637.7841005397431,4602.7674880337991,5058.0645161290322,1.1465744170655399,1406.25,7.6289855933354636,5.0533298777777782,"NA",-22.527382834567899,9,29.107180096,9,-2351.8755200000001,7.5,2363.8755200000001,9,0.31769357009719595,0.4664612194871795,7.6246456823327033,22.390138535384615,16.7697141658996,23.027048911228551,2.4096396022102509,147.61273711317611,1.1413531023714129E-2,21.113965813619622,-135108.34745562129,2637.7841005397431,6.2467938631792655E-3,4.4532541807052457,-152838.54847875261,4602.7674880337991,0.934516129032258,8.3465270228187199E-2,79.912799146505208,112144.76035087131,-9999]
["DBL","DBL3H00130",1.3,1.75,1.1000000000000001,1.5,6000,5.55,9000,13,22,45,0.08,670,6,5167.428048315528,8200.726069304128,8711.1111111111095,1.0266424643565291,1406.25,7.6289855933354636,5.2445369542342348,0.1599605284712492,-22.527382834567899,9,29.107180096,9,-2351.8755200000001,7.5,2363.8755200000001,9,0.55596374767009293,0.81630713410256417,13.34312994408223,39.182742436923078,29.346999790324304,23.027048911228551,2.4096396022102509,147.61273711317611,4.0247777381230533E-3,7.570144560830725,-146589.05078125,5167.428048315528,2.1009763187730696E-3,1.4755449082854739,-153395.20583007814,8200.726069304128,1.45625,3.2880585254832166E-2,29.735839391634606,-44501.019219124893,795.97107918033089]
["DBL","DBL3M00190",1.9,1.5,1.6,1.32,3000,8.7629999999999999,9000,21.3,40,77,0.1,670,6,2697.217055586515,4719.2267597230402,5090.909090909091,1.4280773240276963,1125,5.2231456818719444,3.3220683692799273,0.18560815187626153,-22.532450765432099,9,29.111285120000002,9,-2352.2943999999998,7.5,2364.2943999999998,9,0.32606541889777829,0.47880403157894741,7.825570053546679,22.982593515789475,17.213085596142573,23.027860494065653,2.4103418296573671,147.65575504641797,1.1597418816597087E-2,19.652663848384286,-137378.48826372108,2697.217055586515,6.1170161793573565E-3,3.5792173491154777,-153123.82472456532,4719.2267597230402,1.2599610389610389,4.1020218450747423E-2,48.89784103826431,-52846.034988895,685.98255618858104]
["DBL","DBL3H00250",2.5,3,1.8,2.4,6000,11.536999999999999,9000,5.0999999999999996,11,50,0.14000000000000001,670,6,5281.6697041799443,7559.8738607053911,7840,1.6180147162510377,803.57142857142844,3.9693446757043227,2.5240092890699493,3.7262582005751964E-2,-22.542586627160492,9,29.119495168,9,-2353.1321600000001,7.5,2365.1321600000001,9,0.49565437893157793,0.72798737920000001,11.89570509435787,34.9433942016,26.170162120803372,23.029484006396871,2.4117462845516,147.74179091290171,4.2167009854839343E-3,6.1146970710781732,-149925.0479728948,5281.6697041799443,2.5494884489743047E-3,1.0381964502092076,-153556.2148130773,7559.8738607053911,2.3506,8.6342179881249217E-3,11.558652861064209,-140303.75440374122,3416.9385914766226]
["DBL","DBL3N00300",3,2.1,2.6,1.9,3000,13.87,9000,11.5,25,88,0.17,670,6,2820.6853331160528,4202.7617764020979,4454.545454545454,2.4396317631463873,661.76470588235293,3.3077989147045148,2.0999028625811103,6.276610057813603E-2,-22.550188523456789,9,29.125652704,9,-2353.7604799999999,7.5,2365.7604799999999,9,0.28914701206655774,0.42474910193333332,6.9395282895973862,20.387956892799998,15.268671910218634,23.030701943922061,2.412799625722275,147.80631781276455,1.2105039580304146E-2,17.018279066174461,-144314.12195331251,2820.6853331160528,7.9041780255662396E-3,3.2615353864412282,-153320.58532163582,4202.7617764020979,1.8607196969696969,1.8529581192209019E-2,26.763468898749597,-130540.18583760533,2028.5465131773431]
["DBL","DBL4N00260",2.6,1.9,2.2999999999999998,1.76,3000,11.696,9000,9.5,40,82,0.21,670,6,2757.5298638182544,4497.1365264804444,4780.4878048780483,2.1502863473519551,535.71428571428578,3.8164531577765635,2.4909253378932972,7.6940604405478105E-2,-22.560324385185183,9,29.133862752000002,9,-2354.5982399999998,7.5,2366.5982399999998,9,0.30187806034566494,0.44354438484615383,7.2450734482959582,21.290130472615385,15.943641819965729,23.032326264912953,2.414204080616507,147.89235367924826,1.5375994140163426E-2,11.532293788348614,-148719.25728655621,2757.5298638182544,7.0730667416002329E-3,2.3163907677924471,-153464.50319047019,4497.1365264804444,1.7167764227642277,3.6830207449847545E-2,21.512239000401376,-136457.85682590757,1654.834342118203]
["DBL","DBL4H00260",2.6,3,2.2999999999999998,2.8,3000,11.18,9000,3.8,15,52,0.21,670,6,4878.6046548398872,7231.8207621307947,7538.4615384615381,1.87681792378692,535.71428571428578,3.8164531577765635,2.6058911227191417,4.2183239981241114E-2,-22.560324385185183,9,29.133862752000002,9,-2354.5982399999998,7.5,2366.5982399999998,9,0.47664956896683935,0.70033323923076918,11.439589655204145,33.615995483076922,25.174171294682729,23.032326264912953,2.414204080616507,147.89235367924826,5.4755514654001598E-3,4.4150667905253691,-151861.77970000001,4878.6046548398872,2.8147519070418868E-3,0.88257457190048982,-153591.9828148146,7231.8207621307947,2.5787179487179483,1.3258894405460749E-2,8.6159416792364958,-146800.60770894928,3018.3540792536855]
["DBL","DBL4N00530",5.3,3.2,4.5999999999999996,2.77,3000,24.75,9000,6.14,30,100,0.28000000000000003,670,6,2135.2277730499918,3686.524271197698,3920,4.4398110033872031,401.78571428571422,1.8726848077197147,1.1777062762020203,5.4851840885355788E-2,-22.578062143209877,9,29.148230336000001,9,-2356.06432,7.5,2368.06432,9,0.24944742388346763,0.36664440674213844,5.9867381732032232,17.598931523622646,13.178422224974444,23.035169938171844,2.416661876681415,148.04291644559481,2.487654712052445E-2,15.891991002095363,-147350.11554973299,2135.2277730499918,1.0500457654814156E-2,2.9148144081790948,-153451.59642414679,3686.524271197698,2.7408288000000001,2.1569919943208529E-2,14.014977870351885,-148753.50988233867,2321.2339352407935]
["DBL","DBL4H00530",5.3,6.5,4.5999999999999996,6,3000,24.3,9000,1.65,9.3000000000000007,49,0.28000000000000003,670,6,4082.8803502187902,7562.3178165312938,8000,3.5354591761426972,401.78571428571422,1.8726848077197147,1.1995156516872427,2.8896140580583422E-2,-22.578062143209877,9,29.148230336000001,9,-2356.06432,7.5,2368.06432,9,0.5066900797632935,0.74474645119496863,12.160561914319045,35.747829657358494,26.768670144479334,23.035169938171844,2.416661876681415,148.04291644559481,8.0870991348324494E-3,4.1733461916485854,-151850.50370310832,4082.8803502187902,2.5863080145567341E-3,0.75339771749051754,-153604.89877960016,7562.3178165312938,5.3800170068027207,6.9885466993568207E-3,3.7485857315333218,-152200.87057615002,4406.2615946390706]
["DBL","DBL4N00750",7.5,4.0999999999999996,6.5,3.7,3000,35.15,9000,3.8,22.6,112,0.43,670,6,2124.0900848107913,3324.6118936822086,3500,6.3917960354392633,261.62790697674421,1.3237266048225023,0.83012853530583219,4.7559835179195209E-2,-22.616071624691358,9,29.179018016000001,9,-2359.2059199999999,7.5,2371.2059199999999,9,0.2259136477491753,0.33231659407111108,5.421927545980207,15.951196515413333,11.942677814584492,23.041268285220337,2.4219285825347874,148.36555094490882,2.650362437423711E-2,14.164790947695316,-149665.24954974666,2124.0900848107913,1.3065448676711947E-2,2.7376573361930303,-153514.63042708841,3324.6118936822086,3.7137857142857142,1.7936390308751153E-2,8.8036742149985141,-152119.34359686245,2677.1319537544032]
["DBL","DBL4H00750",7.5,9.3000000000000007,6.4,8.4,3000,34.506,9000,0.86,5.3,49,0.43,670,6,4713.6929238384037,7717.4341533082652,8000,4.6702741437869708,261.62790697674421,1.3238572717645745,0.84562157352344525,2.1218737992150346E-2,-22.616071624691358,9,29.179018016000001,9,-2359.2059199999999,7.5,2371.2059199999999,9,0.51243827416276344,0.75379129874666673,12.298518579906323,36.181982339840005,27.089488701374584,23.041268285220337,2.4219285825347874,148.36555094490882,6.2076710937708952E-3,3.1229962430446174,-152648.47464243328,4713.6929238384037,2.5108153554840081E-3,0.53043273787652168,-153634.70398902424,7717.4341533082652,7.2673346938775509,3.9268588610241678E-3,1.9772244247468989,-153256.93873117288,6000.5432236647839]
["DBL","DBL4N00950",9.5,6.1,8,5.6,3000,42.625,9000,1.61,10,94,0.65,670,6,3013.4051771607901,4038.3014527294663,4170.2127659574471,7.4808492736352665,173.07692307692307,1.0456436398760554,0.6856111033431086,3.4564281535265515E-2,-22.671818864197533,9,29.224173280000002,9,-2363.8136,7.5,2375.8136,9,0.26545742591961269,0.39093740571929825,6.3709782220707041,18.764995474526316,14.046122357684247,23.050224263458681,2.4296530844530677,148.83874821056941,1.4381008959703933E-2,7.1743899582798347,-152207.68856740984,3013.4051771607901,9.0611050818748574E-3,1.4455279799293277,-153604.87960783276,4038.3014527294663,5.5145762411347512,1.0296406991371226E-2,3.6818899566733432,-153280.44653539351,3683.6858403554311]
["DBL","DBL5N01050",10.5,6.5,8.5,5.7,3000,48,9000,2.25,19.8,97,0.81,670,6,1917.2866713738542,3755.8004788639892,4041.2371134020618,7.9961330140906739,138.88888888888889,0.946554563563475,0.60952111400000009,4.1714979583144039E-2,-22.712362311111111,9,29.257013472000004,9,-2367.16464,7.5,2379.16464,9,0.25599741236748058,0.37732259438095239,6.1439378968195335,18.111484530285715,13.554676141432939,23.056746459855987,2.4352709040299971,149.18289167650428,3.5031528165451201E-2,11.232596922913823,-150311.5918367347,1917.2866713738542,1.0320842513719045E-2,2.1189909579797646,-153544.69607078331,3755.8004788639892,5.6054982817869421,1.4740748806449017E-2,5.1239398779878425,-152966.40302175487,3052.2358094348592]
["DBL","DBL5H01050",10.5,14.1,8.5,13,3000,52.54,9000,0.52,4.5,45,0.81,670,6,3863.5689346390782,8216.7311176794683,8711.1111111111095,5.0221792548803545,138.88888888888889,0.946554563563475,0.55685217875904081,1.9229205163029145E-2,-22.712362311111111,9,29.257013472000004,9,-2367.16464,7.5,2379.16464,9,0.55531746375099633,0.81849978165714299,13.327619130023912,39.287989519542862,29.403220552954533,23.056746459855987,2.4352709040299971,149.18289167650428,9.4864941083723058E-3,2.8595412566499929,-152654.49676561932,3863.5689346390782,2.2194399860642092E-3,0.46161111470063243,-153637.69323194874,8216.7311176794683,11.389371851851852,3.3209129788866554E-3,1.1917122025505746,-153488.66938596198,6621.3841598775234]
["DBL","DBL5N01350",13.5,8.6999999999999993,10.7,7.3,3000,62,9000,1.71,16.5,94,0.91,670,6,1782.7422471759269,3849.8552321665934,4170.2127659574471,9.9068017833111792,123.62637362637362,0.73643172440451232,0.47221836438709675,3.8546065607777638E-2,-22.737701965432098,9,29.277538591999999,9,-2369.2590399999999,7.5,2381.2590399999999,9,0.26654703004433394,0.39307806442962961,6.3971287210640151,18.867747092622221,14.119186179462281,23.060826574487265,2.4387820412655792,149.39798134271362,4.1008384057811431E-2,11.12402010137558,-150162.873268,1782.7422471759269,9.8478605730022897E-3,1.9727882825770509,-153553.8853098723,3849.8552321665934,7.0859141843971631,1.2853429156984359E-2,3.9309204612864965,-153226.80738815753,3303.1634348649441]
["DBL","DBL5H01350",13.5,18.600000000000001,10.7,15.7,3000,62.05,9000,0.38,3.1,44,0.91,670,6,4458.5210083774255,8627.0174631560531,8909.0909090909081,5.4481170343876819,123.62637362637362,0.73643172440451232,0.471837849991942,1.6883115538740161E-2,-22.737701965432098,9,29.277538591999999,9,-2369.2590399999999,7.5,2381.2590399999999,9,0.56985916768098999,0.84037379291851855,13.676620024343761,40.337942060088892,30.185846314712467,23.060826574487265,2.4387820412655792,149.39798134271362,7.1350778384935646E-3,2.4758131312281417,-152872.46453244297,4458.5210083774255,2.0266009052471862E-3,0.32682929018379203,-153650.20643273217,8627.0174631560531,11.285584848484845,2.5841732586899986E-3,0.87417877381507836,-153565.31863008926,7541.4963654876065]
["DBL","DBL5N01700",17,10.4,14,9.1,3000,78.72,9000,1.25,12.6,99,1.1299999999999999,670,6,1883.8099949357147,3691.8932322249884,3959.5959595959598,13.308106767775012,99.557522123893818,0.58490729384401297,0.37249357032520325,3.6696334754414583E-2,-22.793449204938273,9,29.322693856000001,9,-2373.8667199999995,7.5,2385.8667199999995,9,0.25312904763223015,0.37372060796862749,6.0750971431735232,17.93858918249412,13.420789344684046,23.069812949941699,2.4465065431838591,149.87117860837418,3.7055681155040154E-2,10.322272936996173,-150946.18246643597,1883.8099949357147,1.0746278590662506E-2,1.9223598900505074,-153569.73748732591,3691.8932322249884,8.9686868686868682,1.1917694680182812E-2,2.876629266555633,-153452.92470316283,3469.6640775057008]
["DBL","DBL5H01700",17,20,14,17.3,3000,78.260000000000005,9000,0.36,3.3,52,1.1299999999999999,670,6,3849.7377980998622,7239.9079347147672,7538.4615384615381,9.7600920652852317,99.557522123893818,0.58490729384401297,0.37468302908254536,1.8844999251672434E-2,-22.793449204938273,9,29.322693856000001,9,-2373.8667199999995,7.5,2385.8667199999995,9,0.48678663006198103,0.71869347686274521,11.682879121487545,34.497286889411768,25.809210278238549,23.069812949941699,2.4465065431838591,149.87117860837418,9.5373037198183477E-3,2.9852959351416128,-152840.03625921108,3849.7377980998622,2.8674590110836359E-3,0.46171763351589684,-153644.29001728,7239.9079347147672,14.240000000000002,3.2409555313663977E-3,0.83683760481618419,-153599.25358941988,6756.3788553728209]
["DBL","DBL5N02200",22,13.7,17,11.3,3000,100.8,9000,0.94,9,97,1.31,670,6,1993.599425106891,3808.055388838392,4041.2371134020618,15.65324101860268,85.877862595419842,0.45228821344215686,0.29126626063492067,3.4251848659143026E-2,-22.839060582716051,9,29.359639072,9,-2377.6366400000002,7.5,2389.6366400000002,9,0.25774724889049694,0.38089683265757573,6.1859339733719265,18.283047967563636,13.675930838344899,23.077175783125572,2.4528265902079065,150.258340007551,3.3033512994437991E-2,9.9133087769103838,-151052.83805647868,1993.599425106891,1.0134765209040697E-2,1.7375418520338772,-153583.78287576869,3808.055388838392,11.002086597938145,1.0530398108715464E-2,2.1598177750753424,-153540.05450043757,3717.2870796137017]
["DBL","DBL6N02200",22,15.1,16,12,3000,101.61599999999999,9000,0.72,8.5,88,2.5099999999999998,670,6,2009.9750487368631,4198.937823682586,4454.545454545454,13.602124352634828,44.820717131474105,0.45340755813640382,0.29135117020941587,3.1480979769726969E-2,-23.143136434567904,9,29.605940512,9,-2402.76944,7.5,2414.76944,9,0.28469356100583942,0.4233425205787878,6.8326454641401462,20.320440987781815,15.181093285834425,23.126498579270908,2.4949602370348876,152.8394160020631,3.3759464464858925E-2,7.6540652075951332,-151772.70628221467,2009.9750487368631,8.419092870149766E-3,1.2329859462942316,-153614.92154107182,4198.937823682586,11.235239393939395,8.9765511695471898E-3,1.6660147607457851,-153574.39497730427,4044.4724212794258]
["DBL","DBL6N02900",29,17.5,20,13.5,3000,133.65,9000,0.55000000000000004,6.5,100,3.82,670,6,2116.5399046720336,3759.7115446666517,3920,17.720865366000044,29.450261780104714,0.3448682931020004,0.22353026250654695,3.3926500598199565E-2,-23.475085906172836,9,29.874819584000001,9,-2430.2060799999999,7.5,2442.2060799999999,9,0.25088932266753561,0.37558142436781611,6.0213437440208546,18.027908369655172,13.450453469177832,23.180811439713576,2.5409561348210068,155.65709062940536,3.0342566754982293E-2,7.6830264927722824,-152188.27759778398,2116.5399046720336,1.0536288800560061E-2,1.2474662928812947,-153625.09569620312,3759.7115446666517,13.094999999999999,1.0565798217458207E-2,1.2813277836401389,-153622.95497777179,3752.9350869825098]
["DBL","DBL7N02600",26,17,20,14.1,3000,116.28,9000,0.46,4.5,92.5,9.74,670,6,2819.9860489968733,4115.0239624259439,4237.8378378378384,17.769952075148112,11.550308008213552,0.38860420301662824,0.2673710585483316,3.1104735669480223E-2,-24.975193441975311,9,31.089906687999999,9,-2554.1945599999999,7.5,2566.1945599999999,9,0.27479154568605424,0.42350033148717947,6.5949970964653017,20.328015911384615,15.079569740181018,23.432266585280207,2.7488154591674427,168.39039886899815,1.7220824282653806E-2,5.6032601730168201,-152746.64354809301,2819.9860489968733,8.8305904092091242E-3,0.99703881228745461,-153634.95437857683,4115.0239624259439,13.528569369369368,8.8971005009516185E-3,1.1113456192638624,-153627.91266368277,4093.3945180072938]
["DBL","DBL7N03200",32,20,23,15.8,3000,143.68,9000,0.36,3.6,97,11.41,670,6,2831.9162601951662,3946.7562203978705,4041.2371134020618,20.159731338806388,9.8597721297107803,0.31683880991444852,0.21876862605790645,3.2213303383261414E-2,-25.398365669135799,9,31.432676191999999,9,-2589.1710400000002,7.5,2601.1710400000002,9,0.26348317129820747,0.40927963791666661,6.3235961111569798,19.645422619999998,14.550678256841687,23.50495211097995,2.8074514510016568,171.9823962946941,1.7145039590367294E-2,5.4313926351874064,-152880.17531200001,2831.9162601951662,9.6305463755274878E-3,0.91914532359160706,-153641.55265899989,3946.7562203978705,15.196701030927835,9.6121105516927437E-3,0.88007178976827916,-153643.42059849223,3952.5270959846976]
["DBL","DBL7N04000",40,23.4,26,17,3000,160.74,9000,0.3,2.9,103.5,13.94,670,6,2920.301063693621,3716.834376251923,3787.4396135265702,22.654772910824359,8.0703012912482066,0.25480387227307189,0.19878040144332462,3.4113881900241054E-2,-26.039458923456792,9,31.951961728000001,9,-2642.1593599999997,7.5,2654.1593599999997,9,0.24779073831484708,0.38941453355999994,5.9469777195563296,18.691897610879998,13.812828500641247,23.616509499740783,2.8962832230618742,177.42416484979037,1.6216734646880525E-2,5.0571060598934992,-153067.15242593733,2920.301063693621,1.0882486140668387E-2,0.88934365739657661,-153645.54140957896,3716.834376251923,16.536644122383251,1.0831024235550506E-2,0.74285636957769552,-153651.1213893948,3732.3209022605124]
["DBL","DBL8N04000",40,23,32,20,3000,139.19999999999999,9000,0.35,7.5,105,7.11,670,6,1948.60539810553,3433.5055264506582,3733.3333333333335,30.843985262798245,15.822784810126581,0.25131825051477297,0.2194690806896552,3.5534519343092388E-2,-24.308760533333334,9,30.550096032000003,9,-2499.11184,7.5,2511.11184,9,0.2404904287872931,0.3659646920500001,5.7717702908950343,17.566305218400004,13.063549907475032,23.319350925851271,2.6564725498716446,162.73354064769259,3.769958647680717E-2,5.0947754889396242,-153075.411853,1948.60539810553,1.2663718386486313E-2,1.2627819521472221,-153627.84085581251,3433.5055264506582,19.838571428571427,1.1735568503445723E-2,0.83153240713572329,-153648.320949113,3583.10614093805]
["DBL","DBL8N06800",68,37,50,28.6,3000,259,9000,0.12,3.4,112,11.36,670,6,2224.3838751757144,3381.0413690339992,3500,47.713751785796006,9.9031690140845079,0.14906846547452951,0.12132206035521235,3.6699273820539204E-2,-25.385695841975306,9,31.422413632000001,9,-2588.1238399999997,7.5,2600.1238399999997,9,0.22936400370318685,0.35619770354901958,5.5047360888764842,17.09748977035294,12.6640943956826,23.502764860391657,2.8056958823838656,171.8748514615894,2.9538327907066585E-2,3.2805938886360808,-153449.50908278546,2224.3838751757144,1.3244462544745124E-2,0.66602868400794624,-153655.15923533321,3381.0413690339992,28.611000000000001,1.2681235706010751E-2,0.29480445019429202,-153662.26790370187,3469.3862090060711]
["DBL","DBL8L09300",93,34,70,32,2000,319.77999999999997,6000,0.16,4.4000000000000004,164,15.3,670,6,1760.3862359333366,2302.1233438887266,2390.2439024390242,66.52558154527965,7.3529411764705879,0.1098917238839454,0.10079149215085374,5.3539686746006634E-2,-26.384078222222222,9,32.231103360000006,9,-2670.6431999999995,7.5,2682.6431999999995,9,0.15525284549499827,0.24548779440860222,3.7260682918799586,11.783414131612906,8.6971925905192737,23.67718711491467,2.9440346894657852,180.34938431023735,4.6482683024047539E-2,5.3133903752165814,-153401.5807064299,1760.3862359333366,2.8359793798970447E-2,1.4525504615718106,-153644.38832128001,2302.1233438887266,31.96,2.7004398815387569E-2,0.39527882076776288,-153662.54768974803,2378.1228881211746]
["DBL","DBL8L11500",115,43,85,32.5,2000,395.66,6000,0.11,3.9,164,19,670,6,1681.3410884637954,2321.8354698296271,2390.2439024390242,80.172467952555593,5.9210526315789478,8.9511354924322106E-2,8.3381016023858862E-2,5.3477692665472809E-2,-27.321645432098769,9,32.990532799999997,9,-2748.136,7.5,2760.136,9,0.15991041536104877,0.25699146927536232,3.8378499686651706,12.335590525217391,9.0759342938683361,23.844742792175253,3.0739467671823091,188.30770195998292,5.1537988275487841E-2,4.6226383980461767,-153465.37580161463,1681.3410884637954,2.8068235056581497E-2,1.0082295030658652,-153654.55132054159,2321.8354698296271,32.267271341463413,2.6988741242284262E-2,0.28358842698938641,-153663.25246880649,2380.8797299835892]
["AKMH","AKMH21C",0.317,1.33,0.255,0.85,8000,1.39,8000,13,19,19.5,1.0699999999999999E-2,675,6,8000,8000,8000,0.255,10514.018691588786,31.281412780309662,20.930184307798566,"NA",-22.509822454123455,9,29.092956187840002,9,-2350.4241007999999,7.5,2362.4241007999999,9,1.7325713651825199,2.5429568697310203,41.581712764380477,122.06192974708897,91.428367030528932,23.024237670769807,2.4072063841059919,147.463679974493,1.2890798205684537E-3,2.5606237543721759,-149353.15581100917,9816.3682187136947,3.8328561689952325E-4,0.14798849945965398,-153649.60118607999,19829.739899773977,0.33704615384615388,0.2237529721483377,40.1438992568076,905857.7932549098,-9999]
["AKMH","AKMH22C",0.63300000000000001,1.18,0.4,0.65573769999999998,8000,2.65,8000,20,35.5,39,1.61E-2,675,6,5390.9579116147352,8000,8000,0.4,6987.5776397515529,15.673066301360668,10.978892280875472,"NA",-22.511190795456788,9,29.094064544320002,9,-2350.5371984000003,7.5,2362.5371984000003,9,0.76980580537497634,1.1299037704810952,18.475339328999432,54.235380983092575,40.623837250316733,23.024456678608551,2.4073959855167137,147.47529481646831,3.7974916272172253E-3,6.6738954861120785,-146343.01364898961,5390.9579116147352,1.5602129081203784E-3,0.87591285167289734,-153537.89491720483,9643.3632627600946,0.6483442573076923,0.15547096771488514,54.882789090447034,341424.84588206641,-9999]
["AKMH","AKMH22E",0.65400000000000003,2.31,0.41,1.28125,8000,2.68,8000,5.24,9.6999999999999993,20.399999999999999,1.61E-2,675,6,8000,8000,8000,0.41,6987.5776397515529,15.170013279645364,10.855994232955224,0.17755379897249923,-22.511190795456788,9,29.094064544320002,9,-2350.5371984000003,7.5,2362.5371984000003,9,1.458603046174068,2.1409049788920491,{"$f":"IF(move1,IF(AccType=1,SQRT((X182^2*time1+Y182^2*time2+Z182^2*time3+AA182^2*time4)/time)/(C182/D182),SQRT((((X182-Y182)*2/PI()+Y182)^2*time1+Y182^2*time2+((Z182-AA182)*2/PI()+AA182)^2*time3+AA182^2*time4)/time)/(C182/D182)),IF(AccType=1,SQRT((X182^2*time1+Y182^2*time2+Z182^2*time3+AA182^2*time4+AB182^2*time5+AC182^2*time6+AD182^2*time7+AE182^2*time8)/time)/(C182/D182),SQRT((((X182-Y182)*2/PI()+Y182)^2*time1+Y182^2*time2+((Z182-AA182)*2/PI()+AA182)^2*time3+AA182^2*time4+((AB182-AC182)*2/PI()+AC182)^2*time5+AC182^2*time6+((AD182-AE182)*2/PI()+AE182)^2*time7+AE182^2*time8)/time)/(C182/D182)))","v":35.00647310817763},102.76343898681836,76.972727857941535,23.024456678608551,2.4073959855167137,147.47529481646831,1.040243252813512E-3,1.7526334950943647,-151818.72164063901,11267.707293151745,4.1657150533018267E-4,4.5004669382021058E-2,-153662.78326829453,19152.174917667664,0.2430723131127448,4.1680816394225113E-2,14.251446922596092,-31653.391467480222,717.10070530925157]
["AKMH","AKMH23D",0.89700000000000002,1.89,0.57999999999999996,1.1153846199999999,8000,3.75,8000,8.7899999999999991,17.3,33.799999999999997,2.1600000000000001E-2,675,6,{"$f":"IF(AQ183<I183,IF(AQ183<0,0,AQ183),I183)","v":6944.8296114539808},{"$f":"IF(AU183<I183,IF(AU183<0,0,AU183),I183)","v":8000},{"$f":"IF(UAC_V*0.98/L183*1000<I183,IF(UAC_V*0.98/L183*1000<0,0,UAC_V*0.98/L183*1000),I183)","v":8000},{"$f":"C183+(E183-C183)/G183*Q183","v":0.57999999999999996},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M183,(inertia/gear^2+gear_inertia)/M183),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M183,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M183))","v":5208.333333333333},{"$f":"IF((C183+(E183-C183)/G183*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X183^2*time1+Y183^2*time2+Z183^2*time3+AA183^2*time4)/time)/(C183+(E183-C183)/G183*mspeed),SQRT((((X183-Y183)*2/PI()+Y183)^2*time1+Y183^2*time2+((Z183-Y183)*2/PI()+Y183)^2*time3+AA183^2*time4)/time)/(C183+(E183-C183)/G183*mspeed)),IF(AccType=1,SQRT((X183^2*time1+Y183^2*time2+Z183^2*time3+AA183^2*time4+AB183^2*time5+AC183^2*time6+AD183^2*time7+AE183^2*time8)/time)/(C183+(E183-C183)/G183*mspeed),SQRT((((X183-Y183)*2/PI()+Y183)^2*time1+Y183^2*time2+((Z183-Y183)*2/PI()+Y183)^2*time3+AA183^2*time4+((AB183-AC183)*2/PI()+AC183)^2*time5+AC183^2*time6+((AD183-AC183)*2/PI()+AC183)^2*time7+AE183^2*time8)/time)/(C183+(E183-C183)/G183*mspeed))))","v":11.059913671021105},{"$f":"IF(move1,MAX(ABS(X183),ABS(Z183))/H183,MAX(ABS(X183),ABS(Z183),ABS(AB183),ABS(AD183))/H183)","v":7.7587182469120002},{"$f":"IF(AZ183>0,speed/(MIN(AZ183,I183)),\"NA\")","v":0.21187733111689194},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M183+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M183+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.512584476444445},{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M183+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M183+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.095193425920002},{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M183+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M183+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2350.6523904000001},{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M183+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M183+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2362.6523904000001},{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},{"$f":"AH183/Irms","v":0.87011459498647981},{"$f":"AI183/Ipeak","v":1.2771719522247491},20.882750279675516,{"$f":"IF(move1,MAX(ABS(X183),ABS(Z183))/(C183/D183),MAX(ABS(X183),ABS(Z183),ABS(AB183),ABS(AD183))/(C183/D183))","v":61.304253706787961},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X183),ABS(Z183))/(C183/D183),MAX(ABS((X183-Y183)*2/PI()+Y183),ABS((Z183-Y183)*2/PI()+Y183))/(C183/D183)),IF(AccType=1,MAX(ABS(X183),ABS(Z183),ABS(AB183),ABS(AD183))/(C183/D183),MAX(ABS((X183-Y183)*2/PI()+Y183),ABS((Z183-Y183)*2/PI()+Y183),ABS((AB183-AC183)*2/PI()+AC183),ABS((AD183-AC183)*2/PI()+AC183))/(C183/D183)))","v":45.918355861638048},{"$f":"IF((C183+(E183-C183)/G183*mspeed)<0,\"NA\",U183*(C183+(E183-C183)/G183*mspeed)*mspeed/9.55)","v":23.024679750811362},{"$f":"IF(move1,IF(speed1>speed2,AM183/2*time1/time,AM183/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z183*-speed/30*PI(),((Z183-AA183)*2/PI()+AA183)*-speed/30*PI()),IF(AccType=1,X183*-speed/30*PI(),((X183-Y183)*2/PI()+Y183)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z183*-speed/30*PI(),((Z183-AA183)*2/PI()+AA183)*-speed/30*PI()),IF(AccType=1,X183*-speed/30*PI(),((X183-Y183)*2/PI()+Y183)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD183*-speed/30*PI(),((AD183-AE183)*2/PI()+AE183)*-speed/30*PI()),IF(AccType=1,AB183*-speed/30*PI(),((AB183-AC183)*2/PI()+AC183)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD183*-speed/30*PI(),((AD183-AE183)*2/PI()+AE183)*-speed/30*PI()),IF(AccType=1,AB183*-speed/30*PI(),((AB183-AC183)*2/PI()+AC183)*-speed/30*PI()),0)/2*time7/time)))","v":2.4075890980646713},{"$f":"IF(move1,MAX(IF(AccType=1,Z183*-speed/30*PI(),((Z183-AA183)*2/PI()+AA183)*-speed/30*PI()),IF(AccType=1,X183*-speed/30*PI(),((X183-Y183)*2/PI()+Y183)*-speed/30*PI()),0),MAX(IF(AccType=1,Z183*-speed/30*PI(),((Z183-AA183)*2/PI()+AA183)*-speed/30*PI()),IF(AccType=1,X183*-speed/30*PI(),((X183-Y183)*2/PI()+Y183)*-speed/30*PI()),IF(AccType=1,AD183*-speed/30*PI(),((AD183-AE183)*2/PI()+AE183)*-speed/30*PI()),IF(AccType=1,AB183*-speed/30*PI(),((AB183-AC183)*2/PI()+AC183)*-speed/30*PI()),0))","v":147.48712474810986},{"$f":"(L183^2)/1000000+((K183/1000)^2*(D183/C183*H183)^2*PI()*PI()*(O183/2)^2)/1200","v":2.5255428389403568E-3},{"$f":"SQRT(3)*L183*J183*D183/C183*H183/1000","v":4.065994918759702},{"$f":"0.75*J183^2*(D183/C183*H183)^2-(UAC_V*0.98)^2","v":-150046.23567990886},{"$f":"-AO183/2/AN183+SQRT((AO183/2/AN183)^2-AP183/AN183)","v":6944.8296114539808},{"$f":"(L183^2)/1000000+((K183/1000)^2*AV183^2*PI()*PI()*(O183/2)^2)/1200","v":1.1630102913265216E-3},{"$f":"SQRT(3)*L183*J183*AV183/1000","v":0.4958608452911899},{"$f":"0.75*J183^2*AV183^2-(UAC_V*0.98)^2","v":-153610.19455334792},{"$f":"-AS183/2/AR183+SQRT((AS183/2/AR183)^2-AT183/AR183)","v":11281.395757311026},{"$f":"D183+(F183-D183)*((0.85*UAC_V-D183*J183)/L183*1000)/G183","v":0.96359294959126462},{"$f":"(L183^2)/1000000+((K183/1000)^2*AJ183^2*PI()*PI()*(O183/2)^2)/1200","v":4.7854161608052538E-2},{"$f":"SQRT(3)*L183*J183*AJ183/1000","v":23.629391188044366},{"$f":"0.75*J183^2*AJ183^2-(UAC_V*0.98)^2","v":-31480.750131816822},{"$f":"IF(((AX183/2/AW183)^2-AY183/AW183)>0,-AX183/2/AW183+SQRT((AX183/2/AW183)^2-AY183/AW183),-9999)","v":600.93240651248391}]
["AKMH","AKMH23E",0.90400000000000003,2.36,0.57999999999999996,1.3809523800000001,8000,3.78,8000,5.46,11.1,27,2.1600000000000001E-2,675,6,8000,8000,8000,0.57999999999999996,5208.333333333333,10.974425278744608,7.697141117968255,8.9873936108217062E-2,-22.512584476444445,9,29.095193425920002,9,-2350.6523904000001,7.5,2362.6523904000001,9,1.0780791944203183,1.5824266335999999,25.873900666087639,75.956478412799996,56.893223469248262,23.024679750811362,2.4075890980646713,147.48712474810986,1.6171323941706118E-3,2.5197207159359865,-151486.70490867045,8930.8769145396127,7.3601964675661894E-4,0.22401194666265456,-153646.79103146517,14296.933169102225,0.87731215376051908,3.0249794936280949E-2,14.527054807836027,-81292.490607039814,1416.6949839629333]
["AKMH","AKMH23F",0.91700000000000004,3.71,0.59,2.1851851899999999,8000,3.8,8000,2.36,4.68,17.600000000000001,2.1600000000000001E-2,675,6,8000,8000,8000,0.59,5208.333333333333,10.818790205461729,7.6566298489263165,4.5027409996798426E-2,-22.512584476444445,9,29.095193425920002,9,-2350.6523904000001,7.5,2362.6523904000001,9,1.6707507556949894,2.4523620413068703,40.098018136679748,117.71337798272978,88.170142413592416,23.024679750811362,2.4075890980646713,147.48712474810986,6.9296313733870345E-4,1.106046711138674,-152676.67164319096,14066.710124580293,3.0978442400999147E-4,8.8301366630249047E-3,-153663.9370711894,22257.597175479947,0.12273887180707366,1.2913394475033674E-2,6.3431771503827683,-121190.55575192242,2827.6988279487841]
["AKMH","AKMH24D",1.1200000000000001,2.41,0.83,1.3174603199999999,8000,4.68,8000,9.0399999999999991,18.7,40.799999999999997,2.7E-2,675,6,5160.7394062905396,8000,8000,0.83,4166.666666666667,8.8555677452635653,6.2171585005128209,0.34709150424559754,-22.513952817777778,9,29.096301782400001,9,-2350.765488,7.5,2362.765488,9,0.88860805041091995,1.3043543023732143,21.326593209862079,62.609006513914288,46.895378919108502,23.02489877566153,2.4077786994753927,147.49873959008517,4.2896681669379755E-3,6.4333042936442517,-147448.33112645653,5160.7394062905396,1.7114565905279665E-3,0.85914605698122792,-153553.14540873305,9224.4295439668203,1.3448621791799997,5.8589807941795073E-2,29.958445194405424,-18873.829382600175,366.83108896673963]
["AKMH","AKMH24E",1.1200000000000001,2.41,0.83,1.66,8000,4.72,8000,5.46,11.8,32.4,2.7E-2,675,6,7759.2288655161246,8000,8000,0.83,4166.666666666667,8.8555677452635653,6.16447071661017,7.0040912328960897E-2,-22.513952817777778,9,29.096301782400001,9,-2350.765488,7.5,2362.765488,9,0.88860805041091995,1.3043543023732143,21.326593209862079,62.609006513914288,46.895378919108502,23.02489877566153,2.4077786994753927,147.49873959008517,2.1129406418444094E-3,3.1119979254913699,-151357.6320948925,7759.2288655161246,1.0718589841090596E-3,0.44866472261039425,-153616.06046303082,11764.061789692465,1.4642783564814812,2.3716294313865276E-2,14.369059053094899,-104493.27095923628,1817.8511706916995]
["AKMH","AKMH24F",1.1299999999999999,3.38,0.84,2.3333333299999999,8000,4.74,8000,2.96,6.16,23.4,2.7E-2,675,6,8000,8000,8000,0.84,4166.666666666667,8.7771440735393984,6.1384602916455693,4.4272932411531213E-2,-22.513952817777778,9,29.096301782400001,9,-2350.765488,7.5,2362.765488,9,1.2352346916004768,1.8131544989769912,29.645632598411446,87.031415950895578,65.188244569521217,23.02489877566153,2.4077786994753927,147.49873959008517,1.1121791840143496E-3,1.7009235504694538,-152343.07584349587,10963.995143504042,5.5417768378432234E-4,0.18414502278180669,-153648.51795720318,16485.661371659608,1.5349413616453842,1.2483620339416218E-2,7.8205533327296992,-125739.63808985791,2875.887083557036]
["AKMH","AKMH31C",1,1.29,0.82,0.96470588000000002,6000,3.8,8000,21.4,37.5,54.5,3.3000000000000002E-2,675,8,3810.2324227162044,6672.3357669464294,7192.660550458716,0.79982992699160704,3409.090909090909,9.9178197131057928,7.6572456025263165,"NA",-22.515473197037039,9,29.097533289600001,9,-2350.8911520000001,7.5,2362.8911520000001,9,0.53272800062755488,0.78199620715800011,12.785472015061316,37.535817943584007,28.114888317687804,23.025142146490033,2.4079893677095279,147.51164497005774,7.4170503511531453E-3,9.9024853803648831,-145410.55191412001,3810.2324227162044,3.1476997858690793E-3,1.9781450520207413,-153334.6457497825,6672.3357669464294,0.97923568402666672,0.14924647465647034,56.794628832414311,117830.81223901245,-9999]
["AKMH","AKMH31E",1.04,2.76,0.74,1.8048780499999999,8000,3.92,8000,4.76,8.6,26.1,3.3000000000000002E-2,675,8,8000,8000,8000,0.74,3409.090909090909,9.5376477827214146,7.4228401248979594,8.3237640552016309E-2,-22.515473197037039,9,29.097533289600001,9,-2350.8911520000001,7.5,2362.8911520000001,9,1.0959520585361142,1.6087578501461535,26.302849404866741,77.22037680701537,57.839215680395291,23.025142146490033,2.4079893677095279,147.51164497005774,1.7345267829895459E-3,2.2385659686787025,-151824.92776231765,8732.7339583757384,6.9678016677149443E-4,0.27216797831080664,-153636.81476768624,14655.067455876806,1.2648206280187742,3.3240893510647337E-2,12.446019656932911,-96815.375750223728,1529.6439643066269]
["AKMH","AKMH31H",1.08,5.59,0.76,3.6190476199999999,8000,3.98,8000,1.31,2.4,13.7,3.3000000000000002E-2,675,8,8000,8000,8000,0.76,3409.090909090909,9.1846012887952284,7.3109380124623122,3.5740787479127907E-2,-22.515473197037039,9,29.097533289600001,9,-2350.8911520000001,7.5,2362.8911520000001,9,2.1374888914068553,3.1376391027944446,51.299733393764527,150.60667693413333,112.80665065738933,23.025142146490033,2.4079893677095279,147.51164497005774,5.0935456003155808E-4,0.64035914287776985,-153117.80703305031,16720.942438243841,1.8780681977851614E-4,-1.2203381735823646E-2,-153663.80163763947,28636.727491261721,-0.39257958044249985,9.8333150320645199E-3,3.5066078035952608,-137285.53246279078,3562.4272282157067]
["AKMH","AKMH32C",1.72,1.3,1.57,1.12142857,3000,6.84,8000,23.8,46.5,89.8,5.8999999999999997E-2,675,8,2464.2594044082307,4034.2772048518818,4365.2561247216036,1.5182861397574059,1906.7796610169491,5.7663193013085028,4.2548055293567257,0.31641791138644804,-22.52206150716049,9,29.102869820800002,9,-2351.435696,7.5,2363.435696,9,0.31214085303928024,0.4582573978565892,7.4913804729427254,21.996355097116282,16.475145193039921,23.026196873630557,2.4089022633907784,147.56756828327212,1.5668815573745158E-2,19.13748785975347,-142309.7829579773,2464.2594044082307,8.4052986474494468E-3,4.0539982769603196,-153154.48795549138,4034.2772048518818,1.0951399919977727,8.5297037226834363E-2,60.98782869157678,-38352.21928856014,402.3917417178472]
["AKMH","AKMH32E",1.77,2.56,1.1000000000000001,1.5068493199999999,7000,7.04,8000,6.32,12.8,47.1,5.8999999999999997E-2,675,8,5254.6407754907004,8000,8000,1.0042857142857144,1906.7796610169491,5.6065413571783242,4.1339303722727276,6.4604482251456818E-2,-22.52206150716049,9,29.102869820800002,9,-2351.435696,7.5,2363.435696,9,0.59731360456434535,0.87692263113521662,14.335526509544287,42.0922862944904,31.526883665360007,23.026196873630557,2.4089022633907784,147.56756828327212,4.4537167907113609E-3,5.2497421263607684,-150558.19534787451,5254.6407754907004,2.2685929666555467E-3,0.78658845534923505,-153594.27422815343,8056.7443565651447,1.5256290697053563,2.3648328022582672E-2,16.254726143295049,-123888.60658833133,1970.8223026684057]
["AKMH","AKMH32H",1.82,4.92,0.95,2.4358974400000002,8000,7.18,8000,1.71,3.53,24.8,5.8999999999999997E-2,675,8,8000,8000,8000,0.95,1906.7796610169491,5.4532031360532152,4.0533244875766021,2.8416685614089401E-2,-22.52206150716049,9,29.102869820800002,9,-2351.435696,7.5,2363.435696,9,1.1164246638882522,1.6390352508967034,26.794191933318054,78.673692043041768,58.926149062375742,23.026196873630557,2.4089022633907784,147.56756828327212,1.2328062965436394E-3,1.4256948394533626,-152837.79122689422,10571.201823705151,6.1600796359837884E-4,5.6434409460977761E-2,-153662.70543274778,15748.221340372174,0.7683083732751621,6.3088636613918263E-3,4.3282912692580293,-146049.00532016807,4480.6053810296307]
["AKMH","AKMH33C",2.25,1.27,2.14,1.1505376300000001,2000,9.68,8000,26.6,53.6,120,8.5000000000000006E-2,675,8,1801.8181909857319,3006.4410534291956,3266.6666666666665,2.0846457420613946,1323.5294117647059,4.4077800978340349,3.0070461107438016,0.1981383411008879,-22.528649817283949,9,29.108206352,9,-2351.9802399999999,7.5,2363.9802399999999,9,0.23311853580420586,0.3422909450651852,5.5948448593009408,16.42996536312889,12.305612365855046,23.027251796103748,2.4098151590720303,147.62349159648659,2.5686549267685453E-2,30.207867674181582,-137821.72101699887,1801.8181909857319,1.4872196698274597E-2,6.1787546793483372,-153001.2046981325,3006.4410534291956,1.1175769665972501,7.164987229445216E-2,68.034115108220874,-73305.652455579024,642.60129445964003]
["AKMH","AKMH33E",2.3199999999999998,2.2000000000000002,1.82,1.6545454500000001,4500,9.8800000000000008,8000,9.0299999999999994,18.5,70.599999999999994,8.5000000000000006E-2,675,8,3535.5099855057251,5306.8300979330616,5552.4079320113315,1.730352211340771,1323.5294117647059,4.2770129406497501,2.9461747319838056,6.8057265785903237E-2,-22.528649817283949,9,29.108206352,9,-2351.9802399999999,7.5,2363.9802399999999,9,0.39164293790076671,0.57505436399425292,9.3994305096184014,27.60260947172414,20.673629246192803,23.027251796103748,2.4098151590720303,147.62349159648659,8.937709586860642E-3,10.34533883045432,-148295.90682871491,3535.5099855057251,5.1070312425785707E-3,1.8223571351431542,-153497.42969167521,5306.8300979330616,1.6503665504888261,2.4233679715332176E-2,22.828101887392634,-127526.12895029757,1870.8355824057951]
["AKMH","AKMH33H",2.38,4.78,0.88,1.69230769,8000,10.1,8000,1.98,4.0999999999999996,33.4,8.5000000000000006E-2,675,8,8000,8000,8000,0.87999999999999989,1323.5294117647059,4.1720512251802644,2.882000628910891,2.6473398105273986E-2,-22.528649817283949,9,29.108206352,9,-2351.9802399999999,7.5,2363.9802399999999,9,0.82948119254093633,1.2179379058347339,19.907548620982471,58.461019480067229,43.785767549384971,23.027251796103748,2.4098151590720303,147.62349159648659,2.0257893228701127E-3,2.3235102772473386,-152454.13679038465,8120.5118707104775,1.1176004551273072E-3,0.11001013836815809,-153661.28785754603,11676.59078676948,0.96041829977082305,5.3565976673443667E-3,5.015396257873534,-148026.87612869503,4809.5055257810291]
["AKMH","AKMH41C",1.85,1.39,1.68,1.2537313400000001,3000,5.65,6000,21.3,66.099999999999994,86.3,8.1000000000000003E-2,675,10,2228.6902963835423,3955.8921022279396,4542.2943221320975,1.62583278087375,1388.8888888888889,5.3615120952370248,5.1517496189734509,0.31289298397252818,-22.52763623111111,9,29.107385347200001,9,-2351.8964640000004,7.5,2363.8964640000004,9,0.31030988797255532,0.45562236072756751,7.4474373113413277,21.86987331492324,16.38002979722809,23.027089487625755,2.4096747135826071,147.61488800983821,2.3637601186047311E-2,13.515824570424,-147531.98074911561,2228.6902963835423,8.7994128245462537E-3,3.9053875424061513,-153152.02743345988,3955.8921022279396,1.2266286667308615,0.24848862422313189,52.151369073108476,-62368.400418130477,406.92492639814265]
["AKMH","AKMH41E",1.92,2.71,1.44,2.02816901,6000,5.77,6000,6.04,18.399999999999999,45.6,8.1000000000000003E-2,675,10,4480.6337142258726,6000,6000,1.44,1388.8888888888889,5.1673063510672188,5.0446075125129992,0.1004879512803669,-22.52763623111111,9,29.107385347200001,9,-2351.8964640000004,7.5,2363.8964640000004,9,0.58293563524820391,0.85591378353854175,13.990455245956893,41.083861609850004,30.770863080186992,23.027089487625755,2.4096747135826071,147.61488800983821,6.696594209071819E-3,3.8851365188560734,-151849.22456787797,4480.6337142258726,2.3315883052228877E-3,0.90805518485527326,-153564.86322008423,7923.1950413112108,1.9034866439207456,6.7992728921837095E-2,14.679189818155033,-127757.1568226009,1267.0569242503059]
["AKMH","AKMH41H",1.96,5.32,1.47,3.9729729699999998,6000,5.84,6000,1.58,5,23.7,8.1000000000000003E-2,675,10,6000,6000,6000,1.47,1388.8888888888889,5.0618511194127853,4.9841413265753429,4.6917654761973876E-2,-22.52763623111111,9,29.107385347200001,9,-2351.8964640000004,7.5,2363.8964640000004,9,1.1210064298289129,1.6459533380857145,26.904154315893908,79.005760228114298,59.173488938598915,23.027089487625755,2.4096747135826071,147.61488800983821,1.8533116999373655E-3,1.028097891283325,-153193.55132098612,8818.5812525415204,5.86094333295779E-4,0.14131890894368407,-153655.11118498415,16071.488141334325,2.1788845302627844,1.856087620221784E-2,3.837896308431461,-147108.13819265438,2713.7749130783623]
["AKMH","AKMH42C",3.22,1.35,2.98,1.2416666700000001,1500,10.5,6000,27.5,97.4,154,0.14499999999999999,675,10,1282.8923583429155,2237.7268324406277,2545.4545454545455,2.8619637068094992,775.86206896551732,3.0820234106114786,2.7733829927619049,0.21373424487654019,-22.543853609876543,9,29.120521424,9,-2353.2368799999999,7.5,2365.2368799999999,9,0.1731726990163622,0.25435238045031056,4.1561447763926926,12.208914261614906,9.1435758968839433,23.029686977933643,2.411921841413379,147.75254539621218,6.1517654942725743E-2,32.290980911651616,-142672.39677605152,1282.8923583429155,2.6562301175501679E-2,8.8606637750627595,-152836.37980124485,2237.7268324406277,1.2079590592045455,0.18679895422535858,67.070279498882925,-106244.3003029782,595.71153208070473]
["AKMH","AKMH42E",3.28,2.63,2.72,2.1587301600000002,3500,10.7,6000,7.8,26.8,80.900000000000006,0.14499999999999999,675,10,2680.8665489958266,4461.726723421476,4845.4882571075404,2.5661237242525643,775.86206896551732,3.0255838522726535,2.721544058317757,8.6655476922995023E-2,-22.543853609876543,9,29.120521424,9,-2353.2368799999999,7.5,2365.2368799999999,9,0.33119474229674001,0.48645179970223573,7.9486738151217606,23.349686385707315,17.487192150034183,23.029686977933643,2.411921841413379,147.75254539621218,1.7415558819135809E-2,9.377119144317879,-150305.2178716138,2680.8665489958266,7.1950053663540669E-3,2.293304053611807,-153463.10633454935,4461.726723421476,2.0982531658052626,5.1706299818309875E-2,19.112778809305958,-139710.25979159612,1469.3122580891295]
["AKMH","AKMH42H",3.4,5.76,2.21,3.7457627100000002,6000,10.8,6000,1.67,6,38.299999999999997,0.14499999999999999,675,10,5975.3837887514901,6000,6000,2.21,775.86206896551732,2.9194179494388952,2.6963445762962959,3.7039237776563677E-2,-22.543853609876543,9,29.120521424,9,-2353.2368799999999,7.5,2365.2368799999999,9,0.69975352575082195,1.027783109082353,16.794084618019728,49.333589235952942,36.94721805548712,23.029686977933643,2.411921841413379,147.75254539621218,3.9448577651210112E-3,2.0269507398631794,-152963.78912838866,5975.3837887514901,1.5276130881286263E-3,0.3173016226407771,-153646.8411946822,9925.6246646981344,2.8641543635333679,1.1571614942257519E-2,4.0931495838115648,-150808.66089559259,3437.542512121554]
["AKMH","AKMH42J",3.42,8.06,2.23,5.1860465099999997,6000,11,6000,0.82,3.1,27.5,0.14499999999999999,675,10,6000,6000,6000,2.23,775.86206896551732,2.9023233356837665,2.6473201294545454,2.6072140534002058E-2,-22.543853609876543,9,29.120521424,9,-2353.2368799999999,7.5,2365.2368799999999,9,0.97344286162257998,1.4297721897992204,23.36262867894192,68.629065110362575,51.398105689193933,23.029686977933643,2.411921841413379,147.75254539621218,2.0842104397634257E-3,1.0125320861721425,-153325.0838923874,8337.5416170241569,7.6628036580559116E-4,8.7998366747935625E-2,-153661.44009502471,14103.523699806881,2.2530324048855013,5.9763175361115866E-3,2.0074941420190981,-152331.75777512696,4883.5251676963908]
["AKMH","AKMH43E",4.5599999999999996,2.68,3.83,2.2267441899999998,2500,15.2,6000,8.6300000000000008,32.6,111,0.20899999999999999,675,10,2003.8988435348947,3258.9401867221322,3531.5315315315315,3.6083894654771376,538.27751196172255,2.1772804039349203,1.9166879934736847,8.3548161960909473E-2,-22.560070988641975,9,29.133657500800005,9,-2354.5772959999999,7.5,2366.5772959999999,9,0.24278423538114757,0.35671693211871358,5.8268216491475417,17.122412741698252,12.822556653427824,23.032285651257677,2.4141689692441521,147.89020278258619,2.9759968241241282E-2,14.822038642177127,-149206.30927866665,2003.8988435348947,1.3342834124804465E-2,3.5878786750585392,-153402.80217947124,3258.9401867221322,2.1624364190126268,4.8249820600464274E-2,21.274973530814847,-144479.99507473272,1523.9587740193329]
["AKMH","AKMH43H",4.68,5.24,2.44,2.7415730300000001,6000,15.4,6000,2.12,8.8000000000000007,57.4,0.20899999999999999,675,10,4140.0687847379822,6000,6000,2.44,538.27751196172255,2.1221946997568359,1.89179594161039,3.9209946325504522E-2,-22.560070988641975,9,29.133657500800005,9,-2354.5772959999999,7.5,2366.5772959999999,9,0.46252580318689346,0.67957783700227947,11.100619276485443,32.619736176109413,24.428123620652009,23.03228565125767,2.4141689692441521,147.89020278258619,8.0288462037590366E-3,3.6342477935022752,-152661.82100785975,4140.0687847379822,3.4244648801770605E-3,0.60155399166970613,-153636.54221818177,6610.8328642891756,2.8540805915340766,1.2796520304947382E-2,5.1487106974459094,-151652.53164980197,3247.23613280483]
["AKMH","AKMH43L",4.59,10.9,2.39,5.69047619,6000,15.3,6000,0.56999999999999995,2,27.5,0.20899999999999999,675,10,6000,6000,6000,2.39,538.27751196172255,2.1638117335768969,1.9041606209673205,2.1220659078919377E-2,-22.560070988641975,9,29.133657500800005,9,-2354.5772959999999,7.5,2366.5772959999999,9,0.98098946731900594,1.4413438033710968,23.543747215656143,69.18450256181265,51.810584000095638,23.032285651257677,2.4141689692441521,147.89020278258619,1.8419978693457655E-3,0.98644623618066496,-153342.321925,8860.1877160919248,7.563574140134645E-4,9.8115901650941105E-3,-153663.96817609866,14247.047159047614,0.36138591534260733,2.9640283719827641E-3,1.4066519884738489,-153009.89427547852,6951.4945062103507]
["AKMH","AKMH44E",5.64,2.79,4.76,2.3333333299999999,2000,19.3,6000,8.66,33.9,132,0.27300000000000002,675,10,{"$f":"IF(AQ208<I208,IF(AQ208<0,0,AQ208),I208)","v":1724.9358937592826},{"$f":"IF(AU208<I208,IF(AU208<0,0,AU208),I208)","v":2753.7394089561476},{"$f":"IF(UAC_V*0.98/L208*1000<I208,IF(UAC_V*0.98/L208*1000<0,0,UAC_V*0.98/L208*1000),I208)","v":2969.6969696969695},{"$f":"C208+(E208-C208)/G208*Q208","v":4.4283546600592949},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M208,(inertia/gear^2+gear_inertia)/M208),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M208,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M208))","v":412.08791208791206},{"$f":"IF((C208+(E208-C208)/G208*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X208^2*time1+Y208^2*time2+Z208^2*time3+AA208^2*time4)/time)/(C208+(E208-C208)/G208*mspeed),SQRT((((X208-Y208)*2/PI()+Y208)^2*time1+Y208^2*time2+((Z208-Y208)*2/PI()+Y208)^2*time3+AA208^2*time4)/time)/(C208+(E208-C208)/G208*mspeed)),IF(AccType=1,SQRT((X208^2*time1+Y208^2*time2+Z208^2*time3+AA208^2*time4+AB208^2*time5+AC208^2*time6+AD208^2*time7+AE208^2*time8)/time)/(C208+(E208-C208)/G208*mspeed),SQRT((((X208-Y208)*2/PI()+Y208)^2*time1+Y208^2*time2+((Z208-Y208)*2/PI()+Y208)^2*time3+AA208^2*time4+((AB208-AC208)*2/PI()+AC208)^2*time5+AC208^2*time6+((AD208-AC208)*2/PI()+AC208)^2*time7+AE208^2*time8)/time)/(C208+(E208-C208)/G208*mspeed))))","v":1.761100040345297},{"$f":"IF(move1,MAX(ABS(X208),ABS(Z208))/H208,MAX(ABS(X208),ABS(Z208),ABS(AB208),ABS(AD208))/H208)","v":1.5101965584248704},{"$f":"IF(AZ208>0,speed/(MIN(AZ208,I208)),\"NA\")","v":8.0253047766373611E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M208+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M208+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.576288367407408},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M208+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M208+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.1467935776},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M208+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M208+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2355.9177119999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M208+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M208+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2367.9177119999999},9,{"$f":"AH208/Irms","v":0.20437353233378866},{"$f":"AI208/Ipeak","v":0.3003825135989362},4.9049647760109281,{"$f":"IF(move1,MAX(ABS(X208),ABS(Z208))/(C208/D208),MAX(ABS(X208),ABS(Z208),ABS(AB208),ABS(AD208))/(C208/D208))","v":14.418360652748937},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X208),ABS(Z208))/(C208/D208),MAX(ABS((X208-Y208)*2/PI()+Y208),ABS((Z208-Y208)*2/PI()+Y208))/(C208/D208)),IF(AccType=1,MAX(ABS(X208),ABS(Z208),ABS(AB208),ABS(AD208))/(C208/D208),MAX(ABS((X208-Y208)*2/PI()+Y208),ABS((Z208-Y208)*2/PI()+Y208),ABS((AB208-AC208)*2/PI()+AC208),ABS((AD208-AC208)*2/PI()+AC208))/(C208/D208)))","v":10.796828639051476},{"$f":"IF((C208+(E208-C208)/G208*mspeed)<0,\"NA\",U208*(C208+(E208-C208)/G208*mspeed)*mspeed/9.55)","v":23.034885507197458},{"$f":"IF(move1,IF(speed1>speed2,AM208/2*time1/time,AM208/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z208*-speed/30*PI(),((Z208-AA208)*2/PI()+AA208)*-speed/30*PI()),IF(AccType=1,X208*-speed/30*PI(),((X208-Y208)*2/PI()+Y208)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z208*-speed/30*PI(),((Z208-AA208)*2/PI()+AA208)*-speed/30*PI()),IF(AccType=1,X208*-speed/30*PI(),((X208-Y208)*2/PI()+Y208)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD208*-speed/30*PI(),((AD208-AE208)*2/PI()+AE208)*-speed/30*PI()),IF(AccType=1,AB208*-speed/30*PI(),((AB208-AC208)*2/PI()+AC208)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD208*-speed/30*PI(),((AD208-AE208)*2/PI()+AE208)*-speed/30*PI()),IF(AccType=1,AB208*-speed/30*PI(),((AB208-AC208)*2/PI()+AC208)*-speed/30*PI()),0)/2*time7/time)))","v":2.416416097074924},{"$f":"IF(move1,MAX(IF(AccType=1,Z208*-speed/30*PI(),((Z208-AA208)*2/PI()+AA208)*-speed/30*PI()),IF(AccType=1,X208*-speed/30*PI(),((X208-Y208)*2/PI()+Y208)*-speed/30*PI()),0),MAX(IF(AccType=1,Z208*-speed/30*PI(),((Z208-AA208)*2/PI()+AA208)*-speed/30*PI()),IF(AccType=1,X208*-speed/30*PI(),((X208-Y208)*2/PI()+Y208)*-speed/30*PI()),IF(AccType=1,AD208*-speed/30*PI(),((AD208-AE208)*2/PI()+AE208)*-speed/30*PI()),IF(AccType=1,AB208*-speed/30*PI(),((AB208-AC208)*2/PI()+AC208)*-speed/30*PI()),0))","v":148.02786016896016},{"$f":"(L208^2)/1000000+((K208/1000)^2*(D208/C208*H208)^2*PI()*PI()*(O208/2)^2)/1200","v":3.8962860377216191E-2},{"$f":"SQRT(3)*L208*J208*D208/C208*H208/1000","v":18.903179524888234},{"$f":"0.75*J208^2*(D208/C208*H208)^2-(UAC_V*0.98)^2","v":-148537.01715808435},{"$f":"-AO208/2/AN208+SQRT((AO208/2/AN208)^2-AP208/AN208)","v":1724.9358937592826},{"$f":"(L208^2)/1000000+((K208/1000)^2*AV208^2*PI()*PI()*(O208/2)^2)/1200","v":1.8613523882171343E-2},{"$f":"SQRT(3)*L208*J208*AV208/1000","v":4.4423224732443147},{"$f":"0.75*J208^2*AV208^2-(UAC_V*0.98)^2","v":-153380.85277553531},{"$f":"-AS208/2/AR208+SQRT((AS208/2/AR208)^2-AT208/AR208)","v":2753.7394089561476},{"$f":"D208+(F208-D208)*((0.85*UAC_V-D208*J208)/L208*1000)/G208","v":2.2436630237899164},{"$f":"(L208^2)/1000000+((K208/1000)^2*AJ208^2*PI()*PI()*(O208/2)^2)/1200","v":4.496947853266367E-2},{"$f":"SQRT(3)*L208*J208*AJ208/1000","v":21.377093616317126},{"$f":"0.75*J208^2*AJ208^2-(UAC_V*0.98)^2","v":-147107.23732379495},{"$f":"IF(((AX208/2/AW208)^2-AY208/AW208)>0,-AX208/2/AW208+SQRT((AX208/2/AW208)^2-AY208/AW208),-9999)","v":1586.5310790958592}]
["AKMH","AKMH44H",5.77,5.49,3.31,3.1226415099999998,5000,19.5,6000,2.25,9.1,68,0.27300000000000002,675,10,3584.6142178625078,5569.8317554526257,5764.7058823529414,3.0296427763173082,412.08791208791206,1.7216994593525048,1.4947073629538461,3.8101448418170446E-2,-22.576288367407408,9,29.1467935776,9,-2355.9177119999999,7.5,2367.9177119999999,9,0.39309369969316627,0.57775814825615257,9.4342487926359908,27.732391116295322,20.766707245369656,23.034885507197458,2.416416097074924,148.02786016896016,1.0485429934784497E-2,4.9168074485711939,-152356.9608841736,3584.6142178625078,4.7993016136823633E-3,0.85030428721465912,-153624.90952741913,5569.8317554526257,3.2086497327874266,1.1967051494385018E-2,5.5032557843980126,-152026.5743821091,3341.7090362579474]
["AKMH","AKMH44K",5.76,9.9,2.5499999999999998,4.3220339000000001,6000,18.600000000000001,6000,0.7,2.8,37.799999999999997,0.27300000000000002,675,10,6000,6000,6000,2.5499999999999998,412.08791208791206,1.7249804375808253,1.5670319127741934,2.1220659078919377E-2,-22.576288367407408,9,29.1467935776,9,-2355.9177119999999,7.5,2367.9177119999999,9,0.71008814661672537,1.0436677387812501,17.04211551880141,50.096051461500004,37.513174774123748,23.034885507197458,2.416416097074924,148.02786016896016,3.0763417382458158E-3,1.465129870273211,-153288.41464111328,6824.7924915050762,1.433544977294695E-3,7.8296427727716708E-2,-153662.92739379586,10326.029513418318,1.7084075444135802,3.6973579058399973E-3,1.7192312145563469,-153146.83993149953,6207.5884461452279]
["AKMH","AKMH51E",3.47,2.38,2.98,1.7325581400000001,2500,11,6000,9,36.6,110,0.34200000000000003,675,10,2104.1281538006397,3351.5212515524422,3563.6363636363635,2.8131018346957211,328.9473684210526,2.861401281374222,2.6509959918545452,0.10488563727086764,-22.59377272888889,9,29.160955910399998,9,-2357.3628479999998,7.5,2369.3628479999998,9,0.28340003692550092,0.41668512888299708,6.8016008862120216,20.000886186383859,14.97607329293724,23.037689801234922,2.4188387817674752,148.17627203864458,2.7778373766452223E-2,12.937071827300191,-150205.9870358528,2104.1281538006397,1.283176659594621E-2,2.7949353904922636,-153502.6019868383,3351.5212515524422,1.6299562626952731,7.3875545985169183E-2,25.679926642830214,-140038.82164501774,1213.9312663439473]
["AKMH","AKMH51H",3.39,5.0199999999999996,1.41,1.7625,5500,11.1,6000,2,7.9,51.3,0.34200000000000003,675,10,4772.5354116403187,6000,6000,1.23,328.9473684210526,2.9321648503689839,2.627113145081081,4.4073729657123313E-2,-22.59377272888889,9,29.160955910399998,9,-2357.3628479999998,7.5,2369.3628479999998,9,0.61186616633450719,0.89963126026430673,14.684787992028172,43.182300492686721,32.333632175577073,23.037689801234922,2.4188387817674752,148.17627203864458,6.098792539119444E-3,2.9210230622990006,-152853.45851045501,4772.5354116403187,2.6504942855495005E-3,0.21511963957773725,-153659.60392187795,7573.5892708910178,1.2105202906255546,1.6047647617664258E-2,5.7459584558098218,-150527.60869100346,2888.8854077938881]
["AKMH","AKMH51L",3.47,10,1.45,3.5365853700000001,5500,11.4,6000,0.57999999999999996,2.1,26.6,0.34200000000000003,675,10,6000,6000,6000,1.2663636363636361,328.9473684210526,2.8645420587780284,2.5579785886315789,2.207606845285159E-2,-22.59377272888889,9,29.160955910399998,9,-2357.3628479999998,7.5,2369.3628479999998,9,1.1907564576701719,1.7507778524495674,28.578154984084126,84.037336917579239,62.924677701416975,23.037689801234922,2.4188387817674752,148.17627203864458,1.6862560839250975E-3,0.87790118269327966,-153391.68723268193,9280.8418735279392,7.2814567817491719E-4,-0.12732224811312629,-153658.2722331447,14614.454645404987,-4.7646833174709489,4.2979290956993129E-3,1.6814782626499638,-152665.0143493964,5767.5104036502335]
["AKMH","AKMH52E",6.15,2.4300000000000002,5.39,1.9318996399999999,1500,20.7,6000,8.98,44.7,179,0.622,675,10,1405.635121914233,2067.2513646067555,2189.9441340782123,5.1025926419325769,180.86816720257235,1.6162100699053121,1.4115181761545896,9.3475209940059673E-2,-22.664723760987656,9,29.218426246400004,9,-2363.2271679999999,7.5,2375.2271679999999,9,0.16334216800727985,0.24051753312585367,3.9202120321747165,11.544841590040976,8.6418899662620792,23.049083637062456,2.4286699660271043,148.77852310403074,5.9524786161286723E-2,22.771492605033828,-149618.08324130715,1405.635121914233,3.3431549142434756E-2,5.1220803700228918,-153459.29581382469,2067.2513646067555,1.8397397571534597,6.2723519499889815E-2,24.060171980289773,-149147.19437813177,1362.1146671418214]
["AKMH","AKMH52H",6.29,4.8099999999999996,3.44,2.38888889,3500,21,6000,2.37,11.9,92.7,0.622,675,10,2894.3284558203327,4138.1697866760896,4228.6947141316068,2.9203474594208982,180.86816720257235,1.5818922596540443,1.3913536307809526,4.492519529039081E-2,-22.664723760987656,9,29.218426246400004,9,-2363.2271679999999,7.5,2375.2271679999999,9,0.31612699908453218,0.46548963382745101,7.5870479780287727,22.343502423717648,16.725226405292986,23.049083637062456,2.4286699660271043,148.77852310403074,1.6102251577923055E-2,6.1108613936221428,-152577.61088209343,2894.3284558203327,8.7551762701068535E-3,0.89725833339903194,-153640.57845490918,4138.1697866760896,2.3579185172466239,1.6738390393540171E-2,6.3644475669406866,-152485.57494881653,2834.1324651013811]
["AKMH","AKMH52L",6.45,9.5,1.19,1.5866666700000001,4500,21.4,6000,0.63,3.24,48.3,0.622,675,10,5670.1818734333683,6000,6000,-0.56333333333333258,180.86816720257235,1.5444303735526193,1.3653470208598133,2.2702412875263148E-2,-22.664723760987656,9,29.218426246400004,9,-2363.2271679999999,7.5,2375.2271679999999,9,0.60887907396722663,0.89656023688888897,14.613097775213438,43.034891370666671,32.213763440129007,23.049083637062456,2.4286699660271043,148.77852310403074,4.4772804104774569E-3,1.6612154882139947,-153368.26842904271,5670.1818734333683,2.3481729172660092E-3,-0.14024170218962803,-153661.89234222006,8119.3494138596006,-2.6609019195764922,4.5728045905609783E-3,1.6978126798062276,-153355.09474774735,5608.3886401453892]
["AKMH","AKMH52M",6.39,10.7,1.18,1.7878787899999999,4500,21.3,6000,0.51,2.5,42.4,0.622,675,10,6000,6000,6000,-0.55666666666666664,180.86816720257235,1.5589307752943915,1.3717571007699532,2.1220659078919377E-2,-22.664723760987656,9,29.218426246400004,9,-2363.2271679999999,7.5,2375.2271679999999,9,0.69222945869118091,1.0192917345998957,16.613507008588343,48.926003260794992,36.623554630104657,23.049083637062456,2.4286699660271043,148.77852310403074,3.4325560183459496E-3,1.3358545776423418,-153415.842925,6493.6281807882824,1.8289467948014832E-3,-0.18450696655599216,-153659.26593918158,9216.5582042850565,-4.9262461528146204,3.5214513943578655E-3,1.3716937318362532,-153402.34887666334,6408.2809316555758]
["AKMH","AKMH53H",8.6,5.29,4.0599999999999996,2.3199999999999998,3000,29.4,6000,2.12,11.4,112,0.91200000000000003,675,10,2508.3089234299155,3440.3952365221699,3500,3.3935352087297828,123.35526315789473,1.1587813981599346,0.99584860865306135,4.5294429722564672E-2,-22.738208758518518,9,29.277949094400004,9,-2369.3009280000001,7.5,2381.3009280000001,9,0.25441758263949371,0.37519464803627911,6.1060219833478495,18.009343105741397,13.476793750045765,23.060908206125671,2.4388522640102908,149.40228313603782,2.1283313385066813E-2,7.4373644261315057,-152561.59268161896,2508.3089234299155,1.2695844215008321E-2,0.98034633816737871,-153644.84584377476,3440.3952365221699,2.3837736785714285,1.7397347350526959E-2,5.5424411813340235,-153051.78192266129,2811.028977589408]
["AKMH","AKMH53L",8.68,9.43,2.14,2.1616161599999999,3500,29.7,6000,0.71,3.64,63.9,0.91200000000000003,675,10,4526.7651673210785,6000,6000,-2.5314285714285703,123.35526315789473,1.1491073370701423,0.9857895317979799,2.5169464844032527E-2,-22.738208758518518,9,29.277949094400004,9,-2369.3009280000001,7.5,2381.3009280000001,9,0.44934702283452954,0.66266095420553006,10.784328548028709,31.807725801865441,23.802431758495977,23.060908206125674,2.4388522640102908,149.40228313603782,6.9195488201411852E-3,2.5355270674118846,-153270.38214115988,4526.7651673210785,4.0885653043707592E-3,-0.11017454767152189,-153663.25680831046,6144.0398349221559,-1.4020433502170739,5.6267004002552674E-3,1.870428722527403,-153449.79943193862,5058.6675268029676]
["AKMH","AKMH53P",8.49,15.2,2.09,3.4833333299999998,3500,29.2,6000,0.3,1.3,38.4,0.91200000000000003,675,10,{"$f":"IF(AQ220<I220,IF(AQ220<0,0,AQ220),I220)","v":6000},{"$f":"IF(AU220<I220,IF(AU220<0,0,AU220),I220)","v":6000},{"$f":"IF(UAC_V*0.98/L220*1000<I220,IF(UAC_V*0.98/L220*1000<0,0,UAC_V*0.98/L220*1000),I220)","v":6000},{"$f":"C220+(E220-C220)/G220*Q220","v":-2.4814285714285731},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M220,(inertia/gear^2+gear_inertia)/M220),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M220,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M220))","v":123.35526315789473},{"$f":"IF((C220+(E220-C220)/G220*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X220^2*time1+Y220^2*time2+Z220^2*time3+AA220^2*time4)/time)/(C220+(E220-C220)/G220*mspeed),SQRT((((X220-Y220)*2/PI()+Y220)^2*time1+Y220^2*time2+((Z220-Y220)*2/PI()+Y220)^2*time3+AA220^2*time4)/time)/(C220+(E220-C220)/G220*mspeed)),IF(AccType=1,SQRT((X220^2*time1+Y220^2*time2+Z220^2*time3+AA220^2*time4+AB220^2*time5+AC220^2*time6+AD220^2*time7+AE220^2*time8)/time)/(C220+(E220-C220)/G220*mspeed),SQRT((((X220-Y220)*2/PI()+Y220)^2*time1+Y220^2*time2+((Z220-Y220)*2/PI()+Y220)^2*time3+AA220^2*time4+((AB220-AC220)*2/PI()+AC220)^2*time5+AC220^2*time6+((AD220-AC220)*2/PI()+AC220)^2*time7+AE220^2*time8)/time)/(C220+(E220-C220)/G220*mspeed))))","v":1.1748263023027998},{"$f":"IF(move1,MAX(ABS(X220),ABS(Z220))/H220,MAX(ABS(X220),ABS(Z220),ABS(AB220),ABS(AD220))/H220)","v":1.0026694895342467},{"$f":"IF(AZ220>0,speed/(MIN(AZ220,I220)),\"NA\")","v":2.1220659078919377E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M220+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M220+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.738208758518518},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M220+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M220+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.277949094400004},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M220+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M220+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2369.3009280000001},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M220+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M220+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2381.3009280000001},9,{"$f":"AH220/Irms","v":0.74050125473167849},{"$f":"AI220/Ipeak","v":1.0920318664970554},17.772030113560284,{"$f":"IF(move1,MAX(ABS(X220),ABS(Z220))/(C220/D220),MAX(ABS(X220),ABS(Z220),ABS(AB220),ABS(AD220))/(C220/D220))","v":52.41752959185866},39.225208329291711,{"$f":"IF((C220+(E220-C220)/G220*mspeed)<0,\"NA\",U220*(C220+(E220-C220)/G220*mspeed)*mspeed/9.55)","v":23.060908206125674},{"$f":"IF(move1,IF(speed1>speed2,AM220/2*time1/time,AM220/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z220*-speed/30*PI(),((Z220-AA220)*2/PI()+AA220)*-speed/30*PI()),IF(AccType=1,X220*-speed/30*PI(),((X220-Y220)*2/PI()+Y220)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z220*-speed/30*PI(),((Z220-AA220)*2/PI()+AA220)*-speed/30*PI()),IF(AccType=1,X220*-speed/30*PI(),((X220-Y220)*2/PI()+Y220)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD220*-speed/30*PI(),((AD220-AE220)*2/PI()+AE220)*-speed/30*PI()),IF(AccType=1,AB220*-speed/30*PI(),((AB220-AC220)*2/PI()+AC220)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD220*-speed/30*PI(),((AD220-AE220)*2/PI()+AE220)*-speed/30*PI()),IF(AccType=1,AB220*-speed/30*PI(),((AB220-AC220)*2/PI()+AC220)*-speed/30*PI()),0)/2*time7/time)))","v":2.4388522640102908},{"$f":"IF(move1,MAX(IF(AccType=1,Z220*-speed/30*PI(),((Z220-AA220)*2/PI()+AA220)*-speed/30*PI()),IF(AccType=1,X220*-speed/30*PI(),((X220-Y220)*2/PI()+Y220)*-speed/30*PI()),0),MAX(IF(AccType=1,Z220*-speed/30*PI(),((Z220-AA220)*2/PI()+AA220)*-speed/30*PI()),IF(AccType=1,X220*-speed/30*PI(),((X220-Y220)*2/PI()+Y220)*-speed/30*PI()),IF(AccType=1,AD220*-speed/30*PI(),((AD220-AE220)*2/PI()+AE220)*-speed/30*PI()),IF(AccType=1,AB220*-speed/30*PI(),((AB220-AC220)*2/PI()+AC220)*-speed/30*PI()),0))","v":149.40228313603782},{"$f":"(L220^2)/1000000+((K220/1000)^2*(D220/C220*H220)^2*PI()*PI()*(O220/2)^2)/1200","v":2.4242518497887833E-3},{"$f":"SQRT(3)*L220*J220*D220/C220*H220/1000","v":1.0431141953556402},{"$f":"0.75*J220^2*(D220/C220*H220)^2-(UAC_V*0.98)^2","v":-153479.52340621059},{"$f":"-AO220/2/AN220+SQRT((AO220/2/AN220)^2-AP220/AN220)","v":7744.5283197820481},{"$f":"(L220^2)/1000000+((K220/1000)^2*AV220^2*PI()*PI()*(O220/2)^2)/1200","v":1.5430860273350966E-3},{"$f":"SQRT(3)*L220*J220*AV220/1000","v":-0.28020009468932427},{"$f":"0.75*J220^2*AV220^2-(UAC_V*0.98)^2","v":-153650.68889481202},{"$f":"-AS220/2/AR220+SQRT((AS220/2/AR220)^2-AT220/AR220)","v":10069.864259557253},{"$f":"D220+(F220-D220)*((0.85*UAC_V-D220*J220)/L220*1000)/G220","v":-14.042847230541668},2.009217582462365E-3,0.78266941935905832,-153560.14335462786,{"$f":"IF(((AX220/2/AW220)^2-AY220/AW220)>0,-AX220/2/AW220+SQRT((AX220/2/AW220)^2-AY220/AW220),-9999)","v":8549.700950603743}]
["AKMH","AKMH54H",10.5,4.12,7.62,2.96498054,1800,36.9,6000,3.22,18.3,166,1.1919999999999999,675,10,1749.8551484643333,2290.6803622143898,2361.4457831325303,6.8349114204569767,94.37919463087249,0.94906934474633597,0.79499781654200552,6.2220186554657893E-2,-22.809159790617283,9,29.335419430400002,9,-2375.1652479999998,7.5,2387.1652479999998,9,0.16237277172575088,0.23980541280406351,3.896946521418021,11.510659814595048,8.611164949121509,23.072347986369248,2.4486834482699193,150.00453420142395,4.1991414331982974E-2,13.404754674944323,-152033.7974316352,1749.8551484643333,2.8118059010943629E-2,2.6450580074484269,-153600.52623872508,2290.6803622143898,2.8570024557032934,3.2662043426732019E-2,7.9723525461675413,-153087.37054434259,2046.3447881447184]
["AKMH","AKMH54L",10.4,9.2899999999999991,2.4700000000000002,2.1858407099999999,3000,36.9,6000,0.67,3.5,72.900000000000006,1.1919999999999999,675,10,4193.8406769511857,5386.5020546323412,5377.2290809327842,-3.838320431078154,94.37919463087249,0.96037109354030403,0.79499781654200552,2.6452307835489616E-2,-22.809159790617283,9,29.335419430400002,9,-2375.1652479999998,7.5,2387.1652479999998,9,0.36964740519950445,0.54592557393512819,8.8715377247881069,26.204427548886152,19.603624088920309,23.072347986369248,2.4486834482699193,150.00453420142395,8.0510147624700979E-3,2.7885067444048564,-153298.21292939427,4193.8406769511857,5.3204788561276002E-3,-0.13131643411383867,-153663.18880901791,5386.5020546323412,-1.552230178012131,6.2823921055094375E-3,1.6584383215393499,-153534.61509808473,4813.3401163089702]
["AKMH","AKMH54P",10.6,14.5,2.52,3.4054054100000002,3000,35.299999999999997,6000,0.32,1.5,47.3,1.1919999999999999,675,10,6000,6000,6000,-5.5600000000000005,94.37919463087249,0.94224923145523454,0.83103171190934855,2.1220659078919377E-2,-22.809159790617283,9,29.335419430400002,9,-2375.1652479999998,7.5,2387.1652479999998,9,0.56606646123936544,0.83601332889308189,13.585595069744771,40.128639786867929,30.020376064841308,23.072347986369248,2.4486834482699193,150.00453420142395,3.31602485349098E-3,1.2659267845101987,-153484.9250227127,6615.1652218500703,2.3008421610915502E-3,-0.30726733593443062,-153653.45004718518,8239.034050044962,-11.720459772391827,2.6542297319048364E-3,0.78702381615794836,-153594.78607520708,7460.2836686078708]
["AKMH","AKMH62H",10.6,5.3,9.93,4.5136363599999996,1800,28.6,6000,3.32,25.4,142.1,1.69,675,10,1672.8911770330321,2526.5156213560003,2758.6206896551726,9.6595747409397106,66.568047337278102,0.938497245473918,1.0292879205594407,6.5915463662832602E-2,-22.935351269135801,9,29.437634528000004,9,-2385.5953599999998,7.5,2397.5953599999998,9,0.2070900121607685,0.30664202633333337,4.970160291858444,14.718817264000002,11.005501120473593,23.092750072603184,2.4661689117031163,151.07568073914643,4.7319175692311227E-2,11.685002952313896,-151973.52206799999,1672.8911770330321,2.2655274210901761E-2,3.5208705045698019,-153510.51994103292,2526.5156213560003,4.3088091993488149,3.6259809271473459E-2,8.9929589569529949,-152662.71646324731,1931.6249541199807]
["AKMH","AKMH62L",10.8,11.9,4.95,4.95,5000,29.1,6000,0.75700000000000001,5.4,65.5,1.69,675,10,3698.8984581396339,5840.4812176027153,5984.7328244274813,3.9666369754048239,66.568047337278102,0.92261754804443963,1.0116025610996564,2.9618278277371173E-2,-22.935351269135801,9,29.437634528000004,9,-2385.5953599999998,7.5,2397.5953599999998,9,0.45636502679873053,0.67574816914197544,10.952760643169533,32.435912118814819,24.252863580302918,23.092750072603184,2.4661689117031163,151.07568073914643,1.0454474076696639E-2,2.753683369635795,-153222.13926343402,3698.8984581396339,4.4327962656641358E-3,0.41874797053155016,-153653.78207197573,5840.4812176027153,4.8759013282442742,7.816978890249484E-3,2.0828636020588482,-153411.19883545354,4298.8303803868894]
["AKMH","AKMH62M",10.9,13.1,3.33,3.6593406599999998,5500,29.3,6000,0.58699999999999997,4.4000000000000004,58.8,1.69,675,10,4150.6742326667145,6000,6000,2.6418181818181807,66.568047337278102,0.91451800779457948,1.0046974241638227,2.6343512982139113E-2,-22.935351269135801,9,29.437634528000004,9,-2385.5953599999998,7.5,2397.5953599999998,9,0.4977759925332233,0.73706615503975537,11.94662382079736,35.379175441908259,26.453589849211752,23.092750072603184,2.4661689117031163,151.07568073914643,8.3935939613951453E-3,2.1051763031600932,-153343.54850500755,4150.6742326667145,3.5034365756582879E-3,0.20321552076774782,-153661.0139360422,6593.755624952094,3.399232104288183,6.2431319708600337E-3,1.5814689531210138,-153483.15492028164,4833.2185065766225]
["AKMH","AKMH63H",14.6,5.2,13.6,4.5333333299999996,1500,41.1,6000,3.45,28.1,194.5,2.42,675,10,1333.1610994811233,1871.1411536841204,2015.4241645244215,13.352572564210586,46.487603305785129,0.68242073056856423,0.71988973002433088,7.5118451318903837E-2,-23.120330745679013,9,29.587467904,9,-2400.8844800000002,7.5,2412.8844800000002,9,0.14770803633145033,0.21954171389954338,3.5449928719548081,10.538002267178083,7.8735084574986791,23.122785090506,2.491800213522863,152.64583530247464,7.262035722555038E-2,17.013420568752341,-151751.13609182305,1333.1610994811233,4.1065692952009097E-2,5.188366272699688,-153486.10569200781,1871.1411536841204,4.4640731182855182,4.7895110142737014E-2,9.1509804266806185,-153110.60395603062,1694.9757647822371]
["AKMH","AKMH63L",14.8,10.6,11.1,7.4,3000,41.6,6000,0.95699999999999996,7.4,98.2,2.42,675,10,2670.9474963003017,3825.7998767331887,3991.8533604887984,10.0815134853624,46.487603305785129,0.67376251253711317,0.71123720923076916,3.7369714691789228E-2,-23.120330745679013,9,29.587467904,9,-2400.8844800000002,7.5,2412.8844800000002,9,0.29702827056464726,0.44147967311711711,7.1286784935515337,21.191024309621621,15.832954377371301,23.122785090506,2.491800213522863,152.64583530247464,1.9638564737897685E-2,4.8497743631161478,-153054.2383593808,2670.9474963003017,1.019764924490856E-2,1.1421898880996473,-153630.17843845853,3825.7998767331887,7.0170449422946373,1.2465817453956807E-2,2.5771874823795611,-153491.80955054177,3407.1428033003294]
["AKMH","AKMH63M",15,13,7.9,6.3709677400000002,4000,42,6000,0.627,4.9000000000000004,79.900000000000006,2.42,675,10,3323.6062541412462,4796.2516391423414,4906.1326658322905,6.486653340522345,46.487603305785129,0.6652965782648127,0.70446352152380953,3.011317525060301E-2,-23.120330745679013,9,29.587467904,9,-2400.8844800000002,7.5,2412.8844800000002,9,0.35942288840652914,0.53421817048888898,8.6261493217566994,25.642472183466669,19.158870579913454,23.122785090506,2.491800213522863,152.64583530247464,1.2925149863435192E-2,3.1584669087615391,-153273.33985012001,3323.6062541412462,6.5687299866683266E-3,0.53077023209720242,-153652.96786505345,4796.2516391423414,6.1169032338900493,8.1961446954860982E-3,1.6624356795577377,-153555.77286734094,4228.18096776316]
["AKMH","AKMH64K",18.7,8.6999999999999993,15.6,6.8421052600000003,2000,52.5,6000,1.43,11.8,147,3.16,675,10,1875.372444682705,2539.4362148785799,2666.6666666666665,14.763873866938201,35.601265822784811,0.53394562714219773,0.56646388175238105,5.2620845942815207E-2,-23.307844187654318,9,29.739353792000003,9,-2416.3830400000002,7.5,2428.3830400000002,9,0.19319935231706978,0.28824908421390377,4.6367844556096749,13.835956042267382,10.329776438716037,23.153386744871675,2.5177826290661667,154.23749883242371,3.8689336465423503E-2,8.8930544020493461,-152749.02919387975,1875.372444682705,2.2867502178685065E-2,2.4139580806143082,-153596.5837195733,2539.4362148785799,6.6300335267358506,2.466395183535567E-2,3.7610137572644184,-153500.35031141734,2419.6485668794335]
["AKMH","AKMH64L",19,12.1,12.5,7.5301204799999999,3000,53.1,6000,0.76700000000000002,6.2,107,3.16,675,10,2619.3866981870251,3552.1230821367899,3663.5514018691588,11.303733322036955,35.601265822784811,0.52587897717643406,0.56006315992467048,3.792844520632159E-2,-23.307844187654318,9,29.739353792000003,9,-2416.3830400000002,7.5,2428.3830400000002,9,0.26445987567322066,0.39456818079298245,6.3470370161572962,18.939272678063158,14.139857923704037,23.153386744871675,2.5177826290661667,154.23749883242371,2.0487460572760574E-2,4.8069107587352695,-153159.4495798226,2619.3866981870251,1.1880853808767937E-2,1.0507204927489511,-153639.89279513751,3552.1230821367899,7.3917527852375828,1.3029272485093718E-2,2.0099479672353433,-153575.78507225536,3356.9515908417725]
["AKMH","AKMH65K",21.9,9.1,17.7,6.9685039399999997,2000,59.8,6000,1.35,11.4,164,4,675,10,{"$f":"IF(AQ232<I232,IF(AQ232<0,0,AQ232),I232)","v":1770.006285802893},{"$f":"IF(AU232<I232,IF(AU232<0,0,AU232),I232)","v":2287.1358158065841},{"$f":"IF(UAC_V*0.98/L232*1000<I232,IF(UAC_V*0.98/L232*1000<0,0,UAC_V*0.98/L232*1000),I232)","v":2390.2439024390242},{"$f":"C232+(E232-C232)/G232*Q232","v":17.097014786806174},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M232,(inertia/gear^2+gear_inertia)/M232),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M232,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M232))","v":28.125},{"$f":"IF((C232+(E232-C232)/G232*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X232^2*time1+Y232^2*time2+Z232^2*time3+AA232^2*time4)/time)/(C232+(E232-C232)/G232*mspeed),SQRT((((X232-Y232)*2/PI()+Y232)^2*time1+Y232^2*time2+((Z232-Y232)*2/PI()+Y232)^2*time3+AA232^2*time4)/time)/(C232+(E232-C232)/G232*mspeed)),IF(AccType=1,SQRT((X232^2*time1+Y232^2*time2+Z232^2*time3+AA232^2*time4+AB232^2*time5+AC232^2*time6+AD232^2*time7+AE232^2*time8)/time)/(C232+(E232-C232)/G232*mspeed),SQRT((((X232-Y232)*2/PI()+Y232)^2*time1+Y232^2*time2+((Z232-Y232)*2/PI()+Y232)^2*time3+AA232^2*time4+((AB232-AC232)*2/PI()+AC232)^2*time5+AC232^2*time6+((AD232-AC232)*2/PI()+AC232)^2*time7+AE232^2*time8)/time)/(C232+(E232-C232)/G232*mspeed))))","v":0.45674591770031381},{"$f":"IF(move1,MAX(ABS(X232),ABS(Z232))/H232,MAX(ABS(X232),ABS(Z232),ABS(AB232),ABS(AD232))/H232)","v":0.50019673578595325},{"$f":"IF(AZ232>0,speed/(MIN(AZ232,I232)),\"NA\")","v":5.7011189032353526E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M232+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M232+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-23.520697283950618},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M232+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M232+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.9117648},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M232+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M232+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2433.9760000000001},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M232+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M232+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2445.9760000000001},9,{"$f":"AH232/Irms","v":0.1728143940275533},{"$f":"AI232/Ipeak","v":0.25893936423135466},4.1475454566612795,{"$f":"IF(move1,MAX(ABS(X232),ABS(Z232))/(C232/D232),MAX(ABS(X232),ABS(Z232),ABS(AB232),ABS(AD232))/(C232/D232))","v":12.429089483105024},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X232),ABS(Z232))/(C232/D232),MAX(ABS((X232-Y232)*2/PI()+Y232),ABS((Z232-Y232)*2/PI()+Y232))/(C232/D232)),IF(AccType=1,MAX(ABS(X232),ABS(Z232),ABS(AB232),ABS(AD232))/(C232/D232),MAX(ABS((X232-Y232)*2/PI()+Y232),ABS((Z232-Y232)*2/PI()+Y232),ABS((AB232-AC232)*2/PI()+AC232),ABS((AD232-AC232)*2/PI()+AC232))/(C232/D232)))","v":9.2715466125891162},{"$f":"IF((C232+(E232-C232)/G232*mspeed)<0,\"NA\",U232*(C232+(E232-C232)/G232*mspeed)*mspeed/9.55)","v":23.18831233110085},{"$f":"IF(move1,IF(speed1>speed2,AM232/2*time1/time,AM232/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z232*-speed/30*PI(),((Z232-AA232)*2/PI()+AA232)*-speed/30*PI()),IF(AccType=1,X232*-speed/30*PI(),((X232-Y232)*2/PI()+Y232)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z232*-speed/30*PI(),((Z232-AA232)*2/PI()+AA232)*-speed/30*PI()),IF(AccType=1,X232*-speed/30*PI(),((X232-Y232)*2/PI()+Y232)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD232*-speed/30*PI(),((AD232-AE232)*2/PI()+AE232)*-speed/30*PI()),IF(AccType=1,AB232*-speed/30*PI(),((AB232-AC232)*2/PI()+AC232)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD232*-speed/30*PI(),((AD232-AE232)*2/PI()+AE232)*-speed/30*PI()),IF(AccType=1,AB232*-speed/30*PI(),((AB232-AC232)*2/PI()+AC232)*-speed/30*PI()),0)/2*time7/time)))","v":2.5472761818450538},{"$f":"IF(move1,MAX(IF(AccType=1,Z232*-speed/30*PI(),((Z232-AA232)*2/PI()+AA232)*-speed/30*PI()),IF(AccType=1,X232*-speed/30*PI(),((X232-Y232)*2/PI()+Y232)*-speed/30*PI()),0),MAX(IF(AccType=1,Z232*-speed/30*PI(),((Z232-AA232)*2/PI()+AA232)*-speed/30*PI()),IF(AccType=1,X232*-speed/30*PI(),((X232-Y232)*2/PI()+Y232)*-speed/30*PI()),IF(AccType=1,AD232*-speed/30*PI(),((AD232-AE232)*2/PI()+AE232)*-speed/30*PI()),IF(AccType=1,AB232*-speed/30*PI(),((AB232-AC232)*2/PI()+AC232)*-speed/30*PI()),0))","v":156.04425202858218},{"$f":"(L232^2)/1000000+((K232/1000)^2*(D232/C232*H232)^2*PI()*PI()*(O232/2)^2)/1200","v":4.3395285351257522E-2},{"$f":"SQRT(3)*L232*J232*D232/C232*H232/1000","v":9.5287669513091746},{"$f":"0.75*J232^2*(D232/C232*H232)^2-(UAC_V*0.98)^2","v":-152820.0324991415},{"$f":"-AO232/2/AN232+SQRT((AO232/2/AN232)^2-AP232/AN232)","v":1770.006285802893},{"$f":"(L232^2)/1000000+((K232/1000)^2*AV232^2*PI()*PI()*(O232/2)^2)/1200","v":2.8194309186611088E-2},{"$f":"SQRT(3)*L232*J232*AV232/1000","v":2.6729645783947484},{"$f":"0.75*J232^2*AV232^2-(UAC_V*0.98)^2","v":-153597.58919879023},{"$f":"-AS232/2/AR232+SQRT((AS232/2/AR232)^2-AT232/AR232)","v":2287.1358158065841},{"$f":"D232+(F232-D232)*((0.85*UAC_V-D232*J232)/L232*1000)/G232","v":6.970356002125305},{"$f":"(L232^2)/1000000+((K232/1000)^2*AJ232^2*PI()*PI()*(O232/2)^2)/1200","v":2.9193061288164644E-2},{"$f":"SQRT(3)*L232*J232*AJ232/1000","v":3.5554160612212891},{"$f":"0.75*J232^2*AJ232^2-(UAC_V*0.98)^2","v":-153546.50126999934},{"$f":"IF(((AX232/2/AW232)^2-AY232/AW232)>0,-AX232/2/AW232+SQRT((AX232/2/AW232)^2-AY232/AW232),-9999)","v":2233.3151901333026}]
["AKMH","AKMH65L",22.2,11.1,16,7.6190476199999999,2500,64.2,6000,1.07,7.6,133,4,675,10,{"$f":"IF(AQ233<I233,IF(AQ233<0,0,AQ233),I233)","v":2131.1234346612991},{"$f":"IF(AU233<I233,IF(AU233<0,0,AU233),I233)","v":2839.5092865806751},{"$f":"IF(UAC_V*0.98/L233*1000<I233,IF(UAC_V*0.98/L233*1000<0,0,UAC_V*0.98/L233*1000),I233)","v":2947.3684210526312},{"$f":"C233+(E233-C233)/G233*Q233","v":15.158016969279927},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M233,(inertia/gear^2+gear_inertia)/M233),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M233,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M233))","v":28.125},{"$f":"IF((C233+(E233-C233)/G233*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X233^2*time1+Y233^2*time2+Z233^2*time3+AA233^2*time4)/time)/(C233+(E233-C233)/G233*mspeed),SQRT((((X233-Y233)*2/PI()+Y233)^2*time1+Y233^2*time2+((Z233-Y233)*2/PI()+Y233)^2*time3+AA233^2*time4)/time)/(C233+(E233-C233)/G233*mspeed)),IF(AccType=1,SQRT((X233^2*time1+Y233^2*time2+Z233^2*time3+AA233^2*time4+AB233^2*time5+AC233^2*time6+AD233^2*time7+AE233^2*time8)/time)/(C233+(E233-C233)/G233*mspeed),SQRT((((X233-Y233)*2/PI()+Y233)^2*time1+Y233^2*time2+((Z233-Y233)*2/PI()+Y233)^2*time3+AA233^2*time4+((AB233-AC233)*2/PI()+AC233)^2*time5+AC233^2*time6+((AD233-AC233)*2/PI()+AC233)^2*time7+AE233^2*time8)/time)/(C233+(E233-C233)/G233*mspeed))))","v":0.45073222487444176},{"$f":"IF(move1,MAX(ABS(X233),ABS(Z233))/H233,MAX(ABS(X233),ABS(Z233),ABS(AB233),ABS(AD233))/H233)","v":0.46591533956386288},{"$f":"IF(AZ233>0,speed/(MIN(AZ233,I233)),\"NA\")","v":4.6138150005853848E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M233+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M233+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-23.520697283950618},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M233+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M233+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.9117648},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M233+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M233+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2433.9760000000001},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M233+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M233+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2445.9760000000001},9,{"$f":"AH233/Irms","v":0.2079469906155724},{"$f":"AI233/Ipeak","v":0.31158088333333334},4.9907277747737373,{"$f":"IF(move1,MAX(ABS(X233),ABS(Z233))/(C233/D233),MAX(ABS(X233),ABS(Z233),ABS(AB233),ABS(AD233))/(C233/D233))","v":14.9558824},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X233),ABS(Z233))/(C233/D233),MAX(ABS((X233-Y233)*2/PI()+Y233),ABS((Z233-Y233)*2/PI()+Y233))/(C233/D233)),IF(AccType=1,MAX(ABS(X233),ABS(Z233),ABS(AB233),ABS(AD233))/(C233/D233),MAX(ABS((X233-Y233)*2/PI()+Y233),ABS((Z233-Y233)*2/PI()+Y233),ABS((AB233-AC233)*2/PI()+AC233),ABS((AD233-AC233)*2/PI()+AC233))/(C233/D233)))","v":11.1564214733902},{"$f":"IF((C233+(E233-C233)/G233*mspeed)<0,\"NA\",U233*(C233+(E233-C233)/G233*mspeed)*mspeed/9.55)","v":23.18831233110085},{"$f":"IF(move1,IF(speed1>speed2,AM233/2*time1/time,AM233/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z233*-speed/30*PI(),((Z233-AA233)*2/PI()+AA233)*-speed/30*PI()),IF(AccType=1,X233*-speed/30*PI(),((X233-Y233)*2/PI()+Y233)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z233*-speed/30*PI(),((Z233-AA233)*2/PI()+AA233)*-speed/30*PI()),IF(AccType=1,X233*-speed/30*PI(),((X233-Y233)*2/PI()+Y233)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD233*-speed/30*PI(),((AD233-AE233)*2/PI()+AE233)*-speed/30*PI()),IF(AccType=1,AB233*-speed/30*PI(),((AB233-AC233)*2/PI()+AC233)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD233*-speed/30*PI(),((AD233-AE233)*2/PI()+AE233)*-speed/30*PI()),IF(AccType=1,AB233*-speed/30*PI(),((AB233-AC233)*2/PI()+AC233)*-speed/30*PI()),0)/2*time7/time)))","v":2.5472761818450538},{"$f":"IF(move1,MAX(IF(AccType=1,Z233*-speed/30*PI(),((Z233-AA233)*2/PI()+AA233)*-speed/30*PI()),IF(AccType=1,X233*-speed/30*PI(),((X233-Y233)*2/PI()+Y233)*-speed/30*PI()),0),MAX(IF(AccType=1,Z233*-speed/30*PI(),((Z233-AA233)*2/PI()+AA233)*-speed/30*PI()),IF(AccType=1,X233*-speed/30*PI(),((X233-Y233)*2/PI()+Y233)*-speed/30*PI()),IF(AccType=1,AD233*-speed/30*PI(),((AD233-AE233)*2/PI()+AE233)*-speed/30*PI()),IF(AccType=1,AB233*-speed/30*PI(),((AB233-AC233)*2/PI()+AC233)*-speed/30*PI()),0))","v":156.04425202858218},{"$f":"(L233^2)/1000000+((K233/1000)^2*(D233/C233*H233)^2*PI()*PI()*(O233/2)^2)/1200","v":2.9926586015348207E-2},{"$f":"SQRT(3)*L233*J233*D233/C233*H233/1000","v":7.9122696286465741},{"$f":"0.75*J233^2*(D233/C233*H233)^2-(UAC_V*0.98)^2","v":-152779.21269325001},{"$f":"-AO233/2/AN233+SQRT((AO233/2/AN233)^2-AP233/AN233)","v":2131.1234346612991},{"$f":"(L233^2)/1000000+((K233/1000)^2*AV233^2*PI()*PI()*(O233/2)^2)/1200","v":1.8386742767036064E-2},{"$f":"SQRT(3)*L233*J233*AV233/1000","v":1.88929976833652},{"$f":"0.75*J233^2*AV233^2-(UAC_V*0.98)^2","v":-153613.55263702531},{"$f":"-AS233/2/AR233+SQRT((AS233/2/AR233)^2-AT233/AR233)","v":2839.5092865806751},{"$f":"D233+(F233-D233)*((0.85*UAC_V-D233*J233)/L233*1000)/G233","v":7.6648705630594289},{"$f":"(L233^2)/1000000+((K233/1000)^2*AJ233^2*PI()*PI()*(O233/2)^2)/1200","v":1.9167207898155948E-2},{"$f":"SQRT(3)*L233*J233*AJ233/1000","v":2.7499256943391202},{"$f":"0.75*J233^2*AJ233^2-(UAC_V*0.98)^2","v":-153557.12438062657},{"$f":"IF(((AX233/2/AW233)^2-AY233/AW233)>0,-AX233/2/AW233+SQRT((AX233/2/AW233)^2-AY233/AW233),-9999)","v":2759.6241821001026}]
["AKMH","AKMH65M",22.2,12.6,16.100000000000001,8.7027026999999997,2500,64.2,6000,0.747,6.1,119,4,675,10,{"$f":"IF(AQ234<I234,IF(AQ234<0,0,AQ234),I234)","v":2396.4362020574767},{"$f":"IF(AU234<I234,IF(AU234<0,0,AU234),I234)","v":3191.5395258926565},{"$f":"IF(UAC_V*0.98/L234*1000<I234,IF(UAC_V*0.98/L234*1000<0,0,UAC_V*0.98/L234*1000),I234)","v":3294.1176470588234},{"$f":"C234+(E234-C234)/G234*Q234","v":14.412643556821919},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M234,(inertia/gear^2+gear_inertia)/M234),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M234,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M234))","v":28.125},{"$f":"IF((C234+(E234-C234)/G234*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X234^2*time1+Y234^2*time2+Z234^2*time3+AA234^2*time4)/time)/(C234+(E234-C234)/G234*mspeed),SQRT((((X234-Y234)*2/PI()+Y234)^2*time1+Y234^2*time2+((Z234-Y234)*2/PI()+Y234)^2*time3+AA234^2*time4)/time)/(C234+(E234-C234)/G234*mspeed)),IF(AccType=1,SQRT((X234^2*time1+Y234^2*time2+Z234^2*time3+AA234^2*time4+AB234^2*time5+AC234^2*time6+AD234^2*time7+AE234^2*time8)/time)/(C234+(E234-C234)/G234*mspeed),SQRT((((X234-Y234)*2/PI()+Y234)^2*time1+Y234^2*time2+((Z234-Y234)*2/PI()+Y234)^2*time3+AA234^2*time4+((AB234-AC234)*2/PI()+AC234)^2*time5+AC234^2*time6+((AD234-AC234)*2/PI()+AC234)^2*time7+AE234^2*time8)/time)/(C234+(E234-C234)/G234*mspeed))))","v":0.45071416292741234},{"$f":"IF(move1,MAX(ABS(X234),ABS(Z234))/H234,MAX(ABS(X234),ABS(Z234),ABS(AB234),ABS(AD234))/H234)","v":0.46591533956386288},{"$f":"IF(AZ234>0,speed/(MIN(AZ234,I234)),\"NA\")","v":4.1116793609436854E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M234+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M234+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-23.520697283950618},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M234+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M234+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.9117648},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M234+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M234+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2433.9760000000001},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M234+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M234+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2445.9760000000001},9,{"$f":"AH234/Irms","v":0.23604793529335244},{"$f":"AI234/Ipeak","v":0.35368640810810814},5.6651504470404586,{"$f":"IF(move1,MAX(ABS(X234),ABS(Z234))/(C234/D234),MAX(ABS(X234),ABS(Z234),ABS(AB234),ABS(AD234))/(C234/D234))","v":16.976947589189191},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X234),ABS(Z234))/(C234/D234),MAX(ABS((X234-Y234)*2/PI()+Y234),ABS((Z234-Y234)*2/PI()+Y234))/(C234/D234)),IF(AccType=1,MAX(ABS(X234),ABS(Z234),ABS(AB234),ABS(AD234))/(C234/D234),MAX(ABS((X234-Y234)*2/PI()+Y234),ABS((Z234-Y234)*2/PI()+Y234),ABS((AB234-AC234)*2/PI()+AC234),ABS((AD234-AC234)*2/PI()+AC234))/(C234/D234)))","v":12.664045996821308},{"$f":"IF((C234+(E234-C234)/G234*mspeed)<0,\"NA\",U234*(C234+(E234-C234)/G234*mspeed)*mspeed/9.55)","v":23.18831233110085},{"$f":"IF(move1,IF(speed1>speed2,AM234/2*time1/time,AM234/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z234*-speed/30*PI(),((Z234-AA234)*2/PI()+AA234)*-speed/30*PI()),IF(AccType=1,X234*-speed/30*PI(),((X234-Y234)*2/PI()+Y234)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z234*-speed/30*PI(),((Z234-AA234)*2/PI()+AA234)*-speed/30*PI()),IF(AccType=1,X234*-speed/30*PI(),((X234-Y234)*2/PI()+Y234)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD234*-speed/30*PI(),((AD234-AE234)*2/PI()+AE234)*-speed/30*PI()),IF(AccType=1,AB234*-speed/30*PI(),((AB234-AC234)*2/PI()+AC234)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD234*-speed/30*PI(),((AD234-AE234)*2/PI()+AE234)*-speed/30*PI()),IF(AccType=1,AB234*-speed/30*PI(),((AB234-AC234)*2/PI()+AC234)*-speed/30*PI()),0)/2*time7/time)))","v":2.5472761818450538},{"$f":"IF(move1,MAX(IF(AccType=1,Z234*-speed/30*PI(),((Z234-AA234)*2/PI()+AA234)*-speed/30*PI()),IF(AccType=1,X234*-speed/30*PI(),((X234-Y234)*2/PI()+Y234)*-speed/30*PI()),0),MAX(IF(AccType=1,Z234*-speed/30*PI(),((Z234-AA234)*2/PI()+AA234)*-speed/30*PI()),IF(AccType=1,X234*-speed/30*PI(),((X234-Y234)*2/PI()+Y234)*-speed/30*PI()),IF(AccType=1,AD234*-speed/30*PI(),((AD234-AE234)*2/PI()+AE234)*-speed/30*PI()),IF(AccType=1,AB234*-speed/30*PI(),((AB234-AC234)*2/PI()+AC234)*-speed/30*PI()),0))","v":156.04425202858218},{"$f":"(L234^2)/1000000+((K234/1000)^2*(D234/C234*H234)^2*PI()*PI()*(O234/2)^2)/1200","v":2.4319354757466882E-2},{"$f":"SQRT(3)*L234*J234*D234/C234*H234/1000","v":5.6102315903746023},{"$f":"0.75*J234^2*(D234/C234*H234)^2-(UAC_V*0.98)^2","v":-153108.3418809117},{"$f":"-AO234/2/AN234+SQRT((AO234/2/AN234)^2-AP234/AN234)","v":2396.4362020574767},{"$f":"(L234^2)/1000000+((K234/1000)^2*AV234^2*PI()*PI()*(O234/2)^2)/1200","v":1.4684178795926317E-2},{"$f":"SQRT(3)*L234*J234*AV234/1000","v":1.2731927840863468},{"$f":"0.75*J234^2*AV234^2-(UAC_V*0.98)^2","v":-153635.3823200083},{"$f":"-AS234/2/AR234+SQRT((AS234/2/AR234)^2-AT234/AR234)","v":3191.5395258926565},{"$f":"D234+(F234-D234)*((0.85*UAC_V-D234*J234)/L234*1000)/G234","v":8.2692472593178472},{"$f":"(L234^2)/1000000+((K234/1000)^2*AJ234^2*PI()*PI()*(O234/2)^2)/1200","v":1.5388052477173564E-2},{"$f":"SQRT(3)*L234*J234*AJ234/1000","v":1.9498476070263946},{"$f":"0.75*J234^2*AJ234^2-(UAC_V*0.98)^2","v":-153596.88069891557},{"$f":"IF(((AX234/2/AW234)^2-AY234/AW234)>0,-AX234/2/AW234+SQRT((AX234/2/AW234)^2-AY234/AW234),-9999)","v":3096.6411360513703}]
["ACC","AHD55 C4-22",0.4,1.6,0.36,1.39,3000,1.4,8000,9.1999999999999993,8.4,22,2.4E-2,560,6,{"$f":"IF(AQ235<I235,IF(AQ235<0,0,AQ235),I235)","v":8000},{"$f":"IF(AU235<I235,IF(AU235<0,0,AU235),I235)","v":8000},{"$f":"IF(UAC_V*0.98/L235*1000<I235,IF(UAC_V*0.98/L235*1000<0,0,UAC_V*0.98/L235*1000),I235)","v":8000},{"$f":"C235+(E235-C235)/G235*Q235","v":0.29333333333333328},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M235,(inertia/gear^2+gear_inertia)/M235),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M235,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M235))","v":4687.5},{"$f":"IF((C235+(E235-C235)/G235*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X235^2*time1+Y235^2*time2+Z235^2*time3+AA235^2*time4)/time)/(C235+(E235-C235)/G235*mspeed),SQRT((((X235-Y235)*2/PI()+Y235)^2*time1+Y235^2*time2+((Z235-Y235)*2/PI()+Y235)^2*time3+AA235^2*time4)/time)/(C235+(E235-C235)/G235*mspeed)),IF(AccType=1,SQRT((X235^2*time1+Y235^2*time2+Z235^2*time3+AA235^2*time4+AB235^2*time5+AC235^2*time6+AD235^2*time7+AE235^2*time8)/time)/(C235+(E235-C235)/G235*mspeed),SQRT((((X235-Y235)*2/PI()+Y235)^2*time1+Y235^2*time2+((Z235-Y235)*2/PI()+Y235)^2*time3+AA235^2*time4+((AB235-AC235)*2/PI()+AC235)^2*time5+AC235^2*time6+((AD235-AC235)*2/PI()+AC235)^2*time7+AE235^2*time8)/time)/(C235+(E235-C235)/G235*mspeed))))","v":24.795991143280599},{"$f":"IF(move1,MAX(ABS(X235),ABS(Z235))/H235,MAX(ABS(X235),ABS(Z235),ABS(AB235),ABS(AD235))/H235)","v":20.782632877714288},{"$f":"IF(AZ235>0,speed/(MIN(AZ235,I235)),\"NA\")","v":"NA"},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M235+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M235+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.513192628148147},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M235+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M235+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.095686028800003},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M235+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M235+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2350.7026559999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M235+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M235+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2362.7026559999999},9,{"$f":"AH235/Irms","v":1.6518435798023601},{"$f":"AI235/Ipeak","v":2.4246405024000004},{"$f":"IF(move1,IF(AccType=1,SQRT((X235^2*time1+Y235^2*time2+Z235^2*time3+AA235^2*time4)/time)/(C235/D235),SQRT((((X235-Y235)*2/PI()+Y235)^2*time1+Y235^2*time2+((Z235-AA235)*2/PI()+AA235)^2*time3+AA235^2*time4)/time)/(C235/D235)),IF(AccType=1,SQRT((X235^2*time1+Y235^2*time2+Z235^2*time3+AA235^2*time4+AB235^2*time5+AC235^2*time6+AD235^2*time7+AE235^2*time8)/time)/(C235/D235),SQRT((((X235-Y235)*2/PI()+Y235)^2*time1+Y235^2*time2+((Z235-AA235)*2/PI()+AA235)^2*time3+AA235^2*time4+((AB235-AC235)*2/PI()+AC235)^2*time5+AC235^2*time6+((AD235-AE235)*2/PI()+AE235)^2*time7+AE235^2*time8)/time)/(C235/D235)))","v":39.64424591525664},{"$f":"IF(move1,MAX(ABS(X235),ABS(Z235))/(C235/D235),MAX(ABS(X235),ABS(Z235),ABS(AB235),ABS(AD235))/(C235/D235))","v":116.38274411520001},87.173244260900162,{"$f":"IF((C235+(E235-C235)/G235*mspeed)<0,\"NA\",U235*(C235+(E235-C235)/G235*mspeed)*mspeed/9.55)","v":23.024777094148789},{"$f":"IF(move1,IF(speed1>speed2,AM235/2*time1/time,AM235/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z235*-speed/30*PI(),((Z235-AA235)*2/PI()+AA235)*-speed/30*PI()),IF(AccType=1,X235*-speed/30*PI(),((X235-Y235)*2/PI()+Y235)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z235*-speed/30*PI(),((Z235-AA235)*2/PI()+AA235)*-speed/30*PI()),IF(AccType=1,X235*-speed/30*PI(),((X235-Y235)*2/PI()+Y235)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD235*-speed/30*PI(),((AD235-AE235)*2/PI()+AE235)*-speed/30*PI()),IF(AccType=1,AB235*-speed/30*PI(),((AB235-AC235)*2/PI()+AC235)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD235*-speed/30*PI(),((AD235-AE235)*2/PI()+AE235)*-speed/30*PI()),IF(AccType=1,AB235*-speed/30*PI(),((AB235-AC235)*2/PI()+AC235)*-speed/30*PI()),0)/2*time7/time)))","v":2.4076733653583253},{"$f":"IF(move1,MAX(IF(AccType=1,Z235*-speed/30*PI(),((Z235-AA235)*2/PI()+AA235)*-speed/30*PI()),IF(AccType=1,X235*-speed/30*PI(),((X235-Y235)*2/PI()+Y235)*-speed/30*PI()),0),MAX(IF(AccType=1,Z235*-speed/30*PI(),((Z235-AA235)*2/PI()+AA235)*-speed/30*PI()),IF(AccType=1,X235*-speed/30*PI(),((X235-Y235)*2/PI()+Y235)*-speed/30*PI()),IF(AccType=1,AD235*-speed/30*PI(),((AD235-AE235)*2/PI()+AE235)*-speed/30*PI()),IF(AccType=1,AB235*-speed/30*PI(),((AB235-AC235)*2/PI()+AC235)*-speed/30*PI()),0))","v":147.49228690009889},{"$f":"(L235^2)/1000000+((K235/1000)^2*(D235/C235*H235)^2*PI()*PI()*(O235/2)^2)/1200","v":6.4779311219441155E-4},{"$f":"SQRT(3)*L235*J235*D235/C235*H235/1000","v":1.963175667330868},{"$f":"0.75*J235^2*(D235/C235*H235)^2-(UAC_V*0.98)^2","v":-151673.2672},{"$f":"-AO235/2/AN235+SQRT((AO235/2/AN235)^2-AP235/AN235)","v":13861.14728222815},{"$f":"(L235^2)/1000000+((K235/1000)^2*AV235^2*PI()*PI()*(O235/2)^2)/1200","v":4.8566741777737081E-4},{"$f":"SQRT(3)*L235*J235*AV235/1000","v":0.19807677609731814},{"$f":"0.75*J235^2*AV235^2-(UAC_V*0.98)^2","v":-153643.73429275356},{"$f":"-AS235/2/AR235+SQRT((AS235/2/AR235)^2-AT235/AR235)","v":17583.642113553429},{"$f":"D235+(F235-D235)*((0.85*UAC_V-D235*J235)/L235*1000)/G235","v":0.5650181818181812},4.0174447828937691E-2,30.560069995587401,328731.59821033129,{"$f":"IF(((AX235/2/AW235)^2-AY235/AW235)>0,-AX235/2/AW235+SQRT((AX235/2/AW235)^2-AY235/AW235),-9999)","v":-9999}]
["ACC","AHD55 G4-44",0.8,1.6,0.65,1.27,3000,2.9,8000,13.4,15,44,3.5000000000000003E-2,560,6,6633.4690311040376,8000,8000,0.39999999999999997,3214.2857142857138,12.40626975045598,10.033773721379312,"NA",-22.515979990123455,9,29.097943792000002,9,-2350.9330399999999,7.5,2362.9330399999999,9,0.82593779476185014,1.2124143246666668,19.822507074284403,58.195887584000005,43.589496803838969,23.025223272411498,2.408059590454239,147.51594676338189,2.4962727678388402E-3,5.9230595056271387,-149133.70120000001,6633.4690311040376,1.9467553211562033E-3,0.82065010667620131,-153577.03375547679,8673.6589001498814,0.80359999999999987,3.3581155786605664E-2,44.514341963703821,102214.95667117293,-9999]
["ACC","AHD70 C4-44",1.2,2.2999999999999998,1.2,2.35,3000,4.7,8000,4.7,12.1,44,0.06,560,6,6804.5952313657299,8000,8000,1.2,1875,8.2597417410994325,6.192143632340426,6.0252192147729824E-2,-22.522314903703705,9,29.103075072000003,9,-2351.4566400000003,7.5,2363.4566400000003,9,0.79155858352202901,1.1621019560000001,18.997406004528695,55.780893888000008,41.779528896098,23.026237443960085,2.4089373747631342,147.56971917993422,2.8154692215574704E-3,3.2266778639389044,-152319.54622447916,6804.5952313657299,1.9997155346759945E-3,0.86849626086397624,-153566.59739732248,8548.7664269974393,2.4246931818181823,2.0853285862272631E-2,14.964930366864227,-124744.94771628421,2113.1837686724493]
["ACC","AHD70 E4-44",1.8,3.5,1.8,3.53,3000,7,8000,2.6,7.6,44,0.08,560,6,7004.1384134881137,8000,8000,1.8,1406.25,5.5066885483513968,4.1581685851428576,3.6750748639689731E-2,-22.527382834567899,9,29.107180096,9,-2351.8755200000001,7.5,2363.8755200000001,9,0.80305874663457866,1.1791103048148146,19.273409919229888,56.597294631111104,42.390110808246213,23.027048911228551,2.4096396022102509,147.61273711317611,2.7280914981752417E-3,2.6969955574744717,-152724.71990740742,7004.1384134881137,1.9906499766788239E-3,0.70841466926841645,-153599.19481616287,8607.9613552061583,3.5752045454545449,9.6187605379534965E-3,8.3994568553160462,-144553.60802371957,3464.5268242511429]
["ACC","AHR92 E4-64",2.2000000000000002,2.9,2,3.92,3000,7.4,6000,2.8,30,64,0.13,560,6,3688.1142625282955,5133.3234789388498,6000,1.8577784347374098,865.38461538461536,4.5089008218778508,3.9347895481081077,8.4179329371848424E-2,-22.540052661728392,9,29.117442655999998,9,-2352.9227199999996,7.5,2364.9227199999996,9,0.54445922844589911,0.79962673960606045,13.067021482701579,38.382083501090904,28.745804143824412,23.029078084985755,2.4113951708280417,147.72028194628078,1.0434953877449355E-2,3.0276500050966888,-153104.51119669422,3688.1142625282955,5.544622760713074E-3,1.447353200636587,-153536.14164505657,5133.3234789388498,4.6631125000000004,5.9145381349966199E-2,8.922223436049789,-148805.23101545434,1512.5322976984471]
["ACC","AHR92 G4-64",3,4,2.4,4.7,3000,9.1999999999999993,6000,1.5,19,64,0.16,560,6,4223.5992571211937,5554.177502256287,6000,1.8891644995487424,703.125,3.3093738053821524,3.1656087165217395,5.5377962732615686E-2,-22.547654558024689,9,29.123600192000001,9,-2353.5510399999998,7.5,2365.5510399999998,9,0.55074650418334414,0.80898889422222231,13.217916100400259,38.831466922666671,29.081442364596342,23.030295935866551,2.4124485119987162,147.78480884614356,8.1168820967928174E-3,2.0396630309931099,-153410.07999999999,4223.5992571211937,4.8234913066725676E-3,0.86758424951125057,-153618.05868957521,5554.177502256287,5.2177083333333334,2.6695565834845211E-2,4.835571430355218,-152236.83013561598,2299.180905015975]
["ACC","AHR92 J4-64",3.8,5.0999999999999996,3.4,3.33,3000,11.4,6000,5,15,64,0.2,560,6,3823.1332875819735,5919.5125418076577,6000,3.0107316610923123,562.5,2.6110157747309115,2.5554219508771934,5.4639859623515995E-2,-22.557790419753086,9,29.131810240000004,9,-2354.3888000000002,7.5,2366.3888000000002,9,0.55440893323275897,0.81454074684210542,13.305814397586214,39.097955848421059,29.279782396556403,23.031920141352959,2.4138529668929491,147.87084471262733,7.9947589840485764E-3,8.4801207538572232,-149274.8125,3823.1332875819735,4.1766615284543939E-3,1.2197534799601926,-153573.19198291778,5919.5125418076577,2.2007031250000004,1.8374389222281979E-2,16.228502638526884,-137589.51892769322,2330.2394140617148]
["ACC","AHR115 A6-44",3.7,7.2,3.2,6.27,3000,11,6000,1.29,6.9,44,0.27,560,6,6000,6000,6000,2.7,416.66666666666663,2.6825078938358797,2.6496525294545457,3.1604937877195927E-2,-22.575528177777777,9,29.146177824000002,9,-2355.8548799999999,7.5,2367.8548799999999,9,0.803948123974357,1.1816018036756757,19.294754975384567,56.716886576432429,42.471155948870326,23.034763612537809,2.4163107629578562,148.02140747897386,3.5507530194128292E-3,2.1043911740374783,-153092.14279269541,6276.5848659724852,2.019582276202251E-3,0.47877395396036793,-153634.39972895262,8604.2197963656199,4.8699836363636351,8.2929288875491312E-3,4.1753904697082911,-151412.72345370211,4028.6095472880193]
["ACC","AHR115 A6-88",3.7,3.6,3.2,3.14,3000,11,6000,5.5,28,88,0.27,560,6,2943.1159930223025,4153.509041703107,4454.545454545454,3.0077484930494824,416.66666666666663,2.6825078938358797,2.6496525294545457,7.0315601174231565E-2,-22.575528177777777,9,29.146177824000002,9,-2355.8548799999999,7.5,2367.8548799999999,9,0.4019740619871785,0.59080090183783784,9.6473774876922835,28.358443288216215,21.235577974435163,23.034763612537809,2.4163107629578562,148.02140747897386,1.4391586469332376E-2,8.972210431942738,-151065.19576333091,2943.1159930223025,8.2810529690146989E-3,2.5502104099358807,-153454.04477224479,4153.509041703107,3.0420757575757578,3.3914091618559752E-2,17.802052390229147,-143433.07704983008,1810.7497105518091]
["ACC","AHR115 C6-64",6.8,9.1,5.2,6.93,3000,22,6000,0.9,6.7,64,0.51,560,6,4479.4457931560491,5991.4255385384668,6000,3.6045730461128183,220.58823529411765,1.4613017939728181,1.3270653687272729,2.8342268914976338E-2,-22.636343348148149,9,29.195438112000005,9,-2360.8814400000001,7.5,2372.8814400000001,9,0.55311279372658539,0.81396595226470592,13.274707049438049,39.070365708705886,29.249561536014365,23.044523390467841,2.4247374923232528,148.5376226778763,6.9761886528627113E-3,2.9372321365436265,-153137.42940527681,4479.4457931560491,4.1911031178635486E-3,0.53373438351821423,-153646.61276903385,5991.4255385384668,5.3498557291666664,6.9388198194668457E-3,2.9181154567385805,-153144.26136359517,4492.3698542087086]
["ACC","AHR115 C6-88",6.8,6.6,5.2,5.09,3000,22,6000,1.7,12.6,88,0.51,560,6,3208.9852539853596,4304.7205013706553,4454.545454545454,4.5041490659356507,220.58823529411765,1.4613017939728181,1.3270653687272729,3.9560725848123132E-2,-22.636343348148149,9,29.195438112000005,9,-2360.8814400000001,7.5,2372.8814400000001,9,0.40115872951598502,0.59034893241176489,9.6278095083836401,28.336748755764713,21.213967707438993,23.044523390467841,2.4247374923232528,148.5376226778763,1.3102182558134706E-2,5.5328630996980221,-152675.73250000001,3208.9852539853596,8.0057520167358502E-3,1.2228866097600146,-153615.72224753583,4304.7205013706553,4.7194780303030299,1.3032663142758718E-2,5.4968530169517056,-152688.55471687851,3218.4433360076191]
["ACC","AHR115 E6-88",9.8000000000000007,9.5,8,7.84,3000,33,6000,1.01,8.1,88,0.75,560,6,3279.3906324110171,4308.1969197491271,4454.545454545454,7.2150818481505237,150,1.0140068997512435,0.8862029818181818,3.3788504052662267E-2,-22.697158518518517,9,29.244698400000001,9,-2365.9079999999999,7.5,2377.9079999999999,9,0.40083252959843835,0.59061359438775507,9.6199807103625208,28.349452530612243,21.218129104801449,23.054299772451163,2.4331642216886484,149.05383787677869,1.2713972497676246E-2,4.92465876081656,-152881.0627611542,3279.3906324110171,8.0115629693093063E-3,1.1426471835303234,-153621.84986486216,4308.1969197491271,7.4224534090909087,9.9304785530888659E-3,3.2664180056272838,-153319.55634725315,3768.2625509277063]
["ACC","AHR142 C6-64",11.3,15,9.75,13,2000,30,6000,0.43,4.7,64,1.1499999999999999,560,6,4649.7135633122225,5956.2561423997622,6000,6.6839014896401823,97.826086956521749,0.8801710606456512,0.97755996266666678,2.4642655778184894E-2,-22.79851713580247,9,29.326798880000002,9,-2374.2856000000002,7.5,2386.2856000000002,9,0.54926986753551843,0.81102873008849563,13.182476820852441,38.929379044247788,29.12448063178833,23.07063058297204,2.4472087706309753,149.91419654161604,6.6891334372540679E-3,1.8982050620294668,-153444.07919570836,4649.7135633122225,4.2526641417402825E-3,0.46656858821265496,-153650.71348586996,5956.2561423997622,9.7882812500000007,5.4829892772276043E-3,1.3882486070575764,-153546.370959778,5166.8113867106322]
["ACC","AHR142 C6-130",11.3,7.4,9.75,6.37,2000,30,6000,1.7,19,130,1.1499999999999999,560,6,2235.6267350218454,2865.0184078968928,3015.3846153846152,9.0796107338799068,97.826086956521749,0.8801710606456512,0.97755996266666678,5.1040192736268725E-2,-22.79851713580247,9,29.326798880000002,9,-2374.2856000000002,7.5,2386.2856000000002,9,0.27097313465085576,0.40010750684365787,6.5033552316205387,19.205160328495577,14.368077111682245,23.07063058297204,2.4472087706309753,149.91419654161604,2.7213765970660598E-2,7.5201660814994913,-152827.41867021692,2235.6267350218454,1.7895273817884399E-2,2.3360927706730079,-153583.27027465694,2865.0184078968928,6.1029130769230768,2.2416523987400048E-2,5.4998589437547505,-153216.5377455444,2494.5821645191586]
["ACC","AHR142 G6-64",21,28,17,22.66,2000,60,6000,0.15,2.1,64,2.2000000000000002,560,6,4876.2346614950402,6000,6000,9,51.136363636363633,0.47478157163357376,0.49237187733333332,2.1698172379186174E-2,-23.064583506172838,9,29.542312639999999,9,-2396.2768000000001,7.5,2408.2768000000001,9,0.55274144524941526,0.82061979555555553,13.265794685985966,39.389750186666667,29.436856529040654,23.113717406138719,2.4840757116045835,152.17263803681411,6.1851978596225952E-3,1.3302150202128977,-153556,4876.2346614950402,4.1598980214901044E-3,0.23263538127127176,-153660.69682491338,6049.8138186401193,13.99084375,4.378867114705429E-3,0.48946685878477475,-153649.377331186,5867.9575518374495]
["ACC","AHR142 G6-130",21,13.8,17,11.11,2000,60,5400,0.6,8.4,130,2.2000000000000002,560,6,2370.6972260905327,2926.3933370159116,3015.3846153846152,15.147213325968178,51.136363636363633,0.47478157163357376,0.49237187733333332,4.4404505294078349E-2,-23.064583506172838,9,29.542312639999999,9,-2396.2768000000001,7.5,2408.2768000000001,9,0.27242256944435467,0.40444832780952383,6.5381416666645125,19.413519734857143,14.508165003598609,23.113717406138719,2.4840757116045835,152.17263803681411,2.5019731436459733E-2,5.3267985407632557,-153244.25469387756,2370.6972260905327,1.746144519178703E-2,1.4007128829005338,-153634.97638194787,2926.3933370159116,10.367973846153845,1.799937170050004E-2,1.9600525550443886,-153607.16855002166,2867.3656790068057]
["ACC","AHR142 J6-88",25,24,21,20.59,2000,76,6000,0.21,3,88,2.7,560,6,3585.126793003948,4361.673760152692,4454.545454545454,16.276652479694615,41.666666666666664,0.39903726374265669,0.39006497684210528,2.9417886835410974E-2,-23.191281777777778,9,29.644938240000002,9,-2406.7488000000003,7.5,2418.7488000000003,9,0.39832902109184132,0.59289876480000003,9.5598965062041916,28.4591407104,21.257256847575913,23.134345751902963,2.5016313977824911,153.24808636786074,1.1290281192967216E-2,2.3353254894857631,-153487.93643008001,3585.126793003948,7.9482599640572187E-3,0.5604701154018521,-153653.85902794878,4361.673760152692,17.510149999999999,8.0450356698341229E-3,0.68040863147875286,-153649.05436771078,4328.1135448605219]
["ACC","AHR142 J6-130",25,16,21,13.73,2000,76,5400,0.43,6.3,130,2.7,560,6,2438.7393724795934,2935.019545722379,3015.3846153846152,19.12996090855524,41.666666666666664,0.39903726374265669,0.39006497684210528,4.3531768151338614E-2,-23.191281777777778,9,29.644938240000002,9,-2406.7488000000003,7.5,2418.7488000000003,9,0.26555268072789423,0.39526584320000002,6.3732643374694611,18.972760473600001,14.17150456505061,23.134345751902963,2.5016313977824911,153.24808636786074,2.3850711138215745E-2,4.709404576560396,-153335.91580672,2438.7393724795934,1.7403533037904966E-2,1.2675507799228889,-153640.23247071475,2935.019545722379,13.091606153846154,1.7490029912874881E-2,1.3721083152836324,-153636.14968596346,2924.8514333457192]
["ACC","AHD190 E8-180",45,21,32,15.238095238095237,2000,130,3900,0.36,5.8,180,7.8,560,6,1840.352062223551,2130.8348237237083,2177.7777777777774,31.149573645795897,14.423076923076923,0.22406323205508644,0.23609014892307692,5.9218261658001398E-2,-24.483604148148149,9,30.69171936,9,-2513.5631999999996,7.5,2525.5631999999996,9,0.19542704096960076,0.29839171600000003,4.6902489832704184,14.322802368000001,10.644376139238174,23.348790119872437,2.6806993967971584,164.21765934453703,4.1564679092293201E-2,6.8090381347147693,-153306.26079999999,1840.352062223551,3.3012159867478588E-2,1.7597848009969976,-153640.10460998595,2130.8348237237083,15.679201058201057,3.2682135296199358E-2,1.194691698664627,-153652.98697334214,2150.0792307758097]
["ACC","AHD190 G8-130",56,37,40,26.143790849673202,2000,170,4000,0.123,2.2000000000000002,130,10,560,6,2605.532148027592,2979.9946511862363,3015.3846153846152,32.160042790510104,11.25,0.18077501942350821,0.18319571764705883,4.2504709822003842E-2,-25.041076543209879,9,31.143272,9,-2559.64,7.5,2571.64,9,0.27781151903902107,0.42868343154761906,6.6674764569365053,20.576804714285714,15.260415301146377,23.443532814751265,2.757944415979956,168.9496320011425,2.1419928941999539E-2,3.1107972728202813,-153520.84822969546,2605.532148027592,1.7089415026806321E-2,0.63681475989450542,-153658.00099055591,2979.9946511862363,22.9934442182001,1.6983433233649089E-2,0.42264471619253069,-153661.3575657378,2995.5257901232203]
["ACC","AHD190 J8-180",67,32,44,20.952380952380953,2000,220,3900,0.18,3.2,180,13,560,6,1868.7686126049393,2147.2089581544392,2177.7777777777774,42.30709698122395,8.6538461538461533,0.15203935581085778,0.14435920727272727,5.8813083322800372E-2,-25.801266172839508,9,31.759025600000001,9,-2622.4720000000002,7.5,2634.4720000000002,9,0.20194717817747496,0.31601020497512439,4.8467322762593987,15.168489838805971,11.218553168611322,23.574859847905383,2.8632785330474064,175.4023219874226,4.0768674538928566E-2,5.8966247910929948,-153395.71154377368,1868.7686126049393,3.2758340488328784E-2,1.2201777334337149,-153652.51208563914,2147.2089581544392,21.74289947089947,3.2495396988819696E-2,0.6295677720445032,-153660.94170077471,2164.8916751173956]
["6SMx7","6SM27M-4000",0.32,0.8,0.3,0.75,4000,1.4350000000000001,9000,31,21,25,8.0000000000000002E-3,670,6,9000,9000,9000,0.27499999999999997,14062.5,30.981934284806442,20.273450877770031,"NA",-22.509138283456789,9,29.092402009599997,9,-2350.3675519999997,7.5,2362.3675519999997,9,1.03237314042891,1.5152292713333333,24.776955370293841,72.731005023999998,54.478050984173713,23.024128170010936,2.4071115834006322,147.45787255350538,1.0451297326641933E-3,4.8156425109188437,-144387.83488281249,9673.6608791594299,6.3847133582665386E-4,0.86231881505624119,-153366.56250448001,14838.082788757194,0.64239999999999997,9.7506916606469179E-2,73.128032956485328,1985419.6816339213,-9999]
["6SMx7","6SM27LL-4500",0.8,0.82,0.72,0.79,4000,3.6259999999999999,9000,37,42,59,1.4E-2,670,6,{"$f":"IF(AQ257<I257,IF(AQ257<0,0,AQ257),I257)","v":3977.1264009376482},{"$f":"IF(AU257<I257,IF(AU257<0,0,AU257),I257)","v":6154.6193373518045},{"$f":"IF(UAC_V*0.98/L257*1000<I257,IF(UAC_V*0.98/L257*1000<0,0,UAC_V*0.98/L257*1000),I257)","v":6644.0677966101694},{"$f":"C257+(E257-C257)/G257*Q257","v":0.67690761325296389},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M257,(inertia/gear^2+gear_inertia)/M257),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M257,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M257))","v":8035.7142857142853},{"$f":"IF((C257+(E257-C257)/G257*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X257^2*time1+Y257^2*time2+Z257^2*time3+AA257^2*time4)/time)/(C257+(E257-C257)/G257*mspeed),SQRT((((X257-Y257)*2/PI()+Y257)^2*time1+Y257^2*time2+((Z257-Y257)*2/PI()+Y257)^2*time3+AA257^2*time4)/time)/(C257+(E257-C257)/G257*mspeed)),IF(AccType=1,SQRT((X257^2*time1+Y257^2*time2+Z257^2*time3+AA257^2*time4+AB257^2*time5+AC257^2*time6+AD257^2*time7+AE257^2*time8)/time)/(C257+(E257-C257)/G257*mspeed),SQRT((((X257-Y257)*2/PI()+Y257)^2*time1+Y257^2*time2+((Z257-Y257)*2/PI()+Y257)^2*time3+AA257^2*time4+((AB257-AC257)*2/PI()+AC257)^2*time5+AC257^2*time6+((AD257-AC257)*2/PI()+AC257)^2*time7+AE257^2*time8)/time)/(C257+(E257-C257)/G257*mspeed))))","v":12.395483765915712},{"$f":"IF(move1,MAX(ABS(X257),ABS(Z257))/H257,MAX(ABS(X257),ABS(Z257),ABS(AB257),ABS(AD257))/H257)","v":8.0236165242140096},{"$f":"IF(AZ257>0,speed/(MIN(AZ257,I257)),\"NA\")","v":"NA"},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M257+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M257+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.510658662716047},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M257+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M257+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.093633516800001},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M257+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M257+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2350.4932159999998},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M257+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M257+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2362.4932159999998},9,{"$f":"AH257/Irms","v":0.4232774610721417},{"$f":"AI257/Ipeak","v":0.62127029905666664},10.158659065731401,{"$f":"IF(move1,MAX(ABS(X257),ABS(Z257))/(C257/D257),MAX(ABS(X257),ABS(Z257),ABS(AB257),ABS(AD257))/(C257/D257))","v":29.820974354719997},22.33680450539039,{"$f":"IF((C257+(E257-C257)/G257*mspeed)<0,\"NA\",U257*(C257+(E257-C257)/G257*mspeed)*mspeed/9.55)","v":23.02437150789202},{"$f":"IF(move1,IF(speed1>speed2,AM257/2*time1/time,AM257/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z257*-speed/30*PI(),((Z257-AA257)*2/PI()+AA257)*-speed/30*PI()),IF(AccType=1,X257*-speed/30*PI(),((X257-Y257)*2/PI()+Y257)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z257*-speed/30*PI(),((Z257-AA257)*2/PI()+AA257)*-speed/30*PI()),IF(AccType=1,X257*-speed/30*PI(),((X257-Y257)*2/PI()+Y257)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD257*-speed/30*PI(),((AD257-AE257)*2/PI()+AE257)*-speed/30*PI()),IF(AccType=1,AB257*-speed/30*PI(),((AB257-AC257)*2/PI()+AC257)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD257*-speed/30*PI(),((AD257-AE257)*2/PI()+AE257)*-speed/30*PI()),IF(AccType=1,AB257*-speed/30*PI(),((AB257-AC257)*2/PI()+AC257)*-speed/30*PI()),0)/2*time7/time)))","v":2.4073222516347665},{"$f":"IF(move1,MAX(IF(AccType=1,Z257*-speed/30*PI(),((Z257-AA257)*2/PI()+AA257)*-speed/30*PI()),IF(AccType=1,X257*-speed/30*PI(),((X257-Y257)*2/PI()+Y257)*-speed/30*PI()),0),MAX(IF(AccType=1,Z257*-speed/30*PI(),((Z257-AA257)*2/PI()+AA257)*-speed/30*PI()),IF(AccType=1,X257*-speed/30*PI(),((X257-Y257)*2/PI()+Y257)*-speed/30*PI()),IF(AccType=1,AD257*-speed/30*PI(),((AD257-AE257)*2/PI()+AE257)*-speed/30*PI()),IF(AccType=1,AB257*-speed/30*PI(),((AB257-AC257)*2/PI()+AC257)*-speed/30*PI()),0))","v":147.47077793347793},{"$f":"(L257^2)/1000000+((K257/1000)^2*(D257/C257*H257)^2*PI()*PI()*(O257/2)^2)/1200","v":5.2846942461981915E-3},{"$f":"SQRT(3)*L257*J257*D257/C257*H257/1000","v":14.052902341914743},{"$f":"0.75*J257^2*(D257/C257*H257)^2-(UAC_V*0.98)^2","v":-139481.00199429813},{"$f":"-AO257/2/AN257+SQRT((AO257/2/AN257)^2-AP257/AN257)","v":3977.1264009376482},{"$f":"(L257^2)/1000000+((K257/1000)^2*AV257^2*PI()*PI()*(O257/2)^2)/1200","v":3.5605714424263414E-3},{"$f":"SQRT(3)*L257*J257*AV257/1000","v":2.9516386168693263},{"$f":"0.75*J257^2*AV257^2-(UAC_V*0.98)^2","v":-153038.30547798087},{"$f":"-AS257/2/AR257+SQRT((AS257/2/AR257)^2-AT257/AR257)","v":6154.6193373518045},{"$f":"D257+(F257-D257)*((0.85*UAC_V-D257*J257)/L257*1000)/G257","v":0.78063644067796611},6.862908825294764E-2,84.456952455757857,358615.28886197519,{"$f":"IF(((AX257/2/AW257)^2-AY257/AW257)>0,-AX257/2/AW257+SQRT((AX257/2/AW257)^2-AY257/AW257),-9999)","v":-9999}]
["6SMx7","6SM37S-6000",0.5,1,0.4,0.95,4500,2,9000,36,32,30,4.4999999999999998E-2,670,6,6506.0405479617602,9000,9000,0.30000000000000004,2500,19.842421790346197,14.549998152000001,"NA",-22.518513955555555,9,29.099996304000001,9,-2351.14248,7.5,2363.14248,9,0.82595234572365739,1.212499846,19.822856297367778,58.199992608000002,43.592110143283413,23.025628919357995,2.4084107041777978,147.53745573000288,2.1127769888058603E-3,7.4824594886975495,-138112,6506.0405479617602,9.596907539589206E-4,1.6599974939740116,-152898.55786666667,11786.962845858156,0.88740740740740731,0.1449378896886164,81.544049543489919,1693400.4488753164,-9999]
["6SMx7","6SM37M-6000",1,1.6,0.8,1.5,6000,4.03,9000,12.8,21,38,7.0000000000000007E-2,670,6,6376.9742477178916,9000,9000,0.70000000000000007,1607.1428571428569,9.9192003049269211,7.2221160258064518,1.0483813190352145,-22.524848869135798,9,29.105127584000002,9,-2351.66608,7.5,2363.66608,9,0.66079098213048304,0.97017091946666678,15.858983571131592,46.568204134400006,34.878914793515619,23.026643163147476,2.4092884884866925,147.59122814655515,2.8012181407337847E-3,5.4322434185440853,-148555.05461247999,6376.9742477178916,1.5135699686582625E-3,1.2298872473550628,-153402.11934882158,9669.2409089015891,1.4598596491228071,4.1156344410665104E-2,29.384422353138202,-4175.7248913420772,121.44813357671012]
["6SMx7","6SM37L-4000",1.5,1.6,1.2,1.5,4000,6.1440000000000001,9000,15.5,30,58,0.1,670,6,4090.8234993576552,6294.1738553264149,6758.620689655173,1.0279369608505189,1125,6.6155978327056362,4.7381648958333331,0.15523791434808079,-22.532450765432099,9,29.111285120000002,9,-2352.2943999999998,7.5,2364.2943999999998,9,0.44055061042188709,0.6469174471111111,10.573214650125291,31.052037461333335,23.256791205454856,23.027860494065653,2.4103418296573671,147.65575504641797,6.2252998985817109E-3,10.204700187062571,-145925.00580352001,4090.8234993576552,3.5068129210221511E-3,2.2798291959706098,-153277.73207767538,6294.1738553264149,1.4641379310344826,3.9397222714936377E-2,36.213467645993092,-56204.484620437812,820.18593852031086]
["6SMx7","6SM37VL-6000",3,3.8,2,2.8,6000,12,9000,3.65,8,48,0.16,670,6,6029.3052923269233,7934.4012930498411,8166.6666666666661,1.6775997844916932,703.125,3.3085570019136821,2.4269666826666669,2.9549063945115694E-2,-22.547654558024689,9,29.123600192000001,9,-2353.5510399999998,7.5,2365.5510399999998,9,0.52320917897417696,0.76853944951111108,12.557020295380246,36.889893576533332,27.627370246366524,23.030295935866551,2.4124485119987162,147.78480884614356,3.3985312323972887E-3,4.612520582588223,-151355.47719999999,6029.3052923269233,2.3377119409033536E-3,0.80949862664132266,-153592.89669850975,7934.4012930498411,2.6676041666666666,5.9199305335752347E-3,8.3836719673783584,-146037.48571434399,4308.8997577049222]
["6SMx7","6SM47L-3000",3,2.2999999999999998,2.2000000000000002,2,3000,11.97,6000,11,25,81,0.16,670,6,3120.4997216769993,4559.0539589953814,4839.5061728395067,1.7842522776012317,703.125,3.3110086228120363,2.4330493059314953,6.4068070445073122E-2,-22.547654558024689,9,29.123600192000001,9,-2353.5510399999998,7.5,2365.5510399999998,9,0.31667923990542285,0.46516861417777777,7.6003017577301488,22.328093480533333,{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X262),ABS(Z262))/(C262/D262),MAX(ABS((X262-Y262)*2/PI()+Y262),ABS((Z262-Y262)*2/PI()+Y262))/(C262/D262)),IF(AccType=1,MAX(ABS(X262),ABS(Z262),ABS(AB262),ABS(AD262))/(C262/D262),MAX(ABS((X262-Y262)*2/PI()+Y262),ABS((Z262-Y262)*2/PI()+Y262),ABS((AB262-AC262)*2/PI()+AC262),ABS((AD262-AC262)*2/PI()+AC262))/(C262/D262)))","v":16.721829359642896},23.030295935866551,2.4124485119987162,147.78480884614356,1.0457211191936206E-2,14.162471962604092,-146021.27739325,3120.4997216769993,6.7300367818471374E-3,2.9499076918947824,-153332.42114804528,4559.0539589953814,1.9114814814814816,{"$f":"(L262^2)/1000000+((K262/1000)^2*AJ262^2*PI()*PI()*(O262/2)^2)/1200","v":1.9497255980169149E-2},{"$f":"SQRT(3)*L262*J262*AJ262/1000","v":25.806084719341012},{"$f":"0.75*J262^2*AJ262^2-(UAC_V*0.98)^2","v":-128288.52337517888},1987.3230704313737]
["6SMx7","6SM57S-3000",4.5999999999999996,2.8,3,2.7,3000,18.149999999999999,6000,6.3,35,97,0.31,670,6,2436.3170006239229,3765.7828910279309,4041.2371134020618,2.5915824581184368,362.90322580645159,2.1612244834242644,1.6063023620936643,5.9073250327794723E-2,-22.585664039506174,9,29.154387872000004,9,-2356.6926400000002,7.5,2368.6926400000002,9,0.25149427244460565,0.36971144040579712,6.0358625386705356,17.746149139478263,13.288241107388183,23.036389088237506,2.4177152178520886,148.10744334545757,2.0476531215102099E-2,11.69364055413944,-150030.74382481095,2436.3170006239229,1.0064768951161665E-2,2.8464252771660949,-153448.7237522986,3765.7828910279309,2.6892233676975947,2.542050283368634E-2,14.065021831760552,-148407.73368243434,2155.3571839538463]
["6SMx7","6SM57M-3000",8,4.3,6,4,3000,31.45,6000,3.9,24,112,0.45,670,6,2221.1737398454484,3293.2397503199059,3500,5.8045068331200627,250,1.242110248142287,0.92792124133545317,4.8190225129914097E-2,-22.621139555555558,9,29.183123040000002,9,-2359.6248000000005,7.5,2371.6248000000005,9,0.22213330498816827,0.32679017987500003,5.3311993197160383,15.685928634000001,11.743824167523032,23.042081888530561,2.4226308099819041,148.4085688781507,2.4727771036915383E-2,12.78917044650211,-150404.21682259082,2221.1737398454484,1.3230081674319664E-2,3.0348653036212778,-153480.43799005254,3293.2397503199059,4.0114017857142859,1.8424341828208714E-2,8.8849051782276973,-152090.70719016867,2642.1116342633536]
["6SMx7","6SM77K-3000",11,6,8.5,5,3000,44.4,6000,2.2000000000000002,18,112,1.2,670,6,2200.0073708799409,3336.7545083606756,3500,8.2193712430327697,93.75,0.90440001231177147,0.66074462702702708,4.330888122143E-2,-22.81118696296296,9,29.337061440000003,9,-2375.3328000000001,7.5,2387.3328000000001,9,0.2257199841110458,0.33337569818181828,5.4172796186650993,16.002033512727277,11.971077504304537,23.07267516827395,2.4489643392487652,150.02174137472068,2.6610598435494747E-2,10.335770707054216,-151534.93119999999,2200.0073708799409,1.3150163259707696E-2,2.1455721643732546,-153572.25334995749,3336.7545083606756,5.0273809523809518,1.5980944380766866E-2,5.1089843626483926,-153143.79669129095,2939.9040308276108]
["6SMx7","6SM77S-3000",17,10,12,8,3000,68,6000,1.1000000000000001,8.3000000000000007,103,1.8,670,6,2646.3833296405514,3679.6922063947363,3805.8252427184466,10.867179656008773,62.5,0.58611394451853949,0.43323841411764702,3.5866114584251069E-2,-22.963224888888885,9,29.460212159999998,9,-2387.8991999999998,7.5,2399.8991999999998,9,0.24368295430050682,0.3610320117647059,5.8483909032121639,17.329536564705883,12.956103298759777,23.097266143427508,2.4700311626622553,151.31227937197667,1.8768004566292549E-2,7.8496542599021524,-152212,2646.3833296405514,1.0924883816046541E-2,1.5445274401360869,-153607.78440443648,3679.6922063947363,7.8705501618122984,1.146498469088947E-2,2.5425232862710501,-153511.66649398551,3549.9790247540404]
["6SMx7","6SM107K-3000",26,16,20,14,3000,112,6000,0.45,4.4000000000000004,97,8.1999999999999993,670,6,2914.5644447309191,3931.0119317620188,4041.2371134020618,18.137976136475963,13.719512195121952,0.38750384775787783,0.27476624857142862,3.2424465579696672E-2,-24.584962765432099,9,30.773819840000005,9,-2521.9408000000003,7.5,2533.9408000000003,9,0.25789501886485366,0.39453615179487184,6.1894804527564879,18.937735286153849,14.068704141608325,23.365916768264842,2.6947439457394844,165.07801800937435,1.62166258145609E-2,5.210861531103216,-152942.53443786982,2914.5644447309191,9.6784717528641696E-3,1.0367363313784272,-153635.44164574344,3931.0119317620188,13.712714776632303,9.692644623035488E-3,1.0636505576470212,-153633.93961874847,3926.7865236071343]
["6SMx7","6SM107S-3000",32,20,23,16,3000,136,6000,0.37,3.6,97,10.4,670,6,2901.7829715720277,3943.3082982923661,4041.2371134020618,20.170075105122901,10.817307692307692,0.31624502401056503,0.22959832705882355,3.2217693878905038E-2,-25.142435160493829,9,31.225372480000001,9,-2568.0176000000001,7.5,2580.0176000000001,9,0.26298937890872837,0.40658037083333332,6.3117450938094803,19.515857799999999,14.468194730626442,23.460901607070017,2.7719889649222837,169.80999066597988,1.6340127082753023E-2,5.2838807961099956,-152922.173125,2901.7829715720277,9.6373470109238531E-3,0.95906655436488519,-153639.56040345144,3943.3082982923661,15.428178694158074,9.6098143302354132E-3,0.89939077990043392,-153642.50717996148,3951.9884617465841]
["6SM45100","6SM45S-3000",0.85,1.3,0.8,1.4,3000,3.2,8000,25.4,54,41.012193308819754,0.15,560,6,3954.5144246497775,7714.2328023854161,8000,0.72142945329357655,750,11.667737243947352,9.100483650000001,"NA",-22.545120592592593,9,29.121547680000003,9,-2353.3416000000002,7.5,2365.3416000000002,9,0.63172750083209717,0.92789245058823544,15.161460019970333,44.538837628235299,33.35612662922653,23.029889956690972,2.4120973982751583,147.76329987952266,6.8520808926598887E-3,8.8304278132491891,-142074.15823944638,3954.5144246497775,2.2002429351720308E-3,2.7957592514093266,-152502.24765281795,7714.2328023854161,1.5495030341248806,0.24184149195307689,60.184263961451023,384704.85085933609,-9999]
["6SM45100","6SM45M-3000",1.7,1.3,1.6,1.3,3000,7.6,8000,34,99,82.024386617639507,0.21,560,6,1596.1474472113118,3997.3598118959449,4779.0665211228734,1.566754672936802,535.71428571428578,5.8344857808969879,3.8334029936842109,"NA",-22.560324385185183,9,29.133862752000002,9,-2354.5982399999998,7.5,2366.5982399999998,9,0.31589716531527784,0.46414242129411765,7.5815319675666686,22.278836222117647,16.684058622750516,23.032326264912953,2.414204080616507,147.89235367924826,3.1232590220516127E-2,28.073112044089445,-124379.68,1596.1474472113118,7.9540780079170974E-3,6.2795119045989551,-152198.76999999999,3997.3598118959449,1.3,0.20867379395342894,80.590572875837481,87672.223114434863,-9999]
["6SM45100","6SM45L-3000",3.2,2.4,2.9,2.2999999999999998,3000,13.1,8000,11.9,47,82.024386617639507,0.34,560,6,2181.8635399211994,4249.8583041530701,4779.0665211228734,2.7750141695846926,330.88235294117646,3.1010827620796246,2.2259958326717557,9.6227265751530094E-2,-22.593265935802467,9,29.160545408000001,9,-2357.32096,7.5,2369.32096,9,0.30989327444824138,0.45563352200000001,7.4374385867577937,21.870409056,16.375951371335432,23.037608498016418,2.4187685590227637,148.17197024532041,2.251217338009889E-2,16.610516586107426,-143411.72364531251,2181.8635399211994,7.573127425809751E-3,3.8435569074001426,-153115.06533515075,4249.8583041530701,2.2734360138317595,5.0578020897673333E-2,27.68580273454004,-125182.14532342952,1323.1588103342915]
["6SM45100","6SM56S-3000",3.8,2.8,3.6,2.9,3000,16.5,8000,9.4,54,80.610173055266415,0.52,560,6,1738.8881333969307,4057.6987022359513,4862.909793423275,3.52948675318427,216.34615384615384,2.6114734350866349,1.7695448863030303,9.6579802062623149E-2,-22.638877313580245,9,29.197490624,9,-2361.0908799999997,7.5,2373.0908799999997,9,0.30455331400591606,0.44820709291228072,7.3092795361419851,21.513940459789474,16.105984545697964,23.044930408358983,2.4250886060468106,148.5591316444972,3.8403480263062589E-2,15.956466082438178,-143868.33941828256,1738.8881333969307,8.3506696864055711E-3,3.8450595302060724,-153095.19102836147,4057.6987022359513,2.92971067551029,6.2489626629231174E-2,21.138083664183366,-136473.38054039644,1318.3290062135181]
["6SM45100","6SM56M-3000",7,4.8,6.4,4.7,3000,28.4,8000,4,30,87.681240867131891,1,560,6,1955.2583562101399,3943.0322815983627,4470.7396487923652,6.2113935436803276,112.5,1.4192082969200968,1.0315496901408452,5.3419116708635722E-2,-22.760507654320985,9,29.296011200000002,9,-2371.1439999999998,7.5,2383.1439999999998,9,0.28366173636543734,0.4185144457142857,6.8078816727704963,20.088693394285713,15.031434534935231,23.064501137139516,2.4419420647776025,149.591562042302,3.2953424124805994E-2,11.830111650082614,-149113.02635102041,1955.2583562101399,9.145914158420379E-3,2.841787003266683,-153401.39095434654,3943.0322815983627,4.6780430884921271,2.2740352414135342E-2,9.1311974887348875,-150952.67170986347,2383.4904490836161]
["6SM45100","6SM56L-3000",10,7.6,8.4,6.7,3000,37.4,8000,1.8,15.8,79.903066274079862,1.5,560,6,2506.9087408795026,4529.1778199353084,4905.9443933650737,7.5844384960345028,75,0.99487382312464701,0.78605980748663096,3.6750361141720166E-2,-22.887205925925926,9,29.398636799999998,9,-2381.616,7.5,2393.616,9,0.31467060151638154,0.46547841599999989,7.5520944363931566,22.342963967999996,16.709493392330973,23.084957751977434,2.4594977509555109,150.66701037334872,2.1314010606039917E-2,7.0807909488499812,-151700.74522432001,2506.9087408795026,7.1354489591107699E-3,1.5880500894480007,-153565.24899809711,4529.1778199353084,6.3748154787426863,1.1543930284253663E-2,4.1625538127035506,-152985.52657828911,3464.5633544257639]
["6SM45100","6SM71K-3000",10.5,8,9.5,7.6,3000,41.9,6000,1.65,19.600000000000001,79.195959492893323,2,560,6,1973.6816669743901,4316.5884560052154,4949.7474683058326,9.0611371813315955,56.25,0.94788692825368859,0.7040874081145585,4.0526248889549324E-2,-23.013904197530863,9,29.501262399999998,9,-2392.0880000000002,7.5,2404.0880000000002,9,0.31573977183756602,0.46827400634920635,7.577754524101584,22.477152304761905,16.801149716065567,23.105486055000849,2.4770534371334194,151.7424587043954,3.5252279737932046E-2,7.2254068636721058,-151583.06471836736,1973.6816669743901,7.8502027519545981E-3,1.6861352930043529,-153550.67680858119,4316.5884560052154,7.4498035807338949,1.429896104262097E-2,3.8026521360335606,-153087.62231873084,3141.7651019349546]
["6SM45100","6SM71S-3000",16.5,12.3,13.4,10.5,3000,59.4,6000,0.8,12,81.317279836452954,3.1,560,6,2267.1484245245379,4409.207273572224,4820.6236213065504,11.943819150642035,36.29032258064516,0.60480100552718097,0.50045519730639731,3.2504965772779212E-2,-23.292640395061728,9,29.727038719999999,9,-2415.1264000000001,7.5,2427.1264000000001,9,0.30952984842192405,0.46166991951515152,7.4287163621261767,22.160156136727274,16.545544537145425,23.15089972330394,2.5156759467248175,154.10844503269809,2.7512136145931836E-2,4.9893166672801996,-152722.85516800001,2267.1484245245379,7.6496031008335044E-3,1.1114314270457903,-153617.29754945086,4409.207273572224,9.863912609983819,9.5305023063762748E-3,1.8642945150949981,-153532.59757886527,3917.061638014145]
["6SM45100","6SM71M-3000",22,15.6,16.3,12.2,3000,71.900000000000006,6000,0.56999999999999995,9,85.559920523572245,4.2,560,6,2492.453254424559,4303.7271525074266,4581.5844334731682,13.822918410235891,26.785714285714285,0.4547371092087954,0.41658991710709314,3.1078334129574541E-2,-23.571376592592596,9,29.952815040000001,9,-2438.1648000000005,7.5,2450.1648000000005,9,0.29501277306640156,0.44248476763636363,7.0803065535936378,21.239268846545453,15.840365041959428,23.19665740602591,2.5542984563162179,156.47443136100091,2.2905530031985463E-2,4.30662109571192,-153030.60797547875,2492.453254424559,8.0745085223920647E-3,0.94726386126612971,-153633.35630001841,4303.7271525074266,11.214117789766433,8.8249452902422684E-3,1.3380459912062357,-153602.85775990086,4096.8719218561064]
["6SM45100","6SM100K-3000",25,18.8,19.899999999999999,15.7,3000,95.8,6000,0.46,10.5,80.610173055266415,7.4,560,6,1722.0538537998812,4265.0915100466891,4862.909793423275,17.749344432920626,15.202702702702702,0.40233419707337514,0.31951585469728605,3.1085096037885267E-2,-24.3822455308642,9,30.609618880000003,9,-2505.1856000000002,7.5,2517.1856000000002,9,0.3146863199148508,0.4795506957866667,7.5524716779564196,23.018433397760003,17.113347210556515,23.331707814134955,2.6666548478548315,163.35730067969968,4.8853158010250253E-2,4.6269165018517153,-152840.34824888012,1722.0538537998812,8.2262670760568282E-3,0.9346390825671298,-153630.39157376648,4265.0915100466891,14.552433549151186,8.8880640003053714E-3,1.0991153529411055,-153617.52206220874,4095.98073360748]
["6SM45100","6SM100S-3000",36,26.7,24.6,19.2,3000,152.6,6000,0.22,7,82.024386617639507,10.8,560,6,1664.2179271915302,4428.7462441971775,4779.0665211228734,19.170764272050729,10.416666666666666,0.28138917770569455,0.20516037326343381,2.8914463454124201E-2,-25.243793777777778,9,31.307472959999998,9,-2576.3951999999999,7.5,2588.3951999999999,9,0.31231235357667597,0.48374393983333336,7.4954964858402233,23.219709112,17.207688948769288,23.478314109383202,2.7860335138646093,170.67034933081717,5.3188478384638596E-2,3.5374441658835698,-153199.02113455915,1664.2179271915302,7.7174196425729685E-3,0.51622379497691928,-153654.0978371544,4428.7462441971775,16.516260328847572,7.8019948104144149E-3,0.53783473468269627,-153653.25140450985,4403.4693804894196]
["6SM45100","6SM100M-3000",46,35,27.1,21.8,3000,198,6000,0.16,5,79.903066274079862,14.1,560,6,1745.4311098239696,4694.685493017103,4905.9443933650737,16.423481393992255,7.9787234042553195,0.22173539069748688,0.16153940363636365,2.7307893296183567E-2,-26.080002370370373,9,31.984801920000002,9,-2645.5104000000001,7.5,2657.5104000000001,9,0.32238156480079994,0.50700546521739132,7.7371575552191985,24.336262330434785,17.981310387344614,23.623622405196041,2.9019010426388059,177.76830831572536,4.8384744955270238E-2,3.3359494307410067,-153228.23531190926,1745.4311098239696,6.8935588536306117E-3,0.36726331042067056,-153658.71836717124,4694.685493017103,16.585687901475424,6.9828340149541823E-3,0.39816711961463525,-153657.79211155369,4662.533030012627]
["6SM45100","6SM100L-3000",57,42,28,22.5,3000,243,6000,0.12,4,81.317279836452954,17.5,560,6,1820.8126926684781,4704.8773554511317,4820.6236213065504,11.519518897305723,6.4285714285714288,0.18023235798294931,0.1344965267489712,2.7271404724106427E-2,-26.941550617283951,9,32.682656000000001,9,-2716.72,7.5,2728.72,9,0.31421989806744782,0.50170743859649125,7.5412775536187473,24.08195705263158,17.740834684469281,23.776381181474601,3.0212797086485828,185.0813569668428,4.458265832959514E-2,3.0262543328496712,-153317.75367534626,1820.8126926684781,6.8870470354920133E-3,0.25733129142601346,-153661.49643124585,4704.8773554511317,15.225370986598282,6.9852598166393531E-3,0.29984634885733474,-153660.60083807475,4668.7714021921602]
["Goldline BH","BH-122-A",0.7,1,0.6,0.85,6000,2.52,9000,34.9,120,42.6,0.03,670,4,3679.8177380343545,7987.7819947008447,9000,0.56687030008831929,3750,14.16629207734414,11.546395847619047,"NA",-22.514713007407408,9,29.096917535999999,9,-2350.8283199999996,7.5,2362.8283199999996,9,0.58995037119263005,0.8659796885714286,14.15880890862312,41.567025051428573,31.134421524369106,23.025020459775291,2.4078840335924601,147.50519228007144,7.9544435058296684E-3,9.2703931835218292,-141824.94279999999,3679.8177380343545,2.1340425197844529E-3,2.1140377256828193,-153048.33243161489,7987.7819947008447,0.8209507042253521,0.46103665322014875,80.174535853446301,731846.50818228663,-9999]
["Goldline BH","BH-124-B",1.3,1.8,1.2,1.6,6000,4.6619999999999999,9000,12.4,58,44.9,4.5999999999999999E-2,670,4,4292.8802237991204,7866.6685785564896,8730.5122494432071,1.1688888570240583,2445.6521739130435,7.6263581393307156,6.2419994755898758,0.22710811496790889,-22.518767352098767,9,29.100201555200002,9,-2351.1634240000003,7.5,2363.1634240000003,9,0.57181416983781996,0.83942889101538476,13.72354007610768,40.292586768738467,30.179334099619286,23.02566948564203,2.4084458155501531,147.53960662666495,6.6274580635321944E-3,6.2248669819393676,-148858.84415468687,4292.8802237991204,2.2867767784231804E-3,1.5083742281596477,-153381.85943371113,7866.6685785564896,1.5641573867854492,0.10281444369320719,29.103036665919259,-48631.442723766129,560.631461766602]
["Goldline BH","BH-126-B",1.9,2.6,1.7,2.2999999999999998,6000,6.66,9000,8.1999999999999993,38,44.9,7.5999999999999998E-2,670,4,{"$f":"IF(AQ284<I284,IF(AQ284<0,0,AQ284),I284)","v":4543.4573904149847},{"$f":"IF(AU284<I284,IF(AU284<0,0,AU284),I284)","v":7935.9498989104277},{"$f":"IF(UAC_V*0.98/L284*1000<I284,IF(UAC_V*0.98/L284*1000<0,0,UAC_V*0.98/L284*1000),I284)","v":8730.5122494432071},{"$f":"C284+(E284-C284)/G284*Q284","v":1.6354683367029856},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M284,(inertia/gear^2+gear_inertia)/M284),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M284,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M284))","v":1480.2631578947369},{"$f":"IF((C284+(E284-C284)/G284*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X284^2*time1+Y284^2*time2+Z284^2*time3+AA284^2*time4)/time)/(C284+(E284-C284)/G284*mspeed),SQRT((((X284-Y284)*2/PI()+Y284)^2*time1+Y284^2*time2+((Z284-Y284)*2/PI()+Y284)^2*time3+AA284^2*time4)/time)/(C284+(E284-C284)/G284*mspeed)),IF(AccType=1,SQRT((X284^2*time1+Y284^2*time2+Z284^2*time3+AA284^2*time4+AB284^2*time5+AC284^2*time6+AD284^2*time7+AE284^2*time8)/time)/(C284+(E284-C284)/G284*mspeed),SQRT((((X284-Y284)*2/PI()+Y284)^2*time1+Y284^2*time2+((Z284-Y284)*2/PI()+Y284)^2*time3+AA284^2*time4+((AB284-AC284)*2/PI()+AC284)^2*time5+AC284^2*time6+((AD284-AC284)*2/PI()+AC284)^2*time7+AE284^2*time8)/time)/(C284+(E284-C284)/G284*mspeed))))","v":5.2188573890519043},{"$f":"IF(move1,MAX(ABS(X284),ABS(Z284))/H284,MAX(ABS(X284),ABS(Z284),ABS(AB284),ABS(AD284))/H284)","v":4.370324187867868},{"$f":"IF(AZ284>0,speed/(MIN(AZ284,I284)),\"NA\")","v":9.3136504285141059E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M284+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M284+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.526369248395056},{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M284+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M284+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.106359091200002},{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M284+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M284+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2351.7917440000001},{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M284+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M284+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2363.7917440000001},{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},{"$f":"AH284/Irms","v":0.5651561570422351},{"$f":"AI284/Ipeak","v":0.82978655303859661},13.563747769013641,{"$f":"IF(move1,MAX(ABS(X284),ABS(Z284))/(C284/D284),MAX(ABS(X284),ABS(Z284),ABS(AB284),ABS(AD284))/(C284/D284))","v":39.829754545852637},29.831723654857658,{"$f":"IF((C284+(E284-C284)/G284*mspeed)<0,\"NA\",U284*(C284+(E284-C284)/G284*mspeed)*mspeed/9.55)","v":23.026886608528979},{"$f":"IF(move1,IF(speed1>speed2,AM284/2*time1/time,AM284/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z284*-speed/30*PI(),((Z284-AA284)*2/PI()+AA284)*-speed/30*PI()),IF(AccType=1,X284*-speed/30*PI(),((X284-Y284)*2/PI()+Y284)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z284*-speed/30*PI(),((Z284-AA284)*2/PI()+AA284)*-speed/30*PI()),IF(AccType=1,X284*-speed/30*PI(),((X284-Y284)*2/PI()+Y284)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD284*-speed/30*PI(),((AD284-AE284)*2/PI()+AE284)*-speed/30*PI()),IF(AccType=1,AB284*-speed/30*PI(),((AB284-AC284)*2/PI()+AC284)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD284*-speed/30*PI(),((AD284-AE284)*2/PI()+AE284)*-speed/30*PI()),IF(AccType=1,AB284*-speed/30*PI(),((AB284-AC284)*2/PI()+AC284)*-speed/30*PI()),0)/2*time7/time)))","v":2.4094991567208273},{"$f":"IF(move1,MAX(IF(AccType=1,Z284*-speed/30*PI(),((Z284-AA284)*2/PI()+AA284)*-speed/30*PI()),IF(AccType=1,X284*-speed/30*PI(),((X284-Y284)*2/PI()+Y284)*-speed/30*PI()),0),MAX(IF(AccType=1,Z284*-speed/30*PI(),((Z284-AA284)*2/PI()+AA284)*-speed/30*PI()),IF(AccType=1,X284*-speed/30*PI(),((X284-Y284)*2/PI()+Y284)*-speed/30*PI()),IF(AccType=1,AD284*-speed/30*PI(),((AD284-AE284)*2/PI()+AE284)*-speed/30*PI()),IF(AccType=1,AB284*-speed/30*PI(),((AB284-AC284)*2/PI()+AC284)*-speed/30*PI()),0))","v":147.6041335265277},{"$f":"(L284^2)/1000000+((K284/1000)^2*(D284/C284*H284)^2*PI()*PI()*(O284/2)^2)/1200","v":5.961796987756271E-3},{"$f":"SQRT(3)*L284*J284*D284/C284*H284/1000","v":5.811855353148716},{"$f":"0.75*J284^2*(D284/C284*H284)^2-(UAC_V*0.98)^2","v":-149475.3225323878},{"$f":"-AO284/2/AN284+SQRT((AO284/2/AN284)^2-AP284/AN284)","v":4543.4573904149847},{"$f":"(L284^2)/1000000+((K284/1000)^2*AV284^2*PI()*PI()*(O284/2)^2)/1200","v":2.2554660235748385E-3},{"$f":"SQRT(3)*L284*J284*AV284/1000","v":1.431729132403863},{"$f":"0.75*J284^2*AV284^2-(UAC_V*0.98)^2","v":-153409.80380199332},{"$f":"-AS284/2/AR284+SQRT((AS284/2/AR284)^2-AT284/AR284)","v":7935.9498989104277},{"$f":"D284+(F284-D284)*((0.85*UAC_V-D284*J284)/L284*1000)/G284","v":2.2451224944320711},4.429283638863326E-2,19.023883076493501,-108784.74254243579,{"$f":"IF(((AX284/2/AW284)^2-AY284/AW284)>0,-AX284/2/AW284+SQRT((AX284/2/AW284)^2-AY284/AW284),-9999)","v":1367.0682129501981}]
["Goldline BH","BH-222-B",2.1,1.3,2,1.2,3000,7.452,6000,35.4,272,98,0.1,670,4,1266.8604277454724,3144.6878665151944,4000,1.9951770711161603,1125,4.7218479502140775,3.906506323134729,"NA",-22.532450765432099,9,29.111285120000002,9,-2352.2943999999998,7.5,2364.2943999999998,9,0.2556766935484166,0.37544316126984129,6.1362406451619984,18.021271740952383,13.497244896022908,23.027860494065653,2.4103418296573671,147.65575504641797,6.1401655913551671E-2,27.719594246423824,-133662.54474212899,1266.8604277454724,1.31089652361459E-2,7.2106376703405957,-152310.57185514018,3144.6878665151944,1.2000068027210884,0.45301509363068987,81.102658978588806,17557.399765651615,-9999]
["Goldline BH","BH-224-B",3.8,2.2000000000000002,3.5,2,3000,13.6,6000,12.5,152,103,0.17,670,4,1447.6210908319472,3191.7229333414207,3805.8252427184466,3.4808277066658579,661.76470588235293,2.6103692638316383,2.1415921105882352,0.1398091934862937,-22.550188523456789,9,29.125652704,9,-2353.7604799999999,7.5,2365.7604799999999,9,0.23914414531820571,0.35129624971929824,5.7394594876369371,16.862219986526316,12.628224888150752,23.030701943922061,2.412799625722275,147.80631781276455,5.7730776135057928E-2,17.558437160307445,-146398.97229916896,1447.6210908319472,1.3642480877959256E-2,4.454979014634449,-153196.31129180806,3191.7229333414207,1.9977346278317152,0.13182230177228718,28.161136161441739,-134975.8675204246,910.69801132926614]
["Goldline BH","BH-226-C",5.5,4.4000000000000004,4.8,3.8,4000,20,6000,3.9,44,75.400000000000006,0.25,670,4,2439.4653177320884,4685.1707783726615,5198.9389920424401,4.6800951137847839,450,1.804002645463376,1.4571036400000001,5.5954456829284738E-2,-22.57046024691358,9,29.142072800000001,9,-2355.4360000000001,7.5,2367.4360000000001,9,0.33050034751962609,0.48570121333333338,7.9320083404710262,23.313658240000002,17.4582734407578,23.033951047860679,2.4156085355107395,147.97838954573197,2.1990272849501009E-2,8.1492297675792642,-150743.67999999999,2439.4653177320884,6.5845302915314673E-3,1.9139206456957087,-153502.91868311446,4685.1707783726615,3.7577453580901854,2.5097881601879174E-2,8.8919676008726203,-150187.09311369565,2275.4926361268699]
["Goldline BH","BH-226-E",5.6,3,3.9,2.6,2500,21.39,6000,8.5,92,112,0.25,670,4,1545.8007910254453,3124.7440639592446,3500,3.4751740365077133,450,1.7753203101704864,1.3624157456755492,8.3750991461479768E-2,-22.57046024691358,9,29.142072800000001,9,-2355.4360000000001,7.5,2367.4360000000001,9,0.22131719699974964,0.32524634821428577,5.3116127279939915,15.611824714285717,11.690808107650314,23.033951047860679,2.4156085355107395,147.97838954573197,4.9107029253663552E-2,18.894769054688123,-146548.79955297353,1545.8007910254453,1.4355664500341595E-2,4.2059043350033534,-153311.44835628188,3124.7440639592446,2.5507142857142857,5.0601758815641155E-2,19.277118090037057,-146257.92375125093,1520.2680261054263]
["Goldline BH","BH-422-D",5.8,4,5.2,3.4,3600,20.88,6000,6.1,89,87.4,0.32,670,4,1444.3939646691883,3650.3830832500407,4485.1258581235697,5.1916028194583266,351.5625,1.7107863362953923,1.3963812444444446,9.1894763293723564E-2,-22.58819800493827,9,29.156440384,9,-2356.9020800000003,7.5,2368.9020800000003,9,0.28494927696359323,0.41891437333333337,{"$f":"IF(move1,IF(AccType=1,SQRT((X289^2*time1+Y289^2*time2+Z289^2*time3+AA289^2*time4)/time)/(C289/D289),SQRT((((X289-Y289)*2/PI()+Y289)^2*time1+Y289^2*time2+((Z289-AA289)*2/PI()+AA289)^2*time3+AA289^2*time4)/time)/(C289/D289)),IF(AccType=1,SQRT((X289^2*time1+Y289^2*time2+Z289^2*time3+AA289^2*time4+AB289^2*time5+AC289^2*time6+AD289^2*time7+AE289^2*time8)/time)/(C289/D289),SQRT((((X289-Y289)*2/PI()+Y289)^2*time1+Y289^2*time2+((Z289-AA289)*2/PI()+AA289)^2*time3+AA289^2*time4+((AB289-AC289)*2/PI()+AC289)^2*time5+AC289^2*time6+((AD289-AE289)*2/PI()+AE289)^2*time7+AE289^2*time8)/time)/(C289/D289)))","v":6.8387826471262372},20.107889920000002,15.056543785519175,23.036795529308819,2.4180663315756465,148.1289523120785,6.1674796721863108E-2,13.297328172680706,-147877.10080000001,1444.3939646691883,1.0647942568065538E-2,3.1379564480725346,-153341.73661333777,3650.3830832500407,3.3981693363844392,6.6714488629146307E-2,13.903597490443383,-147337.38340331861,1385.5409156074568]
["Goldline BH","BH-424-B",11.3,4.2,10.8,4,2000,37.659999999999997,6000,6.3,134,162,0.7,670,4,936.95691598952237,1973.9475312780614,2419.7530864197533,10.806513117180485,160.71428571428572,0.87856329305876812,0.77627285820499214,8.9800200865309862E-2,-22.684488691358027,9,29.234435840000003,9,-2364.8608000000004,7.5,2376.8608000000004,9,0.15367311029002143,0.22637284389380533,3.688154646960514,10.865896506902656,8.1329996585379085,23.052261657986655,2.4314086530708581,148.94629304367405,0.14198584808355877,24.743854540325753,-147831.63510218717,936.95691598952237,3.5726197871974202E-2,7.0823380852309024,-153186.18113898879,1973.9475312780614,4.0064567901234565,6.5318155053464763E-2,14.376956060234464,-151695.0083680278,1417.8582369151688]
["Goldline BH","BH-424-D",11.1,6.3,10,5.6,3000,39.375,6000,3.3,60,106,0.66,670,4,1364.7919113855282,3092.2704027991622,3698.1132075471701,9.9661675189736414,170.45454545454544,0.8945466351852025,0.74225335344761911,5.924258726571182E-2,-22.67435282962963,9,29.226225792000001,9,-2364.02304,7.5,2376.02304,9,0.23464640025127961,0.34558037254054058,5.6315136060307109,16.587857881945947,12.416343795965545,23.050631684760187,2.4300041981766243,148.86025717719025,7.0386342865758539E-2,13.539997057450774,-149584.88998941405,1364.7919113855282,1.4946597273526176E-2,3.3912659341931102,-153408.11079039652,3092.2704027991622,5.5973364779874215,2.9494641012779432E-2,7.5227072569394586,-152404.85251705212,2149.1963864179224]
["Goldline BH","BH-426-B",15.8,8.1,14.4,7.2,2500,52.65,6000,2.1,48,118,1,670,4,1397.6058389804969,2855.098363351764,3322.0338983050847,14.201144916523013,112.5,0.6288591020370794,0.55642946248812919,5.1900025746032599E-2,-22.760507654320985,9,29.296011200000002,9,-2371.1439999999998,7.5,2383.1439999999998,9,0.21207305448207145,0.31289252468354428,5.0897533075697146,15.018841184810126,11.237900028096355,23.064501137139516,2.4419420647776025,149.591562042302,6.9146184205421249E-2,11.584791899217443,-151254.35831391529,1397.6058389804969,1.7760743527636853E-2,3.0536048116415753,-153496.58219000141,2855.098363351764,7.1146067796610168,2.3496630464942027E-2,4.8233313043587565,-153246.29451178527,2453.2541678603948]
["Goldline BH","BH-426-H",15.7,9.1,13,7.5,3000,51.034999999999997,6000,1.9,39.700000000000003,105,1,670,4,1549.7837503656101,3230.5565751911522,3733.3333333333335,12.792499082327963,112.5,0.63317220156414145,0.57403764475360053,4.7160408266192451E-2,-22.760507654320985,9,29.296011200000002,9,-2371.1439999999998,7.5,2383.1439999999998,9,0.23977246027704832,0.35376022016985137,5.7545390466491595,16.980490568152867,12.705710985607409,23.064501137139516,2.4419420647776025,149.591562042302,5.6396090971919492E-2,10.221470660891582,-151294.87386686014,1549.7837503656101,1.3911255247159303E-2,2.5780488542755582,-153513.2894354868,3230.5565751911522,7.4608380952380955,1.9395616569728248E-2,4.390383926184934,-153226.9144893582,2699.8060270141914]
["Goldline BH","BH-622-B",14.9,8.4,12.7,6.7,3000,66.728999999999999,6000,1.91,32,107,1.03,670,6,1068.5876973514869,3138.3029571228153,3663.5514018691588,12.598577831443269,109.22330097087378,0.66708332181088081,0.43912195201486615,5.1208776247373723E-2,-22.768109550617282,9,29.302168736000002,9,-2371.77232,7.5,2383.77232,9,0.23322422032141088,0.34415298851006715,5.5973812877138611,16.519343448483223,12.360268532211853,23.065726508941445,2.4429954059482766,149.65608894216481,0.11871849445291584,13.316356288955962,-149791.92940836717,1068.5876973514869,1.4835715394580361E-2,2.3661193136431873,-153541.75088203346,3138.3029571228153,6.6843451713395643,2.3029219131949892E-2,4.3752782578134912,-153245.9927540987,2486.3697944753399]
["Goldline BH","BH-624-D",25.8,12.4,23.7,11.1,2500,91.08,6000,1.01,23,125,2.0299999999999998,670,6,1243.9558126492584,2685.4793269830388,3136,23.544197365334245,55.418719211822662,0.38579549420877418,0.32397255090030747,4.6946957227210304E-2,-23.02150609382716,9,29.507419936000002,9,-2392.71632,7.5,2404.71632,9,0.19918369080065779,0.29545543217571063,4.7804085792157869,14.181860744434109,10.600283710954796,23.106720028697858,2.478106778304094,151.80698560425819,9.0660483117783408E-2,9.572315740883953,-152197.93234170921,1243.9558126492584,2.0395609186336372E-2,2.4136294363488267,-153570.79028710385,2685.4793269830388,11.03769984,2.002498969124937E-2,2.317979032704832,-153578.03157126304,2712.0810802988467]
["Goldline BH","BH-624-C",27.6,19,18.399999999999999,12.2,3600,91.76,6000,0.53,10,90,2.0299999999999998,670,6,1946.9340437426877,4037.0792731559864,4355.5555555555547,17.283019635268033,55.418719211822662,0.3611162452950491,0.32157170810810809,3.2693794898559822E-2,-23.02150609382716,9,29.507419936000002,9,-2392.71632,7.5,2404.71632,9,0.28529641547008661,0.42318914461352658,6.847113971282079,20.313078941449277,15.183085189077959,23.106720028697858,2.478106778304094,151.80698560425819,3.7636352085199179E-2,5.2188754231707986,-152823.36232461184,1946.9340437426877,9.1793799867779871E-3,0.99766717337742805,-153633.27963614708,4037.0792731559864,12.075543209876543,9.806400879646392E-3,1.2544086357412791,-153615.43391896845,3894.4379160806739]
["Goldline BH","BH-626-E",35.4,20,24.9,14.4,3000,133.19999999999999,6000,0.43,10.7,108,3.04,670,6,{"$f":"IF(AQ297<I297,IF(AQ297<0,0,AQ297),I297)","v":1550.8738139435254},3344.6895746593163,3629.6296296296296,23.693586488692389,37.006578947368418,0.28209565269393361,0.22308351087087092,3.7450177410612455E-2,-23.277436602469137,9,29.714723648000003,9,-2413.86976,7.5,2425.86976,9,0.23456405637095309,0.34974957212806029,5.629537352902874,16.787979462146893,12.5352557364108,23.148413725250013,2.5135692643834693,153.97939123297252,5.9658390536391909E-2,6.0531829050090504,-152878.65570812984,1550.8738139435254,1.3390252215722511E-2,1.147996808933637,-153635.75290052037,3344.6895746593163,14.2720987654321,1.2995664926235915E-2,1.0082913397026918,-153642.20963165039,3399.822464857958]
["Goldline BH","BH-822-D",34.700000000000003,18.100000000000001,30,15.1,3000,128.256,6000,0.58299999999999996,20.8,116,4.88,670,6,{"$f":"IF(AQ298<I298,IF(AQ298<0,0,AQ298),I298)","v":961.63347643145323},{"$f":"IF(AU298<I298,IF(AU298<0,0,AU298),I298)","v":2667.7240643100577},{"$f":"IF(UAC_V*0.98/L298*1000<I298,IF(UAC_V*0.98/L298*1000<0,0,UAC_V*0.98/L298*1000),I298)","v":3379.3103448275865},{"$f":"C298+(E298-C298)/G298*Q298","v":30.520565632580912},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M298,(inertia/gear^2+gear_inertia)/M298),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M298,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M298))","v":23.053278688524589},{"$f":"IF((C298+(E298-C298)/G298*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X298^2*time1+Y298^2*time2+Z298^2*time3+AA298^2*time4)/time)/(C298+(E298-C298)/G298*mspeed),SQRT((((X298-Y298)*2/PI()+Y298)^2*time1+Y298^2*time2+((Z298-Y298)*2/PI()+Y298)^2*time3+AA298^2*time4)/time)/(C298+(E298-C298)/G298*mspeed)),IF(AccType=1,SQRT((X298^2*time1+Y298^2*time2+Z298^2*time3+AA298^2*time4+AB298^2*time5+AC298^2*time6+AD298^2*time7+AE298^2*time8)/time)/(C298+(E298-C298)/G298*mspeed),SQRT((((X298-Y298)*2/PI()+Y298)^2*time1+Y298^2*time2+((Z298-Y298)*2/PI()+Y298)^2*time3+AA298^2*time4+((AB298-AC298)*2/PI()+AC298)^2*time5+AC298^2*time6+((AD298-AC298)*2/PI()+AC298)^2*time7+AE298^2*time8)/time)/(C298+(E298-C298)/G298*mspeed))))","v":0.28839543101039533},{"$f":"IF(move1,MAX(ABS(X298),ABS(Z298))/H298,MAX(ABS(X298),ABS(Z298),ABS(AB298),ABS(AD298))/H298)","v":0.23462750948103792},{"$f":"IF(AZ298>0,speed/(MIN(AZ298,I298)),\"NA\")","v":4.3958324175464691E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M298+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M298+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-23.743686241975308},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M298+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M298+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":30.092385856},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M298+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M298+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2452.40672},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M298+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M298+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2464.40672},9,{"$f":"AH298/Irms","v":0.2172803588935428},{"$f":"AI298/Ipeak","v":0.32701259845917385},{"$f":"IF(move1,IF(AccType=1,SQRT((X298^2*time1+Y298^2*time2+Z298^2*time3+AA298^2*time4)/time)/(C298/D298),SQRT((((X298-Y298)*2/PI()+Y298)^2*time1+Y298^2*time2+((Z298-AA298)*2/PI()+AA298)^2*time3+AA298^2*time4)/time)/(C298/D298)),IF(AccType=1,SQRT((X298^2*time1+Y298^2*time2+Z298^2*time3+AA298^2*time4+AB298^2*time5+AC298^2*time6+AD298^2*time7+AE298^2*time8)/time)/(C298/D298),SQRT((((X298-Y298)*2/PI()+Y298)^2*time1+Y298^2*time2+((Z298-AA298)*2/PI()+AA298)^2*time3+AA298^2*time4+((AB298-AC298)*2/PI()+AC298)^2*time5+AC298^2*time6+((AD298-AE298)*2/PI()+AE298)^2*time7+AE298^2*time8)/time)/(C298/D298)))","v":5.2147286134450272},{"$f":"IF(move1,MAX(ABS(X298),ABS(Z298))/(C298/D298),MAX(ABS(X298),ABS(Z298),ABS(AB298),ABS(AD298))/(C298/D298))","v":15.696604726040345},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X298),ABS(Z298))/(C298/D298),MAX(ABS((X298-Y298)*2/PI()+Y298),ABS((Z298-Y298)*2/PI()+Y298))/(C298/D298)),IF(AccType=1,MAX(ABS(X298),ABS(Z298),ABS(AB298),ABS(AD298))/(C298/D298),MAX(ABS((X298-Y298)*2/PI()+Y298),ABS((Z298-Y298)*2/PI()+Y298),ABS((AB298-AC298)*2/PI()+AC298),ABS((AD298-AC298)*2/PI()+AC298))/(C298/D298)))","v":11.698666307500865},{"$f":"IF((C298+(E298-C298)/G298*mspeed)<0,\"NA\",U298*(C298+(E298-C298)/G298*mspeed)*mspeed/9.55)","v":23.225115150678278},{"$f":"IF(move1,IF(speed1>speed2,AM298/2*time1/time,AM298/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z298*-speed/30*PI(),((Z298-AA298)*2/PI()+AA298)*-speed/30*PI()),IF(AccType=1,X298*-speed/30*PI(),((X298-Y298)*2/PI()+Y298)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z298*-speed/30*PI(),((Z298-AA298)*2/PI()+AA298)*-speed/30*PI()),IF(AccType=1,X298*-speed/30*PI(),((X298-Y298)*2/PI()+Y298)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD298*-speed/30*PI(),((AD298-AE298)*2/PI()+AE298)*-speed/30*PI()),IF(AccType=1,AB298*-speed/30*PI(),((AB298-AC298)*2/PI()+AC298)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD298*-speed/30*PI(),((AD298-AE298)*2/PI()+AE298)*-speed/30*PI()),IF(AccType=1,AB298*-speed/30*PI(),((AB298-AC298)*2/PI()+AC298)*-speed/30*PI()),0)/2*time7/time)))","v":2.5781741895181733},{"$f":"IF(move1,MAX(IF(AccType=1,Z298*-speed/30*PI(),((Z298-AA298)*2/PI()+AA298)*-speed/30*PI()),IF(AccType=1,X298*-speed/30*PI(),((X298-Y298)*2/PI()+Y298)*-speed/30*PI()),0),MAX(IF(AccType=1,Z298*-speed/30*PI(),((Z298-AA298)*2/PI()+AA298)*-speed/30*PI()),IF(AccType=1,X298*-speed/30*PI(),((X298-Y298)*2/PI()+Y298)*-speed/30*PI()),IF(AccType=1,AD298*-speed/30*PI(),((AD298-AE298)*2/PI()+AE298)*-speed/30*PI()),IF(AccType=1,AB298*-speed/30*PI(),((AB298-AC298)*2/PI()+AC298)*-speed/30*PI()),0))","v":157.93704109122439},{"$f":"(L298^2)/1000000+((K298/1000)^2*(D298/C298*H298)^2*PI()*PI()*(O298/2)^2)/1200","v":0.15678737304472865},{"$f":"SQRT(3)*L298*J298*D298/C298*H298/1000","v":7.8363524841025223},{"$f":"0.75*J298^2*(D298/C298*H298)^2-(UAC_V*0.98)^2","v":-152523.08850596202},{"$f":"-AO298/2/AN298+SQRT((AO298/2/AN298)^2-AP298/AN298)","v":961.63347643145323},{"$f":"(L298^2)/1000000+((K298/1000)^2*AV298^2*PI()*PI()*(O298/2)^2)/1200","v":2.0913494945306109E-2},{"$f":"SQRT(3)*L298*J298*AV298/1000","v":1.7874743391884498},{"$f":"0.75*J298^2*AV298^2-(UAC_V*0.98)^2","v":-153604.63866466153},{"$f":"-AS298/2/AR298+SQRT((AS298/2/AR298)^2-AT298/AR298)","v":2667.7240643100577},{"$f":"D298+(F298-D298)*((0.85*UAC_V-D298*J298)/L298*1000)/G298","v":15.259933620689655},{"$f":"(L298^2)/1000000+((K298/1000)^2*AJ298^2*PI()*PI()*(O298/2)^2)/1200","v":1.7838888126419636E-2},{"$f":"SQRT(3)*L298*J298*AJ298/1000","v":1.3703248223199833},{"$f":"0.75*J298^2*AJ298^2-(UAC_V*0.98)^2","v":-153629.1124011841},{"$f":"IF(((AX298/2/AW298)^2-AY298/AW298)>0,-AX298/2/AW298+SQRT((AX298/2/AW298)^2-AY298/AW298),-9999)","v":2896.4697099299806}]
["Goldline BH","BH-824-D",66,32,48.1,23,2500,245.44,6000,0.23300000000000001,11,126,8.4,670,6,1014.722757503444,2715.8217348228168,3111.1111111111113,46.55471637866863,13.392857142857142,0.15281627414753013,0.12554950325945244,4.255844823306678E-2,-24.635642074074077,9,30.814870080000006,9,-2526.1296000000002,7.5,2538.1296000000002,9,0.20326462586800739,0.31126131393939399,4.8783510208321772,14.940543069090912,11.097104302815984,23.374496690506977,2.7017662202106494,165.50819734179311,0.14271393101646412,6.051157801239528,-153087.39835702474,1014.722757503444,2.0409805482221398E-2,1.1440508960480944,-153643.38944865286,2715.8217348228168,22.498742857142858,1.6978975117628105E-2,0.56428273356372005,-153658.98590634609,2991.7433496691488]
["Goldline BH","BH-824-A",66,37,43.9,22.5,3000,246.6,6000,0.155,7.3,108,8.4,670,6,1304.2868113610537,3340.2722468358056,3629.6296296296296,41.393327781642896,13.392857142857142,0.15282691684030092,0.12495892165450125,3.6197193145643347E-2,-24.635642074074077,9,30.814870080000006,9,-2526.1296000000002,7.5,2538.1296000000002,9,0.23502472365988356,0.35989589424242435,5.6405933678372051,17.275002923636368,12.83102685013098,23.374496690506977,2.7017662202106494,165.50819734179311,8.7053081232037838E-2,4.0083620508901507,-153319.62915099846,1304.2868113610537,1.3580257783588932E-2,0.63905712676732973,-153655.24669900394,3340.2722468358056,22.040609567901235,1.2313425827747223E-2,0.37202959959242038,-153661.03347858854,3517.5090499756284]
["Goldline BH","BH-826-C",93,39.700000000000003,55.1,20.3,2500,339.3,6000,0.16700000000000001,9,141,12.6,670,6,1005.5424407615648,2587.4313258971633,2780.1418439716313,53.774541099399002,8.9285714285714288,0.10943068365104876,9.3359637842617152E-2,4.6653413577110954E-2,-25.699907555555555,9,31.67692512,9,-2614.0944,7.5,2626.0944,9,0.18036193303496847,0.28171458944086025,4.3286863928392432,13.522300293161292,10.00464712519652,23.557208676442674,2.8492339841050796,174.54196332258525,0.14566600268378169,5.9072809859540962,-153225.18946925437,1005.5424407615648,2.2614736317164579E-2,0.87086634724138545,-153654.46315332784,2587.4313258971633,21.352822865248228,2.0481135860090378E-2,0.40803553480223353,-153661.90638049316,2729.1455160739579]
["Goldline BH","BH-826-D",93,52,47.5,24,3000,360,6000,8.7999999999999995E-2,4.7,103,12.6,670,6,1392.4510280172392,3660.9714259977022,3805.8252427184466,37.475266705701515,8.9285714285714288,0.10943085832081144,8.7991458666666661E-2,3.3980310989436699E-2,-25.699907555555555,9,31.67692512,9,-2614.0944,7.5,2626.0944,9,0.23624233042363621,0.36899643956989242,5.6698159301672693,17.711829099354837,13.104323690433727,23.557208676442674,2.8492339841050796,174.54196332258525,7.6861537463285862E-2,3.160118876244479,-153428.67265265348,1392.4510280172392,1.1372289125801899E-2,0.339192858219107,-153661.28881621579,3660.9714259977022,21.605592233009709,1.0889792787871659E-2,0.20572882055949959,-153663.00263107719,3746.9920305643136]
["Goldline BH","BH-828-B",124,50,75.7,35,2500,437.5,6000,0.112,4.7,150,12.6,670,6,1411.0932958343328,2472.9892129630571,2613.3333333333335,76.221848405553743,8.9285714285714288,8.2059849137573693E-2,7.2404400274285713E-2,4.8992942261217171E-2,-25.699907555555555,9,31.67692512,9,-2614.0944,7.5,2626.0944,9,0.17036706520935307,0.26610320161290324,4.0888095650244738,12.772953677419356,9.4502334306012461,23.557208676442674,2.8492339841050796,174.54196332258525,7.3387308109770732E-2,5.1332957401738906,-153371.21416493237,1411.0932958343328,2.4693250693292756E-2,1.065701763443563,-153651.3808861266,2472.9892129630571,36.624000000000002,2.2646029903085989E-2,0.27498717867914652,-153663.1598005729,2598.8223731218109]
["Cart. DDR","C041A (240 V)",4.57,2.73,4.2344309430620841,2.5204946089655262,1750,12.3,1750,8.4700000000000006,34.4,102,0.58600000000000008,325,10,1750,1750,1750,4.2344309430620841,191.97952218430032,2.1728965404129359,2.3748810734308941,8.542394225094313E-2,-22.655601485432097,9,29.2110372032,9,-2362.4731839999999,7.5,2374.4731839999999,9,0.24693689199952171,0.36353998707483587,5.9264854079885207,17.449919379592121,13.062629390999115,23.047617449298862,2.4274059566222941,148.70109082419535,2.3540464906972931E-2,10.9950135234466,-150759.09990434512,2307.8809379936233,1.1756985319381446E-2,3.5286050799857045,-153364.81089459581,3464.7786311673785,2.3580816871468246,5.1922017140331234E-2,19.546761538537023,-144483.01464233876,1490.4949492905255]
["Cart. DDR","C041B (240 V)",4.51,4.6900000000000004,4.0107045659157627,4.1347469751708896,2500,12.2,2500,2.87,11.4,58.7,0.58600000000000008,325,10,2500,2500,2500,4.0107045659157627,191.97952218430032,2.2019179001149984,2.3943473117377052,5.0929581789406507E-2,-22.655601485432097,9,29.2110372032,9,-2362.4731839999999,7.5,2374.4731839999999,9,0.42986870749521611,0.63285183149948265,10.316848979885187,30.376887911975167,22.739476338791402,23.047617449298862,2.4274059566222941,148.70109082419535,7.7467992475345167E-3,3.7020029189874455,-152669.65448341324,4206.7952743082778,3.7645751299114905E-3,1.0080072458519986,-153590.27901757773,6254.9188737713575,3.4544827519469146,1.726317905107384E-2,6.6353079642570041,-150469.62443367421,2766.3915324823283]
["Cart. DDR","C042A (240 V)",8.26,4.68,7.4933892029854734,4.2097692151603781,1700,22.2,1700,3.7,18.3,108,0.88700000000000001,325,10,1700,1700,1700,7.4933892029854734,126.83201803833146,1.2031734137720995,1.318595397045045,7.4896443807950741E-2,-22.731873844938274,9,29.2728178144,9,-2368.7773280000001,7.5,2380.7773280000001,9,0.23433463965931403,0.3455326557995157,5.624031351823537,16.585567478376753,12.411675397014889,23.059887893349117,2.437974479701396,149.34851071948552,2.2558272844647256E-2,8.7057238524199949,-152039.56524788679,2410.324122846042,1.2686546378501385E-2,2.6671489537132569,-153511.52907361768,3375.0250166572023,3.8535514674554001,2.2271706754863417E-2,8.5904618969150892,-152082.29484734332,2427.390413838219]
["Cart. DDR","C042B (240 V)",8.4600000000000009,9.19,7.2612851236246332,7.8078334662630464,2500,22.8,2500,0.96,5,56.1,0.88700000000000001,325,10,2500,2500,2500,7.2612851236246332,126.83201803833146,1.1747839464714256,1.2838955181754386,5.0929581789406507E-2,-22.731873844938274,9,29.2728178144,9,-2368.7773280000001,7.5,2380.7773280000001,9,0.44927870460676522,0.66247339370157599,10.782688910562365,31.798722897675646,23.796317319870329,23.059887893349117,2.437974479701396,149.34851071948552,6.300460747672005E-3,2.3103337210129227,-153240.00208578,4751.7976586670457,3.327743050565738E-3,0.55280736908245443,-153639.72484936565,6712.2502134863544,5.9262381786572318,6.0580478921018754E-3,2.2197520880656487,-153272.59782692674,4850.1044325618705]
["Cart. DDR","C043A (240 V)",11.1,4.7300000000000004,10.259764251475941,4.3290144520995533,1250,30,1250,3.97,20.6,143,1.19,325,10,1250,1250,1250,10.259764251475941,94.537815126050418,0.89593373542602739,0.97783363093333331,0.10185916357881301,-22.808652997530864,9,29.335008928000001,9,-2375.12336,7.5,2387.12336,9,0.17633637539622996,0.26042528571591594,4.2320730095095191,12.500413714363965,9.3516228117454716,23.07226619376527,2.4486132255252078,150.00023240809975,3.470874574802256E-2,12.570327371767856,-151732.20467708181,1917.5773514850775,2.1851665244834506E-2,3.9424638092285607,-153473.97822769967,2561.5035713297457,4.0094106877251887,2.8079744496115368E-2,9.1954746880222249,-152630.24829162724,2173.4413354944099]
["Cart. DDR","C043B (240 V)",11.2,9.15,9.2284402202404596,7.5027969270247636,2500,30.2,2500,1.06,5.5,74.5,1.19,325,10,2500,2500,2500,9.2284402202404596,94.537815126050418,0.88812877758702491,0.97135791152317885,5.0929581789406507E-2,-22.808652997530864,9,29.335008928000001,9,-2375.12336,7.5,2387.12336,9,0.3380701443506135,0.49928447115178581,8.1136834644147235,23.965654615285718,17.928827598816991,23.07226619376527,2.4486132255252078,150.00023240809975,9.3364531782374194E-3,3.3746814147138804,-153151.02875317261,3873.4344258152259,5.791569916970757E-3,0.8519760873667539,-153631.30492980295,5077.3809365833813,6.2288036391581549,7.5495946700178708E-3,2.4523059761725987,-153393.12010266332,4348.0678567688465]
["Cart. DDR","C044A (240 V)",14.1,5,13.159840151655576,4.617487772510728,1050,38.1,1050,4.08,22.1,173,1.49,325,10,1050,1050,1050,13.159840151655576,75.503355704697981,0.70573116158435534,0.77156389207349085,0.12126090902239645,-22.884671960493826,9,29.396584288000003,9,-2381.4065599999999,7.5,2393.4065599999999,9,0.14682018246412712,0.2171733472813239,3.5236843791390511,10.424320669503548,7.7960527824477843,23.084547916500341,2.459146637231953,150.64550140672779,4.8260364377784776E-2,16.517440876152222,-151385.0577274785,1608.2324874620938,3.1809253214218999E-2,5.2899739788753166,-153430.24824837802,2114.656778431633,4.3269974791876065,3.6032691810862001E-2,9.5310701139650931,-152905.19334493871,1931.9642084603913]
["Cart. DDR","C044B (240 V)",14.4,9.5299999999999994,12.080970563998754,8.1080339355696331,2150,38.799999999999997,2100,1.08,6,90,1.49,325,10,2100,2100,2100,12.134901481115062,75.503355704697981,0.69120351330809937,0.75764392494845378,6.0630454511198223E-2,-22.884671960493826,9,29.396584288000003,9,-2381.4065599999999,7.5,2393.4065599999999,9,0.27400928303127986,0.40530880825324078,6.5762227927507171,19.454822796155558,14.549708340775778,23.084547916500341,2.459146637231953,150.64550140672779,1.2980735548661795E-2,4.323037734966813,-153087.18965253251,3271.6713492922986,8.473890715735042E-3,1.1965166006281676,-153619.81321063029,4187.7549928509288,7.1070903442646944,9.6670021203235004E-3,2.4495210727249415,-153478.81007760111,3859.8598025882629]
["Cart. DDR","C051A (240 V)",11.7,4.75,10.941902337567806,4.3943382881798412,1200,30,1200,4.13,24,151,2.74,325,10,1200,1200,1200,10.941902337567806,41.058394160583937,0.85221211765941685,0.98843827626666669,0.10610329539459688,-23.201417639506168,9,29.653148288000001,9,-2407.5865600000002,7.5,2419.5865600000002,9,0.16846492794285353,0.25080565236467239,4.043158270628485,12.038671313504276,8.9917916383296781,23.135999099230439,2.5030358526767236,153.33412223434448,4.0369674500952947E-2,13.155780805999616,-151766.33576799804,1782.8140780791962,2.4812488897283998E-2,4.4514956208034464,-153446.73087515862,2398.7306125963792,4.121149070710695,3.2376764588681821E-2,9.7125632716554318,-152629.68258732173,2026.3966959853915]
["Cart. DDR","C051B (240 V)",11.8,9.2899999999999991,10.161231101401743,7.8769233344199554,2450,30.5,2450,1.08,6.4,78,2.74,325,10,2450,2450,2450,10.161231101401743,41.058394160583937,0.84504046690670531,0.97223437009836067,5.1968961009598476E-2,-23.201417639506168,9,29.653148288000001,9,-2407.5865600000002,7.5,2419.5865600000002,9,0.32668971298648664,0.48636607979435026,7.8405531116756793,23.345571830128812,17.437017101605125,23.135999099230439,2.5030358526767236,153.33412223434448,1.0940076816301277E-2,3.5035839775074273,-153159.5990841779,3584.9380274134278,6.4791936517816133E-3,0.99948144813060569,-153622.95121773679,4792.7924061558142,6.8500817085498831,8.6447244192747741E-3,2.5441995942964915,-153398.01744018661,4067.8616768074908]
["Cart. DDR","C052A (240 V)",16.8,9.84,14.907226237277634,8.6168937787731981,1850,26.6,1850,1.1399999999999999,7,105,3.59,325,10,{"$f":"IF(AQ314<I314,IF(AQ314<0,0,AQ314),I314)","v":1850},{"$f":"IF(AU314<I314,IF(AU314<0,0,AU314),I314)","v":1850},{"$f":"IF(UAC_V*0.98/L314*1000<I314,IF(UAC_V*0.98/L314*1000<0,0,UAC_V*0.98/L314*1000),I314)","v":1850},{"$f":"C314+(E314-C314)/G314*Q314","v":14.907226237277634},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M314,(inertia/gear^2+gear_inertia)/M314),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M314,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M314))","v":31.337047353760447},{"$f":"IF((C314+(E314-C314)/G314*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X314^2*time1+Y314^2*time2+Z314^2*time3+AA314^2*time4)/time)/(C314+(E314-C314)/G314*mspeed),SQRT((((X314-Y314)*2/PI()+Y314)^2*time1+Y314^2*time2+((Z314-Y314)*2/PI()+Y314)^2*time3+AA314^2*time4)/time)/(C314+(E314-C314)/G314*mspeed)),IF(AccType=1,SQRT((X314^2*time1+Y314^2*time2+Z314^2*time3+AA314^2*time4+AB314^2*time5+AC314^2*time6+AD314^2*time7+AE314^2*time8)/time)/(C314+(E314-C314)/G314*mspeed),SQRT((((X314-Y314)*2/PI()+Y314)^2*time1+Y314^2*time2+((Z314-Y314)*2/PI()+Y314)^2*time3+AA314^2*time4+((AB314-AC314)*2/PI()+AC314)^2*time5+AC314^2*time6+((AD314-AC314)*2/PI()+AC314)^2*time7+AE314^2*time8)/time)/(C314+(E314-C314)/G314*mspeed))))","v":0.59450008284844003},{"$f":"IF(move1,MAX(ABS(X314),ABS(Z314))/H314,MAX(ABS(X314),ABS(Z314),ABS(AB314),ABS(AD314))/H314)","v":1.121338789774436},{"$f":"IF(AZ314>0,speed/(MIN(AZ314,I314)),\"NA\")","v":6.8823759174873655E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M314+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M314+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-23.416804701234568},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M314+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M314+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.827611808},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M314+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M314+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2425.3889599999998},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M314+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M314+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2437.3889599999998},9,{"$f":"AH314/Irms","v":0.24341570334980092},{"$f":"AI314/Ipeak","v":0.36396788218095238},{"$f":"IF(move1,IF(AccType=1,SQRT((X314^2*time1+Y314^2*time2+Z314^2*time3+AA314^2*time4)/time)/(C314/D314),SQRT((((X314-Y314)*2/PI()+Y314)^2*time1+Y314^2*time2+((Z314-AA314)*2/PI()+AA314)^2*time3+AA314^2*time4)/time)/(C314/D314)),IF(AccType=1,SQRT((X314^2*time1+Y314^2*time2+Z314^2*time3+AA314^2*time4+AB314^2*time5+AC314^2*time6+AD314^2*time7+AE314^2*time8)/time)/(C314/D314),SQRT((((X314-Y314)*2/PI()+Y314)^2*time1+Y314^2*time2+((Z314-AA314)*2/PI()+AA314)^2*time3+AA314^2*time4+((AB314-AC314)*2/PI()+AC314)^2*time5+AC314^2*time6+((AD314-AE314)*2/PI()+AE314)^2*time7+AE314^2*time8)/time)/(C314/D314)))","v":5.8419768803952223},{"$f":"IF(move1,MAX(ABS(X314),ABS(Z314))/(C314/D314),MAX(ABS(X314),ABS(Z314),ABS(AB314),ABS(AD314))/(C314/D314))","v":17.470458344685714},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X314),ABS(Z314))/(C314/D314),MAX(ABS((X314-Y314)*2/PI()+Y314),ABS((Z314-Y314)*2/PI()+Y314))/(C314/D314)),IF(AccType=1,MAX(ABS(X314),ABS(Z314),ABS(AB314),ABS(AD314))/(C314/D314),MAX(ABS((X314-Y314)*2/PI()+Y314),ABS((Z314-Y314)*2/PI()+Y314),ABS((AB314-AC314)*2/PI()+AC314),ABS((AD314-AC314)*2/PI()+AC314))/(C314/D314)))","v":13.03757212878488},{"$f":"IF((C314+(E314-C314)/G314*mspeed)<0,\"NA\",U314*(C314+(E314-C314)/G314*mspeed)*mspeed/9.55)","v":23.171240321946957},{"$f":"IF(move1,IF(speed1>speed2,AM314/2*time1/time,AM314/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z314*-speed/30*PI(),((Z314-AA314)*2/PI()+AA314)*-speed/30*PI()),IF(AccType=1,X314*-speed/30*PI(),((X314-Y314)*2/PI()+Y314)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z314*-speed/30*PI(),((Z314-AA314)*2/PI()+AA314)*-speed/30*PI()),IF(AccType=1,X314*-speed/30*PI(),((X314-Y314)*2/PI()+Y314)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD314*-speed/30*PI(),((AD314-AE314)*2/PI()+AE314)*-speed/30*PI()),IF(AccType=1,AB314*-speed/30*PI(),((AB314-AC314)*2/PI()+AC314)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD314*-speed/30*PI(),((AD314-AE314)*2/PI()+AE314)*-speed/30*PI()),IF(AccType=1,AB314*-speed/30*PI(),((AB314-AC314)*2/PI()+AC314)*-speed/30*PI()),0)/2*time7/time)))","v":2.532880519179169},{"$f":"IF(move1,MAX(IF(AccType=1,Z314*-speed/30*PI(),((Z314-AA314)*2/PI()+AA314)*-speed/30*PI()),IF(AccType=1,X314*-speed/30*PI(),((X314-Y314)*2/PI()+Y314)*-speed/30*PI()),0),MAX(IF(AccType=1,Z314*-speed/30*PI(),((Z314-AA314)*2/PI()+AA314)*-speed/30*PI()),IF(AccType=1,X314*-speed/30*PI(),((X314-Y314)*2/PI()+Y314)*-speed/30*PI()),IF(AccType=1,AD314*-speed/30*PI(),((AD314-AE314)*2/PI()+AE314)*-speed/30*PI()),IF(AccType=1,AB314*-speed/30*PI(),((AB314-AC314)*2/PI()+AC314)*-speed/30*PI()),0))","v":155.1623843971239},{"$f":"(L314^2)/1000000+((K314/1000)^2*(D314/C314*H314)^2*PI()*PI()*(O314/2)^2)/1200","v":1.3470622913447599E-2},{"$f":"SQRT(3)*L314*J314*D314/C314*H314/1000","v":3.2301465843561949},{"$f":"0.75*J314^2*(D314/C314*H314)^2-(UAC_V*0.98)^2","v":-153427.40483091999},{"$f":"-AO314/2/AN314+SQRT((AO314/2/AN314)^2-AP314/AN314)","v":3257.1076012502963},{"$f":"(L314^2)/1000000+((K314/1000)^2*AV314^2*PI()*PI()*(O314/2)^2)/1200","v":1.1633239450362001E-2},{"$f":"SQRT(3)*L314*J314*AV314/1000","v":1.6108858854794301},{"$f":"0.75*J314^2*AV314^2-(UAC_V*0.98)^2","v":-153605.15752072478},{"$f":"-AS314/2/AR314+SQRT((AS314/2/AR314)^2-AT314/AR314)","v":3565.1524602969794},{"$f":"D314+(F314-D314)*((0.85*UAC_V-D314*J314)/L314*1000)/G314","v":7.7698028372207002},{"$f":"(L314^2)/1000000+((K314/1000)^2*AJ314^2*PI()*PI()*(O314/2)^2)/1200","v":1.2737568833962362E-2},{"$f":"SQRT(3)*L314*J314*AJ314/1000","v":2.7030339589276005},{"$f":"0.75*J314^2*AJ314^2-(UAC_V*0.98)^2","v":-153498.32216364818},{"$f":"IF(((AX314/2/AW314)^2-AY314/AW314)>0,-AX314/2/AW314+SQRT((AX314/2/AW314)^2-AY314/AW314),-9999)","v":3366.9474478707548}]
["Cart. DDR","C052B (240 V)",16.5,13.5,13.819742018555456,11.055793614844365,2500,42.4,2500,0.61,3.7,75.400000000000006,3.59,325,10,{"$f":"IF(AQ315<I315,IF(AQ315<0,0,AQ315),I315)","v":2500},{"$f":"IF(AU315<I315,IF(AU315<0,0,AU315),I315)","v":2500},{"$f":"IF(UAC_V*0.98/L315*1000<I315,IF(UAC_V*0.98/L315*1000<0,0,UAC_V*0.98/L315*1000),I315)","v":2500},{"$f":"C315+(E315-C315)/G315*Q315","v":13.819742018555456},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M315,(inertia/gear^2+gear_inertia)/M315),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M315,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M315))","v":31.337047353760447},{"$f":"IF((C315+(E315-C315)/G315*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X315^2*time1+Y315^2*time2+Z315^2*time3+AA315^2*time4)/time)/(C315+(E315-C315)/G315*mspeed),SQRT((((X315-Y315)*2/PI()+Y315)^2*time1+Y315^2*time2+((Z315-Y315)*2/PI()+Y315)^2*time3+AA315^2*time4)/time)/(C315+(E315-C315)/G315*mspeed)),IF(AccType=1,SQRT((X315^2*time1+Y315^2*time2+Z315^2*time3+AA315^2*time4+AB315^2*time5+AC315^2*time6+AD315^2*time7+AE315^2*time8)/time)/(C315+(E315-C315)/G315*mspeed),SQRT((((X315-Y315)*2/PI()+Y315)^2*time1+Y315^2*time2+((Z315-Y315)*2/PI()+Y315)^2*time3+AA315^2*time4+((AB315-AC315)*2/PI()+AC315)^2*time5+AC315^2*time6+((AD315-AC315)*2/PI()+AC315)^2*time7+AE315^2*time8)/time)/(C315+(E315-C315)/G315*mspeed))))","v":0.60536399100903282},{"$f":"IF(move1,MAX(ABS(X315),ABS(Z315))/H315,MAX(ABS(X315),ABS(Z315),ABS(AB315),ABS(AD315))/H315)","v":0.70348141056603775},{"$f":"IF(AZ315>0,speed/(MIN(AZ315,I315)),\"NA\")","v":5.0929581789406507E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M315+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M315+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-23.416804701234568},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M315+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M315+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.827611808},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M315+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M315+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2425.3889599999998},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M315+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M315+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2437.3889599999998},9,{"$f":"AH315/Irms","v":0.34002637053298135},{"$f":"AI315/Ipeak","v":0.50842520127272717},{"$f":"IF(move1,IF(AccType=1,SQRT((X315^2*time1+Y315^2*time2+Z315^2*time3+AA315^2*time4)/time)/(C315/D315),SQRT((((X315-Y315)*2/PI()+Y315)^2*time1+Y315^2*time2+((Z315-AA315)*2/PI()+AA315)^2*time3+AA315^2*time4)/time)/(C315/D315)),IF(AccType=1,SQRT((X315^2*time1+Y315^2*time2+Z315^2*time3+AA315^2*time4+AB315^2*time5+AC315^2*time6+AD315^2*time7+AE315^2*time8)/time)/(C315/D315),SQRT((((X315-Y315)*2/PI()+Y315)^2*time1+Y315^2*time2+((Z315-AA315)*2/PI()+AA315)^2*time3+AA315^2*time4+((AB315-AC315)*2/PI()+AC315)^2*time5+AC315^2*time6+((AD315-AE315)*2/PI()+AE315)^2*time7+AE315^2*time8)/time)/(C315/D315)))","v":8.1606328927915524},{"$f":"IF(move1,MAX(ABS(X315),ABS(Z315))/(C315/D315),MAX(ABS(X315),ABS(Z315),ABS(AB315),ABS(AD315))/(C315/D315))","v":24.404409661090906},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X315),ABS(Z315))/(C315/D315),MAX(ABS((X315-Y315)*2/PI()+Y315),ABS((Z315-Y315)*2/PI()+Y315))/(C315/D315)),IF(AccType=1,MAX(ABS(X315),ABS(Z315),ABS(AB315),ABS(AD315))/(C315/D315),MAX(ABS((X315-Y315)*2/PI()+Y315),ABS((Z315-Y315)*2/PI()+Y315),ABS((AB315-AC315)*2/PI()+AC315),ABS((AD315-AC315)*2/PI()+AC315))/(C315/D315)))","v":18.212129581229433},{"$f":"IF((C315+(E315-C315)/G315*mspeed)<0,\"NA\",U315*(C315+(E315-C315)/G315*mspeed)*mspeed/9.55)","v":23.171240321946957},{"$f":"IF(move1,IF(speed1>speed2,AM315/2*time1/time,AM315/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z315*-speed/30*PI(),((Z315-AA315)*2/PI()+AA315)*-speed/30*PI()),IF(AccType=1,X315*-speed/30*PI(),((X315-Y315)*2/PI()+Y315)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z315*-speed/30*PI(),((Z315-AA315)*2/PI()+AA315)*-speed/30*PI()),IF(AccType=1,X315*-speed/30*PI(),((X315-Y315)*2/PI()+Y315)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD315*-speed/30*PI(),((AD315-AE315)*2/PI()+AE315)*-speed/30*PI()),IF(AccType=1,AB315*-speed/30*PI(),((AB315-AC315)*2/PI()+AC315)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD315*-speed/30*PI(),((AD315-AE315)*2/PI()+AE315)*-speed/30*PI()),IF(AccType=1,AB315*-speed/30*PI(),((AB315-AC315)*2/PI()+AC315)*-speed/30*PI()),0)/2*time7/time)))","v":2.532880519179169},{"$f":"IF(move1,MAX(IF(AccType=1,Z315*-speed/30*PI(),((Z315-AA315)*2/PI()+AA315)*-speed/30*PI()),IF(AccType=1,X315*-speed/30*PI(),((X315-Y315)*2/PI()+Y315)*-speed/30*PI()),0),MAX(IF(AccType=1,Z315*-speed/30*PI(),((Z315-AA315)*2/PI()+AA315)*-speed/30*PI()),IF(AccType=1,X315*-speed/30*PI(),((X315-Y315)*2/PI()+Y315)*-speed/30*PI()),IF(AccType=1,AD315*-speed/30*PI(),((AD315-AE315)*2/PI()+AE315)*-speed/30*PI()),IF(AccType=1,AB315*-speed/30*PI(),((AB315-AC315)*2/PI()+AC315)*-speed/30*PI()),0))","v":155.1623843971239},{"$f":"(L315^2)/1000000+((K315/1000)^2*(D315/C315*H315)^2*PI()*PI()*(O315/2)^2)/1200","v":9.0727693111543883E-3},{"$f":"SQRT(3)*L315*J315*D315/C315*H315/1000","v":2.7636146683829121},{"$f":"0.75*J315^2*(D315/C315*H315)^2-(UAC_V*0.98)^2","v":-153328.14463114049},{"$f":"-AO315/2/AN315+SQRT((AO315/2/AN315)^2-AP315/AN315)","v":3961.4563407684909},{"$f":"(L315^2)/1000000+((K315/1000)^2*AV315^2*PI()*PI()*(O315/2)^2)/1200","v":5.9233158341134452E-3},{"$f":"SQRT(3)*L315*J315*AV315/1000","v":0.73275947465867908},{"$f":"0.75*J315^2*AV315^2-(UAC_V*0.98)^2","v":-153640.388683533},{"$f":"-AS315/2/AR315+SQRT((AS315/2/AR315)^2-AT315/AR315)","v":5031.4816310456554},{"$f":"D315+(F315-D315)*((0.85*UAC_V-D315*J315)/L315*1000)/G315","v":9.1981319290654682},{"$f":"(L315^2)/1000000+((K315/1000)^2*AJ315^2*PI()*PI()*(O315/2)^2)/1200","v":6.6188085338285086E-3},{"$f":"SQRT(3)*L315*J315*AJ315/1000","v":1.4508500864385117},{"$f":"0.75*J315^2*AJ315^2-(UAC_V*0.98)^2","v":-153571.43593965171},{"$f":"IF(((AX315/2/AW315)^2-AY315/AW315)>0,-AX315/2/AW315+SQRT((AX315/2/AW315)^2-AY315/AW315),-9999)","v":4708.5204888421467}]
["Cart. DDR","C052C (240 V)",16.899999999999999,5.74,5.6263423125459218,1.8817198369718799,1850,43.1,950,3.36,90,181,3.59,325,10,604.78285397374259,950,950,11.110824430766824,31.337047353760447,0.59494333090600693,0.69205595842227374,0.13402521523528027,-23.416804701234568,9,29.827611808,9,-2425.3889599999998,7.5,2437.3889599999998,9,0.14115230135077217,0.21105829854280081,3.3876552324185321,10.130798330054439,7.5602489267509974,23.171240321946957,2.532880519179169,155.1623843971239,0.38966255715719988,15.419877996977307,-151849.55113212613,604.78285397374259,3.9723456330812569E-2,2.1537136387336004,-153628.60362597549,1939.6621105047789,2.0446052832810655,0.1279563461292898,7.9636941951139271,-153180.03716894102,1063.4567841809803]
["Cart. DDR","C052D (240 V)",16.5,10.9,14.207490041861877,9.4716600279079177,2050,42.3,2050,0.94,5.59,92.7,3.59,325,10,2050,2050,2050,14.207490041861877,31.337047353760447,0.60540164869623547,0.70514448718676126,6.2109246084642078E-2,-23.416804701234568,9,29.827611808,9,-2425.3889599999998,7.5,2437.3889599999998,9,0.27453981028218494,0.41050627362020203,6.5889554467724389,19.704301133769697,14.704608328548209,23.171240321946957,2.532880519179169,155.1623843971239,1.3610334648499825E-2,4.2174615920284708,-153146.53281687704,3203.0736888053234,9.0489716430969692E-3,1.2710362007956251,-153617.00015989997,4050.5839402503184,8.4215048851145706,9.9825676404507735E-3,2.2193289393136002,-153520.70735711016,3812.0063969903144]
["Cart. DDR","C053A (240 V)",20.9,9.2100000000000009,18.971269216553925,8.2483779202408378,1350,53.7,1350,1.41,9.1,139,4.43,325,10,1350,1350,1350,18.971269216553925,25.39503386004515,0.47867738158465845,0.55865964275605218,9.431404035075279E-2,-23.629657797530864,9,30.000022816000005,9,-2442.9819199999997,7.5,2454.9819199999997,9,0.18341385777129846,0.27541886975215318,4.4019325865111627,13.220105748103354,9.8573571267913405,23.206268217499687,2.5623740719580552,156.96913759328234,2.8855908992907277E-2,8.0330814429213415,-152829.02254711703,2166.3777227331402,2.0287530655556708E-2,2.5575946247498411,-153579.36035577158,2689.0762497097062,7.5342004442944059,2.0975482869540242E-2,3.3462241664692192,-153519.11598555636,2626.7716530936054]
["Cart. DDR","C053B (240 V)",20,18.2,16.123032354981365,14.525254373857084,2500,51.4,2500,0.36,2.2000000000000002,67.400000000000006,4.43,325,10,2500,2500,2500,16.123032354981365,25.39503386004515,0.50031992851525198,0.58365803143968886,5.0929581789406507E-2,-23.629657797530864,9,30.000022816000005,9,-2442.9819199999997,7.5,2454.9819199999997,9,0.37875658642261939,0.56875043255333335,9.0901580741428649,27.300020762560003,20.3558170678007,23.206268217499687,2.5623740719580552,156.96913759328234,6.7200330265574249E-3,1.9657466126983718,-153451.3451522128,4634.5662467703414,4.6616055930398638E-3,0.45926423991719467,-153652.39231865283,5692.1407615713933,10.92797282168485,4.9551241942868062E-3,0.85548335506343121,-153623.72427715801,5482.3799337804458]
["Cart. DDR","C054A (240 V)",24.8,9.7899999999999991,22.631832907667519,8.8061606644620696,1200,63.5,1200,1.35,9,156,5.28,325,10,1200,1200,1200,22.631832907667519,21.30681818181818,0.40406154874599515,0.47518876119685038,0.10610329539459688,-23.845044859259257,9,30.174486336000001,9,-2460.7843199999998,7.5,2472.7843199999998,9,0.16455702585422219,0.24815878799516125,3.9493686205013323,11.91162182376774,8.8741994520681686,23.241915855232889,2.5922187384604998,158.79739975606171,3.4801331736585325E-2,9.1437370939317208,-152805.10856300395,1968.1631515043666,2.5421344015349449E-2,2.9446313988792272,-153574.92564436159,2400.6470353163745,8.0725723210215854,2.5647601479369009E-2,3.2370408473677013,-153556.35665837108,2384.5754103584854]
["Cart. DDR","C054B (240 V)",24,17.399999999999999,18.692240124835369,13.447654766068611,2350,60.9,2300,0.43,2.7,84.3,5.28,325,10,2300,2300,2300,18.805171186009083,21.30681818181818,0.41772756284763252,0.49547596610837441,5.5358241075441857E-2,-23.845044859259257,9,30.174486336000001,9,-2460.7843199999998,7.5,2472.7843199999998,9,0.30222015575678401,0.45576047069999998,7.2532837381628159,21.876502593599998,16.298070086637967,23.241915855232889,2.5922187384604998,158.79739975606171,1.0028600499499269E-2,2.7721195570696691,-153393.66095643953,3775.1921854890793,7.28022841750258E-3,0.67594532718380962,-153647.92659085774,4547.8096952575806,10.766013313664988,7.504650706607819E-3,1.0232761186719046,-153627.16416349547,4456.8184499727513]
["Cart. DDR","C061A (240 V)",33.4,9.89,31.300472141406086,9.2060212180606129,900,85.7,900,1.36,18.100000000000001,206,9.41,325,10,900,900,900,31.300472141406086,11.955366631243358,0.30227445583759832,0.36198569185530921,0.14147106052612918,-24.891572582716048,9,31.022173792,9,-2547.2830400000003,7.5,2559.2830400000003,9,0.12436924734843124,0.19137306562055889,2.9848619363623499,9.1859071497868268,6.8163275456798891,23.417993836051828,2.7372287062900238,167.68060297050738,8.581474180151874E-2,12.313950481271291,-152770.69374790744,1264.4360860420074,4.7517412285890716E-2,4.2145493531427176,-153559.35756050242,1753.8768800001487,8.6852912748069357,4.5565799815879326E-2,3.307632172542498,-153599.5474680175,1800.0754007097357]
["Cart. DDR","C061B (240 V)",32.299999999999997,19.5,26.963295897353099,16.145686166079702,1950,83,1950,0.35,4.3,101,9.41,325,10,1950,1950,1950,26.963295897353099,11.955366631243358,0.31267205021723948,0.37376113002409639,6.5294335627444244E-2,-24.891572582716048,9,31.022173792,9,-2547.2830400000003,7.5,2559.2830400000003,9,0.25356848177642383,0.39017826944272449,6.0856435626341723,18.728556933250776,13.897373055628357,23.417993836051828,2.7372287062900238,167.68060297050738,1.9746875854117676E-2,3.0680344149528032,-153433.31587169555,2710.8710268927598,1.0927713548544058E-2,0.84651364797384321,-153646.43835515622,3711.1682604668435,13.825597808497612,1.0935278565124357E-2,0.85090830252147709,-153646.25554016029,3709.696514664372]
["Cart. DDR","C062A (240 V)",47.3,14.6,43.635259450226378,13.344116039824581,950,121.5,950,0.76,11.1,198,12.6,325,10,950,950,950,43.635259450226378,8.9285714285714288,0.21477016599794177,0.26071543308641976,0.13402521523528027,-25.699907555555555,9,31.67692512,9,-2614.0944,7.5,2626.0944,9,0.13041544814165446,0.20370115695560254,3.1299707553997069,9.7776555338689217,7.2341237220974612,23.557208676442674,2.8492339841050796,174.54196332258525,7.4836020663870462E-2,9.7747892578686457,-153054.70946181676,1366.2876361446313,4.3101883480203662E-2,3.2329694696252349,-153597.34805382404,1850.6154633100869,12.404012450624476,4.0529794856051522E-2,1.8854948127575697,-153641.32954106128,1923.8822577577139]
["Cart. DDR","C062B (240 V)",46,20.6,39.843616787833106,17.708274127925826,1450,117.8,1450,0.38,5.2,136,12.6,325,10,1450,1450,1450,39.843616787833106,8.9285714285714288,0.2208925020500212,0.26890428794567062,8.7809623774838808E-2,-25.699907555555555,9,31.67692512,9,-2614.0944,7.5,2626.0944,9,0.18921114407424847,0.29553652965217392,4.5410674577819634,14.185753423304348,10.495511423968619,23.557208676442674,2.8492339841050796,174.54196332258525,3.3969000998377616E-2,4.7221286133868929,-153362.6037705265,2056.43152952435,1.9871531226371902E-2,1.4079452327906761,-153637.20623677367,2745.3611623898669,15.729054937228078,1.9108452492800063E-2,0.939478267070053,-153652.07013118651,2811.198728289598]
["Cart. DDR","C062C (240 V)",48.4,11.8,44.745275429264296,10.808037543300555,700,124.2,700,1.19,17.8,250.4,12.6,325,10,700,700,700,44.745275429264296,8.9285714285714288,0.21001186343735956,0.25504770628019324,0.18189136353359467,-25.699907555555555,9,31.67692512,9,-2614.0944,7.5,2626.0944,9,0.10300871479930802,0.16089347297520662,2.4722091551833927,7.7228867028099177,5.7138766758908028,23.557208676442674,2.8492339841050796,174.54196332258525,0.12243325195315058,15.627883130453613,-152690.19574200801,1054.7499694901746,6.915681636596957E-2,5.1380283181998019,-153558.73976223258,1453.430254059966,9.9553052347053992,6.4827124483100906E-2,2.9489864424329797,-153629.32496473033,1516.8485360348061]
["Cart. DDR","C063A (240 V)",60.2,13.9,56.231715036410804,12.897182347800642,700,154.4,700,0.93,14.4,264,15.7,325,10,700,700,700,56.231715036410804,7.1656050955414017,0.16978353842179839,0.20928240829015543,0.18189136353359467,-26.485436839506171,9,32.31320384,9,-2679.0207999999998,7.5,2691.0207999999998,9,9.8127525487680223E-2,0.15543796143964564,2.3550606117043253,7.4610221491029902,5.5049648945637797,23.695127193068544,2.9580792384081125,181.20974297507473,0.12388544489239156,15.160485444035794,-152839.56129871577,1051.2246218803016,7.5964402012063365E-2,5.1562525105901766,-153568.6324754901,1388.2915503542124,12.125137565163417,7.0988089507566063E-2,2.3410034653839999,-153644.34213862725,1454.7827769621058]
["Cart. DDR","C063B (240 V)",59,19.8,52.313537816292559,17.437845938764188,1150,149,1150,0.47,7.1,181,15.7,325,10,1150,1150,1150,52.313537816292559,7.1656050955414017,0.17325362876378489,0.2168671398657718,0.11071648215088371,-26.485436839506171,9,32.31320384,9,-2679.0207999999998,7.5,2691.0207999999998,9,0.14262173549603135,0.22591858616949154,3.4229216519047525,10.844092136135593,8.0010949344278046,23.695127193068544,2.9580792384081125,181.20974297507473,5.8677365697970815E-2,7.3677775864762527,-153249.75633707928,1554.5233803459889,3.5430146883034461E-2,2.364480268879233,-153621.33671940785,2049.1799396670194,16.047176674867568,3.3424550609297103E-2,1.1789258313279118,-153653.39389734919,2126.5035934096095]
["Cart. DDR","C063C (240 V)",61.8,11.3,58.163897384492664,10.536937931973309,550,158.9,550,1.45,23.1,333.8,15.7,325,10,550,550,550,58.163897384492664,7.1656050955414017,0.16543495097433156,0.20335559370673378,0.23149809904275684,-26.485436839506171,9,32.31320384,9,-2679.0207999999998,7.5,2691.0207999999998,9,7.7707422979964788E-2,0.12309169477885655,1.8649781515191548,5.9084013493851142,4.35939491417657,23.695127193068544,2.9580792384081125,181.20974297507473,0.20404359640555086,24.357282183837658,-152332.85612228763,806.41549905629211,0.12229571439736486,8.34552960390827,-153507.73016698947,1086.7640831079855,9.9549467228909112,0.11350757843768923,3.6546111520346294,-153634.03255656452,1147.4188057799927]
["Cart. DDR","C091A (230 V)",50,12.8,42.016904976260371,10.426031011478999,600,120,600,0.91600000000000004,7.8,244,28,325,38,600,600,600,42.016904976260371,4.0178571428571432,0.21015655767215982,0.29031494666666663,0.21220659078919377,-29.602214320987649,9,34.837793599999998,9,-2936.6320000000001,7.5,2948.6320000000001,9,0.11142178337810789,0.18580156586666666,2.6741228010745894,8.9184751616,6.5149056717088127,24.267031064205881,3.38994911838466,207.66577191882325,0.23000967725837071,11.89233511510654,-153070.1255606272,790.33603173025085,6.9634281983582666E-2,2.8944244685433196,-153628.82089406365,1464.6986600584273,7.476809122264144,6.7203100758586848E-2,2.5220521318772611,-153637.29033292501,1493.3585468509143]
["Cart. DDR","C092A (230 V)",101,15.3,89.524655489191119,13.165390513116341,400,227,400,0.92100000000000004,11,441,47,325,38,400,400,400,89.524655489191119,2.3936170212765959,0.10817930516215633,0.17065007224669607,0.31830988618379069,-34.41674864197531,9,38.737566400000006,9,-3334.5680000000002,7.5,3346.5680000000002,9,6.8529709384237511E-2,0.12225345831683171,1.6447130252217002,5.868165999207922,4.2312108723832456,25.222918645338218,4.057065193145184,248.53280849859757,0.61929899024442847,24.191052348087272,-152911.73240868273,477.75409202250847,0.24081251416041913,7.9889841228404643,-153581.95616626431,782.18701652510867,11.356191593662583,0.20091291670404904,2.9766208328788486,-153652.61036350243,867.13617652343339]
["Cart. DDR","C092C (230 V)",101.6,18.100000000000001,87.004702223569467,15.344744660241529,450,231.2,450,0.64,7.35,343,47,325,38,450,450,450,87.004702223569467,2.3936170212765959,0.10762500709041778,0.16755002768166094,0.28294212105225836,-34.41674864197531,9,38.737566400000006,9,-3334.5680000000002,7.5,3346.5680000000002,9,8.0592327804361971E-2,0.14377254589895019,1.9342158673046874,6.9010822031496089,4.9759897816657741,25.222918645338218,4.057065193145184,248.53280849859757,0.38975979599526256,15.660564698073852,-153142.84536489355,607.06193173119038,0.14166988362334881,4.6529568094022631,-153617.99449406675,1025.0230184852755,12.237544945499721,0.1216205436408845,1.8919698061360122,-153656.3935822928,1116.2630741455855]
["Cart. DDR","C093A (230 V)",145,15.5,132.09860276627313,15.450128978511476,300,309,300,0.86699999999999999,11,517,66,325,38,{"$f":"IF(AQ333<I333,IF(AQ333<0,0,AQ333),I333)","v":300},{"$f":"IF(AU333<I333,IF(AU333<0,0,AU333),I333)","v":300},{"$f":"IF(UAC_V*0.98/L333*1000<I333,IF(UAC_V*0.98/L333*1000<0,0,UAC_V*0.98/L333*1000),I333)","v":300},{"$f":"C333+(E333-C333)/G333*Q333","v":132.09860276627313},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M333,(inertia/gear^2+gear_inertia)/M333),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M333,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M333))","v":1.7045454545454546},{"$f":"IF((C333+(E333-C333)/G333*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X333^2*time1+Y333^2*time2+Z333^2*time3+AA333^2*time4)/time)/(C333+(E333-C333)/G333*mspeed),SQRT((((X333-Y333)*2/PI()+Y333)^2*time1+Y333^2*time2+((Z333-Y333)*2/PI()+Y333)^2*time3+AA333^2*time4)/time)/(C333+(E333-C333)/G333*mspeed)),IF(AccType=1,SQRT((X333^2*time1+Y333^2*time2+Z333^2*time3+AA333^2*time4+AB333^2*time5+AC333^2*time6+AD333^2*time7+AE333^2*time8)/time)/(C333+(E333-C333)/G333*mspeed),SQRT((((X333-Y333)*2/PI()+Y333)^2*time1+Y333^2*time2+((Z333-Y333)*2/PI()+Y333)^2*time3+AA333^2*time4+((AB333-AC333)*2/PI()+AC333)^2*time5+AC333^2*time6+((AD333-AC333)*2/PI()+AC333)^2*time7+AE333^2*time8)/time)/(C333+(E333-C333)/G333*mspeed))))","v":7.8467404345748185E-2},{"$f":"IF(move1,MAX(ABS(X333),ABS(Z333))/H333,MAX(ABS(X333),ABS(Z333),ABS(AB333),ABS(AD333))/H333)","v":0.13798491650485437},{"$f":"IF(AZ333>0,speed/(MIN(AZ333,I333)),\"NA\")","v":0.42441318157838753},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M333+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M333+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-39.231282962962965},{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M333+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M333+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":42.6373392},{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M333+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M333+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-3732.5039999999999},{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M333+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M333+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":3744.5039999999999},{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},{"$f":"AH333/Irms","v":5.0343411354240371E-2},{"$f":"AI333/Ipeak","v":9.495384448275862E-2},{"$f":"IF(move1,IF(AccType=1,SQRT((X333^2*time1+Y333^2*time2+Z333^2*time3+AA333^2*time4)/time)/(C333/D333),SQRT((((X333-Y333)*2/PI()+Y333)^2*time1+Y333^2*time2+((Z333-AA333)*2/PI()+AA333)^2*time3+AA333^2*time4)/time)/(C333/D333)),IF(AccType=1,SQRT((X333^2*time1+Y333^2*time2+Z333^2*time3+AA333^2*time4+AB333^2*time5+AC333^2*time6+AD333^2*time7+AE333^2*time8)/time)/(C333/D333),SQRT((((X333-Y333)*2/PI()+Y333)^2*time1+Y333^2*time2+((Z333-AA333)*2/PI()+AA333)^2*time3+AA333^2*time4+((AB333-AC333)*2/PI()+AC333)^2*time5+AC333^2*time6+((AD333-AE333)*2/PI()+AE333)^2*time7+AE333^2*time8)/time)/(C333/D333)))","v":1.208241872501769},{"$f":"IF(move1,MAX(ABS(X333),ABS(Z333))/(C333/D333),MAX(ABS(X333),ABS(Z333),ABS(AB333),ABS(AD333))/(C333/D333))","v":4.5577845351724138},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X333),ABS(Z333))/(C333/D333),MAX(ABS((X333-Y333)*2/PI()+Y333),ABS((Z333-Y333)*2/PI()+Y333))/(C333/D333)),IF(AccType=1,MAX(ABS(X333),ABS(Z333),ABS(AB333),ABS(AD333))/(C333/D333),MAX(ABS((X333-Y333)*2/PI()+Y333),ABS((Z333-Y333)*2/PI()+Y333),ABS((AB333-AC333)*2/PI()+AC333),ABS((AD333-AC333)*2/PI()+AC333))/(C333/D333)))","v":3.2511725929696853},{"$f":"IF((C333+(E333-C333)/G333*mspeed)<0,\"NA\",U333*(C333+(E333-C333)/G333*mspeed)*mspeed/9.55)","v":26.258230168105548},{"$f":"IF(move1,IF(speed1>speed2,AM333/2*time1/time,AM333/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z333*-speed/30*PI(),((Z333-AA333)*2/PI()+AA333)*-speed/30*PI()),IF(AccType=1,X333*-speed/30*PI(),((X333-Y333)*2/PI()+Y333)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z333*-speed/30*PI(),((Z333-AA333)*2/PI()+AA333)*-speed/30*PI()),IF(AccType=1,X333*-speed/30*PI(),((X333-Y333)*2/PI()+Y333)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD333*-speed/30*PI(),((AD333-AE333)*2/PI()+AE333)*-speed/30*PI()),IF(AccType=1,AB333*-speed/30*PI(),((AB333-AC333)*2/PI()+AC333)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD333*-speed/30*PI(),((AD333-AE333)*2/PI()+AE333)*-speed/30*PI()),IF(AccType=1,AB333*-speed/30*PI(),((AB333-AC333)*2/PI()+AC333)*-speed/30*PI()),0)/2*time7/time)))","v":4.7241812679057071},{"$f":"IF(move1,MAX(IF(AccType=1,Z333*-speed/30*PI(),((Z333-AA333)*2/PI()+AA333)*-speed/30*PI()),IF(AccType=1,X333*-speed/30*PI(),((X333-Y333)*2/PI()+Y333)*-speed/30*PI()),0),MAX(IF(AccType=1,Z333*-speed/30*PI(),((Z333-AA333)*2/PI()+AA333)*-speed/30*PI()),IF(AccType=1,X333*-speed/30*PI(),((X333-Y333)*2/PI()+Y333)*-speed/30*PI()),IF(AccType=1,AD333*-speed/30*PI(),((AD333-AE333)*2/PI()+AE333)*-speed/30*PI()),IF(AccType=1,AB333*-speed/30*PI(),((AB333-AC333)*2/PI()+AC333)*-speed/30*PI()),0))","v":289.39984507837187},{"$f":"(L333^2)/1000000+((K333/1000)^2*(D333/C333*H333)^2*PI()*PI()*(O333/2)^2)/1200","v":0.6592613406265776},{"$f":"SQRT(3)*L333*J333*D333/C333*H333/1000","v":25.644394149670696},{"$f":"0.75*J333^2*(D333/C333*H333)^2-(UAC_V*0.98)^2","v":-153048.90271643832},{"$f":"-AO333/2/AN333+SQRT((AO333/2/AN333)^2-AP333/AN333)","v":462.76469453408663},{"$f":"(L333^2)/1000000+((K333/1000)^2*AV333^2*PI()*PI()*(O333/2)^2)/1200","v":0.35243618455462389},{"$f":"SQRT(3)*L333*J333*AV333/1000","v":11.952255773689249},{"$f":"0.75*J333^2*AV333^2-(UAC_V*0.98)^2","v":-153530.38393454306},{"$f":"-AS333/2/AR333+SQRT((AS333/2/AR333)^2-AT333/AR333)","v":643.28089371615613},{"$f":"D333+(F333-D333)*((0.85*UAC_V-D333*J333)/L333*1000)/G333","v":15.394997062644586},{"$f":"(L333^2)/1000000+((K333/1000)^2*AJ333^2*PI()*PI()*(O333/2)^2)/1200","v":0.27108644176045077},{"$f":"SQRT(3)*L333*J333*AJ333/1000","v":2.5241217154806597},{"$f":"0.75*J333^2*AJ333^2-(UAC_V*0.98)^2","v":-153658.04091597992},{"$f":"IF(((AX333/2/AW333)^2-AY333/AW333)>0,-AX333/2/AW333+SQRT((AX333/2/AW333)^2-AY333/AW333),-9999)","v":748.23533825154016}]
["Cart. DDR","C093C (230 V)",139.4,20,128.50624833648465,18.227836643473001,350,316.60000000000002,350,0.59,7.54,426,66,325,38,{"$f":"IF(AQ334<I334,IF(AQ334<0,0,AQ334),I334)","v":350},{"$f":"IF(AU334<I334,IF(AU334<0,0,AU334),I334)","v":350},{"$f":"IF(UAC_V*0.98/L334*1000<I334,IF(UAC_V*0.98/L334*1000<0,0,UAC_V*0.98/L334*1000),I334)","v":350},{"$f":"C334+(E334-C334)/G334*Q334","v":128.50624833648465},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M334,(inertia/gear^2+gear_inertia)/M334),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M334,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M334))","v":1.7045454545454546},{"$f":"IF((C334+(E334-C334)/G334*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X334^2*time1+Y334^2*time2+Z334^2*time3+AA334^2*time4)/time)/(C334+(E334-C334)/G334*mspeed),SQRT((((X334-Y334)*2/PI()+Y334)^2*time1+Y334^2*time2+((Z334-Y334)*2/PI()+Y334)^2*time3+AA334^2*time4)/time)/(C334+(E334-C334)/G334*mspeed)),IF(AccType=1,SQRT((X334^2*time1+Y334^2*time2+Z334^2*time3+AA334^2*time4+AB334^2*time5+AC334^2*time6+AD334^2*time7+AE334^2*time8)/time)/(C334+(E334-C334)/G334*mspeed),SQRT((((X334-Y334)*2/PI()+Y334)^2*time1+Y334^2*time2+((Z334-Y334)*2/PI()+Y334)^2*time3+AA334^2*time4+((AB334-AC334)*2/PI()+AC334)^2*time5+AC334^2*time6+((AD334-AC334)*2/PI()+AC334)^2*time7+AE334^2*time8)/time)/(C334+(E334-C334)/G334*mspeed))))","v":8.1486206771454642E-2},{"$f":"IF(move1,MAX(ABS(X334),ABS(Z334))/H334,MAX(ABS(X334),ABS(Z334),ABS(AB334),ABS(AD334))/H334)","v":0.13467258117498421},{"$f":"IF(AZ334>0,speed/(MIN(AZ334,I334)),\"NA\")","v":0.36378272706718934},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M334+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M334+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-39.231282962962965},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M334+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M334+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":42.6373392},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M334+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M334+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-3732.5039999999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M334+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M334+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":3744.5039999999999},9,{"$f":"AH334/Irms","v":6.7568793875733363E-2},{"$f":"AI334/Ipeak","v":0.12744302725968434},{"$f":"IF(move1,IF(AccType=1,SQRT((X334^2*time1+Y334^2*time2+Z334^2*time3+AA334^2*time4)/time)/(C334/D334),SQRT((((X334-Y334)*2/PI()+Y334)^2*time1+Y334^2*time2+((Z334-AA334)*2/PI()+AA334)^2*time3+AA334^2*time4)/time)/(C334/D334)),IF(AccType=1,SQRT((X334^2*time1+Y334^2*time2+Z334^2*time3+AA334^2*time4+AB334^2*time5+AC334^2*time6+AD334^2*time7+AE334^2*time8)/time)/(C334/D334),SQRT((((X334-Y334)*2/PI()+Y334)^2*time1+Y334^2*time2+((Z334-AA334)*2/PI()+AA334)^2*time3+AA334^2*time4+((AB334-AC334)*2/PI()+AC334)^2*time5+AC334^2*time6+((AD334-AE334)*2/PI()+AE334)^2*time7+AE334^2*time8)/time)/(C334/D334)))","v":1.6216510530176007},{"$f":"IF(move1,MAX(ABS(X334),ABS(Z334))/(C334/D334),MAX(ABS(X334),ABS(Z334),ABS(AB334),ABS(AD334))/(C334/D334))","v":6.1172653084648489},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X334),ABS(Z334))/(C334/D334),MAX(ABS((X334-Y334)*2/PI()+Y334),ABS((Z334-Y334)*2/PI()+Y334))/(C334/D334)),IF(AccType=1,MAX(ABS(X334),ABS(Z334),ABS(AB334),ABS(AD334))/(C334/D334),MAX(ABS((X334-Y334)*2/PI()+Y334),ABS((Z334-Y334)*2/PI()+Y334),ABS((AB334-AC334)*2/PI()+AC334),ABS((AD334-AC334)*2/PI()+AC334))/(C334/D334)))","v":4.3635861154311506},{"$f":"IF((C334+(E334-C334)/G334*mspeed)<0,\"NA\",U334*(C334+(E334-C334)/G334*mspeed)*mspeed/9.55)","v":26.258230168105548},{"$f":"IF(move1,IF(speed1>speed2,AM334/2*time1/time,AM334/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z334*-speed/30*PI(),((Z334-AA334)*2/PI()+AA334)*-speed/30*PI()),IF(AccType=1,X334*-speed/30*PI(),((X334-Y334)*2/PI()+Y334)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z334*-speed/30*PI(),((Z334-AA334)*2/PI()+AA334)*-speed/30*PI()),IF(AccType=1,X334*-speed/30*PI(),((X334-Y334)*2/PI()+Y334)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD334*-speed/30*PI(),((AD334-AE334)*2/PI()+AE334)*-speed/30*PI()),IF(AccType=1,AB334*-speed/30*PI(),((AB334-AC334)*2/PI()+AC334)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD334*-speed/30*PI(),((AD334-AE334)*2/PI()+AE334)*-speed/30*PI()),IF(AccType=1,AB334*-speed/30*PI(),((AB334-AC334)*2/PI()+AC334)*-speed/30*PI()),0)/2*time7/time)))","v":4.7241812679057071},{"$f":"IF(move1,MAX(IF(AccType=1,Z334*-speed/30*PI(),((Z334-AA334)*2/PI()+AA334)*-speed/30*PI()),IF(AccType=1,X334*-speed/30*PI(),((X334-Y334)*2/PI()+Y334)*-speed/30*PI()),0),MAX(IF(AccType=1,Z334*-speed/30*PI(),((Z334-AA334)*2/PI()+AA334)*-speed/30*PI()),IF(AccType=1,X334*-speed/30*PI(),((X334-Y334)*2/PI()+Y334)*-speed/30*PI()),IF(AccType=1,AD334*-speed/30*PI(),((AD334-AE334)*2/PI()+AE334)*-speed/30*PI()),IF(AccType=1,AB334*-speed/30*PI(),((AB334-AC334)*2/PI()+AC334)*-speed/30*PI()),0))","v":289.39984507837187},{"$f":"(L334^2)/1000000+((K334/1000)^2*(D334/C334*H334)^2*PI()*PI()*(O334/2)^2)/1200","v":0.5297528901178814},{"$f":"SQRT(3)*L334*J334*D334/C334*H334/1000","v":19.774265937142449},{"$f":"0.75*J334^2*(D334/C334*H334)^2-(UAC_V*0.98)^2","v":-153125.33153508889},{"$f":"-AO334/2/AN334+SQRT((AO334/2/AN334)^2-AP334/AN334)","v":519.29434055471393},{"$f":"(L334^2)/1000000+((K334/1000)^2*AV334^2*PI()*PI()*(O334/2)^2)/1200","v":0.22522535482744502},{"$f":"SQRT(3)*L334*J334*AV334/1000","v":7.0084804793093642},{"$f":"0.75*J334^2*AV334^2-(UAC_V*0.98)^2","v":-153596.33430504741},{"$f":"-AS334/2/AR334+SQRT((AS334/2/AR334)^2-AT334/AR334)","v":810.40087179926252},{"$f":"D334+(F334-D334)*((0.85*UAC_V-D334*J334)/L334*1000)/G334","v":16.099101183017027},{"$f":"(L334^2)/1000000+((K334/1000)^2*AJ334^2*PI()*PI()*(O334/2)^2)/1200","v":0.1846900712154983},{"$f":"SQRT(3)*L334*J334*AJ334/1000","v":1.8996158706080886},{"$f":"0.75*J334^2*AJ334^2-(UAC_V*0.98)^2","v":-153659.02890126535},{"$f":"IF(((AX334/2/AW334)^2-AY334/AW334)>0,-AX334/2/AW334+SQRT((AX334/2/AW334)^2-AY334/AW334),-9999)","v":907.00289353048879}]
["Cart. DDR","C131A (230 V)",188,13.8,168.91644626819826,13.845610349852317,225,389,225,0.93,13,738,123,325,46,{"$f":"IF(AQ335<I335,IF(AQ335<0,0,AQ335),I335)","v":225},{"$f":"IF(AU335<I335,IF(AU335<0,0,AU335),I335)","v":225},{"$f":"IF(UAC_V*0.98/L335*1000<I335,IF(UAC_V*0.98/L335*1000<0,0,UAC_V*0.98/L335*1000),I335)","v":225},{"$f":"C335+(E335-C335)/G335*Q335","v":168.91644626819826},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M335,(inertia/gear^2+gear_inertia)/M335),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M335,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M335))","v":0.91463414634146345},{"$f":"IF((C335+(E335-C335)/G335*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X335^2*time1+Y335^2*time2+Z335^2*time3+AA335^2*time4)/time)/(C335+(E335-C335)/G335*mspeed),SQRT((((X335-Y335)*2/PI()+Y335)^2*time1+Y335^2*time2+((Z335-Y335)*2/PI()+Y335)^2*time3+AA335^2*time4)/time)/(C335+(E335-C335)/G335*mspeed)),IF(AccType=1,SQRT((X335^2*time1+Y335^2*time2+Z335^2*time3+AA335^2*time4+AB335^2*time5+AC335^2*time6+AD335^2*time7+AE335^2*time8)/time)/(C335+(E335-C335)/G335*mspeed),SQRT((((X335-Y335)*2/PI()+Y335)^2*time1+Y335^2*time2+((Z335-Y335)*2/PI()+Y335)^2*time3+AA335^2*time4+((AB335-AC335)*2/PI()+AC335)^2*time5+AC335^2*time6+((AD335-AC335)*2/PI()+AC335)^2*time7+AE335^2*time8)/time)/(C335+(E335-C335)/G335*mspeed))))","v":6.8816401503253799E-2},{"$f":"IF(move1,MAX(ABS(X335),ABS(Z335))/H335,MAX(ABS(X335),ABS(Z335),ABS(AB335),ABS(AD335))/H335)","v":0.13968292442159386},{"$f":"IF(AZ335>0,speed/(MIN(AZ335,I335)),\"NA\")","v":0.56588424210451671},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M335+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M335+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-53.674885925925928},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M335+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M335+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":54.336657600000009},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M335+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M335+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-4926.3119999999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M335+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M335+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":4938.3119999999999},9,{"$f":"AH335/Irms","v":3.9173374201033208E-2},{"$f":"AI335/Ipeak","v":8.3094622659574485E-2},{"$f":"IF(move1,IF(AccType=1,SQRT((X335^2*time1+Y335^2*time2+Z335^2*time3+AA335^2*time4)/time)/(C335/D335),SQRT((((X335-Y335)*2/PI()+Y335)^2*time1+Y335^2*time2+((Z335-AA335)*2/PI()+AA335)^2*time3+AA335^2*time4)/time)/(C335/D335)),IF(AccType=1,SQRT((X335^2*time1+Y335^2*time2+Z335^2*time3+AA335^2*time4+AB335^2*time5+AC335^2*time6+AD335^2*time7+AE335^2*time8)/time)/(C335/D335),SQRT((((X335-Y335)*2/PI()+Y335)^2*time1+Y335^2*time2+((Z335-AA335)*2/PI()+AA335)^2*time3+AA335^2*time4+((AB335-AC335)*2/PI()+AC335)^2*time5+AC335^2*time6+((AD335-AE335)*2/PI()+AE335)^2*time7+AE335^2*time8)/time)/(C335/D335)))","v":0.94016098082479693},{"$f":"IF(move1,MAX(ABS(X335),ABS(Z335))/(C335/D335),MAX(ABS(X335),ABS(Z335),ABS(AB335),ABS(AD335))/(C335/D335))","v":3.9885418876595753},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X335),ABS(Z335))/(C335/D335),MAX(ABS((X335-Y335)*2/PI()+Y335),ABS((Z335-Y335)*2/PI()+Y335))/(C335/D335)),IF(AccType=1,MAX(ABS(X335),ABS(Z335),ABS(AB335),ABS(AD335))/(C335/D335),MAX(ABS((X335-Y335)*2/PI()+Y335),ABS((Z335-Y335)*2/PI()+Y335),ABS((AB335-AC335)*2/PI()+AC335),ABS((AD335-AC335)*2/PI()+AC335))/(C335/D335)))","v":2.7792475236639471},{"$f":"IF((C335+(E335-C335)/G335*mspeed)<0,\"NA\",U335*(C335+(E335-C335)/G335*mspeed)*mspeed/9.55)","v":29.754746189450639},{"$f":"IF(move1,IF(speed1>speed2,AM335/2*time1/time,AM335/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z335*-speed/30*PI(),((Z335-AA335)*2/PI()+AA335)*-speed/30*PI()),IF(AccType=1,X335*-speed/30*PI(),((X335-Y335)*2/PI()+Y335)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z335*-speed/30*PI(),((Z335-AA335)*2/PI()+AA335)*-speed/30*PI()),IF(AccType=1,X335*-speed/30*PI(),((X335-Y335)*2/PI()+Y335)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD335*-speed/30*PI(),((AD335-AE335)*2/PI()+AE335)*-speed/30*PI()),IF(AccType=1,AB335*-speed/30*PI(),((AB335-AC335)*2/PI()+AC335)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD335*-speed/30*PI(),((AD335-AE335)*2/PI()+AE335)*-speed/30*PI()),IF(AccType=1,AB335*-speed/30*PI(),((AB335-AC335)*2/PI()+AC335)*-speed/30*PI()),0)/2*time7/time)))","v":6.7255294921872748},{"$f":"IF(move1,MAX(IF(AccType=1,Z335*-speed/30*PI(),((Z335-AA335)*2/PI()+AA335)*-speed/30*PI()),IF(AccType=1,X335*-speed/30*PI(),((X335-Y335)*2/PI()+Y335)*-speed/30*PI()),0),MAX(IF(AccType=1,Z335*-speed/30*PI(),((Z335-AA335)*2/PI()+AA335)*-speed/30*PI()),IF(AccType=1,X335*-speed/30*PI(),((X335-Y335)*2/PI()+Y335)*-speed/30*PI()),IF(AccType=1,AD335*-speed/30*PI(),((AD335-AE335)*2/PI()+AE335)*-speed/30*PI()),IF(AccType=1,AB335*-speed/30*PI(),((AB335-AC335)*2/PI()+AC335)*-speed/30*PI()),0))","v":412.00095481769455},{"$f":"(L335^2)/1000000+((K335/1000)^2*(D335/C335*H335)^2*PI()*PI()*(O335/2)^2)/1200","v":1.1441624499909331},{"$f":"SQRT(3)*L335*J335*D335/C335*H335/1000","v":33.944606318885967},{"$f":"0.75*J335^2*(D335/C335*H335)^2-(UAC_V*0.98)^2","v":-153135.10575984305},{"$f":"-AO335/2/AN335+SQRT((AO335/2/AN335)^2-AP335/AN335)","v":351.30876533023923},{"$f":"(L335^2)/1000000+((K335/1000)^2*AV335^2*PI()*PI()*(O335/2)^2)/1200","v":0.68650301915258527},{"$f":"SQRT(3)*L335*J335*AV335/1000","v":16.511935219191319},{"$f":"0.75*J335^2*AV335^2-(UAC_V*0.98)^2","v":-153538.852194882},{"$f":"-AS335/2/AR335+SQRT((AS335/2/AR335)^2-AT335/AR335)","v":461.04702374976051},{"$f":"D335+(F335-D335)*((0.85*UAC_V-D335*J335)/L335*1000)/G335","v":13.889865436433501},{"$f":"(L335^2)/1000000+((K335/1000)^2*AJ335^2*PI()*PI()*(O335/2)^2)/1200","v":0.55032356835476992},{"$f":"SQRT(3)*L335*J335*AJ335/1000","v":3.3039020629000668},{"$f":"0.75*J335^2*AJ335^2-(UAC_V*0.98)^2","v":-153658.98949366869},{"$f":"IF(((AX335/2/AW335)^2-AY335/AW335)>0,-AX335/2/AW335+SQRT((AX335/2/AW335)^2-AY335/AW335),-9999)","v":525.41540919679596}]
["Cart. DDR","C131B (230 V)",190,25.9,133.26573901561372,20.253151826081112,450,396,450,0.26100000000000001,3.6,398,123,325,46,{"$f":"IF(AQ336<I336,IF(AQ336<0,0,AQ336),I336)","v":450},{"$f":"IF(AU336<I336,IF(AU336<0,0,AU336),I336)","v":450},{"$f":"IF(UAC_V*0.98/L336*1000<I336,IF(UAC_V*0.98/L336*1000<0,0,UAC_V*0.98/L336*1000),I336)","v":450},{"$f":"C336+(E336-C336)/G336*Q336","v":133.26573901561372},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M336,(inertia/gear^2+gear_inertia)/M336),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M336,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M336))","v":0.91463414634146345},{"$f":"IF((C336+(E336-C336)/G336*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X336^2*time1+Y336^2*time2+Z336^2*time3+AA336^2*time4)/time)/(C336+(E336-C336)/G336*mspeed),SQRT((((X336-Y336)*2/PI()+Y336)^2*time1+Y336^2*time2+((Z336-Y336)*2/PI()+Y336)^2*time3+AA336^2*time4)/time)/(C336+(E336-C336)/G336*mspeed)),IF(AccType=1,SQRT((X336^2*time1+Y336^2*time2+Z336^2*time3+AA336^2*time4+AB336^2*time5+AC336^2*time6+AD336^2*time7+AE336^2*time8)/time)/(C336+(E336-C336)/G336*mspeed),SQRT((((X336-Y336)*2/PI()+Y336)^2*time1+Y336^2*time2+((Z336-Y336)*2/PI()+Y336)^2*time3+AA336^2*time4+((AB336-AC336)*2/PI()+AC336)^2*time5+AC336^2*time6+((AD336-AC336)*2/PI()+AC336)^2*time7+AE336^2*time8)/time)/(C336+(E336-C336)/G336*mspeed))))","v":6.8417699349267835E-2},{"$f":"IF(move1,MAX(ABS(X336),ABS(Z336))/H336,MAX(ABS(X336),ABS(Z336),ABS(AB336),ABS(AD336))/H336)","v":0.13721378181818183},{"$f":"IF(AZ336>0,speed/(MIN(AZ336,I336)),\"NA\")","v":0.28294212105225836},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M336+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M336+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-53.674885925925928},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M336+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M336+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":54.336657600000009},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M336+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M336+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-4926.3119999999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M336+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M336+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":4938.3119999999999},9,{"$f":"AH336/Irms","v":7.2747137169973636E-2},{"$f":"AI336/Ipeak","v":0.15431134121052634},{"$f":"IF(move1,IF(AccType=1,SQRT((X336^2*time1+Y336^2*time2+Z336^2*time3+AA336^2*time4)/time)/(C336/D336),SQRT((((X336-Y336)*2/PI()+Y336)^2*time1+Y336^2*time2+((Z336-AA336)*2/PI()+AA336)^2*time3+AA336^2*time4)/time)/(C336/D336)),IF(AccType=1,SQRT((X336^2*time1+Y336^2*time2+Z336^2*time3+AA336^2*time4+AB336^2*time5+AC336^2*time6+AD336^2*time7+AE336^2*time8)/time)/(C336/D336),SQRT((((X336-Y336)*2/PI()+Y336)^2*time1+Y336^2*time2+((Z336-AA336)*2/PI()+AA336)^2*time3+AA336^2*time4+((AB336-AC336)*2/PI()+AC336)^2*time5+AC336^2*time6+((AD336-AE336)*2/PI()+AE336)^2*time7+AE336^2*time8)/time)/(C336/D336)))","v":1.7459312920793673},{"$f":"IF(move1,MAX(ABS(X336),ABS(Z336))/(C336/D336),MAX(ABS(X336),ABS(Z336),ABS(AB336),ABS(AD336))/(C336/D336))","v":7.4069443781052637},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X336),ABS(Z336))/(C336/D336),MAX(ABS((X336-Y336)*2/PI()+Y336),ABS((Z336-Y336)*2/PI()+Y336))/(C336/D336)),IF(AccType=1,MAX(ABS(X336),ABS(Z336),ABS(AB336),ABS(AD336))/(C336/D336),MAX(ABS((X336-Y336)*2/PI()+Y336),ABS((Z336-Y336)*2/PI()+Y336),ABS((AB336-AC336)*2/PI()+AC336),ABS((AD336-AC336)*2/PI()+AC336))/(C336/D336)))","v":5.1612174074082722},{"$f":"IF((C336+(E336-C336)/G336*mspeed)<0,\"NA\",U336*(C336+(E336-C336)/G336*mspeed)*mspeed/9.55)","v":29.754746189450639},{"$f":"IF(move1,IF(speed1>speed2,AM336/2*time1/time,AM336/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z336*-speed/30*PI(),((Z336-AA336)*2/PI()+AA336)*-speed/30*PI()),IF(AccType=1,X336*-speed/30*PI(),((X336-Y336)*2/PI()+Y336)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z336*-speed/30*PI(),((Z336-AA336)*2/PI()+AA336)*-speed/30*PI()),IF(AccType=1,X336*-speed/30*PI(),((X336-Y336)*2/PI()+Y336)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD336*-speed/30*PI(),((AD336-AE336)*2/PI()+AE336)*-speed/30*PI()),IF(AccType=1,AB336*-speed/30*PI(),((AB336-AC336)*2/PI()+AC336)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD336*-speed/30*PI(),((AD336-AE336)*2/PI()+AE336)*-speed/30*PI()),IF(AccType=1,AB336*-speed/30*PI(),((AB336-AC336)*2/PI()+AC336)*-speed/30*PI()),0)/2*time7/time)))","v":6.7255294921872748},{"$f":"IF(move1,MAX(IF(AccType=1,Z336*-speed/30*PI(),((Z336-AA336)*2/PI()+AA336)*-speed/30*PI()),IF(AccType=1,X336*-speed/30*PI(),((X336-Y336)*2/PI()+Y336)*-speed/30*PI()),0),MAX(IF(AccType=1,Z336*-speed/30*PI(),((Z336-AA336)*2/PI()+AA336)*-speed/30*PI()),IF(AccType=1,X336*-speed/30*PI(),((X336-Y336)*2/PI()+Y336)*-speed/30*PI()),IF(AccType=1,AD336*-speed/30*PI(),((AD336-AE336)*2/PI()+AE336)*-speed/30*PI()),IF(AccType=1,AB336*-speed/30*PI(),((AB336-AC336)*2/PI()+AC336)*-speed/30*PI()),0))","v":412.00095481769455},{"$f":"(L336^2)/1000000+((K336/1000)^2*(D336/C336*H336)^2*PI()*PI()*(O336/2)^2)/1200","v":0.32271319617415239},{"$f":"SQRT(3)*L336*J336*D336/C336*H336/1000","v":9.7123775366621334},{"$f":"0.75*J336^2*(D336/C336*H336)^2-(UAC_V*0.98)^2","v":-153515.1239024667},{"$f":"-AO336/2/AN336+SQRT((AO336/2/AN336)^2-AP336/AN336)","v":674.82724549090801},{"$f":"(L336^2)/1000000+((K336/1000)^2*AV336^2*PI()*PI()*(O336/2)^2)/1200","v":0.17176505221289823},{"$f":"SQRT(3)*L336*J336*AV336/1000","v":2.769586610136519},{"$f":"0.75*J336^2*AV336^2-(UAC_V*0.98)^2","v":-153651.89391367792},{"$f":"-AS336/2/AR336+SQRT((AS336/2/AR336)^2-AT336/AR336)","v":937.77711607732897},{"$f":"D336+(F336-D336)*((0.85*UAC_V-D336*J336)/L336*1000)/G336","v":15.393264934888066},{"$f":"(L336^2)/1000000+((K336/1000)^2*AJ336^2*PI()*PI()*(O336/2)^2)/1200","v":0.15990604685269114},{"$f":"SQRT(3)*L336*J336*AJ336/1000","v":0.92861642309318282},{"$f":"0.75*J336^2*AJ336^2-(UAC_V*0.98)^2","v":-153662.63903616506},{"$f":"IF(((AX336/2/AW336)^2-AY336/AW336)>0,-AX336/2/AW336+SQRT((AX336/2/AW336)^2-AY336/AW336),-9999)","v":977.38418616172828}]
["Cart. DDR","C131C (230 V)",188.8,18.8,166.15776058793875,16.289976528229289,250,394.5,250,0.65,8.67,617,123,325,46,{"$f":"IF(AQ337<I337,IF(AQ337<0,0,AQ337),I337)","v":250},{"$f":"IF(AU337<I337,IF(AU337<0,0,AU337),I337)","v":250},{"$f":"IF(UAC_V*0.98/L337*1000<I337,IF(UAC_V*0.98/L337*1000<0,0,UAC_V*0.98/L337*1000),I337)","v":250},{"$f":"C337+(E337-C337)/G337*Q337","v":166.15776058793875},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M337,(inertia/gear^2+gear_inertia)/M337),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M337,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M337))","v":0.91463414634146345},{"$f":"IF((C337+(E337-C337)/G337*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X337^2*time1+Y337^2*time2+Z337^2*time3+AA337^2*time4)/time)/(C337+(E337-C337)/G337*mspeed),SQRT((((X337-Y337)*2/PI()+Y337)^2*time1+Y337^2*time2+((Z337-Y337)*2/PI()+Y337)^2*time3+AA337^2*time4)/time)/(C337+(E337-C337)/G337*mspeed)),IF(AccType=1,SQRT((X337^2*time1+Y337^2*time2+Z337^2*time3+AA337^2*time4+AB337^2*time5+AC337^2*time6+AD337^2*time7+AE337^2*time8)/time)/(C337+(E337-C337)/G337*mspeed),SQRT((((X337-Y337)*2/PI()+Y337)^2*time1+Y337^2*time2+((Z337-Y337)*2/PI()+Y337)^2*time3+AA337^2*time4+((AB337-AC337)*2/PI()+AC337)^2*time5+AC337^2*time6+((AD337-AC337)*2/PI()+AC337)^2*time7+AE337^2*time8)/time)/(C337+(E337-C337)/G337*mspeed))))","v":6.8568694093927407E-2},{"$f":"IF(move1,MAX(ABS(X337),ABS(Z337))/H337,MAX(ABS(X337),ABS(Z337),ABS(AB337),ABS(AD337))/H337)","v":0.13773550722433461},{"$f":"IF(AZ337>0,speed/(MIN(AZ337,I337)),\"NA\")","v":0.50929581789406508},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M337+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M337+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-53.674885925925928},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M337+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M337+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":54.336657600000009},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M337+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M337+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-4926.3119999999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M337+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M337+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":4938.3119999999999},9,{"$f":"AH337/Irms","v":5.3140495953133353E-2},{"$f":"AI337/Ipeak","v":0.11272170317796613},{"$f":"IF(move1,IF(AccType=1,SQRT((X337^2*time1+Y337^2*time2+Z337^2*time3+AA337^2*time4)/time)/(C337/D337),SQRT((((X337-Y337)*2/PI()+Y337)^2*time1+Y337^2*time2+((Z337-AA337)*2/PI()+AA337)^2*time3+AA337^2*time4)/time)/(C337/D337)),IF(AccType=1,SQRT((X337^2*time1+Y337^2*time2+Z337^2*time3+AA337^2*time4+AB337^2*time5+AC337^2*time6+AD337^2*time7+AE337^2*time8)/time)/(C337/D337),SQRT((((X337-Y337)*2/PI()+Y337)^2*time1+Y337^2*time2+((Z337-AA337)*2/PI()+AA337)^2*time3+AA337^2*time4+((AB337-AC337)*2/PI()+AC337)^2*time5+AC337^2*time6+((AD337-AE337)*2/PI()+AE337)^2*time7+AE337^2*time8)/time)/(C337/D337)))","v":1.2753719028752004},{"$f":"IF(move1,MAX(ABS(X337),ABS(Z337))/(C337/D337),MAX(ABS(X337),ABS(Z337),ABS(AB337),ABS(AD337))/(C337/D337))","v":5.4106417525423742},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X337),ABS(Z337))/(C337/D337),MAX(ABS((X337-Y337)*2/PI()+Y337),ABS((Z337-Y337)*2/PI()+Y337))/(C337/D337)),IF(AccType=1,MAX(ABS(X337),ABS(Z337),ABS(AB337),ABS(AD337))/(C337/D337),MAX(ABS((X337-Y337)*2/PI()+Y337),ABS((Z337-Y337)*2/PI()+Y337),ABS((AB337-AC337)*2/PI()+AC337),ABS((AD337-AC337)*2/PI()+AC337))/(C337/D337)))","v":3.7701779536807045},{"$f":"IF((C337+(E337-C337)/G337*mspeed)<0,\"NA\",U337*(C337+(E337-C337)/G337*mspeed)*mspeed/9.55)","v":29.754746189450639},{"$f":"IF(move1,IF(speed1>speed2,AM337/2*time1/time,AM337/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z337*-speed/30*PI(),((Z337-AA337)*2/PI()+AA337)*-speed/30*PI()),IF(AccType=1,X337*-speed/30*PI(),((X337-Y337)*2/PI()+Y337)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z337*-speed/30*PI(),((Z337-AA337)*2/PI()+AA337)*-speed/30*PI()),IF(AccType=1,X337*-speed/30*PI(),((X337-Y337)*2/PI()+Y337)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD337*-speed/30*PI(),((AD337-AE337)*2/PI()+AE337)*-speed/30*PI()),IF(AccType=1,AB337*-speed/30*PI(),((AB337-AC337)*2/PI()+AC337)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD337*-speed/30*PI(),((AD337-AE337)*2/PI()+AE337)*-speed/30*PI()),IF(AccType=1,AB337*-speed/30*PI(),((AB337-AC337)*2/PI()+AC337)*-speed/30*PI()),0)/2*time7/time)))","v":6.7255294921872748},{"$f":"IF(move1,MAX(IF(AccType=1,Z337*-speed/30*PI(),((Z337-AA337)*2/PI()+AA337)*-speed/30*PI()),IF(AccType=1,X337*-speed/30*PI(),((X337-Y337)*2/PI()+Y337)*-speed/30*PI()),0),MAX(IF(AccType=1,Z337*-speed/30*PI(),((Z337-AA337)*2/PI()+AA337)*-speed/30*PI()),IF(AccType=1,X337*-speed/30*PI(),((X337-Y337)*2/PI()+Y337)*-speed/30*PI()),IF(AccType=1,AD337*-speed/30*PI(),((AD337-AE337)*2/PI()+AE337)*-speed/30*PI()),IF(AccType=1,AB337*-speed/30*PI(),((AB337-AC337)*2/PI()+AC337)*-speed/30*PI()),0))","v":412.00095481769455},{"$f":"(L337^2)/1000000+((K337/1000)^2*(D337/C337*H337)^2*PI()*PI()*(O337/2)^2)/1200","v":0.88537133069084861},{"$f":"SQRT(3)*L337*J337*D337/C337*H337/1000","v":27.287391060309954},{"$f":"0.75*J337^2*(D337/C337*H337)^2-(UAC_V*0.98)^2","v":-153175.01705665368},{"$f":"-AO337/2/AN337+SQRT((AO337/2/AN337)^2-AP337/AN337)","v":400.81575750810538},{"$f":"(L337^2)/1000000+((K337/1000)^2*AV337^2*PI()*PI()*(O337/2)^2)/1200","v":0.43999570649843323},{"$f":"SQRT(3)*L337*J337*AV337/1000","v":9.3541615980887336},{"$f":"0.75*J337^2*AV337^2-(UAC_V*0.98)^2","v":-153606.53817472848},{"$f":"-AS337/2/AR337+SQRT((AS337/2/AR337)^2-AT337/AR337)","v":580.32039226172935},{"$f":"D337+(F337-D337)*((0.85*UAC_V-D337*J337)/L337*1000)/G337","v":13.466220463034013},{"$f":"(L337^2)/1000000+((K337/1000)^2*AJ337^2*PI()*PI()*(O337/2)^2)/1200","v":0.38533774865164938},{"$f":"SQRT(3)*L337*J337*AJ337/1000","v":2.6189125544982348},{"$f":"0.75*J337^2*AJ337^2-(UAC_V*0.98)^2","v":-153659.49586212885},{"$f":"IF(((AX337/2/AW337)^2-AY337/AW337)>0,-AX337/2/AW337+SQRT((AX337/2/AW337)^2-AY337/AW337),-9999)","v":628.0899562564091}]
["Cart. DDR","C132A (230 V)",361,12.4,340.30220559285254,12.988633801253915,110,836,110,1.66,29,1584,225,325,46,110,110,110,340.30220559285254,0.5,4.465754479826118E-2,9.512121212121212E-2,1.1574904952137843,-79.521333333333331,9,75.272279999999995,9,-7062.6,7.5,7074.6,9,2.28062511258194E-2,5.6905847953216376E-2,0.54735002701966562,2.7314807017543861,1.7583352443704143,37.019105869472448,10.306889472480607,631.39241435121937,5.5263087275935305,130.78099985935009,-151959.80627891413,154.41282082304116,3.1738555646029702,61.388097220364358,-153288.51032576227,210.30814389960318,13.479080889929525,2.5203688890981391,8.0080278328212096,-153657.61029508995,245.3300322509416]
["Cart. DDR","C132B (230 V)",361,26.3,307.27514346275262,24.981718980711594,225,742,225,0.36899999999999999,6.5,746,225,325,46,225,225,225,307.27514346275262,0.5,4.479852853176472E-2,0.10717160826594789,0.56588424210451671,-79.521333333333331,9,75.272279999999995,9,-7062.6,7.5,7074.6,9,4.8371322952342762E-2,0.1206954678362573,1.1609117508562263,5.7933824561403506,3.7293723328178952,37.019105869472448,10.306889472480607,631.39241435121937,1.0936786261416498,25.773789240834859,-153365.58620244925,362.87404551527618,0.65981907994071698,11.302695136124443,-153606.61130078015,474.00568799708049,23.705886060469645,0.55907265645054049,1.7781220419019768,-153662.57968234702,522.67604535960152]
["Cart. DDR","C132C (230 V)",361.7,16.899999999999999,337.40847935481816,15.548777850452449,120,818.3,120,1.1399999999999999,19.899999999999999,1313,225,325,46,120,120,120,337.40847935481816,0.5,4.4609605402484896E-2,9.7178703816856088E-2,1.0610329539459689,-79.521333333333331,9,75.272279999999995,9,-7062.6,7.5,7074.6,9,3.1022558682010485E-2,7.7407066936995048E-2,0.74454140836825167,3.7155392129757625,2.3918029315819251,37.019105869472448,10.306889472480607,631.39241435121937,4.2427001788958059,99.124486792586126,-152239.13912925732,178.10513725167536,2.068919688245455,36.683312927270059,-153468.85939026164,263.63577526868812,14.149410479100128,1.7338256903180382,6.2009124358346899,-153658.42401298444,295.91484782829423]
["Cart. DDR","C133A (230 V)",504,16.8,475.34276336779408,15.6362751107827,90,1016,90,1.41,26,1837,302,325,46,90,90,90,475.34276336779408,0.37251655629139074,3.7267136767123225E-2,9.7473294449304942E-2,1.4147106052612919,-99.032867160493822,9,91.076622400000005,9,-8675.2880000000005,7.5,8687.2880000000005,9,2.572134709309366E-2,6.877282441700959E-2,0.61731233023424781,3.3010955720164605,2.0417200222995979,43.023077290447013,13.010465143878513,797.01145733240969,6.7479529459279668,151.93623122948432,-151953.80987200001,139.22542500177823,3.9992397297503981,65.381373680671231,-153347.31333391232,187.81285141928544,14.573542931360898,3.3868296428812177,9.1597808685230167,-153657.78427396511,211.65251994894464]
["Cart. DDR","C133B (230 V)",510,32.700000000000003,443.08736156783669,28.043503896698525,175,1017,175,0.37,7,954,302,325,46,175,175,175,443.08736156783669,0.37251655629139074,3.6926703150993806E-2,9.7377450501960491E-2,0.72756545413437868,-99.032867160493822,9,91.076622400000005,9,-8675.2880000000005,7.5,8687.2880000000005,9,4.9475767643774281E-2,0.13228655049624791,1.1874184234505827,6.3497544238198991,3.9273085134821679,43.023077290447013,13.010465143878513,797.01145733240969,1.8166149604095208,39.866605225854315,-153227.42207690171,279.6613143300176,1.0283961141521614,14.400629199600136,-153607.03525008229,379.54041662640708,23.554329267633079,0.91340421563080409,2.4010751065115201,-153662.41636624697,408.84682413467357]
["Cart. DDR","C133C (230 V)",498.7,20,481.2845479098915,18.948210547633526,100,1072.5999999999999,100,0.94,18.100000000000001,1536,302,325,46,100,100,100,481.2845479098915,0.37251655629139074,3.7425252014767554E-2,9.2329728846255663E-2,1.2732395447351628,-99.032867160493822,9,91.076622400000005,9,-8675.2880000000005,7.5,8687.2880000000005,9,3.0946076310118701E-2,8.2742519852026797E-2,0.74270583144284885,3.9716409528972862,2.4564507988364923,43.023077290447013,13.010465143878513,797.01145733240969,4.9967698431443646,107.57419794181133,-152437.76470959728,164.23029267498509,2.8109422423861532,44.515703055501,-153454.01704125662,225.86444020795631,17.800554869139898,2.3678969705561279,6.143102568169394,-153660.00116844568,253.44723562660212]
["Cart. DDR","CH041A (400 V)",4.57,2.73,4.0794595013314616,2.4282497031734893,2500,12.3,2500,8.4700000000000006,34.4,102,0.58600000000000008,565,10,2307.8809379936233,2500,2500,4.0794595013314616,191.97952218430032,2.1729436586462447,2.3748810734308941,8.542394225094313E-2,-22.655601485432097,9,29.2110372032,9,-2362.4731839999999,7.5,2374.4731839999999,9,0.24693689199952171,0.36353998707483587,5.9264854079885207,17.449919379592121,13.062629390999115,23.047617449298862,2.4274059566222941,148.70109082419535,2.3540464906972931E-2,10.9950135234466,-150759.09990434512,2307.8809379936233,1.1753484114447826E-2,3.524036526195784,-153365.58512500091,3465.468618409041,2.3550286328138643,5.1922017140331234E-2,19.546761538537023,-144483.01464233876,1490.4949492905255]
["Cart. DDR","CH041A (480 V)",4.57,2.73,4.0794595013314616,2.4282497031734893,2500,12.3,2500,8.4700000000000006,34.4,102,0.58600000000000008,679,10,2307.8809379936233,2500,2500,4.0794595013314616,191.97952218430032,2.1729436586462447,2.3748810734308941,8.542394225094313E-2,-22.655601485432097,9,29.2110372032,9,-2362.4731839999999,7.5,2374.4731839999999,9,0.24693689199952171,0.36353998707483587,5.9264854079885207,17.449919379592121,13.062629390999115,23.047617449298862,2.4274059566222941,148.70109082419535,2.3540464906972931E-2,10.9950135234466,-150759.09990434512,2307.8809379936233,1.1753484114447826E-2,3.524036526195784,-153365.58512500091,3465.468618409041,2.3550286328138643,5.1922017140331234E-2,19.546761538537023,-144483.01464233876,1490.4949492905255]
["Cart. DDR","CH042A (400 V)",8.26,4.68,7.1008569409880025,3.98924547246517,2500,22.2,2500,3.7,18.3,108,0.88700000000000001,565,10,2410.324122846042,2500,2500,7.1008569409880025,126.83201803833146,1.2032145385123145,1.318595397045045,5.2453018578165221E-2,-22.731873844938274,9,29.2728178144,9,-2368.7773280000001,7.5,2380.7773280000001,9,0.23433463965931403,0.3455326557995157,5.624031351823537,16.585567478376753,12.411675397014889,23.059887893349117,2.437974479701396,149.34851071948552,2.2558272844647256E-2,8.7057238524199949,-152039.56524788679,2410.324122846042,1.2687029316264814E-2,2.6677787123864802,-153511.45706322312,3374.9378355517601,3.8544613556924112,2.2271706754863417E-2,8.5904618969150892,-152082.29484734332,2427.390413838219]
["Cart. DDR","CH042A (480 V)",8.26,4.68,7.1008569409880025,3.98924547246517,2500,22.2,2500,3.7,18.3,108,0.88700000000000001,679,10,2410.324122846042,2500,2500,7.1008569409880025,126.83201803833146,1.2032145385123145,1.318595397045045,5.2453018578165221E-2,-22.731873844938274,9,29.2728178144,9,-2368.7773280000001,7.5,2380.7773280000001,9,0.23433463965931403,0.3455326557995157,5.624031351823537,16.585567478376753,12.411675397014889,23.059887893349117,2.437974479701396,149.34851071948552,2.2558272844647256E-2,8.7057238524199949,-152039.56524788679,2410.324122846042,1.2687029316264814E-2,2.6677787123864802,-153511.45706322312,3374.9378355517601,3.8544613556924112,2.2271706754863417E-2,8.5904618969150892,-152082.29484734332,2427.390413838219]
["Cart. DDR","CH043A (400 V)",11.1,4.7300000000000004,9.3922637083297165,3.9629804676496692,2250,30,2250,3.97,20.6,143,1.19,565,10,1917.5773514850775,2250,2250,9.3922637083297165,94.537815126050418,0.89608941698428346,0.97783363093333331,5.858173045400044E-2,-22.808652997530864,9,29.335008928000001,9,-2375.12336,7.5,2387.12336,9,0.17633637539622996,0.26042528571591594,4.2320730095095191,12.500413714363965,9.3516228117454716,23.07226619376527,2.4486132255252078,150.00023240809975,3.470874574802256E-2,12.570327371767856,-151732.20467708181,1917.5773514850775,2.1820237548510965E-2,3.898046770870649,-153478.23579847554,2564.3049035695417,3.9642394047593328,2.8079744496115368E-2,9.1954746880222249,-152630.24829162724,2173.4413354944099]
["Cart. DDR","CH043A (480 V)",11.1,4.7300000000000004,9.1749641593615827,3.8712928942453932,2500,30,2500,3.97,20.6,143,1.19,679,10,1917.5773514850775,2500,2500,9.1749641593615827,94.537815126050418,0.89610918551622343,0.97783363093333331,5.858173045400044E-2,-22.808652997530864,9,29.335008928000001,9,-2375.12336,7.5,2387.12336,9,0.17633637539622996,0.26042528571591594,4.2320730095095191,12.500413714363965,9.3516228117454716,23.07226619376527,2.4486132255252078,150.00023240809975,3.470874574802256E-2,12.570327371767856,-151732.20467708181,1917.5773514850775,2.1816222969487868E-2,3.892336422748194,-153478.77966125665,2564.6640580315748,3.9584320893594525,2.8079744496115368E-2,9.1954746880222249,-152630.24829162724,2173.4413354944099]
["Cart. DDR","CH044A (400 V)",14.1,5,12.316011704343641,4.3214076155591723,1850,38.1,1850,4.08,22.1,173,1.49,565,10,1608.2324874620938,1850,1850,12.316011704343641,75.503355704697981,0.70580781859119079,0.77156389207349085,6.8823759174873655E-2,-22.884671960493826,9,29.396584288000003,9,-2381.4065599999999,7.5,2393.4065599999999,9,0.14682018246412712,0.2171733472813239,3.5236843791390511,10.424320669503548,7.7960527824477843,23.084547916500341,2.459146637231953,150.64550140672779,4.8260364377784776E-2,16.517440876152222,-151385.0577274785,1608.2324874620938,3.1805226542143752E-2,5.2843065488464607,-153430.74884140649,2114.8748787412173,4.3223617370183138,3.6032691810862001E-2,9.5310701139650931,-152905.19334493871,1931.9642084603913]
["Cart. DDR","CH044A (480 V)",14.2,5,11.756245129721334,4.1249982911302929,2250,38.1,2250,4.08,22.1,173,1.49,679,10,1613.403409719413,2116.7902202828741,2250,11.900926039922433,75.503355704697981,0.70096343002604533,0.77156389207349085,6.5798355069742909E-2,-22.884671960493826,9,29.396584288000003,9,-2381.4065599999999,7.5,2393.4065599999999,9,0.14578623751719666,0.21564395751173712,3.4988697004127198,10.350909960563381,7.7411510022897012,23.084547916500341,2.459146637231953,150.64550140672779,4.8003085260600042E-2,16.401120869982137,-151417.04248561795,1613.403409719413,3.1769976663008202E-2,5.2344313396000546,-153435.13108148461,2116.7902202828741,4.2815657131541212,3.5947027022998783E-2,9.4639499018949174,-152915.84313086324,1935.0628801975272]
["Cart. DDR","CH051A (400 V)",11.7,4.75,10.27231475555976,4.1254276126746019,2100,30,2100,4.13,24,151,2.74,565,10,1782.8140780791962,2100,2100,10.27231475555976,41.058394160583937,0.85228995077759651,0.98843827626666669,6.2832689534958741E-2,-23.201417639506168,9,29.653148288000001,9,-2407.5865600000002,7.5,2419.5865600000002,9,0.16846492794285353,0.25080565236467239,4.043158270628485,12.038671313504276,8.9917916383296781,23.135999099230439,2.5030358526767236,153.33412223434448,4.0369674500952947E-2,13.155780805999616,-151766.33576799804,1782.8140780791962,2.4810354759458485E-2,4.4491335331039972,-153446.96139209476,2398.8778124377595,4.1189622741019258,3.2376764588681821E-2,9.7125632716554318,-152629.68258732173,2026.3966959853915]
["Cart. DDR","CH051A (480 V)",11.7,4.75,10.030581133423611,4.0283458367163094,2500,30,2500,4.13,24,151,2.74,679,10,1782.8140780791962,2397.6265652679117,2500,10.098942790774801,41.058394160583937,0.85227039884345657,0.98843827626666669,6.2832689534958741E-2,-23.201417639506168,9,29.653148288000001,9,-2407.5865600000002,7.5,2419.5865600000002,9,0.16846492794285353,0.25080565236467239,4.043158270628485,12.038671313504276,8.9917916383296781,23.135999099230439,2.5030358526767236,153.33412223434448,4.0369674500952947E-2,13.155780805999616,-151766.33576799804,1782.8140780791962,2.482851673948169E-2,4.4691955209342726,-153444.99964251198,2397.6265652679117,4.1375354570377825,3.2376764588681821E-2,9.7125632716554318,-152629.68258732173,2026.3966959853915]
["Cart. DDR","CH052A (400 V)",16.8,9.84,14.090942041584047,8.1450532032277732,2500,26.6,2500,1.1399999999999999,7,105,3.59,565,10,2500,2500,2500,14.090942041584047,31.337047353760447,0.59454765081557182,1.121338789774436,5.0929581789406507E-2,-23.416804701234568,9,29.827611808,9,-2425.3889599999998,7.5,2437.3889599999998,9,0.24341570334980092,0.36396788218095238,5.8419768803952223,17.470458344685714,13.03757212878488,23.171240321946957,2.532880519179169,155.1623843971239,1.3470622913447599E-2,3.2301465843561949,-153427.40483091999,3257.1076012502963,1.1625011618450698E-2,1.5999533267222374,-153605.95350005239,3566.8605547602101,7.717071711561581,1.2737568833962362E-2,2.7030339589276005,-153498.32216364818,3366.9474478707548]
["Cart. DDR","CH052A (480 V)",16.8,9.84,14.090942041584047,8.1450532032277732,2500,26.6,2500,1.1399999999999999,7,105,3.59,679,10,2500,2500,2500,14.090942041584047,31.337047353760447,0.59454765081557182,1.121338789774436,5.0929581789406507E-2,-23.416804701234568,9,29.827611808,9,-2425.3889599999998,7.5,2437.3889599999998,9,0.24341570334980092,0.36396788218095238,5.8419768803952223,17.470458344685714,13.03757212878488,23.171240321946957,2.532880519179169,155.1623843971239,1.3470622913447599E-2,3.2301465843561949,-153427.40483091999,3257.1076012502963,1.1625011618450698E-2,1.5999533267222374,-153605.95350005239,3566.8605547602101,7.717071711561581,1.2737568833962362E-2,2.7030339589276005,-153498.32216364818,3366.9474478707548]
["Cart. DDR","CH052C (400 V)",16.899999999999999,5.74,10.504226244065093,3.5131191451722716,2500,43.1,1750,3.36,90,181,3.59,565,10,604.78285397374259,1543.3962126186482,1750,12.951514803329726,31.337047353760447,0.59217264869604302,0.69205595842227374,0.1197264960527518,-23.416804701234568,9,29.827611808,9,-2425.3889599999998,7.5,2437.3889599999998,9,0.14115230135077217,0.21105829854280081,3.3876552324185321,10.130798330054439,7.5602489267509974,23.171240321946957,2.532880519179169,155.1623843971239,0.38966255715719988,15.419877996977307,-151849.55113212613,604.78285397374259,6.1606651439842404E-2,4.3837612342000609,-153517.35183176279,1543.3962126186482,4.1616774017173963,0.1279563461292898,7.9636941951139271,-153180.03716894102,1063.4567841809803]
["Cart. DDR","CH052C (480 V)",16.899999999999999,5.74,12.108508070431398,4.0496682509804005,2500,43.1,2100,3.36,90,181,3.59,679,10,604.78285397374259,1477.0018233204853,2100,14.069183073440714,31.337047353760447,0.59167252777434443,0.69205595842227374,0.1197264960527518,-23.416804701234568,9,29.827611808,9,-2425.3889599999998,7.5,2437.3889599999998,9,0.14115230135077217,0.21105829854280081,3.3876552324185321,10.130798330054439,7.5602489267509974,23.171240321946957,2.532880519179169,155.1623843971239,0.38966255715719988,15.419877996977307,-151849.55113212613,604.78285397374259,6.7119203001615224E-2,4.7843389154203324,-153489.32661657454,1477.0018233204853,4.5419615902268013,0.1279563461292898,7.9636941951139271,-153180.03716894102,1063.4567841809803]
["Cart. DDR","CH053A (400 V)",20.9,9.2100000000000009,16.93679496528561,7.3638238979502662,2350,53.7,2350,1.41,9.1,139,4.43,565,10,2166.3777227331402,2350,2350,16.93679496528561,25.39503386004515,0.47880860276537562,0.55865964275605218,5.4180406158943095E-2,-23.629657797530864,9,30.000022816000005,9,-2442.9819199999997,7.5,2454.9819199999997,9,0.18341385777129846,0.27541886975215318,4.4019325865111627,13.220105748103354,9.8573571267913405,23.206268217499687,2.5623740719580552,156.96913759328234,2.8855908992907277E-2,8.0330814429213415,-152829.02254711703,2166.3777227331402,2.0243795463701839E-2,2.4990596327153791,-153583.19027162326,2693.3602068923965,7.3617671905155939,2.0975482869540242E-2,3.3462241664692192,-153519.11598555636,2626.7716530936054]
["Cart. DDR","CH053A (480 V)",20.9,9.2100000000000009,16.810581709138354,7.3089485691905898,2500,53.7,2500,1.41,9.1,139,4.43,679,10,2166.3777227331402,2500,2500,16.810581709138354,25.39503386004515,0.47878278718091,0.55865964275605218,5.0929581789406507E-2,-23.629657797530864,9,30.000022816000005,9,-2442.9819199999997,7.5,2454.9819199999997,9,0.18341385777129846,0.27541886975215318,4.4019325865111627,13.220105748103354,9.8573571267913405,23.206268217499687,2.5623740719580552,156.96913759328234,2.8855908992907277E-2,8.0330814429213415,-152829.02254711703,2166.3777227331402,2.0258710114067525E-2,2.519174166623944,-153581.88418713078,2691.8938104652434,7.4210208849221146,2.0975482869540242E-2,3.3462241664692192,-153519.11598555636,2626.7716530936054]
["Cart. DDR","CH054A (400 V)",24.8,9.7899999999999991,20.326359874879206,7.9090894454782905,2100,63.5,2100,1.35,9,155.5,5.28,565,10,1972.7015197940109,2100,2100,20.326359874879206,21.30681818181818,0.40417870777244874,0.47518876119685038,6.0630454511198223E-2,-23.845044859259257,9,30.174486336000001,9,-2460.7843199999998,7.5,2472.7843199999998,9,0.16455702585422219,0.24815878799516125,3.9493686205013323,11.91162182376774,8.8741994520681686,23.241915855232889,2.5922187384604998,158.79739975606171,3.4645581736585329E-2,9.1144302442716825,-152805.10856300395,1972.7015197940109,2.522172484360987E-2,2.8752619550394583,-153578.52599425049,2411.2761047322019,7.9077444979527023,2.5491851479369009E-2,3.2266657164466506,-153556.35665837108,2391.8591053770233]
["Cart. DDR","CH054A (480 V)",24.8,9.7899999999999991,19.251381916395662,7.4908100842006471,2500,63.5,2500,1.35,9,156,5.28,679,10,1968.1631515043666,2404.71442517792,2500,19.462863221821433,21.30681818181818,0.40421100371170199,0.47518876119685038,5.3394811470598449E-2,-23.845044859259257,9,30.174486336000001,9,-2460.7843199999998,7.5,2472.7843199999998,9,0.16455702585422219,0.24815878799516125,3.9493686205013323,11.91162182376774,8.8741994520681686,23.241915855232889,2.5922187384604998,158.79739975606171,3.4801331736585325E-2,9.1437370939317208,-152805.10856300395,1968.1631515043666,2.5365851604193915E-2,2.8683659319768853,-153579.47991535455,2404.71442517792,7.8634940311548256,2.5647601479369009E-2,3.2370408473677013,-153556.35665837108,2384.5754103584854]
["Cart. DDR","CH061A (400 V)",33.4,9.89,29.131322896182791,8.5680361459361158,1600,85.7,1600,1.36,18.100000000000001,206,9.41,565,10,1264.4360860420074,1600,1600,29.131322896182791,11.955366631243358,0.3023418616130214,0.36198569185530921,7.9577471545947673E-2,-24.891572582716048,9,31.022173792,9,-2547.2830400000003,7.5,2559.2830400000003,9,0.12436924734843124,0.19137306562055889,2.9848619363623499,9.1859071497868268,6.8163275456798891,23.417993836051828,2.7372287062900238,167.68060297050738,8.581474180151874E-2,12.313950481271291,-152770.69374790744,1264.4360860420074,4.7395268704823301E-2,4.1635879910108953,-153561.87288529263,1756.6187994391605,8.5802707288864699,4.5565799815879326E-2,3.307632172542498,-153599.5474680175,1800.0754007097357]
["Cart. DDR","CH061A (480 V)",33.4,9.89,27.893997920842708,8.204117035541973,1900,85.7,1900,1.36,18.100000000000001,206,9.41,679,10,1264.4360860420074,1759.1326051759381,1900,28.302216957046262,11.955366631243358,0.30238813629227629,0.36198569185530921,7.0732567326521348E-2,-24.891572582716048,9,31.022173792,9,-2547.2830400000003,7.5,2559.2830400000003,9,0.12436924734843124,0.19137306562055889,2.9848619363623499,9.1859071497868268,6.8163275456798891,23.417993836051828,2.7372287062900238,167.68060297050738,8.581474180151874E-2,12.313950481271291,-152770.69374790744,1264.4360860420074,4.7283976141252987E-2,4.1166046866226225,-153564.16475312281,1759.1326051759381,8.4834481152514485,4.5565799815879326E-2,3.307632172542498,-153599.5474680175,1800.0754007097357]
["Cart. DDR","CH062A (400 V)",47.3,14.6,39.701923985832799,12.141261157747033,1650,121.5,1650,0.76,11.1,198,12.6,565,10,1366.2876361446313,1650,1650,39.701923985832799,8.9285714285714288,0.21484560739960024,0.26071543308641976,7.7166033014252289E-2,-25.699907555555555,9,31.67692512,9,-2614.0944,7.5,2626.0944,9,0.13041544814165446,0.20370115695560254,3.1299707553997069,9.7776555338689217,7.2341237220974612,23.557208676442674,2.8492339841050796,174.54196332258525,7.4836020663870462E-2,9.7747892578686457,-153054.70946181676,1366.2876361446313,4.2928299498342884E-2,3.1601629449516371,-153600.31625702322,1855.1284384382759,12.124673889891737,4.0529794856051522E-2,1.8854948127575697,-153641.32954106128,1923.8822577577139]
["Cart. DDR","CH062A (480 V)",47.3,14.6,37.543059525947193,11.481057959005257,2000,121.5,2000,0.76,11.1,198,12.6,679,10,1366.2876361446313,1856.9728425754618,1979.7979797979799,38.240813256529293,8.9285714285714288,0.21487323965751459,0.26071543308641976,6.6180741550115663E-2,-25.699907555555555,9,31.67692512,9,-2614.0944,7.5,2626.0944,9,0.13041544814165446,0.20370115695560254,3.1299707553997069,9.7776555338689217,7.2341237220974612,23.557208676442674,2.8492339841050796,174.54196332258525,7.4836020663870462E-2,9.7747892578686457,-153054.70946181676,1366.2876361446313,4.2857888753789236E-2,3.1301477482241129,-153601.52024713223,1856.9728425754618,12.009513855930972,4.0529794856051522E-2,1.8854948127575697,-153641.32954106128,1923.8822577577139]
["Cart. DDR","CH062C (400 V)",48.4,11.8,40.489017522578173,9.7799559233280622,1250,124.2,1250,1.19,17.8,250.4,12.6,565,10,1054.7499694901746,1250,1250,40.489017522578173,8.9285714285714288,0.2101188134754057,0.25504770628019324,0.10185916357881301,-25.699907555555555,9,31.67692512,9,-2614.0944,7.5,2626.0944,9,0.10300871479930802,0.16089347297520662,2.4722091551833927,7.7228867028099177,5.7138766758908028,23.557208676442674,2.8492339841050796,174.54196332258525,0.12243325195315058,15.627883130453613,-152690.19574200801,1054.7499694901746,6.8825258174048193E-2,5.0043673734048513,-153564.14502033169,1457.8129248586067,9.6963273893168314,6.4827124483100906E-2,2.9489864424329797,-153629.32496473033,1516.8485360348061]
["Cart. DDR","CH062C (480 V)",48.4,11.8,37.889144516715724,9.1519672745690155,1550,124.2,1550,1.19,17.8,250.4,12.6,679,10,1054.7499694901746,1459.8283709124701,1550,38.500616105123044,8.9285714285714288,0.21016252375069877,0.25504770628019324,8.3939794546892488E-2,-25.699907555555555,9,31.67692512,9,-2614.0944,7.5,2626.0944,9,0.10300871479930802,0.16089347297520662,2.4722091551833927,7.7228867028099177,5.7138766758908028,23.557208676442674,2.8492339841050796,174.54196332258525,0.12243325195315058,15.627883130453613,-152690.19574200801,1054.7499694901746,6.8674282621128013E-2,4.9423070491979244,-153566.60631325122,1459.8283709124701,9.5760809772337598,6.4827124483100906E-2,2.9489864424329797,-153629.32496473033,1516.8485360348061]
["Cart. DDR","CH063A (400 V)",60.2,13.9,52.437097410372942,12.026857204213977,1250,154.4,1250,0.93,14.4,264,15.7,565,10,1051.2246218803016,1250,1250,52.437097410372942,7.1656050955414017,0.16981748889402842,0.20928240829015543,0.10185916357881301,-26.485436839506171,9,32.31320384,9,-2679.0207999999998,7.5,2691.0207999999998,9,9.8127525487680223E-2,0.15543796143964564,2.3550606117043253,7.4610221491029902,5.5049648945637797,23.695127193068544,2.9580792384081125,181.20974297507473,0.12388544489239156,15.160485444035794,-152839.56129871577,1051.2246218803016,7.5880247532196674E-2,5.1215237251342005,-153569.9128025026,1389.2721217908679,12.04347141319357,7.0988089507566063E-2,2.3410034653839999,-153644.34213862725,1454.7827769621058]
["Cart. DDR","CH063A (480 V)",60.2,13.9,50.674933880459477,11.622691256986117,1500,154.4,1500,0.93,14.4,264,15.7,679,10,1051.2246218803016,1389.5643959758268,1484.8484848484848,51.376204833980573,7.1656050955414017,0.16982625379308097,0.20928240829015543,8.7520938857549316E-2,-26.485436839506171,9,32.31320384,9,-2679.0207999999998,7.5,2691.0207999999998,9,9.8127525487680223E-2,0.15543796143964564,2.3550606117043253,7.4610221491029902,5.5049648945637797,23.695127193068544,2.9580792384081125,181.20974297507473,0.12388544489239156,15.160485444035794,-152839.56129871577,1051.2246218803016,7.5855218348909931E-2,5.1111491791449239,-153570.29359672192,1389.5643959758268,12.019075246202577,7.0988089507566063E-2,2.3410034653839999,-153644.34213862725,1454.7827769621058]
["Cart. DDR","CH063B (400 V)",58,19.5,45.800491136899048,15.266830378966349,1850,149,1850,0.47,7.1,181,15.7,565,10,1553.198757048619,1850,1850,45.800491136899048,7.1656050955414017,0.17630013838429259,0.2168671398657718,6.8823759174873655E-2,-26.485436839506171,9,32.31320384,9,-2679.0207999999998,7.5,2691.0207999999998,9,0.14288253804265419,0.22633170793103449,3.4291809130237003,10.863921980689655,8.0157259857708016,23.695127193068544,2.9580792384081125,181.20974297507473,5.877223530614345E-2,7.3812505339959316,-153248.239954171,1553.198757048619,3.5192957445022752E-2,2.2569786095208864,-153625.12792311105,2057.4920294526314,15.317587960057732,3.3426979606751464E-2,1.1810816518136211,-153653.35507258438,2126.3947133491693]
["Cart. DDR","CH063B (480 V)",58,19.5,41.73910725740906,13.913035752469687,2200,149,2200,0.47,7.1,181,15.7,679,10,1553.198757048619,2062.6069155487426,2165.7458563535911,42.75462280733435,7.1656050955414017,0.17635403772869473,0.2168671398657718,5.9877855072812514E-2,-26.485436839506171,9,32.31320384,9,-2679.0207999999998,7.5,2691.0207999999998,9,0.14288253804265419,0.22633170793103449,3.4291809130237003,10.863921980689655,8.0157259857708016,23.695127193068544,2.9580792384081125,181.20974297507473,5.877223530614345E-2,7.3812505339959316,-153248.239954171,1553.198757048619,3.5049272899237968E-2,2.1892903662925005,-153627.42455733998,2062.6069155487426,14.858203624229807,3.3426979606751464E-2,1.1810816518136211,-153653.35507258438,2126.3947133491693]
["Cart. DDR","CH063C (400 V)",61.8,11.3,54.07917434743559,9.7969518745354343,950,158.9,950,1.45,23.1,333.8,15.7,565,10,806.41549905629211,950,950,54.07917434743559,7.1656050955414017,0.16552525584069638,0.20335559370673378,0.13402521523528027,-26.485436839506171,9,32.31320384,9,-2679.0207999999998,7.5,2691.0207999999998,9,7.7707422979964788E-2,0.12309169477885655,1.8649781515191548,5.9084013493851142,4.35939491417657,23.695127193068544,2.9580792384081125,181.20974297507473,0.20404359640555086,24.357282183837658,-152332.85612228763,806.41549905629211,0.1218871335591151,8.1872298998624427,-153513.60225823181,1089.17976360122,9.7661192673765704,0.11350757843768923,3.6546111520346294,-153634.03255656452,1147.4188057799927]
["Cart. DDR","CH063C (480 V)",61.8,11.3,51.89835100822674,9.4018751826497731,1150,158.9,1150,1.45,23.1,333.8,15.7,679,10,806.41549905629211,1090.0229496765005,1150,52.414761182022573,7.1656050955414017,0.1655540428324502,0.20335559370673378,0.1109655461738436,-26.485436839506171,9,32.31320384,9,-2679.0207999999998,7.5,2691.0207999999998,9,7.7707422979964788E-2,0.12309169477885655,1.8649781515191548,5.9084013493851142,4.35939491417657,23.695127193068544,2.9580792384081125,181.20974297507473,0.20404359640555086,24.357282183837658,-152332.85612228763,806.41549905629211,0.12174552934126456,8.1316480044725701,-153515.63738276454,1090.0229496765005,9.6998185251079967,0.11350757843768923,3.6546111520346294,-153634.03255656452,1147.4188057799927]
["Cart. DDR","CH091A (400 V)",50,12.8,28.842332447196419,7.1569063144407981,884,120,1200,0.91600000000000004,7.8,244,28,565,38,790.33603173025085,1200,1200,21.279184317461201,4.0178571428571432,0.21115834357698027,0.29031494666666663,0.10610329539459688,-29.602214320987649,9,34.837793599999998,9,-2936.6320000000001,7.5,2948.6320000000001,9,0.11142178337810789,0.18580156586666666,2.6741228010745894,8.9184751616,6.5149056717088127,24.267031064205881,3.38994911838466,207.66577191882325,0.23000967725837071,11.89233511510654,-153070.1255606272,790.33603173025085,6.2740093214163128E-2,1.6303882814439692,-153652.83798899711,1552.0008243936354,4.211580612316947,6.7203100758586848E-2,2.5220521318772611,-153637.29033292501,1493.3585468509143]
["Cart. DDR","CH091A (480 V)",50,12.8,28.842332447196419,7.1569063144407981,884,120,1500,0.91600000000000004,7.8,244,28,679,38,790.33603173025085,1500,1500,14.098980396826505,4.0178571428571432,0.21115834357698027,0.29031494666666663,8.5260137119787971E-2,-29.602214320987649,9,34.837793599999998,9,-2936.6320000000001,7.5,2948.6320000000001,9,0.11142178337810789,0.18580156586666666,2.6741228010745894,8.9184751616,6.5149056717088127,24.267031064205881,3.38994911838466,207.66577191882325,0.23000967725837071,11.89233511510654,-153070.1255606272,790.33603173025085,6.2740093214163128E-2,1.6303882814439692,-153652.83798899711,1552.0008243936354,4.211580612316947,6.7203100758586848E-2,2.5220521318772611,-153637.29033292501,1493.3585468509143]
["Cart. DDR","CH092A (400 V)",101,15.3,69.437028028949783,10.211327651316145,700,227,700,0.92100000000000004,11,441,47,565,38,477.75409202250847,700,700,69.437028028949783,2.3936170212765959,0.10857295546506444,0.17065007224669607,0.18189136353359467,-34.41674864197531,9,38.737566400000006,9,-3334.5680000000002,7.5,3346.5680000000002,9,6.8529709384237511E-2,0.12225345831683171,1.6447130252217002,5.868165999207922,4.2312108723832456,25.222918645338218,4.057065193145184,248.53280849859757,0.61929899024442847,24.191052348087272,-152911.73240868273,477.75409202250847,0.22988925405738475,6.9840214989599252,-153601.29907253417,802.35769819510995,9.9276560094411987,0.20091291670404904,2.9766208328788486,-153652.61036350243,867.13617652343339]
["Cart. DDR","CH092A (480 V)",101,15.3,67.944370989854903,9.9918192632139569,721,227,800,0.92100000000000004,11,441,47,679,38,477.75409202250847,800,800,64.32246434380572,2.3936170212765959,0.10859119221865904,0.17065007224669607,0.15915494309189535,-34.41674864197531,9,38.737566400000006,9,-3334.5680000000002,7.5,3346.5680000000002,9,6.8529709384237511E-2,0.12225345831683171,1.6447130252217002,5.868165999207922,4.2312108723832456,25.222918645338218,4.057065193145184,248.53280849859757,0.61929899024442847,24.191052348087272,-152911.73240868273,477.75409202250847,0.22940217617276631,6.9358188640254355,-153602.16158993094,803.29862544988271,9.8591368649268887,0.20091291670404904,2.9766208328788486,-153652.61036350243,867.13617652343339]
["Cart. DDR","CH092C (400 V)",101.6,18.100000000000001,60.041202281417512,10.589277298309966,800,231.2,800,0.59,7.35,343,47,565,38,608.74320030770593,800,800,60.041202281417512,2.3936170212765959,0.10808889205263039,0.16755002768166094,0.15915494309189535,-34.41674864197531,9,38.737566400000006,9,-3334.5680000000002,7.5,3346.5680000000002,9,8.0592327804361971E-2,0.14377254589895019,1.9342158673046874,6.9010822031496089,4.9759897816657741,25.222918645338218,4.057065193145184,248.53280849859757,0.38975979599526256,14.437083081036832,-153221.09490117052,608.74320030770593,0.13089079471780662,3.1847840884078216,-153642.44680003703,1071.3329906874669,9.0860105289968516,0.1216205436408845,1.744159665031636,-153657.53565917024,1116.8708798494758]
["Cart. DDR","CH092C (480 V)",101.6,18.100000000000001,42.207890907970643,7.4440724705415597,1000,231.2,1000,0.64,7.35,343,47,679,38,607.06193173119038,1000,1000,42.207890907970643,2.3936170212765959,0.10826689164950663,0.16755002768166094,0.12732395447351627,-34.41674864197531,9,38.737566400000006,9,-3334.5680000000002,7.5,3346.5680000000002,9,8.0592327804361971E-2,0.14377254589895019,1.9342158673046874,6.9010822031496089,4.9759897816657741,25.222918645338218,4.057065193145184,248.53280849859757,0.38975979599526256,15.660564698073852,-153142.84536489355,607.06193173119038,0.12765225407013894,3.0026532442842964,-153644.84147229171,1085.3982659035285,7.8971513250302543,0.1216205436408845,1.8919698061360122,-153656.3935822928,1116.2630741455855]
["Cart. DDR","CH093A (400 V)",145,15.5,109.38285179770261,12.793315999731298,550,309,550,0.86699999999999999,11,517,66,565,38,462.76469453408663,550,550,109.38285179770261,1.7045454545454546,7.8731195111282584E-2,0.13798491650485437,0.23149809904275684,-39.231282962962965,9,42.6373392,9,-3732.5039999999999,7.5,3744.5039999999999,9,5.0343411354240371E-2,9.495384448275862E-2,1.208241872501769,4.5577845351724138,3.2511725929696853,26.258230168105548,4.7241812679057071,289.39984507837187,0.6592613406265776,25.644394149670696,-153048.90271643832,462.76469453408663,0.32245349157408898,9.620431287753723,-153577.43386918056,675.37247416472178,12.391511210994381,0.27108644176045077,2.5241217154806597,-153658.04091597992,748.23533825154016]
["Cart. DDR","CH093A (480 V)",145,15.5,96.52771935511548,11.289791737440407,646,309,650,0.86699999999999999,11,517,66,679,38,462.76469453408663,650,650,96.227581394466029,1.7045454545454546,7.8856422147122462E-2,0.13798491650485437,0.19588300688233271,-39.231282962962965,9,42.6373392,9,-3732.5039999999999,7.5,3744.5039999999999,9,5.0343411354240371E-2,9.495384448275862E-2,1.208241872501769,4.5577845351724138,3.2511725929696853,26.258230168105548,4.7241812679057071,289.39984507837187,0.6592613406265776,25.644394149670696,-153048.90271643832,462.76469453408663,0.31384226276290023,8.8377109750543195,-153590.94692329408,685.62524034704154,11.383335252996105,0.27108644176045077,2.5241217154806597,-153658.04091597992,748.23533825154016]
["Cart. DDR","CH093C (400 V)",139.4,20,87.853528586726242,12.461493416556914,700,316.60000000000002,700,0.65,7.54,426,66,565,38,517.26352629577013,700,700,87.853528586726242,1.7045454545454546,8.2044085312169765E-2,0.13467258117498421,0.18189136353359467,-39.231282962962965,9,42.6373392,9,-3732.5039999999999,7.5,3744.5039999999999,9,6.7568793875733363E-2,0.12744302725968434,1.6216510530176007,6.1172653084648489,4.3635861154311506,26.258230168105548,4.7241812679057071,289.39984507837187,0.5297528901178814,21.785208235834901,-153010.20101572841,517.26352629577013,0.20471504343174723,5.6274093835158512,-153620.37475978961,852.62707054191833,11.733428394413517,0.1846900712154983,2.0927971455851826,-153657.96641995007,906.47985094237993]
["Cart. DDR","CH093C (480 V)",139.4,20,67.322540927871728,9.5492965855137211,800,316.60000000000002,800,0.59,7.54,426,66,679,38,519.29434055471393,800,800,67.322540927871728,1.7045454545454546,8.2262126884436376E-2,0.13467258117498421,0.15915494309189535,-39.231282962962965,9,42.6373392,9,-3732.5039999999999,7.5,3744.5039999999999,9,6.7568793875733363E-2,0.12744302725968434,1.6216510530176007,6.1172653084648489,4.3635861154311506,26.258230168105548,4.7241812679057071,289.39984507837187,0.5297528901178814,19.774265937142449,-153125.33153508889,519.29434055471393,0.19813939269711389,4.3253350670248629,-153638.22727600063,869.72346299313642,9.9356782258380392,0.1846900712154983,1.8996158706080886,-153659.02890126535,907.00289353048879]
["Cart. DDR","CH131A (400 V)",188,13.8,142.7619839534301,11.70180196339591,400,389,400,0.93,13,738,123,565,46,351.30876533023923,400,400,142.7619839534301,0.91463414634146345,6.9049165532145171E-2,0.13968292442159386,0.31830988618379069,-53.674885925925928,9,54.336657600000009,9,-4926.3119999999999,7.5,4938.3119999999999,9,3.9173374201033208E-2,8.3094622659574485E-2,0.94016098082479693,3.9885418876595753,2.7792475236639471,29.754746189450639,6.7255294921872748,412.00095481769455,1.1441624499909331,33.944606318885967,-153135.10575984305,351.30876533023923,0.64145745859356085,13.640722293665316,-153578.59131804772,478.78988733195445,11.4745966841341,0.55032356835476992,3.3039020629000668,-153658.98949366869,525.41540919679596]
["Cart. DDR","CH131A (480 V)",188,13.8,121.08508070431398,9.9250066151077032,500,389,500,0.93,13,738,123,679,46,351.30876533023923,486.49742129198643,500,122.89212863337474,0.91463414634146345,6.9220834871724285E-2,0.13968292442159386,0.25464790894703254,-53.674885925925928,9,54.336657600000009,9,-4926.3119999999999,7.5,4938.3119999999999,9,3.9173374201033208E-2,8.3094622659574485E-2,0.94016098082479693,3.9885418876595753,2.7792475236639471,29.754746189450639,6.7255294921872748,412.00095481769455,1.1441624499909331,33.944606318885967,-153135.10575984305,351.30876533023923,0.6236286076572769,12.320851760349553,-153594.31990249571,486.49742129198643,10.364319550781374,0.55032356835476992,3.3039020629000668,-153658.98949366869,525.41540919679596]
["Cart. DDR","CH131B (400 V)",190,25.9,123.9498696799681,18.837366212761111,500,396,800,0.26100000000000001,3.6,398,123,565,46,674.82724549090801,800,800,84.319791487948962,0.91463414634146345,6.8466580197763277E-2,0.13721378181818183,0.15915494309189535,-53.674885925925928,9,54.336657600000009,9,-4926.3119999999999,7.5,4938.3119999999999,9,7.2747137169973636E-2,0.15431134121052634,1.7459312920793673,7.4069443781052637,5.1612174074082722,29.754746189450646,6.7255294921872748,412.00095481769455,0.32271319617415239,9.7123775366621334,-153515.1239024667,674.82724549090801,0.16957157342425536,2.5320602100367609,-153653.8813652003,944.4718099016095,14.073101560186606,0.15990604685269114,0.92861642309318282,-153662.63903616506,977.38418616172828]
["Cart. DDR","CH131B (480 V)",190,25.9,123.9498696799681,18.837366212761111,500,396,1000,0.26100000000000001,3.6,398,123,679,46,674.82724549090801,944.4718099016095,984.9246231155779,65.235027744804597,0.91463414634146345,6.8466580197763277E-2,0.13721378181818183,0.13027011923891299,-53.674885925925928,9,54.336657600000009,9,-4926.3119999999999,7.5,4938.3119999999999,9,7.2747137169973636E-2,0.15431134121052634,1.7459312920793673,7.4069443781052637,5.1612174074082722,29.754746189450646,6.7255294921872748,412.00095481769455,0.32271319617415239,9.7123775366621334,-153515.1239024667,674.82724549090801,0.16957157342425536,2.5320602100367609,-153653.8813652003,944.4718099016095,14.073101560186606,0.15990604685269114,0.92861642309318282,-153662.63903616506,977.38418616172828]
["Cart. DDR","CH131C (400 V)",188.8,18.8,121.27606663602425,11.889810454512183,500,394.5,500,1.1399999999999999,8.67,617,123,565,46,388.41304283085515,500,500,121.27606663602425,0.91463414634146345,6.8932863935997374E-2,0.13773550722433461,0.25464790894703254,-53.674885925925928,9,54.336657600000009,9,-4926.3119999999999,7.5,4938.3119999999999,9,5.3140495953133353E-2,0.11272170317796613,1.2753719028752004,5.4106417525423742,3.7701779536807045,29.754746189450639,6.7255294921872748,412.00095481769455,0.88537133069084861,47.857885859620531,-152159.90003982748,388.41304283085515,0.42518585234514256,14.210491685725442,-153531.38645327941,584.43105396573981,11.664294122765112,0.38533774865164938,4.5931697109661345,-153650.14537851518,625.5280014555882]
["Cart. DDR","CH131C (480 V)",188.8,18.8,91.35493733474793,8.9563664053674454,600,394.5,600,0.65,8.67,617,123,679,46,400.81575750810538,600,600,91.35493733474793,0.91463414634146345,6.9158805752046693E-2,0.13773550722433461,0.21220659078919377,-53.674885925925928,9,54.336657600000009,9,-4926.3119999999999,7.5,4938.3119999999999,9,5.3140495953133353E-2,0.11272170317796613,1.2753719028752004,5.4106417525423742,3.7701779536807045,29.754746189450646,6.7255294921872748,412.00095481769455,0.88537133069084861,27.287391060309954,-153175.01705665368,400.81575750810538,0.41394769910392903,7.0049589383418684,-153631.77589467529,600.80866395569899,10.084315992305083,0.38533774865164938,2.6189125544982348,-153659.49586212885,628.0899562564091]
["Cart. DDR","CH132A (400 V)",361,12.4,315.60425215122842,12.045963822565971,200,836,200,1.66,29,1584,225,565,46,154.41282082304116,200,200,315.60425215122842,0.5,4.4765585835141217E-2,9.512121212121212E-2,0.63661977236758138,-79.521333333333331,9,75.272279999999995,9,-7062.6,7.5,7074.6,9,2.28062511258194E-2,5.6905847953216376E-2,0.54735002701966562,2.7314807017543861,1.7583352443704143,37.019105869472448,10.306889472480607,631.39241435121937,5.5263087275935305,130.78099985935009,-151959.80627891413,154.41282082304116,3.0397478883892477,54.847903754062152,-153364.25653610213,215.77666993749168,12.043040342009887,2.5203688890981391,8.0080278328212096,-153657.61029508995,245.3300322509416]
["Cart. DDR","CH132A (480 V)",361,12.4,298.70199719486919,11.400839587590427,250,836,250,1.66,29,1584,225,679,46,154.41282082304116,217.4553700385778,247.47474747474749,306.81185898938372,0.5,4.4827648545821913E-2,9.512121212121212E-2,0.51899049335826919,-79.521333333333331,9,75.272279999999995,9,-7062.6,7.5,7074.6,9,2.28062511258194E-2,5.6905847953216376E-2,0.54735002701966562,2.7314807017543861,1.7583352443704143,37.019105869472448,10.306889472480607,631.39241435121937,5.5263087275935305,130.78099985935009,-151959.80627891413,154.41282082304116,3.0009166620495438,52.803152759906517,-153386.189048253,217.4553700385778,11.594071155832788,2.5203688890981391,8.0080278328212096,-153657.61029508995,245.3300322509416]
["Cart. DDR","CH132B (400 V)",361,26.3,232.08417017957396,18.868631721916582,395,742,400,0.36899999999999999,6.5,746,225,565,46,362.87404551527618,400,400,230.45232423247995,0.5,4.5044621584890407E-2,0.10717160826594789,0.31830988618379069,-79.521333333333331,9,75.272279999999995,9,-7062.6,7.5,7074.6,9,4.8371322952342762E-2,0.1206954678362573,1.1609117508562263,5.7933824561403506,3.7293723328178952,37.019105869472448,10.306889472480607,631.39241435121937,1.0936786261416498,25.773789240834859,-153365.58620244925,362.87404551527618,0.61587766512185249,8.567979445585566,-153631.02238939222,492.54277333390445,17.970186938541261,0.55907265645054049,1.7781220419019768,-153662.57968234702,522.67604535960152]
["Cart. DDR","CH132B (480 V)",361,26.3,232.08417017957396,18.868631721916582,395,742,500,0.36899999999999999,6.5,746,225,679,46,362.87404551527618,492.54277333390445,500,200.2492143129258,0.5,4.5044621584890407E-2,0.10717160826594789,0.25464790894703254,-79.521333333333331,9,75.272279999999995,9,-7062.6,7.5,7074.6,9,4.8371322952342762E-2,0.1206954678362573,1.1609117508562263,5.7933824561403506,3.7293723328178952,37.019105869472448,10.306889472480607,631.39241435121937,1.0936786261416498,25.773789240834859,-153365.58620244925,362.87404551527618,0.61587766512185249,8.567979445585566,-153631.02238939222,492.54277333390445,17.970186938541261,0.55907265645054049,1.7781220419019768,-153662.57968234702,522.67604535960152]
["Cart. DDR","CH132C (400 V)",361.7,16.899999999999999,298.70199719486919,13.765068995155262,250,818.3,250,0.94,19.899999999999999,1313,225,565,46,180.32263055334741,250,250,298.70199719486919,0.5,4.4747351215265428E-2,9.7178703816856088E-2,0.50929581789406508,-79.521333333333331,9,75.272279999999995,9,-7062.6,7.5,7074.6,9,3.1022558682010485E-2,7.7407066936995048E-2,0.74454140836825167,3.7155392129757625,2.3918029315819251,37.019105869472448,10.306889472480607,631.39241435121937,4.2427001788958059,81.734225951781568,-152695.23494506907,180.32263055334741,2.0523107176987012,29.510466704634176,-153537.71181774072,266.42294354151011,13.804569603338166,1.7338256903180382,5.11303306112685,-153660.20887801866,296.22857990198605]
["Cart. DDR","CH132C (480 V)",361.7,16.899999999999999,279.15777018318443,12.864413372496978,300,818.3,300,1.1399999999999999,19.899999999999999,1313,225,679,46,178.10513725167536,265.57061975927428,298.55293221629853,288.63069623745281,0.5,4.4811978671764639E-2,9.7178703816856088E-2,0.43027227395969159,-79.521333333333331,9,75.272279999999995,9,-7062.6,7.5,7074.6,9,3.1022558682010485E-2,7.7407066936995048E-2,0.74454140836825167,3.7155392129757625,2.3918029315819251,37.019105869472448,10.306889472480607,631.39241435121937,4.2427001788958059,99.124486792586126,-152239.13912925732,178.10513725167536,2.0433085559645732,35.29526128278637,-153483.34775668528,265.57061975927428,13.614014111740151,1.7338256903180382,6.2009124358346899,-153658.42401298444,295.91484782829423]
["Cart. DDR","CH133A (400 V)",504,16.8,445.23595329957726,14.645919516433462,160,1016,160,1.41,26,1837,302,565,46,139.22542500177823,160,160,445.23595329957726,0.37251655629139074,3.7348610978348074E-2,9.7473294449304942E-2,0.79577471545947664,-99.032867160493822,9,91.076622400000005,9,-8675.2880000000005,7.5,8687.2880000000005,9,2.572134709309366E-2,6.877282441700959E-2,0.61731233023424781,3.3010955720164605,2.0417200222995979,43.023077290447013,13.010465143878513,797.01145733240969,6.7479529459279668,151.93623122948432,-151953.80987200001,139.22542500177823,3.9914007803544536,64.969845396882562,-153351.28741278555,188.04143765069381,14.481813058254291,3.3868296428812177,9.1597808685230167,-153657.78427396511,211.65251994894464]
["Cart. DDR","CH133A (480 V)",504,16.8,424.94369805536053,13.978411120242123,200,1016,200,1.41,26,1837,302,679,46,139.22542500177823,188.31760805104847,200,429.56153158212021,0.37251655629139074,3.7395470769836459E-2,9.7473294449304942E-2,0.63661977236758138,-99.032867160493822,9,91.076622400000005,9,-8675.2880000000005,7.5,8687.2880000000005,9,2.572134709309366E-2,6.877282441700959E-2,0.61731233023424781,3.3010955720164605,2.0417200222995979,43.023077290447013,13.010465143878513,797.01145733240969,6.7479529459279668,151.93623122948432,-151953.80987200001,139.22542500177823,3.9819768474967567,64.47163171677677,-153356.06502399093,188.31760805104847,14.37076096425157,3.3868296428812177,9.1597808685230167,-153657.78427396511,211.65251994894464]
["Cart. DDR","CH133B (400 V)",510,32.700000000000003,326.68646213599573,20.676358363037703,342,1017,350,0.37,7,954,302,565,46,279.6613143300176,350,350,322.39842616256874,0.37251655629139074,3.7179410758641625E-2,9.7377450501960491E-2,0.36378272706718934,-99.032867160493822,9,91.076622400000005,9,-8675.2880000000005,7.5,8687.2880000000005,9,4.9475767643774281E-2,0.13228655049624791,1.1874184234505827,6.3497544238198991,3.9273085134821679,43.023077290447013,13.010465143878513,797.01145733240969,1.8166149604095208,39.866605225854315,-153227.42207690171,279.6613143300176,1.0007281850464873,12.604304951202009,-153620.36036963889,385.55474869353935,20.616178980465218,0.91340421563080409,2.4010751065115201,-153662.41636624697,408.84682413467357]
["Cart. DDR","CH133B (480 V)",510,32.700000000000003,326.68646213599573,20.676358363037703,342,1017,400,0.37,7,954,302,679,46,279.6613143300176,385.55474869353935,400,303.3409209845621,0.37251655629139074,3.7179410758641625E-2,9.7377450501960491E-2,0.31830988618379069,-99.032867160493822,9,91.076622400000005,9,-8675.2880000000005,7.5,8687.2880000000005,9,4.9475767643774281E-2,0.13228655049624791,1.1874184234505827,6.3497544238198991,3.9273085134821679,43.023077290447013,13.010465143878513,797.01145733240969,1.8166149604095208,39.866605225854315,-153227.42207690171,279.6613143300176,1.0007281850464873,12.604304951202009,-153620.36036963889,385.55474869353935,20.616178980465218,0.91340421563080409,2.4010751065115201,-153662.41636624697,408.84682413467357]
["Cart. DDR","CH133C (400 V)",498.7,20,433.53806498232291,17.068427755209566,200,1072.5999999999999,200,0.94,18.100000000000001,1536,302,565,46,164.23029267498509,200,200,433.53806498232291,0.37251655629139074,3.7681465582405711E-2,9.2329728846255663E-2,0.63661977236758138,-99.032867160493822,9,91.076622400000005,9,-8675.2880000000005,7.5,8687.2880000000005,9,3.0946076310118701E-2,8.2742519852026797E-2,0.74270583144284885,3.9716409528972862,2.4564507988364923,43.023077290447013,13.010465143878513,797.01145733240969,4.9967698431443646,107.57419794181133,-152437.76470959728,164.23029267498509,2.7680790440921283,42.350688275757584,-153473.94533989902,227.94033206771897,16.934827457595418,2.3678969705561279,6.143102568169394,-153660.00116844568,253.44723562660212]
["Cart. DDR","CH133C (480 V)",498.7,20,377.00622919608168,14.842764928979594,250,1072.5999999999999,250,0.94,18.100000000000001,1536,302,679,46,{"$f":"IF(AQ401<I401,IF(AQ401<0,0,AQ401),I401)","v":164.23029267498509},{"$f":"IF(AU401<I401,IF(AU401<0,0,AU401),I401)","v":230.86818921996112},{"$f":"IF(UAC_V*0.98/L401*1000<I401,IF(UAC_V*0.98/L401*1000<0,0,UAC_V*0.98/L401*1000),I401)","v":250},{"$f":"C401+(E401-C401)/G401*Q401","v":386.31911798060162},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M401,(inertia/gear^2+gear_inertia)/M401),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M401,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M401))","v":0.37251655629139074},{"$f":"IF((C401+(E401-C401)/G401*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X401^2*time1+Y401^2*time2+Z401^2*time3+AA401^2*time4)/time)/(C401+(E401-C401)/G401*mspeed),SQRT((((X401-Y401)*2/PI()+Y401)^2*time1+Y401^2*time2+((Z401-Y401)*2/PI()+Y401)^2*time3+AA401^2*time4)/time)/(C401+(E401-C401)/G401*mspeed)),IF(AccType=1,SQRT((X401^2*time1+Y401^2*time2+Z401^2*time3+AA401^2*time4+AB401^2*time5+AC401^2*time6+AD401^2*time7+AE401^2*time8)/time)/(C401+(E401-C401)/G401*mspeed),SQRT((((X401-Y401)*2/PI()+Y401)^2*time1+Y401^2*time2+((Z401-Y401)*2/PI()+Y401)^2*time3+AA401^2*time4+((AB401-AC401)*2/PI()+AC401)^2*time5+AC401^2*time6+((AD401-AC401)*2/PI()+AC401)^2*time7+AE401^2*time8)/time)/(C401+(E401-C401)/G401*mspeed))))","v":3.7957274171953284E-2},{"$f":"IF(move1,MAX(ABS(X401),ABS(Z401))/H401,MAX(ABS(X401),ABS(Z401),ABS(AB401),ABS(AD401))/H401)","v":9.2329728846255663E-2},{"$f":"IF(AZ401>0,speed/(MIN(AZ401,I401)),\"NA\")","v":0.50929581789406508},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M401+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M401+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-99.032867160493822},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M401+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M401+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":91.076622400000005},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M401+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M401+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-8675.2880000000005},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M401+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M401+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":8687.2880000000005},9,{"$f":"AH401/Irms","v":3.0946076310118701E-2},{"$f":"AI401/Ipeak","v":8.2742519852026797E-2},{"$f":"IF(move1,IF(AccType=1,SQRT((X401^2*time1+Y401^2*time2+Z401^2*time3+AA401^2*time4)/time)/(C401/D401),SQRT((((X401-Y401)*2/PI()+Y401)^2*time1+Y401^2*time2+((Z401-AA401)*2/PI()+AA401)^2*time3+AA401^2*time4)/time)/(C401/D401)),IF(AccType=1,SQRT((X401^2*time1+Y401^2*time2+Z401^2*time3+AA401^2*time4+AB401^2*time5+AC401^2*time6+AD401^2*time7+AE401^2*time8)/time)/(C401/D401),SQRT((((X401-Y401)*2/PI()+Y401)^2*time1+Y401^2*time2+((Z401-AA401)*2/PI()+AA401)^2*time3+AA401^2*time4+((AB401-AC401)*2/PI()+AC401)^2*time5+AC401^2*time6+((AD401-AE401)*2/PI()+AE401)^2*time7+AE401^2*time8)/time)/(C401/D401)))","v":0.74270583144284885},{"$f":"IF(move1,MAX(ABS(X401),ABS(Z401))/(C401/D401),MAX(ABS(X401),ABS(Z401),ABS(AB401),ABS(AD401))/(C401/D401))","v":3.9716409528972862},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X401),ABS(Z401))/(C401/D401),MAX(ABS((X401-Y401)*2/PI()+Y401),ABS((Z401-Y401)*2/PI()+Y401))/(C401/D401)),IF(AccType=1,MAX(ABS(X401),ABS(Z401),ABS(AB401),ABS(AD401))/(C401/D401),MAX(ABS((X401-Y401)*2/PI()+Y401),ABS((Z401-Y401)*2/PI()+Y401),ABS((AB401-AC401)*2/PI()+AC401),ABS((AD401-AC401)*2/PI()+AC401))/(C401/D401)))","v":2.4564507988364923},{"$f":"IF((C401+(E401-C401)/G401*mspeed)<0,\"NA\",U401*(C401+(E401-C401)/G401*mspeed)*mspeed/9.55)","v":43.023077290447013},{"$f":"IF(move1,IF(speed1>speed2,AM401/2*time1/time,AM401/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z401*-speed/30*PI(),((Z401-AA401)*2/PI()+AA401)*-speed/30*PI()),IF(AccType=1,X401*-speed/30*PI(),((X401-Y401)*2/PI()+Y401)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z401*-speed/30*PI(),((Z401-AA401)*2/PI()+AA401)*-speed/30*PI()),IF(AccType=1,X401*-speed/30*PI(),((X401-Y401)*2/PI()+Y401)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD401*-speed/30*PI(),((AD401-AE401)*2/PI()+AE401)*-speed/30*PI()),IF(AccType=1,AB401*-speed/30*PI(),((AB401-AC401)*2/PI()+AC401)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD401*-speed/30*PI(),((AD401-AE401)*2/PI()+AE401)*-speed/30*PI()),IF(AccType=1,AB401*-speed/30*PI(),((AB401-AC401)*2/PI()+AC401)*-speed/30*PI()),0)/2*time7/time)))","v":13.010465143878513},{"$f":"IF(move1,MAX(IF(AccType=1,Z401*-speed/30*PI(),((Z401-AA401)*2/PI()+AA401)*-speed/30*PI()),IF(AccType=1,X401*-speed/30*PI(),((X401-Y401)*2/PI()+Y401)*-speed/30*PI()),0),MAX(IF(AccType=1,Z401*-speed/30*PI(),((Z401-AA401)*2/PI()+AA401)*-speed/30*PI()),IF(AccType=1,X401*-speed/30*PI(),((X401-Y401)*2/PI()+Y401)*-speed/30*PI()),IF(AccType=1,AD401*-speed/30*PI(),((AD401-AE401)*2/PI()+AE401)*-speed/30*PI()),IF(AccType=1,AB401*-speed/30*PI(),((AB401-AC401)*2/PI()+AC401)*-speed/30*PI()),0))","v":797.01145733240969},{"$f":"(L401^2)/1000000+((K401/1000)^2*(D401/C401*H401)^2*PI()*PI()*(O401/2)^2)/1200","v":4.9967698431443646},{"$f":"SQRT(3)*L401*J401*D401/C401*H401/1000","v":107.57419794181133},{"$f":"0.75*J401^2*(D401/C401*H401)^2-(UAC_V*0.98)^2","v":-152437.76470959728},{"$f":"-AO401/2/AN401+SQRT((AO401/2/AN401)^2-AP401/AN401)","v":164.23029267498509},{"$f":"(L401^2)/1000000+((K401/1000)^2*AV401^2*PI()*PI()*(O401/2)^2)/1200","v":2.7100205273807316},{"$f":"SQRT(3)*L401*J401*AV401/1000","v":39.228084797981012},{"$f":"0.75*J401^2*AV401^2-(UAC_V*0.98)^2","v":-153500.93836668675},{"$f":"-AS401/2/AR401+SQRT((AS401/2/AR401)^2-AT401/AR401)","v":230.86818921996112},{"$f":"D401+(F401-D401)*((0.85*UAC_V-D401*J401)/L401*1000)/G401","v":15.686187747886057},{"$f":"(L401^2)/1000000+((K401/1000)^2*AJ401^2*PI()*PI()*(O401/2)^2)/1200","v":2.3678969705561279},{"$f":"SQRT(3)*L401*J401*AJ401/1000","v":6.143102568169394},{"$f":"0.75*J401^2*AJ401^2-(UAC_V*0.98)^2","v":-153660.00116844568},{"$f":"IF(((AX401/2/AW401)^2-AY401/AW401)>0,-AX401/2/AW401+SQRT((AX401/2/AW401)^2-AY401/AW401),-9999)","v":253.44723562660212}]
["KBM","KBM-10H01-A (120 V)",0.48699999999999999,1.73,0.44870188775305436,1.5599425940517813,4150,1.17,6565,13,19,17.382100000000001,4.9200000000000008E-3,160,6,6565,6565,6565,0.42641515496356674,22865.85365853658,20.359130922104086,24.864760543507693,"NA",-22.508357822103701,9,29.091769835904,9,-2350.3030444800002,7.5,2362.3030444800002,9,1.4669370378561164,2.1530100024004928,35.206488908546795,103.34448011522366,77.408860441793465,23.024003260606882,2.4070034403737761,147.45124779178613,7.6374634761367834E-4,1.6267065951735979,-151474.45449587636,13058.254406887478,3.2787881010026924E-4,0.38413889413729851,-153541.90100647189,21062.109580485896,0.9814813644999717,0.16042360387531007,30.296809620718854,605838.68979320209,-9999]
["KBM","KBM-10H01-A (240 V)",0.48699999999999999,1.73,0.414767427451606,1.4419671375733765,9900,1.17,13766,13,19,17.382100000000001,4.9200000000000008E-3,325,6,13058.254406887478,13766,13766,0.38656024306048564,22865.85365853658,20.357338193050541,24.864760543507693,"NA",-22.508357822103701,9,29.091769835904,9,-2350.3030444800002,7.5,2362.3030444800002,9,1.4669370378561164,2.1530100024004928,35.206488908546795,103.34448011522366,77.408860441793465,23.024003260606882,2.4070034403737761,147.45124779178613,7.6374634761367834E-4,1.6267065951735979,-151474.45449587636,13058.254406887478,3.4052410932198325E-4,0.46909689482150196,-153481.92067414316,20552.6128883659,1.1985504916030405,0.16042360387531007,30.296809620718854,605838.68979320209,-9999]
["KBM","KBM-10H01-A (400 V)",0.48699999999999999,1.73,0.36804580590000802,1.2795362463496316,14400,1.17,16000,13,19,17.382100000000001,4.9200000000000008E-3,565,6,13058.254406887478,16000,16000,0.35482867322223111,22865.85365853658,20.358233003766667,24.864760543507693,"NA",-22.508357822103701,9,29.091769835904,9,-2350.3030444800002,7.5,2362.3030444800002,9,1.4669370378561164,2.1530100024004928,35.206488908546795,103.34448011522366,77.408860441793465,23.024003260606882,2.4070034403737761,147.45124779178613,7.6374634761367834E-4,1.6267065951735979,-151474.45449587636,13058.254406887478,3.380067200498532E-4,0.45345447066345806,-153493.8613836903,20649.747172399973,1.1585838336024141,0.16042360387531007,30.296809620718854,605838.68979320209,-9999]
["KBM","KBM-10H01-B (120 V)",0.50900000000000001,3.37,0.4297183463481174,2.790016532580947,9000,1.19,12319,3.42,5.2,9.3041110000000007,4.9200000000000008E-3,160,6,12319,12319,12319,0.40048103429582871,22865.85365853658,19.478458172725233,24.44686540832269,"NA",-22.508357822103701,9,29.091769835904,9,-2350.3030444800002,7.5,2362.3030444800002,9,2.7340499871209332,4.0127400273001177,65.617199690902396,192.61152131040566,144.27319539442297,23.024003260606882,2.4070034403737761,147.45124779178613,2.1081346565340067E-4,0.43423087158044971,-153119.45768244949,25940.227342568163,8.8965969527187469E-5,6.0344412293786023E-2,-153653.48366610272,41220.68158712962,1.0949024954060449,4.1748459324268954E-2,7.9514671145163094,28929.274491004588,-9999]
["KBM","KBM-10H01-B (240 V)",0.50900000000000001,3.37,0.30970691628693148,2.0108227261844664,18500,1.19,20000,3.42,5.2,9.3041110000000007,4.9200000000000008E-3,325,6,20000,20000,20000,0.29354801760749349,22865.85365853658,19.480126019565066,24.44686540832269,"NA",-22.508357822103701,9,29.091769835904,9,-2350.3030444800002,7.5,2362.3030444800002,9,2.7340499871209332,4.0127400273001177,65.617199690902396,192.61152131040566,144.27319539442297,23.024003260606882,2.4070034403737761,147.45124779178613,2.1081346565340067E-4,0.43423087158044971,-153119.45768244949,25940.227342568163,8.7772488223988214E-5,4.2781167557851635E-2,-153658.71438521615,41597.748286872236,0.77623105992697461,4.1748459324268954E-2,7.9514671145163094,28929.274491004588,-9999]
["KBM","KBM-10H01-C (120 V)",0.49199999999999999,5.21,0.34500684437985052,3.8004719583592257,15500,1.23,19702,1.44,2.2000000000000002,5.8349039999999999,4.9200000000000008E-3,160,6,19702,19702,19702,0.30515747406269778,22865.85365853658,20.152374845196476,23.651845395043903,6.9210509287196978E-2,-22.508357822103701,9,29.091769835904,9,-2350.3030444800002,7.5,2362.3030444800002,9,4.3728738874491153,6.4180267973009757,104.94897329877877,308.06528627044685,230.75236069969139,23.024003260606882,2.4070034403737761,147.45124779178613,9.482626404107243E-5,0.18955470407524055,-153400.15934799999,39233.536220237569,3.4046385710745982E-5,4.0758993057434607E-4,-153663.99878011338,67175.647724479873,2.8007001311999069E-2,1.911054518388261E-2,3.3581723951703011,-70854.806858619166,1839.662152248741]
["KBM","KBM-10H01-C (240 V)",0.49199999999999999,5.21,0.29520674928335428,3.2518919286555881,18600,1.23,20000,1.44,2.2000000000000002,5.8349039999999999,4.9200000000000008E-3,325,6,20000,20000,20000,0.28039435406812285,22865.85365853658,20.153372075360178,23.651845395043903,6.9210509287196978E-2,-22.508357822103701,9,29.091769835904,9,-2350.3030444800002,7.5,2362.3030444800002,9,4.3728738874491153,6.4180267973009757,104.94897329877877,308.06528627044685,230.75236069969139,23.024003260606882,2.4070034403737761,147.45124779178613,9.482626404107243E-5,0.18955470407524055,-153400.15934799999,39233.536220237569,3.4269130472090922E-5,-1.1482360705550997E-2,-153663.03186716529,67130.472523704011,-0.78899518173095462,1.911054518388261E-2,3.3581723951703011,-70854.806858619166,1839.662152248741]
["KBM","KBM-10H02-A (120 V)",0.876,1.53,0.85343954991306192,1.4551398975499776,2070,2.33,3359,20,36,35.4,1.03E-2,160,6,3359,3359,3359,0.83939103775747581,10922.330097087379,11.316847844979018,12.486212054660943,"NA",-22.509721095506173,9,29.092874087359998,9,-2350.4157231999998,7.5,2362.4157231999998,9,0.72124991052682619,1.0586020108842467,17.309997852643829,50.812896522443836,38.060533127157036,23.024221448302207,2.4071923395570511,147.46281961582824,2.8418987989117139E-3,4.9904203768525361,-148695.70075295551,6408.5244608318253,1.3945263648290124E-3,1.488620259018296,-153221.91952433056,9961.9137213821086,1.2139199255160222,0.14022146003486075,46.673326214691194,280917.25457702542,-9999]
["KBM","KBM-10H02-A (240 V)",0.876,1.53,0.79409940026903569,1.3539631718142127,4750,2.33,6753,20,36,35.4,1.03E-2,325,6,6408.5244608318253,6753,6753,0.75956321052985221,10922.330097087379,11.318666775598295,12.486212054660943,"NA",-22.509721095506173,9,29.092874087359998,9,-2350.4157231999998,7.5,2362.4157231999998,9,0.72124991052682619,1.0586020108842467,17.309997852643829,50.812896522443836,38.060533127157036,23.024221448302207,2.4071923395570511,147.46281961582824,2.8418987989117139E-3,4.9904203768525361,-148695.70075295551,6408.5244608318253,1.3927081354739642E-3,1.4790160911392265,-153227.60548576224,9971.5511178805264,1.2060880485240404,0.14022146003486075,46.673326214691194,280917.25457702542,-9999]
["KBM","KBM-10H02-A (400 V)",0.876,1.53,0.70832694452986378,1.2077185754984889,9100,2.33,11291,20,36,35.4,1.03E-2,565,6,6408.5244608318253,9953.8456568124038,11073.446327683616,0.69259431703781527,10922.330097087379,11.319006163505666,12.486212054660943,"NA",-22.509721095506173,9,29.092874087359998,9,-2350.4157231999998,7.5,2362.4157231999998,9,0.72124991052682619,1.0586020108842467,17.309997852643829,50.812896522443836,38.060533127157036,23.024221448302207,2.4071923395570511,147.46281961582824,2.8418987989117139E-3,4.9904203768525361,-148695.70075295551,6408.5244608318253,1.3960546856578299E-3,1.4966454117217529,-153217.1401639799,9953.8456568124038,1.2204641685578708,0.14022146003486075,46.673326214691194,280917.25457702542,-9999]
["KBM","KBM-10H02-A (480 V)",0.876,1.53,0.64240722484365043,1.0953234865194381,11000,2.33,13564,20,36,35.4,1.03E-2,679,6,6408.5244608318253,9997.8587225428309,11073.446327683616,0.66368840321637312,10922.330097087379,11.319812168388957,12.486212054660943,"NA",-22.509721095506173,9,29.092874087359998,9,-2350.4157231999998,7.5,2362.4157231999998,9,0.72124991052682619,1.0586020108842467,17.309997852643829,50.812896522443836,38.060533127157036,23.024221448302207,2.4071923395570511,147.46281961582824,2.8418987989117139E-3,4.9904203768525361,-148695.70075295551,6408.5244608318253,1.3877857103813988E-3,1.4526964789001859,-153242.9988788724,9997.8587225428309,1.1846252869263332,0.14022146003486075,46.673326214691194,280917.25457702542,-9999]
["KBM","KBM-10H02-B (120 V)",0.89900000000000002,2.99,0.82321522288911386,2.6814828107137259,4350,2.48,6174,5.22,9.6999999999999993,18.536100000000001,1.03E-2,160,6,{"$f":"IF(AQ413<I413,IF(AQ413<0,0,AQ413),I413)","v":6174},{"$f":"IF(AU413<I413,IF(AU413<0,0,AU413),I413)","v":6174},{"$f":"IF(UAC_V*0.98/L413*1000<I413,IF(UAC_V*0.98/L413*1000<0,0,UAC_V*0.98/L413*1000),I413)","v":6174},{"$f":"C413+(E413-C413)/G413*Q413","v":0.79143788186606645},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M413,(inertia/gear^2+gear_inertia)/M413),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M413,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M413))","v":10922.330097087379},{"$f":"IF((C413+(E413-C413)/G413*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X413^2*time1+Y413^2*time2+Z413^2*time3+AA413^2*time4)/time)/(C413+(E413-C413)/G413*mspeed),SQRT((((X413-Y413)*2/PI()+Y413)^2*time1+Y413^2*time2+((Z413-Y413)*2/PI()+Y413)^2*time3+AA413^2*time4)/time)/(C413+(E413-C413)/G413*mspeed)),IF(AccType=1,SQRT((X413^2*time1+Y413^2*time2+Z413^2*time3+AA413^2*time4+AB413^2*time5+AC413^2*time6+AD413^2*time7+AE413^2*time8)/time)/(C413+(E413-C413)/G413*mspeed),SQRT((((X413-Y413)*2/PI()+Y413)^2*time1+Y413^2*time2+((Z413-Y413)*2/PI()+Y413)^2*time3+AA413^2*time4+((AB413-AC413)*2/PI()+AC413)^2*time5+AC413^2*time6+((AD413-AC413)*2/PI()+AC413)^2*time7+AE413^2*time8)/time)/(C413+(E413-C413)/G413*mspeed))))","v":11.029015827712424},{"$f":"IF(move1,MAX(ABS(X413),ABS(Z413))/H413,MAX(ABS(X413),ABS(Z413),ABS(AB413),ABS(AD413))/H413)","v":11.730997615870967},{"$f":"IF(AZ413>0,speed/(MIN(AZ413,I413)),\"NA\")","v":0.13160821478503421},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M413+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M413+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.509721095506173},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M413+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M413+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.092874087359998},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M413+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M413+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2350.4157231999998},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M413+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M413+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2362.4157231999998},9,{"$f":"AH413/Irms","v":1.3734407988893134},{"$f":"AI413/Ipeak","v":2.0158438431870223},{"$f":"IF(move1,IF(AccType=1,SQRT((X413^2*time1+Y413^2*time2+Z413^2*time3+AA413^2*time4)/time)/(C413/D413),SQRT((((X413-Y413)*2/PI()+Y413)^2*time1+Y413^2*time2+((Z413-AA413)*2/PI()+AA413)^2*time3+AA413^2*time4)/time)/(C413/D413)),IF(AccType=1,SQRT((X413^2*time1+Y413^2*time2+Z413^2*time3+AA413^2*time4+AB413^2*time5+AC413^2*time6+AD413^2*time7+AE413^2*time8)/time)/(C413/D413),SQRT((((X413-Y413)*2/PI()+Y413)^2*time1+Y413^2*time2+((Z413-AA413)*2/PI()+AA413)^2*time3+AA413^2*time4+((AB413-AC413)*2/PI()+AC413)^2*time5+AC413^2*time6+((AD413-AE413)*2/PI()+AE413)^2*time7+AE413^2*time8)/time)/(C413/D413)))","v":32.962579173343521},{"$f":"IF(move1,MAX(ABS(X413),ABS(Z413))/(C413/D413),MAX(ABS(X413),ABS(Z413),ABS(AB413),ABS(AD413))/(C413/D413))","v":96.760504472977075},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X413),ABS(Z413))/(C413/D413),MAX(ABS((X413-Y413)*2/PI()+Y413),ABS((Z413-Y413)*2/PI()+Y413))/(C413/D413)),IF(AccType=1,MAX(ABS(X413),ABS(Z413),ABS(AB413),ABS(AD413))/(C413/D413),MAX(ABS((X413-Y413)*2/PI()+Y413),ABS((Z413-Y413)*2/PI()+Y413),ABS((AB413-AC413)*2/PI()+AC413),ABS((AD413-AC413)*2/PI()+AC413))/(C413/D413)))","v":72.476804865227734},{"$f":"IF((C413+(E413-C413)/G413*mspeed)<0,\"NA\",U413*(C413+(E413-C413)/G413*mspeed)*mspeed/9.55)","v":23.024221448302207},{"$f":"IF(move1,IF(speed1>speed2,AM413/2*time1/time,AM413/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z413*-speed/30*PI(),((Z413-AA413)*2/PI()+AA413)*-speed/30*PI()),IF(AccType=1,X413*-speed/30*PI(),((X413-Y413)*2/PI()+Y413)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z413*-speed/30*PI(),((Z413-AA413)*2/PI()+AA413)*-speed/30*PI()),IF(AccType=1,X413*-speed/30*PI(),((X413-Y413)*2/PI()+Y413)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD413*-speed/30*PI(),((AD413-AE413)*2/PI()+AE413)*-speed/30*PI()),IF(AccType=1,AB413*-speed/30*PI(),((AB413-AC413)*2/PI()+AC413)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD413*-speed/30*PI(),((AD413-AE413)*2/PI()+AE413)*-speed/30*PI()),IF(AccType=1,AB413*-speed/30*PI(),((AB413-AC413)*2/PI()+AC413)*-speed/30*PI()),0)/2*time7/time)))","v":2.4071923395570511},{"$f":"IF(move1,MAX(IF(AccType=1,Z413*-speed/30*PI(),((Z413-AA413)*2/PI()+AA413)*-speed/30*PI()),IF(AccType=1,X413*-speed/30*PI(),((X413-Y413)*2/PI()+Y413)*-speed/30*PI()),0),MAX(IF(AccType=1,Z413*-speed/30*PI(),((Z413-AA413)*2/PI()+AA413)*-speed/30*PI()),IF(AccType=1,X413*-speed/30*PI(),((X413-Y413)*2/PI()+Y413)*-speed/30*PI()),IF(AccType=1,AD413*-speed/30*PI(),((AD413-AE413)*2/PI()+AE413)*-speed/30*PI()),IF(AccType=1,AB413*-speed/30*PI(),((AB413-AC413)*2/PI()+AC413)*-speed/30*PI()),0))","v":147.46281961582824},{"$f":"(L413^2)/1000000+((K413/1000)^2*(D413/C413*H413)^2*PI()*PI()*(O413/2)^2)/1200","v":8.1742603491368859E-4},{"$f":"SQRT(3)*L413*J413*D413/C413*H413/1000","v":1.3823329860401852},{"$f":"0.75*J413^2*(D413/C413*H413)^2-(UAC_V*0.98)^2","v":-152273.635648},{"$f":"-AO413/2/AN413+SQRT((AO413/2/AN413)^2-AP413/AN413)","v":12829.226322161918},{"$f":"(L413^2)/1000000+((K413/1000)^2*AV413^2*PI()*PI()*(O413/2)^2)/1200","v":3.6488722987117656E-4},{"$f":"SQRT(3)*L413*J413*AV413/1000","v":0.29308214940825628},{"$f":"0.75*J413^2*AV413^2-(UAC_V*0.98)^2","v":-153601.49971222773},{"$f":"-AS413/2/AR413+SQRT((AS413/2/AR413)^2-AT413/AR413)","v":20119.538049342602},{"$f":"D413+(F413-D413)*((0.85*UAC_V-D413*J413)/L413*1000)/G413","v":1.7487989095104577},{"$f":"(L413^2)/1000000+((K413/1000)^2*AJ413^2*PI()*PI()*(O413/2)^2)/1200","v":3.6928544583476441E-2},{"$f":"SQRT(3)*L413*J413*AJ413/1000","v":12.146426691271154},{"$f":"0.75*J413^2*AJ413^2-(UAC_V*0.98)^2","v":-46314.42042622708},{"$f":"IF(((AX413/2/AW413)^2-AY413/AW413)>0,-AX413/2/AW413+SQRT((AX413/2/AW413)^2-AY413/AW413),-9999)","v":967.44686250386621}]
["KBM","KBM-10H02-B (240 V)",0.89900000000000002,2.99,0.70664794732801528,2.301784844716662,10000,2.48,12944,5.22,9.6999999999999993,18.536100000000001,1.03E-2,325,6,12829.226322161918,12944,12944,0.650019503021383,10922.330097087379,11.029509637502374,11.730997615870967,0.13160821478503421,-22.509721095506173,9,29.092874087359998,9,-2350.4157231999998,7.5,2362.4157231999998,9,1.3734407988893134,2.0158438431870223,32.962579173343521,96.760504472977075,72.476804865227734,23.024221448302207,2.4071923395570511,147.46281961582824,8.1742603491368859E-4,1.3823329860401852,-152273.635648,12829.226322161918,3.6579274978514389E-4,0.29924709631147284,-153598.84268626707,20086.669137932673,1.7855846791088543,3.6928544583476441E-2,12.146426691271154,-46314.42042622708,967.44686250386621]
["KBM","KBM-10H02-B (400 V)",0.89900000000000002,2.99,0.49317090918607037,1.6064198996288936,15200,2.48,16000,5.22,9.6999999999999993,18.536000000000001,1.03E-2,565,6,12829.257894707194,16000,16000,0.47181148335375828,10922.330097087379,11.031542638123508,11.730997615870967,0.1316081059789968,-22.509721095506173,9,29.092874087359998,9,-2350.4157231999998,7.5,2362.4157231999998,9,1.3734407988893134,2.0158438431870223,32.962579173343521,96.760504472977075,72.476804865227734,23.024221448302207,2.4071923395570511,147.46281961582824,8.1742232770368856E-4,1.382325528522228,-152273.635648,12829.257894707194,3.5717577991008323E-4,0.23412313253438657,-153624.11619174603,20413.889665184211,1.3970024737225284,3.6928540876266437E-2,12.146361162779771,-46314.42042622708,967.44766233347173]
["KBM","KBM-10H02-C (120 V)",0.86799999999999999,5.14,0.70215416069953829,4.058694570517563,8500,2.2400000000000002,11008,1.77,3.2,10.46,1.03E-2,160,6,11008,11008,11008,0.65321988246829621,10922.330097087379,11.423695106338918,12.987890217571426,4.4811679041663992E-2,-22.509721095506173,9,29.092874087359998,9,-2350.4157231999998,7.5,2362.4157231999998,9,2.4453545805356072,3.5891266515224269,58.688509932854572,172.27807927307649,129.04195572397091,23.024221448302207,2.4071923395570511,147.46281961582824,2.4277718973342478E-4,0.42536033604146428,-153250.58082077836,24263.720089521878,1.1035501930651188E-4,3.5775645240805939E-2,-153661.07550023857,37153.46852293305,1.1156344000935423,1.2731256476991599E-2,4.1380574395818988,-114537.61995145146,2841.3118454038704]
["KBM","KBM-10H02-C (240 V)",0.86799999999999999,5.14,0.25034642399860291,1.4470891560612886,18500,2.2400000000000002,20000,1.77,3.2,10.46,1.03E-2,325,6,20000,20000,20000,0.20026640432281406,10922.330097087379,11.427750023037083,12.987890217571426,4.4811679041663992E-2,-22.509721095506173,9,29.092874087359998,9,-2350.4157231999998,7.5,2362.4157231999998,9,2.4453545805356072,3.5891266515224269,58.688509932854572,172.27807927307649,129.04195572397091,23.024221448302207,2.4071923395570511,147.46281961582824,2.4277718973342478E-4,0.42536033604146428,-153250.58082077836,24263.720089521878,1.1045787917593393E-4,-3.76754880045677E-2,-153660.7566455559,37468.725154718493,-1.1748794515176284,1.2731256476991599E-2,4.1380574395818988,-114537.61995145146,2841.3118454038704]
["KBM","KBM-10H03-A (120 V)",1.1579999999999999,1.54,1.0725659208366858,1.3983910310778171,1380,3.46,2455,21.2,41,46.4,1.55E-2,160,6,2455,2455,2455,1.0060140113435243,7258.0645161290322,8.5688103596019669,8.4086535819653179,"NA",-22.511038757530862,9,29.093941393600002,9,-2350.5246320000001,7.5,2362.5246320000001,9,0.54917984109962215,0.80607134690097881,13.180316186390932,38.691424651246983,28.980991891001882,23.024432343988057,2.4073749186933,147.47400427847106,4.7875027048190433E-3,7.8397593019290408,-146527.10173990889,4773.7712936945718,2.2450492354651745E-3,1.4657319052751316,-153414.5329850367,7946.4806059425755,0.86028048762851783,0.10666232595834731,49.377342706282711,129448.78109366767,-9999]
["KBM","KBM-10H03-A (240 V)",1.1579999999999999,1.54,1.0203357995480415,1.3302943931525966,3650,3.46,5155,21.2,41,46.4,1.55E-2,325,6,4773.7712936945718,5155,5155,0.96357288949867237,7258.0645161290322,8.564835828519703,8.4086535819653179,"NA",-22.511038757530862,9,29.093941393600002,9,-2350.5246320000001,7.5,2362.5246320000001,9,0.54917984109962215,0.80607134690097881,13.180316186390932,38.691424651246983,28.980991891001882,23.024432343988057,2.4073749186933,147.47400427847106,4.7875027048190433E-3,7.8397593019290408,-146527.10173990889,4773.7712936945718,2.3202297222781974E-3,1.9754169488811952,-153210.87127002742,7711.4948014369738,1.1594293949234582,0.10666232595834731,49.377342706282711,129448.78109366767,-9999]
["KBM","KBM-10H03-A (400 V)",1.1579999999999999,1.54,0.98952855922352334,1.290128499639535,6900,3.46,8619,21.2,41,46.4,1.55E-2,565,6,4773.7712936945718,7593.59082106804,8448.2758620689656,0.9725937411170491,7258.0645161290322,8.5626523636927594,8.4086535819653179,"NA",-22.511038757530862,9,29.093941393600002,9,-2350.5246320000001,7.5,2362.5246320000001,9,0.54917984109962215,0.80607134690097881,13.180316186390932,38.691424651246983,28.980991891001882,23.024432343988057,2.4073749186933,147.47400427847106,4.7875027048190433E-3,7.8397593019290408,-146527.10173990889,4773.7712936945718,2.363288768676954E-3,2.2151311656497477,-153094.22558697878,7593.59082106804,1.300124608387089,0.10666232595834731,49.377342706282711,129448.78109366767,-9999]
["KBM","KBM-10H03-A (480 V)",1.1579999999999999,1.54,0.87628839255302382,1.1424881258839945,8500,3.46,10354,21.2,41,46.4,1.55E-2,679,6,4773.7712936945718,7652.6798656519368,8448.2758620689656,0.90437073573765692,7258.0645161290322,8.5640848448607461,8.4086535819653179,"NA",-22.511038757530862,9,29.093941393600002,9,-2350.5246320000001,7.5,2362.5246320000001,9,0.54917984109962215,0.80607134690097881,13.180316186390932,38.691424651246983,28.980991891001882,23.024432343988057,2.4073749186933,147.47400427847106,4.7875027048190433E-3,7.8397593019290408,-146527.10173990889,4773.7712936945718,2.3412799670856801E-3,2.0960338524259736,-153153.84677949012,7652.6798656519368,1.2302229474307746,0.10666232595834731,49.377342706282711,129448.78109366767,-9999]
["KBM","KBM-10H03-B (120 V)",1.17,2.4,1.0672743242632983,2.1431211330588318,2550,3.57,3799,8.77,17,30,1.55E-2,160,6,3799,3799,3799,1.0169588854416747,7258.0645161290322,8.4773416487765303,8.1495634155742298,0.17366993886831819,-22.511038757530862,9,29.093941393600002,9,-2350.5246320000001,7.5,2362.5246320000001,9,0.84708658806974702,1.2433308287863249,20.330078113673927,59.679879781743594,44.701949530176726,23.024432343988057,2.4073749186933,147.47400427847106,2.0472182408516689E-3,3.3371449556365054,-150570.51765140827,7799.6606254813905,9.3778368391033069E-4,0.60562556473237483,-153562.11602092849,12477.656238320184,1.3289930932206606,4.36476041709341E-2,20.370793171877207,-38394.773763500256,733.13755565986094]
["KBM","KBM-10H03-B (240 V)",1.17,2.4,0.98185139021865797,1.971589136985257,6030,3.57,7967,8.77,17,30,1.55E-2,325,6,7799.6606254813905,7967,7967,0.92141293961393833,7258.0645161290322,8.475880769579943,8.1495634155742298,0.17366993886831819,-22.511038757530862,9,29.093941393600002,9,-2350.5246320000001,7.5,2362.5246320000001,9,0.84708658806974702,1.2433308287863249,20.330078113673927,59.679879781743594,44.701949530176726,23.02443234398805,2.4073749186933,147.47400427847106,2.0472182408516689E-3,3.3371449556365054,-150570.51765140827,7799.6606254813905,9.578637725931277E-4,0.74947201712286848,-153507.9699154305,12274.23666877771,1.6446517325578867,4.36476041709341E-2,20.370793171877207,-38394.773763500256,733.13755565986094]
["KBM","KBM-10H03-B (400 V)",1.17,2.4,0.73391973757660023,1.4737344128044181,11450,3.57,13319,8.77,17,30,1.55E-2,565,6,7799.6606254813905,12343.918687793326,13066.666666666666,0.6998742968815701,7258.0645161290322,8.4769879082739905,8.1495634155742298,0.17366993886831819,-22.511038757530862,9,29.093941393600002,9,-2350.5246320000001,7.5,2362.5246320000001,9,0.84708658806974702,1.2433308287863249,20.330078113673927,59.679879781743594,44.701949530176726,23.024432343988057,2.4073749186933,147.47400427847106,2.0472182408516689E-3,3.3371449556365054,-150570.51765140827,7799.6606254813905,9.5072948522776344E-4,0.7017497674183828,-153527.20757331341,12343.918687793326,1.5399293695277867,4.36476041709341E-2,20.370793171877207,-38394.773763500256,733.13755565986094]
["KBM","KBM-10H03-B (480 V)",1.17,2.4,0.49415940372588485,0.99228795928892544,14300,3.57,16000,8.77,17,30,1.55E-2,679,6,7799.6606254813905,12462.657747265937,13066.666666666666,0.58099510188304671,7258.0645161290322,8.4784642116083848,8.1495634155742298,0.17366993886831819,-22.511038757530862,9,29.093941393600002,9,-2350.5246320000001,7.5,2362.5246320000001,9,0.84708658806974702,1.2433308287863249,20.330078113673927,59.679879781743594,44.701949530176726,23.024432343988057,2.4073749186933,147.47400427847106,2.0472182408516689E-3,3.3371449556365054,-150570.51765140827,7799.6606254813905,9.39184061038899E-4,0.61674661113134377,-153558.33989379389,12462.657747265937,1.3533972708417745,4.36476041709341E-2,20.370793171877207,-38394.773763500256,733.13755565986094]
["KBM","KBM-10H03-C (120 V)",1.19,3.05,1.0724594626807715,2.6878683275207305,3250,3.58,4762,5.44,11,24,1.55E-2,160,6,4762,4762,4762,1.0177759880879489,7258.0645161290322,8.334117860347618,8.1267992719553082,8.4136313654528075E-2,-22.511038757530862,9,29.093941393600002,9,-2350.5246320000001,7.5,2362.5246320000001,9,1.0584133366690798,1.5535105260938378,25.401920080057916,74.56850525250421,55.853958998051695,23.024432343988057,2.4073749186933,147.47400427847106,1.3300813298191641E-3,2.074945400814947,-151795.33749289796,9931.3545179129706,5.9747701778112337E-4,0.3501745406040202,-153610.77855517046,15743.942051897709,1.5485092316259543,2.8517795051391528E-2,12.630621783585831,-84422.417256947534,1513.3055982975541]
["KBM","KBM-10H03-C (240 V)",1.19,3.05,0.94236479462306444,2.3618165278773544,7600,3.58,9983,5.44,11,24,1.55E-2,325,6,9931.3545179129706,9983,9983,0.8647181243055333,7258.0645161290322,8.3335608407807609,8.1267992719553082,8.4136313654528075E-2,-22.511038757530862,9,29.093941393600002,9,-2350.5246320000001,7.5,2362.5246320000001,9,1.0584133366690798,1.5535105260938378,25.401920080057916,74.56850525250421,55.853958998051695,23.024432343988057,2.4073749186933,147.47400427847106,1.3300813298191641E-3,2.074945400814947,-151795.33749289796,9931.3545179129706,6.0598850183207103E-4,0.41378521054568701,-153589.6865449365,15582.458591118722,1.8298024103495585,2.8517795051391528E-2,12.630621783585831,-84422.417256947534,1513.3055982975541]
["KBM","KBM-10H03-C (400 V)",1.19,3.05,0.47746482927568601,1.1966537074578596,14500,3.58,16000,5.44,11,24,1.55E-2,565,6,9931.3545179129706,15860.287787619554,16000,0.41061980231115502,7258.0645161290322,8.3361355971865727,8.1267992719553082,8.4136313654528075E-2,-22.511038757530862,9,29.093941393600002,9,-2350.5246320000001,7.5,2362.5246320000001,9,1.0584133366690798,1.5535105260938378,25.401920080057916,74.56850525250421,55.853958998051695,23.024432343988057,2.4073749186933,147.47400427847106,1.3300813298191641E-3,2.074945400814947,-151795.33749289796,9931.3545179129706,5.9178687787578017E-4,0.30022420529412086,-153624.87909138695,15860.287787619554,1.3276235121308375,2.8517795051391528E-2,12.630621783585831,-84422.417256947534,1513.3055982975541]
["KBM","KBM-10H03-D (120 V)",1.18,4.66,1.0070167308359925,3.888095485853253,5500,15.5,7333,2.34,4.7,15.7,1.55E-2,160,6,4362.3892199889115,7333,7333,0.94936612494915151,7258.0645161290322,8.404048540728061,1.8770284770064518,4.3243912539601762E-2,-22.511038757530862,9,29.093941393600002,9,-2350.5246320000001,7.5,2362.5246320000001,9,1.6308211495317355,2.3936752629621476,39.139707588761652,114.89641262218308,86.060723597609311,23.024432343988057,2.4073749186933,147.47400427847106,6.3732086860845052E-3,3.895038410101912,-138276.63721026285,4362.3892199889115,2.5131691137003095E-4,0.10932826023173861,-153651.87712636893,24509.685810481686,1.7181311033487874,1.2357119312661207E-2,5.4762230698649548,-123247.93939823,2944.3208765376162]
["KBM","KBM-10H03-D (240 V)",1.18,4.66,0.62437708443743556,2.4107223337352726,13000,15.5,15373,2.34,4.7,15.7,1.55E-2,325,6,4362.3892199889115,15373,15373,0.52295453223513055,7258.0645161290322,8.4058337085353649,1.8770284770064518,4.3243912539601762E-2,-22.511038757530862,9,29.093941393600002,9,-2350.5246320000001,7.5,2362.5246320000001,9,1.6308211495317355,2.3936752629621476,39.139707588761652,114.89641262218308,86.060723597609311,23.02443234398805,2.4073749186933,147.47400427847106,6.3732086860845052E-3,3.895038410101912,-138276.63721026285,4362.3892199889115,2.4823556411030754E-4,6.5745446151779158E-2,-153659.61598473601,24747.783383157002,1.033212233483634,1.2357119312661207E-2,5.4762230698649548,-123247.93939823,2944.3208765376162]
["KBM","KBM-10H04-A (120 V)",1.44,1.6,1.3285977858106046,1.4285997696888222,1150,4.66,2022,20.399999999999999,44,56.2,2.01E-2,160,6,2022,2022,2022,1.244125846007863,5597.0149253731342,6.8929219314796359,6.2435376714849786,"NA",-22.51220438162963,9,29.094885549120001,9,-2350.6209744000003,7.5,2362.6209744000003,9,0.4588422865287709,0.67349272104444458,11.012214876690502,32.32765061013334,24.214223848925975,23.024618912070828,2.4075364310061378,147.48389840311674,7.0004029838826405E-3,10.281832335505445,-145296.25546666665,3880.2457845585423,3.2467208620977754E-3,1.5585732290054541,-153471.72545068353,6639.4666855984187,0.78487428766140122,8.7183236172635487E-2,48.08367613179157,29340.894057432073,-9999]
["KBM","KBM-10H04-A (240 V)",1.44,1.6,1.2891550390443522,1.3861882140261852,3000,4.66,4251,20.399999999999999,44,56.2,2.01E-2,325,6,3880.2457845585423,4251,4251,1.2262526903258473,5597.0149253731342,6.8879703119595019,6.2435376714849786,"NA",-22.51220438162963,9,29.094885549120001,9,-2350.6209744000003,7.5,2362.6209744000003,9,0.4588422865287709,0.67349272104444458,11.012214876690502,32.32765061013334,24.214223848925975,23.024618912070828,2.4075364310061378,147.48389840311674,7.0004029838826405E-3,10.281832335505445,-145296.25546666665,3880.2457845585423,3.3683309970382953E-3,2.403205087782319,-153206.86018620405,6396.912812400049,1.2102183242176054,8.7183236172635487E-2,48.08367613179157,29340.894057432073,-9999]
["KBM","KBM-10H04-A (400 V)",1.44,1.6,1.1791305349069114,1.2678822955988294,5750,4.66,7109,20.399999999999999,44,56.2,2.01E-2,565,6,3880.2457845585423,6351.5911283913847,6975.0889679715301,1.1518371860602665,5597.0149253731342,6.8874485620778785,6.2435376714849786,"NA",-22.51220438162963,9,29.094885549120001,9,-2350.6209744000003,7.5,2362.6209744000003,9,0.4588422865287709,0.67349272104444458,11.012214876690502,32.32765061013334,24.214223848925975,23.024618912070828,2.4075364310061378,147.48389840311674,7.0004029838826405E-3,10.281832335505445,-145296.25546666665,3880.2457845585423,3.3947440386239078E-3,2.5499372986951294,-153149.33293118782,6351.5911283913847,1.2841104823619254,8.7183236172635487E-2,48.08367613179157,29340.894057432073,-9999]
["KBM","KBM-10H04-A (480 V)",1.44,1.6,1.1106983262583334,1.1942992755465951,7050,4.66,8541,20.399999999999999,44,56.2,2.01E-2,679,6,3880.2457845585423,6350.8688602603361,6975.0889679715301,1.1433543623549562,5597.0149253731342,6.8875909485942888,6.2435376714849786,"NA",-22.51220438162963,9,29.094885549120001,9,-2350.6209744000003,7.5,2362.6209744000003,9,0.4588422865287709,0.67349272104444458,11.012214876690502,32.32765061013334,24.214223848925975,23.024618912070828,2.4075364310061378,147.48389840311674,7.0004029838826405E-3,10.281832335505445,-145296.25546666665,3880.2457845585423,3.3951737718109568E-3,2.5522548531256102,-153148.39697799363,6350.8688602603361,1.2852775682895472,8.7183236172635487E-2,48.08367613179157,29340.894057432073,-9999]
["KBM","KBM-10H04-B (120 V)",1.41,2.4,1.2732395447351628,2.1115083660616301,2100,4.75,3131,9.02,19,36.4,2.01E-2,160,6,3131,3131,3131,1.2060966736027594,5597.0149253731342,7.0362834721296448,6.1252390629726321,0.11534569941398465,-22.51220438162963,9,29.094885549120001,9,-2350.6209744000003,7.5,2362.6209744000003,9,0.70290733255471283,1.0317335301106383,16.869775981313108,49.523209445310634,37.094130151546167,23.024618912070828,2.4075364310061378,147.48389840311674,3.0717459418121767E-3,4.5978445844263867,-149675.16735174286,6272.0276700584254,1.3633441210829955E-3,0.68156965042168161,-153576.3488278182,10366.500175523484,1.1985100909530624,3.8093686956725256E-2,21.094718777028483,-69701.623724127858,1103.8465683626464]
["KBM","KBM-10H04-B (240 V)",1.41,2.4,1.1888682496021099,1.971589136985257,4980,4.75,6571,9.02,19,36.4,2.01E-2,325,6,6272.0276700584254,6571,6571,1.1182215397862378,5597.0149253731342,7.0339878658271937,6.1252390629726321,0.11534569941398465,-22.51220438162963,9,29.094885549120001,9,-2350.6209744000003,7.5,2362.6209744000003,9,0.70290733255471283,1.0317335301106383,16.869775981313108,49.523209445310634,37.094130151546167,23.024618912070828,2.4075364310061378,147.48389840311674,3.0717459418121767E-3,4.5978445844263867,-149675.16735174286,6272.0276700584254,1.3975007832171147E-3,0.93696973579545961,-153498.35117177185,10150.480566385038,1.6476198471773387,3.8093686956725256E-2,21.094718777028483,-69701.623724127858,1103.8465683626464]
["KBM","KBM-10H04-B (400 V)",1.41,2.4,0.90467020283814192,1.5002822600964212,9500,4.75,10987,9.02,19,36.4,2.01E-2,565,6,6272.0276700584254,10189.064900965408,10769.23076923077,0.86801704213959396,5597.0149253731342,7.0349613898427714,6.1252390629726321,0.11534569941398465,-22.51220438162963,9,29.094885549120001,9,-2350.6209744000003,7.5,2362.6209744000003,9,0.70290733255471283,1.0317335301106383,16.869775981313108,49.523209445310634,37.094130151546167,23.024618912070828,2.4075364310061378,147.48389840311674,3.0717459418121767E-3,4.5978445844263867,-149675.16735174286,6272.0276700584254,1.3909694684274138E-3,0.89379425926185718,-153513.26560464289,10189.064900965408,1.5716976809317984,3.8093686956725256E-2,21.094718777028483,-69701.623724127858,1103.8465683626464]
["KBM","KBM-10H04-B (480 V)",1.41,2.4,0.71412130987319988,1.1842807792258705,11500,4.75,13200,9.02,19,36.4,2.01E-2,679,6,6272.0276700584254,10236.830756836338,10769.23076923077,0.79055718451156431,5597.0149253731342,7.0357722795348243,6.1252390629726321,0.11534569941398465,-22.51220438162963,9,29.094885549120001,9,-2350.6209744000003,7.5,2362.6209744000003,9,0.70290733255471283,1.0317335301106383,16.869775981313108,49.523209445310634,37.094130151546167,23.024618912070828,2.4075364310061378,147.48389840311674,3.0717459418121767E-3,4.5978445844263867,-149675.16735174286,6272.0276700584254,1.3831305431620958E-3,0.83904644704639286,-153531.16600118094,10236.830756836338,1.4754260741235412,3.8093686956725256E-2,21.094718777028483,-69701.623724127858,1103.8465683626464]
["KBM","KBM-10H04-C (120 V)",1.44,3.1,1.308607309866695,2.726265228888948,2700,4.8,3944,5.44,11.8,29,2.01E-2,160,6,3944,3944,3944,1.2480693444867574,5597.0149253731342,6.8877985094049947,6.0614344894000007,6.8610075117881225E-2,-22.51220438162963,9,29.094885549120001,9,-2350.6209744000003,7.5,2362.6209744000003,9,0.88900693014949361,1.3048921470236112,21.336166323587847,62.634823057133339,46.915058707294072,23.024618912070828,2.4075364310061378,147.48389840311674,1.9415401765434858E-3,2.8235661324880161,-151294.04586666665,8130.2519753706019,8.6600671035342983E-4,0.42562124246199406,-153610.14939297418,13074.845403846019,1.557635261842389,2.3526562465565549E-2,12.81946169705831,-104811.86022522437,1855.7617704798718]
["KBM","KBM-10H04-C (240 V)",1.44,3.1,1.1519786357127662,2.3999554910682628,6300,4.8,8273,5.44,11.8,29,2.01E-2,325,6,8130.2519753706019,8273,8273,1.061777659246304,5597.0149253731342,6.8874856300077214,6.0614344894000007,6.8610075117881225E-2,-22.51220438162963,9,29.094885549120001,9,-2350.6209744000003,7.5,2362.6209744000003,9,0.88900693014949361,1.3048921470236112,21.336166323587847,62.634823057133339,46.915058707294072,23.024618912070828,2.4075364310061378,147.48389840311674,1.9415401765434858E-3,2.8235661324880161,-151294.04586666665,8130.2519753706019,8.7672855735160238E-4,0.50874804525693984,-153587.0604715955,12948.673366502098,1.8618523128726556,2.3526562465565549E-2,12.81946169705831,-104811.86022522437,1855.7617704798718]
["KBM","KBM-10H04-C (400 V)",1.44,3.1,0.66845076098596046,1.3926057520540844,12000,4.8,13833,5.44,11.8,29,2.01E-2,565,6,8130.2519753706019,13091.75950708416,13517.241379310346,0.59825524291286669,5597.0149253731342,6.8894589994952566,6.0614344894000007,6.8610075117881225E-2,-22.51220438162963,9,29.094885549120001,9,-2350.6209744000003,7.5,2362.6209744000003,9,0.88900693014949361,1.3048921470236112,21.336166323587847,62.634823057133339,46.915058707294072,23.024618912070828,2.4075364310061378,147.48389840311674,1.9415401765434858E-3,2.8235661324880161,-151294.04586666665,8130.2519753706019,8.6464387787398597E-4,0.41386087058748855,-153613.08417948769,13091.75950708416,1.5145961272866342,2.3526562465565549E-2,12.81946169705831,-104811.86022522437,1855.7617704798718]
["KBM","KBM-10H04-D (120 V)",1.41,4.21,1.2277667038517641,3.5484586816524977,4200,4.91,5489,2.94,6.2,20.9,2.01E-2,160,6,5489,5489,5489,1.1718384374862698,5597.0149253731342,7.0338754414380862,5.9256386047087579,4.3688773687000221E-2,-22.51220438162963,9,29.094885549120001,9,-2350.6209744000003,7.5,2362.6209744000003,9,1.2330166125230588,1.8098325674024114,29.59239870055341,86.871963235315746,65.069286640837234,23.024618912070828,2.4075364310061378,147.48389840311674,1.048361926170838E-3,1.5602662671762528,-152270.69923737546,11330.624690495149,4.4543386133887215E-4,0.18528187306995139,-153644.35222837829,18365.527954287223,1.74091949505085,1.2484297348203289E-2,6.925167615397255,-126216.16999304794,2914.3403151048401]
["KBM","KBM-10H04-D (240 V)",1.41,4.21,0.909696148409465,2.629179619680535,9500,4.91,11509,2.94,6.2,20.9,2.01E-2,325,6,{"$f":"IF(AQ443<I443,IF(AQ443<0,0,AQ443),I443)","v":11330.624690495149},{"$f":"IF(AU443<I443,IF(AU443<0,0,AU443),I443)","v":11509},{"$f":"IF(UAC_V*0.98/L443*1000<I443,IF(UAC_V*0.98/L443*1000<0,0,UAC_V*0.98/L443*1000),I443)","v":11509},{"$f":"C443+(E443-C443)/G443*Q443","v":0.80389504968889824},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M443,(inertia/gear^2+gear_inertia)/M443),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M443,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M443))","v":5597.0149253731342},{"$f":"IF((C443+(E443-C443)/G443*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X443^2*time1+Y443^2*time2+Z443^2*time3+AA443^2*time4)/time)/(C443+(E443-C443)/G443*mspeed),SQRT((((X443-Y443)*2/PI()+Y443)^2*time1+Y443^2*time2+((Z443-Y443)*2/PI()+Y443)^2*time3+AA443^2*time4)/time)/(C443+(E443-C443)/G443*mspeed)),IF(AccType=1,SQRT((X443^2*time1+Y443^2*time2+Z443^2*time3+AA443^2*time4+AB443^2*time5+AC443^2*time6+AD443^2*time7+AE443^2*time8)/time)/(C443+(E443-C443)/G443*mspeed),SQRT((((X443-Y443)*2/PI()+Y443)^2*time1+Y443^2*time2+((Z443-Y443)*2/PI()+Y443)^2*time3+AA443^2*time4+((AB443-AC443)*2/PI()+AC443)^2*time5+AC443^2*time6+((AD443-AC443)*2/PI()+AC443)^2*time7+AE443^2*time8)/time)/(C443+(E443-C443)/G443*mspeed))))","v":7.0349027793404604},{"$f":"IF(move1,MAX(ABS(X443),ABS(Z443))/H443,MAX(ABS(X443),ABS(Z443),ABS(AB443),ABS(AD443))/H443)","v":5.9256386047087579},{"$f":"IF(AZ443>0,speed/(MIN(AZ443,I443)),\"NA\")","v":4.3688773687000221E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M443+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M443+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.51220438162963},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M443+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M443+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.094885549120001},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M443+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M443+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2350.6209744000003},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M443+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M443+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2362.6209744000003},9,{"$f":"AH443/Irms","v":1.2330166125230588},{"$f":"AI443/Ipeak","v":1.8098325674024114},{"$f":"IF(move1,IF(AccType=1,SQRT((X443^2*time1+Y443^2*time2+Z443^2*time3+AA443^2*time4)/time)/(C443/D443),SQRT((((X443-Y443)*2/PI()+Y443)^2*time1+Y443^2*time2+((Z443-AA443)*2/PI()+AA443)^2*time3+AA443^2*time4)/time)/(C443/D443)),IF(AccType=1,SQRT((X443^2*time1+Y443^2*time2+Z443^2*time3+AA443^2*time4+AB443^2*time5+AC443^2*time6+AD443^2*time7+AE443^2*time8)/time)/(C443/D443),SQRT((((X443-Y443)*2/PI()+Y443)^2*time1+Y443^2*time2+((Z443-AA443)*2/PI()+AA443)^2*time3+AA443^2*time4+((AB443-AC443)*2/PI()+AC443)^2*time5+AC443^2*time6+((AD443-AE443)*2/PI()+AE443)^2*time7+AE443^2*time8)/time)/(C443/D443)))","v":29.59239870055341},{"$f":"IF(move1,MAX(ABS(X443),ABS(Z443))/(C443/D443),MAX(ABS(X443),ABS(Z443),ABS(AB443),ABS(AD443))/(C443/D443))","v":86.871963235315746},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X443),ABS(Z443))/(C443/D443),MAX(ABS((X443-Y443)*2/PI()+Y443),ABS((Z443-Y443)*2/PI()+Y443))/(C443/D443)),IF(AccType=1,MAX(ABS(X443),ABS(Z443),ABS(AB443),ABS(AD443))/(C443/D443),MAX(ABS((X443-Y443)*2/PI()+Y443),ABS((Z443-Y443)*2/PI()+Y443),ABS((AB443-AC443)*2/PI()+AC443),ABS((AD443-AC443)*2/PI()+AC443))/(C443/D443)))","v":65.069286640837234},{"$f":"IF((C443+(E443-C443)/G443*mspeed)<0,\"NA\",U443*(C443+(E443-C443)/G443*mspeed)*mspeed/9.55)","v":23.024618912070828},{"$f":"IF(move1,IF(speed1>speed2,AM443/2*time1/time,AM443/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z443*-speed/30*PI(),((Z443-AA443)*2/PI()+AA443)*-speed/30*PI()),IF(AccType=1,X443*-speed/30*PI(),((X443-Y443)*2/PI()+Y443)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z443*-speed/30*PI(),((Z443-AA443)*2/PI()+AA443)*-speed/30*PI()),IF(AccType=1,X443*-speed/30*PI(),((X443-Y443)*2/PI()+Y443)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD443*-speed/30*PI(),((AD443-AE443)*2/PI()+AE443)*-speed/30*PI()),IF(AccType=1,AB443*-speed/30*PI(),((AB443-AC443)*2/PI()+AC443)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD443*-speed/30*PI(),((AD443-AE443)*2/PI()+AE443)*-speed/30*PI()),IF(AccType=1,AB443*-speed/30*PI(),((AB443-AC443)*2/PI()+AC443)*-speed/30*PI()),0)/2*time7/time)))","v":2.4075364310061378},{"$f":"IF(move1,MAX(IF(AccType=1,Z443*-speed/30*PI(),((Z443-AA443)*2/PI()+AA443)*-speed/30*PI()),IF(AccType=1,X443*-speed/30*PI(),((X443-Y443)*2/PI()+Y443)*-speed/30*PI()),0),MAX(IF(AccType=1,Z443*-speed/30*PI(),((Z443-AA443)*2/PI()+AA443)*-speed/30*PI()),IF(AccType=1,X443*-speed/30*PI(),((X443-Y443)*2/PI()+Y443)*-speed/30*PI()),IF(AccType=1,AD443*-speed/30*PI(),((AD443-AE443)*2/PI()+AE443)*-speed/30*PI()),IF(AccType=1,AB443*-speed/30*PI(),((AB443-AC443)*2/PI()+AC443)*-speed/30*PI()),0))","v":147.48389840311674},{"$f":"(L443^2)/1000000+((K443/1000)^2*(D443/C443*H443)^2*PI()*PI()*(O443/2)^2)/1200","v":1.048361926170838E-3},{"$f":"SQRT(3)*L443*J443*D443/C443*H443/1000","v":1.5602662671762528},{"$f":"0.75*J443^2*(D443/C443*H443)^2-(UAC_V*0.98)^2","v":-152270.69923737546},{"$f":"-AO443/2/AN443+SQRT((AO443/2/AN443)^2-AP443/AN443)","v":11330.624690495149},{"$f":"(L443^2)/1000000+((K443/1000)^2*AV443^2*PI()*PI()*(O443/2)^2)/1200","v":4.44108144463453E-4},{"$f":"SQRT(3)*L443*J443*AV443/1000","v":0.17044657463181917},{"$f":"0.75*J443^2*AV443^2-(UAC_V*0.98)^2","v":-153647.37261349114},{"$f":"-AS443/2/AR443+SQRT((AS443/2/AR443)^2-AT443/AR443)","v":18409.317377867999},{"$f":"D443+(F443-D443)*((0.85*UAC_V-D443*J443)/L443*1000)/G443","v":1.6015261489133623},{"$f":"(L443^2)/1000000+((K443/1000)^2*AJ443^2*PI()*PI()*(O443/2)^2)/1200","v":1.2484297348203289E-2},{"$f":"SQRT(3)*L443*J443*AJ443/1000","v":6.925167615397255},{"$f":"0.75*J443^2*AJ443^2-(UAC_V*0.98)^2","v":-126216.16999304794},{"$f":"IF(((AX443/2/AW443)^2-AY443/AW443)>0,-AX443/2/AW443+SQRT((AX443/2/AW443)^2-AY443/AW443),-9999)","v":2914.3403151048401}]
["KBM","KBM-14H01-A (120 V)",1.2,1.53,1.1018419137131217,1.3519532683596587,1300,3.28,2308,21.4,38,49.3,2.41E-2,160,8,2308,2308,2308,1.0257316437306807,4668.0497925311201,8.2707652013130648,8.8706422420487812,"NA",-22.513217967802468,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},29.095706553919999,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},-2350.7047504000002,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},2362.7047504000002,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},0.52652523381384297,0.77285470533850009,12.636605611532232,37.097025856248003,27.786488268200884,23.02478115015731,2.4076768764955609,147.49250198976512,5.7538220217480916E-3,7.6419703522315059,-147657.01057971999,4445.0730180362134,2.5174324218753372E-3,1.2360451909651493,-153506.84982512702,7567.1729183710268,0.67641468762134505,0.14914497756569986,50.775590516073585,111525.38488288183,-9999]
["KBM","KBM-14H01-A (240 V)",1.2,1.53,1.083203791789616,1.3290844071038235,3350,3.28,4849,21.4,38,49.3,2.41E-2,325,8,4445.0730180362134,4849,4849,1.0309418466829396,4668.0497925311201,8.264546570573744,8.8706422420487812,"NA",-22.513217967802468,9,29.095706553919999,9,-2350.7047504000002,7.5,2362.7047504000002,9,0.52652523381384297,0.77285470533850009,12.636605611532232,37.097025856248003,27.786488268200884,23.024781150157313,2.4076768764955609,147.49250198976512,5.7538220217480916E-3,7.6419703522315059,-147657.01057971999,4445.0730180362134,2.6845175235373957E-3,2.1128023417985262,-153204.8401458647,7171.1807961759523,1.1562122052490484,0.14914497756569986,50.775590516073585,111525.38488288183,-9999]
["KBM","KBM-14H01-A (400 V)",1.2,1.53,0.9698504344662372,1.1900005330874077,6400,3.28,8109,21.4,38,49.3,2.41E-2,565,8,4445.0730180362134,7132.6008691266979,7951.3184584178498,0.94350547013199249,4668.0497925311201,8.2647141985490666,8.8706422420487812,"NA",-22.513217967802468,9,29.095706553919999,9,-2350.7047504000002,7.5,2362.7047504000002,9,0.52652523381384297,0.77285470533850009,12.636605611532232,37.097025856248003,27.786488268200884,23.02478115015731,2.4076768764955609,147.49250198976512,5.7538220217480916E-3,7.6419703522315059,-147657.01057971999,4445.0730180362134,2.7036229891806616E-3,2.1908142707132536,-153170.30663274063,7132.6008691266979,1.1989035363697096,0.14914497756569986,50.775590516073585,111525.38488288183,-9999]
["KBM","KBM-14H01-A (480 V)",1.2,1.53,0.89449107256710791,1.0975350583645496,7900,3.28,9741,21.4,38,49.3,2.41E-2,679,8,4445.0730180362134,7141.7496191269238,7951.3184584178498,0.92381414352737568,4668.0497925311201,8.2651287599290253,8.8706422420487812,"NA",-22.513217967802468,9,29.095706553919999,9,-2350.7047504000002,7.5,2362.7047504000002,9,0.52652523381384297,0.77285470533850009,12.636605611532232,37.097025856248003,27.786488268200884,23.02478115015731,2.4076768764955609,147.49250198976512,5.7538220217480916E-3,7.6419703522315059,-147657.01057971999,4445.0730180362134,2.699049099649355E-3,2.1723931189756565,-153178.57402999263,7141.7496191269238,1.1888227256604482,0.14914497756569986,50.775590516073585,111525.38488288183,-9999]
["KBM","KBM-14H01-B (120 V)",1.25,3.25,1.1186318857316073,2.8391672226690541,3500,3.43,5022,4.74,9,23.7,2.41E-2,160,8,5022,5022,5022,1.0615055228983235,4668.0497925311201,7.9341361298641786,8.4827132810262391,8.2637801753461693E-2,-22.513217967802468,9,29.095706553919999,9,-2350.7047504000002,7.5,2362.7047504000002,9,1.0736985160125425,1.5760174383373331,25.768764384301019,75.648837040191992,56.662642742997875,23.02478115015731,2.4076768764955609,147.49250198976512,1.4094217263012007E-3,1.7352209524491575,-152323.8516290932,9798.5633729420624,5.904412583365166E-4,0.31956116301099619,-153618.54817741772,15861.624739946792,1.6423536424624663,3.4784617176517263E-2,11.025140716392816,-99562.214399284887,1540.7471129661635]
["KBM","KBM-14H01-B (240 V)",1.25,3.25,0.93691211782398764,2.377949537624334,7950,3.43,10088,4.74,9,23.7,2.41E-2,325,8,9798.5633729420624,10088,10088,0.85271313768658952,4668.0497925311201,7.9343966026807147,8.4827132810262391,8.2637801753461693E-2,-22.513217967802468,9,29.095706553919999,9,-2350.7047504000002,7.5,2362.7047504000002,9,1.0736985160125425,1.5760174383373331,25.768764384301019,75.648837040191992,56.662642742997875,23.02478115015731,2.4076768764955609,147.49250198976512,1.4094217263012007E-3,1.7352209524491575,-152323.8516290932,9798.5633729420624,5.9424651016313861E-4,0.34005133741149479,-153612.53259267774,15794.351138401822,1.747660908978429,3.4784617176517263E-2,11.025140716392816,-99562.214399284887,1540.7471129661635]
["KBM","KBM-14H01-B (400 V)",1.25,3.25,0.56102117439893107,1.4239116101495712,12000,3.43,12000,4.74,9,23.7,2.41E-2,565,8,9798.5633729420624,12000,12000,0.56102117439893107,4668.0497925311201,7.9369386753968163,8.4827132810262391,8.2637801753461693E-2,-22.513217967802468,9,29.095706553919999,9,-2350.7047504000002,7.5,2362.7047504000002,9,1.0736985160125425,1.5760174383373331,25.768764384301019,75.648837040191992,56.662642742997875,23.02478115015731,2.4076768764955609,147.49250198976512,1.4094217263012007E-3,1.7352209524491575,-152323.8516290932,9798.5633729420624,5.7617741086241493E-4,0.22684068655054646,-153641.09737707867,16133.938252500984,1.165825735219761,3.4784617176517263E-2,11.025140716392816,-99562.214399284887,1540.7471129661635]
["KBM","KBM-14H01-C (120 V)",1.21,6.25,0.91036627448564134,4.5747048969127704,7500,3.59,9539,1.29,2.4,12.1,2.41E-2,160,8,9539,9539,9539,0.82890585230913771,4668.0497925311201,8.1969658285372162,8.1046536361894148,3.5298977579945622E-2,-22.513217967802468,9,29.095706553919999,9,-2350.7047504000002,7.5,2362.7047504000002,9,2.1330628496752673,3.1309945930096421,51.193508392206418,150.28774046446281,112.56882299546623,23.02478115015731,2.4076768764955609,147.49250198976512,4.070488535243762E-4,0.50133128093326429,-153234.84035714401,18796.35970087838,1.4642132823273831E-4,3.3051129574138867E-3,-153663.98134729243,32384.154657159346,0.12225048726151755,9.7514066073061487E-3,3.0433635383984425,-137848.71821109712,3607.0153642595224]
["KBM","KBM-14H01-C (240 V)",1.21,6.25,0.64723010190704111,3.2524125723971915,13500,3.59,12000,1.29,2.4,12.1,2.41E-2,325,8,12000,12000,12000,0.70976009058403655,4668.0497925311201,8.197226865504172,8.1046536361894148,3.5298977579945622E-2,-22.513217967802468,9,29.095706553919999,9,-2350.7047504000002,7.5,2362.7047504000002,9,2.1330628496752673,3.1309945930096421,51.193508392206418,150.28774046446281,112.56882299546623,23.02478115015731,2.4076768764955609,147.49250198976512,4.070488535243762E-4,0.50133128093326429,-153234.84035714401,18796.35970087838,1.4642909359909777E-4,4.2909072292890878E-3,-153663.96856108727,32379.930138514974,0.15871333486435812,9.7514066073061487E-3,3.0433635383984425,-137848.71821109712,3607.0153642595224]
["KBM","KBM-14H02-A (120 V)",2.08,1.59,1.9757165349338732,1.4634937295806467,725,6.67,1461,23.8,47,80.8,4.8800000000000003E-2,160,8,1461,1461,1461,1.8698508379839844,2305.3278688524588,4.7724636839680654,4.3629349712983512,0.32107667006684237,-22.519476862419754,9,29.100776258560003,9,-2351.2220671999999,7.5,2363.2220671999999,9,0.3156906302461282,0.46344385267538474,7.5765751259070768,22.245304928418467,16.661787045075236,23.025783072774679,2.4085441273927497,147.54562913731883,1.4085709989137867E-2,16.982771584944864,-142619.79589675603,2635.7666629768173,6.7841183528351712E-3,3.1225463957515189,-153290.63372487912,4528.9049768064124,0.93747556064576687,8.7229350204959019E-2,55.497130024958537,-35724.756872520302,396.55311750620098]
["KBM","KBM-14H02-A (240 V)",2.08,1.59,1.8621128341751756,1.3793428401297596,2000,6.67,2944,23.8,47,80.8,4.8800000000000003E-2,325,8,2635.7666629768173,2944,2944,1.7592700919058584,2305.3278688524588,4.770685263099752,4.3629349712983512,0.32107667006684237,-22.519476862419754,9,29.100776258560003,9,-2351.2220671999999,7.5,2363.2220671999999,9,0.3156906302461282,0.46344385267538474,7.5765751259070768,22.245304928418467,16.661787045075236,23.025783072774672,2.4085441273927497,147.54562913731883,1.4085709989137867E-2,16.982771584944864,-142619.79589675603,2635.7666629768173,6.9445318265932143E-3,3.9840248528763875,-153056.19906334486,4416.5670559745931,1.1961154324748013,8.7229350204959019E-2,55.497130024958537,-35724.756872520302,396.55311750620098]
["KBM","KBM-14H02-A (400 V)",2.08,1.59,1.7384616860807027,1.2877493970968168,3900,6.67,4924,23.8,47,80.8,4.8800000000000003E-2,565,8,2635.7666629768173,4369.3869483216858,4851.4851485148511,1.6973556278998019,2305.3278688524588,4.769596835704454,4.3629349712983512,0.32107667006684237,-22.519476862419754,9,29.100776258560003,9,-2351.2220671999999,7.5,2363.2220671999999,9,0.3156906302461282,0.46344385267538474,7.5765751259070768,22.245304928418467,16.661787045075236,23.025783072774672,2.4085441273927497,147.54562913731883,1.4085709989137867E-2,16.982771584944864,-142619.79589675603,2635.7666629768173,7.0200483352117465E-3,4.3306501974841325,-152945.83621960433,4369.3869483216858,1.3001820332824954,8.7229350204959019E-2,55.497130024958537,-35724.756872520302,396.55311750620098]
["KBM","KBM-14H02-A (480 V)",2.08,1.59,1.6370222718023522,1.2126090902239646,4900,6.67,5915,23.8,47,80.8,4.8800000000000003E-2,679,8,2635.7666629768173,4368.5616921439205,4851.4851485148511,1.6850662175760844,2305.3278688524588,4.7697409327315397,4.3629349712983512,0.32107667006684237,-22.519476862419754,9,29.100776258560003,9,-2351.2220671999999,7.5,2363.2220671999999,9,0.3156906302461282,0.46344385267538474,7.5765751259070768,22.245304928418467,16.661787045075236,23.025783072774672,2.4085441273927497,147.54562913731883,1.4085709989137867E-2,16.982771584944864,-142619.79589675603,2635.7666629768173,7.021410656907384E-3,4.3366489311474909,-152943.84526823263,4368.5616921439205,1.3019830205190257,8.7229350204959019E-2,55.497130024958537,-35724.756872520302,396.55311750620098]
["KBM","KBM-14H02-B (120 V)",2.08,2.42,1.909859317102744,2.1702946785258455,1350,6.83,2139,10.3,20,53.4,4.8800000000000003E-2,160,8,2139,2139,2139,1.8104215402094588,2305.3278688524588,4.7715558952887216,4.260728588368961,9.2661947090067587E-2,-22.519476862419754,9,29.100776258560003,9,-2351.2220671999999,7.5,2363.2220671999999,9,0.48048511018593093,0.70536737325435894,11.531642644462343,33.857633916209231,25.359449464831489,23.025783072774672,2.4085441273927497,147.54562913731883,6.1754293340383886E-3,7.5702782718222004,-148639.63499340508,4331.2745887798419,2.9444817851330971E-3,1.2657520652780609,-153523.53931437919,7009.0242682484886,1.3286467685095329,3.6703075430612221E-2,24.158998685883432,-102494.00730262404,1374.0694910042969]
["KBM","KBM-14H02-B (240 V)",2.08,2.42,1.7941102675813656,2.0387616677060971,3300,6.83,4489,10.3,20,53.4,4.8800000000000003E-2,325,8,4331.2745887798419,4489,4489,1.6911033306584091,2305.3278688524588,4.7695489354528,4.260728588368961,9.2661947090067587E-2,-22.519476862419754,9,29.100776258560003,9,-2351.2220671999999,7.5,2363.2220671999999,9,0.48048511018593093,0.70536737325435894,11.531642644462343,33.857633916209231,25.359449464831489,23.025783072774672,2.4085441273927497,147.54562913731883,6.1754293340383886E-3,7.5702782718222004,-148639.63499340508,4331.2745887798419,3.0106265293973144E-3,1.6560722317400691,-153423.55483693659,6868.9330114414306,1.7383617846489097,3.6703075430612221E-2,24.158998685883432,-102494.00730262404,1374.0694910042969]
["KBM","KBM-14H02-B (400 V)",2.08,2.42,1.382510102678852,1.5710342075896044,6700,6.83,7505,10.3,20,53.4,4.8800000000000003E-2,565,8,4331.2745887798419,6892.4685496652119,7340.8239700374534,1.3624735550753386,2305.3278688524588,4.7704386711176232,4.260728588368961,9.2661947090067587E-2,-22.519476862419754,9,29.100776258560003,9,-2351.2220671999999,7.5,2363.2220671999999,9,0.48048511018593093,0.70536737325435894,11.531642644462343,33.857633916209231,25.359449464831489,23.025783072774672,2.4085441273927497,147.54562913731883,6.1754293340383886E-3,7.5702782718222004,-148639.63499340508,4331.2745887798419,2.9987787850372545E-3,1.5932043630486481,-153441.46390200124,6892.4685496652119,1.6723700372354156,3.6703075430612221E-2,24.158998685883432,-102494.00730262404,1374.0694910042969]
["KBM","KBM-14H02-B (480 V)",2.08,2.42,1.2401683877290546,1.4092822587830165,7700,6.83,9016,10.3,20,53.4,4.8800000000000003E-2,679,8,4331.2745887798419,6901.9430903502298,7340.8239700374534,1.3272116891725787,2305.3278688524588,4.770691654539899,4.260728588368961,9.2661947090067587E-2,-22.519476862419754,9,29.100776258560003,9,-2351.2220671999999,7.5,2363.2220671999999,9,0.48048511018593093,0.70536737325435894,11.531642644462343,33.857633916209231,25.359449464831489,23.025783072774672,2.4085441273927497,147.54562913731883,6.1754293340383886E-3,7.5702782718222004,-148639.63499340508,4331.2745887798419,2.994089431561812E-3,1.5676248849138976,-153448.55233452906,6901.9430903502298,1.6455195252779806,3.6703075430612221E-2,24.158998685883432,-102494.00730262404,1374.0694910042969]
["KBM","KBM-14H02-C (120 V)",2.11,3.1,1.9098593171027443,2.7322737011484182,1800,6.98,2704,6.3,12.8,42.3,4.8800000000000003E-2,160,8,2704,2704,2704,1.8093442185810114,2305.3278688524588,4.7028890014651976,4.1691656530888253,6.4253052232251417E-2,-22.519476862419754,9,29.100776258560003,9,-2351.2220671999999,7.5,2363.2220671999999,9,0.6067463065447658,0.89072281202148529,14.561911357074379,42.754694977031292,32.023369658304311,23.025783072774672,2.4085441273927497,147.54562913731883,4.0566879184936264E-3,4.7334326853383857,-150533.51458586511,5536.054700105693,1.8412399312701772E-3,0.71648123781986828,-153592.27527061742,8940.8445224476582,1.552255752653448,2.3899480198210258E-2,14.781161862485638,-123137.54173932117,1981.6016523742169]
["KBM","KBM-14H02-C (240 V)",2.11,3.1,1.7301078519636623,2.4751185292756257,4250,6.98,5671,6.3,12.8,42.3,4.8800000000000003E-2,325,8,5536.054700105693,5671,5671,1.6030897949378657,2305.3278688524588,4.7018098481337338,4.1691656530888253,6.4253052232251417E-2,-22.519476862419754,9,29.100776258560003,9,-2351.2220671999999,7.5,2363.2220671999999,9,0.6067463065447658,0.89072281202148529,14.561911357074379,42.754694977031292,32.023369658304311,23.025783072774672,2.4085441273927497,147.54562913731883,4.0566879184936264E-3,4.7334326853383857,-150533.51458586511,5536.054700105693,1.8743352297453885E-3,0.91672128017134991,-153546.58221060882,8809.7547910769063,1.9860755671086621,2.3899480198210258E-2,14.781161862485638,-123137.54173932117,1981.6016523742169]
["KBM","KBM-14H02-C (400 V)",2.11,3.1,1.2055986939211072,1.7247477738499388,8000,6.98,9481,6.3,12.8,42.3,4.8800000000000003E-2,565,8,5536.054700105693,8868.5444085571617,9267.1394799054378,1.1074096067352801,2305.3278688524588,4.7029811310940195,4.1691656530888253,6.4253052232251417E-2,-22.519476862419754,9,29.100776258560003,9,-2351.2220671999999,7.5,2363.2220671999999,9,0.6067463065447658,0.89072281202148529,14.561911357074379,42.754694977031292,32.023369658304311,23.025783072774672,2.4085441273927497,147.54562913731883,4.0566879184936264E-3,4.7334326853383857,-150533.51458586511,5536.054700105693,1.8589609596233233E-3,0.82973274517109807,-153567.8087134549,8868.5444085571617,1.7976150091184686,2.3899480198210258E-2,14.781161862485638,-123137.54173932117,1981.6016523742169]
["KBM","KBM-14H02-C (480 V)",2.11,3.1,0.5496668278490825,0.78636169935491063,10250,6.98,11390,6.3,12.8,42.3,4.8800000000000003E-2,679,8,5536.054700105693,8985.8900392516189,9267.1394799054378,0.74209928687367688,2305.3278688524588,4.7049215765020085,4.1691656530888253,6.4253052232251417E-2,-22.519476862419754,9,29.100776258560003,9,-2351.2220671999999,7.5,2363.2220671999999,9,0.6067463065447658,0.89072281202148529,14.561911357074379,42.754694977031292,32.023369658304311,23.025783072774672,2.4085441273927497,147.54562913731883,4.0566879184936264E-3,4.7334326853383857,-150533.51458586511,5536.054700105693,1.830941692471891E-3,0.64154726836249387,-153606.4935452689,8985.8900392516189,1.3899113966263463,2.3899480198210258E-2,14.781161862485638,-123137.54173932117,1981.6016523742169]
["KBM","KBM-14H02-D (120 V)",2.1749999999999998,5.97,1.8608885653821607,4.975637875353371,3900,7.31,5084,1.69,3.6,22.6,4.8800000000000003E-2,160,8,5084,5084,5084,1.7655275554879244,2305.3278688524588,4.5607558954589802,3.9809543445362525,2.8883352209631275E-2,-22.519476862419754,9,29.100776258560003,9,-2351.2220671999999,7.5,2363.2220671999999,9,1.1335559806677717,1.6640961136360464,27.205343536026522,79.876613454530229,59.827776132704763,23.025783072774672,2.4085441273927497,147.54562913731883,1.1973672377044277E-3,1.3273584470053374,-152801.61823222431,10755.974003784639,5.1937914218352856E-4,0.14871886142139226,-153653.17431878843,17057.428742948701,2.2480723327018768,6.6152474238970506E-3,3.9578436238019949,-145996.73643664827,4408.2125076555194]
["KBM","KBM-14H02-D (240 V)",2.1749999999999998,5.97,1.1051433127055206,2.9549286435976487,8900,7.31,10660,1.69,3.6,22.6,4.8800000000000003E-2,325,8,10660,10660,10660,0.8935761475776236,2305.3278688524588,4.5626035503331455,3.9809543445362525,2.8883352209631275E-2,-22.519476862419754,9,29.100776258560003,9,-2351.2220671999999,7.5,2363.2220671999999,9,1.1335559806677717,1.6640961136360464,27.205343536026522,79.876613454530229,59.827776132704763,23.025783072774672,2.4085441273927497,147.54562913731883,1.1973672377044277E-3,1.3273584470053374,-152801.61823222431,10755.974003784639,5.1255064250706639E-4,6.7785760717655755E-2,-153661.75094498586,17248.681473398992,1.0246668900236191,6.6152474238970506E-3,3.9578436238019949,-145996.73643664827,4408.2125076555194]
["KBM","KBM-14H03-A (120 V)",2.82,1.64,2.5783100780887045,1.4403966916696673,500,10.4,1051,26.6,54,108,7.3099999999999998E-2,160,8,1051,1051,1051,2.3119677841424568,1538.9876880984953,3.5282826525336337,2.7986311406461537,0.20309919202309643,-22.525634398419751,9,29.10576386272,9,-2351.7310063999998,7.5,2363.7310063999998,9,0.24018243133671266,0.35264075601995271,5.7643783520811036,16.92675628895773,12.677855310014287,23.026768941962501,2.4093973337409955,147.59789592620766,2.5701254041447769E-2,30.094982734427266,-134251.53459821941,1773.8287865214879,1.1777763555206391E-2,2.7092844008870518,-153506.67356899669,3497.0226778250926,0.54448833130165464,7.3340196514171077E-2,63.082923275899425,-68370.464141096236,626.90527325700532]
["KBM","KBM-14H03-A (240 V)",2.82,1.64,2.5464790894703255,1.422614016463869,1500,10.4,2217,26.6,54,108,7.3099999999999998E-2,325,8,1773.8287865214879,2217,2217,2.4157360942371411,1538.9876880984953,3.5199144946252789,2.7986311406461537,0.20309919202309643,-22.525634398419751,9,29.10576386272,9,-2351.7310063999998,7.5,2363.7310063999998,9,0.24018243133671266,0.35264075601995271,5.7643783520811036,16.92675628895773,12.677855310014287,23.026768941962501,2.4093973337409955,147.59789592620766,2.5701254041447769E-2,30.094982734427266,-134251.53459821941,1773.8287865214879,1.2256210949961044E-2,6.181462447849241,-152845.01684683276,3288.2207635724017,1.2422963687870101,7.3340196514171077E-2,63.082923275899425,-68370.464141096236,626.90527325700532]
["KBM","KBM-14H03-A (400 V)",2.82,1.64,2.4124538742350454,1.3477395945447181,2850,10.4,3710,26.6,54,108,7.3099999999999998E-2,565,8,1773.8287865214879,3250.367444687759,3629.6296296296296,2.3552018738964802,1538.9876880984953,3.5188236066421603,2.7986311406461537,0.20309919202309643,-22.525634398419751,9,29.10576386272,9,-2351.7310063999998,7.5,2363.7310063999998,9,0.24018243133671266,0.35264075601995271,5.7643783520811036,16.92675628895773,12.677855310014287,23.026768941962501,2.4093973337409955,147.59789592620766,2.5701254041447769E-2,30.094982734427266,-134251.53459821941,1773.8287865214879,1.2372273201658596E-2,6.7601047214501948,-152684.51149166297,3250.367444687759,1.3585868423417329,7.3340196514171077E-2,63.082923275899425,-68370.464141096236,626.90527325700532]
["KBM","KBM-14H03-A (480 V)",2.82,1.64,2.3210095867568072,1.2966534004227974,3600,10.4,4458,26.6,54,108,7.3099999999999998E-2,679,8,1773.8287865214879,3243.8940856336185,3629.6296296296296,2.3703688749145924,1538.9876880984953,3.5187019363818894,2.7986311406461537,0.20309919202309643,-22.525634398419751,9,29.10576386272,9,-2351.7310063999998,7.5,2363.7310063999998,9,0.24018243133671266,0.35264075601995271,5.7643783520811036,16.92675628895773,12.677855310014287,23.026768941962501,2.4093973337409955,147.59789592620766,2.5701254041447769E-2,30.094982734427266,-134251.53459821941,1773.8287865214879,1.2392947278849141E-2,6.8580568075376585,-152655.92079956675,3243.8940856336185,1.3782723976432794,7.3340196514171077E-2,63.082923275899425,-68370.464141096236,626.90527325700532]
["KBM","KBM-14H03-B (120 V)",2.87,2.81,2.6571955716212092,2.5306624491630565,1150,10.4,1789,9.01,19,63.7,7.3099999999999998E-2,160,8,1789,1789,1789,2.5389503283742116,1538.9876880984953,3.4585776703626934,2.7986311406461537,7.1170460857191878E-2,-22.525634398419751,9,29.10576386272,9,-2351.7310063999998,7.5,2363.7310063999998,9,0.40436254406356303,0.59369335405228807,9.7047010575255133,28.497280994509829,21.343983395856039,23.026768941962501,2.4093973337409955,147.59789592620766,8.9833134574440338E-3,10.122379445261004,-147351.13691571791,3525.6325187170551,4.1808368829513399E-3,1.6005296375362674,-153506.17035304374,5871.0334421838224,1.6100481709273635,2.5699652125862931E-2,21.217798712490055,-125926.85262034897,1838.9406216241214]
["KBM","KBM-14H03-B (240 V)",2.87,2.81,2.4794664818526857,2.3613966493835101,2850,10.4,3757,9.01,19,63.7,7.3099999999999998E-2,325,8,3525.6325187170551,3757,3757,2.3551809025686108,1538.9876880984953,3.4572925054999786,2.7986311406461537,6.9237664868736157E-2,-22.525634398419751,9,29.10576386272,9,-2351.7310063999998,7.5,2363.7310063999998,9,0.40436254406356303,0.59369335405228807,9.7047010575255133,28.497280994509829,21.343983395856039,23.026768941962501,2.4093973337409955,147.59789592620766,8.9833134574440338E-3,10.122379445261004,-147351.13691571791,3525.6325187170551,4.2539215581335393E-3,2.0203956968905401,-153412.50230229431,5772.5318953584647,2.0324112219099222,2.5699652125862931E-2,21.217798712490055,-125926.85262034897,1838.9406216241214]
["KBM","KBM-14H03-B (400 V)",2.87,2.81,1.961016263096568,1.8676345362824456,5600,10.4,6283,9.01,19,63.7,7.3099999999999998E-2,565,8,3525.6325187170551,5785.518365878298,6153.8461538461534,1.9309031956893761,1538.9876880984953,3.457969232615381,2.7986311406461537,6.9237664868736157E-2,-22.525634398419751,9,29.10576386272,9,-2351.7310063999998,7.5,2363.7310063999998,9,0.40436254406356303,0.59369335405228807,9.7047010575255133,28.497280994509829,21.343983395856039,23.026768941962501,2.4093973337409955,147.59789592620766,8.9833134574440338E-3,10.122379445261004,-147351.13691571791,3525.6325187170551,4.2436847330842211E-3,1.9669908144777621,-153425.62219980828,5785.518365878298,1.9786887345340294,2.5699652125862931E-2,21.217798712490055,-125926.85262034897,1838.9406216241214]
["KBM","KBM-14H03-B (480 V)",2.87,2.81,1.7923295129733443,1.7069804885460422,6500,10.4,7549,9.01,19,63.7,7.3099999999999998E-2,679,8,3525.6325187170551,5787.199657967335,6153.8461538461534,1.9105085732427458,1538.9876880984953,3.4580622944088968,2.7986311406461537,6.9237664868736157E-2,-22.525634398419751,9,29.10576386272,9,-2351.7310063999998,7.5,2363.7310063999998,9,0.40436254406356303,0.59369335405228807,9.7047010575255133,28.497280994509829,21.343983395856039,23.026768941962501,2.4093973337409955,147.59789592620766,8.9833134574440338E-3,10.122379445261004,-147351.13691571791,3525.6325187170551,4.2423722079214139E-3,1.9600382096684901,-153427.30438110352,5787.199657967335,1.97169478178625,2.5699652125862931E-2,21.217798712490055,-125926.85262034897,1838.9406216241214]
["KBM","KBM-14H03-C (120 V)",2.92,6.04,2.4828171122335672,4.9855765305894924,3000,10.4,3806,1.96,4.0999999999999996,30,7.3099999999999998E-2,160,8,3806,3806,3806,2.365360643053652,1538.9876880984953,3.3982554139204071,2.7986311406461537,3.3453482520629602E-2,-22.525634398419751,9,29.10576386272,9,-2351.7310063999998,7.5,2363.7310063999998,9,0.85428067918308548,1.2542723582393609,20.502736300394051,60.205073195489319,45.092585600653891,23.026768941962501,2.4093973337409955,147.59789592620766,1.9237196708762545E-3,2.190914249130445,-152330.63743137699,8347.3758060706514,9.1066108621379023E-4,0.22358135478538255,-153650.11427160897,12867.191335960953,2.1953189688966304,5.3979691476663165E-3,4.5924357791328996,-147805.53711514999,4824.6284280471318]
["KBM","KBM-14H03-C (240 V)",2.92,6.04,1.7796416363911933,3.573577583114846,6600,10.4,7980,1.96,4.0999999999999996,30,7.3099999999999998E-2,325,8,7980,7980,7980,1.5412030694548065,1538.9876880984953,3.3989548577602915,2.7986311406461537,2.6390416665735494E-2,-22.525634398419751,9,29.10576386272,9,-2351.7310063999998,7.5,2363.7310063999998,9,0.85428067918308548,1.2542723582393609,20.502736300394051,60.205073195489319,45.092585600653891,23.026768941962501,2.4093973337409955,147.59789592620766,1.9237196708762545E-3,2.190914249130445,-152330.63743137699,8347.3758060706514,9.0843049702661507E-4,0.19882062994907795,-153653.01954364072,12896.458968349003,1.9521963302984888,5.3979691476663165E-3,4.5924357791328996,-147805.53711514999,4824.6284280471318]
["KBM","KBM-17H01-A (120 V)",2.08,1.65,1.909859317102744,1.4805110985292589,750,5.95,1460,21.3,66,77.900000000000006,5.1199999999999996E-2,160,10,1460,1460,1460,1.7487928039600082,2197.265625,4.7767199851117503,4.8909695565445377,0.3595669952794579,-22.520085014123456,9,29.101268861439998,9,-2351.2723328000002,7.5,2363.2723328000002,9,0.3276048694559886,0.48094044091923066,7.8625168669437269,23.085141164123073,17.290782495833962,23.025880434977246,2.4086283946864042,147.55079128930785,2.6022022275276519E-2,13.564858363011515,-146083.53895630967,2123.005912046563,6.5934349673397261E-3,2.2003637281399651,-153464.54081150936,4660.4783564736599,0.76562620354535271,0.273846891584901,49.692670468712315,-51933.831046681385,354.10356385618547]
["KBM","KBM-17H01-A (240 V)",2.08,1.65,1.8853739412424524,1.4615301870096529,1950,5.95,3068,21.3,66,77.900000000000006,5.1199999999999996E-2,325,10,2123.005912046563,3068,3068,1.7737883342214584,2197.265625,4.7702400791874293,4.8909695565445377,0.3595669952794579,-22.520085014123456,9,29.101268861439998,9,-2351.2723328000002,7.5,2363.2723328000002,9,0.3276048694559886,0.48094044091923066,7.8625168669437269,23.085141164123073,17.290782495833962,23.02588043497725,2.4086283946864042,147.55079128930785,2.6022022275276519E-2,13.564858363011515,-146083.53895630967,2123.005912046563,7.5170461543337978E-3,3.6549728803868304,-153113.6570454055,4276.6181157833662,1.2717638337173085,0.273846891584901,49.692670468712315,-51933.831046681385,354.10356385618547]
["KBM","KBM-17H01-A (400 V)",2.08,1.65,1.7590809499630535,1.363628643382212,3800,5.95,5132,21.3,66,77.900000000000006,5.1199999999999996E-2,565,10,2123.005912046563,4209.0754494756029,5032.0924261874188,1.7245335540053832,2197.265625,4.7694580537305331,4.8909695565445377,0.3595669952794579,-22.520085014123456,9,29.101268861439998,9,-2351.2723328000002,7.5,2363.2723328000002,9,0.3276048694559886,0.48094044091923066,7.8625168669437269,23.085141164123073,17.290782495833962,23.02588043497725,2.4086283946864042,147.55079128930785,2.6022022275276519E-2,13.564858363011515,-146083.53895630967,2123.005912046563,7.7130743779944303E-3,3.8944231839583949,-153039.18510055548,4209.0754494756029,1.3550816163714758,0.273846891584901,49.692670468712315,-51933.831046681385,354.10356385618547]
["KBM","KBM-17H01-A (480 V)",2.08,1.65,1.6634258568314222,1.2894774083964513,4650,5.95,6166,21.3,66,77.900000000000006,5.1199999999999996E-2,679,10,2123.005912046563,4215.9883150059477,5032.0924261874188,1.7023071570037982,2197.265625,4.769719455990959,4.8909695565445377,0.3595669952794579,-22.520085014123456,9,29.101268861439998,9,-2351.2723328000002,7.5,2363.2723328000002,9,0.3276048694559886,0.48094044091923066,7.8625168669437269,23.085141164123073,17.290782495833962,23.025880434977246,2.4086283946864042,147.55079128930785,2.6022022275276519E-2,13.564858363011515,-146083.53895630967,2123.005912046563,7.6925171116010212E-3,3.8700077340612133,-153046.99489233203,4215.9883150059477,1.3465861535652275,0.273846891584901,49.692670468712315,-51933.831046681385,354.10356385618547]
["KBM","KBM-17H01-B (120 V)",2.0699999999999998,3.11,1.8568076694054458,2.7265898229154857,1800,6.14,2782,6.02,18,41.2,5.1199999999999996E-2,160,10,2782,2782,2782,1.7404994090477501,2197.265625,4.7942678103916823,4.7396203357394135,0.10504265952276617,-22.520085014123456,9,29.101268861439998,9,-2351.2723328000002,7.5,2363.2723328000002,9,0.62046856376428028,0.91087908775239923,14.891245530342728,43.722196212115165,32.747947243171062,23.02588043497725,2.4086283946864042,147.55079128930785,7.3666213224903567E-3,3.9628966775858756,-151351.02427225394,4271.7131351150792,1.8373113690526124E-3,0.62246794037584874,-153606.93372125144,8975.7054282260306,1.4489808766002814,7.314241397388678E-2,14.06819620685509,-124515.08390950903,1212.116630062294]
["KBM","KBM-17H01-B (240 V)",2.0699999999999998,3.11,1.7052315331274501,2.50401106186116,4200,6.14,5838,6.02,18,41.2,5.1199999999999996E-2,325,10,4271.7131351150792,5838,5838,1.5629718310471556,2197.265625,4.7926430392451067,4.7396203357394135,0.10504265952276617,-22.520085014123456,9,29.101268861439998,9,-2351.2723328000002,7.5,2363.2723328000002,9,0.62046856376428028,0.91087908775239923,14.891245530342728,43.722196212115165,32.747947243171062,23.02588043497725,2.4086283946864042,147.55079128930785,7.3666213224903567E-3,3.9628966775858756,-151351.02427225394,4271.7131351150792,1.9599053388811181E-3,0.85268486594442117,-153556.91646823884,8636.6459414378005,1.9848798377855836,7.314241397388678E-2,14.06819620685509,-124515.08390950903,1212.116630062294]
["KBM","KBM-17H01-B (400 V)",2.0699999999999998,3.11,1.0653261508694498,1.5643555813060936,8650,6.14,9600,6.02,18,41.2,5.1199999999999996E-2,565,10,4271.7131351150792,8812.9822130209686,9514.5631067961167,1.0463962124537745,2197.265625,4.7941498435239804,4.7396203357394135,0.10504265952276617,-22.520085014123456,9,29.101268861439998,9,-2351.2723328000002,7.5,2363.2723328000002,9,0.62046856376428028,0.91087908775239923,14.891245530342728,43.722196212115165,32.747947243171062,23.02588043497725,2.4086283946864042,147.55079128930785,7.3666213224903567E-3,3.9628966775858756,-151351.02427225394,4271.7131351150792,1.8937488246923593E-3,0.7374328619459376,-153583.90773961411,8812.9822130209686,1.7165962219533726,7.314241397388678E-2,14.06819620685509,-124515.08390950903,1212.116630062294]
["KBM","KBM-17H01-B (480 V)",2.0699999999999998,3.11,0.71619724391352901,1.0516846459816871,9600,6.14,9600,6.02,18,41.2,5.1199999999999996E-2,679,10,4271.7131351150792,8982.0331538677638,9514.5631067961167,0.80334362094101719,2197.265625,4.7954298727781701,4.7396203357394135,0.10504265952276617,-22.520085014123456,9,29.101268861439998,9,-2351.2723328000002,7.5,2363.2723328000002,9,0.62046856376428028,0.91087908775239923,14.891245530342728,43.722196212115165,32.747947243171062,23.02588043497725,2.4086283946864042,147.55079128930785,7.3666213224903567E-3,3.9628966775858756,-151351.02427225394,4271.7131351150792,1.8352083341529315E-3,0.61777066104835976,-153607.79174084915,8982.0331538677638,1.4380465497440718,7.314241397388678E-2,14.06819620685509,-124515.08390950903,1212.116630062294]
["KBM","KBM-17H01-C (120 V)",2.0699999999999998,6.1,1.7384616860807027,4.8970751720583179,3900,6.35,5468,1.56,5,21.5,5.1199999999999996E-2,160,10,5468,5468,5468,1.605166281920329,2197.265625,4.7925484476748386,4.5828769860535434,5.0683418548307636E-2,-22.520085014123456,9,29.101268861439998,9,-2351.2723328000002,7.5,2363.2723328000002,9,1.216996218315791,1.7866117155272141,29.207909239578985,85.757362345306277,64.232308097538095,23.02588043497725,2.4086283946864042,147.55079128930785,2.2622186719710811E-3,1.0870684727370978,-153024.88812091996,7987.8229923093695,4.7174131636943284E-4,7.8938278714198992E-2,-153660.62993410148,17964.538031892549,1.3588263704534436,2.1670536070373538E-2,3.7314464521083459,-146133.60918066415,2512.1421979884922]
["KBM","KBM-17H01-C (240 V)",2.0699999999999998,6.1,0.90187801085407349,2.5405014390255594,9000,6.35,9600,1.56,5,21.5,5.1199999999999996E-2,325,10,7987.8229923093695,9600,9600,0.82400321157767853,2197.265625,4.7948518939029725,4.5828769860535434,5.0683418548307636E-2,-22.520085014123456,9,29.101268861439998,9,-2351.2723328000002,7.5,2363.2723328000002,9,1.216996218315791,1.7866117155272141,29.207909239578985,85.757362345306277,64.232308097538095,23.02588043497725,2.4086283946864042,147.55079128930785,2.2622186719710811E-3,1.0870684727370978,-153024.88812091996,7987.8229923093695,4.6225218859326825E-4,1.1986902057879855E-3,-153663.99922289985,18231.21840125155,2.0633992635261222E-2,2.1670536070373538E-2,3.7314464521083459,-146133.60918066415,2512.1421979884922]
["KBM","KBM-17H02-A (120 V)",3.58,1.59,3.3104228163114229,1.4330834702646853,375,12.2,812,27.5,97,140,9.5399999999999999E-2,160,10,812,812,812,2.9962755382530011,1179.2452830188679,2.7811914246048737,2.3860935216786889,0.22558207605808417,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,0.18343308105764991,0.26935196772301678,4.4023939453835981,12.928894450704806,9.683295724133048,23.027673819780158,2.4101803173445311,147.6458609217724,7.6400195858433745E-2,36.132273191648366,-137011.68920923583,1123.407414947286,2.0560117020112425E-2,4.6976694321155188,-153382.51915697151,2619.4819340350796,0.70446771719370693,0.20100462985110029,64.572046688814666,-100480.97431655023,564.42407436986332]
["KBM","KBM-17H02-A (240 V)",3.58,1.59,3.2293984816464585,1.3980080007127527,1100,12.2,1710,27.5,97,140,9.5399999999999999E-2,325,10,1123.407414947286,1710,1710,3.0349740032867674,1179.2452830188679,2.774281054611476,2.3860935216786889,0.22558207605808417,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,0.18343308105764991,0.26935196772301678,4.4023939453835981,12.928894450704806,9.683295724133048,23.027673819780158,2.4101803173445311,147.6458609217724,7.6400195858433745E-2,36.132273191648366,-137011.68920923583,1123.407414947286,2.2482521790643348E-2,8.1396675658875957,-152818.92107036783,2432.4049792727496,1.2206335740985117,0.20100462985110029,64.572046688814666,-100480.97431655023,564.42407436986332]
["KBM","KBM-17H02-A (400 V)",3.58,1.59,3.1376260209545084,1.3582796627508693,2100,12.2,2861,27.5,97,140,9.5399999999999999E-2,565,10,1123.407414947286,2379.2045393146518,2800,3.0788103909429911,1179.2452830188679,2.772420526934809,2.3860935216786889,0.22558207605808417,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,0.18343308105764991,0.26935196772301678,4.4023939453835981,12.928894450704806,9.683295724133048,23.027673819780158,2.4101803173445311,147.6458609217724,7.6400195858433745E-2,36.132273191648366,-137011.68920923583,1123.407414947286,2.3159860545850314E-2,9.0455892120288528,-152620.34331386769,2379.2045393146518,1.3564865887126321,0.20100462985110029,64.572046688814666,-100480.97431655023,564.42407436986332]
["KBM","KBM-17H02-A (480 V)",3.58,1.59,3.0667933265015219,1.3276161586586674,2600,12.2,3438,27.5,97,140,9.5399999999999999E-2,679,10,1123.407414947286,2371.3145921646969,2800,3.1119328947449061,1179.2452830188679,2.7721923025296178,2.3860935216786889,0.22558207605808417,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,0.18343308105764991,0.26935196772301678,4.4023939453835981,12.928894450704806,9.683295724133048,23.027673819780158,2.4101803173445311,147.6458609217724,7.6400195858433745E-2,36.132273191648366,-137011.68920923583,1123.407414947286,2.3265330966520854E-2,9.1786110475818141,-152589.42218414808,2371.3145921646969,1.3764346906774634,0.20100462985110029,64.572046688814666,-100480.97431655023,564.42407436986332]
["KBM","KBM-17H02-B (120 V)",3.52,2.99,3.246760839074665,2.7056340325622208,1000,12.3,1565,7.78,27,72.8,9.5399999999999999E-2,160,10,1565,1565,1565,3.0923807131518508,1179.2452830188679,2.8208547226831366,2.3666943873560977,9.0398393495602816E-2,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,0.35082625540617784,0.51515103861147737,8.4198301297482683,24.727249853350912,18.519856719958725,23.027673819780158,2.4101803173445311,147.6458609217724,2.1662477493410739E-2,10.249560421072978,-148708.49715344116,2394.1603770163474,5.7603530886716119E-3,1.7194896838398708,-153524.53141355061,5015.4557158499192,1.752782267567117,5.6711459086774198E-2,18.168088053721792,-138093.74582592171,1408.475853939922]
["KBM","KBM-17H02-B (240 V)",3.52,2.99,3.0516230392837325,2.5430191994031106,2300,12.3,3285,7.78,27,72.8,9.5399999999999999E-2,325,10,2394.1603770163474,3285,3285,2.8510355148030699,1179.2452830188679,2.8196157406098599,2.3666943873560977,9.0398393495602816E-2,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,0.35082625540617784,0.51515103861147737,8.4198301297482683,24.727249853350912,18.519856719958725,23.027673819780158,2.4101803173445311,147.6458609217724,2.1662477493410739E-2,10.249560421072978,-148708.49715344116,2394.1603770163474,5.9891674449140328E-3,2.1037366374156021,-153455.23389387203,4889.2482833707127,2.1444689714327669,5.6711459086774198E-2,18.168088053721792,-138093.74582592171,1408.475853939922]
["KBM","KBM-17H02-B (400 V)",3.52,2.99,2.6043536142310146,2.1702946785258455,4400,12.3,5495,7.78,27,72.8,9.5399999999999999E-2,565,10,2394.1603770163474,4877.4682297245845,5384.6153846153848,2.5049917826703711,1179.2452830188679,2.819695093373892,2.3666943873560977,9.0398393495602816E-2,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,0.35082625540617784,0.51515103861147737,8.4198301297482683,24.727249853350912,18.519856719958725,23.027673819780158,2.4101803173445311,147.6458609217724,2.1662477493410739E-2,10.249560421072978,-148708.49715344116,2394.1603770163474,6.0118473545439271E-3,2.1380646116128297,-153448.36517501326,4877.4682297245845,2.1794616003620866,5.6711459086774198E-2,18.168088053721792,-138093.74582592171,1408.475853939922]
["KBM","KBM-17H02-B (480 V)",3.52,2.99,2.2252489291013626,1.8543741075844689,5450,12.3,6602,7.78,27,72.8,9.5399999999999999E-2,679,10,2394.1603770163474,4909.6193740458875,5384.6153846153848,2.3536266161008053,1179.2452830188679,2.8202195782495485,2.3666943873560977,9.0398393495602816E-2,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,0.35082625540617784,0.51515103861147737,8.4198301297482683,24.727249853350912,18.519856719958725,23.027673819780158,2.4101803173445311,147.6458609217724,2.1662477493410739E-2,10.249560421072978,-148708.49715344116,2394.1603770163474,5.9504768835502006E-3,2.0438448499696094,-153466.9515150105,4909.6193740458875,2.0834175653121987,5.6711459086774198E-2,18.168088053721792,-138093.74582592171,1408.475853939922]
["KBM","KBM-17H02-C (120 V)",3.64,5.27,3.2166051656467265,4.5304298107700376,1900,12.7,2797,2.5099999999999998,9.1999999999999993,43,9.5399999999999999E-2,160,10,2797,2797,2797,3.0167182359546807,1179.2452830188679,2.7268653181150251,2.2921528318488193,4.8291637196096783E-2,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,0.59796091075441582,0.87804199223219781,14.351061858105981,42.146015627145495,31.565911104590597,23.027673819780158,2.4101803173445311,147.6458609217724,7.7328293424558442E-3,3.437286694500266,-152066.52300970949,4217.8431474142853,1.9420247578248891E-3,0.4322002334295148,-153638.74350435688,8783.9501129140008,2.3119699908676874,1.9189867544676362E-2,5.9009391132707556,-148955.90340474193,2636.5632201802291]
["KBM","KBM-17H02-C (240 V)",3.64,5.27,2.6891697281044387,3.7875629973301956,4350,12.7,5622,2.5099999999999998,9.1999999999999993,43,9.5399999999999999E-2,325,10,4217.8431474142853,5622,5622,2.4111338417018744,1179.2452830188679,2.7267944588750992,2.2921528318488193,4.8291637196096783E-2,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,0.59796091075441582,0.87804199223219781,14.351061858105981,42.146015627145495,31.565911104590597,23.027673819780158,2.4101803173445311,147.6458609217724,7.7328293424558442E-3,3.437286694500266,-152066.52300970949,4217.8431474142853,1.9740182218015876E-3,0.50103998048407961,-153630.05718468854,8695.9119911981434,2.6802146540095269,1.9189867544676362E-2,5.9009391132707556,-148955.90340474193,2636.5632201802291]
["KBM","KBM-17H02-C (400 V)",3.64,5.27,0.99787623049680418,1.4054594795729638,7560,12.7,9375,2.5099999999999998,9.1999999999999993,43,9.5399999999999999E-2,565,10,4217.8431474142853,8966.2468526173179,9116.2790697674427,0.50641085548499554,1179.2452830188679,2.728974747426907,2.2921528318488193,4.8291637196096783E-2,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,0.59796091075441582,0.87804199223219781,14.351061858105981,42.146015627145495,31.565911104590597,23.027673819780158,2.4101803173445311,147.6458609217724,7.7328293424558442E-3,3.437286694500266,-152066.52300970949,4217.8431474142853,1.882400105132946E-3,0.2589760723172238,-153654.93177311617,8966.2468526173179,1.38534147193571,1.9189867544676362E-2,5.9009391132707556,-148955.90340474193,2636.5632201802291]
["KBM","KBM-17H02-D (120 V)",3.58,6.5,3.083627022405472,5.4577469423105702,2400,12.8,3365,1.65,3.1,34.200000000000003,9.5399999999999999E-2,160,10,3365,3365,3365,2.8840437209976724,1179.2452830188679,2.7723546004258992,2.2742453878500002,3.7837727926750747E-2,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,0.74988366470108447,1.1011243963519555,17.997207952826027,52.853971024893859,39.585800130103657,23.027673819780158,2.4101803173445311,147.6458609217724,2.236880984939061E-3,2.2714907743900832,-152561.16700477514,7766.345432792582,1.1802650599786523E-3,0.22664462550406314,-153653.02059901552,11314.261773324422,2.3188611650744777,4.2660663232428463E-3,3.8691013420278981,-150464.30924154396,5502.6717769360639]
["KBM","KBM-17H02-D (240 V)",3.58,6.5,2.1997486777344109,3.8933604915653293,5600,12.8,7054,1.65,3.1,34.200000000000003,9.5399999999999999E-2,325,10,7054,7054,7054,1.8413762808461667,1179.2452830188679,2.7730368865255017,2.2742453878500002,2.3138569704844611E-2,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,0.74988366470108447,1.1011243963519555,17.997207952826027,52.853971024893859,39.585800130103657,23.027673819780158,2.4101803173445311,147.6458609217724,2.236880984939061E-3,2.2714907743900832,-152561.16700477514,7766.345432792582,1.1776906258336869E-3,0.19728522027036505,-153655.68088938965,11338.982901982712,2.0184773175656545,4.2660663232428463E-3,3.8691013420278981,-150464.30924154396,5502.6717769360639]
["KBM","KBM-17H02-E (120 V)",3.75,9.33,3.0012074983043124,7.2844842191852246,3500,12.9,4633,0.8,3.1,24.8,9.5399999999999999E-2,160,10,4633,4633,4633,2.7588126684696799,1179.2452830188679,2.6466321543996205,2.2566155786418607,2.7481967294089416E-2,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,1.0275759687444843,1.5088860066588801,24.661823249867624,72.426528319626243,54.244970029359763,23.027673819780158,2.4101803173445311,147.6458609217724,2.650497638264534E-3,1.1029158588490393,-153169.5511057408,7396.6946454182671,6.194475386623636E-4,5.1322690170313684E-2,-153662.92933039871,15708.69104266813,1.4935065012785467,6.4293856071793339E-3,1.8640680758546981,-152251.59194872665,4723.4638418858458]
["KBM","KBM-17H02-E (240 V)",3.75,9.33,1.1013522061959158,2.6731849664949414,7500,12.9,9600,0.8,3.1,24.8,9.5399999999999999E-2,325,10,7396.6946454182671,9600,9600,0.35973082393077238,1179.2452830188679,2.6488165282967553,2.2566155786418607,2.69556322934997E-2,-22.531285141333335,9,29.110340964480002,9,-2352.1980576000001,7.5,2364.1980576000001,9,1.0275759687444843,1.5088860066588801,24.661823249867624,72.426528319626243,54.244970029359763,23.027673819780158,2.4101803173445311,147.6458609217724,2.650497638264534E-3,1.1029158588490393,-153169.5511057408,7396.6946454182671,6.2810372814611998E-4,-8.8357804173731375E-2,-153660.82658788111,15711.544835542602,-2.5712400214066555,6.4293856071793339E-3,1.8640680758546981,-152251.59194872665,4723.4638418858458]
["KBM","KBM-17H03-A (120 V)",4.88,3,4.5018112474564687,2.7283704530039206,700,18.5,1136,8.61,33,100,0.14200000000000002,160,10,1136,1136,1136,4.2662536815864982,792.25352112676046,2.0363793870008098,1.5740489551567567,0.11208094583936291,-22.543093420246912,9,29.119905670399998,9,-2353.1740479999999,7.5,2365.1740479999999,9,0.25392219585196252,0.37294961155737699,6.0941327004471004,17.901581354754097,13.407006004885607,23.029565194145103,2.4118165072963111,147.74609270622588,3.8962277474955669E-2,16.9604331690743,-146472.59266793411,1733.4287755686771,1.0710165384786493E-2,2.655830382414456,-153487.66412449611,3663.6776439709288,1.7808877888605958,5.0248527436390501E-2,19.993811012522741,-143670.18802988812,1503.6290570751598]
["KBM","KBM-17H03-A (240 V)",4.88,3,4.2971834634811747,2.6043536142310151,1700,18.5,2389,8.61,33,100,0.14200000000000002,325,10,1733.4287755686771,2389,2389,4.0609713495626627,792.25352112676046,2.0345486661087824,1.5740489551567567,8.4677769343713807E-2,-22.543093420246912,9,29.119905670399998,9,-2353.1740479999999,7.5,2365.1740479999999,9,0.25392219585196252,0.37294961155737699,6.0941327004471004,17.901581354754097,13.407006004885607,23.029565194145103,2.4118165072963111,147.74609270622588,3.8962277474955669E-2,16.9604331690743,-146472.59266793411,1733.4287755686771,1.1152623091708504E-2,3.3834849023631395,-153377.80074788703,3559.8636344365968,2.2688222057821061,5.0248527436390501E-2,19.993811012522741,-143670.18802988812,1503.6290570751598]
["KBM","KBM-17H03-A (400 V)",4.88,3,3.5950293027816365,2.1788056380494769,3400,18.5,3997,8.61,33,100,0.14200000000000002,565,10,1733.4287755686771,3566.0030291015619,3920,3.532291353356638,792.25352112676046,2.0348738823398707,1.5740489551567567,8.4677769343713807E-2,-22.543093420246912,9,29.119905670399998,9,-2353.1740479999999,7.5,2365.1740479999999,9,0.25392219585196252,0.37294961155737699,6.0941327004471004,17.901581354754097,13.407006004885607,23.029565194145103,2.4118165072963111,147.74609270622588,3.8962277474955669E-2,16.9604331690743,-146472.59266793411,1733.4287755686771,1.1124720508905341E-2,3.3422804769765051,-153384.72903033055,3566.0030291015619,2.241192256782365,5.0248527436390501E-2,19.993811012522741,-143670.18802988812,1503.6290570751598]
["KBM","KBM-17H03-A (480 V)",4.88,3,3.4812625526936092,2.1098560925415812,3950,18.5,4803,8.61,33,100,0.14200000000000002,679,10,1733.4287755686771,3554.6901317259994,3920,3.6212460251099641,792.25352112676046,2.0346531475261997,1.5740489551567567,8.4677769343713807E-2,-22.543093420246912,9,29.119905670399998,9,-2353.1740479999999,7.5,2365.1740479999999,9,0.25392219585196252,0.37294961155737699,6.0941327004471004,17.901581354754097,13.407006004885607,23.029565194145107,2.4118165072963111,147.74609270622588,3.8962277474955669E-2,16.9604331690743,-146472.59266793411,1733.4287755686771,1.1176302341017902E-2,3.4180630192156674,-153371.92112991677,3554.6901317259994,2.2920088318830087,5.0248527436390501E-2,19.993811012522741,-143670.18802988812,1503.6290570751598]
["KBM","KBM-17H03-B (120 V)",4.8899999999999997,5.32,4.3653927248062727,4.5951502366381822,1400,18.8,1998,2.81,11,57,0.14200000000000002,160,10,1998,1998,1998,4.1413104744020952,792.25352112676046,2.0306757849464701,1.5489311526808509,6.3725702939697829E-2,-22.543093420246912,9,29.119905670399998,9,-2353.1740479999999,7.5,2365.1740479999999,9,0.44936785820247516,0.66001149525616909,10.784828596859404,31.680551772296116,23.726470831386383,23.029565194145103,2.4118165072963111,147.74609270622588,1.3656948226580453E-2,5.6741710728172361,-151186.60561991413,3125.9466512272679,3.3884465529413908E-3,0.65678580118015295,-153630.80766477133,6637.2505129270749,2.36745619723597,1.7254872452447424E-2,6.582258701285876,-150330.19501303066,2767.086164809496]
["KBM","KBM-17H03-B (240 V)",4.8899999999999997,5.32,3.8500338614610872,4.0526672225906184,3150,18.8,4194,2.81,11,57,0.14200000000000002,325,10,{"$f":"IF(AQ507<I507,IF(AQ507<0,0,AQ507),I507)","v":3125.9466512272679},{"$f":"IF(AU507<I507,IF(AU507<0,0,AU507),I507)","v":4194},{"$f":"IF(UAC_V*0.98/L507*1000<I507,IF(UAC_V*0.98/L507*1000<0,0,UAC_V*0.98/L507*1000),I507)","v":4194},{"$f":"C507+(E507-C507)/G507*Q507","v":3.5053593698310479},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M507,(inertia/gear^2+gear_inertia)/M507),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M507,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M507))","v":792.25352112676046},{"$f":"IF((C507+(E507-C507)/G507*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X507^2*time1+Y507^2*time2+Z507^2*time3+AA507^2*time4)/time)/(C507+(E507-C507)/G507*mspeed),SQRT((((X507-Y507)*2/PI()+Y507)^2*time1+Y507^2*time2+((Z507-Y507)*2/PI()+Y507)^2*time3+AA507^2*time4)/time)/(C507+(E507-C507)/G507*mspeed)),IF(AccType=1,SQRT((X507^2*time1+Y507^2*time2+Z507^2*time3+AA507^2*time4+AB507^2*time5+AC507^2*time6+AD507^2*time7+AE507^2*time8)/time)/(C507+(E507-C507)/G507*mspeed),SQRT((((X507-Y507)*2/PI()+Y507)^2*time1+Y507^2*time2+((Z507-Y507)*2/PI()+Y507)^2*time3+AA507^2*time4+((AB507-AC507)*2/PI()+AC507)^2*time5+AC507^2*time6+((AD507-AC507)*2/PI()+AC507)^2*time7+AE507^2*time8)/time)/(C507+(E507-C507)/G507*mspeed))))","v":2.0302645228878466},{"$f":"IF(move1,MAX(ABS(X507),ABS(Z507))/H507,MAX(ABS(X507),ABS(Z507),ABS(AB507),ABS(AD507))/H507)","v":1.5489311526808509},{"$f":"IF(AZ507>0,speed/(MIN(AZ507,I507)),\"NA\")","v":4.6013729566054935E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M507+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M507+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.543093420246912},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M507+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M507+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.119905670399998},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M507+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M507+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2353.1740479999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M507+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M507+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2365.1740479999999},9,{"$f":"AH507/Irms","v":0.44936785820247516},{"$f":"AI507/Ipeak","v":0.66001149525616909},{"$f":"IF(move1,IF(AccType=1,SQRT((X507^2*time1+Y507^2*time2+Z507^2*time3+AA507^2*time4)/time)/(C507/D507),SQRT((((X507-Y507)*2/PI()+Y507)^2*time1+Y507^2*time2+((Z507-AA507)*2/PI()+AA507)^2*time3+AA507^2*time4)/time)/(C507/D507)),IF(AccType=1,SQRT((X507^2*time1+Y507^2*time2+Z507^2*time3+AA507^2*time4+AB507^2*time5+AC507^2*time6+AD507^2*time7+AE507^2*time8)/time)/(C507/D507),SQRT((((X507-Y507)*2/PI()+Y507)^2*time1+Y507^2*time2+((Z507-AA507)*2/PI()+AA507)^2*time3+AA507^2*time4+((AB507-AC507)*2/PI()+AC507)^2*time5+AC507^2*time6+((AD507-AE507)*2/PI()+AE507)^2*time7+AE507^2*time8)/time)/(C507/D507)))","v":10.784828596859404},{"$f":"IF(move1,MAX(ABS(X507),ABS(Z507))/(C507/D507),MAX(ABS(X507),ABS(Z507),ABS(AB507),ABS(AD507))/(C507/D507))","v":31.680551772296116},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X507),ABS(Z507))/(C507/D507),MAX(ABS((X507-Y507)*2/PI()+Y507),ABS((Z507-Y507)*2/PI()+Y507))/(C507/D507)),IF(AccType=1,MAX(ABS(X507),ABS(Z507),ABS(AB507),ABS(AD507))/(C507/D507),MAX(ABS((X507-Y507)*2/PI()+Y507),ABS((Z507-Y507)*2/PI()+Y507),ABS((AB507-AC507)*2/PI()+AC507),ABS((AD507-AC507)*2/PI()+AC507))/(C507/D507)))","v":23.726470831386383},{"$f":"IF((C507+(E507-C507)/G507*mspeed)<0,\"NA\",U507*(C507+(E507-C507)/G507*mspeed)*mspeed/9.55)","v":23.029565194145103},{"$f":"IF(move1,IF(speed1>speed2,AM507/2*time1/time,AM507/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z507*-speed/30*PI(),((Z507-AA507)*2/PI()+AA507)*-speed/30*PI()),IF(AccType=1,X507*-speed/30*PI(),((X507-Y507)*2/PI()+Y507)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z507*-speed/30*PI(),((Z507-AA507)*2/PI()+AA507)*-speed/30*PI()),IF(AccType=1,X507*-speed/30*PI(),((X507-Y507)*2/PI()+Y507)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD507*-speed/30*PI(),((AD507-AE507)*2/PI()+AE507)*-speed/30*PI()),IF(AccType=1,AB507*-speed/30*PI(),((AB507-AC507)*2/PI()+AC507)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD507*-speed/30*PI(),((AD507-AE507)*2/PI()+AE507)*-speed/30*PI()),IF(AccType=1,AB507*-speed/30*PI(),((AB507-AC507)*2/PI()+AC507)*-speed/30*PI()),0)/2*time7/time)))","v":2.4118165072963111},{"$f":"IF(move1,MAX(IF(AccType=1,Z507*-speed/30*PI(),((Z507-AA507)*2/PI()+AA507)*-speed/30*PI()),IF(AccType=1,X507*-speed/30*PI(),((X507-Y507)*2/PI()+Y507)*-speed/30*PI()),0),MAX(IF(AccType=1,Z507*-speed/30*PI(),((Z507-AA507)*2/PI()+AA507)*-speed/30*PI()),IF(AccType=1,X507*-speed/30*PI(),((X507-Y507)*2/PI()+Y507)*-speed/30*PI()),IF(AccType=1,AD507*-speed/30*PI(),((AD507-AE507)*2/PI()+AE507)*-speed/30*PI()),IF(AccType=1,AB507*-speed/30*PI(),((AB507-AC507)*2/PI()+AC507)*-speed/30*PI()),0))","v":147.74609270622588},{"$f":"(L507^2)/1000000+((K507/1000)^2*(D507/C507*H507)^2*PI()*PI()*(O507/2)^2)/1200","v":1.3656948226580453E-2},{"$f":"SQRT(3)*L507*J507*D507/C507*H507/1000","v":5.6741710728172361},{"$f":"0.75*J507^2*(D507/C507*H507)^2-(UAC_V*0.98)^2","v":-151186.60561991413},{"$f":"-AO507/2/AN507+SQRT((AO507/2/AN507)^2-AP507/AN507)","v":3125.9466512272679},{"$f":"(L507^2)/1000000+((K507/1000)^2*AV507^2*PI()*PI()*(O507/2)^2)/1200","v":3.4767645167887262E-3},{"$f":"SQRT(3)*L507*J507*AV507/1000","v":0.83938827239097935},{"$f":"0.75*J507^2*AV507^2-(UAC_V*0.98)^2","v":-153609.78542075813},{"$f":"-AS507/2/AR507+SQRT((AS507/2/AR507)^2-AT507/AR507)","v":6527.3227266711574},{"$f":"D507+(F507-D507)*((0.85*UAC_V-D507*J507)/L507*1000)/G507","v":3.0256667604392011},{"$f":"(L507^2)/1000000+((K507/1000)^2*AJ507^2*PI()*PI()*(O507/2)^2)/1200","v":1.7254872452447424E-2},{"$f":"SQRT(3)*L507*J507*AJ507/1000","v":6.582258701285876},{"$f":"0.75*J507^2*AJ507^2-(UAC_V*0.98)^2","v":-150330.19501303066},{"$f":"IF(((AX507/2/AW507)^2-AY507/AW507)>0,-AX507/2/AW507+SQRT((AX507/2/AW507)^2-AY507/AW507),-9999)","v":2767.086164809496}]
["KBM","KBM-17H03-B (400 V)",4.8899999999999997,5.32,1.8011681364546206,1.8959664594259165,6150,18.8,7006,2.81,11,57,0.14200000000000002,565,10,3125.9466512272679,6670.6653373199451,6877.1929824561403,1.5396644479737343,792.25352112676046,2.0318534238077621,1.5489311526808509,4.6013729566054935E-2,-22.543093420246912,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},29.119905670399998,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},-2353.1740479999999,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},2365.1740479999999,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},0.44936785820247516,0.66001149525616909,10.784828596859404,31.680551772296116,23.726470831386383,23.029565194145103,2.4118165072963111,147.74609270622588,1.3656948226580453E-2,5.6741710728172361,-151186.60561991413,3125.9466512272679,3.363475262917753E-3,0.59508045801233156,-153636.75155805569,6670.6653373199451,2.1450325443148244,1.7254872452447424E-2,6.582258701285876,-150330.19501303066,2767.086164809496]
["KBM","KBM-17H03-C (120 V)",5.05,6.14,4.4762327744595565,5.2723589805177342,1600,18.8,2239,2.1,8.8000000000000007,51.34,0.14200000000000002,160,10,2239,2239,2239,4.2470844887593415,792.25352112676046,1.9660920278016047,1.5489311526808509,5.6866437906885337E-2,-22.543093420246912,9,29.119905670399998,9,-2353.1740479999999,7.5,2365.1740479999999,9,0.50219944150175067,0.73760817168422432,12.052786596042017,35.405192240842766,26.515960549543792,23.029565194145103,2.4118165072963111,147.74609270622588,1.0955224928801929E-2,4.2684542281114854,-151935.8973450101,3534.363102979074,2.7505846253614743E-3,0.50138812579135317,-153640.1561506624,7383.1859498492558,2.6849627079425651,1.3831168935810033E-2,4.9515725950923013,-151338.50943801663,3133.6851649825476]
["KBM","KBM-17H03-C (240 V)",5.05,6.14,3.8063629746453294,4.4833486156010949,3575,18.8,4700,2.1,8.8000000000000007,51.34,0.14200000000000002,325,10,3534.363102979074,4700,4700,3.415008665967286,792.25352112676046,1.9659991701473449,1.5489311526808509,4.0630742327372689E-2,-22.543093420246912,9,29.119905670399998,9,-2353.1740479999999,7.5,2365.1740479999999,9,0.50219944150175067,0.73760817168422432,12.052786596042017,35.405192240842766,26.515960549543792,23.029565194145103,2.4118165072963111,147.74609270622588,1.0955224928801929E-2,4.2684542281114854,-151935.8973450101,3534.363102979074,2.7975768830157742E-3,0.59523436676717578,-153630.39497089791,7304.8804551432968,3.187514811471102,1.3831168935810033E-2,4.9515725950923013,-151338.50943801663,3133.6851649825476]
["KBM","KBM-17H03-C (400 V)",5.05,6.14,1.429447174066097,1.6836833616797373,6480,18.8,7200,2.1,8.8000000000000007,51.34,0.14200000000000002,565,10,3534.363102979074,7200,7200,1.0271635267401082,792.25352112676046,1.9678248538003347,1.5489311526808509,4.0630742327372689E-2,-22.543093420246912,9,29.119905670399998,9,-2353.1740479999999,7.5,2365.1740479999999,9,0.50219944150175067,0.73760817168422432,12.052786596042017,35.405192240842766,26.515960549543792,23.029565194145103,2.4118165072963111,147.74609270622588,1.0955224928801929E-2,4.2684542281114854,-151935.8973450101,3534.363102979074,2.6850283901855353E-3,0.32836063356906242,-153653.77341929721,7503.8957196752772,1.7583903777095209,1.3831168935810033E-2,4.9515725950923013,-151338.50943801663,3133.6851649825476]
["KBM","KBM-17H03-D (120 V)",5,10.38,4.0139416156057672,8.0278832312115345,2950,19,3838,0.74,2.9,30,0.14200000000000002,160,10,3838,3838,3838,3.7171213290491307,792.25352112676046,1.9855694307879459,1.5326266142315788,3.3174558226554525E-2,-22.543093420246912,9,29.119905670399998,9,-2353.1740479999999,7.5,2365.1740479999999,9,0.85748509850424348,1.2594359202448,20.579642364101844,60.452924171750404,45.274922998258511,23.029565194145103,2.4118165072963111,147.74609270622588,3.5903972108365162E-3,1.5166820675931789,-153025.0209738448,6320.6504837280818,9.0414252997404547E-4,5.9514005347201734E-2,-153663.01613421319,13003.786341272755,1.5477669823315203,4.4446221296384836E-3,1.7408899661069028,-152822.13947941898,5671.1808853031025]
["KBM","KBM-17H03-D (240 V)",5,10.38,1.4103576495527956,2.8207152991055913,6500,19,8030,0.74,2.9,30,0.14200000000000002,325,10,6320.6504837280818,8030,8030,0.56541106552445353,792.25352112676046,1.9874947686070055,1.5326266142315788,2.2451048035423631E-2,-22.543093420246912,9,29.119905670399998,9,-2353.1740479999999,7.5,2365.1740479999999,9,0.85748509850424348,1.2594359202448,20.579642364101844,60.452924171750404,45.274922998258511,23.029565194145103,2.4118165072963111,147.74609270622588,3.5903972108365162E-3,1.5166820675931789,-153025.0209738448,6320.6504837280818,9.1082957552895841E-4,-9.6225918931582999E-2,-153661.42793681272,13041.5763368015,-2.5025252341517366,4.4446221296384836E-3,1.7408899661069028,-152822.13947941898,5671.1808853031025]
["KBM","KBM-17H04-A (120 V)",5.98,3.15,5.4908455366703892,2.8014518044236678,600,23.7,960,8.64,34,118,0.20300000000000001,160,10,960,960,960,5.1973528586726223,554.18719211822656,1.6629208002759646,1.2292162866497891,0.13262911924324611,-22.558550609382717,9,29.132425993600002,9,-2354.4516320000002,7.5,2366.4516320000002,9,0.21759820431836011,0.31970158124247489,5.2223569036406428,15.345675899638795,11.49207465346929,23.032041975389276,2.413958301010017,147.87729740261364,5.0969185492360604E-2,22.045202524812183,-144938.2215893424,1483.8612147317745,1.454025045470241E-2,2.8433271530470328,-153518.84578247531,3153.0344692275717,1.6101652711137364,4.5315583182935666E-2,20.293399996418568,-146269.89479649093,1586.5968843346568]
["KBM","KBM-17H04-A (240 V)",5.98,3.15,5.2862177526950962,2.6970498738240285,1400,23.7,2018,8.64,34,118,0.20300000000000001,325,10,1483.8612147317745,2018,2018,4.9799624463847882,554.18719211822656,1.6609447905532619,1.2292162866497891,8.0249719213907236E-2,-22.558550609382717,9,29.132425993600002,9,-2354.4516320000002,7.5,2366.4516320000002,9,0.21759820431836011,0.31970158124247489,5.2223569036406428,15.345675899638795,11.49207465346929,23.032041975389276,2.413958301010017,147.87729740261364,5.0969185492360604E-2,22.045202524812183,-144938.2215893424,1483.8612147317745,1.5173099595343102E-2,4.0480581262293462,-153369.78184082641,3048.7104083918875,2.2923998046862888,4.5315583182935666E-2,20.293399996418568,-146269.89479649093,1586.5968843346568]
["KBM","KBM-17H04-A (400 V)",5.98,3.15,4.703912762493796,2.3999554910682632,2700,23.7,3377,8.64,34,118,0.20300000000000001,565,10,1483.8612147317745,3028.7175970716567,3322.0338983050847,4.5485526401357044,554.18719211822656,1.6608032203972798,1.2292162866497891,8.0249719213907236E-2,-22.558550609382717,9,29.132425993600002,9,-2354.4516320000002,7.5,2366.4516320000002,9,0.21759820431836011,0.31970158124247489,5.2223569036406428,15.345675899638795,11.49207465346929,23.032041975389276,2.413958301010017,147.87729740261364,5.0969185492360604E-2,22.045202524812183,-144938.2215893424,1483.8612147317745,1.5308726530424165E-2,4.2621645505985377,-153337.83570352665,3028.7175970716567,2.4136474523486995,4.5315583182935666E-2,20.293399996418568,-146269.89479649093,1586.5968843346568]
["KBM","KBM-17H04-A (480 V)",5.98,3.15,4.332815167158464,2.2106199832441145,3350,23.7,4058,8.64,34,118,0.20300000000000001,679,10,1483.8612147317745,3029.8718976675736,3322.0338983050847,4.4902211834952741,554.18719211822656,1.6609209501559634,1.2292162866497891,8.0249719213907236E-2,-22.558550609382717,9,29.132425993600002,9,-2354.4516320000002,7.5,2366.4516320000002,9,0.21759820431836011,0.31970158124247489,5.2223569036406428,15.345675899638795,11.49207465346929,23.032041975389276,2.413958301010017,147.87729740261364,5.0969185492360604E-2,22.045202524812183,-144938.2215893424,1483.8612147317745,1.5300776386291452E-2,4.2499117347228497,-153339.70831382982,3029.8718976675736,2.4067087296712044,4.5315583182935666E-2,20.293399996418568,-146269.89479649093,1586.5968843346568]
["KBM","KBM-17H04-B (120 V)",6.12,5.53,5.4510568008974154,4.7816287727170312,1200,23.7,1660,2.8,12,69.3,0.20300000000000001,160,10,1660,1660,1660,5.1946285745747582,554.18719211822656,1.6232458124167142,1.2292162866497891,7.6701177393684497E-2,-22.558550609382717,9,29.132425993600002,9,-2354.4516320000002,7.5,2366.4516320000002,9,0.3732670431520686,0.54841474586263617,8.9584090356496464,26.323907801406538,19.713456455308506,23.032041975389276,2.413958301010017,147.87729740261364,1.838140627174089E-2,7.1973719747136995,-150967.36953630333,2676.7424399270685,5.0041301443439802E-3,0.87706118839638625,-153623.95638053431,5453.7661220101918,2.6096243723790291,1.630907780656872E-2,6.6254391739647875,-151378.91225135777,2850.2603248305468]
["KBM","KBM-17H04-B (240 V)",6.12,5.53,4.8647359963937822,4.267312277538406,2650,23.7,3485,2.8,12,69.3,0.20300000000000001,325,10,2676.7424399270685,3485,3485,4.469209414125408,554.18719211822656,1.6227520287028394,1.2292162866497891,4.4670991405350288E-2,-22.558550609382717,9,29.132425993600002,9,-2354.4516320000002,7.5,2366.4516320000002,9,0.3732670431520686,0.54841474586263617,8.9584090356496464,26.323907801406538,19.713456455308506,23.032041975389276,2.413958301010017,147.87729740261364,1.838140627174089E-2,7.1973719747136995,-150967.36953630333,2676.7424399270685,5.1246810023667733E-3,1.1086592816538476,-153600.01624351132,5367.6236505435572,3.2987256993528455,1.630907780656872E-2,6.6254391739647875,-151378.91225135777,2850.2603248305468]
["KBM","KBM-17H04-B (400 V)",6.12,5.53,2.902986161996171,2.5464790894703255,5000,23.7,5822,2.8,12,69.3,0.20300000000000001,565,10,2676.7424399270685,5438.8676694340584,5656.5656565656564,2.6206174888718001,554.18719211822656,1.6237527704951191,1.2292162866497891,4.4670991405350288E-2,-22.558550609382717,9,29.132425993600002,9,-2354.4516320000002,7.5,2366.4516320000002,9,0.3732670431520686,0.54841474586263617,8.9584090356496464,26.323907801406538,19.713456455308506,23.032041975389276,2.413958301010017,147.87729740261364,1.838140627174089E-2,7.1973719747136995,-150967.36953630333,2676.7424399270685,5.02409550952501E-3,0.91945752192389862,-153619.99146824761,5438.8676694340584,2.7357712213522429,1.630907780656872E-2,6.6254391739647875,-151378.91225135777,2850.2603248305468]
["KBM","KBM-17H04-B (480 V)",6.12,5.53,1.8009638297240791,1.5797928330912976,5700,23.7,6987,2.8,12,69.3,0.20300000000000001,679,10,2676.7424399270685,5490.211310280949,5656.5656565656564,1.9599260997260748,554.18719211822656,1.6244275701570734,1.2292162866497891,4.4670991405350288E-2,-22.558550609382717,9,29.132425993600002,9,-2354.4516320000002,7.5,2366.4516320000002,9,0.3732670431520686,0.54841474586263617,8.9584090356496464,26.323907801406538,19.713456455308506,23.032041975389276,2.413958301010017,147.87729740261364,1.838140627174089E-2,7.1973719747136995,-150967.36953630333,2676.7424399270685,4.9570507144434161E-3,0.76787574828483374,-153633.30586191727,5490.211310280949,2.2847519582376532,1.630907780656872E-2,6.6254391739647875,-151378.91225135777,2850.2603248305468]
["KBM","KBM-17H04-C (120 V)",6.1,6.2,5.4052622182153129,5.3517447705102104,1325,23.7,1868,2.23,9.1,61.4,0.20300000000000001,160,10,1868,1868,1868,5.1205508102839286,554.18719211822656,1.6283821770719675,1.2292162866497891,6.8160575199955178E-2,-22.558550609382717,9,29.132425993600002,9,-2354.4516320000002,7.5,2366.4516320000002,9,0.41986318102042786,0.61687514057486348,10.076716344490269,29.610006747593449,22.174351280355321,23.032041975389276,2.413958301010017,147.87729740261364,1.3650068039579633E-2,5.7127347815458362,-151499.82991037812,3128.7999276186952,3.9033685091200386E-3,0.66382710399336098,-153634.77777854432,6189.2616027740032,2.7991174331804727,1.2142228332812498E-2,5.2587773627790781,-151830.11188505465,3326.2177957895346]
["KBM","KBM-17H04-C (240 V)",6.1,6.2,4.6473243382833438,4.601311226023113,3000,23.7,3922,2.23,9.1,61.4,0.20300000000000001,325,10,3128.7999276186952,3922,3922,4.2008686849157586,554.18719211822656,1.628144235048093,1.2292162866497891,3.8278898824571334E-2,-22.558550609382717,9,29.132425993600002,9,-2354.4516320000002,7.5,2366.4516320000002,9,0.41986318102042786,0.61687514057486348,10.076716344490269,29.610006747593449,22.174351280355321,23.032041975389276,2.413958301010017,147.87729740261364,1.3650068039579633E-2,5.7127347815458362,-151499.82991037812,3128.7999276186952,3.9632327342043732E-3,0.79900318502704837,-153621.66492948975,6125.9040607845473,3.3691057971599507,1.2142228332812498E-2,5.2587773627790781,-151830.11188505465,3326.2177957895346]
["KBM","KBM-17H04-C (400 V)",6.1,6.2,1.6122189040477708,1.5962563406413572,5775,23.7,6548,2.23,9.1,61.4,0.20300000000000001,565,10,3128.7999276186952,6268.6504177782617,6384.3648208469058,1.2286007199933628,554.18719211822656,1.6298834778200098,1.2292162866497891,3.8278898824571334E-2,-22.558550609382717,9,29.132425993600002,9,-2354.4516320000002,7.5,2366.4516320000002,9,0.41986318102042786,0.61687514057486348,10.076716344490269,29.610006747593449,22.174351280355321,23.032041975389276,2.413958301010017,147.87729740261364,1.3650068039579633E-2,5.7127347815458362,-151499.82991037812,3128.7999276186952,3.835714235491664E-3,0.46604202599344774,-153649.59698445129,6268.6504177782617,1.9651297027577428,1.2142228332812498E-2,5.2587773627790781,-151830.11188505465,3326.2177957895346]
["KBM","KBM-17H04-D (120 V)",6.07,9.56,5.5993602705966818,8.48387919787376,2200,24,2881,0.94,3.8,40,0.20300000000000001,160,10,2881,2881,2881,5.4536758816313817,554.18719211822656,1.6345875971130004,1.2138510830666667,4.4194361150127134E-2,-22.558550609382717,9,29.132425993600002,9,-2354.4516320000002,7.5,2366.4516320000002,9,0.65060161727127774,0.95588273098165855,15.614438814510667,45.882371087119608,34.360404667726016,23.032041975389276,2.413958301010017,147.87729740261364,5.8421555307359733E-3,2.4616647977020558,-152717.15725371163,4906.440667596582,1.6902127822147339E-3,0.35897950975402926,-153643.86464243388,9428.656244690419,5.5121520369693808,5.1054376036522671E-3,2.2377251461576226,-152881.59158910217,5257.4246667912976]
["KBM","KBM-17H04-D (240 V)",6.07,9.56,3.9629580829881941,6.0044819439215056,5000,24,6037,0.94,3.8,40,0.20300000000000001,325,10,4906.440667596582,6037,6037,3.5259575893999453,554.18719211822656,1.635829096205452,1.2138510830666667,2.421793226591764E-2,-22.558550609382717,9,29.132425993600002,9,-2354.4516320000002,7.5,2366.4516320000002,9,0.65060161727127774,0.95588273098165855,15.614438814510667,45.882371087119608,34.360404667726016,23.032041975389276,2.413958301010017,147.87729740261364,5.8421555307359733E-3,2.4616647977020558,-152717.15725371163,4906.440667596582,1.6401078344869991E-3,0.23935925733914043,-153655.04799155093,9606.4543476589315,3.6753758419622784,5.1054376036522671E-3,2.2377251461576226,-152881.59158910217,5257.4246667912976]
["KBM","KBM-25H01-A (120 V)",4.9000000000000004,3.1,4.4336019861313707,2.6870315067462855,700,14.37,1132,8.98,37,100.3,0.26600000000000001,160,10,1132,1132,1132,4.1457677832867308,422.93233082706763,2.0296515979961161,2.0282085469171891,0.11247699158437832,-22.574514591604942,9,29.145356819200003,9,-2355.7711040000004,7.5,2367.7711040000004,9,0.26137244674179755,0.38414373358639459,6.2729387218031407,18.438899212146939,13.807610339746674,23.034601090365786,2.4161703174684339,148.01280389232554,3.3325286234856297E-2,14.182744492534097,-148665.28126735182,1910.0159915136342,1.0509748274555501E-2,1.9717334935656416,-153567.38722194213,3729.8972859108426,1.2638930239130319,6.372606216464835E-2,21.540531720550998,-142133.42455773099,1333.9700300361328]
["KBM","KBM-25H01-A (240 V)",4.9000000000000004,3.1,4.1090912580089336,2.4903583381872325,1650,14.37,2379,8.98,37,100.3,0.26600000000000001,325,10,1910.0159915136342,2379,2379,3.7596533956383351,422.93233082706763,2.0279298890463142,2.0282085469171891,9.5447387577416179E-2,-22.574514591604942,9,29.145356819200003,9,-2355.7711040000004,7.5,2367.7711040000004,9,0.26137244674179755,0.38414373358639459,6.2729387218031407,18.438899212146939,13.807610339746674,23.034601090365786,2.4161703174684339,148.01280389232554,3.3325286234856297E-2,14.182744492534097,-148665.28126735182,1910.0159915136342,1.1130534747861603E-2,3.0422089999073121,-153434.00614310813,3578.6643497812502,1.9500742594350455,6.372606216464835E-2,21.540531720550998,-142133.42455773099,1333.9700300361328]
["KBM","KBM-25H01-A (400 V)",4.9000000000000004,3.1,3.304359770860303,2.0026422853698809,3150,14.37,3979,8.98,37,100.3,0.26600000000000001,565,10,1910.0159915136342,3562.7665402776902,3908.2751744765701,3.0952718670793842,422.93233082706763,2.0281803397476472,2.0282085469171891,9.5447387577416179E-2,-22.574514591604942,9,29.145356819200003,9,-2355.7711040000004,7.5,2367.7711040000004,9,0.26137244674179755,0.38414373358639459,6.2729387218031407,18.438899212146939,13.807610339746674,23.034601090365786,2.4161703174684339,148.01280389232554,3.3325286234856297E-2,14.182744492534097,-148665.28126735182,1910.0159915136342,1.1203886897470851E-2,3.1447156071848834,-153418.24583055242,3562.7665402776902,2.0157816109944222,6.372606216464835E-2,21.540531720550998,-142133.42455773099,1333.9700300361328]
["KBM","KBM-25H01-A (480 V)",4.9000000000000004,3.1,2.7893997920842706,1.6905453285359218,3800,14.37,4779,8.98,37,100.3,0.26600000000000001,679,10,1910.0159915136342,3579.7330571055081,3908.2751744765701,2.9117407014185011,422.93233082706763,2.0286302366901978,2.0282085469171891,9.5447387577416179E-2,-22.574514591604942,9,29.145356819200003,9,-2355.7711040000004,7.5,2367.7711040000004,9,0.26137244674179755,0.38414373358639459,6.2729387218031407,18.438899212146939,13.807610339746674,23.034601090365786,2.4161703174684339,148.01280389232554,3.3325286234856297E-2,14.182744492534097,-148665.28126735182,1910.0159915136342,1.1125656557063964E-2,3.0352691638118157,-153435.05426251687,3579.7330571055081,1.9456257827738637,6.372606216464835E-2,21.540531720550998,-142133.42455773099,1333.9700300361328]
["KBM","KBM-25H01-B (120 V)",4.96,5.34,4.2630788328186258,4.4874514029669745,1400,14.64,1989,2.87,12,57.5,0.26600000000000001,160,10,1989,1989,1989,3.9698741417687478,422.93233082706763,2.0035115765882554,1.9908030614207652,6.4014054536710038E-2,-22.574514591604942,9,29.145356819200003,9,-2355.7711040000004,7.5,2367.7711040000004,9,0.44478872538019476,0.65371390043064526,10.674929409124674,31.378267220670971,23.497003911928427,23.034601090365786,2.4161703174684339,148.01280389232554,1.0661921313160422E-2,4.5051683668662887,-152129.28982882324,3571.9927187594176,3.4133048569001873E-3,0.54350439006404405,-153641.66374124622,6629.9984580107584,1.9014840533811195,1.9653547958523167E-2,6.7161882092973029,-150253.24884213958,2599.3863809011759]
["KBM","KBM-25H01-B (240 V)",4.96,5.34,3.3346749981159021,3.510184208543055,3150,14.64,4173,2.87,12,57.5,0.26600000000000001,325,10,3571.9927187594176,4173,4173,2.8068313546468762,422.93233082706763,2.0036748348858402,1.9908030614207652,4.898231190600244E-2,-22.574514591604942,9,29.145356819200003,9,-2355.7711040000004,7.5,2367.7711040000004,9,0.44478872538019476,0.65371390043064526,10.674929409124674,31.378267220670971,23.497003911928427,23.034601090365786,2.4161703174684339,148.01280389232554,1.0661921313160422E-2,4.5051683668662887,-152129.28982882324,3571.9927187594176,3.4318952803662601E-3,0.58880699208769227,-153637.78497739648,6605.6263404691445,2.0599780359494804,1.9653547958523167E-2,6.7161882092973029,-150253.24884213958,2599.3863809011759]
["KBM","KBM-25H01-B (400 V)",4.96,5.34,1.4226503076377583,1.497526639618693,4900,14.64,6970,2.87,12,57.5,0.26600000000000001,565,10,3571.9927187594176,6752.9979943203571,6817.391304347826,8.4956045360826238E-2,422.93233082706763,2.0055264575601606,1.9908030614207652,4.898231190600244E-2,-22.574514591604942,9,29.145356819200003,9,-2355.7711040000004,7.5,2367.7711040000004,9,0.44478872538019476,0.65371390043064526,10.674929409124674,31.378267220670971,23.497003911928427,23.034601090365786,2.4161703174684339,148.01280389232554,1.0661921313160422E-2,4.5051683668662887,-152129.28982882324,3571.9927187594176,3.3308840523264302E-3,0.26071606851076046,-153658.86027460266,6752.9979943203571,0.91213144879108299,1.9653547958523167E-2,6.7161882092973029,-150253.24884213958,2599.3863809011759]
["KBM","KBM-25H01-C (120 V)",4.8499999999999996,6.45,3.9834208613857238,5.2002883307907624,1750,15.1,2470,1.97,7.9,46.3,0.26600000000000001,160,10,2470,2470,2470,3.6268854443558505,422.93233082706763,2.0490312108458819,1.9301560807417222,5.1548159705877034E-2,-22.574514591604942,9,29.145356819200003,9,-2355.7711040000004,7.5,2367.7711040000004,9,0.54942974255234545,0.80750666444948471,13.18631382125629,38.760319893575264,29.024910195390337,23.034601090365786,2.4161703174684339,148.01280389232554,7.3185968558146762E-3,3.1725083064621877,-152490.22849449178,4353.0458910691596,2.1689100070932141E-3,0.22147468947117219,-153658.27960221903,8366.096034090504,1.4018974858829534,1.2954406036766833E-2,4.5854158647014236,-151211.91520086213,3244.1203568546744]
["KBM","KBM-25H01-C (240 V)",4.8499999999999996,6.45,2.3166932544737429,3.0244037264670274,4225,15.1,5178,1.97,7.9,46.3,0.26600000000000001,325,10,4353.0458910691596,5178,5178,1.7452751885597726,422.93233082706763,2.0500125636826243,1.9301560807417222,3.9247605041683092E-2,-22.574514591604942,9,29.145356819200003,9,-2355.7711040000004,7.5,2367.7711040000004,9,0.54942974255234545,0.80750666444948471,13.18631382125629,38.760319893575264,29.024910195390337,23.034601090365786,2.4161703174684339,148.01280389232554,7.3185968558146762E-3,3.1725083064621877,-152490.22849449178,4353.0458910691596,2.1503152948842705E-3,0.11351522276042314,-153662.49725172503,8427.0744507834206,0.71853224301729668,1.2954406036766833E-2,4.5854158647014236,-151211.91520086213,3244.1203568546744]
["KBM","KBM-25H01-D (120 V)",4.75,7.95,3.6744032513824534,5.9941325471165632,2300,15.2,3097,1.3,5.2,37.1,0.26600000000000001,160,10,3097,3097,3097,3.3016855954484603,422.93233082706763,2.0919990181023089,1.9174576854736844,4.1112029213276162E-2,-22.574514591604942,9,29.145356819200003,9,-2355.7711040000004,7.5,2367.7711040000004,9,0.6914610297335636,1.0162525733010528,16.595064713605527,48.780123518450537,36.528044875031021,23.034601090365786,2.4161703174684339,148.01280389232554,4.9747269056431677E-3,2.1251764578237542,-152843.68211200001,5333.4432197968008,1.3772716784303245E-3,3.2886518709925802E-2,-153663.80356087344,10550.792928923116,0.39367697345812402,8.7949433029762079E-3,3.0514363607997481,-151972.77720591778,3987.0108679924983]
["KBM","KBM-25H01-D (240 V)",4.75,7.95,1.3252085057447611,2.1618409555379463,4900,15.2,6489,1.3,5.2,37.1,0.26600000000000001,325,10,5333.4432197968008,6489,6489,0.21459754975056189,422.93233082706763,2.0942663571476774,1.9174576854736844,3.1934689593064794E-2,-22.574514591604942,9,29.145356819200003,9,-2355.7711040000004,7.5,2367.7711040000004,9,0.6914610297335636,1.0162525733010528,16.595064713605527,48.780123518450537,36.528044875031021,23.034601090365786,2.4161703174684339,148.01280389232554,4.9747269056431677E-3,2.1251764578237542,-152843.68211200001,5333.4432197968008,1.4124631024484383E-3,-0.21272405986575513,-153655.78087821839,10505.612481348415,-2.5464709356542352,8.7949433029762079E-3,3.0514363607997481,-151972.77720591778,3987.0108679924983]
["KBM","KBM-25H01-E (120 V)",5.09,10.44,3.6221469807121007,7.2733875114700819,2900,15.32,3815,0.75,3.4,30,0.26600000000000001,160,10,3815,3815,3815,3.1590140453160913,422.93233082706763,1.9523013253858894,1.9024384346736294,3.3374562116255904E-2,-22.574514591604942,9,29.145356819200003,9,-2355.7711040000004,7.5,2367.7711040000004,9,0.84737745646260187,1.2454057186986249,20.337058955102446,59.779474497533997,44.764694501557827,23.034601090365786,2.4161703174684339,148.01280389232554,3.2469255087942362E-3,1.2245728517823724,-153247.45036963266,6684.0723498953557,9.064733254580831E-4,-6.4312989210696711E-2,-153662.85106650522,13055.40104106591,-1.6502720725860112,5.6630768867448941E-3,1.7445313183949394,-152818.61402198311,5042.9732650753785]
["KBM","KBM-25H01-E (240 V)",5.09,10.44,1.4421386680163577,2.8958607791493125,4900,15.32,6918,0.75,3.4,30,0.26600000000000001,325,10,6684.0723498953557,6918,6918,-6.0184631563844349E-2,422.93233082706763,1.9543358029831577,1.9024384346736294,2.5247794858498644E-2,-22.574514591604942,9,29.145356819200003,9,-2355.7711040000004,7.5,2367.7711040000004,9,0.84737745646260187,1.2454057186986249,20.337058955102446,59.779474497533997,44.764694501557827,23.034601090365786,2.4161703174684339,148.01280389232554,3.2469255087942362E-3,1.2245728517823724,-153247.45036963266,6684.0723498953557,1.003764727610282E-3,-0.2574896930932018,-153645.583071653,12501.045409573962,-6.607188605373965,5.6630768867448941E-3,1.7445313183949394,-152818.61402198311,5042.9732650753785]
["KBM","KBM-25H01-F (120 V)",4.63,12,2.4658943081579734,6.2905467044846262,3950,15.73,4765,0.56000000000000005,2.1,23.7,0.26600000000000001,160,10,4765,4765,4765,2.0193762983222134,422.93233082706763,2.1471683308625344,1.8528516731849969,2.6720662009132479E-2,-22.574514591604942,9,29.145356819200003,9,-2355.7711040000004,7.5,2367.7711040000004,9,1.070765684415641,1.5737233703671709,25.698376425975386,75.538721777624204,56.565699712750266,23.034601090365786,2.4161703174684339,148.01280389232554,2.0688350544394588E-3,0.93718640071617698,-153273.07335465855,8383.8392899637893,6.2455388671766503E-4,-0.19140314347884466,-153647.69422486887,15838.747164404838,-8.3263002118182285,3.463062062204399E-3,1.3003197654023217,-152911.43564408485,6459.8316599721411]
["KBM","KBM-25H02-A (120 V)",8.6999999999999993,3.33,8.0801740338962258,3.0262824096989611,390,29.4,707,8.9600000000000009,45,162,0.51500000000000001,160,10,707,707,707,7.576366774268287,218.44660194174756,1.1448293946681727,0.99307701931972792,0.18009045894415313,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.15820129728671475,0.23281663396896557,3.7968311348811539,11.175198430510347,8.3661345134243472,23.044726895810197,2.4249130491850321,148.54837716118678,7.8970404630503171E-2,28.291499266412547,-146039.31501732377,1192.5062070467523,2.7652128251120685E-2,4.6234161923159816,-153460.37272055165,2273.658430231148,1.8389898748961822,5.538693056860429E-2,21.033352224760538,-149449.68524414304,1463.706702652353]
["KBM","KBM-25H02-A (240 V)",8.6999999999999993,3.33,8.0691556147590937,3.0221556609584623,1000,29.4,1484,8.9600000000000009,45,162,0.51500000000000001,325,10,1192.5062070467523,1484,1484,7.7638269323024955,218.44660194174756,1.1420267361703538,0.99307701931972792,8.6987341277316776E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.15820129728671475,0.23281663396896557,3.7968311348811539,11.175198430510347,8.3661345134243472,23.044726895810197,2.4249130491850321,148.54837716118678,7.8970404630503171E-2,28.291499266412547,-146039.31501732377,1192.5062070467523,2.9371349624219775E-2,6.8901726109948918,-153211.75873905176,2169.6526720753591,2.7406050290184676,5.538693056860429E-2,21.033352224760538,-149449.68524414304,1463.706702652353]
["KBM","KBM-25H02-A (400 V)",8.6999999999999993,3.33,7.5170103891095179,2.8153596962956997,1950,29.4,2482,8.9600000000000009,45,162,0.51500000000000001,565,10,1192.5062070467523,2159.2573549353597,2419.7530864197533,7.3900620419859528,218.44660194174756,1.1419561988332962,0.99307701931972792,8.6987341277316776E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.15820129728671475,0.23281663396896557,3.7968311348811539,11.175198430510347,8.3661345134243472,23.044726895810197,2.4249130491850321,148.54837716118678,7.8970404630503171E-2,28.291499266412547,-146039.31501732377,1192.5062070467523,2.9566231827116322E-2,7.1016105331379134,-153183.57712082405,2159.2573549353597,2.8247056554419196,5.538693056860429E-2,21.033352224760538,-149449.68524414304,1463.706702652353]
["KBM","KBM-25H02-A (480 V)",8.6999999999999993,3.33,7.4404935895461071,2.7867017189311265,2400,29.4,2982,8.9600000000000009,45,162,0.51500000000000001,679,10,1192.5062070467523,2150.2987083140774,2419.7530864197533,7.5715354135365391,218.44660194174756,1.1417174730587329,0.99307701931972792,8.6987341277316776E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.15820129728671475,0.23281663396896557,3.7968311348811539,11.175198430510347,8.3661345134243472,23.0447268958102,2.4249130491850321,148.54837716118678,7.8970404630503171E-2,28.291499266412547,-146039.31501732377,1192.5062070467523,2.9737466374039338E-2,7.2823268524686267,-153158.81515407155,2150.2987083140774,2.8965865910215505,5.538693056860429E-2,21.033352224760538,-149449.68524414304,1463.706702652353]
["KBM","KBM-25H02-B (120 V)",8.75,5.18,8.0214091318315255,4.6636099603671664,750,29.7,1098,3.7,19,104,0.51500000000000001,160,10,1098,1098,1098,7.6833429690013535,218.44660194174756,1.1364734799748317,0.98304593831649834,0.11595988567715507,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.24468467313678544,0.36008972720533333,5.8724321552828505,17.284306905855999,12.939621380762986,23.044726895810197,2.4249130491850321,148.54837716118678,3.3762794270852589E-2,11.718549173790825,-150489.89694113919,1944.8030327709869,1.1509201863706504E-2,2.0367733159706503,-153568.11322252566,3565.4040365460501,3.0559553592876858,2.3244217575149845E-2,8.6241690236091895,-151944.87344332979,2377.9433211392879]
["KBM","KBM-25H02-B (240 V)",8.75,5.18,7.6956096012669404,4.4741916286435703,1700,29.7,2303,3.7,19,104,0.51500000000000001,325,10,1944.8030327709869,2303,2303,7.321611124539861,218.44660194174756,1.1354598052114926,0.98304593831649834,5.5286128733615401E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.24468467313678544,0.36008972720533333,5.8724321552828505,17.284306905855999,12.939621380762986,23.044726895810197,2.4249130491850321,148.54837716118678,3.3762794270852589E-2,11.718549173790825,-150489.89694113919,1944.8030327709869,1.1944533254788855E-2,2.5987829949010828,-153507.89624041726,3477.7954492784393,3.8991893494583216,2.3244217575149845E-2,8.6241690236091895,-151944.87344332979,2377.9433211392879]
["KBM","KBM-25H02-B (400 V)",8.75,5.18,6.7906109052542005,3.9480295960780238,3150,29.7,3845,3.7,19,104,0.51500000000000001,565,10,1944.8030327709869,3469.6120037877195,3769.2307692307691,6.5918031989775301,218.44660194174756,1.1354649916776494,0.98304593831649834,5.3543729718719513E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.24468467313678544,0.36008972720533333,5.8724321552828505,17.284306905855999,12.939621380762986,23.044726895810197,2.4249130491850321,148.54837716118678,3.3762794270852589E-2,11.718549173790825,-150489.89694113919,1944.8030327709869,1.198794278886975E-2,2.6482930531648887,-153501.89163980581,3469.6120037877195,3.9734737711480363,2.3244217575149845E-2,8.6241690236091895,-151944.87344332979,2377.9433211392879]
["KBM","KBM-25H02-B (480 V)",8.75,5.18,6.0876765732649973,3.5393468449215102,4000,29.7,4614,3.7,19,104,0.51500000000000001,679,10,1944.8030327709869,3476.0956985344624,3769.2307692307691,6.4363772470547325,218.44660194174756,1.1355905922686844,0.98304593831649834,5.3543729718719513E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.24468467313678544,0.36008972720533333,5.8724321552828505,17.284306905855999,12.939621380762986,23.044726895810197,2.4249130491850321,148.54837716118678,3.3762794270852589E-2,11.718549173790825,-150489.89694113919,1944.8030327709869,1.1953512052455815E-2,2.609100687412218,-153506.65425302665,3476.0956985344624,3.9146699174123745,2.3244217575149845E-2,8.6241690236091895,-151944.87344332979,2377.9433211392879]
["KBM","KBM-25H02-C (120 V)",8.75,6.5,7.9912534584035866,5.7907633756547732,950,29.7,1380,2.35,12,83.4,0.51500000000000001,160,10,1380,1380,1380,7.6478208132599468,218.44660194174756,1.1359746087510529,0.98304593831649834,9.2263735125736421E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.30703675200561875,0.45185004379047616,7.36888204813485,21.688802101942855,16.23697663609255,23.044726895810197,2.4249130491850321,148.54837716118678,2.1368232093066306E-2,7.4895598082909327,-151647.86089251022,2494.505989375738,7.337838989681553E-3,1.2197596284211623,-153610.52430749193,4493.0123449513167,3.593186131004622,1.4761610052030336E-2,5.5118793923391847,-152572.03851754233,3033.643175464445]
["KBM","KBM-25H02-C (240 V)",8.75,6.5,7.4617759365874656,5.4070840120199026,2150,29.7,2895,2.35,12,83.4,0.51500000000000001,325,10,2494.505989375738,2895,2895,7.015391319265448,218.44660194174756,1.1353990936265663,0.98304593831649834,4.3980640578071252E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.30703675200561875,0.45185004379047616,7.36888204813485,21.688802101942855,16.23697663609255,23.044726895810197,2.4249130491850321,148.54837716118678,2.1368232093066306E-2,7.4895598082909327,-151647.86089251022,2494.505989375738,7.5606839064013415E-3,1.5346388756595384,-153579.35129886432,4406.636928024066,4.5207621203678707,1.4761610052030336E-2,5.5118793923391847,-152572.03851754233,3033.643175464445]
["KBM","KBM-25H02-C (400 V)",8.75,6.5,6.0399300903374282,4.3767609350271224,4000,29.7,4826,2.35,12,83.4,0.51500000000000001,565,10,2494.505989375738,4415.235536774805,4700.2398081534775,5.7586007569284323,218.44660194174756,1.1356250209563081,0.98304593831649834,4.197064292309962E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.30703675200561875,0.45185004379047616,7.36888204813485,21.688802101942855,16.23697663609255,23.044726895810197,2.4249130491850321,148.54837716118678,2.1368232093066306E-2,7.4895598082909327,-151647.86089251022,2494.505989375738,7.537482105573764E-3,1.5049305823702706,-153582.59691894855,4415.235536774805,4.4332469862910138,1.4761610052030336E-2,5.5118793923391847,-152572.03851754233,3033.643175464445]
["KBM","KBM-25H02-C (480 V)",8.75,6.5,4.8414933688554562,3.5083285281561278,5000,29.7,5791,2.35,12,83.4,0.51500000000000001,679,10,2494.505989375738,4440.5276033819109,4700.2398081534775,5.2788336832802827,218.44660194174756,1.1359256061430596,0.98304593831649834,4.197064292309962E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.30703675200561875,0.45185004379047616,7.36888204813485,21.688802101942855,16.23697663609255,23.044726895810197,2.4249130491850321,148.54837716118678,2.1368232093066306E-2,7.4895598082909327,-151647.86089251022,2494.505989375738,7.4705072927413975E-3,1.4156810862161993,-153591.96579506644,4440.5276033819109,4.1703344875431618,1.4761610052030336E-2,5.5118793923391847,-152572.03851754233,3033.643175464445]
["KBM","KBM-25H02-D (120 V)",8.6199999999999992,8,7.7953441514397719,7.0228325688646587,1225,29.8,1717,1.57,7.8,67,0.51500000000000001,160,10,1717,1717,1717,7.4641354351200722,218.44660194174756,1.152768667047398,0.97974712644295303,7.4154894859357168E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.38359044512570617,0.56451013859242083,9.2061706830169481,27.096486652436198,20.285353641379238,23.044726895810197,2.4249130491850321,148.54837716118678,1.4057540157768531E-2,5.0388806019076311,-152249.97027621514,3116.6232925234358,4.6994494575990581E-3,0.74728304918279265,-153632.89998019626,5638.7091612250952,4.101569251892097,9.6366958638988611E-3,3.695878331418684,-152903.2784227751,3796.1644222114273]
["KBM","KBM-25H02-D (240 V)",8.6199999999999992,8,6.9736147541916713,6.2825358145870904,2725,29.8,3597,1.57,7.8,67,0.51500000000000001,325,10,3116.6232925234358,3597,3597,6.4467714755330068,218.44660194174756,1.1525635962643406,0.97974712644295303,3.5397262850574443E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.38359044512570617,0.56451013859242083,9.2061706830169481,27.096486652436198,20.285353641379238,23.044726895810197,2.4249130491850321,148.54837716118678,1.4057540157768531E-2,5.0388806019076311,-152249.97027621514,3116.6232925234358,4.791791456787548E-3,0.89636116935619969,-153619.25376776958,5569.2937863000743,4.9198057079468542,9.6366958638988611E-3,3.695878331418684,-152903.2784227751,3796.1644222114273]
["KBM","KBM-25H02-D (400 V)",8.6199999999999992,8,4.4612543893712751,4.0191480985326802,5180,29.8,5995,1.57,7.8,67,0.51500000000000001,565,10,3116.6232925234358,5627.1628417135989,5850.746268656716,4.1022512030367775,218.44660194174756,1.1531541559131806,0.97974712644295303,3.3540157989085377E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.38359044512570617,0.56451013859242083,9.2061706830169481,27.096486652436198,20.285353641379238,23.044726895810197,2.4249130491850321,148.54837716118678,1.4057540157768531E-2,5.0388806019076311,-152249.97027621514,3116.6232925234358,4.7143399008942842E-3,0.77326842204578106,-153630.69948471079,5627.1628417135989,4.2441936650248966,9.6366958638988611E-3,3.695878331418684,-152903.2784227751,3796.1644222114273]
["KBM","KBM-25H02-D (480 V)",8.6199999999999992,8,2.8488734813449264,2.5665526858963297,6000,29.8,7193,1.57,7.8,67,0.51500000000000001,679,10,3116.6232925234358,5679.2397708312928,5850.746268656716,3.1573981254591601,218.44660194174756,1.1536272565984063,0.97974712644295303,3.3540157989085377E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.38359044512570617,0.56451013859242083,9.2061706830169481,27.096486652436198,20.285353641379238,23.044726895810197,2.4249130491850321,148.54837716118678,1.4057540157768531E-2,5.0388806019076311,-152249.97027621514,3116.6232925234358,4.6488202397724819E-3,0.65121907745134822,-153640.38191764109,5679.2397708312928,3.5743084862435177,9.6366958638988611E-3,3.695878331418684,-152903.2784227751,3796.1644222114273]
["KBM","KBM-25H02-E (120 V)",8.85,10.199999999999999,7.8184865793893579,8.7848163813363573,1600,29.8,2143,0.96,5,54,0.51500000000000001,160,10,2143,2143,2143,7.4684167122696214,218.44660194174756,1.1226787368886624,0.97974712644295303,5.9413884495341233E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.47636732058238113,0.7010450483841808,11.432815693977147,33.650162322440679,25.191658666167061,23.044726895810197,2.4249130491850321,148.54837716118678,8.9797996966562328E-3,3.0838893371993312,-152848.6387650813,3957.5574936335047,3.0340101497143687E-3,0.43021548935557813,-153648.13191295599,7045.7687550613282,4.7913778662999542,6.178210964610506E-3,2.2619467850722992,-153225.35088661703,4800.3577052387191]
["KBM","KBM-25H02-E (240 V)",8.85,10.199999999999999,6.5120897548433847,7.3169547807229041,3600,29.8,4480,0.96,5,54,0.51500000000000001,325,10,3957.5574936335047,4480,4480,5.940600583805101,218.44660194174756,1.1226920528909707,0.97974712644295303,2.8420525552124168E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.47636732058238113,0.7010450483841808,11.432815693977147,33.650162322440679,25.191658666167061,23.044726895810197,2.4249130491850321,148.54837716118678,8.9797996966562328E-3,3.0838893371993312,-152848.6387650813,3957.5574936335047,3.0605500849525047E-3,0.47614095370788578,-153644.56325378962,7007.9501022700379,5.3028570176592016,6.178210964610506E-3,2.2619467850722992,-153225.35088661703,4800.3577052387191]
["KBM","KBM-25H02-E (400 V)",8.85,10.199999999999999,2.9443664472000637,3.3082769069663636,6000,29.8,7430,0.96,5,54,0.51500000000000001,565,10,3957.5574936335047,7147.507999926459,7259.2592592592591,1.8149061561213902,218.44660194174756,1.1236368157429211,0.97974712644295303,2.6523847240501532E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.47636732058238113,0.7010450483841808,11.432815693977147,33.650162322440679,25.191658666167061,23.044726895810197,2.4249130491850321,148.54837716118678,8.9797996966562328E-3,3.0838893371993312,-152848.6387650813,3957.5574936335047,2.9678587304904289E-3,0.28519197605017149,-153657.02688072674,7147.507999926459,3.1762280891837928,6.178210964610506E-3,2.2619467850722992,-153225.35088661703,4800.3577052387191]
["KBM","KBM-25H02-F (120 V)",8.93,12.74,7.639437268410977,10.669605123479018,2100,30.1,2666,0.61,3.2,43.3,0.51500000000000001,160,10,2666,2666,2666,7.2915998845636496,218.44660194174756,1.1125215632493168,0.96998220491694354,4.7758422533201901E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.58966184735681548,0.86777472015752144,14.151884336563571,41.653186567561029,31.182995443335638,23.044726895810197,2.4249130491850321,148.54837716118678,5.7575324103834452E-3,1.9645488096689794,-153149.3762053278,4989.7163539131598,1.9312868643388522E-3,0.23676996249479956,-153656.52489277508,8858.6503788610935,5.1754515421341818,3.9222495902741916E-3,1.4265801933389377,-153392.63327341512,6074.4516286314611]
["KBM","KBM-25H02-F (240 V)",8.93,12.74,5.6022539968347154,7.8243770905512786,4500,30.1,5564,0.61,3.2,43.3,0.51500000000000001,325,10,4989.7163539131598,5564,5564,4.8154269418640796,218.44660194174756,1.1128675461423969,0.96998220491694354,2.288352884139401E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.58966184735681548,0.86777472015752144,14.151884336563571,41.653186567561029,31.182995443335638,23.044726895810193,2.4249130491850321,148.54837716118678,5.7575324103834452E-3,1.9645488096689794,-153149.3762053278,4989.7163539131598,1.9148898061164185E-3,0.19940133863754547,-153658.69823644983,8905.9950216216039,4.3586270601279153,3.9222495902741916E-3,1.4265801933389377,-153392.63327341512,6074.4516286314611]
["KBM","KBM-25H02-G (120 V)",8.74,14.37,7.341021750113673,11.615540743850747,2400,30,3027,0.49,2.5,38.200000000000003,0.51500000000000001,160,10,3027,3027,3027,6.9755386823308703,218.44660194174756,1.1366531508033879,0.97321547893333338,4.2062753377441781E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.67956404867640352,1.0000791213009153,16.309537168233685,48.003797822443929,35.937279524391599,23.044726895810197,2.4249130491850321,148.54837716118678,4.5858355526250377E-3,1.5991406403466366,-153225.88653209747,5608.6583819447242,1.483742185209655E-3,0.1415641275568448,-153660.56663704893,10128.990042004445,4.366496802678645,3.1189374267087521E-3,1.1651055417047493,-153431.43528766496,6829.5148155657362]
["KBM","KBM-25H02-G (240 V)",8.74,14.37,4.3692536263907114,6.9133759911245436,5300,30,6316,0.49,2.5,38.200000000000003,0.51500000000000001,325,10,5608.6583819447242,6316,6316,3.5313897932610816,218.44660194174756,1.1373521753720532,0.97321547893333338,2.0158954159834749E-2,-22.637610330864199,9,29.196464368000001,9,-2360.9861599999999,7.5,2372.9861599999999,9,0.67956404867640352,1.0000791213009153,16.309537168233685,48.003797822443929,35.937279524391599,23.044726895810197,2.4249130491850321,148.54837716118678,4.5858355526250377E-3,1.5991406403466366,-153225.88653209747,5608.6583819447242,1.464945669019559E-3,6.831311594752025E-2,-153663.20049446792,10218.46079764567,2.1070945550530471,3.1189374267087521E-3,1.1651055417047493,-153431.43528766496,6829.5148155657362]
["KBM","KBM-25H03-A (120 V)",11.86,5.3,11.285532328334398,4.9281800560412217,550,42.2,827,3.97,21,139,0.76600000000000001,160,10,827,827,827,10.996209519150085,146.86684073107048,0.83840461192898486,0.69308015211374407,0.15395883249518291,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.1847859296385829,0.27229888072962338,4.4348623113259897,13.070346275021922,9.7823279578965963,23.054952121099216,2.4337260036463415,149.08825222337217,5.1569116979886337E-2,18.024763117748442,-149460.12745909963,1536.6078992554526,2.0595275169771693E-2,3.5830180496259696,-153497.88517230027,2644.4289247351535,3.748720503529785,2.7998238507081108E-2,9.3499255566001871,-152532.83303252983,2173.0744124811331]
["KBM","KBM-25H03-A (240 V)",11.86,5.3,11.018419137131216,4.8115367411053347,1300,42.2,1735,3.97,21,139,0.76600000000000001,325,10,1536.6078992554526,1735,1735,10.736813233017431,146.86684073107048,0.83778103204427956,0.69308015211374407,7.3385564538049716E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.1847859296385829,0.27229888072962338,4.4348623113259897,13.070346275021922,9.7823279578965963,23.054952121099216,2.4337260036463415,149.08825222337217,5.1569116979886337E-2,18.024763117748442,-149460.12745909963,1536.6078992554526,2.1106797944968027E-2,4.2416374520940385,-153431.20293624804,2597.5513817883689,4.4377988234987074,2.7998238507081108E-2,9.3499255566001871,-152532.83303252983,2173.0744124811331]
["KBM","KBM-25H03-A (400 V)",11.86,5.3,9.9869726790164322,4.3611234406185293,2400,42.2,2899,3.97,21,139,0.76600000000000001,565,10,1536.6078992554526,2600.0443571597552,2820.1438848920861,9.8308524513627589,146.86684073107048,0.83798986568775113,0.69308015211374407,5.8591621962978548E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.1847859296385829,0.27229888072962338,4.4348623113259897,13.070346275021922,9.7823279578965963,23.054952121099216,2.4337260036463415,149.08825222337217,5.1569116979886337E-2,18.024763117748442,-149460.12745909963,1536.6078992554526,2.107836527132264E-2,4.2077352424953629,-153434.90942664797,2600.0443571597552,4.4023287514875467,2.7998238507081108E-2,9.3499255566001871,-152532.83303252983,2173.0744124811331]
["KBM","KBM-25H03-A (480 V)",11.86,5.3,9.3846535409358971,4.09810198294144,2900,42.2,3479,3.97,21,139,0.76600000000000001,679,10,1536.6078992554526,2603.7784812154614,2820.1438848920861,9.6374986745986213,146.86684073107048,0.83810470216431643,0.69308015211374407,5.8591621962978548E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.1847859296385829,0.27229888072962338,4.4348623113259897,13.070346275021922,9.7823279578965963,23.054952121099216,2.4337260036463415,149.08825222337217,5.1569116979886337E-2,18.024763117748442,-149460.12745909963,1536.6078992554526,2.1036030724186586E-2,4.1567445685157649,-153440.42816872982,2603.7784812154614,4.3489799314736262,2.7998238507081108E-2,9.3499255566001871,-152532.83303252983,2173.0744124811331]
["KBM","KBM-25H03-B (120 V)",11.84,7.27,10.742958658702936,6.4716618425921304,800,42.3,1144,2.1,11.4,100,0.76600000000000001,160,10,1144,1144,1144,10.271230881945197,146.86684073107048,0.84033923866509308,0.69144166475650126,0.1112971630013254,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.25389867067956118,0.37414279312286042,6.0935680963094683,17.958854069897299,13.441067020196201,23.054952121099216,2.4337260036463415,149.08825222337217,2.8026622426156465E-2,9.4471975711842582,-151432.76145127526,2162.0355844575142,1.0433862742216306E-2,1.4656220666618673,-153610.29879894285,3767.3717961543398,4.0294156891308797,1.4827649191093882E-2,4.8889283072528285,-153066.45950016356,3052.3174692410967]
["KBM","KBM-25H03-B (240 V)",11.84,7.27,10.02022080068974,6.0362775907769519,1825,42.3,2399,2.1,11.4,100,0.76600000000000001,325,10,2162.0355844575142,2399,2399,9.447862849783391,146.86684073107048,0.83974896429611268,0.69144166475650126,5.3073761764700404E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.25389867067956118,0.37414279312286042,6.0935680963094683,17.958854069897299,13.441067020196201,23.054952121099216,2.4337260036463415,149.08825222337217,2.8026622426156465E-2,9.4471975711842582,-151432.76145127526,2162.0355844575142,1.0688176899723806E-2,1.8458476881723964,-153578.82115780172,3705.2848174621886,5.0747650459494356,1.4827649191093882E-2,4.8889283072528285,-153066.45950016356,3052.3174692410967]
["KBM","KBM-25H03-B (400 V)",11.84,7.27,5.2661562052465376,3.1723832561726133,3400,42.3,4000,2.1,11.4,100,0.76600000000000001,565,10,2162.0355844575142,3803.0268751757112,3920,4.4869104045133819,146.86684073107048,0.84122769206773418,0.69144166475650126,4.1713863566483163E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.25389867067956118,0.37414279312286042,6.0935680963094683,17.958854069897299,13.441067020196201,23.054952121099216,2.4337260036463415,149.08825222337217,2.8026622426156465E-2,9.4471975711842582,-151432.76145127526,2162.0355844575142,1.0301030167183634E-2,1.2208177263761331,-153626.74010197414,3803.0268751757112,3.3563782997844158,1.4827649191093882E-2,4.8889283072528285,-153066.45950016356,3052.3174692410967]
["KBM","KBM-25H03-B (480 V)",11.84,7.27,6.6499920800324466,4.006019325320751,4150,42.3,4800,2.1,11.4,100,0.76600000000000001,679,10,{"$f":"IF(AQ571<I571,IF(AQ571<0,0,AQ571),I571)","v":2162.0355844575142},{"$f":"IF(AU571<I571,IF(AU571<0,0,AU571),I571)","v":3727.4565184104436},{"$f":"IF(UAC_V*0.98/L571*1000<I571,IF(UAC_V*0.98/L571*1000<0,0,UAC_V*0.98/L571*1000),I571)","v":3920},{"$f":"C571+(E571-C571)/G571*Q571","v":7.1784267826783417},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M571,(inertia/gear^2+gear_inertia)/M571),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M571,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M571))","v":146.86684073107048},{"$f":"IF((C571+(E571-C571)/G571*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X571^2*time1+Y571^2*time2+Z571^2*time3+AA571^2*time4)/time)/(C571+(E571-C571)/G571*mspeed),SQRT((((X571-Y571)*2/PI()+Y571)^2*time1+Y571^2*time2+((Z571-Y571)*2/PI()+Y571)^2*time3+AA571^2*time4)/time)/(C571+(E571-C571)/G571*mspeed)),IF(AccType=1,SQRT((X571^2*time1+Y571^2*time2+Z571^2*time3+AA571^2*time4+AB571^2*time5+AC571^2*time6+AD571^2*time7+AE571^2*time8)/time)/(C571+(E571-C571)/G571*mspeed),SQRT((((X571-Y571)*2/PI()+Y571)^2*time1+Y571^2*time2+((Z571-Y571)*2/PI()+Y571)^2*time3+AA571^2*time4+((AB571-AC571)*2/PI()+AC571)^2*time5+AC571^2*time6+((AD571-AC571)*2/PI()+AC571)^2*time7+AE571^2*time8)/time)/(C571+(E571-C571)/G571*mspeed))))","v":0.84014873722494443},{"$f":"IF(move1,MAX(ABS(X571),ABS(Z571))/H571,MAX(ABS(X571),ABS(Z571),ABS(AB571),ABS(AD571))/H571)","v":0.69144166475650126},{"$f":"IF(AZ571>0,speed/(MIN(AZ571,I571)),\"NA\")","v":4.1713863566483163E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M571+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M571+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.701212863209879},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M571+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M571+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.247982419200003},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M571+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M571+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2366.2431040000001},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M571+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M571+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2378.2431040000001},9,{"$f":"AH571/Irms","v":0.25389867067956118},{"$f":"AI571/Ipeak","v":0.37414279312286042},{"$f":"IF(move1,IF(AccType=1,SQRT((X571^2*time1+Y571^2*time2+Z571^2*time3+AA571^2*time4)/time)/(C571/D571),SQRT((((X571-Y571)*2/PI()+Y571)^2*time1+Y571^2*time2+((Z571-AA571)*2/PI()+AA571)^2*time3+AA571^2*time4)/time)/(C571/D571)),IF(AccType=1,SQRT((X571^2*time1+Y571^2*time2+Z571^2*time3+AA571^2*time4+AB571^2*time5+AC571^2*time6+AD571^2*time7+AE571^2*time8)/time)/(C571/D571),SQRT((((X571-Y571)*2/PI()+Y571)^2*time1+Y571^2*time2+((Z571-AA571)*2/PI()+AA571)^2*time3+AA571^2*time4+((AB571-AC571)*2/PI()+AC571)^2*time5+AC571^2*time6+((AD571-AE571)*2/PI()+AE571)^2*time7+AE571^2*time8)/time)/(C571/D571)))","v":6.0935680963094683},{"$f":"IF(move1,MAX(ABS(X571),ABS(Z571))/(C571/D571),MAX(ABS(X571),ABS(Z571),ABS(AB571),ABS(AD571))/(C571/D571))","v":17.958854069897299},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X571),ABS(Z571))/(C571/D571),MAX(ABS((X571-Y571)*2/PI()+Y571),ABS((Z571-Y571)*2/PI()+Y571))/(C571/D571)),IF(AccType=1,MAX(ABS(X571),ABS(Z571),ABS(AB571),ABS(AD571))/(C571/D571),MAX(ABS((X571-Y571)*2/PI()+Y571),ABS((Z571-Y571)*2/PI()+Y571),ABS((AB571-AC571)*2/PI()+AC571),ABS((AD571-AC571)*2/PI()+AC571))/(C571/D571)))","v":13.441067020196201},{"$f":"IF((C571+(E571-C571)/G571*mspeed)<0,\"NA\",U571*(C571+(E571-C571)/G571*mspeed)*mspeed/9.55)","v":23.054952121099216},{"$f":"IF(move1,IF(speed1>speed2,AM571/2*time1/time,AM571/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z571*-speed/30*PI(),((Z571-AA571)*2/PI()+AA571)*-speed/30*PI()),IF(AccType=1,X571*-speed/30*PI(),((X571-Y571)*2/PI()+Y571)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z571*-speed/30*PI(),((Z571-AA571)*2/PI()+AA571)*-speed/30*PI()),IF(AccType=1,X571*-speed/30*PI(),((X571-Y571)*2/PI()+Y571)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD571*-speed/30*PI(),((AD571-AE571)*2/PI()+AE571)*-speed/30*PI()),IF(AccType=1,AB571*-speed/30*PI(),((AB571-AC571)*2/PI()+AC571)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD571*-speed/30*PI(),((AD571-AE571)*2/PI()+AE571)*-speed/30*PI()),IF(AccType=1,AB571*-speed/30*PI(),((AB571-AC571)*2/PI()+AC571)*-speed/30*PI()),0)/2*time7/time)))","v":2.4337260036463415},{"$f":"IF(move1,MAX(IF(AccType=1,Z571*-speed/30*PI(),((Z571-AA571)*2/PI()+AA571)*-speed/30*PI()),IF(AccType=1,X571*-speed/30*PI(),((X571-Y571)*2/PI()+Y571)*-speed/30*PI()),0),MAX(IF(AccType=1,Z571*-speed/30*PI(),((Z571-AA571)*2/PI()+AA571)*-speed/30*PI()),IF(AccType=1,X571*-speed/30*PI(),((X571-Y571)*2/PI()+Y571)*-speed/30*PI()),IF(AccType=1,AD571*-speed/30*PI(),((AD571-AE571)*2/PI()+AE571)*-speed/30*PI()),IF(AccType=1,AB571*-speed/30*PI(),((AB571-AC571)*2/PI()+AC571)*-speed/30*PI()),0))","v":149.08825222337217},{"$f":"(L571^2)/1000000+((K571/1000)^2*(D571/C571*H571)^2*PI()*PI()*(O571/2)^2)/1200","v":2.8026622426156465E-2},{"$f":"SQRT(3)*L571*J571*D571/C571*H571/1000","v":9.4471975711842582},{"$f":"0.75*J571^2*(D571/C571*H571)^2-(UAC_V*0.98)^2","v":-151432.76145127526},{"$f":"-AO571/2/AN571+SQRT((AO571/2/AN571)^2-AP571/AN571)","v":2162.0355844575142},{"$f":"(L571^2)/1000000+((K571/1000)^2*AV571^2*PI()*PI()*(O571/2)^2)/1200","v":1.0594306353178483E-2},{"$f":"SQRT(3)*L571*J571*AV571/1000","v":1.7153431130487291},{"$f":"0.75*J571^2*AV571^2-(UAC_V*0.98)^2","v":-153590.43995011289},{"$f":"-AS571/2/AR571+SQRT((AS571/2/AR571)^2-AT571/AR571)","v":3727.4565184104436},{"$f":"D571+(F571-D571)*((0.85*UAC_V-D571*J571)/L571*1000)/G571","v":4.7159705146250204},{"$f":"(L571^2)/1000000+((K571/1000)^2*AJ571^2*PI()*PI()*(O571/2)^2)/1200","v":1.4827649191093882E-2},{"$f":"SQRT(3)*L571*J571*AJ571/1000","v":4.8889283072528285},{"$f":"0.75*J571^2*AJ571^2-(UAC_V*0.98)^2","v":-153066.45950016356},{"$f":"IF(((AX571/2/AW571)^2-AY571/AW571)>0,-AX571/2/AW571+SQRT((AX571/2/AW571)^2-AY571/AW571),-9999)","v":3052.3174692410967}]
["KBM","KBM-25H03-C (120 V)",11.9,8.1999999999999993,10.769484482551585,7.2278419345983789,900,42.4,1276,1.66,9.1,90,0.76600000000000001,160,10,1276,1276,1276,10.297180221928691,146.86684073107048,0.83591142241739447,0.68981090611320761,9.9783663380498641E-2,-22.701212863209879,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},29.247982419200003,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},-2366.2431040000001,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},2378.2431040000001,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},0.28493421958477033,0.41987649831484591,6.8384212700344875,20.154071919112603,15.084048811817976,23.054952121099216,2.4337260036463415,149.08825222337217,2.26347239484481E-2,7.5603860555854405,-151899.81983612682,2428.9135688196961,8.4123043512300474E-3,1.1082292183040663,-153626.09345678077,4208.0524417693268,4.282707078391307,1.1974156414553714E-2,3.9032750355321024,-153193.76679003061,3417.5522991067669]
["KBM","KBM-25H03-C (240 V)",11.9,8.1999999999999993,9.8753701274580923,6.6277651862134848,2050,42.4,2676,1.66,9.1,90,0.76600000000000001,325,10,2428.9135688196961,2676,2676,9.257117298086758,146.86684073107048,0.83549220131508595,0.68981090611320761,4.7579953091747486E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.28493421958477033,0.41987649831484591,6.8384212700344875,20.154071919112603,15.084048811817976,23.054952121099216,2.4337260036463415,149.08825222337217,2.26347239484481E-2,7.5603860555854405,-151899.81983612682,2428.9135688196961,8.5999469531840862E-3,1.4021760393026821,-153603.31797391374,4145.4868600693262,5.4186527024273552,1.1974156414553714E-2,3.9032750355321024,-153193.76679003061,3417.5522991067669]
["KBM","KBM-25H03-C (400 V)",11.9,8.1999999999999993,7.4635291734146705,5.0090799821574974,3800,42.4,4459,1.66,9.1,90,0.76600000000000001,565,10,2428.9135688196961,4160.7603526307767,4355.5555555555547,7.042344231352808,146.86684073107048,0.83577298657083898,0.68981090611320761,3.7255890570217304E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.28493421958477033,0.41987649831484591,6.8384212700344875,20.154071919112603,15.084048811817976,23.054952121099216,2.4337260036463415,149.08825222337217,2.26347239484481E-2,7.5603860555854405,-151899.81983612682,2428.9135688196961,8.5524340414915093E-3,1.3338844680192115,-153609.0849452462,4160.7603526307767,5.1547426819193607,1.1974156414553714E-2,3.9032750355321024,-153193.76679003061,3417.5522991067669]
["KBM","KBM-25H03-C (480 V)",11.9,8.1999999999999993,5.2243241637149138,3.5062578279965866,4725,42.4,5351,1.66,9.1,90,0.76600000000000001,679,10,2428.9135688196961,4191.564491416907,4355.5555555555547,5.9779839594534536,146.86684073107048,0.83615629642282996,0.68981090611320761,3.7255890570217304E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.28493421958477033,0.41987649831484591,6.8384212700344875,20.154071919112603,15.084048811817976,23.054952121099216,2.4337260036463415,149.08825222337217,2.26347239484481E-2,7.5603860555854405,-151899.81983612682,2428.9135688196961,8.4598957961167526E-3,1.1896767258783445,-153620.31695333036,4191.564491416907,4.5974576836311574,1.1974156414553714E-2,3.9032750355321024,-153193.76679003061,3417.5522991067669]
["KBM","KBM-25H03-D (120 V)",11.9,10.24,10.663381187156988,8.9608245270226785,1200,42.6,1595,1.06,5.7,72.099999999999994,0.76600000000000001,160,10,1595,1595,1595,10.256327494596164,146.86684073107048,0.83555914027793809,0.68657235725821597,7.9826930704398918E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.35582029372537177,0.52433357838341743,8.5396870494089221,25.168011762404035,18.836665833294646,23.054952121099216,2.4337260036463415,149.08825222337217,1.4175455120792279E-2,4.8524866773580868,-152531.60437547549,3113.5879934132313,5.3913178962383193E-3,0.71133249754351313,-153639.66592852134,5272.7525463276661,5.3736687637724874,7.5687807866019865E-3,2.4934794349295584,-153364.993203094,4339.7179147854085]
["KBM","KBM-25H03-D (240 V)",11.9,10.24,9.1956189341983965,7.7274108690742835,2700,42.6,3338,1.06,5.7,72.099999999999994,0.76600000000000001,325,10,3113.5879934132313,3338,3338,8.5565837045756474,146.86684073107048,0.83551404675445362,0.68657235725821597,3.8143785042994691E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.35582029372537177,0.52433357838341743,8.5396870494089221,25.168011762404035,18.836665833294646,23.054952121099216,2.4337260036463415,149.08825222337217,1.4175455120792279E-2,4.8524866773580868,-152531.60437547549,3113.5879934132313,5.4382463304319664E-3,0.79314964287930156,-153633.74621297669,5242.7067088522444,5.9917457386755864,7.5687807866019865E-3,2.4934794349295584,-153364.993203094,4339.7179147854085]
["KBM","KBM-25H03-D (400 V)",11.9,10.199999999999999,5.0010749128257421,4.2025839603577664,4850,42.6,5560,1.06,5.7,72.099999999999994,0.76600000000000001,565,10,3121.6326928012982,5309.3687432366978,5436.8932038834955,4.3476418103557695,146.86684073107048,0.83617132878090661,0.68657235725821597,2.9300268811987981E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.35443037070300698,0.5222854003428572,8.5063288968721675,25.069699216457145,18.763085107383336,23.054952121099216,2.4337260036463415,149.08825222337217,1.4105458934623991E-2,4.833531651274658,-152540.43393730611,3121.6326928012982,5.3369637662603773E-3,0.60284659940540364,-153646.52234710159,5309.3687432366978,4.5541261670996818,7.5502984338194912E-3,2.4837392808868644,-153367.32463121318,4345.4875888859642]
["KBM","KBM-25H03-E (120 V)",11.8,12.7,10.269407475568853,10.80990260586195,1525,42.6,2006,0.69,3.6,57.4,0.76600000000000001,160,10,2006,2006,2006,9.7866435383548325,146.86684073107048,0.84261127908794187,0.68657235725821597,6.3471562549110808E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.44504039485165703,0.6558075154022599,10.680969476439769,31.478760739308473,23.559862514779358,23.054952121099216,2.4337260036463415,149.08825222337217,8.8965411141455411E-3,3.1452337211898,-152913.37664952004,3972.8357508514664,3.3767764324775722E-3,0.38057503238453844,-153653.01002233286,6689.4648679916218,5.5477729988906699,4.7738990849929726E-3,1.6161972455128073,-153465.79940751352,5503.0708483446288]
["KBM","KBM-25H03-E (240 V)",11.8,12.7,8.0747728480446916,8.4997608926786228,3400,42.6,4193,0.69,3.6,57.4,0.76600000000000001,325,10,3972.8357508514664,4193,4193,7.2059183976033507,146.86684073107048,0.84275731167487389,0.68657235725821597,3.036583698390562E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.44504039485165703,0.6558075154022599,10.680969476439769,31.478760739308473,23.559862514779358,23.054952121099216,2.4337260036463415,149.08825222337217,8.8965411141455411E-3,3.1452337211898,-152913.37664952004,3972.8357508514664,3.3774678314679625E-3,0.38217579070360652,-153652.91737675885,6688.5488286995205,5.571107802870408,4.7738990849929726E-3,1.6161972455128073,-153465.79940751352,5503.0708483446288]
["KBM","KBM-25H03-F (120 V)",11.75,14.79,9.936430230872384,12.20691674554347,1850,42,2347,0.51,2.7,49.4,0.76600000000000001,160,10,2347,2347,2347,9.4492171631662085,146.86684073107048,0.84616627487223339,0.69638053379047626,5.4249661045384007E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.52048476991322434,0.76698166663114897,12.491634477917383,36.815119998295152,27.553790087480809,23.054952121099216,2.4337260036463415,149.08825222337217,6.6296963679867288E-3,2.3069455819869047,-153118.79376831197,4634.981843088075,2.4839608818044093E-3,0.23534900718339147,-153658.32571883019,7817.8947162901541,5.3933004941987086,3.5783769413793641E-3,1.2023726748033967,-153515.89684625281,6384.0333901501353]
["KBM","KBM-25H03-F (240 V)",11.75,14.79,6.7427350280639562,8.2834582654348363,4100,42,4902,0.51,2.7,49.4,0.76600000000000001,325,10,4634.981843088075,4902,4902,5.7632651481876858,146.86684073107048,0.84655217346002876,0.69638053379047626,2.5973878921565947E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.52048476991322434,0.76698166663114897,12.491634477917383,36.815119998295152,27.553790087480809,23.054952121099216,2.4337260036463415,149.08825222337217,6.6296963679867288E-3,2.3069455819869047,-153118.79376831197,4634.981843088075,2.4656792051405228E-3,0.17934520424414416,-153660.70492240024,7858.0063287233515,4.1099071980719639,3.5783769413793641E-3,1.2023726748033967,-153515.89684625281,6384.0333901501353]
["KBM","KBM-25H03-G (120 V)",11.2,20,8.5422798546777301,14.856138877700401,2750,42,3324,0.28000000000000003,1.3,34.6,0.76600000000000001,160,10,3324,3324,3324,7.9875411770722824,146.86684073107048,0.88777550171842134,0.69638053379047626,3.8304438770612598E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.73839660563126464,1.0880945840476193,17.721518535150352,52.228540034285729,39.089760640381961,23.054952121099216,2.4337260036463415,149.08825222337217,3.1518043091219939E-3,1.2585081167795462,-153333.25,6778.1169748221164,1.1984438699627735E-3,3.2253932320982594E-2,-153663.78275331823,11309.953018095399,1.9221528187389829,1.7281315293213809E-3,0.65593041398520446,-153574.15304804896,9239.0682339022642]
["KBM","KBM-25H03-G (240 V)",11.2,20,3.5388569699256727,6.1545338607403011,5100,42,6937,0.28000000000000003,1.3,34.6,0.76600000000000001,325,10,6778.1169748221164,6937,6937,0.77934329419105808,146.86684073107048,0.88872046095037593,0.69638053379047626,1.8354325280887453E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.73839660563126464,1.0880945840476193,17.721518535150352,52.228540034285729,39.089760640381961,23.054952121099216,2.4337260036463415,149.08825222337217,3.1518043091219939E-3,1.2585081167795462,-153333.25,6778.1169748221164,1.2106810194487652E-3,-0.10467111968701767,-153661.71207622695,11309.264960412585,-6.2378095713954558,1.7281315293213809E-3,0.65593041398520446,-153574.15304804896,9239.0682339022642]
["KBM","KBM-25H03-H (120 V)",11,21.1,7.9793274858614645,15.198719020688504,2950,42.6,3642,0.25,1.1000000000000001,31.8,0.76600000000000001,160,10,3642,3642,3642,7.2707493910194758,146.86684073107048,0.90405347286784954,0.68657235725821597,3.4959899635781513E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.79317220837627478,1.168811418646061,19.036133001030596,56.102948095010923,41.989510156977566,23.054952121099216,2.4337260036463415,149.08825222337217,2.6725191589977554E-3,1.1251932683351202,-153351.00311224174,7367.4173284860999,1.0112404717056555E-3,5.9957202112164711E-4,-153663.99991112726,12326.74469637485,4.3542524250710812E-2,1.4498974350348659E-3,0.57818732156567576,-153581.35379859892,10094.561784353507]
["KBM","KBM-25H03-H (240 V)",11,21.1,3.0300652627110845,5.7715528813544461,5200,42.6,7600,0.25,1.1000000000000001,31.8,0.76600000000000001,325,10,7367.4173284860999,7600,7600,-0.64836615449918433,146.86684073107048,0.90498395068000814,0.68657235725821597,1.6753151904410034E-2,-22.701212863209879,9,29.247982419200003,9,-2366.2431040000001,7.5,2378.2431040000001,9,0.79317220837627478,1.168811418646061,19.036133001030596,56.102948095010923,41.989510156977566,23.054952121099216,2.4337260036463415,149.08825222337217,2.6725191589977554E-3,1.1251932683351202,-153351.00311224174,7367.4173284860999,1.0357633792879802E-3,-0.13670864363181437,-153659.37961976294,12246.228278814366,-9.9281474467140427,1.4498974350348659E-3,0.57818732156567576,-153581.35379859892,10094.561784353507]
["KBM","KBM-25H04-A (120 V)",14.82,5.5,13.687325105903,4.9772091294192728,450,54.4,685,4.08,23,167,1.02,160,10,685,685,685,13.095817105652344,110.29411764705883,0.67247406218329009,0.53860507764705878,0.18587438609272447,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.15352794145308343,0.2265387978407557,3.6846705948740022,10.873862296356274,8.1362351236552488,23.065318022925041,2.4426442922247182,149.63457997554386,7.222341182475106E-2,23.825973101413155,-148575.28227769674,1278.7882818883591,2.906696095120611E-2,3.8836994951700072,-153528.79327182058,2232.4032337460185,3.2908520444229445,3.5089475234723111E-2,9.6019790059766255,-152837.52718965168,1954.6784987020242]
["KBM","KBM-25H04-A (240 V)",14.82,5.5,13.187123856185615,4.7953177658856783,1050,54.4,1437,4.08,23,167,1.02,325,10,1278.7882818883591,1437,1437,12.585292363179741,110.29411764705883,0.67150340913534345,0.53860507764705878,8.860400450488258E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.15352794145308343,0.2265387978407557,3.6846705948740022,10.873862296356274,8.1362351236552488,23.065318022925041,2.4426442922247182,149.63457997554386,7.222341182475106E-2,23.825973101413155,-148575.28227769674,1278.7882818883591,2.9829546847520979E-2,4.9847368622416433,-153441.26342298227,2186.0094194731246,4.2238158524930487,3.5089475234723111E-2,9.6019790059766255,-152837.52718965168,1954.6784987020242]
["KBM","KBM-25H04-A (400 V)",14.82,5.5,12.032113697747288,4.3753140719081047,2000,54.4,2400,4.08,23,167,1.02,565,10,1278.7882818883591,2175.092493782206,2347.3053892215567,11.788044715225949,110.29411764705883,0.6713410454481159,0.53860507764705878,6.5138054446326532E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.15352794145308343,0.2265387978407557,3.6846705948740022,10.873862296356274,8.1362351236552488,23.065318022925041,2.4426442922247182,149.63457997554386,7.222341182475106E-2,23.825973101413155,-148575.28227769674,1278.7882818883591,3.0024273699432738E-2,5.2288591933188382,-153418.91261372267,2175.092493782206,4.4306728642968194,3.5089475234723111E-2,9.6019790059766255,-152837.52718965168,1954.6784987020242]
["KBM","KBM-25H04-A (480 V)",14.82,5.5,11.399472798957003,4.1452628359843651,2400,54.4,2888,4.08,23,167,1.02,679,10,1278.7882818883591,2175.3083435338385,2347.3053892215567,11.719707766786133,110.29411764705883,0.67137254610432695,0.53860507764705878,6.5138054446326532E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.15352794145308343,0.2265387978407557,3.6846705948740022,10.873862296356274,8.1362351236552488,23.065318022925041,2.4426442922247182,149.63457997554386,7.222341182475106E-2,23.825973101413155,-148575.28227769674,1278.7882818883591,3.0020369982609905E-2,5.2240772949933652,-153419.36068356642,2175.3083435338385,4.4266209236407059,3.5089475234723111E-2,9.6019790059766255,-152837.52718965168,1954.6784987020242]
["KBM","KBM-25H04-B (120 V)",14.9,6.2,13.641852265019601,5.5681029653141225,525,53.8,772,3.2,18,148,1.02,160,10,772,772,772,13.049923711609775,110.29411764705883,0.66872935963849933,0.54461182572490707,0.16492740216776719,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.17213863785814665,0.25399988896644293,4.1313273085955196,12.191994670389262,9.1225116302860147,23.065318022925041,2.4426442922247182,149.63457997554386,5.5291116436579142E-2,18.363692750852262,-149815.10012500337,1488.3686188128727,2.2765615054083959E-2,2.9500352209808911,-153564.67216256133,2533.2199812172807,3.596291446267303,2.7448116780994885E-2,7.4831895621485378,-153024.86872234469,2228.7727245063138]
["KBM","KBM-25H04-B (240 V)",14.9,6.2,13.130282805081366,5.359299104114843,1200,53.8,1618,3.2,18,148,1.02,325,10,1488.3686188128727,1618,1618,12.513831315518042,110.29411764705883,0.66780956553102322,0.54461182572490707,7.8692184470652821E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.17213863785814665,0.25399988896644293,4.1313273085955196,12.191994670389262,9.1225116302860147,23.065318022925041,2.4426442922247182,149.63457997554386,5.5291116436579142E-2,18.363692750852262,-149815.10012500337,1488.3686188128727,2.3365920452134509E-2,3.8426641876223324,-153495.46836127152,2482.1363157890073,4.6844662228232439,2.7448116780994885E-2,7.4831895621485378,-153024.86872234469,2228.7727245063138]
["KBM","KBM-25H04-B (400 V)",14.9,6.2,11.735024470642415,4.7898059063846592,2250,53.8,2704,3.2,18,148,1.02,565,10,1488.3686188128727,2474.1425475094811,2648.6486486486488,11.419733058217803,110.29411764705883,0.66774169876635758,0.54461182572490707,5.7127383637431792E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.17213863785814665,0.25399988896644293,4.1313273085955196,12.191994670389262,9.1225116302860147,23.065318022925041,2.4426442922247182,149.63457997554386,5.5291116436579142E-2,18.363692750852262,-149815.10012500337,1488.3686188128727,2.3467306863276863E-2,3.9736780670287875,-153483.78043530422,2474.1425475094811,4.8441809579222603,2.7448116780994885E-2,7.4831895621485378,-153024.86872234469,2228.7727245063138]
["KBM","KBM-25H04-B (480 V)",14.9,6.2,10.92863942564348,4.4606691533238694,2700,53.8,3245,3.2,18,148,1.02,679,10,1488.3686188128727,2476.0417866190878,2648.6486486486488,11.258053803022843,110.29411764705883,0.66780568892624259,0.54461182572490707,5.7127383637431792E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.17213863785814665,0.25399988896644293,4.1313273085955196,12.191994670389262,9.1225116302860147,23.065318022925041,2.4426442922247182,149.63457997554386,5.5291116436579142E-2,18.363692750852262,-149815.10012500337,1488.3686188128727,2.3443046209509603E-2,3.9427241386994654,-153486.57722751686,2476.0417866190878,4.8064460363567818,2.7448116780994885E-2,7.4831895621485378,-153024.86872234469,2228.7727245063138]
["KBM","KBM-25H04-C (120 V)",15.1,8.6300000000000008,13.687325105903,7.646550338493296,750,54.4,1060,1.66,9.6,108,1.02,160,10,1060,1060,1060,13.103419483009572,110.29411764705883,0.65934208598688981,0.53860507764705878,0.12011693818256251,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.23643229038950553,0.34886865757880797,5.6743749693481327,16.745695563782782,12.52976290326413,23.065318022925041,2.4426442922247182,149.63457997554386,2.9981511393068736E-2,9.6543984552800897,-151666.24173668306,2093.8958751652181,1.2078311157655085E-2,1.4519621607983648,-153618.81408358217,3506.7103491465787,4.6758742993646072,1.4638998014384744E-2,3.8907678980563576,-153339.53851944988,3106.3052194267198]
["KBM","KBM-25H04-C (240 V)",15.1,8.6300000000000008,12.638774892591691,7.0607680964199391,1700,54.4,2223,1.66,9.6,108,1.02,325,10,2093.8958751652181,2223,2223,11.8815862271949,110.29411764705883,0.65891901658787133,0.53860507764705878,5.7275733006530036E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.23643229038950553,0.34886865757880797,5.6743749693481327,16.745695563782782,12.52976290326413,23.065318022925041,2.4426442922247182,149.63457997554386,2.9981511393068736E-2,9.6543984552800897,-151666.24173668306,2093.8958751652181,1.2311718967845687E-2,1.8154541763515164,-153593.35798468723,3459.0909537136813,5.8464578169231292,1.4638998014384744E-2,3.8907678980563576,-153339.53851944988,3106.3052194267198]
["KBM","KBM-25H04-C (400 V)",15.1,8.6300000000000008,10.064655448858906,5.6227125412619587,3150,54.4,3707,1.66,9.6,108,1.02,565,10,2093.8958751652181,3463.1823413966049,3629.6296296296296,9.56402656115573,110.29411764705883,0.65906529861023588,0.53860507764705878,4.0988874395612156E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.23643229038950553,0.34886865757880797,5.6743749693481327,16.745695563782782,12.52976290326413,23.065318022925041,2.4426442922247182,149.63457997554386,2.9981511393068736E-2,9.6543984552800897,-151666.24173668306,2093.8958751652181,1.2290765966627306E-2,1.785848802773123,-153595.64317673256,3463.1823413966049,5.751117174325266,1.4638998014384744E-2,3.8907678980563576,-153339.53851944988,3106.3052194267198]
["KBM","KBM-25H04-C (480 V)",15.1,8.6300000000000008,8.0858978879934362,4.517261389940467,3850,54.4,4450,1.66,9.6,108,1.02,679,10,2093.8958751652181,3477.5732865809937,3629.6296296296296,8.7644015236193873,110.29411764705883,0.65928213238387923,0.53860507764705878,4.0988874395612156E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.23643229038950553,0.34886865757880797,5.6743749693481327,16.745695563782782,12.52976290326413,23.065318022925041,2.4426442922247182,149.63457997554386,2.9981511393068736E-2,9.6543984552800897,-151666.24173668306,2093.8958751652181,1.2218355273905961E-2,1.679523464171863,-153603.54048639609,3477.5732865809937,5.4087088584890566,1.4638998014384744E-2,3.8907678980563576,-153339.53851944988,3106.3052194267198]
["KBM","KBM-25H04-D (120 V)",15,10.7,13.369015219719209,9.284038347027229,1000,54.8,1325,1.08,6.2,87,1.02,160,10,1325,1325,1325,12.838945166127953,110.29411764705883,0.66350141331670909,0.53467365372262776,9.6093550546050011E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.29509745197553033,0.43543228277333329,7.0823388474127276,20.900749573119999,15.638731496951603,23.065318022925041,2.4426442922247182,149.63457997554386,1.9646805771190295E-2,6.361751671399408,-152327.23542315519,2627.2716701826521,7.7956048882860483E-3,0.87139954541850662,-153638.91950165955,4383.8760334509388,5.354435527023119,9.5020582164081994E-3,2.5451018036521531,-153450.05023150504,3886.9062584152575]
["KBM","KBM-25H04-D (240 V)",15,10.7,11.777465788800255,8.1787956866668434,2250,54.8,2776,1.08,6.2,87,1.02,325,10,2627.2716701826521,2776,2776,11.024108902093115,110.29411764705883,0.6633059561693716,0.53467365372262776,4.5865977836281074E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.29509745197553033,0.43543228277333329,7.0823388474127276,20.900749573119999,15.638731496951603,23.065318022925041,2.4426442922247182,149.63457997554386,1.9646805771190295E-2,6.361751671399408,-152327.23542315519,2627.2716701826521,7.899837578543397E-3,1.0529072320323314,-153627.38308761836,4343.7268349425221,6.46973471525724,9.5020582164081994E-3,2.5451018036521531,-153450.05023150504,3886.9062584152575]
["KBM","KBM-25H04-D (400 V)",15,10.7,6.9376214952587638,4.8177927050408087,4150,54.8,4626,1.08,6.2,87,1.02,565,10,2627.2716701826521,4384.0602005486962,4505.7471264367814,6.4829029579770214,110.29411764705883,0.66380824146447315,0.53467365372262776,3.2757145659959373E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.29509745197553033,0.43543228277333329,7.0823388474127276,20.900749573119999,15.638731496951603,23.065318022925041,2.4426442922247182,149.63457997554386,1.9646805771190295E-2,6.361751671399408,-152327.23542315519,2627.2716701826521,7.7951457174341241E-3,0.87051623665072408,-153638.9703224246,4384.0602005486962,5.3490079136253241,9.5020582164081994E-3,2.5451018036521531,-153450.05023150504,3886.9062584152575]
["KBM","KBM-25H04-D (480 V)",15,10.7,4.0432128096111288,2.8077866733410617,4700,54.8,5551,1.08,6.2,87,1.02,679,10,2627.2716701826521,4415.6954329426435,4505.7471264367814,4.7059925199309376,110.29411764705883,0.66419098632337059,0.53467365372262776,3.2757145659959373E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.29509745197553033,0.43543228277333329,7.0823388474127276,20.900749573119999,15.638731496951603,23.065318022925041,2.4426442922247182,149.63457997554386,1.9646805771190295E-2,6.361751671399408,-152327.23542315519,2627.2716701826521,7.7192966386971963E-3,0.70967143686942813,-153647.36525471302,4415.6954329426435,4.3606747032008597,9.5020582164081994E-3,2.5451018036521531,-153450.05023150504,3886.9062584152575]
["KBM","KBM-25H04-E (120 V)",14.6,13.8,12.584608714480584,11.65241547637091,1400,53.8,1837,0.65,3.5,65.5,1.02,160,10,1837,1837,1837,11.955518720357738,110.29411764705883,0.68152596523731079,0.54461182572490707,6.9310808096633786E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.39102018025179103,0.5769714667397261,9.3844843260429851,27.694630403506853,20.722170143829107,23.065318022925041,2.4426442922247182,149.63457997554386,1.0803707883045573E-2,3.7499354350619143,-152844.58296328111,3591.758642260118,4.3823648527384126E-3,0.44594655851381121,-153652.41161161644,5870.6165566707805,6.047383807448881,5.3718459868918938E-3,1.5280955789833675,-153527.93123369801,5205.6963630102255]
["KBM","KBM-25H04-E (240 V)",14.6,13.8,9.9719703688069501,9.233305897043472,3050,53.8,3681,0.65,3.5,65.5,1.02,325,10,3591.758642260118,3681,3681,9.014499320517503,110.29411764705883,0.6816067465069463,0.54461182572490707,3.4589501351131827E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.39102018025179103,0.5769714667397261,9.3844843260429851,27.694630403506853,20.722170143829107,23.065318022925041,2.4426442922247182,149.63457997554386,1.0803707883045573E-2,3.7499354350619143,-152844.58296328111,3591.758642260118,4.3881039049424352E-3,0.45962862305915048,-153651.68961767174,5865.2499807781651,6.2329232941974766,5.3718459868918938E-3,1.5280955789833675,-153527.93123369801,5205.6963630102255]
["KBM","KBM-25H04-E (400 V)",14.6,13.8,4.5670548887239537,4.2287545265962532,4600,53.8,6135,0.65,3.5,65.5,1.02,565,10,3591.758642260118,5937.8229472675985,5984.7328244274813,1.6491626716497461,110.29411764705883,0.6822964550157895,0.54461182572490707,2.4458582597754592E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.39102018025179103,0.5769714667397261,9.3844843260429851,27.694630403506853,20.722170143829107,23.065318022925041,2.4426442922247182,149.63457997554386,1.0803707883045573E-2,3.7499354350619143,-152844.58296328111,3591.758642260118,4.3174200170493712E-3,0.24219375527942125,-153660.58191159627,5937.8229472675985,3.2843365779593707,5.3718459868918938E-3,1.5280955789833675,-153527.93123369801,5205.6963630102255]
["KBM","KBM-25H04-F (120 V)",14.5,19.399999999999999,11.793381283109445,15.316079588453825,2000,54.1,2495,0.33,1.8,46.3,1.02,160,10,2495,2495,2495,11.123493150679034,110.29411764705883,0.68614576437503672,0.541591797116451,5.1031645079565639E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.55348603625445902,0.81669864187586205,13.283664870107017,39.20153481004138,29.332071322029758,23.065318022925041,2.4426442922247182,149.63457997554386,5.6340120734180987E-3,1.9155193835389135,-153236.09128783623,5047.9819894634711,2.1583274594738104E-3,0.12404711036354542,-153662.20546748952,8409.0272861507765,4.6873900491254776,2.7168673006891337E-3,0.77624406126689915,-153593.72924692329,7377.3697288757721]
["KBM","KBM-25H04-F (240 V)",14.5,19.399999999999999,4.8481044203377346,6.2962395069321229,4550,54.1,5206,0.33,1.8,46.3,1.02,325,10,5047.9819894634711,5206,5206,3.4565344202809332,110.29411764705883,0.68695465989133198,0.541591797116451,2.4457156064832168E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.55348603625445902,0.81669864187586205,13.283664870107017,39.20153481004138,29.332071322029758,23.065318022925041,2.4426442922247182,149.63457997554386,5.6340120734180987E-3,1.9155193835389135,-153236.09128783623,5047.9819894634711,2.1449049110676211E-3,-3.5737654290870384E-2,-153663.85105356487,8472.4553689827499,-1.350425049089587,2.7168673006891337E-3,0.77624406126689915,-153593.72924692329,7377.3697288757721]
["KBM","KBM-25H04-G (120 V)",14,20.3,11.77006323330761,16.577553849729028,2150,54.5,2701,0.3,1.5,42.8,1.02,160,10,2701,2701,2701,11.198577113099468,110.29411764705883,0.71034700669247208,0.53761681144954132,4.7139561078680586E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.59984762434278371,0.88510767760000009,14.396342984226809,42.485168524800002,31.789010285859575,23.065318022925041,2.4426442922247182,149.63457997554386,4.7209896331133934E-3,1.7574790454747957,-153242.46583281251,5514.2570011714552,1.8531850785698056E-3,0.15106157794804662,-153660.88569957908,9065.221183557007,6.7924799604761965,2.2993544513037248E-3,0.70697272323670923,-153595.78847069058,8020.8105557357767]
["KBM","KBM-25H04-G (240 V)",14,20.3,4.8473059841683774,6.8271915269977148,4600,54.5,5637,0.3,1.5,42.8,1.02,325,10,5514.2570011714552,5637,5637,2.7839703984254651,110.29411764705883,0.71142266464876436,0.53761681144954132,2.2587183692303756E-2,-22.765575585185182,9,29.300116224,9,-2371.56288,7.5,2383.56288,9,0.59984762434278371,0.88510767760000009,14.396342984226809,42.485168524800002,31.789010285859575,23.065318022925041,2.4426442922247182,149.63457997554386,4.7209896331133934E-3,1.7574790454747957,-153242.46583281251,5514.2570011714552,1.8348482714517621E-3,-5.6710522568628755E-2,-153663.56108566115,9166.8210548026746,-2.5499871862057759,2.2993544513037248E-3,0.70697272323670923,-153595.78847069058,8020.8105557357767]
["KBM","KBM-35H01-A (120 V)",12.6,5.41,11.650141834326739,4.9156716600534764,500,40.799999999999997,798,4.13,32,144,1.52,160,10,798,798,798,11.084026367585476,74.013157894736835,0.79132310956208407,0.72065543686274514,0.15955382766104795,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.1777807441558695,0.26301063701693123,4.2667378597408678,12.6245105768127,9.4412180721564702,23.085777508955925,2.4601999784026272,150.71002830659057,8.5350833684642746E-2,18.045131622824574,-149738.13706494667,1223.0318494915673,2.2931403343415226E-2,3.3262209868483215,-153530.61185796018,2516.0015688726317,3.2290734835570714,3.9503849956045209E-2,9.7252595374277639,-152523.70446240439,1845.6977003245859]
["KBM","KBM-35H01-A (240 V)",12.6,5.41,11.459155902616464,4.8350868787411239,1200,40.799999999999997,1675,4.13,32,144,1.52,325,10,1223.0318494915673,1675,1675,11.007571780735482,74.013157894736835,0.78999857993338463,0.72065543686274514,7.6014301178218668E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.1777807441558695,0.26301063701693123,4.2667378597408678,12.6245105768127,9.4412180721564702,23.085777508955925,2.4601999784026272,150.71002830659057,8.5350833684642746E-2,18.045131622824574,-149738.13706494667,1223.0318494915673,2.4725920104490172E-2,4.4841077355320698,-153421.58075106266,2401.9349895356108,4.3531423328368373,3.9503849956045209E-2,9.7252595374277639,-152523.70446240439,1845.6977003245859]
["KBM","KBM-35H01-A (400 V)",12.6,5.41,10.926171907145932,4.6101991169392118,2150,40.799999999999997,2795,4.13,32,144,1.52,565,10,1223.0318494915673,2376.5134786033295,2722.2222222222222,10.749825570449953,74.013157894736835,0.78975874655523381,0.72065543686274514,6.8984186549685231E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.1777807441558695,0.26301063701693123,4.2667378597408678,12.6245105768127,9.4412180721564702,23.085777508955925,2.4601999784026272,150.71002830659057,8.5350833684642746E-2,18.045131622824574,-149738.13706494667,1223.0318494915673,2.5170734542057597E-2,4.7274588048231685,-153394.55475078005,2376.5134786033295,4.5893859522927141,3.9503849956045209E-2,9.7252595374277639,-152523.70446240439,1845.6977003245859]
["KBM","KBM-35H01-A (480 V)",12.6,5.41,10.504226244065093,4.4321629721793636,2700,40.799999999999997,3353,4.13,32,144,1.52,679,10,1223.0318494915673,2374.1594881620031,2722.2222222222222,10.757147723076379,74.013157894736835,0.7897555268179578,0.72065543686274514,6.8984186549685231E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.1777807441558695,0.26301063701693123,4.2667378597408678,12.6245105768127,9.4412180721564702,23.085777508955925,2.4601999784026272,150.71002830659057,8.5350833684642746E-2,18.045131622824574,-149738.13706494667,1223.0318494915673,2.5212777695955181E-2,4.7498150947366824,-153392.00029617347,2374.1594881620031,4.6110892916787254,3.9503849956045209E-2,9.7252595374277639,-152523.70446240439,1845.6977003245859]
["KBM","KBM-35H01-B (120 V)",12.45,6.1,11.632779476898532,5.5394187985231103,550,41.4,901,3.3,25,127,1.52,160,10,901,901,901,11.111244197610141,74.013157894736835,0.80029728185205162,0.71021115516908218,0.1413140449206618,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.20287030555968985,0.30012838876572961,4.8688873334325562,14.406162660755021,10.773623455388226,23.085777508955925,2.4601999784026272,150.71002830659057,6.9005192470452642E-2,14.724451059951607,-150303.44666413122,1373.0151110400286,1.7732973108812052E-2,2.5645287194197586,-153562.05927905126,2871.3138733588553,3.532883193752145,3.1045334387135984E-2,7.8206001297805194,-152715.99041493703,2095.5299156968172]
["KBM","KBM-35H01-B (240 V)",12.45,6.1,11.275515583664278,5.3692931350782276,1300,41.4,1892,3.3,25,127,1.52,325,10,1373.0151110400286,1892,1892,10.740673449456011,74.013157894736835,0.79946535300570409,0.71021115516908218,6.7295959024057217E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.20287030555968985,0.30012838876572961,4.8688873334325562,14.406162660755021,10.773623455388226,23.085777508955925,2.4601999784026272,150.71002830659057,6.9005192470452642E-2,14.724451059951607,-150303.44666413122,1373.0151110400286,1.8948868779574017E-2,3.4003488537781155,-153484.78287049118,2757.7297708727929,4.6843052399604641,3.1045334387135984E-2,7.8206001297805194,-152715.99041493703,2095.5299156968172]
["KBM","KBM-35H01-B (400 V)",12.45,6.1,10.646449810232319,5.0697380048725327,2350,41.4,3153,3.3,25,127,1.52,565,10,1373.0151110400286,2724.9402708575922,3086.6141732283463,10.358695088250721,74.013157894736835,0.7992713614818554,0.71021115516908218,6.0759788500169325E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.20287030555968985,0.30012838876572961,4.8688873334325562,14.406162660755021,10.773623455388226,23.085777508955925,2.4601999784026272,150.71002830659057,6.9005192470452642E-2,14.724451059951607,-150303.44666413122,1373.0151110400286,1.933636059122246E-2,3.626460236670805,-153460.15577766518,2724.9402708575922,4.9957952609099578,3.1045334387135984E-2,7.8206001297805194,-152715.99041493703,2095.5299156968172]
["KBM","KBM-35H01-B (480 V)",12.45,6.1,10.207868763825012,4.8608898875357198,2900,41.4,3783,3.3,25,127,1.52,679,10,1373.0151110400286,2721.9561594250072,3086.6141732283463,10.345523128087684,74.013157894736835,0.79927946347065026,0.71021115516908218,6.0759788500169325E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.20287030555968985,0.30012838876572961,4.8688873334325562,14.406162660755021,10.773623455388226,23.085777508955925,2.4601999784026272,150.71002830659057,6.9005192470452642E-2,14.724451059951607,-150303.44666413122,1373.0151110400286,1.9372456275620578E-2,3.6468092638449914,-153457.86171171701,2721.9561594250072,5.0238279889385034,3.1045334387135984E-2,7.8206001297805194,-152715.99041493703,2095.5299156968172]
["KBM","KBM-35H01-C (120 V)",12.45,8.32,11.482589759268032,7.5049606269725704,815,40.799999999999997,1242,1.75,13.4,93,1.52,160,10,1242,1242,1242,10.975738013510302,74.013157894736835,0.79987017932088456,0.72065543686274514,0.10251526125081825,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.2767017938125606,0.40935544172637223,6.640843051501454,19.649061202865866,14.694515926037713,23.085777508955925,2.4601999784026272,150.71002830659057,3.6096094692917982E-2,7.6859182800421619,-151956.48063916387,1948.0695590381824,9.5069223338159915E-3,1.3588501263301223,-153610.62753885341,3948.8412916595526,4.820476105837499,1.6621208942611279E-2,4.1422557407298264,-153168.03854140337,2913.6063346899114]
["KBM","KBM-35H01-C (240 V)",12.45,8.32,10.976501238239955,7.1741838158431079,1840,40.799999999999997,2600,1.75,13.4,93,1.52,325,10,1948.0695590381824,2600,2600,10.367882184469501,74.013157894736835,0.79931892482999833,0.72065543686274514,4.8970751720583176E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.2767017938125606,0.40935544172637223,6.640843051501454,19.649061202865866,14.694515926037713,23.085777508955925,2.4601999784026272,150.71002830659057,3.6096094692917982E-2,7.6859182800421619,-151956.48063916387,1948.0695590381824,1.004127976823984E-2,1.7310548471013316,-153577.38446977476,3825.5843320865429,6.1408601041840871,1.6621208942611279E-2,4.1422557407298264,-153168.03854140337,2913.6063346899114]
["KBM","KBM-35H01-C (400 V)",12.45,8.32,9.6876921882023268,6.3318249596093636,3450,40.799999999999997,4334,1.75,13.4,93,1.52,565,10,1948.0695590381824,3809.476529532737,4215.0537634408602,9.3998704995976325,74.013157894736835,0.79931871712303781,0.72065543686274514,4.3699779533554271E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.2767017938125606,0.40935544172637223,6.640843051501454,19.649061202865866,14.694515926037713,23.085777508955925,2.4601999784026272,150.71002830659057,3.6096094692917982E-2,7.6859182800421619,-151956.48063916387,1948.0695590381824,1.0115950451454019E-2,1.776868526393804,-153572.73910972109,3809.476529532737,6.3033826238281794,1.6621208942611279E-2,4.1422557407298264,-153168.03854140337,2913.6063346899114]
["KBM","KBM-35H01-C (480 V)",12.45,8.32,8.8330993416001924,5.7732675435295375,4200,40.799999999999997,5201,1.75,13.4,93,1.52,679,10,1948.0695590381824,3819.9300660591666,4215.0537634408602,9.1604029592927088,74.013157894736835,0.79940502223000731,0.72065543686274514,4.3699779533554271E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.2767017938125606,0.40935544172637223,6.640843051501454,19.649061202865866,14.694515926037713,23.085777508955925,2.4601999784026272,150.71002830659057,3.6096094692917982E-2,7.6859182800421619,-151956.48063916387,1948.0695590381824,1.0067362518938132E-2,1.7471942644427734,-153575.76182802342,3819.9300660591666,6.1981141560835962,1.6621208942611279E-2,4.1422557407298264,-153168.03854140337,2913.6063346899114]
["KBM","KBM-35H01-D (120 V)",12.65,10.57,11.589373583328015,9.4222549457951352,1100,41.2,1556,1.08,8.5,74,1.52,160,10,1556,1556,1556,11.149695723325811,74.013157894736835,0.78688950622702114,0.71365878213592226,8.1827734237478314E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.34597320243096896,0.51183626660026349,8.3033568583432551,24.568140796812649,18.373240964776734,23.085777508955925,2.4601999784026272,150.71002830659057,2.3081960173350388E-2,4.7653826622573376,-152627.25456913153,2470.3032777851363,5.9996264964296275E-3,0.82182382998011749,-153633.16570455063,4992.3218640052155,5.9369395578762525,1.0490964939276107E-2,2.5433250771078737,-153368.68852959067,3704.20186270568]
["KBM","KBM-35H01-D (240 V)",12.65,10.57,10.757574928986886,8.745995877225111,2450,41.2,3252,1.08,8.5,74,1.52,325,10,2470.3032777851363,3252,3252,10.138095375128716,74.013157894736835,0.78662446663531671,0.71365878213592226,3.9152507525681508E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.34597320243096896,0.51183626660026349,8.3033568583432551,24.568140796812649,18.373240964776734,23.085777508955925,2.4601999784026272,150.71002830659057,2.3081960173350388E-2,4.7653826622573376,-152627.25456913153,2470.3032777851363,6.2599230279906121E-3,1.0055522310922813,-153617.83787027691,4874.1099677034554,7.2642123536706382,1.0490964939276107E-2,2.5433250771078737,-153368.68852959067,3704.20186270568]
["KBM","KBM-35H01-D (400 V)",12.65,10.57,8.4999233343583658,6.9105067759011103,4550,41.2,5420,1.08,8.5,74,1.52,565,10,2470.3032777851363,4898.7690987405831,5297.2972972972975,8.1818093786704189,74.013157894736835,0.78681748777066873,0.71365878213592226,3.4372844459538809E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.34597320243096896,0.51183626660026349,8.3033568583432551,24.568140796812649,18.373240964776734,23.085777508955925,2.4601999784026272,150.71002830659057,2.3081960173350388E-2,4.7653826622573376,-152627.25456913153,2470.3032777851363,6.20366704898845E-3,0.96880032860589516,-153621.15056260469,4898.7690987405831,6.9987128442393836,1.0490964939276107E-2,2.5433250771078737,-153368.68852959067,3704.20186270568]
["KBM","KBM-35H01-D (480 V)",12.65,10.57,6.1741141716683536,5.0196050176165476,5800,41.2,6505,1.08,8.5,74,1.52,679,10,2470.3032777851363,4959.4986865065393,5297.2972972972975,7.1125608173142911,74.013157894736835,0.78710013988161198,0.71365878213592226,3.4372844459538809E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.34597320243096896,0.51183626660026349,8.3033568583432551,24.568140796812649,18.373240964776734,23.085777508955925,2.4601999784026272,150.71002830659057,2.3081960173350388E-2,4.7653826622573376,-152627.25456913153,2470.3032777851363,6.0695197202148927E-3,0.87495456126241389,-153629.04996876032,4959.4986865065393,6.3207614048241441,1.0490964939276107E-2,2.5433250771078737,-153368.68852959067,3704.20186270568]
["KBM","KBM-35H01-E (120 V)",12.2,12.8,10.777063289365486,11.226107593089049,1400,41.1,1996,0.74,5.4,57.8,1.52,160,10,1996,1996,1996,10.171298803981079,74.013157894736835,0.8160426682647699,0.71539517819951337,6.3789556349457044E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.43441832698188892,0.64268288139890717,10.426039847565335,30.848778307147544,23.070204701030207,23.085777508955925,2.4601999784026272,150.71002830659057,1.4489686842120434E-2,3.1945680687306601,-152900.32491037034,3140.0728816593228,3.5842248470563456E-3,0.47200210952729532,-153647.32859465,6481.8265441972562,6.3712369071742074,6.5320025282322577E-3,1.7091163685737738,-153445.41135453008,4717.7242530762242]
["KBM","KBM-35H01-E (240 V)",12.2,12.8,9.5955028593145926,9.9953154784527012,3100,41.1,4166,0.74,5.4,57.8,1.52,325,10,3140.0728816593228,4166,4166,8.6998919070659984,74.013157894736835,0.81578075451427556,0.71539517819951337,3.0562639095899249E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.43441832698188892,0.64268288139890717,10.426039847565335,30.848778307147544,23.070204701030207,23.085777508955925,2.4601999784026272,150.71002830659057,1.4489686842120434E-2,3.1945680687306601,-152900.32491037034,3140.0728816593228,3.689555911852562E-3,0.56497997359066743,-153640.11361434861,6376.9428756120224,7.6262821434424275,6.5320025282322577E-3,1.7091163685737738,-153445.41135453008,4717.7242530762242]
["KBM","KBM-35H01-E (400 V)",12.2,12.8,5.1268764455012183,5.3404962973971024,6100,41.1,6943,0.74,5.4,57.8,1.52,565,10,3140.0728816593228,6524.9228409219431,6782.0069204152251,4.6341663217357203,74.013157894736835,0.81625554335822492,0.71539517819951337,2.6988426547078035E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.43441832698188892,0.64268288139890717,10.426039847565335,30.848778307147544,23.070204701030207,23.085777508955925,2.4601999784026272,150.71002830659057,1.4489686842120434E-2,3.1945680687306601,-152900.32491037034,3140.0728816593228,3.5430287252557055E-3,0.43020518341046066,-153650.15045169528,6524.9228409219431,5.8070485001590253,6.5320025282322577E-3,1.7091163685737738,-153445.41135453008,4717.7242530762242]
["KBM","KBM-35H01-F (120 V)",12.4,14.58,11.071215728829969,12.725535320494217,1600,41.1,2288,0.56999999999999995,4.4000000000000004,52.6,1.52,160,10,2288,2288,2288,10.499838492226855,74.013157894736835,0.80258928461031376,0.71539517819951337,5.5648581500662701E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.48684850258461726,0.72024861524516126,11.684364062030815,34.571933531767741,25.854559799650001,23.085777508955925,2.4601999784026272,150.71002830659057,1.2063253765421899E-2,2.5095675373278952,-153094.92920741139,3459.946232924819,2.9772247416614862E-3,0.37759737978873181,-153651.11671944591,7120.7948783069487,7.2712276988300211,5.4277188389068552E-3,1.3426362700084025,-153501.11343290147,5195.7396226611681]
["KBM","KBM-35H01-F (240 V)",12.4,14.58,9.4962449378164226,10.915224066455659,3600,41.1,4576,0.56999999999999995,4.4000000000000004,52.6,1.52,325,10,3459.946232924819,4576,4576,8.7090046765133202,74.013157894736835,0.80255492710033682,0.71539517819951337,2.7824290750331351E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.48684850258461726,0.72024861524516126,11.684364062030815,34.571933531767741,25.854559799650001,23.085777508955925,2.4601999784026272,150.71002830659057,1.2063253765421899E-2,2.5095675373278952,-153094.92920741139,3459.946232924819,3.0318624896363763E-3,0.42378560420389039,-153647.77215241559,7049.2804928002743,8.1606541480156203,5.4277188389068552E-3,1.3426362700084025,-153501.11343290147,5195.7396226611681]
["KBM","KBM-35H01-F (400 V)",12.4,14.58,3.7039695846841094,4.2574363042346084,6600,41.1,7200,0.56999999999999995,4.4000000000000004,52.6,1.52,565,10,3459.946232924819,7200,7200,2.9134213651099383,74.013157894736835,0.80329039227181487,0.71539517819951337,2.4505453259858149E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.48684850258461726,0.72024861524516126,11.684364062030815,34.571933531767741,25.854559799650001,23.085777508955925,2.4601999784026272,150.71002830659057,1.2063253765421899E-2,2.5095675373278952,-153094.92920741139,3459.946232924819,2.8553485020913318E-3,0.24497850269222521,-153658.57718895195,7293.0502228390733,4.7174439488702458,5.4277188389068552E-3,1.3426362700084025,-153501.11343290147,5195.7396226611681]
["KBM","KBM-35H01-G (120 V)",12.4,20.100000000000001,10.605814505613111,16.834626199385891,2350,41.2,3026,0.3,2.2000000000000002,38.1,1.52,160,10,3026,3026,3026,10.089699869780969,74.013157894736835,0.80249293188240201,0.71365878213592226,4.2076653824691432E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.6711697463615095,0.99293533377419363,16.108073912676229,47.660896021161292,35.643117419270581,23.085777508955925,2.4601999784026272,150.71002830659057,5.8902206027177956E-3,1.3221430488509529,-153362.94423405308,4991.6363046666393,1.5140342757535077E-3,0.15679480852903671,-153659.765975024,10022.591147644687,7.9199934306015045,2.7159248304641989E-3,0.70563894024695661,-153578.24585219292,7391.0089572593151]
["KBM","KBM-35H01-G (240 V)",12.4,20.100000000000001,7.1259373576805212,11.31101167885797,5300,41.2,6316,0.3,2.2000000000000002,38.1,1.52,325,10,4991.6363046666393,6316,6316,6.1149095002094658,74.013157894736835,0.80282609254347403,0.71365878213592226,2.0158954159834749E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.6711697463615095,0.99293533377419363,16.108073912676229,47.660896021161292,35.643117419270581,23.085777508955925,2.4601999784026272,150.71002830659057,5.8902206027177956E-3,1.3221430488509529,-153362.94423405308,4991.6363046666393,1.4824188195792208E-3,0.11015201660221281,-153661.91034321176,10144.084169031068,5.5639804406883382,2.7159248304641989E-3,0.70563894024695661,-153578.24585219292,7391.0089572593151]
["KBM","KBM-35H01-H (120 V)",12.2,21.2,10.313240312354818,17.450491222258577,2500,41.4,3237,0.27,1.6,35.700000000000003,1.52,160,10,3237,3237,3237,9.7570235564370194,74.013157894736835,0.81565380419963995,0.71021115516908218,3.9333937124966412E-2,-22.892273856790123,9,29.402741824,9,-2382.0348799999997,7.5,2394.0348799999997,9,0.71950535406375338,1.0644435223169399,17.268128497530082,51.093289071213114,38.210026536081273,23.085777508955925,2.4601999784026272,150.71002830659057,3.9987667004109289E-3,1.2010718241405245,-153381.0292574394,6044.9498918775498,1.3014497319819411E-3,0.11948163479422873,-153661.1996914348,10820.161396958167,7.1566297345849677,2.0430064216224635E-3,0.63792547684830181,-153584.17416495772,8515.6660268360665]
["KBM","KBM-35H01-H (240 V)",12.2,21.2,6.3605136185653901,10.762290386743469,5600,41.4,6756,0.27,1.6,35.700000000000003,1.52,325,10,{"$f":"IF(AQ635<I635,IF(AQ635<0,0,AQ635),I635)","v":6044.9498918775498},{"$f":"IF(AU635<I635,IF(AU635<0,0,AU635),I635)","v":6756},{"$f":"IF(UAC_V*0.98/L635*1000<I635,IF(UAC_V*0.98/L635*1000<0,0,UAC_V*0.98/L635*1000),I635)","v":6756},{"$f":"C635+(E635-C635)/G635*Q635","v":5.1550767869692455},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M635,(inertia/gear^2+gear_inertia)/M635),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M635,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M635))","v":74.013157894736835},{"$f":"IF((C635+(E635-C635)/G635*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X635^2*time1+Y635^2*time2+Z635^2*time3+AA635^2*time4)/time)/(C635+(E635-C635)/G635*mspeed),SQRT((((X635-Y635)*2/PI()+Y635)^2*time1+Y635^2*time2+((Z635-Y635)*2/PI()+Y635)^2*time3+AA635^2*time4)/time)/(C635+(E635-C635)/G635*mspeed)),IF(AccType=1,SQRT((X635^2*time1+Y635^2*time2+Z635^2*time3+AA635^2*time4+AB635^2*time5+AC635^2*time6+AD635^2*time7+AE635^2*time8)/time)/(C635+(E635-C635)/G635*mspeed),SQRT((((X635-Y635)*2/PI()+Y635)^2*time1+Y635^2*time2+((Z635-Y635)*2/PI()+Y635)^2*time3+AA635^2*time4+((AB635-AC635)*2/PI()+AC635)^2*time5+AC635^2*time6+((AD635-AC635)*2/PI()+AC635)^2*time7+AE635^2*time8)/time)/(C635+(E635-C635)/G635*mspeed))))","v":0.81608189342407633},{"$f":"IF(move1,MAX(ABS(X635),ABS(Z635))/H635,MAX(ABS(X635),ABS(Z635),ABS(AB635),ABS(AD635))/H635)","v":0.71021115516908218},{"$f":"IF(AZ635>0,speed/(MIN(AZ635,I635)),\"NA\")","v":1.8846056020354687E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M635+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M635+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.892273856790123},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M635+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M635+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.402741824},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M635+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M635+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2382.0348799999997},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M635+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M635+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2394.0348799999997},9,{"$f":"AH635/Irms","v":0.71950535406375338},{"$f":"AI635/Ipeak","v":1.0644435223169399},{"$f":"IF(move1,IF(AccType=1,SQRT((X635^2*time1+Y635^2*time2+Z635^2*time3+AA635^2*time4)/time)/(C635/D635),SQRT((((X635-Y635)*2/PI()+Y635)^2*time1+Y635^2*time2+((Z635-AA635)*2/PI()+AA635)^2*time3+AA635^2*time4)/time)/(C635/D635)),IF(AccType=1,SQRT((X635^2*time1+Y635^2*time2+Z635^2*time3+AA635^2*time4+AB635^2*time5+AC635^2*time6+AD635^2*time7+AE635^2*time8)/time)/(C635/D635),SQRT((((X635-Y635)*2/PI()+Y635)^2*time1+Y635^2*time2+((Z635-AA635)*2/PI()+AA635)^2*time3+AA635^2*time4+((AB635-AC635)*2/PI()+AC635)^2*time5+AC635^2*time6+((AD635-AE635)*2/PI()+AE635)^2*time7+AE635^2*time8)/time)/(C635/D635)))","v":17.268128497530082},{"$f":"IF(move1,MAX(ABS(X635),ABS(Z635))/(C635/D635),MAX(ABS(X635),ABS(Z635),ABS(AB635),ABS(AD635))/(C635/D635))","v":51.093289071213114},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X635),ABS(Z635))/(C635/D635),MAX(ABS((X635-Y635)*2/PI()+Y635),ABS((Z635-Y635)*2/PI()+Y635))/(C635/D635)),IF(AccType=1,MAX(ABS(X635),ABS(Z635),ABS(AB635),ABS(AD635))/(C635/D635),MAX(ABS((X635-Y635)*2/PI()+Y635),ABS((Z635-Y635)*2/PI()+Y635),ABS((AB635-AC635)*2/PI()+AC635),ABS((AD635-AC635)*2/PI()+AC635))/(C635/D635)))","v":38.210026536081273},{"$f":"IF((C635+(E635-C635)/G635*mspeed)<0,\"NA\",U635*(C635+(E635-C635)/G635*mspeed)*mspeed/9.55)","v":23.085777508955925},{"$f":"IF(move1,IF(speed1>speed2,AM635/2*time1/time,AM635/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z635*-speed/30*PI(),((Z635-AA635)*2/PI()+AA635)*-speed/30*PI()),IF(AccType=1,X635*-speed/30*PI(),((X635-Y635)*2/PI()+Y635)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z635*-speed/30*PI(),((Z635-AA635)*2/PI()+AA635)*-speed/30*PI()),IF(AccType=1,X635*-speed/30*PI(),((X635-Y635)*2/PI()+Y635)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD635*-speed/30*PI(),((AD635-AE635)*2/PI()+AE635)*-speed/30*PI()),IF(AccType=1,AB635*-speed/30*PI(),((AB635-AC635)*2/PI()+AC635)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD635*-speed/30*PI(),((AD635-AE635)*2/PI()+AE635)*-speed/30*PI()),IF(AccType=1,AB635*-speed/30*PI(),((AB635-AC635)*2/PI()+AC635)*-speed/30*PI()),0)/2*time7/time)))","v":2.4601999784026272},{"$f":"IF(move1,MAX(IF(AccType=1,Z635*-speed/30*PI(),((Z635-AA635)*2/PI()+AA635)*-speed/30*PI()),IF(AccType=1,X635*-speed/30*PI(),((X635-Y635)*2/PI()+Y635)*-speed/30*PI()),0),MAX(IF(AccType=1,Z635*-speed/30*PI(),((Z635-AA635)*2/PI()+AA635)*-speed/30*PI()),IF(AccType=1,X635*-speed/30*PI(),((X635-Y635)*2/PI()+Y635)*-speed/30*PI()),IF(AccType=1,AD635*-speed/30*PI(),((AD635-AE635)*2/PI()+AE635)*-speed/30*PI()),IF(AccType=1,AB635*-speed/30*PI(),((AB635-AC635)*2/PI()+AC635)*-speed/30*PI()),0))","v":150.71002830659057},{"$f":"(L635^2)/1000000+((K635/1000)^2*(D635/C635*H635)^2*PI()*PI()*(O635/2)^2)/1200","v":3.9987667004109289E-3},{"$f":"SQRT(3)*L635*J635*D635/C635*H635/1000","v":1.2010718241405245},{"$f":"0.75*J635^2*(D635/C635*H635)^2-(UAC_V*0.98)^2","v":-153381.0292574394},{"$f":"-AO635/2/AN635+SQRT((AO635/2/AN635)^2-AP635/AN635)","v":6044.9498918775498},{"$f":"(L635^2)/1000000+((K635/1000)^2*AV635^2*PI()*PI()*(O635/2)^2)/1200","v":1.2818828891783486E-3},{"$f":"SQRT(3)*L635*J635*AV635/1000","v":6.2567740117303636E-2},{"$f":"0.75*J635^2*AV635^2-(UAC_V*0.98)^2","v":-153663.2321002708},{"$f":"-AS635/2/AR635+SQRT((AS635/2/AR635)^2-AT635/AR635)","v":10924.278471337606},{"$f":"D635+(F635-D635)*((0.85*UAC_V-D635*J635)/L635*1000)/G635","v":3.7476399625803296},{"$f":"(L635^2)/1000000+((K635/1000)^2*AJ635^2*PI()*PI()*(O635/2)^2)/1200","v":2.0430064216224635E-3},{"$f":"SQRT(3)*L635*J635*AJ635/1000","v":0.63792547684830181},{"$f":"0.75*J635^2*AJ635^2-(UAC_V*0.98)^2","v":-153584.17416495772},{"$f":"IF(((AX635/2/AW635)^2-AY635/AW635)>0,-AX635/2/AW635+SQRT((AX635/2/AW635)^2-AY635/AW635),-9999)","v":8515.6660268360665}]
["KBM","KBM-35H02-A (120 V)",17.3,4.97,16.160348067792452,4.5522107233218172,325,58.8,531,5.5,44,215,2.2799999999999998,160,10,531,531,531,15.43798407383936,49.342105263157897,0.57778700870212141,0.50269953632653064,0.23978145851886304,-23.084855229629628,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},29.558732736000003,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},-2397.9523199999999,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},2409.9523199999999,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},0.11911199523951034,0.17691100878843932,2.8586878857482483,8.491728421845087,6.3455396474077794,23.117013146935228,2.486884621393048,152.34470976978153,0.15981473447468164,34.597872067302063,-147190.1614300411,857.53146581675219,5.005183974008047E-2,6.3503839498350283,-153445.89628820811,1688.6360668889681,3.100546201179478,6.2253799073365201E-2,12.99661753616539,-152750.46799685579,1465.5104761548641]
["KBM","KBM-35H02-A (240 V)",17.3,4.97,15.875705573416559,4.4720297389905799,800,58.8,1114,5.5,44,215,2.2799999999999998,325,10,857.53146581675219,1114,1114,15.316670010982557,49.342105263157897,0.57650498062205369,0.50269953632653064,0.11429439360279736,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.11911199523951034,0.17691100878843932,2.8586878857482483,8.491728421845087,6.3455396474077794,23.117013146935228,2.486884621393048,152.34470976978153,0.15981473447468164,34.597872067302063,-147190.1614300411,857.53146581675219,5.2802152501024095E-2,8.3252791049951913,-153289.14725702503,1626.8323976123518,4.064779815938893,6.2253799073365201E-2,12.99661753616539,-152750.46799685579,1465.5104761548641]
["KBM","KBM-35H02-A (400 V)",17.3,4.97,15.311803145737517,4.3131839847147937,1450,58.8,1863,5.5,44,215,2.2799999999999998,565,10,857.53146581675219,1610.1495498953313,1823.2558139534885,15.092210848279965,49.342105263157897,0.57620191741030768,0.50269953632653064,8.6880275880103386E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.11911199523951034,0.17691100878843932,2.8586878857482483,8.491728421845087,6.3455396474077794,23.117013146935228,2.486884621393048,152.34470976978153,0.15981473447468164,34.597872067302063,-147190.1614300411,857.53146581675219,5.362397440525446E-2,8.8300997322324388,-153242.30902498015,1610.1495498953313,4.3112562007405,6.2253799073365201E-2,12.99661753616539,-152750.46799685579,1465.5104761548641]
["KBM","KBM-35H02-A (480 V)",17.3,4.97,15.006037491521562,4.2270528145131161,1750,58.8,2235,5.5,44,215,2.2799999999999998,679,10,857.53146581675219,1607.3225630716925,1823.2558139534885,15.193064172161183,49.342105263157897,0.57615725894271785,0.50269953632653064,8.6880275880103386E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.11911199523951034,0.17691100878843932,2.8586878857482483,8.491728421845087,6.3455396474077794,23.117013146935228,2.486884621393048,152.34470976978153,0.15981473447468164,34.597872067302063,-147190.1614300411,857.53146581675219,5.3766592406847689E-2,8.9147952846383145,-153234.18077356945,1607.3225630716925,4.352608420597325,6.2253799073365201E-2,12.99661753616539,-152750.46799685579,1465.5104761548641]
["KBM","KBM-35H02-B (120 V)",17.600000000000001,6.3,16.472536610011169,5.7395597944289785,400,58.8,661,3.43,28,174,2.2799999999999998,160,10,661,661,661,15.736866748043456,49.342105263157897,0.56740039135370457,0.50269953632653064,0.19262322915811841,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.14841339355627209,0.22043089043181818,3.5619214453505301,10.580682740727273,7.9065342757793786,23.117013146935228,2.486884621393048,152.34470976978153,0.10169026752584735,21.757510581125761,-149755.05176800271,1111.2584359485968,3.2526294475423566E-2,3.862214476207408,-153540.82734954893,2114.1147632211291,3.7362195762648978,4.0353362628209155E-2,8.1731628757945671,-153112.40309655943,1849.254802024449]
["KBM","KBM-35H02-B (240 V)",17.600000000000001,6.3,16.083025828233634,5.6038417519977815,950,58.8,1386,3.43,28,174,2.2799999999999998,325,10,1111.2584359485968,1386,1386,15.386814524138753,49.342105263157897,0.56652470965892299,0.50269953632653064,9.1864325016967008E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.14841339355627209,0.22043089043181818,3.5619214453505301,10.580682740727273,7.9065342757793786,23.117013146935228,2.486884621393048,152.34470976978153,0.10169026752584735,21.757510581125761,-149755.05176800271,1111.2584359485968,3.4240428290349845E-2,5.1263351208187977,-153447.00211577702,2043.4103647544835,4.9591015079269551,4.0353362628209155E-2,8.1731628757945671,-153112.40309655943,1849.254802024449]
["KBM","KBM-35H02-B (400 V)",17.600000000000001,6.3,15.305400360670603,5.3328921117319172,1800,58.8,2313,3.43,28,174,2.2799999999999998,565,10,1111.2584359485968,2021.2269895976979,2252.8735632183907,15.0233851548146,49.342105263157897,0.56629435897621605,0.50269953632653064,6.8851493225341329E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.14841339355627209,0.22043089043181818,3.5619214453505301,10.580682740727273,7.9065342757793786,23.117013146935228,2.486884621393048,152.34470976978153,0.10169026752584735,21.757510581125761,-149755.05176800271,1111.2584359485968,3.4833068348206632E-2,5.4961614478324536,-153414.5632294504,2021.2269895976979,5.3168631939541404,4.0353362628209155E-2,8.1731628757945671,-153112.40309655943,1849.254802024449]
["KBM","KBM-35H02-B (480 V)",17.600000000000001,6.3,14.823112654331526,5.16484761474966,2200,58.8,2776,3.43,28,174,2.2799999999999998,679,10,1111.2584359485968,2018.7762202641377,2252.8735632183907,15.051857209187311,49.342105263157897,0.56628538152543606,0.50269953632653064,6.8851493225341329E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.14841339355627209,0.22043089043181818,3.5619214453505301,10.580682740727273,7.9065342757793786,23.117013146935228,2.486884621393048,152.34470976978153,0.10169026752584735,21.757510581125761,-149755.05176800271,1111.2584359485968,3.4900136742243348E-2,5.5364584438365148,-153410.89215797721,2018.7762202641377,5.3558456032073121,4.0353362628209155E-2,8.1731628757945671,-153112.40309655943,1849.254802024449]
["KBM","KBM-35H02-C (120 V)",17.5,8.6999999999999993,16.119212636347161,7.8630305543156886,625,59.2,923,1.8,14.6,124,2.2799999999999998,160,10,923,923,923,15.460853221357487,49.342105263157897,0.57021219387028954,0.49930291783783787,0.13794577949460052,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.20612298250645247,0.30614401762285715,4.9469515801548596,14.694912845897143,10.980939032266109,23.117013146935228,2.486884621393048,152.34470976978153,5.3339831827869243E-2,11.37778514160213,-151559.19389424328,1582.3588978511495,1.6559892901456714E-2,2.0092265861243424,-153598.36213133472,2985.4802653506345,5.1972558707967824,2.0660977955745126E-2,4.2451622919340899,-153370.98811646627,2623.7610746392966]
["KBM","KBM-35H02-C (240 V)",17.5,8.6999999999999993,15.48350232079725,7.5529279613645128,1400,59.2,1935,1.8,14.6,124,2.2799999999999998,325,10,1582.3588978511495,1935,1935,14.712912136244771,49.342105263157897,0.56965533756774223,0.49930291783783787,6.5800493267967067E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.20612298250645247,0.30614401762285715,4.9469515801548596,14.694912845897143,10.980939032266109,23.117013146935228,2.486884621393048,152.34470976978153,5.3339831827869243E-2,11.37778514160213,-151559.19389424328,1582.3588978511495,1.726035169202407E-2,2.5348583103583557,-153559.52701200583,2910.2010335656405,6.5569046946369021,2.0660977955745126E-2,4.2451622919340899,-153370.98811646627,2623.7610746392966]
["KBM","KBM-35H02-C (400 V)",17.5,8.6999999999999993,14.155427879702691,6.9050867705866787,2550,59.2,3224,1.8,14.6,124,2.2799999999999998,565,10,1582.3588978511495,2892.351613556963,3161.2903225806449,13.706400561255077,49.342105263157897,0.5695621942575565,0.49930291783783787,4.8527267099204227E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.20612298250645247,0.30614401762285715,4.9469515801548596,14.694912845897143,10.980939032266109,23.117013146935228,2.486884621393048,152.34470976978153,5.3339831827869243E-2,11.37778514160213,-151559.19389424328,1582.3588978511495,1.7437914362831139E-2,2.6516000574379022,-153549.68251065613,2892.351613556963,6.8588799594310039,2.0660977955745126E-2,4.2451622919340899,-153370.98811646627,2623.7610746392966]
["KBM","KBM-35H02-C (480 V)",17.5,8.6999999999999993,13.100441253251635,6.3904591479276274,3200,59.2,3869,1.8,14.6,124,2.2799999999999998,679,10,1582.3588978511495,2895.1341733706049,3161.2903225806449,13.519589726417893,49.342105263157897,0.56960795617951665,0.49930291783783787,4.8527267099204227E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.20612298250645247,0.30614401762285715,4.9469515801548596,14.694912845897143,10.980939032266109,23.117013146935228,2.486884621393048,152.34470976978153,5.3339831827869243E-2,11.37778514160213,-151559.19389424328,1582.3588978511495,1.740994789043911E-2,2.6335563715177921,-153551.23303912004,2895.1341733706049,6.8122064517108036,2.0660977955745126E-2,4.2451622919340899,-153370.98811646627,2623.7610746392966]
["KBM","KBM-35H02-D (120 V)",17.45,10.92,15.952942531093511,9.7274039823740921,850,59.4,1165,1.1399999999999999,9.3000000000000007,99,2.2799999999999998,160,10,1165,1165,1165,15.398150645557577,49.342105263157897,0.57152417986828896,0.49762176323232332,0.10929094804593671,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.25946119920286581,0.38536456718853879,6.2270687808687795,18.497499225049861,13.822464506577438,23.117013146935228,2.486884621393048,152.34470976978153,3.4373633840441876E-2,7.2663167473263588,-152317.21500172239,2002.0026704673478,1.0501885974165558E-2,1.2271909822872074,-153625.5856109834,3766.7256867838596,6.2778579121974181,1.3198780909901005E-2,2.7020050521531145,-153477.77330624781,3309.189195216954]
["KBM","KBM-35H02-D (240 V)",17.45,10.92,15.020785439916175,9.1590155121440091,1850,59.4,2437,1.1399999999999999,9.3000000000000007,99,2.2799999999999998,325,10,2002.0026704673478,2437,2437,14.250002225446334,49.342105263157897,0.57119798897587504,0.49762176323232332,5.2246185668246313E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.25946119920286581,0.38536456718853879,6.2270687808687795,18.497499225049861,13.822464506577438,23.117013146935228,2.486884621393048,152.34470976978153,3.4373633840441876E-2,7.2663167473263588,-152317.21500172239,2002.0026704673478,1.0874825046858716E-2,1.5189911219318206,-153605.14544361524,3689.1116414379985,7.7706001519049126,1.3198780909901005E-2,2.7020050521531145,-153477.77330624781,3309.189195216954]
["KBM","KBM-35H02-D (400 V)",17.45,10.92,12.441369265697876,7.5862007717669977,3500,59.4,4061,1.1399999999999999,9.3000000000000007,99,2.2799999999999998,565,10,2002.0026704673478,3689.2264070400279,3959.5959595959598,12.170579209114376,49.342105263157897,0.57128380192328831,0.49762176323232332,3.8475876404270914E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.25946119920286581,0.38536456718853879,6.2270687808687795,18.497499225049861,13.822464506577438,23.117013146935228,2.486884621393048,152.34470976978153,3.4373633840441876E-2,7.2663167473263588,-152317.21500172239,2002.0026704673478,1.0874248519556684E-2,1.518583300642991,-153605.17704211327,3689.2264070400279,7.7685138881189211,1.3198780909901005E-2,2.7020050521531145,-153477.77330624781,3309.189195216954]
["KBM","KBM-35H02-D (480 V)",17.45,10.92,10.548641577020971,6.4320985225737637,4300,59.4,4873,1.1399999999999999,9.3000000000000007,99,2.2799999999999998,679,10,2002.0026704673478,3705.6481239737191,3959.5959595959598,11.502556769073845,49.342105263157897,0.57141039094049551,0.49762176323232332,3.8475876404270914E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.25946119920286581,0.38536456718853879,6.2270687808687795,18.497499225049861,13.822464506577438,23.117013146935228,2.486884621393048,152.34470976978153,3.4373633840441876E-2,7.2663167473263588,-152317.21500172239,2002.0026704673478,1.0792507720717708E-2,1.4596089607688871,-153609.65711870327,3705.6481239737191,7.466822846105857,1.3198780909901005E-2,2.7020050521531145,-153477.77330624781,3309.189195216954]
["KBM","KBM-35H02-E (120 V)",17.100000000000001,12,15.580431271101332,10.671528267877624,950,59.4,1305,0.94,7.4,88.4,2.2799999999999998,160,10,1305,1305,1305,15.012592430302355,49.342105263157897,0.58312622006792747,0.49762176323232332,9.7566248638709788E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.2909580313662366,0.43214521543859652,6.982992752789678,20.742970341052633,15.500418073374222,23.117013146935228,2.486884621393048,152.34470976978153,2.7378895815966042E-2,5.9994622722815141,-152512.5101030471,2253.1561378740516,8.3352040953843035E-3,0.97870148199852725,-153633.35666912576,4234.9272816847788,6.8000091952456856,1.051981850757505E-2,2.2309208273739696,-153504.77773611021,3715.3796735825608]
["KBM","KBM-35H02-E (240 V)",17.100000000000001,12,14.533563583806249,9.9544956053467466,2050,59.4,2728,0.94,7.4,88.4,2.2799999999999998,325,10,2253.1561378740516,2728,2728,13.684761686157778,49.342105263157897,0.58286279135050389,0.49762176323232332,4.6673003839265495E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.2909580313662366,0.43214521543859652,6.982992752789678,20.742970341052633,15.500418073374222,23.117013146935228,2.486884621393048,152.34470976978153,2.7378895815966042E-2,5.9994622722815141,-152512.5101030471,2253.1561378740516,8.5882898943108812E-3,1.1930934477932444,-153618.46090454335,4160.4085627941186,8.2896026674185102,1.051981850757505E-2,2.2309208273739696,-153504.77773611021,3715.3796735825608]
["KBM","KBM-35H02-E (400 V)",17.100000000000001,12,11.496360954248335,7.8742198316769416,3850,59.4,4547,0.94,7.4,88.4,2.2799999999999998,565,10,2253.1561378740516,4174.7848500237424,4434.3891402714926,11.023639638128428,49.342105263157897,0.58301702690697199,0.49762176323232332,3.4269432913902963E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.2909580313662366,0.43214521543859652,6.982992752789678,20.742970341052633,15.500418073374222,23.117013146935228,2.486884621393048,152.34470976978153,2.7378895815966042E-2,5.9994622722815141,-152512.5101030471,2253.1561378740516,8.5378926312561099E-3,1.153582876953219,-153621.42711509031,4174.7848500237424,8.0150835725123244,1.051981850757505E-2,2.2309208273739696,-153504.77773611021,3715.3796735825608]
["KBM","KBM-35H02-E (480 V)",17.100000000000001,12,9.1226258870120436,6.2483738952137289,4700,59.4,5457,0.94,7.4,88.4,2.2799999999999998,679,10,2253.1561378740516,4203.5162500050792,4434.3891402714926,9.9653145284436739,49.342105263157897,0.58320035067010312,0.49762176323232332,3.4269432913902963E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.2909580313662366,0.43214521543859652,6.982992752789678,20.742970341052633,15.500418073374222,23.117013146935228,2.486884621393048,152.34470976978153,2.7378895815966042E-2,5.9994622722815141,-152512.5101030471,2253.1561378740516,8.4393973669149754E-3,1.0721690564651323,-153627.22420949992,4203.5162500050792,7.449421071615137,1.051981850757505E-2,2.2309208273739696,-153504.77773611021,3715.3796735825608]
["KBM","KBM-35H02-F (120 V)",17.3,14.92,15.597184423005743,13.106877666391382,1200,59.4,1607,0.61,4.9000000000000004,72.099999999999994,2.2799999999999998,160,10,1607,1607,1607,15.019646139808524,49.342105263157897,0.5762373346152736,0.49762176323232332,7.9230836635666629E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.35757564768078359,0.5310889841294798,8.5818155443388058,25.492271238215032,19.0493866276306,23.117013146935228,2.486884621393048,152.34470976978153,1.8154352086988401E-2,3.9024279373386861,-152931.61529938379,2796.916872940772,5.513236410808457E-3,0.60832543053478261,-153646.20322033876,5224.191013076359,7.9856495094279758,6.9898928739482221E-3,1.4511313460471418,-153562.72950654716,4584.4841937935353]
["KBM","KBM-35H02-F (240 V)",17.3,14.92,13.873506360085971,11.658408705954598,2650,59.4,3356,0.61,4.9000000000000004,72.099999999999994,2.2799999999999998,325,10,2796.916872940772,3356,3356,12.960636733754157,49.342105263157897,0.57614407079611918,0.49762176323232332,3.7939199783526896E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.35757564768078359,0.5310889841294798,8.5818155443388058,25.492271238215032,19.0493866276306,23.117013146935228,2.486884621393048,152.34470976978153,1.8154352086988401E-2,3.9024279373386861,-152931.61529938379,2796.916872940772,5.6227734078775574E-3,0.70626771998621352,-153640.01121822372,5164.8664220732444,9.2713639583907526,6.9898928739482221E-3,1.4511313460471418,-153562.72950654716,4584.4841937935353]
["KBM","KBM-35H02-F (400 V)",17.3,14.92,7.6956096012669395,6.4668988245940673,5100,59.4,5593,0.61,4.9000000000000004,72.099999999999994,2.2799999999999998,565,10,2796.916872940772,5252.861306938913,5436.8932038834955,7.4077390779920602,49.342105263157897,0.57658120118612211,0.49762176323232332,2.7772798223601066E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.35757564768078359,0.5310889841294798,8.5818155443388058,25.492271238215032,19.0493866276306,23.117013146935228,2.486884621393048,152.34470976978153,1.8154352086988401E-2,3.9024279373386861,-152931.61529938379,2796.916872940772,5.4624426417988767E-3,0.55709492685418871,-153649.07453444772,5252.861306938913,7.3131330798172112,6.9898928739482221E-3,1.4511313460471418,-153562.72950654716,4584.4841937935353]
["KBM","KBM-35H02-F (480 V)",17.3,14.92,6.2689363695640994,5.2680137559362183,5400,59.4,6711,0.61,4.9000000000000004,72.099999999999994,2.2799999999999998,679,10,2796.916872940772,5276.8328104900702,5436.8932038834955,6.5205410185763206,49.342105263157897,0.57669950511077528,0.49762176323232332,2.7772798223601066E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.35757564768078359,0.5310889841294798,8.5818155443388058,25.492271238215032,19.0493866276306,23.117013146935228,2.486884621393048,152.34470976978153,1.8154352086988401E-2,3.9024279373386861,-152931.61529938379,2796.916872940772,5.4211388999505124E-3,0.51166849754218746,-153651.40938809284,5276.8328104900702,6.7168082761154437,6.9898928739482221E-3,1.4511313460471418,-153562.72950654716,4584.4841937935353]
["KBM","KBM-35H02-G (120 V)",17.100000000000001,18.64,15.094049441618461,16.057499405977087,1550,59.4,2032,0.39,3.1,57,2.2799999999999998,160,10,2032,2032,2032,14.470263526044331,49.342105263157897,0.58289478895582336,0.49762176323232332,6.2659426414132025E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.45195480872222088,0.67126556798128656,10.846915409333301,32.220747263101757,24.077316073974625,23.117013146935228,2.486884621393048,152.34470976978153,1.1533272593584727E-2,2.4930806770391358,-153185.74120789274,3537.977740736279,3.4060161806484233E-3,0.34322692288443074,-153654.93530928035,6666.4100638283626,8.91417707244503,4.3945077812852038E-3,0.9270606854929192,-153597.86876619063,5807.5029383650763]
["KBM","KBM-35H02-G (240 V)",17.100000000000001,18.64,12.44217172759582,13.236352901697682,3400,59.4,4241,0.39,3.1,57,2.2799999999999998,325,10,3537.977740736279,4241,4241,11.290044204921728,49.342105263157897,0.5829522065300663,0.49762176323232332,3.0022153848978134E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.45195480872222088,0.67126556798128656,10.846915409333301,32.220747263101757,24.077316073974625,23.117013146935228,2.486884621393048,152.34470976978153,1.1533272593584727E-2,2.4930806770391358,-153185.74120789274,3537.977740736279,3.4222112164554144E-3,0.36049325899491452,-153654.00035474141,6648.2119964169224,9.3626126910373095,4.3945077812852038E-3,0.9270606854929192,-153597.86876619063,5807.5029383650763]
["KBM","KBM-35H02-G (400 V)",17.100000000000001,18.64,3.6056826762543186,3.8358326343131051,5800,59.4,7068,0.39,3.1,57,2.2799999999999998,565,10,3537.977740736279,6826.1425239818409,6877.1929824561403,1.218252876599097,49.342105263157897,0.58367795252442178,0.49762176323232332,2.1924044778763453E-2,-23.084855229629628,9,29.558732736000003,9,-2397.9523199999999,7.5,2409.9523199999999,9,0.45195480872222088,0.67126556798128656,10.846915409333301,32.220747263101757,24.077316073974625,23.117013146935228,2.486884621393048,152.34470976978153,1.1533272593584727E-2,2.4930806770391358,-153185.74120789274,3537.977740736279,3.2766455911482596E-3,0.14401975994174171,-153662.40399420948,6826.1425239818409,3.7404339708047623,4.3945077812852038E-3,0.9270606854929192,-153597.86876619063,5807.5029383650763]
["KBM","KBM-35H03-A (120 V)",21.8,10.199999999999999,20.567715722644937,9.3489616921113345,650,76.099999999999994,867,1.41,12,132,3.04,160,10,867,867,867,20.156322356204864,37.006578947368418,0.45796069947251244,0.39046943032851517,0.14685577217245244,-23.277436602469137,9,29.714723648000003,9,-2413.86976,7.5,2425.86976,9,0.19425777402390762,0.28965040253211005,4.6621865765737827,13.903219321541282,10.381261791979842,23.148413725250013,2.5135692643834693,153.97939123297252,5.4962565284357029E-2,11.478417209983911,-151773.58933588077,1560.603075234483,1.88625219325293E-2,2.2469914249745417,-153591.55724196642,2794.5981024722278,6.9702401895327348,2.0614959457423504E-2,3.3466000586356124,-153503.30595798237,2648.8120862642718]
["KBM","KBM-35H03-A (240 V)",21.8,10.199999999999999,19.644267261628229,8.9292123916491946,1400,76.099999999999994,1818,1.41,12,132,3.04,325,10,1560.603075234483,1818,1818,19.000627058314372,37.006578947368418,0.4577945124332396,0.39046943032851517,7.0035178478281779E-2,-23.277436602469137,9,29.714723648000003,9,-2413.86976,7.5,2425.86976,9,0.19425777402390762,0.28965040253211005,4.6621865765737827,13.903219321541282,10.381261791979842,23.148413725250013,2.5135692643834693,153.97939123297252,5.4962565284357029E-2,11.478417209983911,-151773.58933588077,1560.603075234483,1.9300471651469815E-2,2.5663398933577954,-153569.50246142907,2755.075047787926,7.9608694834633518,2.0614959457423504E-2,3.3466000586356124,-153503.30595798237,2648.8120862642718]
["KBM","KBM-35H03-A (400 V)",21.8,10.199999999999999,17.188733853924695,7.8130608426930426,2550,76.099999999999994,3029,1.41,12,132,3.04,565,10,1560.603075234483,2757.9518566478291,2969.6969696969695,16.812686263111502,37.006578947368418,0.45791985149687314,0.39046943032851517,4.8068322828097053E-2,-23.277436602469137,9,29.714723648000003,9,-2413.86976,7.5,2425.86976,9,0.19425777402390762,0.28965040253211005,4.6621865765737827,13.903219321541282,10.381261791979842,23.148413725250013,2.5135692643834693,153.97939123297252,5.4962565284357029E-2,11.478417209983911,-151773.58933588077,1560.603075234483,1.9267648967005745E-2,2.5437960485275015,-153571.15538429029,2757.9518566478291,7.8909377465122486,2.0614959457423504E-2,3.3466000586356124,-153503.30595798237,2648.8120862642718]
["KBM","KBM-35H03-A (480 V)",21.8,10.199999999999999,15.586916362161105,7.0849619828005022,3100,76.099999999999994,3635,1.41,12,132,3.04,679,10,1560.603075234483,2764.8805111003335,2969.6969696969695,16.258569721258993,37.006578947368418,0.45801132395723965,0.39046943032851517,4.8068322828097053E-2,-23.277436602469137,9,29.714723648000003,9,-2413.86976,7.5,2425.86976,9,0.19425777402390762,0.28965040253211005,4.6621865765737827,13.903219321541282,10.381261791979842,23.148413725250013,2.5135692643834693,153.97939123297252,5.4962565284357029E-2,11.478417209983911,-151773.58933588077,1560.603075234483,1.9189200506992642E-2,2.4890876667742283,-153575.10598294181,2764.8805111003335,7.7212305740848821,2.0614959457423504E-2,3.3466000586356124,-153503.30595798237,2648.8120862642718]
["KBM","KBM-35H03-B (120 V)",21.7,14,19.629109648000426,12.345351979874481,900,76.599999999999994,1197,0.75,6.2,96.2,3.04,160,10,1197,1197,1197,18.945715831840566,37.006578947368418,0.46026624748827843,0.38792067425587473,0.10636921844069863,-23.277436602469137,9,29.714723648000003,9,-2413.86976,7.5,2425.86976,9,0.26785701921070126,0.39939144688172051,6.4285684610568303,19.170789450322584,14.314453324804591,23.148413725250013,2.5135692643834693,153.97939123297252,2.8557938666551951E-2,6.1758115339889281,-152633.66623309054,2206.2605912194163,9.7234107021318961E-3,0.96260668921243664,-153638.96845735353,3925.8475876381681,7.7028583664661774,1.0873979036851156E-2,1.7888409558278755,-153577.55630472381,3676.7579795479251]
["KBM","KBM-35H03-B (240 V)",21.7,14,17.910753839658661,11.264625056389095,2050,76.599999999999994,2504,0.75,6.2,96.2,3.04,325,10,2206.2605912194163,2504,2504,17.07157444610014,37.006578947368418,0.46005287345927154,0.38792067425587473,5.0848224629998509E-2,-23.277436602469137,9,29.714723648000003,9,-2413.86976,7.5,2425.86976,9,0.26785701921070126,0.39939144688172051,6.4285684610568303,19.170789450322584,14.314453324804591,23.148413725250013,2.5135692643834693,153.97939123297252,2.8557938666551951E-2,6.1758115339889281,-152633.66623309054,2206.2605912194163,9.9572516567399006E-3,1.1784074983211812,-153626.48708100923,3869.1984581713355,9.4297142948136852,1.0873979036851156E-2,1.7888409558278755,-153577.55630472381,3676.7579795479251]
["KBM","KBM-35H03-B (400 V)",21.7,14,13.105153077224749,8.2422346397639927,3800,76.599999999999994,4173,0.75,6.2,96.2,3.04,565,10,2206.2605912194163,3890.3310601911166,4074.8440748440748,12.900842120720895,37.006578947368418,0.46024776414305668,0.38792067425587473,3.4629408620790253E-2,-23.277436602469137,9,29.714723648000003,9,-2413.86976,7.5,2425.86976,9,0.26785701921070126,0.39939144688172051,6.4285684610568303,19.170789450322584,14.314453324804591,23.148413725250013,2.5135692643834693,153.97939123297252,2.8557938666551951E-2,6.1758115339889281,-152633.66623309054,2206.2605912194163,9.8679382305438077E-3,1.1009882307676908,-153631.25422920543,3890.3310601911166,8.810198910718448,1.0873979036851156E-2,1.7888409558278755,-153577.55630472381,3676.7579795479251]
["KBM","KBM-35H03-B (480 V)",21.7,14,10.26549382942725,6.4562854273127357,4800,76.599999999999994,5007,0.75,6.2,96.2,3.04,679,10,2206.2605912194163,3896.7407182090428,4074.8440748440748,12.417227960940959,37.006578947368418,0.46030455116348001,0.38792067425587473,3.4629408620790253E-2,-23.277436602469137,9,29.714723648000003,9,-2413.86976,7.5,2425.86976,9,0.26785701921070126,0.39939144688172051,6.4285684610568303,19.170789450322584,14.314453324804591,23.148413725250013,2.5135692643834693,153.97939123297252,2.8557938666551951E-2,6.1758115339889281,-152633.66623309054,2206.2605912194163,9.8413264746536177E-3,1.0768446872285196,-153632.67464480799,3896.7407182090428,8.6170002778489838,1.0873979036851156E-2,1.7888409558278755,-153577.55630472381,3676.7579795479251]
["KBM","KBM-35H03-C (120 V)",20.7,20.2,18.044877685729375,17.185597795932736,1450,75.2,1813,0.36,2.8,63.6,3.04,160,10,1813,1813,1813,17.380181547743007,37.006578947368418,0.48231280934213955,0.39514260170212767,7.0228325688646592E-2,-23.277436602469137,9,29.714723648000003,9,-2413.86976,7.5,2425.86976,9,0.40514991649695925,0.60410368124959746,9.7235979959270225,28.996976699980678,21.651475053122304,23.148413725250013,2.5135692643834693,153.97939123297252,1.2726010844285641E-2,2.9101750186989843,-153140.56351116823,3356.5016857011433,4.1851083187243619E-3,0.36976593975609601,-153655.54955486557,6015.2611869870007,9.3240943769801277,4.8006602198707206E-3,0.85863331026432643,-153618.43396464395,5568.0828426426224]
["KBM","KBM-35H03-C (240 V)",20.7,20.2,14.724399251211478,14.023237382106169,3100,75.2,3783,0.36,2.8,63.6,3.04,325,10,3356.5016857011433,3783,3783,13.407839473333233,37.006578947368418,0.48236279402669491,0.39514260170212767,3.3656874034765069E-2,-23.277436602469137,9,29.714723648000003,9,-2413.86976,7.5,2425.86976,9,0.40514991649695925,0.60410368124959746,9.7235979959270225,28.996976699980678,21.651475053122304,23.148413725250013,2.5135692643834693,153.97939123297252,1.2726010844285641E-2,2.9101750186989843,-153140.56351116823,3356.5016857011433,4.1990247384286186E-3,0.38768998647315311,-153654.71044425585,6003.2227110025178,9.7760708443569762,4.8006602198707206E-3,0.85863331026432643,-153618.43396464395,5568.0828426426224]
["KBM","KBM-35H03-C (400 V)",20.7,20.2,5.7009300615516914,5.4294572014778009,5000,75.2,6305,0.36,2.8,63.6,3.04,565,10,3356.5016857011433,6112.9947454684125,6163.5220125786154,2.3621528558704554,37.006578947368418,0.48291889904313801,0.39514260170212767,2.2866749305239877E-2,-23.277436602469137,9,29.714723648000003,9,-2413.86976,7.5,2425.86976,9,0.40514991649695925,0.60410368124959746,9.7235979959270225,28.996976699980678,21.651475053122304,23.148413725250013,2.5135692643834693,153.97939123297252,1.2726010844285641E-2,2.9101750186989843,-153140.56351116823,3356.5016857011433,4.0812606379096363E-3,0.18818720276219852,-153661.81120064948,6112.9947454684125,4.7453674079663699,4.8006602198707206E-3,0.85863331026432643,-153618.43396464395,5568.0828426426224]
["KBM","KBM-35H03-D (120 V)",20,21.5,17.188733853924695,17.904931097838226,1550,75.7,1996,0.32,2.2999999999999998,57.8,3.04,160,10,1996,1996,1996,16.379814691892705,37.006578947368418,0.49921846229777261,0.39253267698811101,6.3789556349457044E-2,-23.277436602469137,9,29.714723648000003,9,-2413.86976,7.5,2425.86976,9,0.44631675825983103,0.66548599836666678,10.711602198235944,31.943327921600005,23.851457852455649,23.148413725250013,2.5135692643834693,153.97939123297252,1.0543996780891933E-2,2.60701054511095,-153155.40755152001,3689.5949146101025,3.4127796385887933E-3,0.26053464347203975,-153658.92056635089,6671.9728114760919,8.1325555007463954,3.9596310711968313E-3,0.76410558370091541,-153620.3090911984,6132.9537402629312]
["KBM","KBM-35H03-D (240 V)",20,21.5,13.298799803649256,13.852916462134642,3400,75.7,4166,0.32,2.2999999999999998,57.8,3.04,325,10,3689.5949146101025,4166,4166,11.789058818236118,37.006578947368418,0.4993057193996519,0.39253267698811101,3.0562639095899249E-2,-23.277436602469137,9,29.714723648000003,9,-2413.86976,7.5,2425.86976,9,0.44631675825983103,0.66548599836666678,10.711602198235944,31.943327921600005,23.851457852455649,23.148413725250013,2.5135692643834693,153.97939123297252,1.0543996780891933E-2,2.60701054511095,-153155.40755152001,3689.5949146101025,3.4201216214621356E-3,0.27350647729833161,-153658.40217182474,6662.9516482848067,8.5374696309092801,3.9596310711968313E-3,0.76410558370091541,-153620.3090911984,6132.9537402629312]
["KBM","KBM-35H04-A (120 V)",25.6,10.86,23.786429676643269,9.7485367527226519,550,92.3,778,1.35,11,147,3.81,160,10,778,778,778,23.034622342597206,29.527559055118111,0.3908844956046939,0.32364861399783318,0.16365546847495663,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.17636978518192367,0.26401224804843748,4.2328748443661679,12.672587906324999,9.4549943817012476,23.180394992492932,2.5406050210974489,155.63558166278446,5.9753067325012302E-2,13.458705545314521,-151568.38295437687,1484.0215552265863,2.2624089883763143E-2,2.1955434754160708,-153608.23144115365,2557.6131313940546,6.3874911390727886,2.3833162061686553E-2,3.2499225083626722,-153541.80558667265,2470.9153029035483]
["KBM","KBM-35H04-A (240 V)",25.6,10.86,22.612734314496489,9.2675140633182327,1250,92.3,1633,1.35,11,147,3.81,325,10,1484.0215552265863,1633,1633,21.697436108458213,29.527559055118111,0.39057640654115078,0.32364861399783318,7.7969353627382901E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.17636978518192367,0.26401224804843748,4.2328748443661679,12.672587906324999,9.4549943817012476,23.180394992492932,2.5406050210974489,155.63558166278446,5.9753067325012302E-2,13.458705545314521,-151568.38295437687,1484.0215552265863,2.3217427070613264E-2,2.7636973262577511,-153575.63377630658,2513.0710444826059,8.0404202331749151,2.3833162061686553E-2,3.2499225083626722,-153541.80558667265,2470.9153029035483]
["KBM","KBM-35H04-A (400 V)",25.6,10.86,20.136560191191975,8.252688602947531,2300,92.3,2721,1.35,11,147,3.81,565,10,1484.0215552265863,2504.1080083553388,2666.6666666666665,19.651720270259332,29.527559055118111,0.39057152090831482,0.32364861399783318,5.1529064684612678E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.17636978518192367,0.26401224804843748,4.2328748443661679,12.672587906324999,9.4549943817012476,23.180394992492932,2.5406050210974489,155.63558166278446,5.9753067325012302E-2,13.458705545314521,-151568.38295437687,1484.0215552265863,2.334412569546845E-2,2.8704848699729633,-153568.6730136894,2504.1080083553388,8.351097064165474,2.3833162061686553E-2,3.2499225083626722,-153541.80558667265,2470.9153029035483]
["KBM","KBM-35H04-A (480 V)",25.6,10.86,18.416500557776462,7.5477461302362556,2800,92.3,3266,1.35,11,147,3.81,679,10,1484.0215552265863,2507.2779194360105,2666.6666666666665,19.167489451511436,29.527559055118111,0.3906360193912688,0.32364861399783318,5.1529064684612678E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.17636978518192367,0.26401224804843748,4.2328748443661679,12.672587906324999,9.4549943817012476,23.180394992492932,2.5406050210974489,155.63558166278446,5.9753067325012302E-2,13.458705545314521,-151568.38295437687,1484.0215552265863,2.3299050716221834E-2,2.832954896368796,-153571.14941176292,2507.2779194360105,8.2419111716835118,2.3833162061686553E-2,3.2499225083626722,-153541.80558667265,2470.9153029035483]
["KBM","KBM-35H04-B (120 V)",25.9,13.3,23.708598419206478,11.795322596620139,725,93,948,0.9,7.6,122,3.81,160,10,948,948,948,23.034553519183092,29.527559055118111,0.38625287941115316,0.32121254916129033,0.1343079688539201,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.21349425989868023,0.31958478286486491,5.1238622375683258,15.340069577513516,11.445197519435288,23.180394992492932,2.5406050210974489,155.63558166278446,4.1970652956830092E-2,9.0823407759937265,-152278.47000182615,1799.6587277287767,1.5591757137014354E-2,1.468122349044181,-153627.79697608566,3092.2444533172966,7.7196797215297233,1.6439723015316831E-2,2.1766382639742874,-153584.42202814773,2991.0298774510707]
["KBM","KBM-35H04-B (240 V)",25.9,13.3,22.117403059351133,11.003683114105042,1550,93,1984,0.9,7.6,122,3.81,325,10,1799.6587277287767,1984,1984,21.05827591596945,29.527559055118111,0.38605983386981885,0.32121254916129033,6.4175380278990057E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.21349425989868023,0.31958478286486491,5.1238622375683258,15.340069577513516,11.445197519435288,23.180394992492932,2.5406050210974489,155.63558166278446,4.1970652956830092E-2,9.0823407759937265,-152278.47000182615,1799.6587277287767,1.5914862276834321E-2,1.7718234485654178,-153611.26957919769,3051.6100806818349,9.3166005918555115,1.6439723015316831E-2,2.1766382639742874,-153584.42202814773,2991.0298774510707]
["KBM","KBM-35H04-B (400 V)",25.9,13.3,18.327948183424581,9.1183821808082506,2850,93,3307,0.9,7.6,122,3.81,565,10,1799.6587277287767,3050.5805694773012,3213.1147540983607,17.795033634133237,29.527559055118111,0.38613158538758863,0.32121254916129033,4.2568600010783116E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.21349425989868023,0.31958478286486491,5.1238622375683258,15.340069577513516,11.445197519435288,23.180394992492932,2.5406050210974489,155.63558166278446,4.1970652956830092E-2,9.0823407759937265,-152278.47000182615,1799.6587277287767,1.5923364894834594E-2,1.7791154996881311,-153610.83465531393,3050.5805694773012,9.3549436490380522,1.6439723015316831E-2,2.1766382639742874,-153584.42202814773,2991.0298774510707]
["KBM","KBM-35H04-B (480 V)",25.9,13.3,16.149545696089383,8.0345998488006884,3400,93,3968,0.9,7.6,122,3.81,679,10,1799.6587277287767,3056.4254084698982,3213.1147540983607,17.134842271000856,29.527559055118111,0.38620152141263009,0.32121254916129033,4.2568600010783116E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.21349425989868023,0.31958478286486491,5.1238622375683258,15.340069577513516,11.445197519435288,23.180394992492932,2.5406050210974489,155.63558166278446,4.1970652956830092E-2,9.0823407759937265,-152278.47000182615,1799.6587277287767,1.587529290397462E-2,1.7374852237340437,-153613.2936223009,3056.4254084698982,9.1360433664466978,1.6439723015316831E-2,2.1766382639742874,-153584.42202814773,2991.0298774510707]
["KBM","KBM-35H04-C (120 V)",25.3,14.7,22.977994908892388,13.055678925507038,800,93,1080,0.73,6.1,107,3.81,160,10,1080,1080,1080,22.165293127004723,29.527559055118111,0.39539561250301808,0.32121254916129033,0.11789255043844099,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.24156340328456868,0.36160217058498029,5.7975216788296482,17.356904188079053,12.949954089496259,23.180394992492932,2.5406050210974489,155.63558166278446,3.3788718806741905E-2,7.3104990884043923,-152497.01168395576,2019.0145978646967,1.1985639969863468E-2,1.1330515896012832,-153635.96685508126,3533.3154094680863,8.3749537864810435,1.2732082659151179E-2,1.7520056158462227,-153596.97397855803,3405.1730754874529]
["KBM","KBM-35H04-C (240 V)",25.3,14.7,21.088029959676135,11.98183520436144,1800,93,2260,0.73,6.1,107,3.81,325,10,2019.0145978646967,2260,2260,20.011637616037813,29.527559055118111,0.39520016851054424,0.32121254916129033,5.6338032952883303E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.24156340328456868,0.36160217058498029,5.7975216788296482,17.356904188079053,12.949954089496259,23.180394992492932,2.5406050210974489,155.63558166278446,3.3788718806741905E-2,7.3104990884043923,-152497.01168395576,2019.0145978646967,1.222223533958201E-2,1.3600786505357374,-153623.60752171275,3490.1025050413737,10.053024900856112,1.2732082659151179E-2,1.7520056158462227,-153596.97397855803,3405.1730754874529]
["KBM","KBM-35H04-C (400 V)",25.3,14.7,16.14699240823229,9.1744275046774373,3300,93,3766,0.73,6.1,107,3.81,565,10,2019.0145978646967,3503.6277551873309,3663.5514018691588,15.582202593346151,29.527559055118111,0.39535082141252809,0.32121254916129033,3.7391331263034185E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.24156340328456868,0.36160217058498029,5.7975216788296482,17.356904188079053,12.949954089496259,23.180394992492932,2.5406050210974489,155.63558166278446,3.3788718806741905E-2,7.3104990884043923,-152497.01168395576,2019.0145978646967,1.2146403494992009E-2,1.2916660235544664,-153627.56884626593,3503.6277551873309,9.5473527896846075,1.2732082659151179E-2,1.7520056158462227,-153596.97397855803,3405.1730754874529]
["KBM","KBM-35H04-C (480 V)",25.3,14.7,11.206042017217307,6.3670693279643791,4150,93,4520,0.73,6.1,107,3.81,679,10,2019.0145978646967,3529.7485461682049,3663.5514018691588,13.312499349522174,29.527559055118111,0.39556727883949599,0.32121254916129033,3.7391331263034185E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.24156340328456868,0.36160217058498029,5.7975216788296482,17.356904188079053,12.949954089496259,23.180394992492932,2.5406050210974489,155.63558166278446,3.3788718806741905E-2,7.3104990884043923,-152497.01168395576,2019.0145978646967,1.2004522202082415E-2,1.1528130563516019,-153634.98047989138,3529.7485461682049,8.5210207196250494,1.2732082659151179E-2,1.7520056158462227,-153596.97397855803,3405.1730754874529]
["KBM","KBM-35H04-D (120 V)",24.7,19.2,21.838826104261813,16.544565230501373,1150,91.5,1443,0.43,3.4,80,3.81,160,10,1443,1443,1443,21.109848755173736,29.527559055118111,0.40487432616133412,0.32647832865573773,8.8235588685735458E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.32317562802476546,0.48376950723886641,7.7562150725943706,23.220936347465589,17.325097630101915,23.180394992492932,2.5406050210974489,155.63558166278446,1.842450150702819E-2,4.2378388639899969,-152962.46569386157,2768.6290962387889,6.6201880446799697E-3,0.57346612150568321,-153651.15377372989,4774.5050867673162,9.6247331285592104,7.1134568685653028E-3,1.0322734573451116,-153622.37544958049,4575.1607072595225]
["KBM","KBM-35H04-D (240 V)",24.7,19.2,18.65932552809381,14.13585267279834,2500,91.5,3015,0.43,3.4,80,3.81,325,10,2768.6290962387889,3015,3015,17.414946586881136,29.527559055118111,0.40484819190394916,0.32647832865573773,4.2230167321232595E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.32317562802476546,0.48376950723886641,7.7562150725943706,23.220936347465589,17.325097630101915,23.180394992492932,2.5406050210974489,155.63558166278446,1.842450150702819E-2,4.2378388639899969,-152962.46569386157,2768.6290962387889,6.6772449572880775E-3,0.64349136977810095,-153647.82495535238,4748.9995667035519,10.799997545424059,7.1134568685653028E-3,1.0322734573451116,-153622.37544958049,4575.1607072595225]
["KBM","KBM-35H04-D (400 V)",24.7,19.2,10.111019914073351,7.6598635712676897,4250,91.5,5025,0.43,3.4,80,3.81,565,10,2768.6290962387889,4807.5046312580234,4900,8.1972730991944829,29.527559055118111,0.40521895209536685,0.32647832865573773,2.7829394991849828E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.32317562802476546,0.48376950723886641,7.7562150725943706,23.220936347465589,17.325097630101915,23.180394992492932,2.5406050210974489,155.63558166278446,1.842450150702819E-2,4.2378388639899969,-152962.46569386157,2768.6290962387889,6.549853424255076E-3,0.47309050801491925,-153655.25724106352,4807.5046312580234,7.9400852370194901,7.1134568685653028E-3,1.0322734573451116,-153622.37544958049,4575.1607072595225]
["KBM","KBM-35H04-E (120 V)",24.7,20.7,22.042959618227506,17.776580337280247,1200,92.1,1536,0.37,2.8,75,3.81,160,10,1536,1536,1536,21.298988311331208,29.527559055118111,0.40477456455046296,0.32435143400651473,8.2893199527028824E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.34842372396420024,0.52156399999190295,8.3621693751408053,25.03507199961134,18.678620882453625,23.180394992492932,2.5406050210974489,155.63558166278446,1.5228744898188632E-2,3.7098524518699181,-153052.3108793491,3050.7437804982533,5.7831473378660656E-3,0.47606611672611726,-153653.92715788912,5113.5420567201427,9.9047531763561665,6.1874244411316325E-3,0.89777689064841582,-153628.17762909411,4910.8602468914223]
["KBM","KBM-35H04-E (240 V)",24.7,20.7,18.657856405542191,15.046658391566282,2600,92.1,3208,0.37,2.8,75,3.81,325,10,3050.7437804982533,3208,3208,17.244924364992055,29.527559055118111,0.40481453262427214,0.32435143400651473,3.9689511992991353E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.34842372396420024,0.52156399999190295,8.3621693751408053,25.03507199961134,18.678620882453625,23.180394992492932,2.5406050210974489,155.63558166278446,1.5228744898188632E-2,3.7098524518699181,-153052.3108793491,3050.7437804982533,5.8223660705325024E-3,0.53182968768802819,-153651.42920814638,5091.637998738116,11.064937418007846,6.1874244411316325E-3,0.89777689064841582,-153628.17762909411,4910.8602468914223]
["KBM","KBM-35H04-E (400 V)",24.7,20.7,6.8402026628842849,5.5162924700679721,4600,92.1,5347,0.37,2.8,75,3.81,565,10,3050.7437804982533,5173.5807363495733,5226.666666666667,4.6132383786066811,29.527559055118111,0.40538326411516351,0.32435143400651473,2.5927016463991703E-2,-23.47255194074074,9,29.872767072000002,9,-2429.9966400000003,7.5,2441.9966400000003,9,0.34842372396420024,0.52156399999190295,8.3621693751408053,25.03507199961134,18.678620882453625,23.180394992492932,2.5406050210974489,155.63558166278446,1.5228744898188632E-2,3.7098524518699181,-153052.3108793491,3050.7437804982533,5.6844623195075484E-3,0.29191556518468803,-153660.21268012456,5173.5807363495733,6.0734245095503194,6.1874244411316325E-3,0.89777689064841582,-153628.17762909411,4910.8602468914223]
["KBM","KBM-45H01-A (120 V)",30.7,10.24,28.329579870357374,9.1979155423238232,450,118,617,1.36,21,187,6.1,160,10,617,617,617,27.449890622245555,18.442622950819672,0.32761244887240326,0.25714230779661018,0.20635973172368924,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.13924920058351348,0.21085110841259502,3.3419808140043235,10.120853203804561,7.5339861350389885,23.27649774014472,2.6210100637922698,160.56113501897829,0.1754392238223442,17.337430403901937,-151515.05026587733,881.21957338010338,3.8456892304321241E-2,2.7319586825711104,-153610.64132343451,1963.3851580952091,6.2020174614555126,4.0115911855723559E-2,3.3186844383955889,-153585.26121420652,1915.7382890812353]
["KBM","KBM-45H01-A (240 V)",30.7,10.24,27.341143907997175,8.876994775323757,950,118,1293,1.36,21,187,6.1,325,10,881.21957338010338,1293,1293,26.128420076884577,18.442622950819672,0.32720134631703462,0.25714230779661018,9.8471735865055116E-2,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.13924920058351348,0.21085110841259502,3.3419808140043235,10.120853203804561,7.5339861350389885,23.27649774014472,2.6210100637922698,160.56113501897829,0.1754392238223442,17.337430403901937,-151515.05026587733,881.21957338010338,4.0398752061809769E-2,3.4086514346795891,-153580.93425174337,1908.0445814256541,7.738226735553102,4.0115911855723559E-2,3.3186844383955889,-153585.26121420652,1915.7382890812353]
["KBM","KBM-45H01-A (400 V)",30.7,10.24,24.99187334951591,8.1142445939986718,1750,118,2155,1.36,21,187,6.1,565,10,881.21957338010338,1893.3525871280328,2096.2566844919784,24.524287793515128,18.442622950819672,0.32713643878005599,0.25714230779661018,6.646208158974537E-2,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.13924920058351348,0.21085110841259502,3.3419808140043235,10.120853203804561,7.5339861350389885,23.27649774014472,2.6210100637922698,160.56113501897829,0.1754392238223442,17.337430403901937,-151515.05026587733,881.21957338010338,4.0950510992111867E-2,3.5776516034744095,-153572.49330123936,1893.3525871280328,8.1218862705750503,4.0115911855723559E-2,3.3186844383955889,-153585.26121420652,1915.7382890812353]
["KBM","KBM-45H01-A (480 V)",30.7,10.24,23.64587725936731,7.6772328764179578,2100,118,2586,1.36,21,187,6.1,679,10,881.21957338010338,1893.7334450945198,2096.2566844919784,24.338748495362886,18.442622950819672,0.32715950222568463,0.25714230779661018,6.646208158974537E-2,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.13924920058351348,0.21085110841259502,3.3419808140043235,10.120853203804561,7.5339861350389885,23.27649774014472,2.6210100637922698,160.56113501897829,0.1754392238223442,17.337430403901937,-151515.05026587733,881.21957338010338,4.0936013818488784E-2,3.5733134604023684,-153572.71508274262,1893.7334450945198,8.1120379374890721,4.0115911855723559E-2,3.3186844383955889,-153585.26121420652,1915.7382890812353]
["KBM","KBM-45H01-B (120 V)",30.2,12.5,27.738432938873189,11.184851991481125,525,118,763,0.92,14,150,6.1,160,10,763,763,763,26.622522537829035,18.442622950819672,0.33291543470070201,0.25714230779661018,0.16687281058127951,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.17279620474157731,0.26164797461368655,4.1471089137978554,12.559102781456954,9.3490246640922869,23.27649774014472,2.6210100637922698,160.56113501897829,0.11863570911371593,11.674137148365727,-152149.71690934608,1084.339697934495,2.4482624226236947E-2,1.676496412377797,-153632.77066421427,2471.0255745874833,7.0139540216069776,2.6022469086555762E-2,2.2346320292802906,-153608.51577437459,2387.0350404631986]
["KBM","KBM-45H01-B (240 V)",30.2,12.5,26.101410667070837,10.52476236575437,1200,118,1596,0.92,14,150,6.1,325,10,{"$f":"IF(AQ699<I699,IF(AQ699<0,0,AQ699),I699)","v":1084.339697934495},{"$f":"IF(AU699<I699,IF(AU699<0,0,AU699),I699)","v":1596},{"$f":"IF(UAC_V*0.98/L699*1000<I699,IF(UAC_V*0.98/L699*1000<0,0,UAC_V*0.98/L699*1000),I699)","v":1596},{"$f":"C699+(E699-C699)/G699*Q699","v":24.748876187204214},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M699,(inertia/gear^2+gear_inertia)/M699),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M699,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M699))","v":18.442622950819672},{"$f":"IF((C699+(E699-C699)/G699*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X699^2*time1+Y699^2*time2+Z699^2*time3+AA699^2*time4)/time)/(C699+(E699-C699)/G699*mspeed),SQRT((((X699-Y699)*2/PI()+Y699)^2*time1+Y699^2*time2+((Z699-Y699)*2/PI()+Y699)^2*time3+AA699^2*time4)/time)/(C699+(E699-C699)/G699*mspeed)),IF(AccType=1,SQRT((X699^2*time1+Y699^2*time2+Z699^2*time3+AA699^2*time4+AB699^2*time5+AC699^2*time6+AD699^2*time7+AE699^2*time8)/time)/(C699+(E699-C699)/G699*mspeed),SQRT((((X699-Y699)*2/PI()+Y699)^2*time1+Y699^2*time2+((Z699-Y699)*2/PI()+Y699)^2*time3+AA699^2*time4+((AB699-AC699)*2/PI()+AC699)^2*time5+AC699^2*time6+((AD699-AC699)*2/PI()+AC699)^2*time7+AE699^2*time8)/time)/(C699+(E699-C699)/G699*mspeed))))","v":0.33260326117069483},{"$f":"IF(move1,MAX(ABS(X699),ABS(Z699))/H699,MAX(ABS(X699),ABS(Z699),ABS(AB699),ABS(AD699))/H699)","v":0.25714230779661018},{"$f":"IF(AZ699>0,speed/(MIN(AZ699,I699)),\"NA\")","v":7.9776913830523974E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M699+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M699+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-24.052830024691357},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M699+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M699+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":30.342792320000001},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M699+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M699+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2477.9584},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M699+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M699+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2489.9584},9,{"$f":"AH699/Irms","v":0.17279620474157731},{"$f":"AI699/Ipeak","v":0.26164797461368655},{"$f":"IF(move1,IF(AccType=1,SQRT((X699^2*time1+Y699^2*time2+Z699^2*time3+AA699^2*time4)/time)/(C699/D699),SQRT((((X699-Y699)*2/PI()+Y699)^2*time1+Y699^2*time2+((Z699-AA699)*2/PI()+AA699)^2*time3+AA699^2*time4)/time)/(C699/D699)),IF(AccType=1,SQRT((X699^2*time1+Y699^2*time2+Z699^2*time3+AA699^2*time4+AB699^2*time5+AC699^2*time6+AD699^2*time7+AE699^2*time8)/time)/(C699/D699),SQRT((((X699-Y699)*2/PI()+Y699)^2*time1+Y699^2*time2+((Z699-AA699)*2/PI()+AA699)^2*time3+AA699^2*time4+((AB699-AC699)*2/PI()+AC699)^2*time5+AC699^2*time6+((AD699-AE699)*2/PI()+AE699)^2*time7+AE699^2*time8)/time)/(C699/D699)))","v":4.1471089137978554},{"$f":"IF(move1,MAX(ABS(X699),ABS(Z699))/(C699/D699),MAX(ABS(X699),ABS(Z699),ABS(AB699),ABS(AD699))/(C699/D699))","v":12.559102781456954},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X699),ABS(Z699))/(C699/D699),MAX(ABS((X699-Y699)*2/PI()+Y699),ABS((Z699-Y699)*2/PI()+Y699))/(C699/D699)),IF(AccType=1,MAX(ABS(X699),ABS(Z699),ABS(AB699),ABS(AD699))/(C699/D699),MAX(ABS((X699-Y699)*2/PI()+Y699),ABS((Z699-Y699)*2/PI()+Y699),ABS((AB699-AC699)*2/PI()+AC699),ABS((AD699-AC699)*2/PI()+AC699))/(C699/D699)))","v":9.3490246640922869},{"$f":"IF((C699+(E699-C699)/G699*mspeed)<0,\"NA\",U699*(C699+(E699-C699)/G699*mspeed)*mspeed/9.55)","v":23.27649774014472},{"$f":"IF(move1,IF(speed1>speed2,AM699/2*time1/time,AM699/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z699*-speed/30*PI(),((Z699-AA699)*2/PI()+AA699)*-speed/30*PI()),IF(AccType=1,X699*-speed/30*PI(),((X699-Y699)*2/PI()+Y699)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z699*-speed/30*PI(),((Z699-AA699)*2/PI()+AA699)*-speed/30*PI()),IF(AccType=1,X699*-speed/30*PI(),((X699-Y699)*2/PI()+Y699)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD699*-speed/30*PI(),((AD699-AE699)*2/PI()+AE699)*-speed/30*PI()),IF(AccType=1,AB699*-speed/30*PI(),((AB699-AC699)*2/PI()+AC699)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD699*-speed/30*PI(),((AD699-AE699)*2/PI()+AE699)*-speed/30*PI()),IF(AccType=1,AB699*-speed/30*PI(),((AB699-AC699)*2/PI()+AC699)*-speed/30*PI()),0)/2*time7/time)))","v":2.6210100637922698},{"$f":"IF(move1,MAX(IF(AccType=1,Z699*-speed/30*PI(),((Z699-AA699)*2/PI()+AA699)*-speed/30*PI()),IF(AccType=1,X699*-speed/30*PI(),((X699-Y699)*2/PI()+Y699)*-speed/30*PI()),0),MAX(IF(AccType=1,Z699*-speed/30*PI(),((Z699-AA699)*2/PI()+AA699)*-speed/30*PI()),IF(AccType=1,X699*-speed/30*PI(),((X699-Y699)*2/PI()+Y699)*-speed/30*PI()),IF(AccType=1,AD699*-speed/30*PI(),((AD699-AE699)*2/PI()+AE699)*-speed/30*PI()),IF(AccType=1,AB699*-speed/30*PI(),((AB699-AC699)*2/PI()+AC699)*-speed/30*PI()),0))","v":160.56113501897829},{"$f":"(L699^2)/1000000+((K699/1000)^2*(D699/C699*H699)^2*PI()*PI()*(O699/2)^2)/1200","v":0.11863570911371593},{"$f":"SQRT(3)*L699*J699*D699/C699*H699/1000","v":11.674137148365727},{"$f":"0.75*J699^2*(D699/C699*H699)^2-(UAC_V*0.98)^2","v":-152149.71690934608},{"$f":"-AO699/2/AN699+SQRT((AO699/2/AN699)^2-AP699/AN699)","v":1084.339697934495},{"$f":"(L699^2)/1000000+((K699/1000)^2*AV699^2*PI()*PI()*(O699/2)^2)/1200","v":2.568878446802977E-2},{"$f":"SQRT(3)*L699*J699*AV699/1000","v":2.1261554160842771},{"$f":"0.75*J699^2*AV699^2-(UAC_V*0.98)^2","v":-153613.77181274063},{"$f":"-AS699/2/AR699+SQRT((AS699/2/AR699)^2-AT699/AR699)","v":2404.3299736778872},{"$f":"D699+(F699-D699)*((0.85*UAC_V-D699*J699)/L699*1000)/G699","v":8.895191317501725},{"$f":"(L699^2)/1000000+((K699/1000)^2*AJ699^2*PI()*PI()*(O699/2)^2)/1200","v":2.6022469086555762E-2},{"$f":"SQRT(3)*L699*J699*AJ699/1000","v":2.2346320292802906},{"$f":"0.75*J699^2*AJ699^2-(UAC_V*0.98)^2","v":-153608.51577437459},{"$f":"IF(((AX699/2/AW699)^2-AY699/AW699)>0,-AX699/2/AW699+SQRT((AX699/2/AW699)^2-AY699/AW699),-9999)","v":2387.0350404631986}]
["KBM","KBM-45H01-B (400 V)",30.2,12.5,23.09597313705644,9.3128923939743711,2150,118,2660,0.92,14,150,6.1,565,10,1084.339697934495,2390.705568383235,2613.3333333333335,22.300634149217089,18.442622950819672,0.33257600154762207,0.25714230779661018,5.3339792803715758E-2,-24.052830024691357,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},30.342792320000001,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},-2477.9584,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},2489.9584,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},0.17279620474157731,0.26164797461368655,4.1471089137978554,12.559102781456954,9.3490246640922869,23.27649774014472,2.6210100637922698,160.56113501897829,0.11863570911371593,11.674137148365727,-152149.71690934608,1084.339697934495,2.5950927040498811E-2,2.2118227097726146,-153609.64267000594,2390.705568383235,9.2535973687459876,2.6022469086555762E-2,2.2346320292802906,-153608.51577437459,2387.0350404631986]
["KBM","KBM-45H01-B (480 V)",30.2,12.5,20.720171836492035,8.3549079985854977,2650,118,3192,0.92,14,150,6.1,679,10,1084.339697934495,2397.5487113569716,2613.3333333333335,21.623264227432436,18.442622950819672,0.33264290050482848,0.25714230779661018,5.3339792803715758E-2,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.17279620474157731,0.26164797461368655,4.1471089137978554,12.559102781456954,9.3490246640922869,23.27649774014472,2.6210100637922698,160.56113501897829,0.11863570911371593,11.674137148365727,-152149.71690934608,1084.339697934495,2.5818590111406043E-2,2.1689983990431627,-153611.72717716609,2397.5487113569716,9.0744334026046189,2.6022469086555762E-2,2.2346320292802906,-153608.51577437459,2387.0350404631986]
["KBM","KBM-45H01-C (120 V)",31.3,14.3,28.427521373798537,12.69085775616006,650,119,854,0.69,11,135,6.1,160,10,854,854,854,27.526005004959924,18.442622950819672,0.32111497153752544,0.25498144806722689,0.14909128158491367,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.19073167790338039,0.28880586406815761,4.5775602696811291,13.862681475271566,10.31941160750133,23.27649774014472,2.6210100637922698,160.56113501897829,9.1764589441662964E-2,8.7716672376422391,-152608.55217931513,1242.6816076419614,1.9916763280895779E-2,1.3304279028309061,-153639.71963779654,2744.2263174994464,8.246085967115544,2.0874437927596908E-2,1.6649393661632352,-153625.97499186557,2673.257936174266]
["KBM","KBM-45H01-C (240 V)",31.3,14.3,26.601611916788226,11.875719605709028,1400,119,1783,0.69,11,135,6.1,325,10,1242.6816076419614,1783,1783,25.316267176881006,18.442622950819672,0.32087239613643509,0.25498144806722689,7.1409957640783103E-2,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.19073167790338039,0.28880586406815761,4.5775602696811291,13.862681475271566,10.31941160750133,23.27649774014472,2.6210100637922698,160.56113501897829,9.1764589441662964E-2,8.7716672376422391,-152608.55217931513,1242.6816076419614,2.0745623510874483E-2,1.6239607888176342,-153627.82374974462,2682.4119892465224,10.065423495193325,2.0874437927596908E-2,1.6649393661632352,-153625.97499186557,2673.257936174266]
["KBM","KBM-45H01-C (400 V)",31.3,14.3,22.23076245107594,9.9244475228017581,2500,119,2972,0.69,11,135,6.1,565,10,1242.6816076419614,2684.038231512895,2903.7037037037039,21.563127875206209,18.442622950819672,0.32093435167127538,0.25498144806722689,4.7628757685736538E-2,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.19073167790338039,0.28880586406815761,4.5775602696811291,13.862681475271566,10.31941160750133,23.27649774014472,2.6210100637922698,160.56113501897829,9.1764589441662964E-2,8.7716672376422391,-152608.55217931513,1242.6816076419614,2.0722903504055458E-2,1.6166253181219135,-153628.14982964069,2684.038231512895,10.019957730504039,2.0874437927596908E-2,1.6649393661632352,-153625.97499186557,2673.257936174266]
["KBM","KBM-45H01-C (480 V)",31.3,14.3,18.621128341751753,8.3130037239963173,3100,119,3567,0.69,11,135,6.1,679,10,1242.6816076419614,2699.6715471470766,2903.7037037037039,20.258455140096043,18.442622950819672,0.32103981489544547,0.25498144806722689,4.7628757685736538E-2,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.19073167790338039,0.28880586406815761,4.5775602696811291,13.862681475271566,10.31941160750133,23.27649774014472,2.6210100637922698,160.56113501897829,9.1764589441662964E-2,8.7716672376422391,-152608.55217931513,1242.6816076419614,2.0507013043603577E-2,1.5451854451049976,-153631.24831193738,2699.6715471470766,9.5771683594123687,2.0874437927596908E-2,1.6649393661632352,-153625.97499186557,2673.257936174266]
["KBM","KBM-45H01-D (120 V)",29.7,20.2,26.335954793732576,17.326286048508273,950,118,1263,0.35,5,91.2,6.1,160,10,1263,1263,1263,25.227590425772888,18.442622950819672,0.33824878455403573,0.25714230779661018,0.10081073196636284,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.28393965452000491,0.42994136143658812,6.8145517084801179,20.63718534895623,15.362367693152482,23.27649774014472,2.6210100637922698,160.56113501897829,4.1426920880529877E-2,4.4371124731678089,-153072.23236778559,1869.4291339814943,8.7484891262132672E-3,0.50627634514378839,-153656.29583448597,4162.0778734294272,9.1572300799845276,9.5305909087390304E-3,0.84934017170150544,-153642.3172849078,3970.7806978359772]
["KBM","KBM-45H01-D (240 V)",29.7,20.2,22.804629703024432,15.003045857252916,2100,118,2635,0.35,5,91.2,6.1,325,10,1869.4291339814943,2635,2635,21.047952032128276,18.442622950819672,0.33818353840213228,0.25714230779661018,4.8320286327710162E-2,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.28393965452000491,0.42994136143658812,6.8145517084801179,20.63718534895623,15.362367693152482,23.27649774014472,2.6210100637922698,160.56113501897829,4.1426920880529877E-2,4.4371124731678089,-153072.23236778559,1869.4291339814943,8.9583270142866486E-3,0.61732659570674109,-153652.5453899948,4107.1760183923088,11.16584198650383,9.5305909087390304E-3,0.84934017170150544,-153642.3172849078,3970.7806978359772]
["KBM","KBM-45H01-D (400 V)",29.7,20.2,12.723792477454767,8.3709161035886623,3700,118,4392,0.35,5,91.2,6.1,565,10,1869.4291339814943,4177.6347928738414,4298.2456140350869,10.532325622369839,18.442622950819672,0.33851425898297555,0.25714230779661018,3.2065219452413009E-2,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.28393965452000491,0.42994136143658812,6.8145517084801179,20.63718534895623,15.362367693152482,23.27649774014472,2.6210100637922698,160.56113501897829,4.1426920880529877E-2,4.4371124731678089,-153072.23236778559,1869.4291339814943,8.6913752066192663E-3,0.47154422455342859,-153657.31663481463,4177.6347928738414,8.5290158201984756,9.5305909087390304E-3,0.84934017170150544,-153642.3172849078,3970.7806978359772]
["KBM","KBM-45H01-E (120 V)",31.2,23.4,27.345712949425653,19.960374415639162,1100,118,1394,0.26,3.2,82.7,6.1,160,10,1394,1394,1394,26.315567137726692,18.442622950819672,0.32193723394249935,0.25714230779661018,9.1337126595061879E-2,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.31310672299173808,0.47410612999999996,7.5145613518017136,22.757094239999997,16.940432691335221,23.27649774014472,2.6210100637922698,160.56113501897829,2.3330214601692188E-2,3.2959662470946212,-153266.90492500001,2493.4316135688764,7.083716855870106E-3,0.4012681717532543,-153658.11429601384,4629.2015980656179,10.774452933632702,7.4435272044031135E-3,0.6309050210375049,-153649.45020222967,4501.1673836301397]
["KBM","KBM-45H01-E (240 V)",31.2,23.4,23.167423890072417,16.910528386914173,2300,118,2909,0.26,3.2,82.7,6.1,325,10,2493.4316135688764,2909,2909,21.04053743313942,18.442622950819672,0.3219346009524886,0.25714230779661018,4.3768977130806554E-2,-24.052830024691357,9,30.342792320000001,9,-2477.9584,7.5,2489.9584,9,0.31310672299173808,0.47410612999999996,7.5145613518017136,22.757094239999997,16.940432691335221,23.27649774014472,2.6210100637922698,160.56113501897829,2.3330214601692188E-2,3.2959662470946212,-153266.90492500001,2493.4316135688764,7.1428710734378099E-3,0.44719567913717512,-153656.6898853741,4606.8937016335212,12.00765257791301,7.4435272044031135E-3,0.6309050210375049,-153649.45020222967,4501.1673836301397]
["KBM","KBM-45H02-A (120 V)",43.7,13.3,40.226411866476546,12.00788413924673,400,171,568,0.95,16,202,9.2200000000000006,160,10,568,568,568,38.767504850396691,12.20173535791757,0.23161129842656489,0.18118816411695907,0.22416189167872583,-24.84342723950617,9,30.983176064000002,9,-2543.30368,7.5,2555.30368,9,0.12778539251371007,0.19645129750724641,3.0668494203290417,9.4296622803478272,6.9984552953243915,23.409789758829294,2.730557545542418,167.2719326047096,0.18337496924834726,17.298239926827986,-151830.66806828923,863.9889508548714,4.4227732883788937E-2,2.6806264745974939,-153619.97393456331,1833.6436985481287,8.0649318223329907,4.3382118402487777E-2,2.3261504200176488,-153630.84776139259,1855.225893808109]
["KBM","KBM-45H02-A (240 V)",43.7,13.3,38.46847317687061,11.483126321453913,880,171,1188,0.95,16,202,9.2200000000000006,325,10,863.9889508548714,1188,1188,36.63743878877532,12.20173535791757,0.23128824808237469,0.18118816411695907,0.10717504585312818,-24.84342723950617,9,30.983176064000002,9,-2543.30368,7.5,2555.30368,9,0.12778539251371007,0.19645129750724641,3.0668494203290417,9.4296622803478272,6.9984552953243915,23.409789758829294,2.730557545542418,167.2719326047096,0.18337496924834726,17.298239926827986,-151830.66806828923,863.9889508548714,4.6019497755223432E-2,3.3085236760941479,-153596.93348130528,1791.3300259637037,9.9540231110641315,4.3382118402487777E-2,2.3261504200176488,-153630.84776139259,1855.225893808109]
["KBM","KBM-45H02-A (400 V)",43.7,13.3,34.85493253712508,10.40445747376868,1600,171,1980,0.95,16,202,9.2200000000000006,565,10,863.9889508548714,1781.4762894002708,1940.5940594059405,33.851701272964078,12.20173535791757,0.23123917462694921,0.18118816411695907,6.8629892941051054E-2,-24.84342723950617,9,30.983176064000002,9,-2543.30368,7.5,2555.30368,9,0.12778539251371007,0.19645129750724641,3.0668494203290417,9.4296622803478272,6.9984552953243915,23.409789758829294,2.730557545542418,167.2719326047096,0.18337496924834726,17.298239926827986,-151830.66806828923,863.9889508548714,4.6461397291574134E-2,3.4458367982177625,-153591.25105847497,1781.4762894002708,10.367143319617215,4.3382118402487777E-2,2.3261504200176488,-153630.84776139259,1855.225893808109]
["KBM","KBM-45H02-A (480 V)",43.7,13.3,32.565549894187811,9.7210596699068095,1950,171,2376,0.95,16,202,9.2200000000000006,679,10,863.9889508548714,1782.4761066244373,1940.5940594059405,33.522107038968123,12.20173535791757,0.23126058038458758,0.18118816411695907,6.8629892941051054E-2,-24.84342723950617,9,30.983176064000002,9,-2543.30368,7.5,2555.30368,9,0.12778539251371007,0.19645129750724641,3.0668494203290417,9.4296622803478272,6.9984552953243915,23.409789758829294,2.730557545542418,167.2719326047096,0.18337496924834726,17.298239926827986,-151830.66806828923,863.9889508548714,4.6416137330960366E-2,3.4320255343126402,-153591.83306006656,1782.4761066244373,10.325590756128568,4.3382118402487777E-2,2.3261504200176488,-153630.84776139259,1855.225893808109]
["KBM","KBM-45H02-B (120 V)",43.5,14.9,39.894839068368434,13.387529888714239,450,171,638,0.76,12,180,9.2200000000000006,160,10,638,638,638,38.388682945820136,12.20173535791757,0.2326007804262335,0.18118816411695907,0.19956732676099728,-24.84342723950617,9,30.983176064000002,9,-2543.30368,7.5,2555.30368,9,0.14381626934137418,0.22109641923065135,3.45159046419298,10.612628123071264,7.8764224292534282,23.409789758829294,2.730557545542418,167.2719326047096,0.13397977436369921,13.878414256467329,-152177.80877874911,1015.2165380078853,3.4673565661469549E-2,2.076299385125898,-153630.73596345159,2075.2126579468704,8.7628070827535929,3.4236872450179021E-2,1.8662753718539882,-153637.12512528096,2091.2862121431285]
["KBM","KBM-45H02-B (240 V)",43.5,14.9,37.515093728803905,12.588957627115404,1050,171,1334,0.76,12,180,9.2200000000000006,325,10,1015.2165380078853,1334,1334,35.896319080213722,12.20173535791757,0.23232575698573954,0.18118816411695907,9.5445243233520438E-2,-24.84342723950617,9,30.983176064000002,9,-2543.30368,7.5,2555.30368,9,0.14381626934137418,0.22109641923065135,3.45159046419298,10.612628123071264,7.8764224292534282,23.409789758829294,2.730557545542418,167.2719326047096,0.13397977436369921,13.878414256467329,-152177.80877874911,1015.2165380078853,3.5905593124238293E-2,2.5782022251605698,-153612.71044202297,2032.799501673029,10.881036174866573,3.4236872450179021E-2,1.8662753718539882,-153637.12512528096,2091.2862121431285]
["KBM","KBM-45H02-B (400 V)",43.5,14.9,32.769165125026028,10.996364135914774,1900,171,2223,0.76,12,180,9.2200000000000006,565,10,1015.2165380078853,2027.0852984448106,2177.7777777777774,32.051411781527051,12.20173535791757,0.23231956540590729,0.18118816411695907,6.0883084168109156E-2,-24.84342723950617,9,30.983176064000002,9,-2543.30368,7.5,2555.30368,9,0.14381626934137418,0.22109641923065135,3.45159046419298,10.612628123071264,7.8764224292534282,23.409789758829294,2.730557545542418,167.2719326047096,0.13397977436369921,13.878414256467329,-152177.80877874911,1015.2165380078853,3.6080015771448933E-2,2.6415635583491195,-153610.15850283334,2027.0852984448106,11.14844613665475,3.4236872450179021E-2,1.8662753718539882,-153637.12512528096,2091.2862121431285]
["KBM","KBM-45H02-B (480 V)",43.5,14.9,29.257419325829272,9.8179259482648558,2350,171,2667,0.76,12,180,9.2200000000000006,679,10,1015.2165380078853,2031.3080686626404,2177.7777777777774,31.188906790629112,12.20173535791757,0.23236863670316163,0.18118816411695907,6.0883084168109156E-2,-24.84342723950617,9,30.983176064000002,9,-2543.30368,7.5,2555.30368,9,0.14381626934137418,0.22109641923065135,3.45159046419298,10.612628123071264,7.8764224292534282,23.409789758829294,2.730557545542418,167.2719326047096,0.13397977436369921,13.878414256467329,-152177.80877874911,1015.2165380078853,3.5950928388171356E-2,2.5948196713502698,-153612.04715179917,2031.3080686626404,10.951168390004492,3.4236872450179021E-2,1.8662753718539882,-153637.12512528096,2091.2862121431285]
["KBM","KBM-45H02-C (120 V)",41.8,21.1,37.242256683503506,18.345939252957393,750,168,941,0.38,5.9,123,9.2200000000000006,160,10,941,941,941,36.081551385569064,12.20173535791757,0.24185163539413729,0.18442366704761906,0.13530707170405554,-24.84342723950617,9,30.983176064000002,9,-2543.30368,7.5,2555.30368,9,0.21194207445968385,0.32582985194896336,5.0866097870324127,15.639832893550242,11.607485833290935,23.409789758829294,2.730557545542418,167.2719326047096,6.6603654677383994E-2,6.8653833220766289,-152885.14005950413,1464.4104450032271,1.6025061124486862E-2,0.90580953448853596,-153650.44175238334,3068.3379969812563,11.188904120057463,1.6093359261876928E-2,0.93969625858064287,-153649.40833732582,3060.8261806805717]
["KBM","KBM-45H02-C (240 V)",41.8,21.1,33.243488738319641,16.376102826758444,1600,168,1964,0.38,5.9,123,9.2200000000000006,325,10,1464.4104450032271,1964,1964,31.296882426287361,12.20173535791757,0.24175776782569181,0.18442366704761906,6.4828897389774071E-2,-24.84342723950617,9,30.983176064000002,9,-2543.30368,7.5,2555.30368,9,0.21194207445968385,0.32582985194896336,5.0866097870324127,15.639832893550242,11.607485833290935,23.409789758829294,2.730557545542418,167.2719326047096,6.6603654677383994E-2,6.8653833220766289,-152885.14005950413,1464.4104450032271,1.6363170222055044E-2,1.0630546746116374,-153645.32584372375,3031.951415207378,13.131255938175414,1.6093359261876928E-2,0.93969625858064287,-153649.40833732582,3060.8261806805717]
["KBM","KBM-45H02-C (400 V)",41.8,21.1,22.654882933908411,11.160040854142075,2900,168,3274,0.38,5.9,123,9.2200000000000006,565,10,1464.4104450032271,3056.4104002292602,3186.9918699186992,21.622298305376194,12.20173535791757,0.24191923554169539,0.18442366704761906,4.1597904277336624E-2,-24.84342723950617,9,30.983176064000002,9,-2543.30368,7.5,2555.30368,9,0.21194207445968385,0.32582985194896336,5.0866097870324127,15.639832893550242,11.607485833290935,23.409789758829294,2.730557545542418,167.2719326047096,6.6603654677383994E-2,6.8653833220766289,-152885.14005950413,1464.4104450032271,1.6133880593906788E-2,0.95923562451027045,-153648.79521145928,3056.4104002292602,11.848843517913638,1.6093359261876928E-2,0.93969625858064287,-153649.40833732582,3060.8261806805717]
["KBM","KBM-45H02-C (480 V)",41.8,21.1,12.34587629984274,6.0817124629767196,3500,168,3929,0.38,5.9,123,9.2200000000000006,679,10,1464.4104450032271,3096.3833606721769,3186.9918699186992,15.74249756332944,12.20173535791757,0.24215316356280306,0.18442366704761906,4.1597904277336624E-2,-24.84342723950617,9,30.983176064000002,9,-2543.30368,7.5,2555.30368,9,0.21194207445968385,0.32582985194896336,5.0866097870324127,15.639832893550242,11.607485833290935,23.409789758829294,2.730557545542418,167.2719326047096,6.6603654677383994E-2,6.8653833220766289,-152885.14005950413,1464.4104450032271,1.5777495396456218E-2,0.77058671684522706,-153654.18765469996,3096.3833606721769,9.5185804108802277,1.6093359261876928E-2,0.93969625858064287,-153649.40833732582,3060.8261806805717]
["KBM","KBM-45H03-A (120 V)",54.6,14.1,50.202016335272141,12.67727685234145,350,218,480,0.93,16,240,12.2,160,10,480,480,480,48.568479545516077,9.221311475409836,0.18653242019293467,0.14493038825688073,0.26525823848649221,-25.598548938271605,9,31.594824640000002,9,-2605.7168000000001,7.5,2617.7168000000001,9,0.10902825348992427,0.1699813138827839,2.6166780837581824,8.1591030663736266,6.0388058768851884,23.53960068107552,2.8351894351627531,173.68160465774793,0.22442625491965246,21.763953091181758,-151608.14212606268,774.85134692641111,6.1460082687145083E-2,3.3105784588722567,-153616.43086053667,1554.2616738179361,8.5634559337064236,5.9519555226012447E-2,2.3345645505849419,-153640.3446543366,1587.1635685969388]
["KBM","KBM-45H03-A (240 V)",54.6,14.1,47.7464829275686,12.05719265847692,800,218,1005,0.93,16,240,12.2,325,10,774.85134692641111,1005,1005,45.990269177758051,9.221311475409836,0.18622827474743342,0.14493038825688073,0.12669050196369777,-25.598548938271605,9,31.594824640000002,9,-2605.7168000000001,7.5,2617.7168000000001,9,0.10902825348992427,0.1699813138827839,2.6166780837581824,8.1591030663736266,6.0388058768851884,23.53960068107552,2.8351894351627531,173.68160465774793,0.22442625491965246,21.763953091181758,-151608.14212606268,774.85134692641111,6.3539020590363843E-2,4.1064165014054721,-153590.81138679245,1522.7780632806696,10.622046023705963,5.9519555226012447E-2,2.3345645505849419,-153640.3446543366,1587.1635685969388]
["KBM","KBM-45H03-A (400 V)",54.6,14.1,43.688031878725276,11.032331282506384,1400,218,1676,0.93,16,240,12.2,565,10,774.85134692641111,1514.7039861644841,1633.3333333333333,42.793998849860998,9.221311475409836,0.18616962276119806,0.14493038825688073,8.0221066683171999E-2,-25.598548938271605,9,31.594824640000002,9,-2605.7168000000001,7.5,2617.7168000000001,9,0.10902825348992427,0.1699813138827839,2.6166780837581824,8.1591030663736266,6.0388058768851884,23.53960068107552,2.8351894351627531,173.68160465774793,0.22442625491965246,21.763953091181758,-151608.14212606268,774.85134692641111,6.4103678014459833E-2,4.2971953484070902,-153583.85291726401,1514.7039861644841,11.115532666501977,5.9519555226012447E-2,2.3345645505849419,-153640.3446543366,1587.1635685969388]
["KBM","KBM-45H03-A (480 V)",54.6,14.1,40.837285986285153,10.312445956132615,1700,218,2011,0.93,16,240,12.2,679,10,774.85134692641111,1515.53208788746,1633.3333333333333,42.330685468115725,9.221311475409836,0.18619250206508464,0.14493038825688073,8.0221066683171999E-2,-25.598548938271605,9,31.594824640000002,9,-2605.7168000000001,7.5,2617.7168000000001,9,0.10902825348992427,0.1699813138827839,2.6166780837581824,8.1591030663736266,6.0388058768851884,23.53960068107552,2.8351894351627531,173.68160465774793,0.22442625491965246,21.763953091181758,-151608.14212606268,774.85134692641111,6.4045186990435682E-2,4.2778282274938686,-153584.57372246552,1515.53208788746,11.065435836427261,5.9519555226012447E-2,2.3345645505849419,-153640.3446543366,1587.1635685969388]
["KBM","KBM-45H03-B (120 V)",53,19.899999999999999,49.482718670389282,18.125537974501569,550,216,699,0.47,7.7,165,12.2,160,10,699,699,699,48.529855182912925,9.221311475409836,0.19169558890213351,0.1462723362962963,0.18215158007656118,-25.598548938271605,9,31.594824640000002,9,-2605.7168000000001,7.5,2617.7168000000001,9,0.15852209092324676,0.24714505123270439,3.8045301821579223,11.862962459169811,8.7801473805310213,23.53960068107552,2.8351894351627531,173.68160465774793,0.10741161384298485,10.893649239278348,-152574.27002985831,1142.2004448178975,2.9425390557169421E-2,1.8045641969638115,-153634.09686004624,2254.5238478256624,13.434759830909318,2.8164817592025885E-2,1.1793541385472961,-153651.22795055914,2314.8436559985871]
["KBM","KBM-45H03-B (240 V)",53,19.899999999999999,45.50447416401321,16.668305554583593,1150,216,1459,0.47,7.7,165,12.2,325,10,1142.2004448178975,1459,1459,43.490458961126322,9.221311475409836,0.19170546920039055,0.1462723362962963,8.7267960571292852E-2,-25.598548938271605,9,31.594824640000002,9,-2605.7168000000001,7.5,2617.7168000000001,9,0.15852209092324676,0.24714505123270439,3.8045301821579223,11.862962459169811,8.7801473805310213,23.53960068107552,2.8351894351627531,173.68160465774793,0.10741161384298485,10.893649239278348,-152574.27002985831,1142.2004448178975,2.9707019996305706E-2,1.9165717762077612,-153630.26953743474,2242.0671849388332,14.268642564987623,2.8164817592025885E-2,1.1793541385472961,-153651.22795055914,2314.8436559985871]
["KBM","KBM-45H03-B (400 V)",53,19.899999999999999,33.533576381687716,12.283361311973522,2150,216,2432,0.47,7.7,165,12.2,565,10,1142.2004448178975,2263.6843197462658,2375.757575757576,32.504261438924701,9.221311475409836,0.1919097781419716,0.1462723362962963,5.5003263025377287E-2,-25.598548938271605,9,31.594824640000002,9,-2605.7168000000001,7.5,2617.7168000000001,9,0.15852209092324676,0.24714505123270439,3.8045301821579223,11.862962459169811,8.7801473805310213,23.53960068107552,2.8351894351627531,173.68160465774793,0.10741161384298485,10.893649239278348,-152574.27002985831,1142.2004448178975,2.9222645771087748E-2,1.719418877108154,-153636.85214623547,2263.6843197462658,12.800863333953796,2.8164817592025885E-2,1.1793541385472961,-153651.22795055914,2314.8436559985871]
["KBM","KBM-45H03-B (480 V)",53,19.899999999999999,24.699622899069141,9.0474809154099418,2600,216,2918,0.47,7.7,165,12.2,679,10,1142.2004448178975,2281.1243314531234,2375.757575757576,28.170508156064543,9.221311475409836,0.19205751165236762,0.1462723362962963,5.5003263025377287E-2,-25.598548938271605,9,31.594824640000002,9,-2605.7168000000001,7.5,2617.7168000000001,9,0.15852209092324676,0.24714505123270439,3.8045301821579223,11.862962459169811,8.7801473805310213,23.53960068107552,2.8351894351627531,173.68160465774793,0.10741161384298485,10.893649239278348,-152574.27002985831,1142.2004448178975,2.8847242961019343E-2,1.5494601081834931,-153641.95384181035,2281.1243314531234,11.535541077476807,2.8164817592025885E-2,1.1793541385472961,-153651.22795055914,2314.8436559985871]
["KBM","KBM-43H01-A (400 V)",6.12,5.12,4.82490774847009,3.9875270648513141,4750,18,5478,2.9,6.8,72.8,1.94,565,16,3505.2149373042757,5061.9311014268451,5384.6153846153848,4.73985942163449,57.989690721649488,1.6265653520963337,1.6382748515555556,4.1053112507000299E-2,-22.998700404938269,9,29.488947328000002,9,-2390.8313599999997,7.5,2402.8313599999997,9,0.34665763180402537,0.51396858088017428,8.3197831632966093,24.670491882248367,18.441762287270254,23.10301887981867,2.4749467547920703,151.61340490466978,1.0819322829054226E-2,5.5065685307322925,-152233.65979238754,3505.2149373042757,5.700088493422531E-3,1.4828482471209443,-153560.27805160204,5061.9311014268451,4.0551479473410481,1.3577758345464777E-2,6.743609662732716,-151518.8281040889,3101.4446091463888]
["KBM","KBM-43H02-A (400 V)",11.6,5.12,9.9780405138429078,4.3194980579406526,2450,34.5,2866,3.55,12,139,2.85,565,16,1857.4406026742151,2630.4569208447001,2820.1438848920861,9.8585736507381068,39.473684210526315,0.85978651846475773,0.86016596869565221,5.6703419316203839E-2,-23.229291259259259,9,29.675725920000001,9,-2409.8903999999998,7.5,2421.8903999999998,9,0.18318888025367067,0.27288023834482761,4.3965331260880962,13.098251440551724,9.7821024788854753,23.140548154174382,2.5068981036358635,153.57072086717474,3.6897123643143917E-2,13.014720551425221,-151472.30506920334,1857.4406026742151,2.0764225009738554E-2,3.7294116319948825,-153484.0337570408,2630.4569208447001,4.3635156746401194,2.6574128670536809E-2,8.3605719539738494,-152759.5545339582,2245.4369773276012]
["KBM","KBM-43H02-A (480 V)",11.6,5.12,6.8754935415698784,2.9764041305497306,3000,34.5,3439,3.55,12,139,2.85,679,16,1857.4406026742151,2682.7115802976487,2820.1438848920861,7.3751706042594938,39.473684210526315,0.86129209317925337,0.86016596869565221,5.6703419316203839E-2,-23.229291259259259,9,29.675725920000001,9,-2409.8903999999998,7.5,2421.8903999999998,9,0.18318888025367067,0.27288023834482761,4.3965331260880962,13.098251440551724,9.7821024788854753,23.140548154174382,2.5068981036358635,153.57072086717474,3.6897123643143917E-2,13.014720551425221,-151472.30506920334,1857.4406026742151,2.0231400278668727E-2,2.962030246405813,-153550.47555534623,2682.7115802976487,3.4656580405516459,2.6574128670536809E-2,8.3605719539738494,-152759.5545339582,2245.4369773276012]
["KBM","KBM-43H03-A (400 V)",21,4.78,18.636530433018713,4.2068917456024186,1240,64.5,1491,4.83,19,268,4.75,565,16,1016.1125416515356,1366.0453605652117,1462.686567164179,18.396284970313019,23.684210526315791,0.47691039611090352,0.46613493333333333,9.500567972903054E-2,-23.710744691358023,9,30.065703200000002,9,-2449.6840000000002,7.5,2461.6840000000002,9,9.4793386421271983E-2,0.14257347350793653,2.2750412741105275,6.8435267283809535,5.1011347800488958,23.219664617832066,2.5736097111119163,157.65742452515221,0.11278233636413708,32.916289147443393,-149892.69064923251,1016.1125416515356,7.5229627786043307E-2,9.4915754593880362,-153350.42095712695,1366.0453605652117,4.2334628461043602,7.676869230843833E-2,11.436927039030714,-153208.7089409664,1340.172027995189]
["KBM","KBM-43H03-A (480 V)",21,4.78,16.182532804310163,3.652941942282204,1490,64.5,1790,4.83,19,268,4.75,679,16,1016.1125416515356,1375.958854137958,1462.686567164179,16.551250575551283,23.684210526315791,0.47758137757837266,0.46613493333333333,9.500567972903054E-2,-23.710744691358023,9,30.065703200000002,9,-2449.6840000000002,7.5,2461.6840000000002,9,9.4793386421271983E-2,0.14257347350793653,2.2750412741105275,6.8435267283809535,5.1011347800488958,23.219664617832066,2.5736097111119163,157.65742452515221,0.11278233636413708,32.916289147443393,-149892.69064923251,1016.1125416515356,7.4692842395100545E-2,8.7115023800268521,-153399.84639633962,1375.958854137958,3.8855321561096443,7.676869230843833E-2,11.436927039030714,-153208.7089409664,1340.172027995189]
["KBM","KBM-43S01-A (240 V)",6.12,5.12,4.9618894022767375,4.1007350432039154,2550,18,3284,2.9,6.8,72.8,1.94,325,16,3284,3284,3284,4.6285352145399239,57.989690721649488,1.627637401861719,1.6382748515555556,4.1053112507000299E-2,-22.998700404938269,9,29.488947328000002,9,-2390.8313599999997,7.5,2402.8313599999997,9,0.34665763180402537,0.51396858088017428,8.3197831632966093,24.670491882248367,18.441762287270254,23.10301887981867,2.4749467547920703,151.61340490466978,1.0819322829054226E-2,5.5065685307322925,-152233.65979238754,3505.2149373042757,5.5705097572272657E-3,1.2194155305114529,-153593.8575883398,5142.656832276868,3.334737991638868,1.3577758345464777E-2,6.743609662732716,-151518.8281040889,3101.4446091463888]
["KBM","KBM-43S02-A (240 V)",11.6,5.12,10.136945606160719,4.3882881411951162,1300,34.5,1717,3.55,12,139,2.85,325,16,1717,1717,1717,9.6676427736753503,39.473684210526315,0.86055018746575718,0.86016596869565221,7.4154894859357168E-2,-23.229291259259259,9,29.675725920000001,9,-2409.8903999999998,7.5,2421.8903999999998,9,0.18318888025367067,0.27288023834482761,4.3965331260880962,13.098251440551724,9.7821024788854753,23.140548154174382,2.5068981036358635,153.57072086717474,3.6897123643143917E-2,13.014720551425221,-151472.30506920334,1857.4406026742151,2.0425249167109714E-2,3.2621718677296756,-153526.30312490804,2662.9292754976691,3.8168321126285392,2.6574128670536809E-2,8.3605719539738494,-152759.5545339582,2245.4369773276012]
["KBM","KBM-43S03-A (240 V)",21,4.78,18.813539541609121,4.2468486549907727,670,64.5,893,4.83,19,268,4.75,325,16,893,893,893,18.085807180084991,23.684210526315791,0.47759665480991426,0.46613493333333333,0.14258001620774499,-23.710744691358023,9,30.065703200000002,9,-2449.6840000000002,7.5,2461.6840000000002,9,9.4793386421271983E-2,0.14257347350793653,2.2750412741105275,6.8435267283809535,5.1011347800488958,23.219664617832066,2.5736097111119163,157.65742452515221,0.11278233636413708,32.916289147443393,-149892.69064923251,1016.1125416515356,7.4624569867563051E-2,8.6072203320760323,-153406.13270687757,1377.2623448214838,3.8390199435265577,7.676869230843833E-2,11.436927039030714,-153208.7089409664,1340.172027995189]
["KBM","KBM-57H01-A (400 V)",18.8,5.67,13.222102964557459,3.9468964073305846,1625,46.1,1975,3.39,13,203,6.56,565,24,1279.4377584448944,1806.623322877077,1931.0344827586207,12.598671460407754,17.149390243902442,0.53556312565164133,0.660243120867679,7.6580686859537492E-2,-24.1693924345679,9,30.437207872000002,9,-2487.5926400000003,7.5,2499.5926400000003,9,0.12601425712743822,0.19124442446170212,3.024342171058517,9.1797323741617021,6.8303445076300084,23.295979741050616,2.637161295075944,161.55054748354115,7.9900891930766382E-2,16.572289009537378,-151997.85447950911,1279.4377584448944,4.4402546088286456E-2,4.7611198014252611,-153526.47990873642,1806.623322877077,3.9944109725749914,5.054697945851172E-2,8.1413977452774411,-153261.88907006473,1662.6118110830071]
["KBM","KBM-57H01-A (480 V)",18.8,5.67,10.713844949600761,3.1981626715226152,2050,46.1,2370,3.39,13,203,6.56,679,24,1279.4377584448944,1816.8301527896365,1931.0344827586207,11.633575455757295,17.149390243902442,0.53588817900456343,0.660243120867679,7.6580686859537492E-2,-24.1693924345679,9,30.437207872000002,9,-2487.5926400000003,7.5,2499.5926400000003,9,0.12601425712743822,0.19124442446170212,3.024342171058517,9.1797323741617021,6.8303445076300084,23.295979741050619,2.637161295075944,161.55054748354115,7.9900891930766382E-2,16.572289009537378,-151997.85447950911,1279.4377584448944,4.4045717923545849E-2,4.4872533640461318,-153541.84559954656,1816.8301527896365,3.7646467263235648,5.054697945851172E-2,8.1413977452774411,-153261.88907006473,1662.6118110830071]
["KBM","KBM-57H02-A (400 V)",33.5,5.22,26.795904964199107,4.1479729046747842,825,115,1023,4.4000000000000004,22,390,11.8,565,24,591.24074264297644,935.5831883411937,1005.1282051282051,25.897286535106705,9.5338983050847457,0.30387739562985261,0.27402368834782609,0.13443191847469002,-25.497190320987656,9,31.512724160000001,9,-2597.3391999999999,7.5,2609.3391999999999,9,6.5737638599423262E-2,0.10229876872835821,1.5777033263861584,4.9103408989611941,3.6356201977072149,23.522035958765496,2.8211448862204263,172.82124599291055,0.33616593689141883,53.260034962049318,-149001.55535148139,591.24074264297644,0.16203764956574188,12.37532386519517,-153412.27639584406,935.5831883411937,4.1636926368760099,0.1596767571599077,10.805787391460493,-153472.07849909691,947.12592008041611]
["KBM","KBM-57H02-A (480 V)",33.5,5.22,24.931661036070302,3.8593902532616569,1015,115,1228,4.4000000000000004,22,390,11.8,679,24,591.24074264297644,936.33113238928058,1005.1282051282051,25.595761059318733,9.5338983050847457,0.30394125402031558,0.27402368834782609,0.13443191847469002,-25.497190320987656,9,31.512724160000001,9,-2597.3391999999999,7.5,2609.3391999999999,9,6.5737638599423262E-2,0.10229876872835821,1.5777033263861584,4.9103408989611941,3.6356201977072149,23.522035958765496,2.8211448862204263,172.82124599291055,0.33616593689141883,53.260034962049318,-149001.55535148139,591.24074264297644,0.1618789006580636,12.276081173041625,-153416.29755265103,936.33113238928058,4.1303023134319812,0.1596767571599077,10.805787391460493,-153472.07849909691,947.12592008041611]
["KBM","KBM-57H03-A (400 V)",59.9,5.47,51.264644827494706,4.635139676988671,475,218,597,5.92,35,669,22.1,565,24,313.42017937668498,532.89566684649765,585.94917787742895,50.212119256613555,5.0904977375565608,0.17354969306838203,0.1542514289908257,0.22567556296293184,-28.107174716049386,9,33.626811520000004,9,-2813.0623999999998,7.5,2825.0623999999998,9,3.9288526350594578E-2,6.3974213624930443E-2,0.94292463241426983,3.0707622539966613,2.2535591959547494,23.987873036513005,3.1827920214853416,194.97548161247241,1.0225387978968383,136.56061042339675,-143247.09575722038,313.42017937668498,0.47909136956578102,31.978967846445947,-153092.76256838508,532.89566684649765,4.6618252571789167,0.45492909168097662,15.458858513952588,-153530.51187963519,564.19025968899325]
["KBM","KBM-57H03-A (480 V)",59.9,5.47,49.392913373346836,4.465905368295374,580,218,717,5.92,35,669,22.1,679,24,313.42017937668498,532.7223754069621,585.94917787742895,50.249379058004486,5.0904977375565608,0.17354554951600393,0.1542514289908257,0.22567556296293184,-28.107174716049386,9,33.626811520000004,9,-2813.0623999999998,7.5,2825.0623999999998,9,3.9288526350594578E-2,6.3974213624930443E-2,0.94292463241426983,3.0707622539966613,2.2535591959547494,23.987873036513005,3.1827920214853416,194.97548161247241,1.0225387978968383,136.56061042339675,-143247.09575722038,313.42017937668498,0.47925580945897855,32.062249134471863,-153089.78340183743,532.7223754069621,4.6739658244990956,0.45492909168097662,15.458858513952588,-153530.51187963519,564.19025968899325]
["KBM","KBM-57S01-A (240 V)",18.8,5.67,16.00592325412811,4.7778875385457047,880,46.1,1183,3.39,13,203,6.56,325,24,1183,1183,1183,15.043871829129039,17.149390243902442,0.5353997904984148,0.660243120867679,0.10762802575952347,-24.1693924345679,9,30.437207872000002,9,-2487.5926400000003,7.5,2499.5926400000003,9,0.12601425712743822,0.19124442446170212,3.024342171058517,9.1797323741617021,6.8303445076300084,23.295979741050619,2.637161295075944,161.55054748354115,7.9900891930766382E-2,16.572289009537378,-151997.85447950911,1279.4377584448944,4.4521396058562819E-2,4.8489046602847843,-153521.362005845,1803.2915969892933,4.0680593616261254,5.054697945851172E-2,8.1413977452774411,-153261.88907006473,1662.6118110830071]
["KBM","KBM-57S02-A (240 V)",33.5,5.22,29.506253494564866,4.5675315007066359,445,115,612,4.4000000000000004,22,390,11.8,325,24,591.24074264297644,612,612,28.007476716120671,9.5338983050847457,0.3040491829942133,0.27402368834782609,0.20804567724430761,-25.497190320987656,9,31.512724160000001,9,-2597.3391999999999,7.5,2609.3391999999999,9,6.5737638599423262E-2,0.10229876872835821,1.5777033263861584,4.9103408989611941,3.6356201977072149,23.522035958765496,2.8211448862204263,172.82124599291055,0.33616593689141883,53.260034962049318,-149001.55535148139,591.24074264297644,0.16140096261223713,11.972330126947202,-153428.40386477875,938.6056364574207,4.028104907703983,0.1596767571599077,10.805787391460493,-153472.07849909691,947.12592008041611]
["KBM","KBM-57S03-A (240 V)",59.9,5.47,53.858032742297389,4.8696232135892759,250,218,357,5.92,35,669,22.1,325,24,313.42017937668498,357,357,51.272070756000673,5.0904977375565608,0.17393808939179767,0.1542514289908257,0.35664973241881309,-28.107174716049386,9,33.626811520000004,9,-2813.0623999999998,7.5,2825.0623999999998,9,3.9288526350594578E-2,6.3974213624930443E-2,0.94292463241426983,3.0707622539966613,2.2535591959547494,23.987873036513005,3.1827920214853416,194.97548161247241,1.0225387978968383,136.56061042339675,-143247.09575722038,313.42017937668498,0.4752134762472352,29.947938027772931,-153163.01857394,537.08168707618631,4.3657460918901076,0.45492909168097662,15.458858513952588,-153530.51187963519,564.19025968899325]
["KBM","KBM-79H01-A (400 V)",43.4,4.95,35.571129781038607,4.0102739324733498,600,152,744,6.26,23,534,32.5,565,32,409.12559339504384,673.0517250586347,734.08239700374531,34.617942323113105,3.4615384615384617,0.24448644005049877,0.23527252631578952,0.18383693095975384,-30.742498765432103,9,35.761424000000005,9,-3030.88,7.5,3042.88,9,5.0088982867112643E-2,8.4974581797235049E-2,1.2021355888107035,4.0787799262672824,2.9696409145807849,24.48574088711127,3.5479502939858385,217.34480689824358,0.61991499195707211,100.37724576294784,-144830.5969969462,409.12559339504384,0.30336834734728069,23.4127329527272,-153183.4243989994,673.0517250586347,4.0436717499856032,0.29497849944478388,17.194128009727798,-153404.81025998498,692.59181933030868]
["KBM","KBM-79H01-A (480 V)",43.4,4.95,33.814974895278034,3.8122857830076704,730,152,894,6.26,23,534,32.5,679,32,409.12559339504384,672.96696093434559,734.08239700374531,34.563828472323081,3.4615384615384617,0.24449676457658304,0.23527252631578952,0.18383693095975384,-30.742498765432103,9,35.761424000000005,9,-3030.88,7.5,3042.88,9,5.0088982867112643E-2,8.4974581797235049E-2,1.2021355888107035,4.0787799262672824,2.9696409145807849,24.48574088711127,3.5479502939858385,217.34480689824358,0.61991499195707211,100.37724576294784,-144830.5969969462,409.12559339504384,0.30340849346855064,23.438523505370419,-153182.36504920834,672.96696093434559,4.0481261009300429,0.29497849944478388,17.194128009727798,-153404.81025998498,692.59181933030868]
["KBM","KBM-79H02-A (400 V)",79.31,5.39,67.254331666546648,4.5137135346675601,350,319,443,6.4,32,901,59.7,565,32,223.17093581699675,397.09663857401756,435.07214206437294,65.632098940064125,1.8844221105527637,0.14197570434850856,0.12960582018808778,0.30278259956489506,-37.634884740740738,9,41.344256639999998,9,-3600.5567999999998,7.5,3612.5567999999998,9,3.1578145613674273E-2,5.8537580194174745E-2,0.75787549472818261,2.8098038493203878,2.0110383795814371,25.906712990171997,4.5029796220640597,275.8491961071835,1.8251555411105096,216.52940908268576,-139225.42915637666,223.17093581699675,0.85626161383676169,45.354868163047946,-153030.51221602107,397.09663857401756,4.5410733461077477,0.82052065172984001,20.085643552734961,-153539.75986081333,420.51278592786855]
["KBM","KBM-79H02-A (480 V)",79.31,5.39,64.846386115581552,4.3521064507101714,430,319,532,6.4,32,901,59.7,679,32,223.17093581699675,396.78800261876535,435.07214206437294,65.963515200354792,1.8844221105527637,0.14194329080550017,0.12960582018808778,0.30278259956489506,-37.634884740740738,9,41.344256639999998,9,-3600.5567999999998,7.5,3612.5567999999998,9,3.1578145613674273E-2,5.8537580194174745E-2,0.75787549472818261,2.8098038493203878,2.0110383795814371,25.906712990171997,4.5029796220640597,275.8491961071835,1.8251555411105096,216.52940908268576,-139225.42915637666,223.17093581699675,0.85686097909777736,45.659555012536835,-153021.97228509732,396.78800261876535,4.5715795604825651,0.82052065172984001,20.085643552734961,-153539.75986081333,420.51278592786855]
["KBM","KBM-79H03-A (400 V)",143,6.76,122.74824985962429,5.7358995261506687,240,637,307,5.75,34,1300,114,565,32,140.14450962597201,273.42334490160994,301.53846153846155,119.92791140211177,0.98684210526315785,8.8968189930548405E-2,8.2400936891679752E-2,0.43267325895702036,-51.394317037037034,9,52.489396800000002,9,-4737.8159999999998,7.5,4749.8159999999998,9,2.4731305304197069E-2,5.1694102909090912E-2,0.59355132730072968,2.4813169396363639,1.7342571948576453,29.169090394748729,6.4095271409849222,392.64288485885407,3.8970718944828411,389.87188259144398,-131178.78034979338,140.14450962597201,1.771078475922266,74.725092824458883,-152837.98823999646,273.42334490160994,5.771578924069714,1.6973205432124621,22.453566272267768,-153589.41972805574,294.27276088297384]
["KBM","KBM-79H03-A (480 V)",143,6.76,119.2070523758296,5.5704230082163368,300,637,369,5.75,34,1300,114,679,32,140.14450962597201,273.02566928828185,301.53846153846155,121.3463818352328,0.98684210526315785,8.8897301793253211E-2,8.2400936891679752E-2,0.43267325895702036,-51.394317037037034,9,52.489396800000002,9,-4737.8159999999998,7.5,4749.8159999999998,9,2.4731305304197069E-2,5.1694102909090912E-2,0.59355132730072968,2.4813169396363639,1.7342571948576453,29.169090394748729,6.4095271409849222,392.64288485885407,3.8970718944828411,389.87188259144398,-131178.78034979338,140.14450962597201,1.7730546928429931,75.630289570175592,-152817.85492596618,273.02566928828185,5.8414940524722709,1.6973205432124621,22.453566272267768,-153589.41972805574,294.27276088297384]
["KBM","KBM-79S01-A (240 V)",43.4,4.95,38.505228167394037,4.3410629275528798,310,152,445,6.26,23,534,32.5,325,32,409.12559339504384,445,445,36.373633982226927,3.4615384615384617,0.24483185949490147,0.23527252631578952,0.28612124600790173,-30.742498765432103,9,35.761424000000005,9,-3030.88,7.5,3042.88,9,5.0088982867112643E-2,8.4974581797235049E-2,1.2021355888107035,4.0787799262672824,2.9696409145807849,24.48574088711127,3.5479502939858385,217.34480689824358,0.61991499195707211,100.37724576294784,-144830.5969969462,409.12559339504384,0.30135230222879755,22.078882354739797,-153236.62248906351,677.39681103880525,3.8132990723202731,0.29497849944478388,17.194128009727798,-153404.81025998498,692.59181933030868]
["KBM","KBM-79S02-A (240 V)",79.31,5.39,71.354466152866408,4.7888903458299605,180,319,265,6.4,32,901,59.7,325,32,223.17093581699675,265,265,67.597686280608883,1.8844221105527637,0.14236788847855592,0.12960582018808778,0.48046775273025005,-37.634884740740738,9,41.344256639999998,9,-3600.5567999999998,7.5,3612.5567999999998,9,3.1578145613674273E-2,5.8537580194174745E-2,0.75787549472818261,2.8098038493203878,2.0110383795814371,25.906712990171997,4.5029796220640597,275.8491961071835,1.8251555411105096,216.52940908268576,-139225.42915637666,223.17093581699675,0.85088529294532522,42.524313532912494,-153107.11560300941,399.93880271540075,4.2576692330277242,0.82052065172984001,20.085643552734961,-153539.75986081333,420.51278592786855]
["KBM","KBM-79S03-A (240 V)",143,6.76,128.72451797272495,6.0151643912488302,125,637,184,5.75,34,1300,114,325,32,140.14450962597201,184,184,121.98649045585114,0.98684210526315785,8.93872456184958E-2,8.2400936891679752E-2,0.69197801344302323,-51.394317037037034,9,52.489396800000002,9,-4737.8159999999998,7.5,4749.8159999999998,9,2.4731305304197069E-2,5.1694102909090912E-2,0.59355132730072968,2.4813169396363639,1.7342571948576453,29.169090394748729,6.4095271409849222,392.64288485885407,3.8970718944828411,389.87188259144398,-131178.78034979338,140.14450962597201,1.7604431513559573,69.651915293527239,-152946.33886034664,275.63382249434324,5.3797394039185242,1.6973205432124621,22.453566272267768,-153589.41972805574,294.27276088297384]
["KBM","KBM-118H01-A (400 V)",325,43.7,109.48238123518914,14.443585914932603,785,994,872,0.27600000000000002,2.5,648,267,565,38,424.00805538635876,587.9353912273682,604.93827160493834,163.58543247786005,0.42134831460674155,5.4332737250197868E-2,9.0708237573589687E-2,0.2117268674201421,-90.16398814814815,9,83.892830400000008,9,-7942.2479999999996,7.5,7954.2479999999996,9,9.7076729086812821E-2,0.25257476167141502,2.3298414980835078,12.123588560227921,7.6210455852952599,40.253492306625496,11.78156711142492,721.7300741591414,0.75139721169624418,41.402748804354658,-152643.41695687795,424.00805538635876,0.4313529871939909,7.6944111806974762,-153628.75148878217,587.9353912273682,24.838803712825154,0.42098179170626515,2.3608004249344492,-153660.68175425433,601.35945912268107]
["KBM","KBM-118H02-A (400 V)",445,46.5,239.54167706034417,24.797275058006644,590,1451,685,0.29199999999999998,2.7,585,396,565,38,399.83122280328899,645.45776489990044,670.08547008547009,220.22937304286069,0.28409090909090912,4.9914558771312879E-2,8.4667224136610764E-2,0.19134436900623855,-122.85214222222223,9,110.37023520000001,9,-10644.023999999999,7.5,10656.023999999999,9,9.503042435712937E-2,0.26744497253433208,2.2807301845711048,12.83735868164794,7.8307756307809937,50.705635802064052,16.310934145325312,999.1957435691877,0.83981762885279965,44.860044415419679,-152193.89730078646,399.83122280328899,0.356828607882751,7.6851581969995841,-153620.85465957125,645.45776489990044,25.97487503689597,0.3435522807350887,2.3168831204106852,-153660.07864168775,665.41782825793541]
["KBM","KBM-118H02-A (480 V)",445,46.5,139.13728616498514,14.403445772772789,710,1451,822,0.29199999999999998,2.7,585,396,679,38,399.83122280328899,651.75229819667891,670.08547008547009,164.22996243007879,0.28409090909090912,5.012451794260607E-2,8.4667224136610764E-2,0.19134436900623855,-122.85214222222223,9,110.37023520000001,9,-10644.023999999999,7.5,10656.023999999999,9,9.503042435712937E-2,0.26744497253433208,2.2807301845711048,12.83735868164794,7.8307756307809937,50.705635802064052,16.310934145325312,999.1957435691877,0.83981762885279965,44.860044415419679,-152193.89730078646,399.83122280328899,0.35202238757371207,6.2947411281110615,-153635.05430208932,651.75229819667891,21.275438969640152,0.3435522807350887,2.3168831204106852,-153660.07864168775,665.41782825793541]
["KBM","KBM-118H03-A (400 V)",560,44,374.83733148884318,29.284166522565872,435,1932,516,0.373,4.3,775,542,565,38,265.09524922361442,474.83301675429266,505.80645161290329,357.8819575185571,0.20756457564575645,4.9326510181898722E-2,8.2737079467321006E-2,0.25402822242940126,-159.84803753086419,9,140.33691039999999,9,-13701.848,7.5,13713.848,9,8.8906911579687678E-2,0.26165601381540271,2.1337658779125044,12.55948866313933,7.7386570813837681,63.089542877353473,21.43719450927459,1313.2266562348211,1.8656705274531626,76.005134736652323,-151259.51279653001,265.09524922361442,0.64962323848073444,14.958225946889472,-153570.86846057099,474.83301675429266,29.875069712136579,0.60391271238222166,3.8746882355159551,-153657.75100565143,501.21971982424805]
["KBM","KBM-118H03-A (480 V)",560,44,302.72162633703306,23.650127057580708,535,1932,619,0.373,4.3,775,542,679,38,265.09524922361442,477.52563124887513,505.80645161290329,330.36071441104252,0.20756457564575645,4.9436543055061087E-2,8.2737079467321006E-2,0.25402822242940126,-159.84803753086419,9,140.33691039999999,9,-13701.848,7.5,13713.848,9,8.8906911579687678E-2,0.26165601381540271,2.1337658779125044,12.55948866313933,7.7386570813837681,63.089542877353473,21.43719450927459,1313.2266562348211,1.8656705274531626,76.005134736652323,-151259.51279653001,265.09524922361442,0.6440299123351505,14.078594398635271,-153581.49976264671,477.52563124887513,28.118240130982034,0.60391271238222166,3.8746882355159551,-153657.75100565143,501.21971982424805]
["KBM","KBM-118H04-A (400 V)",672,42.8,502.32108656444967,31.395067910278105,340,2400,413,0.45500000000000002,4.5,970,648,565,38,229.22256954278296,379.61233386752502,404.12371134020617,482.55232841948526,0.1736111111111111,4.7078098053898093E-2,7.7795029629629628E-2,0.3179559308790017,-186.70807111111111,9,162.09353760000002,9,-15921.912,7.5,15933.912,9,8.2572662615912312E-2,0.24774012411816573,1.9817439027818955,11.891525957671956,7.3620858106512941,72.285018923202216,25.15899997899119,1541.2217024167196,2.3457249252312979,116.85020965642296,-150036.09812499999,229.22256954278296,1.0013785537261357,24.24482715828627,-153507.81665322161,379.61233386752502,31.715775430593695,0.94415876076730343,5.627877470450712,-153655.58438600742,400.44528850751163]
["KBM","KBM-118H04-A (480 V)",672,42.8,450.74953525668928,28.17184595354308,420,2400,495,0.45500000000000002,4.5,970,648,679,38,{"$f":"IF(AQ763<I763,IF(AQ763<0,0,AQ763),I763)","v":229.22256954278296},{"$f":"IF(AU763<I763,IF(AU763<0,0,AU763),I763)","v":380.07080505983259},{"$f":"IF(UAC_V*0.98/L763*1000<I763,IF(UAC_V*0.98/L763*1000<0,0,UAC_V*0.98/L763*1000),I763)","v":404.12371134020617},{"$f":"C763+(E763-C763)/G763*Q763","v":471.78370891701854},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M763,(inertia/gear^2+gear_inertia)/M763),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M763,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M763))","v":0.1736111111111111},{"$f":"IF((C763+(E763-C763)/G763*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X763^2*time1+Y763^2*time2+Z763^2*time3+AA763^2*time4)/time)/(C763+(E763-C763)/G763*mspeed),SQRT((((X763-Y763)*2/PI()+Y763)^2*time1+Y763^2*time2+((Z763-Y763)*2/PI()+Y763)^2*time3+AA763^2*time4)/time)/(C763+(E763-C763)/G763*mspeed)),IF(AccType=1,SQRT((X763^2*time1+Y763^2*time2+Z763^2*time3+AA763^2*time4+AB763^2*time5+AC763^2*time6+AD763^2*time7+AE763^2*time8)/time)/(C763+(E763-C763)/G763*mspeed),SQRT((((X763-Y763)*2/PI()+Y763)^2*time1+Y763^2*time2+((Z763-Y763)*2/PI()+Y763)^2*time3+AA763^2*time4+((AB763-AC763)*2/PI()+AC763)^2*time5+AC763^2*time6+((AD763-AC763)*2/PI()+AC763)^2*time7+AE763^2*time8)/time)/(C763+(E763-C763)/G763*mspeed))))","v":4.7121962882586389E-2},{"$f":"IF(move1,MAX(ABS(X763),ABS(Z763))/H763,MAX(ABS(X763),ABS(Z763),ABS(AB763),ABS(AD763))/H763)","v":7.7795029629629628E-2},{"$f":"IF(AZ763>0,speed/(MIN(AZ763,I763)),\"NA\")","v":0.3179559308790017},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M763+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M763+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-186.70807111111111},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M763+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M763+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":162.09353760000002},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M763+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M763+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-15921.912},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M763+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M763+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":15933.912},9,{"$f":"AH763/Irms","v":8.2572662615912312E-2},{"$f":"AI763/Ipeak","v":0.24774012411816573},{"$f":"IF(move1,IF(AccType=1,SQRT((X763^2*time1+Y763^2*time2+Z763^2*time3+AA763^2*time4)/time)/(C763/D763),SQRT((((X763-Y763)*2/PI()+Y763)^2*time1+Y763^2*time2+((Z763-AA763)*2/PI()+AA763)^2*time3+AA763^2*time4)/time)/(C763/D763)),IF(AccType=1,SQRT((X763^2*time1+Y763^2*time2+Z763^2*time3+AA763^2*time4+AB763^2*time5+AC763^2*time6+AD763^2*time7+AE763^2*time8)/time)/(C763/D763),SQRT((((X763-Y763)*2/PI()+Y763)^2*time1+Y763^2*time2+((Z763-AA763)*2/PI()+AA763)^2*time3+AA763^2*time4+((AB763-AC763)*2/PI()+AC763)^2*time5+AC763^2*time6+((AD763-AE763)*2/PI()+AE763)^2*time7+AE763^2*time8)/time)/(C763/D763)))","v":1.9817439027818955},{"$f":"IF(move1,MAX(ABS(X763),ABS(Z763))/(C763/D763),MAX(ABS(X763),ABS(Z763),ABS(AB763),ABS(AD763))/(C763/D763))","v":11.891525957671956},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X763),ABS(Z763))/(C763/D763),MAX(ABS((X763-Y763)*2/PI()+Y763),ABS((Z763-Y763)*2/PI()+Y763))/(C763/D763)),IF(AccType=1,MAX(ABS(X763),ABS(Z763),ABS(AB763),ABS(AD763))/(C763/D763),MAX(ABS((X763-Y763)*2/PI()+Y763),ABS((Z763-Y763)*2/PI()+Y763),ABS((AB763-AC763)*2/PI()+AC763),ABS((AD763-AC763)*2/PI()+AC763))/(C763/D763)))","v":7.3620858106512941},{"$f":"IF((C763+(E763-C763)/G763*mspeed)<0,\"NA\",U763*(C763+(E763-C763)/G763*mspeed)*mspeed/9.55)","v":72.285018923202216},{"$f":"IF(move1,IF(speed1>speed2,AM763/2*time1/time,AM763/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z763*-speed/30*PI(),((Z763-AA763)*2/PI()+AA763)*-speed/30*PI()),IF(AccType=1,X763*-speed/30*PI(),((X763-Y763)*2/PI()+Y763)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z763*-speed/30*PI(),((Z763-AA763)*2/PI()+AA763)*-speed/30*PI()),IF(AccType=1,X763*-speed/30*PI(),((X763-Y763)*2/PI()+Y763)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD763*-speed/30*PI(),((AD763-AE763)*2/PI()+AE763)*-speed/30*PI()),IF(AccType=1,AB763*-speed/30*PI(),((AB763-AC763)*2/PI()+AC763)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD763*-speed/30*PI(),((AD763-AE763)*2/PI()+AE763)*-speed/30*PI()),IF(AccType=1,AB763*-speed/30*PI(),((AB763-AC763)*2/PI()+AC763)*-speed/30*PI()),0)/2*time7/time)))","v":25.15899997899119},{"$f":"IF(move1,MAX(IF(AccType=1,Z763*-speed/30*PI(),((Z763-AA763)*2/PI()+AA763)*-speed/30*PI()),IF(AccType=1,X763*-speed/30*PI(),((X763-Y763)*2/PI()+Y763)*-speed/30*PI()),0),MAX(IF(AccType=1,Z763*-speed/30*PI(),((Z763-AA763)*2/PI()+AA763)*-speed/30*PI()),IF(AccType=1,X763*-speed/30*PI(),((X763-Y763)*2/PI()+Y763)*-speed/30*PI()),IF(AccType=1,AD763*-speed/30*PI(),((AD763-AE763)*2/PI()+AE763)*-speed/30*PI()),IF(AccType=1,AB763*-speed/30*PI(),((AB763-AC763)*2/PI()+AC763)*-speed/30*PI()),0))","v":1541.2217024167196},{"$f":"(L763^2)/1000000+((K763/1000)^2*(D763/C763*H763)^2*PI()*PI()*(O763/2)^2)/1200","v":2.3457249252312979},{"$f":"SQRT(3)*L763*J763*D763/C763*H763/1000","v":116.85020965642296},{"$f":"0.75*J763^2*(D763/C763*H763)^2-(UAC_V*0.98)^2","v":-150036.09812499999},{"$f":"-AO763/2/AN763+SQRT((AO763/2/AN763)^2-AP763/AN763)","v":229.22256954278296},{"$f":"(L763^2)/1000000+((K763/1000)^2*AV763^2*PI()*PI()*(O763/2)^2)/1200","v":0.99976998151047247},{"$f":"SQRT(3)*L763*J763*AV763/1000","v":23.92022958061802},{"$f":"0.75*J763^2*AV763^2-(UAC_V*0.98)^2","v":-153511.97072399047},{"$f":"-AS763/2/AR763+SQRT((AS763/2/AR763)^2-AT763/AR763)","v":380.07080505983259},{"$f":"D763+(F763-D763)*((0.85*UAC_V-D763*J763)/L763*1000)/G763","v":31.291154384156478},{"$f":"(L763^2)/1000000+((K763/1000)^2*AJ763^2*PI()*PI()*(O763/2)^2)/1200","v":0.94415876076730343},{"$f":"SQRT(3)*L763*J763*AJ763/1000","v":5.627877470450712},{"$f":"0.75*J763^2*AJ763^2-(UAC_V*0.98)^2","v":-153655.58438600742},{"$f":"IF(((AX763/2/AW763)^2-AY763/AW763)>0,-AX763/2/AW763+SQRT((AX763/2/AW763)^2-AY763/AW763),-9999)","v":400.44528850751163}]
["KBM","KBM-118S01-A (240 V)",325,43.7,252.45952847951898,33.306006395714903,400,994,523,0.27600000000000002,2.5,648,267,325,38,424.00805538635876,523,523,230.15333348697106,0.42134831460674155,5.3982749522242184E-2,9.0708237573589687E-2,0.24344924373521273,-90.16398814814815,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},83.892830400000008,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},-7942.2479999999996,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},7954.2479999999996,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},9.7076729086812821E-2,0.25257476167141502,2.3298414980835078,12.123588560227921,7.6210455852952599,40.253492306625496,11.78156711142492,721.7300741591414,0.75139721169624418,41.402748804354658,-152643.41695687795,424.00805538635876,0.43722271502306459,9.4634542956203305,-153610.68009401835,582.00988198255095,30.549560996153815,0.42098179170626515,2.3608004249344492,-153660.68175425433,601.35945912268107]
["KBM","KBM-118S02-A (240 V)",445,46.5,356.90495988357532,36.946683217761418,320,1451,411,0.29199999999999998,2.7,585,396,325,38,399.83122280328899,411,411,331.85293285046703,0.28409090909090912,4.9730524590608692E-2,8.4667224136610764E-2,0.30979064348787411,-122.85214222222223,9,110.37023520000001,9,-10644.023999999999,7.5,10656.023999999999,9,9.503042435712937E-2,0.26744497253433208,2.2807301845711048,12.83735868164794,7.8307756307809937,50.705635802064052,16.310934145325312,999.1957435691877,0.83981762885279965,44.860044415419679,-152193.89730078646,399.83122280328899,0.36150040949692719,8.8292646921229725,-153607.05214770723,639.757679432945,29.841812122372421,0.3435522807350887,2.3168831204106852,-153660.07864168775,665.41782825793541]
["KBM","KBM-118S03-A (240 V)",560,44,467.30600312088416,36.508281493819069,235,1932,309,0.373,4.3,775,542,325,38,265.09524922361442,309,309,438.11725516746043,0.20756457564575645,4.9264533683861501E-2,8.2737079467321006E-2,0.41205163260037625,-159.84803753086419,9,140.33691039999999,9,-13701.848,7.5,13713.848,9,8.8906911579687678E-2,0.26165601381540271,2.1337658779125044,12.55948866313933,7.7386570813837681,63.089542877353473,21.43719450927459,1313.2266562348211,1.8656705274531626,76.005134736652323,-151259.51279653001,265.09524922361442,0.65233012942540403,15.365852863225449,-153565.72344049354,473.55703039923333,30.689195838143718,0.60391271238222166,3.8746882355159551,-153657.75100565143,501.21971982424805]
["KBM","KBM-118S04-A (240 V)",672,42.8,577.08722068131567,36.067951292582229,185,2400,247,0.45500000000000002,4.5,970,648,325,38,229.22256954278296,247,247,545.27861355829714,0.1736111111111111,4.7100211377095823E-2,7.7795029629629628E-2,0.51548159705877028,-186.70807111111111,9,162.09353760000002,9,-15921.912,7.5,15933.912,9,8.2572662615912312E-2,0.24774012411816573,1.9817439027818955,11.891525957671956,7.3620858106512941,72.285018923202216,25.15899997899119,1541.2217024167196,2.3457249252312979,116.85020965642296,-150036.09812499999,229.22256954278296,0.99784570121316019,23.526041914563411,-153516.94009773468,380.62379286090191,30.775499336897255,0.94415876076730343,5.627877470450712,-153655.58438600742,400.44528850751163]
["KBM","KBM-60H01-A (400 V)",54,13.7,34.759439571269944,8.6038216760569171,1250,127,1639,0.91600000000000004,7.8,245,16.3,565,38,761.29308542055537,1435.4252920298613,1600,31.905290342217572,6.9018404907975457,0.19030036458629579,0.25540436661417326,8.486088559590306E-2,-26.637474765432103,9,32.436354560000005,9,-2691.5872000000004,7.5,2703.5872000000004,9,0.10794281551191688,0.17144215180246916,2.5906275722860053,8.2292232865185202,6.0686044418527754,23.722116829940735,2.979146061821603,182.50028097233078,0.24755724953138974,12.524278422296174,-153010.69908371847,761.29308542055537,7.232290207237474E-2,3.2072310465352643,-153621.15813833461,1435.4252920298613,8.2510280192071122,6.6677617714403142E-2,2.3589080693635047,-153640.82445947643,1500.3844654628876]
["KBM","KBM-60H01-A (480 V)",54,13.7,24.858012674165401,6.1529734341993567,1600,127,1895,0.91600000000000004,7.8,245,16.3,679,38,761.29308542055537,1462.0374544251308,1600,27.370826895779597,6.9018404907975457,0.19052261107564716,0.25540436661417326,8.486088559590306E-2,-26.637474765432103,9,32.436354560000005,9,-2691.5872000000004,7.5,2703.5872000000004,9,0.10794281551191688,0.17144215180246916,2.5906275722860053,8.2292232865185202,6.0686044418527754,23.722116829940735,2.979146061821603,182.50028097233078,0.24755724953138974,12.524278422296174,-153010.69908371847,761.29308542055537,6.9905415095751225E-2,2.8747648585239767,-153629.57987092127,1462.0374544251308,7.3957145750186903,6.6677617714403142E-2,2.3589080693635047,-153640.82445947643,1500.3844654628876]
["KBM","KBM-60H02-A (400 V)",108,16.399999999999999,88.643815200699777,13.055053785080968,725,255,974,0.92100000000000004,11,411,31.7,565,38,446.96442055897234,803.66743274534781,953.77128953771285,86.543537454623262,3.5488958990536279,9.7972932278865221E-2,0.13959695309803924,0.13675701258912987,-30.539781530864197,9,35.597223040000003,9,-3014.1247999999996,7.5,3026.1247999999996,9,6.6580993494291307E-2,0.11261467165432099,1.5979438438629914,5.4055042394074073,3.9378705228545119,24.446499698886274,3.5198611961011839,215.62408956856882,0.70760195024155381,25.38764123306548,-152710.10390747918,446.96442055897234,0.2273496500025925,8.361216514288067,-153560.53456112798,803.66743274534781,12.752854073449626,0.17449200997970557,2.5818054419180747,-153654.13485691548,931.02322186611298]
["KBM","KBM-60H02-A (480 V)",108,16.399999999999999,84.001439455620698,12.371346017028085,885,255,1169,0.92100000000000004,11,411,31.7,679,38,446.96442055897234,802.82589553852665,953.77128953771285,86.229756089630655,3.5488958990536279,9.7981408972334288E-2,0.13959695309803924,0.13675701258912987,-30.539781530864197,9,35.597223040000003,9,-3014.1247999999996,7.5,3026.1247999999996,9,6.6580993494291307E-2,0.11261467165432099,1.5979438438629914,5.4055042394074073,3.9378705228545119,24.446499698886274,3.5198611961011839,215.62408956856882,0.70760195024155381,25.38764123306548,-152710.10390747918,446.96442055897234,0.22779646739523066,8.3931257039457385,-153559.74333700037,802.82589553852665,12.801523216104993,0.17449200997970557,2.5818054419180747,-153654.13485691548,931.02322186611298]
["KBM","KBM-60H03-A (400 V)",154,18.7,119.77083853017209,14.090686885902599,590,393,778,0.86699999999999999,11,515,47.5,565,38,358.38962772909792,662.73310691202528,761.1650485436893,115.55118893577553,2.3684210526315788,7.1169924499007428E-2,9.8830005089058523E-2,0.16967574914346495,-34.543446913580247,9,38.840192000000002,9,-3345.04,7.5,3357.04,9,5.4989754935648782E-2,9.8256438095238097E-2,1.3197541184555708,4.7163090285714286,3.3996182575254545,25.249187335413296,4.0746208793230929,249.60825682964426,1.0833844362918668,36.906289996527782,-152380.1143922068,358.38962772909792,0.33352633394232695,10.663407620725721,-153556.81905732327,662.73310691202528,13.788247075183261,0.26937713415846465,2.629160547906225,-153657.48431974111,750.39571132737876]
["KBM","KBM-60H03-A (480 V)",154,18.7,110.74531456811052,13.028860537424766,720,393,930,0.86699999999999999,11,515,47.5,679,38,358.38962772909792,663.16787201296358,761.1650485436893,114.15955876047738,2.3684210526315788,7.1191234631064054E-2,9.8830005089058523E-2,0.16967574914346495,-34.543446913580247,9,38.840192000000002,9,-3345.04,7.5,3357.04,9,5.4989754935648782E-2,9.8256438095238097E-2,1.3197541184555708,4.7163090285714286,3.3996182575254545,25.249187335413289,4.0746208793230929,249.60825682964426,1.0833844362918668,36.906289996527782,-152380.1143922068,358.38962772909792,0.33312710985346489,10.632197921680245,-153557.44553431447,663.16787201296358,13.747891584997859,0.26937713415846465,2.629160547906225,-153657.48431974111,750.39571132737876]
["KBM","KBM-60S01-A (240 V)",54,13.7,44.708070377632424,11.066354053869413,660,127,983,0.91600000000000004,7.8,245,16.3,325,38,761.29308542055537,983,983,40.160656335170714,6.9018404907975457,0.19019704985814115,0.25540436661417326,0.12952589468312947,-26.637474765432103,9,32.436354560000005,9,-2691.5872000000004,7.5,2703.5872000000004,9,0.10794281551191688,0.17144215180246916,2.5906275722860053,8.2292232865185202,6.0686044418527754,23.722116829940735,2.979146061821603,182.50028097233078,0.24755724953138974,12.524278422296174,-153010.69908371847,761.29308542055537,7.2670226109468605E-2,3.2522058880969,-153619.94817518294,1431.7325874256796,8.3667317750326671,6.6677617714403142E-2,2.3589080693635047,-153640.82445947643,1500.3844654628876]
["KBM","KBM-60S02-A (240 V)",108,16.399999999999999,95.989033210228826,14.136823742301742,385,255,584,0.92100000000000004,11,411,31.7,325,38,446.96442055897234,584,584,89.780767259152299,3.5488958990536279,9.8064066566277475E-2,0.13959695309803924,0.21802046998889771,-30.539781530864197,9,35.597223040000003,9,-3014.1247999999996,7.5,3026.1247999999996,9,6.6580993494291307E-2,0.11261467165432099,1.5979438438629914,5.4055042394074073,3.9378705228545119,24.446499698886274,3.5198611961011839,215.62408956856882,0.70760195024155381,25.38764123306548,-152710.10390747918,446.96442055897234,0.21854809297479377,7.7057685726332714,-153576.12035612063,820.83441596643695,11.753139266593166,0.17449200997970557,2.5818054419180747,-153654.13485691548,931.02322186611298]
["KBM","KBM-60S03-A (240 V)",154,18.7,133.38699992463609,15.692588226427775,315,393,467,0.86699999999999999,11,515,47.5,325,38,358.38962772909792,467,467,123.44040941207953,2.3684210526315788,7.1246752978219779E-2,9.8830005089058523E-2,0.27264230079982071,-34.543446913580247,9,38.840192000000002,9,-3345.04,7.5,3357.04,9,5.4989754935648782E-2,9.8256438095238097E-2,1.3197541184555708,4.7163090285714286,3.3996182575254545,25.249187335413289,4.0746208793230929,249.60825682964426,1.0833844362918668,36.906289996527782,-152380.1143922068,358.38962772909792,0.32314721536459268,9.8198306951795189,-153573.10634849468,674.35129848966801,12.697465639261475,0.26937713415846465,2.629160547906225,-153657.48431974111,750.39571132737876]
["KBM","KBM-88H01-A (400 V)",205,17,162.33804195373327,13.306396881453548,425,414,542,0.93,13,738,98.4,565,46,315.00667676066973,466.356594627199,531.16531165311653,158.18662241274026,1.1432926829268293,5.9824771990640103E-2,0.11905187942028986,0.24246240331314403,-47.441330962962965,9,49.28747808,9,-4411.0896000000002,7.5,4423.0896000000002,9,4.19155225138651E-2,8.5151130829268284E-2,1.0059725403327624,4.0872542798048777,2.8732326200849267,28.181644367577132,5.8617897322341772,359.08889693019734,1.4113098397515564,40.812701158126359,-152899.42874987031,315.00667676066973,0.67241775662622771,15.670769818796241,-153551.2781914821,466.356594627199,13.182275801047108,0.55071419234561325,3.4156292665058023,-153658.64488579411,525.12864977699394]
["KBM","KBM-88H01-A (480 V)",205,17,151.31962281660205,12.403247771852628,520,414,651,0.93,13,738,98.4,679,46,315.00667676066973,466.84395218769458,531.16531165311653,156.80700107841608,1.1432926829268293,5.9843435508776049E-2,0.11905187942028986,0.24246240331314403,-47.441330962962965,9,49.28747808,9,-4411.0896000000002,7.5,4423.0896000000002,9,4.19155225138651E-2,8.5151130829268284E-2,1.0059725403327624,4.0872542798048777,2.8732326200849267,28.181644367577132,5.8617897322341772,359.08889693019734,1.4113098397515564,40.812701158126359,-152899.42874987031,315.00667676066973,0.67115140053170197,15.592920538203897,-153552.3953688507,466.84395218769458,13.11678886584559,0.55071419234561325,3.4156292665058023,-153658.64488579411,525.12864977699394]
["KBM","KBM-88H01-B (400 V)",205,32,66.998273370021394,10.197606296806908,935,414,1006,0.26100000000000001,3.7,397,98.4,565,46,600.40243190909291,952.6645847028816,987.40554156171288,64.391061402963459,1.1432926829268293,6.0135423183342245E-2,0.11905187942028986,0.13006214796179064,-47.441330962962965,9,49.28747808,9,-4411.0896000000002,7.5,4423.0896000000002,9,7.8899807084922544E-2,0.16028448156097561,1.8935953700381412,7.6936551149268295,5.4084378731010387,28.181644367577132,5.8617897322341772,359.08889693019734,0.4063632653612248,11.59813340574218,-153450.62909716862,600.40243190909291,0.1669461829669705,2.2470398076081426,-153655.99095880156,952.6645847028816,12.520426549720277,0.159351293474919,0.97065185036408075,-153662.50553424199,978.94703777244411]
["KBM","KBM-88H01-B (480 V)",205,32,67.048252621692072,10.20521348884202,940,414,1068,0.26100000000000001,3.7,397,98.4,679,46,600.40243190909291,952.13716301534157,987.40554156171288,65.267036827881725,1.1432926829268293,6.0129879701746047E-2,0.11905187942028986,0.13006214796179064,-47.441330962962965,9,49.28747808,9,-4411.0896000000002,7.5,4423.0896000000002,9,7.8899807084922544E-2,0.16028448156097561,1.8935953700381412,7.6936551149268295,5.4084378731010387,28.181644367577132,5.8617897322341772,359.08889693019734,0.4063632653612248,11.59813340574218,-153450.62909716862,600.40243190909291,0.16711153472301887,2.2668488568680969,-153655.84912704877,952.13716301534157,12.630801873485925,0.159351293474919,0.97065185036408075,-153662.50553424199,978.94703777244411]
["KBM","KBM-88H02-A (400 V)",385,15,331.71240770731868,12.907097576160259,190,789,257,1.66,29,1560,198,565,46,149.19769377310638,215.66783868864522,251.28205128205127,324.51357969113531,0.56818181818181823,3.9778197041517603E-2,9.2116130122517959E-2,0.51148358370593361,-72.679626666666664,9,69.730497600000007,9,-6497.1120000000001,7.5,6509.1120000000001,9,2.4459567985700297E-2,5.8993203463203463E-2,0.5870296316568071,2.8316737662337661,1.856970216540855,35.002958943051894,9.3588824188735504,573.31820447469818,5.8912834617309935,137.87986404702104,-151711.0437921572,149.19769377310638,3.0307669411326721,57.300196178495682,-153326.71033837792,215.66783868864522,12.775055486666997,2.4462176955356889,8.3291033699592596,-153656.87331905946,248.93067642757114]
["KBM","KBM-88H02-A (480 V)",385,15,323.05067172269821,12.570065047575806,235,789,309,1.66,29,1560,198,679,46,149.19769377310638,215.13076300222383,251.28205128205127,328.28848400097371,0.56818181818181823,3.9738984076259608E-2,9.2116130122517959E-2,0.51148358370593361,-72.679626666666664,9,69.730497600000007,9,-6497.1120000000001,7.5,6509.1120000000001,9,2.4459567985700297E-2,5.8993203463203463E-2,0.5870296316568071,2.8316737662337661,1.856970216540855,35.002958943051901,9.3588824188735504,573.31820447469818,5.8912834617309935,137.87986404702104,-151711.0437921572,149.19769377310638,3.0435838744744936,57.911845800952499,-153319.47112466375,215.13076300222383,12.911422521797972,2.4462176955356889,8.3291033699592596,-153656.87331905946,248.93067642757114]
["KBM","KBM-88H02-B (400 V)",385,31.7,273.02307055855135,22.563890128805898,440,789,545,0.36899999999999999,6.4,733,198,565,46,333.13202353645516,486.78463189451486,534.7885402455662,261.11670822992357,0.56818181818181823,3.9717785820826773E-2,9.2116130122517959E-2,0.23945424460004111,-72.679626666666664,9,69.730497600000007,9,-6497.1120000000001,7.5,6509.1120000000001,9,5.1691220343113298E-2,0.12467230331890332,1.2405892882347191,5.9842705593073591,3.9243970576230072,35.002958943051894,9.3588824188735504,573.31820447469818,1.2894056295513745,30.434523324444495,-153233.01210987655,333.13202353645516,0.62670872655903109,10.493988338004364,-153612.75951711362,486.78463189451486,22.400082046974838,0.54003360596062111,1.8385011657560533,-153662.42724933114,531.72561082049162]
["KBM","KBM-88H02-B (480 V)",385,31.7,233.08964847367582,19.263607311874036,550,789,654,0.36899999999999999,6.4,733,198,679,46,333.13202353645516,489.59321572574953,534.7885402455662,249.77404089854167,0.56818181818181823,3.9768273228182598E-2,9.2116130122517959E-2,0.23945424460004111,-72.679626666666664,9,69.730497600000007,9,-6497.1120000000001,7.5,6509.1120000000001,9,5.1691220343113298E-2,0.12467230331890332,1.2405892882347191,5.9842705593073591,3.9243970576230072,35.002958943051894,9.3588824188735504,573.31820447469818,1.2894056295513745,30.434523324444495,-153233.01210987655,333.13202353645516,0.6202234764432768,10.106283158454405,-153616.47578152592,489.59321572574953,21.572500811678005,0.54003360596062111,1.8385011657560533,-153662.42724933114,531.72561082049162]
["KBM","KBM-88H03-A (400 V)",538,18.100000000000001,462.41745283790686,15.413915094596895,165,1200,221,1.41,26,1812,298,565,46,126.22164547992375,188.19735362708036,216.3355408388521,451.79130087090959,0.37751677852348992,3.4824848219796235E-2,8.1682734156378597E-2,0.59341756559669345,-98.019280987654312,9,90.255617599999994,9,-8591.5120000000006,7.5,8603.5120000000006,9,2.5767615392195287E-2,6.8701556144537768E-2,0.61842276941268692,3.2976746949378128,2.043110935538655,42.703594881187691,12.870019654455247,788.4078706840362,8.0771003636998877,178.65512478481151,-151233.72970149666,126.22164547992375,3.9695658068161701,67.594250552412674,-153316.10904585826,188.19735362708036,15.274669559949619,3.2956213535948571,9.0412792198975502,-153657.77580220561,214.56047453783987]
["KBM","KBM-88H03-A (480 V)",538,18.100000000000001,443.08736156783664,14.769578718927887,225,1200,265,1.41,26,1812,298,679,46,126.22164547992375,187.52927190618459,216.3355408388521,458.89378675609532,0.37751677852348992,3.4771879417466366E-2,8.1682734156378597E-2,0.59341756559669345,-98.019280987654312,9,90.255617599999994,9,-8591.5120000000006,7.5,8603.5120000000006,9,2.5767615392195287E-2,6.8701556144537768E-2,0.61842276941268692,3.2976746949378128,2.043110935538655,42.703594881187691,12.870019654455247,788.4078706840362,8.0771003636998877,178.65512478481151,-151233.72970149666,126.22164547992375,3.9927981537812891,68.728943437255907,-153304.33104161479,187.52927190618459,15.531082771522501,3.2956213535948571,9.0412792198975502,-153657.77580220561,214.56047453783987]
["KBM","KBM-88H03-B (400 V)",545,35.5,400.51687418082179,25.839798334246566,345,1200,426,0.37,7,940,298,565,46,254.02977245253496,379.58806696605825,417.02127659574467,386.03167988720105,0.37751677852348992,3.4313141078885945E-2,8.1682734156378597E-2,0.30688390913335967,-98.019280987654312,9,90.255617599999994,9,-8591.5120000000006,7.5,8603.5120000000006,9,4.9889572342798699E-2,0.13301546158492844,1.1973497362271688,6.3847421560765651,3.9557378232908675,42.703594881187691,12.870019654455247,788.4078706840362,2.1861561239418492,47.087247227828627,-153036.67744129282,254.02977245253496,1.0251064874372537,15.520054954632348,-153595.84922312279,379.58806696605825,25.763392483883763,0.88693599392574018,2.3829652264155987,-153662.39335579722,414.89289820727055]
["KBM","KBM-88H03-B (480 V)",545,35.5,359.5029302781636,23.193737437300879,425,1200,511,0.37,7,940,298,679,46,254.02977245253496,380.34619657053793,417.02127659574467,378.99269425016382,0.37751677852348992,3.4338272363220214E-2,8.1682734156378597E-2,0.30688390913335967,-98.019280987654312,9,90.255617599999994,9,-8591.5120000000006,7.5,8603.5120000000006,9,4.9889572342798699E-2,0.13301546158492844,1.1973497362271688,6.3847421560765651,3.9557378232908675,42.703594881187684,12.870019654455247,788.4078706840362,2.1861561239418492,47.087247227828627,-153036.67744129282,254.02977245253496,1.0214808271420253,15.31993841096463,-153597.59537321306,380.34619657053793,25.431197715753072,0.88693599392574018,2.3829652264155987,-153662.39335579722,414.89289820727055]
["KBM","KBM-88S01-A (240 V)",205,17,179.31456921686876,14.697915509579408,225,414,325,0.93,13,738,98.4,325,46,315.00667676066973,325,325,167.89882220214378,1.1432926829268293,5.9915082915764771E-2,0.11905187942028986,0.39176601376466541,-47.441330962962965,9,49.28747808,9,-4411.0896000000002,7.5,4423.0896000000002,9,4.19155225138651E-2,8.5151130829268284E-2,1.0059725403327624,4.0872542798048777,2.8732326200849267,28.181644367577132,5.8617897322341772,359.08889693019734,1.4113098397515564,40.812701158126359,-152899.42874987031,315.00667676066973,0.65963465812842459,14.866227669365211,-153562.55542101015,471.35594379950959,12.505493700996979,0.55071419234561325,3.4156292665058023,-153658.64488579411,525.12864977699394]
["KBM","KBM-88S01-B (240 V)",205,32,156.03550620729419,23.74969653079059,500,414,604,0.26100000000000001,3.7,397,98.4,325,46,600.40243190909291,604,604,145.85089149841139,1.1432926829268293,5.9808725886395721E-2,0.11905187942028986,0.2108012491283382,-47.441330962962965,9,49.28747808,9,-4411.0896000000002,7.5,4423.0896000000002,9,7.8899807084922544E-2,0.16028448156097561,1.8935953700381412,7.6936551149268295,5.4084378731010387,28.181644367577132,5.8617897322341772,359.08889693019734,0.4063632653612248,11.59813340574218,-153450.62909716862,600.40243190909291,0.17737260676206618,3.2691581732212933,-153647.04761282424,921.54965995594273,18.215634030446537,0.159351293474919,0.97065185036408075,-153662.50553424199,978.94703777244411]
["KBM","KBM-88S02-A (240 V)",385,15,346.63946605414804,13.487916967087473,100,789,154,1.66,29,1560,198,325,46,149.19769377310638,154,154,325.92477772338799,0.56818181818181823,4.0019974827125909E-2,9.2116130122517959E-2,0.82677892515270301,-72.679626666666664,9,69.730497600000007,9,-6497.1120000000001,7.5,6509.1120000000001,9,2.4459567985700297E-2,5.8993203463203463E-2,0.5870296316568071,2.8316737662337661,1.856970216540855,35.002958943051894,9.3588824188735504,573.31820447469818,5.8912834617309935,137.87986404702104,-151711.0437921572,149.19769377310638,2.9557552361836645,53.580658768006025,-153369.07817697921,218.90647626978839,11.945786130315788,2.4462176955356889,8.3291033699592596,-153656.87331905946,248.93067642757114]
["KBM","KBM-88S02-B (240 V)",385,31.7,323.45702476889028,26.731985518090106,235,789,327,0.36899999999999999,6.4,733,198,325,46,327,327,327,299.36360467841325,0.56818181818181823,3.9734963628909416E-2,9.2116130122517959E-2,0.38936989135631883,-72.679626666666664,9,69.730497600000007,9,-6497.1120000000001,7.5,6509.1120000000001,9,5.1691220343113298E-2,0.12467230331890332,1.2405892882347191,5.9842705593073591,3.9243970576230072,35.002958943051894,9.3588824188735504,573.31820447469818,1.2894056295513745,30.434523324444495,-153233.01210987655,333.13202353645516,0.62536711268951861,10.414967247959693,-153613.52830656496,487.36102802333812,22.231406530724104,0.54003360596062111,1.8385011657560533,-153662.42724933114,531.72561082049162]
["KBM","KBM-88S03-A (240 V)",538,18.100000000000001,482.76999404541584,16.092333134847195,90,1200,132,1.41,26,1812,298,325,46,126.22164547992375,132,132,456.99599126660991,0.37751677852348992,3.5054093839518317E-2,8.1682734156378597E-2,0.9645754126781535,-98.019280987654312,9,90.255617599999994,9,-8591.5120000000006,7.5,8603.5120000000006,9,2.5767615392195287E-2,6.8701556144537768E-2,0.61842276941268692,3.2976746949378128,2.043110935538655,42.703594881187691,12.870019654455247,788.4078706840362,8.0771003636998877,178.65512478481151,-151233.72970149666,126.22164547992375,3.8787830169156052,62.96455584522618,-153362.13281118378,190.89251651404209,14.228470271729279,3.2956213535948571,9.0412792198975502,-153657.77580220561,214.56047453783987]
["KBM","KBM-88S03-B (240 V)",545,35.5,463.67140087438844,29.914283927379898,180,1200,255,0.37,7,940,298,325,46,254.02977245253496,255,255,429.7844845720503,0.37751677852348992,3.4360148299975968E-2,8.1682734156378597E-2,0.49930962538633827,-98.019280987654312,9,90.255617599999994,9,-8591.5120000000006,7.5,8603.5120000000006,9,4.9889572342798699E-2,0.13301546158492844,1.1973497362271688,6.3847421560765651,3.9557378232908675,42.703594881187691,12.870019654455247,788.4078706840362,2.1861561239418492,47.087247227828627,-153036.67744129282,254.02977245253496,1.0137647819533937,14.885102408964276,-153601.31148887353,381.97794510331005,24.709367115384339,0.88693599392574018,2.3829652264155987,-153662.39335579722,414.89289820727055]
["KBM","KBM-163H01-A (400 V)",776,43.2,534.60145384567647,29.535991925175495,300,1966,365,0.37,4.2,1100,1060,565,56,228.8884452378488,334.35835300342399,356.36363636363637,506.95459896806454,0.10613207547169812,6.1766178294869113E-2,0.14807092925411,0.36199211786709212,-291.10744691358025,9,246.65703200000002,9,-24550.84,7.5,24562.84,9,0.10862139771205616,0.3376246162657503,2.6069135450893479,16.205981580756013,10.134983572326528,108.78771813858621,39.624885389587796,2427.3911271991933,2.5725241885138996,77.154378213855807,-152434.08304182507,228.8884452378488,1.310900278111971,20.995907309246878,-153572.91980914495,334.35835300342399,29.783765938265645,1.2216836688962396,7.1446027378262045,-153653.45344043773,351.73128968588242]
["KBM","KBM-163H01-A (480 V)",776,43.2,440.54088247836631,24.339275275047861,375,1966,438,0.37,4.2,1100,1060,679,56,228.8884452378488,335.89645601928447,356.36363636363637,475.52125676033756,0.10613207547169812,6.1929092520326565E-2,0.14807092925411,0.36199211786709212,-291.10744691358025,9,246.65703200000002,9,-24550.84,7.5,24562.84,9,0.10862139771205616,0.3376246162657503,2.6069135450893479,16.205981580756013,10.134983572326528,108.78771813858621,39.624885389587796,2427.3911271991933,2.5725241885138996,77.154378213855807,-152434.08304182507,228.8884452378488,1.3016456276355377,20.009873361916778,-153581.27375372729,335.89645601928447,28.385026466714926,1.2216836688962396,7.1446027378262045,-153653.45344043773,351.73128968588242]
["KBM","KBM-163H02-A (400 V)",1090,40.6,843.68035333013711,31.017660048902101,200,2915,243,0.50900000000000001,6.3,1645,1570,565,56,149.45650791721917,220.2829668136086,238.29787234042556,818.69988723541405,7.1656050955414011E-2,6.2646530791720362E-2,0.14419886241873661,0.542731219265841,-420.33968395061726,9,351.33514400000001,9,-35232.28,7.5,35244.28,9,0.10332040605329401,0.32618102386076187,2.4796897452790563,15.65668914531657,9.8455421593756505,154.65824394462641,57.531685291054437,3524.3484248668165,5.7231399054328129,157.46440871065298,-151373.27467312798,149.45650791721917,2.9567405867374492,45.391773224812034,-153473.64578334524,220.2829668136086,31.299171138760283,2.7308331816564397,14.278544789330388,-153645.16454566192,234.59854519839286]
["KBM","KBM-163H02-A (480 V)",1090,40.6,781.87301838940914,28.74533155843416,245,2915,291,0.50900000000000001,6.3,1645,1570,679,56,149.45650791721917,220.35873143153665,238.29787234042556,812.86338454066026,7.1656050955414011E-2,6.2680637064320227E-2,0.14419886241873661,0.542731219265841,-420.33968395061726,9,351.33514400000001,9,-35232.28,7.5,35244.28,9,0.10332040605329401,0.32618102386076187,2.4796897452790563,15.65668914531657,9.8455421593756505,154.65824394462641,57.531685291054437,3524.3484248668165,5.7231399054328129,157.46440871065298,-151373.27467312798,149.45650791721917,2.955266442853512,45.258130447919079,-153474.76501772518,220.35873143153665,31.207019899708328,2.7308331816564397,14.278544789330388,-153645.16454566192,234.59854519839286]
["KBM","KBM-163H03-A (400 V)",1375,38.6,1115.3578411880026,30.810990088066365,150,3930,183,0.64,8.4,2190,1680,565,56,108.18501456669327,164.06954844696992,178.99543378995435,1091.0041883061276,6.6964285714285712E-2,5.3008044810639469E-2,0.11404918669305437,0.72149185635505397,-448.21330370370367,9,373.91277600000001,9,-37536.120000000003,7.5,37548.120000000003,9,8.2873504834981668E-2,0.26213687156004489,1.9889641160395599,12.582569834882154,7.9185030778422343,164.59536664986572,61.393936250194322,3760.9470576970889,10.334029821388199,267.83163534448545,-149924.8272924198,108.18501456669327,5.2368434273326256,75.558107454145812,-153366.41302297427,164.06954844696992,31.124067978103419,4.8246285247245515,19.223293910439736,-153644.73773332671,176.47316924234107]
["KBM","KBM-163H03-A (480 V)",1375,38.6,1063.9507945693204,29.390905927329289,180,3930,220,0.64,8.4,2190,1680,679,56,108.18501456669327,163.99705862597972,178.99543378995435,1091.6046956745579,6.6964285714285712E-2,5.3005496307735975E-2,0.11404918669305437,0.72149185635505397,-448.21330370370367,9,373.91277600000001,9,-37536.120000000003,7.5,37548.120000000003,9,8.2873504834981668E-2,0.26213687156004489,1.9889641160395599,12.582569834882154,7.9185030778422343,164.59536664986572,61.393936250194322,3760.9470576970889,10.334029821388199,267.83163534448545,-149924.8272924198,108.18501456669327,5.239968638031379,75.825516874116474,-153364.30290187721,163.99705862597972,31.234219876365337,4.8246285247245515,19.223293910439736,-153644.73773332671,176.47316924234107]
["KBM","KBM-163S01-A (240 V)",776,43.2,580.77085597351629,32.086787622846202,165,1966,219,0.37,4.2,1100,1060,325,56,219,219,219,516.8776815648489,0.10613207547169812,6.245805847107689E-2,0.14807092925411,0.58138791997039396,-291.10744691358025,9,246.65703200000002,9,-24550.84,7.5,24562.84,9,0.10862139771205616,0.3376246162657503,2.6069135450893479,16.205981580756013,10.134983572326528,108.78771813858621,39.624885389587796,2427.3911271991933,2.5725241885138996,77.154378213855807,-152434.08304182507,228.8884452378488,1.2720725501734422,16.467901446960873,-153607.9686408953,341.08431583107301,23.360558558700465,1.2216836688962396,7.1446027378262045,-153653.45344043773,351.73128968588242]
["KBM","KBM-163S02-A (240 V)",1090,40.6,945.38036196585824,34.756630954627141,110,2915,146,0.50900000000000001,6.3,1645,1570,325,56,146,146,146,898.05029860923003,7.1656050955414011E-2,6.275544005017572E-2,0.14419886241873661,0.87208187995559083,-420.33968395061726,9,351.33514400000001,9,-35232.28,7.5,35244.28,9,0.10332040605329401,0.32618102386076187,2.4796897452790563,15.65668914531657,9.8455421593756505,154.65824394462641,57.531685291054437,3524.3484248668165,5.7231399054328129,157.46440871065298,-151373.27467312798,149.45650791721917,2.9407998340771555,43.925048799963939,-153485.74869854498,221.10915143796859,30.287814773382017,2.7308331816564397,14.278544789330388,-153645.16454566192,234.59854519839286]
["KBM","KBM-163S03-A (240 V)",1375,38.6,1209.1796801406749,33.402753595046264,80,3930,110,0.64,8.4,2190,1680,325,56,108.18501456669327,110,110,1146.9970601934281,6.6964285714285712E-2,5.3310506881091659E-2,0.11404918669305437,1.1574904952137843,-448.21330370370367,9,373.91277600000001,9,-37536.120000000003,7.5,37548.120000000003,9,8.2873504834981668E-2,0.26213687156004489,1.9889641160395599,12.582569834882154,7.9185030778422343,164.59536664986572,61.393936250194322,3760.9470576970889,10.334029821388199,267.83163534448545,-149924.8272924198,108.18501456669327,5.1852808644107755,71.000905633190328,-153401.22771623125,165.28974737676293,29.246855008582799,4.8246285247245515,19.223293910439736,-153644.73773332671,176.47316924234107]
["KBM","KBM-260H01-A (400 V)",1932,33.1,1710.4475354640751,28.84397193025422,85,6494,111,1.06,16,3584,4880,565,58,54.516705088836581,96.945501843353469,109.375,1679.3115898933293,2.3053278688524591E-2,0.10456913641468277,0.19388393008551102,1.2175354755560648,-1259.0822419753085,9,1030.7166159999999,9,-104556.92,7.5,104568.92,9,0.13990159136148908,0.44940068807564176,3.3576381926757377,21.571233027630804,13.676642937061514,455.29018592232785,173.75032778880868,10643.816376395909,34.764057805170467,732.0953520520244,-143232.67909925466,54.516705088836581,14.317874763451499,189.77190515237746,-152963.08098522181,96.945501843353469,28.840143963831196,13.176273654876185,89.99409259225439,-153506.37249137912,104.5751495785909]
["KBM","KBM-260H01-A (480 V)",1932,33.1,1680.6761990504149,28.341925784998566,105,6494,134,1.06,16,3584,4880,679,58,54.516705088836581,96.720490843809401,109.375,1700.4937010611836,2.3053278688524591E-2,0.10430620911878927,0.19388393008551102,1.2175354755560648,-1259.0822419753085,9,1030.7166159999999,9,-104556.92,7.5,104568.92,9,0.13990159136148908,0.44940068807564176,3.3576381926757377,21.571233027630804,13.676642937061514,455.29018592232785,173.75032778880868,10643.816376395909,34.764057805170467,732.0953520520244,-143232.67909925466,54.516705088836581,14.359490941533707,192.43433970804284,-152943.27571707609,96.720490843809401,29.244761263836768,13.176273654876185,89.99409259225439,-153506.37249137912,104.5751495785909]
["KBM","KBM-260H02-A (400 V)",2706,31,2428.9938042061262,27.322764951699956,55,9741,74,1.48,24,5380,7190,565,58,32.531595539804037,63.446898902972372,72.862453531598504,2386.4511981812566,1.564673157162726E-2,0.11043725397283451,0.18934691066524212,1.8491248472629098,-1844.4282567901234,9,1504.846888,9,-152937.56,7.5,152949.56,9,0.13675773461813476,0.44020445276310222,3.2821856308352344,21.129813732628907,13.414191176296569,665.58649687698903,254.8575979307459,15612.38766583162,78.559271215097397,1539.012202733609,-133206.16912284453,32.531595539804037,31.92352823683802,377.12100979870769,-152435.60818645751,63.446898902972372,27.344885527522781,29.66131218446273,184.9988845974942,-153368.3937056709,68.856332043767765]
["KBM","KBM-260H02-A (480 V)",2706,31,2406.2823087173174,27.067292561499631,68,9741,89,1.48,24,5380,7190,679,58,32.531595539804037,63.241336387467889,72.862453531598504,2427.2566568281854,1.564673157162726E-2,0.10984649900246664,0.18934691066524212,1.8491248472629098,-1844.4282567901234,9,1504.846888,9,-152937.56,7.5,152949.56,9,0.13675773461813476,0.44020445276310222,3.2821856308352344,21.129813732628907,13.414191176296569,665.58649687698903,254.8575979307459,15612.38766583162,78.559271215097397,1539.012202733609,-133206.16912284453,32.531595539804037,32.032002700034298,383.92539092926717,-152390.88062457513,63.241336387467889,27.838268336399167,29.66131218446273,184.9988845974942,-153368.3937056709,68.856332043767765]
["KBM","KBM-260H03-A (400 V)",3444,29.5,3366.1270463935866,28.286781902467116,40,12812,55,1.9,32,7180,9560,565,58,21.740132594661269,45.940391551555592,54.596100278551532,3354.5621505011313,1.1767782426778242E-2,0.1115641629975163,0.190835003449698,2.4982405166178112,-2444.9780641975308,9,1991.292232,9,-202574.84,7.5,202586.84,9,0.13541115157816161,0.43630742410609735,3.2498676378758788,20.942756357092673,13.304559587811228,881.41830251674094,338.07155041403217,20710.012754992935,136.85574434483163,2593.07140327052,-121056.30713575242,21.740132594661269,57.22527223347371,668.70250151465632,-151495.51203662701,45.940391551555592,28.300510867707303,52.806163024639204,314.36861049996043,-153184.74188947713,50.965450935000867]
["KBM","KBM-260H03-A (480 V)",3444,29.5,3288.7777440509253,27.636787765133825,50,12812,67,1.9,32,7180,9560,679,58,21.740132594661269,46.036809926411763,54.596100278551532,3301.0812501304722,1.1767782426778242E-2,0.11241310888216056,0.190835003449698,2.4982405166178112,-2444.9780641975308,9,1991.292232,9,-202574.84,7.5,202586.84,9,0.13541115157816161,0.43630742410609735,3.2498676378758788,20.942756357092673,13.304559587811228,881.41830251674094,338.07155041403217,20710.012754992935,136.85574434483163,2593.07140327052,-121056.30713575242,21.740132594661269,57.115872100034501,662.22321884636699,-151537.33086539499,46.036809926411763,28.026297732339135,52.806163024639204,314.36861049996043,-153184.74188947713,50.965450935000867]
["KBM","KBM-260S01-A (240 V)",1932,33.1,1761.3147035503084,29.701765658521222,45,6494,67,1.06,16,3584,4880,325,58,54.516705088836581,67,67,1677.8685586193481,2.3053278688524591E-2,0.10605879285676741,0.19388393008551102,1.9003575294554667,-1259.0822419753085,9,1030.7166159999999,9,-104556.92,7.5,104568.92,9,0.13990159136148908,0.44940068807564176,3.3576381926757377,21.571233027630804,13.676642937061514,455.29018592232785,173.75032778880868,10643.816376395909,34.764057805170467,732.0953520520244,-143232.67909925466,54.516705088836581,14.105067112297689,175.52721049961201,-153064.35680603932,98.135153643726284,26.675339620550218,13.176273654876185,89.99409259225439,-153506.37249137912,104.5751495785909]
["KBM","KBM-260S02-A (240 V)",2706,31,2482.8171122335671,27.928201487441697,28,9741,44,1.48,24,5380,7190,325,58,32.531595539804037,44,44,2355.2840335098908,1.564673157162726E-2,0.11327993808014404,0.18934691066524212,2.8937262380344606,-1844.4282567901234,9,1504.846888,9,-152937.56,7.5,152949.56,9,0.13675773461813476,0.44020445276310222,3.2821856308352344,21.129813732628907,13.414191176296569,665.58649687698903,254.8575979307459,15612.38766583162,78.559271215097397,1539.012202733609,-133206.16912284453,32.531595539804037,31.434980748370013,344.81523220754104,-152637.05226259361,64.41337476865958,25.002407205830799,29.66131218446273,184.9988845974942,-153368.3937056709,68.856332043767765]
["KBM","KBM-260S03-A (240 V)",3444,29.5,3317.1240770731874,27.874992244312498,19,12812,33,1.9,32,7180,9560,325,58,21.740132594661269,33,33,3223.6365549165885,1.1767782426778242E-2,0.11511700409475321,0.190835003449698,3.858301650712614,-2444.9780641975308,9,1991.292232,9,-202574.84,7.5,202586.84,9,0.13541115157816161,0.43630742410609735,3.2498676378758788,20.942756357092673,13.304559587811228,881.41830251674094,338.07155041403217,20710.012754992935,136.85574434483163,2593.07140327052,-121056.30713575242,21.740132594661269,56.383905302603416,617.12434165373304,-151817.12937389166,46.705154499549089,26.117644390650447,52.806163024639204,314.36861049996043,-153184.74188947713,50.965450935000867]
["KBM","KBMS-10H01-A (120 V)",0.48699999999999999,1.73,0.44870188775305436,1.5599425940517813,4150,1.17,6565,13,19,17.382100000000001,1.0200000000000001E-2,160,6,6565,6565,6565,0.42641515496356674,11029.411764705881,20.359320269852049,24.865686805333336,"NA",-22.509695755851851,9,29.092853562240002,9,-2350.4136288,7.5,2362.4136288,9,1.4669506809347717,2.1530902063088297,35.206816342434522,103.34832990282382,77.411311292699168,23.024217392692538,2.4071888284198142,147.46260452616195,7.6374634761367834E-4,1.6267065951735979,-151474.45449587636,13058.254406887478,3.2787881010026924E-4,0.38413889413729851,-153541.90100647189,21062.109580485896,0.9814813644999717,0.16043374328445106,30.297768851521052,605886.78395999316,-9999]
["KBM","KBMS-10H01-A (240 V)",0.48699999999999999,1.73,0.414767427451606,1.4419671375733765,9900,1.17,13766,13,19,17.382100000000001,1.0200000000000001E-2,325,6,13058.254406887478,13766,13766,0.38656024306048564,11029.411764705881,20.357527524125434,24.865686805333336,"NA",-22.509695755851851,9,29.092853562240002,9,-2350.4136288,7.5,2362.4136288,9,1.4669506809347717,2.1530902063088297,35.206816342434522,103.34832990282382,77.411311292699168,23.024217392692538,2.4071888284198142,147.46260452616195,7.6374634761367834E-4,1.6267065951735979,-151474.45449587636,13058.254406887478,3.4052410932198325E-4,0.46909689482150196,-153481.92067414316,20552.6128883659,1.1985504916030405,0.16043374328445106,30.297768851521052,605886.78395999316,-9999]
["KBM","KBMS-10H01-A (400 V)",0.48699999999999999,1.73,0.36804580590000802,1.2795362463496316,14400,1.17,16000,13,19,17.382100000000001,1.0200000000000001E-2,565,6,13058.254406887478,16000,16000,0.35482867322223111,11029.411764705881,20.358422343163642,24.865686805333336,"NA",-22.509695755851851,9,29.092853562240002,9,-2350.4136288,7.5,2362.4136288,9,1.4669506809347717,2.1530902063088297,35.206816342434522,103.34832990282382,77.411311292699168,23.024217392692538,2.4071888284198142,147.46260452616195,7.6374634761367834E-4,1.6267065951735979,-151474.45449587636,13058.254406887478,3.380067200498532E-4,0.45345447066345806,-153493.8613836903,20649.747172399973,1.1585838336024141,0.16043374328445106,30.297768851521052,605886.78395999316,-9999]
["KBM","KBMS-10H01-B (120 V)",0.50900000000000001,3.37,0.4297183463481174,2.790016532580947,9000,1.19,12319,3.42,5.2,9.3041110000000007,1.0200000000000001E-2,160,6,12319,12319,12319,0.40048103429582871,11029.411764705881,19.478639329877907,24.447776102722692,"NA",-22.509695755851851,9,29.092853562240002,9,-2350.4136288,7.5,2362.4136288,9,2.7340754148373647,4.0128895098538315,65.61780995609675,192.61869647298391,144.27776324479024,23.024217392692538,2.4071888284198142,147.46260452616195,2.1081346565340067E-4,0.43423087158044971,-153119.45768244949,25940.227342568163,8.8965969527187469E-5,6.0344412293786023E-2,-153653.48366610272,41220.68158712962,1.0949024954060449,4.1751097490071568E-2,7.9517188668385614,28940.836887710087,-9999]
["KBM","KBMS-10H01-B (240 V)",0.50900000000000001,3.37,0.30970691628693148,2.0108227261844664,18500,1.19,20000,3.42,5.2,9.3041110000000007,1.0200000000000001E-2,325,6,20000,20000,20000,0.29354801760749349,11029.411764705881,19.480307192229358,24.447776102722692,"NA",-22.509695755851851,9,29.092853562240002,9,-2350.4136288,7.5,2362.4136288,9,2.7340754148373647,4.0128895098538315,65.61780995609675,192.61869647298391,144.27776324479024,23.024217392692538,2.4071888284198142,147.46260452616195,2.1081346565340067E-4,0.43423087158044971,-153119.45768244949,25940.227342568163,8.7772488223988214E-5,4.2781167557851635E-2,-153658.71438521615,41597.748286872236,0.77623105992697461,4.1751097490071568E-2,7.9517188668385614,28940.836887710087,-9999]
["KBM","KBMS-10H01-C (120 V)",0.49199999999999999,5.21,0.34500684437985052,3.8004719583592257,15500,1.23,19702,1.44,2.2000000000000002,5.8349039999999999,1.0200000000000001E-2,160,6,19702,19702,19702,0.30515747406269778,11029.411764705881,20.152562270033403,23.652726473365856,6.9215374847899719E-2,-22.509695755851851,9,29.092853562240002,9,-2350.4136288,7.5,2362.4136288,9,4.3729145568581327,6.418265881574797,104.94994936459518,308.07676231559026,230.75966657693832,23.024217392692538,2.4071888284198142,147.46260452616195,9.482626404107243E-5,0.18955470407524055,-153400.15934799999,39233.536220237569,3.4046385710745982E-5,4.0758993057434607E-4,-153663.99878011338,67175.647724479873,2.8007001311999069E-2,1.9111753169503771E-2,3.3582787186558707,-70849.563112678166,1839.5328314454662]
["KBM","KBMS-10H01-C (240 V)",0.49199999999999999,5.21,0.29520674928335428,3.2518919286555881,18600,1.23,20000,1.44,2.2000000000000002,5.8349039999999999,1.0200000000000001E-2,325,6,20000,20000,20000,0.28039435406812285,11029.411764705881,20.153559509471727,23.652726473365856,6.9215374847899719E-2,-22.509695755851851,9,29.092853562240002,9,-2350.4136288,7.5,2362.4136288,9,4.3729145568581327,6.418265881574797,104.94994936459518,308.07676231559026,230.75966657693832,23.024217392692538,2.4071888284198142,147.46260452616195,9.482626404107243E-5,0.18955470407524055,-153400.15934799999,39233.536220237569,3.4269130472090922E-5,-1.1482360705550997E-2,-153663.03186716529,67130.472523704011,-0.78899518173095462,1.9111753169503771E-2,3.3582787186558707,-70849.563112678166,1839.5328314454662]
["KBM","KBMS-10H02-A (120 V)",0.876,1.53,0.85343954991306192,1.4551398975499776,2070,2.33,3359,20,36,35.4,1.49E-2,160,6,3359,3359,3359,0.83939103775747581,7550.3355704697988,11.316939543383354,12.486617271622316,"NA",-22.510886719604937,9,29.093818242879998,9,-2350.5120655999999,7.5,2362.5120655999999,9,0.72125575468650982,1.0586363658582192,17.310138112476235,50.814545561194521,38.061582937831126,23.02440800947161,2.4073538518698867,147.47271374047381,2.8418987989117139E-3,4.9904203768525361,-148695.70075295551,6408.5244608318253,1.3945263648290124E-3,1.488620259018296,-153221.91952433056,9961.9137213821086,1.2139199255160222,0.14022912637081419,46.674613589092694,280941.22872001922,-9999]
["KBM","KBMS-10H02-A (240 V)",0.876,1.53,0.79409940026903569,1.3539631718142127,4750,2.33,6753,20,36,35.4,1.49E-2,325,6,6408.5244608318253,6753,6753,0.75956321052985221,7550.3355704697988,11.318758488741102,12.486617271622316,"NA",-22.510886719604937,9,29.093818242879998,9,-2350.5120655999999,7.5,2362.5120655999999,9,0.72125575468650982,1.0586363658582192,17.310138112476235,50.814545561194521,38.061582937831126,23.02440800947161,2.4073538518698867,147.47271374047381,2.8418987989117139E-3,4.9904203768525361,-148695.70075295551,6408.5244608318253,1.3927081354739642E-3,1.4790160911392265,-153227.60548576224,9971.5511178805264,1.2060880485240404,0.14022912637081419,46.674613589092694,280941.22872001922,-9999]
["KBM","KBMS-10H02-A (400 V)",0.876,1.53,0.70832694452986378,1.2077185754984889,9100,2.33,11291,20,36,35.4,1.49E-2,565,6,6408.5244608318253,9953.8456568124038,11073.446327683616,0.69259431703781527,7550.3355704697988,11.319097879398473,12.486617271622316,"NA",-22.510886719604937,9,29.093818242879998,9,-2350.5120655999999,7.5,2362.5120655999999,9,0.72125575468650982,1.0586363658582192,17.310138112476235,50.814545561194521,38.061582937831126,23.02440800947161,2.4073538518698867,147.47271374047381,2.8418987989117139E-3,4.9904203768525361,-148695.70075295551,6408.5244608318253,1.3960546856578299E-3,1.4966454117217529,-153217.1401639799,9953.8456568124038,1.2204641685578708,0.14022912637081419,46.674613589092694,280941.22872001922,-9999]
["KBM","KBMS-10H02-A (480 V)",0.876,1.53,0.64240722484365043,1.0953234865194381,11000,2.33,13564,20,36,35.4,1.49E-2,679,6,6408.5244608318253,9997.8587225428309,11073.446327683616,0.66368840321637312,7550.3355704697988,11.319903890812677,12.486617271622316,"NA",-22.510886719604937,9,29.093818242879998,9,-2350.5120655999999,7.5,2362.5120655999999,9,0.72125575468650982,1.0586363658582192,17.310138112476235,50.814545561194521,38.061582937831126,23.02440800947161,2.4073538518698867,147.47271374047381,2.8418987989117139E-3,4.9904203768525361,-148695.70075295551,6408.5244608318253,1.3877857103813988E-3,1.4526964789001859,-153242.9988788724,9997.8587225428309,1.1846252869263332,0.14022912637081419,46.674613589092694,280941.22872001922,-9999]
["KBM","KBMS-10H02-B (120 V)",0.89900000000000002,2.99,0.82321522288911386,2.6814828107137259,4350,2.48,6174,5.22,9.6999999999999993,18.536100000000001,1.49E-2,160,6,6174,6174,6174,0.79143788186606645,7550.3355704697988,11.02910519386514,11.731378323741934,0.1316214539420642,-22.510886719604937,9,29.093818242879998,9,-2350.5120655999999,7.5,2362.5120655999999,9,1.3734519276357127,2.0159092636774933,32.962846263257106,96.763644656519674,72.478803968159824,23.02440800947161,2.4073538518698867,147.47271374047381,8.1742603491368859E-4,1.3823329860401852,-152273.635648,12829.226322161918,3.6488722987117656E-4,0.29308214940825628,-153601.49971222773,20119.538049342602,1.7487989095104577,3.6930562832066804E-2,12.14676172200627,-46308.498371044261,967.34955176502172]
["KBM","KBMS-10H02-B (240 V)",0.89900000000000002,2.99,0.70664794732801528,2.301784844716662,10000,2.48,12944,5.22,9.6999999999999993,18.536100000000001,1.49E-2,325,6,12829.226322161918,12944,12944,0.650019503021383,7550.3355704697988,11.029599007656344,11.731378323741934,0.1316214539420642,-22.510886719604937,9,29.093818242879998,9,-2350.5120655999999,7.5,2362.5120655999999,9,1.3734519276357127,2.0159092636774933,32.962846263257106,96.763644656519674,72.478803968159824,23.02440800947161,2.4073538518698867,147.47271374047381,8.1742603491368859E-4,1.3823329860401852,-152273.635648,12829.226322161918,3.6579274978514389E-4,0.29924709631147284,-153598.84268626707,20086.669137932673,1.7855846791088543,3.6930562832066804E-2,12.14676172200627,-46308.498371044261,967.34955176502172]
["KBM","KBMS-10H02-B (400 V)",0.89900000000000002,2.99,0.49317090918607037,1.6064198996288936,15200,2.48,16000,5.22,9.6999999999999993,18.536000000000001,1.49E-2,565,6,12829.257894707194,16000,16000,0.47181148335375828,7550.3355704697988,11.03163202475052,11.731378323741934,0.13162134511896714,-22.510886719604937,9,29.093818242879998,9,-2350.5120655999999,7.5,2362.5120655999999,9,1.3734519276357127,2.0159092636774933,32.962846263257106,96.763644656519674,72.478803968159824,23.02440800947161,2.4073538518698867,147.47271374047381,8.1742232770368856E-4,1.382325528522228,-152273.635648,12829.257894707194,3.5717577991008323E-4,0.23412313253438657,-153624.11619174603,20413.889665184211,1.3970024737225284,3.69305591248568E-2,12.146696191707436,-46308.498371044261,967.35035155911351]
["KBM","KBMS-10H02-C (120 V)",0.86799999999999999,5.14,0.70215416069953829,4.058694570517563,8500,2.2400000000000002,11008,1.77,3.2,10.46,1.49E-2,160,6,{"$f":"IF(AQ827<I827,IF(AQ827<0,0,AQ827),I827)","v":11008},{"$f":"IF(AU827<I827,IF(AU827<0,0,AU827),I827)","v":11008},{"$f":"IF(UAC_V*0.98/L827*1000<I827,IF(UAC_V*0.98/L827*1000<0,0,UAC_V*0.98/L827*1000),I827)","v":11008},{"$f":"C827+(E827-C827)/G827*Q827","v":0.65321988246829621},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M827,(inertia/gear^2+gear_inertia)/M827),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M827,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M827))","v":7550.3355704697988},{"$f":"IF((C827+(E827-C827)/G827*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X827^2*time1+Y827^2*time2+Z827^2*time3+AA827^2*time4)/time)/(C827+(E827-C827)/G827*mspeed),SQRT((((X827-Y827)*2/PI()+Y827)^2*time1+Y827^2*time2+((Z827-Y827)*2/PI()+Y827)^2*time3+AA827^2*time4)/time)/(C827+(E827-C827)/G827*mspeed)),IF(AccType=1,SQRT((X827^2*time1+Y827^2*time2+Z827^2*time3+AA827^2*time4+AB827^2*time5+AC827^2*time6+AD827^2*time7+AE827^2*time8)/time)/(C827+(E827-C827)/G827*mspeed),SQRT((((X827-Y827)*2/PI()+Y827)^2*time1+Y827^2*time2+((Z827-Y827)*2/PI()+Y827)^2*time3+AA827^2*time4+((AB827-AC827)*2/PI()+AC827)^2*time5+AC827^2*time6+((AD827-AC827)*2/PI()+AC827)^2*time7+AE827^2*time8)/time)/(C827+(E827-C827)/G827*mspeed))))","v":11.423787670507599},{"$f":"IF(move1,MAX(ABS(X827),ABS(Z827))/H827,MAX(ABS(X827),ABS(Z827),ABS(AB827),ABS(AD827))/H827)","v":12.988311715571426},{"$f":"IF(AZ827>0,speed/(MIN(AZ827,I827)),\"NA\")","v":4.4813350117841488E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M827+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M827+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.510886719604937},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M827+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M827+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.093818242879998},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M827+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M827+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2350.5120655999999},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M827+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M827+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2362.5120655999999},9,{"$f":"AH827/Irms","v":2.4453743948086397},{"$f":"AI827/Ipeak","v":3.5892431300019965},{"$f":"IF(move1,IF(AccType=1,SQRT((X827^2*time1+Y827^2*time2+Z827^2*time3+AA827^2*time4)/time)/(C827/D827),SQRT((((X827-Y827)*2/PI()+Y827)^2*time1+Y827^2*time2+((Z827-AA827)*2/PI()+AA827)^2*time3+AA827^2*time4)/time)/(C827/D827)),IF(AccType=1,SQRT((X827^2*time1+Y827^2*time2+Z827^2*time3+AA827^2*time4+AB827^2*time5+AC827^2*time6+AD827^2*time7+AE827^2*time8)/time)/(C827/D827),SQRT((((X827-Y827)*2/PI()+Y827)^2*time1+Y827^2*time2+((Z827-AA827)*2/PI()+AA827)^2*time3+AA827^2*time4+((AB827-AC827)*2/PI()+AC827)^2*time5+AC827^2*time6+((AD827-AE827)*2/PI()+AE827)^2*time7+AE827^2*time8)/time)/(C827/D827)))","v":58.688985475407357},{"$f":"IF(move1,MAX(ABS(X827),ABS(Z827))/(C827/D827),MAX(ABS(X827),ABS(Z827),ABS(AB827),ABS(AD827))/(C827/D827))","v":172.28367024009583},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X827),ABS(Z827))/(C827/D827),MAX(ABS((X827-Y827)*2/PI()+Y827),ABS((Z827-Y827)*2/PI()+Y827))/(C827/D827)),IF(AccType=1,MAX(ABS(X827),ABS(Z827),ABS(AB827),ABS(AD827))/(C827/D827),MAX(ABS((X827-Y827)*2/PI()+Y827),ABS((Z827-Y827)*2/PI()+Y827),ABS((AB827-AC827)*2/PI()+AC827),ABS((AD827-AC827)*2/PI()+AC827))/(C827/D827)))","v":129.04551504412211},{"$f":"IF((C827+(E827-C827)/G827*mspeed)<0,\"NA\",U827*(C827+(E827-C827)/G827*mspeed)*mspeed/9.55)","v":23.02440800947161},{"$f":"IF(move1,IF(speed1>speed2,AM827/2*time1/time,AM827/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z827*-speed/30*PI(),((Z827-AA827)*2/PI()+AA827)*-speed/30*PI()),IF(AccType=1,X827*-speed/30*PI(),((X827-Y827)*2/PI()+Y827)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z827*-speed/30*PI(),((Z827-AA827)*2/PI()+AA827)*-speed/30*PI()),IF(AccType=1,X827*-speed/30*PI(),((X827-Y827)*2/PI()+Y827)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD827*-speed/30*PI(),((AD827-AE827)*2/PI()+AE827)*-speed/30*PI()),IF(AccType=1,AB827*-speed/30*PI(),((AB827-AC827)*2/PI()+AC827)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD827*-speed/30*PI(),((AD827-AE827)*2/PI()+AE827)*-speed/30*PI()),IF(AccType=1,AB827*-speed/30*PI(),((AB827-AC827)*2/PI()+AC827)*-speed/30*PI()),0)/2*time7/time)))","v":2.4073538518698867},{"$f":"IF(move1,MAX(IF(AccType=1,Z827*-speed/30*PI(),((Z827-AA827)*2/PI()+AA827)*-speed/30*PI()),IF(AccType=1,X827*-speed/30*PI(),((X827-Y827)*2/PI()+Y827)*-speed/30*PI()),0),MAX(IF(AccType=1,Z827*-speed/30*PI(),((Z827-AA827)*2/PI()+AA827)*-speed/30*PI()),IF(AccType=1,X827*-speed/30*PI(),((X827-Y827)*2/PI()+Y827)*-speed/30*PI()),IF(AccType=1,AD827*-speed/30*PI(),((AD827-AE827)*2/PI()+AE827)*-speed/30*PI()),IF(AccType=1,AB827*-speed/30*PI(),((AB827-AC827)*2/PI()+AC827)*-speed/30*PI()),0))","v":147.47271374047381},{"$f":"(L827^2)/1000000+((K827/1000)^2*(D827/C827*H827)^2*PI()*PI()*(O827/2)^2)/1200","v":2.4277718973342478E-4},{"$f":"SQRT(3)*L827*J827*D827/C827*H827/1000","v":0.42536033604146428},{"$f":"0.75*J827^2*(D827/C827*H827)^2-(UAC_V*0.98)^2","v":-153250.58082077836},{"$f":"-AO827/2/AN827+SQRT((AO827/2/AN827)^2-AP827/AN827)","v":24263.720089521878},{"$f":"(L827^2)/1000000+((K827/1000)^2*AV827^2*PI()*PI()*(O827/2)^2)/1200","v":1.1035501930651188E-4},{"$f":"SQRT(3)*L827*J827*AV827/1000","v":3.5775645240805939E-2},{"$f":"0.75*J827^2*AV827^2-(UAC_V*0.98)^2","v":-153661.07550023857},{"$f":"-AS827/2/AR827+SQRT((AS827/2/AR827)^2-AT827/AR827)","v":37153.46852293305},{"$f":"D827+(F827-D827)*((0.85*UAC_V-D827*J827)/L827*1000)/G827","v":1.1156344000935423},{"$f":"(L827^2)/1000000+((K827/1000)^2*AJ827^2*PI()*PI()*(O827/2)^2)/1200","v":1.2731952774659163E-2},{"$f":"SQRT(3)*L827*J827*AJ827/1000","v":4.1381715782056414},{"$f":"0.75*J827^2*AJ827^2-(UAC_V*0.98)^2","v":-114535.46150255325},{"$f":"IF(((AX827/2/AW827)^2-AY827/AW827)>0,-AX827/2/AW827+SQRT((AX827/2/AW827)^2-AY827/AW827),-9999)","v":2841.205893750508}]
["KBM","KBMS-10H02-C (240 V)",0.86799999999999999,5.14,0.25034642399860291,1.4470891560612886,18500,2.2400000000000002,20000,1.77,3.2,10.46,1.49E-2,325,6,20000,20000,20000,0.20026640432281406,7550.3355704697988,11.427842620062034,12.988311715571426,4.4813350117841488E-2,-22.510886719604937,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},29.093818242879998,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},-2350.5120655999999,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},2362.5120655999999,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},2.4453743948086397,3.5892431300019965,58.688985475407357,172.28367024009583,129.04551504412211,23.02440800947161,2.4073538518698867,147.47271374047381,2.4277718973342478E-4,0.42536033604146428,-153250.58082077836,24263.720089521878,1.1045787917593393E-4,-3.76754880045677E-2,-153660.7566455559,37468.725154718493,-1.1748794515176284,1.2731952774659163E-2,4.1381715782056414,-114535.46150255325,2841.205893750508]
["KBM","KBMS-10H03-A (120 V)",1.1579999999999999,1.54,1.0725659208366858,1.3983910310778171,1380,3.46,2455,21.2,41,46.4,2.0199999999999999E-2,160,6,2455,2455,2455,1.0060140113435243,5569.3069306930693,8.5688813025332848,8.4089323913988459,"NA",-22.512229721283951,9,29.094906074240004,9,-2350.6230688000001,7.5,2362.6230688000001,9,0.54918438787170765,0.80609807416396106,13.180425308920983,38.692707559870129,28.981808615997515,23.024622967966629,2.4075399421433734,147.48411349278294,4.7875027048190433E-3,7.8397593019290408,-146527.10173990889,4773.7712936945718,2.2450492354651745E-3,1.4657319052751316,-153414.5329850367,7946.4806059425755,0.86028048762851783,0.1066682164823497,49.378734229049002,129464.73834895407,-9999]
["KBM","KBMS-10H03-A (240 V)",1.1579999999999999,1.54,1.0203357995480415,1.3302943931525966,3650,3.46,5155,21.2,41,46.4,2.0199999999999999E-2,325,6,4773.7712936945718,5155,5155,0.96357288949867237,5569.3069306930693,8.5649067385450657,8.4089323913988459,"NA",-22.512229721283951,9,29.094906074240004,9,-2350.6230688000001,7.5,2362.6230688000001,9,0.54918438787170765,0.80609807416396106,13.180425308920983,38.692707559870129,28.981808615997515,23.024622967966625,2.4075399421433734,147.48411349278294,4.7875027048190433E-3,7.8397593019290408,-146527.10173990889,4773.7712936945718,2.3202297222781974E-3,1.9754169488811952,-153210.87127002742,7711.4948014369738,1.1594293949234582,0.1066682164823497,49.378734229049002,129464.73834895407,-9999]
["KBM","KBMS-10H03-A (400 V)",1.1579999999999999,1.54,0.98952855922352334,1.290128499639535,6900,3.46,8619,21.2,41,46.4,2.0199999999999999E-2,565,6,4773.7712936945718,7593.59082106804,8448.2758620689656,0.9725937411170491,5569.3069306930693,8.5627232556407726,8.4089323913988459,"NA",-22.512229721283951,9,29.094906074240004,9,-2350.6230688000001,7.5,2362.6230688000001,9,0.54918438787170765,0.80609807416396106,13.180425308920983,38.692707559870129,28.981808615997515,23.024622967966636,2.4075399421433734,147.48411349278294,4.7875027048190433E-3,7.8397593019290408,-146527.10173990889,4773.7712936945718,2.363288768676954E-3,2.2151311656497477,-153094.22558697878,7593.59082106804,1.300124608387089,0.1066682164823497,49.378734229049002,129464.73834895407,-9999]
["KBM","KBMS-10H03-A (480 V)",1.1579999999999999,1.54,0.87628839255302382,1.1424881258839945,8500,3.46,10354,21.2,41,46.4,2.0199999999999999E-2,679,6,4773.7712936945718,7652.6798656519368,8448.2758620689656,0.90437073573765692,5569.3069306930693,8.5641557486685613,8.4089323913988459,"NA",-22.512229721283951,9,29.094906074240004,9,-2350.6230688000001,7.5,2362.6230688000001,9,0.54918438787170765,0.80609807416396106,13.180425308920983,38.692707559870129,28.981808615997515,23.024622967966629,2.4075399421433734,147.48411349278294,4.7875027048190433E-3,7.8397593019290408,-146527.10173990889,4773.7712936945718,2.3412799670856801E-3,2.0960338524259736,-153153.84677949012,7652.6798656519368,1.2302229474307746,0.1066682164823497,49.378734229049002,129464.73834895407,-9999]
["KBM","KBMS-10H03-B (120 V)",1.17,2.4,1.0672743242632983,2.1431211330588318,2550,3.57,3799,8.77,17,30,2.0199999999999999E-2,160,6,3799,3799,3799,1.0169588854416747,5569.3069306930693,8.4774118344197067,8.1498336342408972,0.17369300130289897,-22.512229721283951,9,29.094906074240004,9,-2350.6230688000001,7.5,2362.6230688000001,9,0.84709360127264388,1.2433720544547011,20.330246430543454,59.681858613825653,44.70320929380636,23.024622967966629,2.4075399421433734,147.48411349278294,2.0472182408516689E-3,3.3371449556365054,-150570.51765140827,7799.6606254813905,9.3778368391033069E-4,0.60562556473237483,-153562.11602092849,12477.656238320184,1.3289930932206606,4.365001357975698E-2,20.371367249397636,-38388.276775047023,733.04021185907857]
["KBM","KBMS-10H03-B (240 V)",1.17,2.4,0.98185139021865797,1.971589136985257,6030,3.57,7967,8.77,17,30,2.0199999999999999E-2,325,6,7799.6606254813905,7967,7967,0.92141293961393833,5569.3069306930693,8.4759509431282023,8.1498336342408972,0.17369300130289897,-22.512229721283951,9,29.094906074240004,9,-2350.6230688000001,7.5,2362.6230688000001,9,0.84709360127264388,1.2433720544547011,20.330246430543454,59.681858613825653,44.70320929380636,23.024622967966629,2.4075399421433734,147.48411349278294,2.0472182408516689E-3,3.3371449556365054,-150570.51765140827,7799.6606254813905,9.578637725931277E-4,0.74947201712286848,-153507.9699154305,12274.23666877771,1.6446517325578867,4.365001357975698E-2,20.371367249397636,-38388.276775047023,733.04021185907857]
["KBM","KBMS-10H03-B (400 V)",1.17,2.4,0.73391973757660023,1.4737344128044181,11450,3.57,13319,8.77,17,30,2.0199999999999999E-2,565,6,7799.6606254813905,12343.918687793326,13066.666666666666,0.6998742968815701,5569.3069306930693,8.4770580909884767,8.1498336342408972,0.17369300130289897,-22.512229721283951,9,29.094906074240004,9,-2350.6230688000001,7.5,2362.6230688000001,9,0.84709360127264388,1.2433720544547011,20.330246430543454,59.681858613825653,44.70320929380636,23.024622967966625,2.4075399421433734,147.48411349278294,2.0472182408516689E-3,3.3371449556365054,-150570.51765140827,7799.6606254813905,9.5072948522776344E-4,0.7017497674183828,-153527.20757331341,12343.918687793326,1.5399293695277867,4.365001357975698E-2,20.371367249397636,-38388.276775047023,733.04021185907857]
["KBM","KBMS-10H03-B (480 V)",1.17,2.4,0.49415940372588485,0.99228795928892544,14300,3.57,16000,8.77,17,30,2.0199999999999999E-2,679,6,7799.6606254813905,12462.657747265937,13066.666666666666,0.58099510188304671,5569.3069306930693,8.4785344065454886,8.1498336342408972,0.17369300130289897,-22.512229721283951,9,29.094906074240004,9,-2350.6230688000001,7.5,2362.6230688000001,9,0.84709360127264388,1.2433720544547011,20.330246430543454,59.681858613825653,44.70320929380636,23.024622967966629,2.4075399421433734,147.48411349278294,2.0472182408516689E-3,3.3371449556365054,-150570.51765140827,7799.6606254813905,9.39184061038899E-4,0.61674661113134377,-153558.33989379389,12462.657747265937,1.3533972708417745,4.365001357975698E-2,20.371367249397636,-38388.276775047023,733.04021185907857]
["KBM","KBMS-10H03-C (120 V)",1.19,3.05,1.0724594626807715,2.6878683275207305,3250,3.58,4762,5.44,11,24,2.0199999999999999E-2,160,6,4762,4762,4762,1.0177759880879489,5569.3069306930693,8.3341868602117941,8.1270687358212292,8.41408360964125E-2,-22.512229721283951,9,29.094906074240004,9,-2350.6230688000001,7.5,2362.6230688000001,9,1.0584220994892963,1.5535620365271712,25.40213038774311,74.57097775330422,55.855533040948174,23.024622967966629,2.4075399421433734,147.48411349278294,1.3300813298191641E-3,2.074945400814947,-151795.33749289796,9931.3545179129706,5.9747701778112337E-4,0.3501745406040202,-153610.77855517046,15743.942051897709,1.5485092316259543,2.8519369951525229E-2,12.6309777322214,-84418.514552138513,1513.2242604247779]
["KBM","KBMS-10H03-C (240 V)",1.19,3.05,0.94236479462306444,2.3618165278773544,7600,3.58,9983,5.44,11,24,2.0199999999999999E-2,325,6,9931.3545179129706,9983,9983,0.8647181243055333,5569.3069306930693,8.333629836033257,8.1270687358212292,8.41408360964125E-2,-22.512229721283951,9,29.094906074240004,9,-2350.6230688000001,7.5,2362.6230688000001,9,1.0584220994892963,1.5535620365271712,25.40213038774311,74.57097775330422,55.855533040948174,23.024622967966629,2.4075399421433734,147.48411349278294,1.3300813298191641E-3,2.074945400814947,-151795.33749289796,9931.3545179129706,6.0598850183207103E-4,0.41378521054568701,-153589.6865449365,15582.458591118722,1.8298024103495585,2.8519369951525229E-2,12.6309777322214,-84418.514552138513,1513.2242604247779]
["KBM","KBMS-10H03-C (400 V)",1.19,3.05,0.47746482927568601,1.1966537074578596,14500,3.58,16000,5.44,11,24,2.0199999999999999E-2,565,6,9931.3545179129706,15860.287787619554,16000,0.41061980231115502,5569.3069306930693,8.3362046137560029,8.1270687358212292,8.41408360964125E-2,-22.512229721283951,9,29.094906074240004,9,-2350.6230688000001,7.5,2362.6230688000001,9,1.0584220994892963,1.5535620365271712,25.40213038774311,74.57097775330422,55.855533040948174,23.024622967966625,2.4075399421433734,147.48411349278294,1.3300813298191641E-3,2.074945400814947,-151795.33749289796,9931.3545179129706,5.9178687787578017E-4,0.30022420529412086,-153624.87909138695,15860.287787619554,1.3276235121308375,2.8519369951525229E-2,12.6309777322214,-84418.514552138513,1513.2242604247779]
["KBM","KBMS-10H03-D (120 V)",1.18,4.66,1.0070167308359925,3.888095485853253,5500,15.5,7333,2.34,4.7,15.7,2.0199999999999999E-2,160,6,4362.3892199889115,7333,7333,0.94936612494915151,5569.3069306930693,8.4041181195626233,1.877090714467097,4.324543042662269E-2,-22.512229721283951,9,29.094906074240004,9,-2350.6230688000001,7.5,2362.6230688000001,9,1.6308346514331602,2.3937546311080236,39.140031634395847,114.90022229318512,86.063148909495425,23.024622967966625,2.4075399421433734,147.48411349278294,6.3732086860845052E-3,3.895038410101912,-138276.63721026285,4362.3892199889115,2.5131691137003095E-4,0.10932826023173861,-153651.87712636893,24509.685810481686,1.7181311033487874,1.2357801911316328E-2,5.4763773975111461,-123246.22503958481,2944.2175327530854]
["KBM","KBMS-10H03-D (240 V)",1.18,4.66,0.62437708443743556,2.4107223337352726,13000,15.5,15373,2.34,4.7,15.7,2.0199999999999999E-2,325,6,4362.3892199889115,15373,15373,0.52295453223513055,5569.3069306930693,8.4059033021496976,1.877090714467097,4.324543042662269E-2,-22.512229721283951,9,29.094906074240004,9,-2350.6230688000001,7.5,2362.6230688000001,9,1.6308346514331602,2.3937546311080236,39.140031634395847,114.90022229318512,86.063148909495425,23.024622967966629,2.4075399421433734,147.48411349278294,6.3732086860845052E-3,3.895038410101912,-138276.63721026285,4362.3892199889115,2.4823556411030754E-4,6.5745446151779158E-2,-153659.61598473601,24747.783383157002,1.033212233483634,1.2357801911316328E-2,5.4763773975111461,-123246.22503958481,2944.2175327530854]
["KBM","KBMS-10H04-A (120 V)",1.44,1.6,1.3285977858106046,1.4285997696888222,1150,4.66,2022,20.399999999999999,44,56.2,2.5499999999999998E-2,160,6,2022,2022,2022,1.244125846007863,4411.7647058823532,6.8929875006455328,6.2437755162231756,"NA",-22.513572722962962,9,29.0959939056,9,-2350.7340719999997,7.5,2362.7340719999997,9,0.45884665128239871,0.67351837744444454,11.012319630777569,32.328882117333336,24.215007850759307,23.024837934580031,2.4077260324168588,147.49551324509201,7.0004029838826405E-3,10.281832335505445,-145296.25546666665,3880.2457845585423,3.2467208620977754E-3,1.5585732290054541,-153471.72545068353,6639.4666855984187,0.78487428766140122,8.7188677326653641E-2,48.085232972534264,29352.744818873965,-9999]
["KBM","KBMS-10H04-A (240 V)",1.44,1.6,1.2891550390443522,1.3861882140261852,3000,4.66,4251,20.399999999999999,44,56.2,2.5499999999999998E-2,325,6,3880.2457845585423,4251,4251,1.2262526903258473,4411.7647058823532,6.8880358340229417,6.2437755162231756,"NA",-22.513572722962962,9,29.0959939056,9,-2350.7340719999997,7.5,2362.7340719999997,9,0.45884665128239871,0.67351837744444454,11.012319630777569,32.328882117333336,24.215007850759307,23.024837934580031,2.4077260324168588,147.49551324509201,7.0004029838826405E-3,10.281832335505445,-145296.25546666665,3880.2457845585423,3.3683309970382953E-3,2.403205087782319,-153206.86018620405,6396.912812400049,1.2102183242176054,8.7188677326653641E-2,48.085232972534264,29352.744818873965,-9999]
["KBM","KBMS-10H04-A (400 V)",1.44,1.6,1.1791305349069114,1.2678822955988294,5750,4.66,7109,20.399999999999999,44,56.2,2.5499999999999998E-2,565,6,3880.2457845585423,6351.5911283913847,6975.0889679715301,1.1518371860602665,4411.7647058823532,6.8875140791781542,6.2437755162231756,"NA",-22.513572722962962,9,29.0959939056,9,-2350.7340719999997,7.5,2362.7340719999997,9,0.45884665128239871,0.67351837744444454,11.012319630777569,32.328882117333336,24.215007850759307,23.024837934580031,2.4077260324168588,147.49551324509201,7.0004029838826405E-3,10.281832335505445,-145296.25546666665,3880.2457845585423,3.3947440386239078E-3,2.5499372986951294,-153149.33293118782,6351.5911283913847,1.2841104823619254,8.7188677326653641E-2,48.085232972534264,29352.744818873965,-9999]
["KBM","KBMS-10H04-A (480 V)",1.44,1.6,1.1106983262583334,1.1942992755465951,7050,4.66,8541,20.399999999999999,44,56.2,2.5499999999999998E-2,679,6,3880.2457845585423,6350.8688602603361,6975.0889679715301,1.1433543623549562,4411.7647058823532,6.8876564670490206,6.2437755162231756,"NA",-22.513572722962962,9,29.0959939056,9,-2350.7340719999997,7.5,2362.7340719999997,9,0.45884665128239871,0.67351837744444454,11.012319630777569,32.328882117333336,24.215007850759307,23.024837934580031,2.4077260324168588,147.49551324509201,7.0004029838826405E-3,10.281832335505445,-145296.25546666665,3880.2457845585423,3.3951737718109568E-3,2.5522548531256102,-153148.39697799363,6350.8688602603361,1.2852775682895472,8.7188677326653641E-2,48.085232972534264,29352.744818873965,-9999]
["KBM","KBMS-10H04-B (120 V)",1.41,2.4,1.2732395447351628,2.1115083660616301,2100,4.75,3131,9.02,19,36.4,2.5499999999999998E-2,160,6,3131,3131,3131,1.2060966736027594,4411.7647058823532,7.0363504050273153,6.1254724011789472,0.11535473167912645,-22.513572722962962,9,29.0959939056,9,-2350.7340719999997,7.5,2362.7340719999997,9,0.70291401898580208,1.031772833531915,16.86993645565925,49.525096009531914,37.095331175631273,23.024837934580031,2.4077260324168588,147.49551324509201,3.0717459418121767E-3,4.5978445844263867,-149675.16735174286,6272.0276700584254,1.3633441210829955E-3,0.68156965042168161,-153576.3488278182,10366.500175523484,1.1985100909530624,3.8096067971800991E-2,21.095401776339056,-69696.186612205449,1103.7601372753716]
["KBM","KBMS-10H04-B (240 V)",1.41,2.4,1.1888682496021099,1.971589136985257,4980,4.75,6571,9.02,19,36.4,2.5499999999999998E-2,325,6,6272.0276700584254,6571,6571,1.1182215397862378,4411.7647058823532,7.0340547768878263,6.1254724011789472,0.11535473167912645,-22.513572722962962,9,29.0959939056,9,-2350.7340719999997,7.5,2362.7340719999997,9,0.70291401898580208,1.031772833531915,16.86993645565925,49.525096009531914,37.095331175631273,23.024837934580031,2.4077260324168588,147.49551324509201,3.0717459418121767E-3,4.5978445844263867,-149675.16735174286,6272.0276700584254,1.3975007832171147E-3,0.93696973579545961,-153498.35117177185,10150.480566385038,1.6476198471773387,3.8096067971800991E-2,21.095401776339056,-69696.186612205449,1103.7601372753716]
["KBM","KBMS-10H04-B (400 V)",1.41,2.4,0.90467020283814192,1.5002822600964212,9500,4.75,10987,9.02,19,36.4,2.5499999999999998E-2,565,6,6272.0276700584254,10189.064900965408,10769.23076923077,0.86801704213959396,4411.7647058823532,7.0350283101640869,6.1254724011789472,0.11535473167912645,-22.513572722962962,9,29.0959939056,9,-2350.7340719999997,7.5,2362.7340719999997,9,0.70291401898580208,1.031772833531915,16.86993645565925,49.525096009531914,37.095331175631273,23.024837934580031,2.4077260324168588,147.49551324509201,3.0717459418121767E-3,4.5978445844263867,-149675.16735174286,6272.0276700584254,1.3909694684274138E-3,0.89379425926185718,-153513.26560464289,10189.064900965408,1.5716976809317984,3.8096067971800991E-2,21.095401776339056,-69696.186612205449,1103.7601372753716]
["KBM","KBMS-10H04-B (480 V)",1.41,2.4,0.71412130987319988,1.1842807792258705,11500,4.75,13200,9.02,19,36.4,2.5499999999999998E-2,679,6,6272.0276700584254,10236.830756836338,10769.23076923077,0.79055718451156431,4411.7647058823532,7.0358392075697562,6.1254724011789472,0.11535473167912645,-22.513572722962962,9,29.0959939056,9,-2350.7340719999997,7.5,2362.7340719999997,9,0.70291401898580208,1.031772833531915,16.86993645565925,49.525096009531914,37.095331175631273,23.024837934580031,2.4077260324168588,147.49551324509201,3.0717459418121767E-3,4.5978445844263867,-149675.16735174286,6272.0276700584254,1.3831305431620958E-3,0.83904644704639286,-153531.16600118094,10236.830756836338,1.4754260741235412,3.8096067971800991E-2,21.095401776339056,-69696.186612205449,1103.7601372753716]
["KBM","KBMS-10H04-C (120 V)",1.44,3.1,1.308607309866695,2.726265228888948,2700,4.8,3944,5.44,11.8,29,2.5499999999999998E-2,160,6,3944,3944,3944,1.2480693444867574,4411.7647058823532,6.8878640298341569,6.0616653970000005,6.8613395345796913E-2,-22.513572722962962,9,29.0959939056,9,-2350.7340719999997,7.5,2362.7340719999997,9,0.88901538685964743,1.3049418562986113,21.336369284631537,62.637209102333337,46.916577710846155,23.024837934580031,2.4077260324168588,147.49551324509201,1.9415401765434858E-3,2.8235661324880161,-151294.04586666665,8130.2519753706019,8.6600671035342983E-4,0.42562124246199406,-153610.14939297418,13074.845403846019,1.557635261842389,2.3528031503813617E-2,12.819876762250388,-104808.69673029502,1855.6719694722967]
["KBM","KBMS-10H04-C (240 V)",1.44,3.1,1.1519786357127662,2.3999554910682628,6300,4.8,8273,5.44,11.8,29,2.5499999999999998E-2,325,6,8130.2519753706019,8273,8273,1.061777659246304,4411.7647058823532,6.8875511474606066,6.0616653970000005,6.8613395345796913E-2,-22.513572722962962,9,29.0959939056,9,-2350.7340719999997,7.5,2362.7340719999997,9,0.88901538685964743,1.3049418562986113,21.336369284631537,62.637209102333337,46.916577710846155,23.024837934580031,2.4077260324168588,147.49551324509201,1.9415401765434858E-3,2.8235661324880161,-151294.04586666665,8130.2519753706019,8.7672855735160238E-4,0.50874804525693984,-153587.0604715955,12948.673366502098,1.8618523128726556,2.3528031503813617E-2,12.819876762250388,-104808.69673029502,1855.6719694722967]
["KBM","KBMS-10H04-C (400 V)",1.44,3.1,0.66845076098596046,1.3926057520540844,12000,4.8,13833,5.44,11.8,29,2.5499999999999998E-2,565,6,8130.2519753706019,13091.75950708416,13517.241379310346,0.59825524291286669,4411.7647058823532,6.8895245357198904,6.0616653970000005,6.8613395345796913E-2,-22.513572722962962,9,29.0959939056,9,-2350.7340719999997,7.5,2362.7340719999997,9,0.88901538685964743,1.3049418562986113,21.336369284631537,62.637209102333337,46.916577710846155,23.024837934580031,2.4077260324168588,147.49551324509201,1.9415401765434858E-3,2.8235661324880161,-151294.04586666665,8130.2519753706019,8.6464387787398597E-4,0.41386087058748855,-153613.08417948769,13091.75950708416,1.5145961272866342,2.3528031503813617E-2,12.819876762250388,-104808.69673029502,1855.6719694722967]
["KBM","KBMS-10H04-D (120 V)",1.41,4.21,1.2277667038517641,3.5484586816524977,4200,4.91,5489,2.94,6.2,20.9,2.5499999999999998E-2,160,6,5489,5489,5489,1.1718384374862698,4411.7647058823532,7.0339423514292783,5.9258643392260693,4.3690477406760922E-2,-22.513572722962962,9,29.0959939056,9,-2350.7340719999997,7.5,2362.7340719999997,9,1.2330283416375944,1.8099015121539006,29.592680199302269,86.875272583387229,65.071393437253192,23.024837934580031,2.4077260324168588,147.49551324509201,1.048361926170838E-3,1.5602662671762528,-152270.69923737546,11330.624690495149,4.4543386133887215E-4,0.18528187306995139,-153644.35222837829,18365.527954287223,1.74091949505085,1.2485077501648218E-2,6.9253918366706895,-126214.3925668912,2914.2266697642772]
["KBM","KBMS-10H04-D (240 V)",1.41,4.21,0.909696148409465,2.629179619680535,9500,4.91,11509,2.94,6.2,20.9,2.5499999999999998E-2,325,6,11330.624690495149,11509,11509,0.80389504968889824,4411.7647058823532,7.0349696991042405,5.9258643392260693,4.3690477406760922E-2,-22.513572722962962,9,29.0959939056,9,-2350.7340719999997,7.5,2362.7340719999997,9,1.2330283416375944,1.8099015121539006,29.592680199302269,86.875272583387229,65.071393437253192,23.024837934580031,2.4077260324168588,147.49551324509201,1.048361926170838E-3,1.5602662671762528,-152270.69923737546,11330.624690495149,4.44108144463453E-4,0.17044657463181917,-153647.37261349114,18409.317377867999,1.6015261489133623,1.2485077501648218E-2,6.9253918366706895,-126214.3925668912,2914.2266697642772]
["KBM","KBMS-14H01-A (120 V)",1.2,1.53,1.1018419137131217,1.3519532683596587,1300,3.28,2308,21.4,38,49.3,3.3599999999999998E-2,160,8,2308,2308,2308,1.0257316437306807,3348.2142857142858,8.270903617696538,8.8712367196097563,"NA",-22.515625234962965,9,29.097656440320002,9,-2350.9037184000003,7.5,2362.9037184000003,9,0.52653404554007366,0.77290649919600007,12.636817092961767,37.099511961408005,27.788070971901927,23.025166484145092,2.4080104345329412,147.51293550805499,5.7538220217480916E-3,7.6419703522315059,-147657.01057971999,4445.0730180362134,2.5174324218753372E-3,1.2360451909651493,-153506.84982512702,7567.1729183710268,0.67641468762134505,0.14916169160119641,50.778482666900878,111555.59583795373,-9999]
["KBM","KBMS-14H01-A (240 V)",1.2,1.53,1.083203791789616,1.3290844071038235,3350,3.28,4849,21.4,38,49.3,3.3599999999999998E-2,325,8,4445.0730180362134,4849,4849,1.0309418466829396,3348.2142857142858,8.2646848828845751,8.8712367196097563,"NA",-22.515625234962965,9,29.097656440320002,9,-2350.9037184000003,7.5,2362.9037184000003,9,0.52653404554007366,0.77290649919600007,12.636817092961767,37.099511961408005,27.788070971901927,23.025166484145092,2.4080104345329412,147.51293550805499,5.7538220217480916E-3,7.6419703522315059,-147657.01057971999,4445.0730180362134,2.6845175235373957E-3,2.1128023417985262,-153204.8401458647,7171.1807961759523,1.1562122052490484,0.14916169160119641,50.778482666900878,111555.59583795373,-9999]
["KBM","KBMS-14H01-A (400 V)",1.2,1.53,0.9698504344662372,1.1900005330874077,6400,3.28,8109,21.4,38,49.3,3.3599999999999998E-2,565,8,4445.0730180362134,7132.6008691266979,7951.3184584178498,0.94350547013199249,3348.2142857142858,8.2648525136652573,8.8712367196097563,"NA",-22.515625234962965,9,29.097656440320002,9,-2350.9037184000003,7.5,2362.9037184000003,9,0.52653404554007366,0.77290649919600007,12.636817092961767,37.099511961408005,27.788070971901927,23.025166484145092,2.4080104345329412,147.51293550805499,5.7538220217480916E-3,7.6419703522315059,-147657.01057971999,4445.0730180362134,2.7036229891806616E-3,2.1908142707132536,-153170.30663274063,7132.6008691266979,1.1989035363697096,0.14916169160119641,50.778482666900878,111555.59583795373,-9999]
["KBM","KBMS-14H01-A (480 V)",1.2,1.53,0.89449107256710791,1.0975350583645496,7900,3.28,9741,21.4,38,49.3,3.3599999999999998E-2,679,8,4445.0730180362134,7141.7496191269238,7951.3184584178498,0.92381414352737568,3348.2142857142858,8.2652670819831577,8.8712367196097563,"NA",-22.515625234962965,9,29.097656440320002,9,-2350.9037184000003,7.5,2362.9037184000003,9,0.52653404554007366,0.77290649919600007,12.636817092961767,37.099511961408005,27.788070971901927,23.025166484145092,2.4080104345329412,147.51293550805499,5.7538220217480916E-3,7.6419703522315059,-147657.01057971999,4445.0730180362134,2.699049099649355E-3,2.1723931189756565,-153178.57402999263,7141.7496191269238,1.1888227256604482,0.14916169160119641,50.778482666900878,111555.59583795373,-9999]
["KBM","KBMS-14H01-B (120 V)",1.25,3.25,1.1186318857316073,2.8391672226690541,3500,3.43,5022,4.74,9,23.7,3.3599999999999998E-2,160,8,5022,5022,5022,1.0615055228983235,3348.2142857142858,7.934268912551433,8.4832817610262392,8.2645236537764011E-2,-22.515625234962965,9,29.097656440320002,9,-2350.9037184000003,7.5,2362.9037184000003,9,1.0737164850228951,1.5761230571839999,25.769195640549484,75.653906744832,56.665870217211769,23.025166484145092,2.4080104345329412,147.51293550805499,1.4094217263012007E-3,1.7352209524491575,-152323.8516290932,9798.5633729420624,5.904412583365166E-4,0.31956116301099619,-153618.54817741772,15861.624739946792,1.6423536424624663,3.4788515927275387E-2,11.025768702586966,-99556.05100547176,1540.6085070049587]
["KBM","KBMS-14H01-B (240 V)",1.25,3.25,0.93691211782398764,2.377949537624334,7950,3.43,10088,4.74,9,23.7,3.3599999999999998E-2,325,8,9798.5633729420624,10088,10088,0.85271313768658952,3348.2142857142858,7.9345293897271434,8.4832817610262392,8.2645236537764011E-2,-22.515625234962965,9,29.097656440320002,9,-2350.9037184000003,7.5,2362.9037184000003,9,1.0737164850228951,1.5761230571839999,25.769195640549484,75.653906744832,56.665870217211769,23.025166484145092,2.4080104345329412,147.51293550805499,1.4094217263012007E-3,1.7352209524491575,-152323.8516290932,9798.5633729420624,5.9424651016313861E-4,0.34005133741149479,-153612.53259267774,15794.351138401822,1.747660908978429,3.4788515927275387E-2,11.025768702586966,-99556.05100547176,1540.6085070049587]
["KBM","KBMS-14H01-B (400 V)",1.25,3.25,0.56102117439893107,1.4239116101495712,12000,3.43,12000,4.74,9,23.7,3.3599999999999998E-2,565,8,9798.5633729420624,12000,12000,0.56102117439893107,3348.2142857142858,7.9370715049864078,8.4832817610262392,8.2645236537764011E-2,-22.515625234962965,9,29.097656440320002,9,-2350.9037184000003,7.5,2362.9037184000003,9,1.0737164850228951,1.5761230571839999,25.769195640549484,75.653906744832,56.665870217211769,23.025166484145092,2.4080104345329412,147.51293550805499,1.4094217263012007E-3,1.7352209524491575,-152323.8516290932,9798.5633729420624,5.7617741086241493E-4,0.22684068655054646,-153641.09737707867,16133.938252500984,1.165825735219761,3.4788515927275387E-2,11.025768702586966,-99556.05100547176,1540.6085070049587]
["KBM","KBMS-14H01-C (120 V)",1.21,6.25,0.91036627448564134,4.5747048969127704,7500,3.59,9539,1.29,2.4,12.1,3.3599999999999998E-2,160,8,9539,9539,9539,0.82890585230913771,3348.2142857142858,8.1971030098424311,8.1051967800334275,3.5301199520312951E-2,-22.515625234962965,9,29.097656440320002,9,-2350.9037184000003,7.5,2362.9037184000003,9,2.1330985478045439,3.1312044206611573,51.194365147309057,150.29781219173555,112.57523485618995,23.025166484145092,2.4080104345329412,147.51293550805499,4.070488535243762E-4,0.50133128093326429,-153234.84035714401,18796.35970087838,1.4642132823273831E-4,3.3051129574138867E-3,-153663.98134729243,32384.154657159346,0.12225048726151755,9.7525008295394327E-3,3.043536886778754,-137846.91649958523,3606.7883302450318]
["KBM","KBMS-14H01-C (240 V)",1.21,6.25,0.64723010190704111,3.2524125723971915,13500,3.59,12000,1.29,2.4,12.1,3.3599999999999998E-2,325,8,12000,12000,12000,0.70976009058403655,3348.2142857142858,8.1973640511780026,8.1051967800334275,3.5301199520312951E-2,-22.515625234962965,9,29.097656440320002,9,-2350.9037184000003,7.5,2362.9037184000003,9,2.1330985478045439,3.1312044206611573,51.194365147309057,150.29781219173555,112.57523485618995,23.025166484145092,2.4080104345329412,147.51293550805499,4.070488535243762E-4,0.50133128093326429,-153234.84035714401,18796.35970087838,1.4642909359909777E-4,4.2909072292890878E-3,-153663.96856108727,32379.930138514974,0.15871333486435812,9.7525008295394327E-3,3.043536886778754,-137846.91649958523,3606.7883302450318]
["KBM","KBMS-14H02-A (120 V)",2.08,1.59,1.9757165349338732,1.4634937295806467,725,6.67,1461,23.8,47,80.8,5.5600000000000004E-2,160,8,1461,1461,1461,1.8698508379839844,2023.3812949640287,4.7725208611952361,4.363144222896552,0.32115167812941214,-22.521199958913581,9,29.10217196672,9,-2351.3644863999998,7.5,2363.3644863999998,9,0.31569441242574786,0.46346607999884615,7.5766658982179491,22.246371839944615,16.662466262048149,23.026058936671546,2.408782884724769,147.56025523462102,1.4085709989137867E-2,16.982771584944864,-142619.79589675603,2635.7666629768173,6.7841183528351712E-3,3.1225463957515189,-153290.63372487912,4528.9049768064124,0.93747556064576687,8.723592986045213E-2,55.49939236287937,-35715.141101024303,396.46049871241672]
["KBM","KBMS-14H02-A (240 V)",2.08,1.59,1.8621128341751756,1.3793428401297596,2000,6.67,2944,23.8,47,80.8,5.5600000000000004E-2,325,8,2635.7666629768173,2944,2944,1.7592700919058584,2023.3812949640287,4.770742419020281,4.363144222896552,0.32115167812941214,-22.521199958913581,9,29.10217196672,9,-2351.3644863999998,7.5,2363.3644863999998,9,0.31569441242574786,0.46346607999884615,7.5766658982179491,22.246371839944615,16.662466262048149,23.026058936671546,2.408782884724769,147.56025523462102,1.4085709989137867E-2,16.982771584944864,-142619.79589675603,2635.7666629768173,6.9445318265932143E-3,3.9840248528763875,-153056.19906334486,4416.5670559745931,1.1961154324748013,8.723592986045213E-2,55.49939236287937,-35715.141101024303,396.46049871241672]
["KBM","KBMS-14H02-A (400 V)",2.08,1.59,1.7384616860807027,1.2877493970968168,3900,6.67,4924,23.8,47,80.8,5.5600000000000004E-2,565,8,2635.7666629768173,4369.3869483216858,4851.4851485148511,1.6973556278998019,2023.3812949640287,4.7696539785849135,4.363144222896552,0.32115167812941214,-22.521199958913581,9,29.10217196672,9,-2351.3644863999998,7.5,2363.3644863999998,9,0.31569441242574786,0.46346607999884615,7.5766658982179491,22.246371839944615,16.662466262048149,23.026058936671546,2.408782884724769,147.56025523462102,1.4085709989137867E-2,16.982771584944864,-142619.79589675603,2635.7666629768173,7.0200483352117465E-3,4.3306501974841325,-152945.83621960433,4369.3869483216858,1.3001820332824954,8.723592986045213E-2,55.49939236287937,-35715.141101024303,396.46049871241672]
["KBM","KBMS-14H02-A (480 V)",2.08,1.59,1.6370222718023522,1.2126090902239646,4900,6.67,5915,23.8,47,80.8,5.5600000000000004E-2,679,8,2635.7666629768173,4368.5616921439205,4851.4851485148511,1.6850662175760844,2023.3812949640287,4.7697980773383755,4.363144222896552,0.32115167812941214,-22.521199958913581,9,29.10217196672,9,-2351.3644863999998,7.5,2363.3644863999998,9,0.31569441242574786,0.46346607999884615,7.5766658982179491,22.246371839944615,16.662466262048149,23.026058936671546,2.408782884724769,147.56025523462102,1.4085709989137867E-2,16.982771584944864,-142619.79589675603,2635.7666629768173,7.021410656907384E-3,4.3366489311474909,-152943.84526823263,4368.5616921439205,1.3019830205190257,8.723592986045213E-2,55.49939236287937,-35715.141101024303,396.46049871241672]
["KBM","KBMS-14H02-B (120 V)",2.08,2.42,1.909859317102744,2.1702946785258455,1350,6.83,2139,10.3,20,53.4,5.5600000000000004E-2,160,8,2139,2139,2139,1.8104215402094588,2023.3812949640287,4.7716130616399921,4.2609329380263548,9.2667738151919907E-2,-22.521199958913581,9,29.10217196672,9,-2351.3644863999998,7.5,2363.3644863999998,9,0.4804908667108867,0.70540120352025637,11.531780801061281,33.859257768972306,25.360483241607874,23.026058936671546,2.408782884724769,147.56025523462102,6.1754293340383886E-3,7.5702782718222004,-148639.63499340508,4331.2745887798419,2.9444817851330971E-3,1.2657520652780609,-153523.53931437919,7009.0242682484886,1.3286467685095329,3.6705835397766007E-2,24.159983526339722,-102489.83533285229,1373.9836216222393]
["KBM","KBMS-14H02-B (240 V)",2.08,2.42,1.7941102675813656,2.0387616677060971,3300,6.83,4489,10.3,20,53.4,5.5600000000000004E-2,325,8,4331.2745887798419,4489,4489,1.6911033306584091,2023.3812949640287,4.7696060777593825,4.2609329380263548,9.2667738151919907E-2,-22.521199958913581,9,29.10217196672,9,-2351.3644863999998,7.5,2363.3644863999998,9,0.4804908667108867,0.70540120352025637,11.531780801061281,33.859257768972306,25.360483241607874,23.026058936671546,2.408782884724769,147.56025523462102,6.1754293340383886E-3,7.5702782718222004,-148639.63499340508,4331.2745887798419,3.0106265293973144E-3,1.6560722317400691,-153423.55483693659,6868.9330114414306,1.7383617846489097,3.6705835397766007E-2,24.159983526339722,-102489.83533285229,1373.9836216222393]
["KBM","KBMS-14H02-B (400 V)",2.08,2.42,1.382510102678852,1.5710342075896044,6700,6.83,7505,10.3,20,53.4,5.5600000000000004E-2,565,8,4331.2745887798419,6892.4685496652119,7340.8239700374534,1.3624735550753386,2023.3812949640287,4.7704958240838193,4.2609329380263548,9.2667738151919907E-2,-22.521199958913581,9,29.10217196672,9,-2351.3644863999998,7.5,2363.3644863999998,9,0.4804908667108867,0.70540120352025637,11.531780801061281,33.859257768972306,25.360483241607874,23.026058936671546,2.408782884724769,147.56025523462102,6.1754293340383886E-3,7.5702782718222004,-148639.63499340508,4331.2745887798419,2.9987787850372545E-3,1.5932043630486481,-153441.46390200124,6892.4685496652119,1.6723700372354156,3.6705835397766007E-2,24.159983526339722,-102489.83533285229,1373.9836216222393]
["KBM","KBMS-14H02-B (480 V)",2.08,2.42,1.2401683877290546,1.4092822587830165,7700,6.83,9016,10.3,20,53.4,5.5600000000000004E-2,679,8,4331.2745887798419,6901.9430903502298,7340.8239700374534,1.3272116891725787,2023.3812949640287,4.7707488105370013,4.2609329380263548,9.2667738151919907E-2,-22.521199958913581,9,29.10217196672,9,-2351.3644863999998,7.5,2363.3644863999998,9,0.4804908667108867,0.70540120352025637,11.531780801061281,33.859257768972306,25.360483241607874,23.026058936671546,2.408782884724769,147.56025523462102,6.1754293340383886E-3,7.5702782718222004,-148639.63499340508,4331.2745887798419,2.994089431561812E-3,1.5676248849138976,-153448.55233452906,6901.9430903502298,1.6455195252779806,3.6705835397766007E-2,24.159983526339722,-102489.83533285229,1373.9836216222393]
["KBM","KBMS-14H02-C (120 V)",2.11,3.1,1.9098593171027443,2.7322737011484182,1800,6.98,2704,6.3,12.8,42.3,5.5600000000000004E-2,160,8,2704,2704,2704,1.8093442185810114,2023.3812949640287,4.7029453451423011,4.1693656112779367,6.4256238920509579E-2,-22.521199958913581,9,29.10217196672,9,-2351.3644863999998,7.5,2363.3644863999998,9,0.60675357576119182,0.89076553215671417,14.562085818268605,42.756745543522278,32.024675089477029,23.02605893667155,2.408782884724769,147.56025523462102,4.0566879184936264E-3,4.7334326853383857,-150533.51458586511,5536.054700105693,1.8412399312701772E-3,0.71648123781986828,-153592.27527061742,8940.8445224476582,1.552255752653448,2.3901282876699976E-2,14.781764415860568,-123135.05286929426,1981.5033779214314]
["KBM","KBMS-14H02-C (240 V)",2.11,3.1,1.7301078519636623,2.4751185292756257,4250,6.98,5671,6.3,12.8,42.3,5.5600000000000004E-2,325,8,5536.054700105693,5671,5671,1.6030897949378657,2023.3812949640287,4.7018661788818763,4.1693656112779367,6.4256238920509579E-2,-22.521199958913581,9,29.10217196672,9,-2351.3644863999998,7.5,2363.3644863999998,9,0.60675357576119182,0.89076553215671417,14.562085818268605,42.756745543522278,32.024675089477029,23.026058936671546,2.408782884724769,147.56025523462102,4.0566879184936264E-3,4.7334326853383857,-150533.51458586511,5536.054700105693,1.8743352297453885E-3,0.91672128017134991,-153546.58221060882,8809.7547910769063,1.9860755671086621,2.3901282876699976E-2,14.781764415860568,-123135.05286929426,1981.5033779214314]
["KBM","KBMS-14H02-C (400 V)",2.11,3.1,1.2055986939211072,1.7247477738499388,8000,6.98,9481,6.3,12.8,42.3,5.5600000000000004E-2,565,8,5536.054700105693,8868.5444085571617,9267.1394799054378,1.1074096067352801,2023.3812949640287,4.7030374758748952,4.1693656112779367,6.4256238920509579E-2,-22.521199958913581,9,29.10217196672,9,-2351.3644863999998,7.5,2363.3644863999998,9,0.60675357576119182,0.89076553215671417,14.562085818268605,42.756745543522278,32.024675089477029,23.026058936671546,2.408782884724769,147.56025523462102,4.0566879184936264E-3,4.7334326853383857,-150533.51458586511,5536.054700105693,1.8589609596233233E-3,0.82973274517109807,-153567.8087134549,8868.5444085571617,1.7976150091184686,2.3901282876699976E-2,14.781764415860568,-123135.05286929426,1981.5033779214314]
["KBM","KBMS-14H02-C (480 V)",2.11,3.1,0.5496668278490825,0.78636169935491063,10250,6.98,11390,6.3,12.8,42.3,5.5600000000000004E-2,679,8,5536.054700105693,8985.8900392516189,9267.1394799054378,0.74209928687367688,2023.3812949640287,4.7049779445306861,4.1693656112779367,6.4256238920509579E-2,-22.521199958913581,9,29.10217196672,9,-2351.3644863999998,7.5,2363.3644863999998,9,0.60675357576119182,0.89076553215671417,14.562085818268605,42.756745543522278,32.024675089477029,23.026058936671546,2.408782884724769,147.56025523462102,4.0566879184936264E-3,4.7334326853383857,-150533.51458586511,5536.054700105693,1.830941692471891E-3,0.64154726836249387,-153606.4935452689,8985.8900392516189,1.3899113966263463,2.3901282876699976E-2,14.781764415860568,-123135.05286929426,1981.5033779214314]
["KBM","KBMS-14H02-D (120 V)",2.1749999999999998,5.97,1.8608885653821607,4.975637875353371,3900,7.31,5084,1.69,3.6,22.6,5.5600000000000004E-2,160,8,5084,5084,5084,1.7655275554879244,2023.3812949640287,4.560810536288785,3.9811452758850892,2.8884510276366238E-2,-22.521199958913581,9,29.10217196672,9,-2351.3644863999998,7.5,2363.3644863999998,9,1.1335695614076389,1.6641759256831266,27.205669473783335,79.880444432790071,59.830215009212495,23.026058936671546,2.408782884724769,147.56025523462102,1.1973672377044277E-3,1.3273584470053374,-152801.61823222431,10755.974003784639,5.1937914218352856E-4,0.14871886142139226,-153653.17431878843,17057.428742948701,2.2480723327018768,6.6157451323324429E-3,3.9580049651129929,-145996.11131262282,4408.0357691816134]
["KBM","KBMS-14H02-D (240 V)",2.1749999999999998,5.97,1.1051433127055206,2.9549286435976487,8900,7.31,10660,1.69,3.6,22.6,5.5600000000000004E-2,325,8,10660,10660,10660,0.8935761475776236,2023.3812949640287,4.5626582132990601,3.9811452758850892,2.8884510276366238E-2,-22.521199958913581,9,29.10217196672,9,-2351.3644863999998,7.5,2363.3644863999998,9,1.1335695614076389,1.6641759256831266,27.205669473783335,79.880444432790071,59.830215009212495,23.026058936671546,2.408782884724769,147.56025523462102,1.1973672377044277E-3,1.3273584470053374,-152801.61823222431,10755.974003784639,5.1255064250706639E-4,6.7785760717655755E-2,-153661.75094498586,17248.681473398992,1.0246668900236191,6.6157451323324429E-3,3.9580049651129929,-145996.11131262282,4408.0357691816134]
["KBM","KBMS-14H03-A (120 V)",2.82,1.64,2.5783100780887045,1.4403966916696673,500,10.4,1051,26.6,54,108,8.8099999999999998E-2,160,8,1051,1051,1051,2.3119677841424568,1276.9580022701475,3.5283759125350249,2.7989271760307695,0.20314779039009376,-22.529435346567901,9,29.108842630720002,9,-2352.0451664000002,7.5,2364.0451664000002,9,0.24018877986830336,0.3526780578781088,5.764530716839281,16.928546778149222,12.678995170835798,23.027377588353687,2.4099240043263332,147.63015937613909,2.5701254041447769E-2,30.094982734427266,-134251.53459821941,1773.8287865214879,1.1777763555206391E-2,2.7092844008870518,-153506.67356899669,3497.0226778250926,0.54448833130165464,7.3351287576299773E-2,63.088595035908533,-68355.126037275739,626.75530080353292]
["KBM","KBMS-14H03-A (240 V)",2.82,1.64,2.5464790894703255,1.422614016463869,1500,10.4,2217,26.6,54,108,8.8099999999999998E-2,325,8,1773.8287865214879,2217,2217,2.4157360942371411,1276.9580022701475,3.5200075334384904,2.7989271760307695,0.20314779039009376,-22.529435346567901,9,29.108842630720002,9,-2352.0451664000002,7.5,2364.0451664000002,9,0.24018877986830336,0.3526780578781088,5.764530716839281,16.928546778149222,12.678995170835798,23.027377588353687,2.4099240043263332,147.63015937613909,2.5701254041447769E-2,30.094982734427266,-134251.53459821941,1773.8287865214879,1.2256210949961044E-2,6.181462447849241,-152845.01684683276,3288.2207635724017,1.2422963687870101,7.3351287576299773E-2,63.088595035908533,-68355.126037275739,626.75530080353292]
["KBM","KBMS-14H03-A (400 V)",2.82,1.64,2.4124538742350454,1.3477395945447181,2850,10.4,3710,26.6,54,108,8.8099999999999998E-2,565,8,1773.8287865214879,3250.367444687759,3629.6296296296296,2.3552018738964802,1276.9580022701475,3.5189166166208858,2.7989271760307695,0.20314779039009376,-22.529435346567901,9,29.108842630720002,9,-2352.0451664000002,7.5,2364.0451664000002,9,0.24018877986830336,0.3526780578781088,5.764530716839281,16.928546778149222,12.678995170835798,23.027377588353687,2.4099240043263332,147.63015937613909,2.5701254041447769E-2,30.094982734427266,-134251.53459821941,1773.8287865214879,1.2372273201658596E-2,6.7601047214501948,-152684.51149166297,3250.367444687759,1.3585868423417329,7.3351287576299773E-2,63.088595035908533,-68355.126037275739,626.75530080353292]
["KBM","KBMS-14H03-A (480 V)",2.82,1.64,2.3210095867568072,1.2966534004227974,3600,10.4,4458,26.6,54,108,8.8099999999999998E-2,679,8,1773.8287865214879,3243.8940856336185,3629.6296296296296,2.3703688749145924,1276.9580022701475,3.5187949431446119,2.7989271760307695,0.20314779039009376,-22.529435346567901,9,29.108842630720002,9,-2352.0451664000002,7.5,2364.0451664000002,9,0.24018877986830336,0.3526780578781088,5.764530716839281,16.928546778149222,12.678995170835798,23.027377588353687,2.4099240043263332,147.63015937613909,2.5701254041447769E-2,30.094982734427266,-134251.53459821941,1773.8287865214879,1.2392947278849141E-2,6.8580568075376585,-152655.92079956675,3243.8940856336185,1.3782723976432794,7.3351287576299773E-2,63.088595035908533,-68355.126037275739,626.75530080353292]
["KBM","KBMS-14H03-B (120 V)",2.87,2.81,2.6571955716212092,2.5306624491630565,1150,10.4,1789,9.01,19,63.7,8.8099999999999998E-2,160,8,1789,1789,1789,2.5389503283742116,1276.9580022701475,3.4586690879134152,2.7989271760307695,7.1170460857191878E-2,-22.529435346567901,9,29.108842630720002,9,-2352.0451664000002,7.5,2364.0451664000002,9,0.40437323222410337,0.5937561541254589,9.704957573378481,28.500295398022025,21.345902424733797,23.027377588353687,2.4099240043263332,147.63015937613909,8.9833134574440338E-3,10.122379445261004,-147351.13691571791,3525.6325187170551,4.1808368829513399E-3,1.6005296375362674,-153506.17035304374,5871.0334421838224,1.6100481709273635,2.57035439408595E-2,21.219706396154184,-125921.86472481962,1838.7535195000817]
["KBM","KBMS-14H03-B (240 V)",2.87,2.81,2.4794664818526857,2.3613966493835101,2850,10.4,3757,9.01,19,63.7,8.8099999999999998E-2,325,8,3525.6325187170551,3757,3757,2.3551809025686108,1276.9580022701475,3.4573838890810649,2.7989271760307695,6.9244710138275073E-2,-22.529435346567901,9,29.108842630720002,9,-2352.0451664000002,7.5,2364.0451664000002,9,0.40437323222410337,0.5937561541254589,9.704957573378481,28.500295398022025,21.345902424733797,23.027377588353687,2.4099240043263332,147.63015937613909,8.9833134574440338E-3,10.122379445261004,-147351.13691571791,3525.6325187170551,4.2539215581335393E-3,2.0203956968905401,-153412.50230229431,5772.5318953584647,2.0324112219099222,2.57035439408595E-2,21.219706396154184,-125921.86472481962,1838.7535195000817]
["KBM","KBMS-14H03-B (400 V)",2.87,2.81,1.961016263096568,1.8676345362824456,5600,10.4,6283,9.01,19,63.7,8.8099999999999998E-2,565,8,3525.6325187170551,5785.518365878298,6153.8461538461534,1.9309031956893761,1276.9580022701475,3.4580606340838016,2.7989271760307695,6.9244710138275073E-2,-22.529435346567901,9,29.108842630720002,9,-2352.0451664000002,7.5,2364.0451664000002,9,0.40437323222410337,0.5937561541254589,9.704957573378481,28.500295398022025,21.345902424733797,23.027377588353687,2.4099240043263332,147.63015937613909,8.9833134574440338E-3,10.122379445261004,-147351.13691571791,3525.6325187170551,4.2436847330842211E-3,1.9669908144777621,-153425.62219980828,5785.518365878298,1.9786887345340294,2.57035439408595E-2,21.219706396154184,-125921.86472481962,1838.7535195000817]
["KBM","KBMS-14H03-B (480 V)",2.87,2.81,1.7923295129733443,1.7069804885460422,6500,10.4,7549,9.01,19,63.7,8.8099999999999998E-2,679,8,3525.6325187170551,5787.199657967335,6153.8461538461534,1.9105085732427458,1276.9580022701475,3.4581536983371381,2.7989271760307695,6.9244710138275073E-2,-22.529435346567901,9,29.108842630720002,9,-2352.0451664000002,7.5,2364.0451664000002,9,0.40437323222410337,0.5937561541254589,9.704957573378481,28.500295398022025,21.345902424733797,23.027377588353687,2.4099240043263332,147.63015937613909,8.9833134574440338E-3,10.122379445261004,-147351.13691571791,3525.6325187170551,4.2423722079214139E-3,1.9600382096684901,-153427.30438110352,5787.199657967335,1.97169478178625,2.57035439408595E-2,21.219706396154184,-125921.86472481962,1838.7535195000817]
["KBM","KBMS-14H03-C (120 V)",2.92,6.04,2.4828171122335672,4.9855765305894924,3000,10.4,3806,1.96,4.0999999999999996,30,8.8099999999999998E-2,160,8,3806,3806,3806,2.365360643053652,1276.9580022701475,3.3983452370258216,2.7989271760307695,3.3453482520629602E-2,-22.529435346567901,9,29.108842630720002,9,-2352.0451664000002,7.5,2364.0451664000002,9,0.85430325963515663,1.254405033458539,20.503278231243758,60.21144160600987,45.096639856709821,23.027377588353687,2.4099240043263332,147.63015937613909,1.9237196708762545E-3,2.190914249130445,-152330.63743137699,8347.3758060706514,9.1066108621379023E-4,0.22358135478538255,-153650.11427160897,12867.191335960953,2.1953189688966304,5.3987780051849271E-3,4.5928486831684747,-147804.4836037549,4824.2425509484419]
["KBM","KBMS-14H03-C (240 V)",2.92,6.04,1.7796416363911933,3.573577583114846,6600,10.4,7980,1.96,4.0999999999999996,30,8.8099999999999998E-2,325,8,7980,7980,7980,1.5412030694548065,1276.9580022701475,3.3990446993534911,2.7989271760307695,2.6392527558234916E-2,-22.529435346567901,9,29.108842630720002,9,-2352.0451664000002,7.5,2364.0451664000002,9,0.85430325963515663,1.254405033458539,20.503278231243758,60.21144160600987,45.096639856709821,23.027377588353687,2.4099240043263332,147.63015937613909,1.9237196708762545E-3,2.190914249130445,-152330.63743137699,8347.3758060706514,9.0843049702661507E-4,0.19882062994907795,-153653.01954364072,12896.458968349003,1.9521963302984888,5.3987780051849271E-3,4.5928486831684747,-147804.4836037549,4824.2425509484419]
["KBM","KBMS-17H01-A (120 V)",2.08,1.65,1.909859317102744,1.4805110985292589,750,5.95,1460,21.3,66,77.900000000000006,8.6199999999999999E-2,160,10,1460,1460,1460,1.7487928039600082,1305.1044083526683,4.777014575499722,4.8921769165445381,0.3598192098040367,-22.528953893135803,9,29.108452653440004,9,-2352.0053727999998,7.5,2364.0053727999998,9,0.32762507353868453,0.48105916344326927,7.8630017649284287,23.090839845276925,17.294410388932924,23.027300489548558,2.4098572927188568,147.62607267248109,2.6022022275276519E-2,13.564858363011515,-146083.53895630967,2123.005912046563,6.5934349673397261E-3,2.2003637281399651,-153464.54081150936,4660.4783564736599,0.76562620354535271,0.27395927211146981,49.703096815600077,-51891.137213004957,353.8553557017118]
["KBM","KBMS-17H01-A (240 V)",2.08,1.65,1.8853739412424524,1.4615301870096529,1950,5.95,3068,21.3,66,77.900000000000006,8.6199999999999999E-2,325,10,2123.005912046563,3068,3068,1.7737883342214584,1305.1044083526683,4.770534269945947,4.8921769165445381,0.3598192098040367,-22.528953893135803,9,29.108452653440004,9,-2352.0053727999998,7.5,2364.0053727999998,9,0.32762507353868453,0.48105916344326927,7.8630017649284287,23.090839845276925,17.294410388932924,23.027300489548562,2.4098572927188568,147.62607267248109,2.6022022275276519E-2,13.564858363011515,-146083.53895630967,2123.005912046563,7.5170461543337978E-3,3.6549728803868304,-153113.6570454055,4276.6181157833662,1.2717638337173085,0.27395927211146981,49.703096815600077,-51891.137213004957,353.8553557017118]
["KBM","KBMS-17H01-A (400 V)",2.08,1.65,1.7590809499630535,1.363628643382212,3800,5.95,5132,21.3,66,77.900000000000006,8.6199999999999999E-2,565,10,2123.005912046563,4209.0754494756029,5032.0924261874188,1.7245335540053832,1305.1044083526683,4.7697521962598923,4.8921769165445381,0.3598192098040367,-22.528953893135803,9,29.108452653440004,9,-2352.0053727999998,7.5,2364.0053727999998,9,0.32762507353868453,0.48105916344326927,7.8630017649284287,23.090839845276925,17.294410388932924,23.027300489548562,2.4098572927188568,147.62607267248109,2.6022022275276519E-2,13.564858363011515,-146083.53895630967,2123.005912046563,7.7130743779944303E-3,3.8944231839583949,-153039.18510055548,4209.0754494756029,1.3550816163714758,0.27395927211146981,49.703096815600077,-51891.137213004957,353.8553557017118]
["KBM","KBMS-17H01-A (480 V)",2.08,1.65,1.6634258568314222,1.2894774083964513,4650,5.95,6166,21.3,66,77.900000000000006,8.6199999999999999E-2,679,10,{"$f":"IF(AQ891<I891,IF(AQ891<0,0,AQ891),I891)","v":2123.005912046563},{"$f":"IF(AU891<I891,IF(AU891<0,0,AU891),I891)","v":4215.9883150059477},{"$f":"IF(UAC_V*0.98/L891*1000<I891,IF(UAC_V*0.98/L891*1000<0,0,UAC_V*0.98/L891*1000),I891)","v":5032.0924261874188},{"$f":"C891+(E891-C891)/G891*Q891","v":1.7023071570037982},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M891,(inertia/gear^2+gear_inertia)/M891),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M891,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M891))","v":1305.1044083526683},{"$f":"IF((C891+(E891-C891)/G891*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X891^2*time1+Y891^2*time2+Z891^2*time3+AA891^2*time4)/time)/(C891+(E891-C891)/G891*mspeed),SQRT((((X891-Y891)*2/PI()+Y891)^2*time1+Y891^2*time2+((Z891-Y891)*2/PI()+Y891)^2*time3+AA891^2*time4)/time)/(C891+(E891-C891)/G891*mspeed)),IF(AccType=1,SQRT((X891^2*time1+Y891^2*time2+Z891^2*time3+AA891^2*time4+AB891^2*time5+AC891^2*time6+AD891^2*time7+AE891^2*time8)/time)/(C891+(E891-C891)/G891*mspeed),SQRT((((X891-Y891)*2/PI()+Y891)^2*time1+Y891^2*time2+((Z891-Y891)*2/PI()+Y891)^2*time3+AA891^2*time4+((AB891-AC891)*2/PI()+AC891)^2*time5+AC891^2*time6+((AD891-AC891)*2/PI()+AC891)^2*time7+AE891^2*time8)/time)/(C891+(E891-C891)/G891*mspeed))))","v":4.7700136146415471},{"$f":"IF(move1,MAX(ABS(X891),ABS(Z891))/H891,MAX(ABS(X891),ABS(Z891),ABS(AB891),ABS(AD891))/H891)","v":4.8921769165445381},{"$f":"IF(AZ891>0,speed/(MIN(AZ891,I891)),\"NA\")","v":0.3598192098040367},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M891+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M891+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.528953893135803},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M891+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M891+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.108452653440004},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M891+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M891+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2352.0053727999998},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M891+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M891+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2364.0053727999998},9,{"$f":"AH891/Irms","v":0.32762507353868453},{"$f":"AI891/Ipeak","v":0.48105916344326927},{"$f":"IF(move1,IF(AccType=1,SQRT((X891^2*time1+Y891^2*time2+Z891^2*time3+AA891^2*time4)/time)/(C891/D891),SQRT((((X891-Y891)*2/PI()+Y891)^2*time1+Y891^2*time2+((Z891-AA891)*2/PI()+AA891)^2*time3+AA891^2*time4)/time)/(C891/D891)),IF(AccType=1,SQRT((X891^2*time1+Y891^2*time2+Z891^2*time3+AA891^2*time4+AB891^2*time5+AC891^2*time6+AD891^2*time7+AE891^2*time8)/time)/(C891/D891),SQRT((((X891-Y891)*2/PI()+Y891)^2*time1+Y891^2*time2+((Z891-AA891)*2/PI()+AA891)^2*time3+AA891^2*time4+((AB891-AC891)*2/PI()+AC891)^2*time5+AC891^2*time6+((AD891-AE891)*2/PI()+AE891)^2*time7+AE891^2*time8)/time)/(C891/D891)))","v":7.8630017649284287},{"$f":"IF(move1,MAX(ABS(X891),ABS(Z891))/(C891/D891),MAX(ABS(X891),ABS(Z891),ABS(AB891),ABS(AD891))/(C891/D891))","v":23.090839845276925},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X891),ABS(Z891))/(C891/D891),MAX(ABS((X891-Y891)*2/PI()+Y891),ABS((Z891-Y891)*2/PI()+Y891))/(C891/D891)),IF(AccType=1,MAX(ABS(X891),ABS(Z891),ABS(AB891),ABS(AD891))/(C891/D891),MAX(ABS((X891-Y891)*2/PI()+Y891),ABS((Z891-Y891)*2/PI()+Y891),ABS((AB891-AC891)*2/PI()+AC891),ABS((AD891-AC891)*2/PI()+AC891))/(C891/D891)))","v":17.294410388932924},{"$f":"IF((C891+(E891-C891)/G891*mspeed)<0,\"NA\",U891*(C891+(E891-C891)/G891*mspeed)*mspeed/9.55)","v":23.027300489548562},{"$f":"IF(move1,IF(speed1>speed2,AM891/2*time1/time,AM891/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z891*-speed/30*PI(),((Z891-AA891)*2/PI()+AA891)*-speed/30*PI()),IF(AccType=1,X891*-speed/30*PI(),((X891-Y891)*2/PI()+Y891)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z891*-speed/30*PI(),((Z891-AA891)*2/PI()+AA891)*-speed/30*PI()),IF(AccType=1,X891*-speed/30*PI(),((X891-Y891)*2/PI()+Y891)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD891*-speed/30*PI(),((AD891-AE891)*2/PI()+AE891)*-speed/30*PI()),IF(AccType=1,AB891*-speed/30*PI(),((AB891-AC891)*2/PI()+AC891)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD891*-speed/30*PI(),((AD891-AE891)*2/PI()+AE891)*-speed/30*PI()),IF(AccType=1,AB891*-speed/30*PI(),((AB891-AC891)*2/PI()+AC891)*-speed/30*PI()),0)/2*time7/time)))","v":2.4098572927188568},{"$f":"IF(move1,MAX(IF(AccType=1,Z891*-speed/30*PI(),((Z891-AA891)*2/PI()+AA891)*-speed/30*PI()),IF(AccType=1,X891*-speed/30*PI(),((X891-Y891)*2/PI()+Y891)*-speed/30*PI()),0),MAX(IF(AccType=1,Z891*-speed/30*PI(),((Z891-AA891)*2/PI()+AA891)*-speed/30*PI()),IF(AccType=1,X891*-speed/30*PI(),((X891-Y891)*2/PI()+Y891)*-speed/30*PI()),IF(AccType=1,AD891*-speed/30*PI(),((AD891-AE891)*2/PI()+AE891)*-speed/30*PI()),IF(AccType=1,AB891*-speed/30*PI(),((AB891-AC891)*2/PI()+AC891)*-speed/30*PI()),0))","v":147.62607267248109},{"$f":"(L891^2)/1000000+((K891/1000)^2*(D891/C891*H891)^2*PI()*PI()*(O891/2)^2)/1200","v":2.6022022275276519E-2},{"$f":"SQRT(3)*L891*J891*D891/C891*H891/1000","v":13.564858363011515},{"$f":"0.75*J891^2*(D891/C891*H891)^2-(UAC_V*0.98)^2","v":-146083.53895630967},{"$f":"-AO891/2/AN891+SQRT((AO891/2/AN891)^2-AP891/AN891)","v":2123.005912046563},{"$f":"(L891^2)/1000000+((K891/1000)^2*AV891^2*PI()*PI()*(O891/2)^2)/1200","v":7.6925171116010212E-3},{"$f":"SQRT(3)*L891*J891*AV891/1000","v":3.8700077340612133},{"$f":"0.75*J891^2*AV891^2-(UAC_V*0.98)^2","v":-153046.99489233203},{"$f":"-AS891/2/AR891+SQRT((AS891/2/AR891)^2-AT891/AR891)","v":4215.9883150059477},{"$f":"D891+(F891-D891)*((0.85*UAC_V-D891*J891)/L891*1000)/G891","v":1.3465861535652275},{"$f":"(L891^2)/1000000+((K891/1000)^2*AJ891^2*PI()*PI()*(O891/2)^2)/1200","v":0.27395927211146981},{"$f":"SQRT(3)*L891*J891*AJ891/1000","v":49.703096815600077},{"$f":"0.75*J891^2*AJ891^2-(UAC_V*0.98)^2","v":-51891.137213004957},{"$f":"IF(((AX891/2/AW891)^2-AY891/AW891)>0,-AX891/2/AW891+SQRT((AX891/2/AW891)^2-AY891/AW891),-9999)","v":353.8553557017118}]
["KBM","KBMS-17H01-B (120 V)",2.0699999999999998,3.11,1.8568076694054458,2.7265898229154857,1800,6.14,2782,6.02,18,41.2,8.6199999999999999E-2,160,10,2782,2782,2782,1.7404994090477501,1305.1044083526683,4.7945634829910198,4.7407903344364826,0.10506976627311593,-22.528953893135803,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},29.108452653440004,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},-2352.0053727999998,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},2364.0053727999998,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},0.62050682936818702,0.91110394275562001,14.892163904836488,43.732989252269761,32.754818305937434,23.027300489548562,2.4098572927188568,147.62607267248109,7.3666213224903567E-3,3.9628966775858756,-151351.02427225394,4271.7131351150792,1.8373113690526124E-3,0.62246794037584874,-153606.93372125144,8975.7054282260306,1.4489808766002814,7.3172397801371192E-2,14.071147947873516,-124502.85077367314,1211.8039183846029]
["KBM","KBMS-17H01-B (240 V)",2.0699999999999998,3.11,1.7052315331274501,2.50401106186116,4200,6.14,5838,6.02,18,41.2,8.6199999999999999E-2,325,10,4271.7131351150792,5838,5838,1.5629718310471556,1305.1044083526683,4.7929386116413832,4.7407903344364826,0.10506976627311593,-22.528953893135803,9,29.108452653440004,9,-2352.0053727999998,7.5,2364.0053727999998,9,0.62050682936818702,0.91110394275562001,14.892163904836488,43.732989252269761,32.754818305937434,23.027300489548562,2.4098572927188568,147.62607267248109,7.3666213224903567E-3,3.9628966775858756,-151351.02427225394,4271.7131351150792,1.9599053388811181E-3,0.85268486594442117,-153556.91646823884,8636.6459414378005,1.9848798377855836,7.3172397801371192E-2,14.071147947873516,-124502.85077367314,1211.8039183846029]
["KBM","KBMS-17H01-B (400 V)",2.0699999999999998,3.11,1.0653261508694498,1.5643555813060936,8650,6.14,9600,6.02,18,41.2,8.6199999999999999E-2,565,10,4271.7131351150792,8812.9822130209686,9514.5631067961167,1.0463962124537745,1305.1044083526683,4.7944455088480522,4.7407903344364826,0.10506976627311593,-22.528953893135803,9,29.108452653440004,9,-2352.0053727999998,7.5,2364.0053727999998,9,0.62050682936818702,0.91110394275562001,14.892163904836488,43.732989252269761,32.754818305937434,23.027300489548562,2.4098572927188568,147.62607267248109,7.3666213224903567E-3,3.9628966775858756,-151351.02427225394,4271.7131351150792,1.8937488246923593E-3,0.7374328619459376,-153583.90773961411,8812.9822130209686,1.7165962219533726,7.3172397801371192E-2,14.071147947873516,-124502.85077367314,1211.8039183846029]
["KBM","KBMS-17H01-B (480 V)",2.0699999999999998,3.11,0.71619724391352901,1.0516846459816871,9600,6.14,9600,6.02,18,41.2,8.6199999999999999E-2,679,10,4271.7131351150792,8982.0331538677638,9514.5631067961167,0.80334362094101719,1305.1044083526683,4.7957256170443436,4.7407903344364826,0.10506976627311593,-22.528953893135803,9,29.108452653440004,9,-2352.0053727999998,7.5,2364.0053727999998,9,0.62050682936818702,0.91110394275562001,14.892163904836488,43.732989252269761,32.754818305937434,23.027300489548562,2.4098572927188568,147.62607267248109,7.3666213224903567E-3,3.9628966775858756,-151351.02427225394,4271.7131351150792,1.8352083341529315E-3,0.61777066104835976,-153607.79174084915,8982.0331538677638,1.4380465497440718,7.3172397801371192E-2,14.071147947873516,-124502.85077367314,1211.8039183846029]
["KBM","KBMS-17H01-C (120 V)",2.0699999999999998,6.1,1.7384616860807027,4.8970751720583179,3900,6.35,5468,1.56,5,21.5,8.6199999999999999E-2,160,10,5468,5468,5468,1.605166281920329,1305.1044083526683,4.7928440142374535,4.5840082918803162,5.0694399807009974E-2,-22.528953893135803,9,29.108452653440004,9,-2352.0053727999998,7.5,2364.0053727999998,9,1.2170712730372799,1.7870527494563611,29.20971055289472,85.778531973905331,64.245785101677924,23.027300489548562,2.4098572927188568,147.62607267248109,2.2622186719710811E-3,1.0870684727370978,-153024.88812091996,7987.8229923093695,4.7174131636943284E-4,7.8938278714198992E-2,-153660.62993410148,17964.538031892549,1.3588263704534436,2.1679436704741546E-2,3.7322293714953663,-146130.4488472403,2511.5980257825249]
["KBM","KBMS-17H01-C (240 V)",2.0699999999999998,6.1,0.90187801085407349,2.5405014390255594,9000,6.35,9600,1.56,5,21.5,8.6199999999999999E-2,325,10,7987.8229923093695,9600,9600,0.82400321157767853,1305.1044083526683,4.7951476025239703,4.5840082918803162,5.0694399807009974E-2,-22.528953893135803,9,29.108452653440004,9,-2352.0053727999998,7.5,2364.0053727999998,9,1.2170712730372799,1.7870527494563611,29.20971055289472,85.778531973905331,64.245785101677924,23.027300489548562,2.4098572927188568,147.62607267248109,2.2622186719710811E-3,1.0870684727370978,-153024.88812091996,7987.8229923093695,4.6225218859326825E-4,1.1986902057879855E-3,-153663.99922289985,18231.21840125155,2.0633992635261222E-2,2.1679436704741546E-2,3.7322293714953663,-146130.4488472403,2511.5980257825249]
["KBM","KBMS-17H02-A (120 V)",3.58,1.59,3.3104228163114229,1.4330834702646853,375,12.2,812,27.5,97,140,0.128,160,10,812,812,812,2.9962755382530011,878.90625,2.7813512215078009,2.386641979803279,0.22565131281628945,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.18344362043943718,0.26941387991284921,4.4026468905464924,12.931866235816761,9.6851876212945474,23.028996904169631,2.4113249480833296,147.71598015295655,7.6400195858433745E-2,36.132273191648366,-137011.68920923583,1123.407414947286,2.0560117020112425E-2,4.6976694321155188,-153382.51915697151,2619.4819340350796,0.70446771719370693,0.20107552150632421,64.584662607539357,-100460.19076365187,564.2508917161723]
["KBM","KBMS-17H02-A (240 V)",3.58,1.59,3.2293984816464585,1.3980080007127527,1100,12.2,1710,27.5,97,140,0.128,325,10,1123.407414947286,1710,1710,3.0349740032867674,878.90625,2.7744404544702759,2.386641979803279,0.22565131281628945,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.18344362043943718,0.26941387991284921,4.4026468905464924,12.931866235816761,9.6851876212945474,23.028996904169631,2.4113249480833296,147.71598015295655,7.6400195858433745E-2,36.132273191648366,-137011.68920923583,1123.407414947286,2.2482521790643348E-2,8.1396675658875957,-152818.92107036783,2432.4049792727496,1.2206335740985117,0.20107552150632421,64.584662607539357,-100460.19076365187,564.2508917161723]
["KBM","KBMS-17H02-A (400 V)",3.58,1.59,3.1376260209545084,1.3582796627508693,2100,12.2,2861,27.5,97,140,0.128,565,10,1123.407414947286,2379.2045393146518,2800,3.0788103909429911,878.90625,2.7725798198946165,2.386641979803279,0.22565131281628945,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.18344362043943718,0.26941387991284921,4.4026468905464924,12.931866235816761,9.6851876212945474,23.028996904169631,2.4113249480833296,147.71598015295655,7.6400195858433745E-2,36.132273191648366,-137011.68920923583,1123.407414947286,2.3159860545850314E-2,9.0455892120288528,-152620.34331386769,2379.2045393146518,1.3564865887126321,0.20107552150632421,64.584662607539357,-100460.19076365187,564.2508917161723]
["KBM","KBMS-17H02-A (480 V)",3.58,1.59,3.0667933265015219,1.3276161586586674,2600,12.2,3438,27.5,97,140,0.128,679,10,1123.407414947286,2371.3145921646969,2800,3.1119328947449061,878.90625,2.7723515823765008,2.386641979803279,0.22565131281628945,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.18344362043943718,0.26941387991284921,4.4026468905464924,12.931866235816761,9.6851876212945474,23.028996904169631,2.4113249480833296,147.71598015295655,7.6400195858433745E-2,36.132273191648366,-137011.68920923583,1123.407414947286,2.3265330966520854E-2,9.1786110475818141,-152589.42218414808,2371.3145921646969,1.3764346906774634,0.20107552150632421,64.584662607539357,-100460.19076365187,564.2508917161723]
["KBM","KBMS-17H02-B (120 V)",3.52,2.99,3.246760839074665,2.7056340325622208,1000,12.3,1565,7.78,27,72.8,0.128,160,10,1565,1565,1565,3.0923807131518508,878.90625,2.8210167984914771,2.3672383864715445,9.0416768855465429E-2,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.35084641257644078,0.51526944921439399,8.4203139018345787,24.732933562290913,18.523475081450311,23.028996904169631,2.4113249480833296,147.71598015295655,2.1662477493410739E-2,10.249560421072978,-148708.49715344116,2394.1603770163474,5.7603530886716119E-3,1.7194896838398708,-153524.53141355061,5015.4557158499192,1.752782267567117,5.6731550386416293E-2,18.171637687565262,-138087.66107995043,1408.1896100163494]
["KBM","KBMS-17H02-B (240 V)",3.52,2.99,3.0516230392837325,2.5430191994031106,2300,12.3,3285,7.78,27,72.8,0.128,325,10,2394.1603770163474,3285,3285,2.8510355148030699,878.90625,2.8197777452309043,2.3672383864715445,9.0416768855465429E-2,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.35084641257644078,0.51526944921439399,8.4203139018345787,24.732933562290913,18.523475081450311,23.028996904169631,2.4113249480833296,147.71598015295655,2.1662477493410739E-2,10.249560421072978,-148708.49715344116,2394.1603770163474,5.9891674449140328E-3,2.1037366374156021,-153455.23389387203,4889.2482833707127,2.1444689714327669,5.6731550386416293E-2,18.171637687565262,-138087.66107995043,1408.1896100163494]
["KBM","KBMS-17H02-B (400 V)",3.52,2.99,2.6043536142310146,2.1702946785258455,4400,12.3,5495,7.78,27,72.8,0.128,565,10,2394.1603770163474,4877.4682297245845,5384.6153846153848,2.5049917826703711,878.90625,2.8198571025542507,2.3672383864715445,9.0416768855465429E-2,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.35084641257644078,0.51526944921439399,8.4203139018345787,24.732933562290913,18.523475081450311,23.028996904169631,2.4113249480833296,147.71598015295655,2.1662477493410739E-2,10.249560421072978,-148708.49715344116,2394.1603770163474,6.0118473545439271E-3,2.1380646116128297,-153448.36517501326,4877.4682297245845,2.1794616003620866,5.6731550386416293E-2,18.171637687565262,-138087.66107995043,1408.1896100163494]
["KBM","KBMS-17H02-B (480 V)",3.52,2.99,2.2252489291013626,1.8543741075844689,5450,12.3,6602,7.78,27,72.8,0.128,679,10,2394.1603770163474,4909.6193740458875,5384.6153846153848,2.3536266161008053,878.90625,2.8203816175648551,2.3672383864715445,9.0416768855465429E-2,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.35084641257644078,0.51526944921439399,8.4203139018345787,24.732933562290913,18.523475081450311,23.028996904169631,2.4113249480833296,147.71598015295655,2.1662477493410739E-2,10.249560421072978,-148708.49715344116,2394.1603770163474,5.9504768835502006E-3,2.0438448499696094,-153466.9515150105,4909.6193740458875,2.0834175653121987,5.6731550386416293E-2,18.171637687565262,-138087.66107995043,1408.1896100163494]
["KBM","KBMS-17H02-C (120 V)",3.64,5.27,3.2166051656467265,4.5304298107700376,1900,12.7,2797,2.5099999999999998,9.1999999999999993,43,0.128,160,10,2797,2797,2797,3.0167182359546807,878.90625,2.7270219936421682,2.2926796971338583,4.8300528100882541E-2,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.59799526736171904,0.87824381553040276,14.351886416681257,42.155703145459334,31.572078370294367,23.028996904169631,2.4113249480833296,147.71598015295655,7.7328293424558442E-3,3.437286694500266,-152066.52300970949,4217.8431474142853,1.9420247578248891E-3,0.4322002334295148,-153638.74350435688,8783.9501129140008,2.3119699908676874,1.9196644233916708E-2,5.9020920234241405,-148954.06351366051,2636.077895620148]
["KBM","KBMS-17H02-C (240 V)",3.64,5.27,2.6891697281044387,3.7875629973301956,4350,12.7,5622,2.5099999999999998,9.1999999999999993,43,0.128,325,10,4217.8431474142853,5622,5622,2.4111338417018744,878.90625,2.7269511303309337,2.2926796971338583,4.8300528100882541E-2,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.59799526736171904,0.87824381553040276,14.351886416681257,42.155703145459334,31.572078370294367,23.028996904169631,2.4113249480833296,147.71598015295655,7.7328293424558442E-3,3.437286694500266,-152066.52300970949,4217.8431474142853,1.9740182218015876E-3,0.50103998048407961,-153630.05718468854,8695.9119911981434,2.6802146540095269,1.9196644233916708E-2,5.9020920234241405,-148954.06351366051,2636.077895620148]
["KBM","KBMS-17H02-C (400 V)",3.64,5.27,0.99787623049680418,1.4054594795729638,7560,12.7,9375,2.5099999999999998,9.1999999999999993,43,0.128,565,10,4217.8431474142853,8966.2468526173179,9116.2790697674427,0.50641085548499554,878.90625,2.7291315441540034,2.2926796971338583,4.8300528100882541E-2,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.59799526736171904,0.87824381553040276,14.351886416681257,42.155703145459334,31.572078370294367,23.028996904169631,2.4113249480833296,147.71598015295655,7.7328293424558442E-3,3.437286694500266,-152066.52300970949,4217.8431474142853,1.882400105132946E-3,0.2589760723172238,-153654.93177311617,8966.2468526173179,1.38534147193571,1.9196644233916708E-2,5.9020920234241405,-148954.06351366051,2636.077895620148]
["KBM","KBMS-17H02-D (120 V)",3.58,6.5,3.083627022405472,5.4577469423105702,2400,12.8,3365,1.65,3.1,34.200000000000003,0.128,160,10,3365,3365,3365,2.8840437209976724,878.90625,2.772513889597815,2.2747681369999997,3.7837727926750747E-2,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.74992675022411426,1.101377496499069,17.998242005378742,52.866119831955309,39.593534300889658,23.028996904169631,2.4113249480833296,147.71598015295655,2.236880984939061E-3,2.2714907743900832,-152561.16700477514,7766.345432792582,1.1802650599786523E-3,0.22664462550406314,-153653.02059901552,11314.261773324422,2.3188611650744777,4.2672763849017671E-3,3.8698572769962261,-150463.05882486905,5501.8444957523216]
["KBM","KBMS-17H02-D (240 V)",3.58,6.5,2.1997486777344109,3.8933604915653293,5600,12.8,7054,1.65,3.1,34.200000000000003,0.128,325,10,7054,7054,7054,1.8413762808461667,878.90625,2.7731962148990363,2.2747681369999997,2.3142048920469536E-2,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,0.74992675022411426,1.101377496499069,17.998242005378742,52.866119831955309,39.593534300889658,23.028996904169631,2.4113249480833296,147.71598015295655,2.236880984939061E-3,2.2714907743900832,-152561.16700477514,7766.345432792582,1.1776906258336869E-3,0.19728522027036505,-153655.68088938965,11338.982901982712,2.0184773175656545,4.2672763849017671E-3,3.8698572769962261,-150463.05882486905,5501.8444957523216]
["KBM","KBMS-17H02-E (120 V)",3.75,9.33,3.0012074983043124,7.2844842191852246,3500,12.9,4633,0.8,3.1,24.8,0.128,160,10,4633,4633,4633,2.7588126684696799,878.90625,2.646784220027941,2.2571342754728683,2.7481967294089416E-2,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,1.0276350094332607,1.5092328332949334,24.663240226398258,72.443175998156804,54.255568270676342,23.028996904169631,2.4113249480833296,147.71598015295655,2.650497638264534E-3,1.1029158588490393,-153169.5511057408,7396.6946454182671,6.194475386623636E-4,5.1322690170313684E-2,-153662.92933039871,15708.69104266813,1.4935065012785467,6.4316578126047156E-3,1.8644322726325331,-152251.03998958046,4722.617961796891]
["KBM","KBMS-17H02-E (240 V)",3.75,9.33,1.1013522061959158,2.6731849664949414,7500,12.9,9600,0.8,3.1,24.8,0.128,325,10,7396.6946454182671,9600,9600,0.35973082393077238,878.90625,2.6489687194310658,2.2571342754728683,2.6960460385212118E-2,-22.539545868641973,9,29.1170321536,9,-2352.8808319999998,7.5,2364.8808319999998,9,1.0276350094332607,1.5092328332949334,24.663240226398258,72.443175998156804,54.255568270676342,23.028996904169631,2.4113249480833296,147.71598015295655,2.650497638264534E-3,1.1029158588490393,-153169.5511057408,7396.6946454182671,6.2810372814611998E-4,-8.8357804173731375E-2,-153660.82658788111,15711.544835542602,-2.5712400214066555,6.4316578126047156E-3,1.8644322726325331,-152251.03998958046,4722.617961796891]
["KBM","KBMS-17H03-A (120 V)",4.88,3,4.5018112474564687,2.7283704530039206,700,18.5,1136,8.61,33,100,0.17499999999999999,160,10,1136,1136,1136,4.2662536815864982,642.85714285714289,2.0364978551117598,1.5744150789189189,0.11208094583936291,-22.551455506172839,9,29.12667896,9,-2353.8651999999997,7.5,2365.8651999999997,9,0.25393696799268584,0.37303635963114751,6.0944872318244601,17.905745262295081,13.409656830756509,23.030904958779317,2.412975182584054,147.817072296075,3.8962277474955669E-2,16.9604331690743,-146472.59266793411,1733.4287755686771,1.0710165384786493E-2,2.655830382414456,-153487.66412449611,3663.6776439709288,1.7808877888605958,5.0264444843346377E-2,19.997764177865587,-143666.2356971619,1503.360952356245]
["KBM","KBMS-17H03-A (240 V)",4.88,3,4.2971834634811747,2.6043536142310151,1700,18.5,2389,8.61,33,100,0.17499999999999999,325,10,1733.4287755686771,2389,2389,4.0609713495626627,642.85714285714289,2.03466702771598,1.5744150789189189,8.4692870513870352E-2,-22.551455506172839,9,29.12667896,9,-2353.8651999999997,7.5,2365.8651999999997,9,0.25393696799268584,0.37303635963114751,6.0944872318244601,17.905745262295081,13.409656830756509,23.030904958779317,2.412975182584054,147.817072296075,3.8962277474955669E-2,16.9604331690743,-146472.59266793411,1733.4287755686771,1.1152623091708504E-2,3.3834849023631395,-153377.80074788703,3559.8636344365968,2.2688222057821061,5.0264444843346377E-2,19.997764177865587,-143666.2356971619,1503.360952356245]
["KBM","KBMS-17H03-A (400 V)",4.88,3,3.5950293027816365,2.1788056380494769,3400,18.5,3997,8.61,33,100,0.17499999999999999,565,10,1733.4287755686771,3566.0030291015619,3920,3.532291353356638,642.85714285714289,2.0349922628668002,1.5744150789189189,8.4692870513870352E-2,-22.551455506172839,9,29.12667896,9,-2353.8651999999997,7.5,2365.8651999999997,9,0.25393696799268584,0.37303635963114751,6.0944872318244601,17.905745262295081,13.409656830756509,23.030904958779317,2.412975182584054,147.817072296075,3.8962277474955669E-2,16.9604331690743,-146472.59266793411,1733.4287755686771,1.1124720508905341E-2,3.3422804769765051,-153384.72903033055,3566.0030291015619,2.241192256782365,5.0264444843346377E-2,19.997764177865587,-143666.2356971619,1503.360952356245]
["KBM","KBMS-17H03-A (480 V)",4.88,3,3.4812625526936092,2.1098560925415812,3950,18.5,4803,8.61,33,100,0.17499999999999999,679,10,1733.4287755686771,3554.6901317259994,3920,3.6212460251099641,642.85714285714289,2.034771515211693,1.5744150789189189,8.4692870513870352E-2,-22.551455506172839,9,29.12667896,9,-2353.8651999999997,7.5,2365.8651999999997,9,0.25393696799268584,0.37303635963114751,6.0944872318244601,17.905745262295081,13.409656830756509,23.030904958779317,2.412975182584054,147.817072296075,3.8962277474955669E-2,16.9604331690743,-146472.59266793411,1733.4287755686771,1.1176302341017902E-2,3.4180630192156674,-153371.92112991677,3554.6901317259994,2.2920088318830087,5.0264444843346377E-2,19.997764177865587,-143666.2356971619,1503.360952356245]
["KBM","KBMS-17H03-B (120 V)",4.8899999999999997,5.32,4.3653927248062727,4.5951502366381822,1400,18.8,1998,2.81,11,57,0.17499999999999999,160,10,1998,1998,1998,4.1413104744020952,642.85714285714289,2.0307939212454964,1.5492914340425532,6.3725702939697829E-2,-22.551455506172839,9,29.12667896,9,-2353.8651999999997,7.5,2365.8651999999997,9,0.44939400056161644,0.66016501391956373,10.785456013478795,31.687920668139061,23.731162016180519,23.030904958779317,2.412975182584054,147.817072296075,1.3656948226580453E-2,5.6741710728172361,-151186.60561991413,3125.9466512272679,3.3884465529413908E-3,0.65678580118015295,-153630.80766477133,6637.2505129270749,2.36745619723597,1.7260411466811364E-2,6.5835601418646288,-150328.87656651673,2766.6225833197295]
["KBM","KBMS-17H03-B (240 V)",4.8899999999999997,5.32,3.8500338614610872,4.0526672225906184,3150,18.8,4194,2.81,11,57,0.17499999999999999,325,10,3125.9466512272679,4194,4194,3.5053593698310479,642.85714285714289,2.0303826352613514,1.5492914340425532,4.6021439729859191E-2,-22.551455506172839,9,29.12667896,9,-2353.8651999999997,7.5,2365.8651999999997,9,0.44939400056161644,0.66016501391956373,10.785456013478795,31.687920668139061,23.731162016180519,23.030904958779317,2.412975182584054,147.817072296075,1.3656948226580453E-2,5.6741710728172361,-151186.60561991413,3125.9466512272679,3.4767645167887262E-3,0.83938827239097935,-153609.78542075813,6527.3227266711574,3.0256667604392011,1.7260411466811364E-2,6.5835601418646288,-150328.87656651673,2766.6225833197295]
["KBM","KBMS-17H03-B (400 V)",4.8899999999999997,5.32,1.8011681364546206,1.8959664594259165,6150,18.8,7006,2.81,11,57,0.17499999999999999,565,10,3125.9466512272679,6670.6653373199451,6877.1929824561403,1.5396644479737343,642.85714285714289,2.0319716286169358,1.5492914340425532,4.6021439729859191E-2,-22.551455506172839,9,29.12667896,9,-2353.8651999999997,7.5,2365.8651999999997,9,0.44939400056161644,0.66016501391956373,10.785456013478795,31.687920668139061,23.731162016180519,23.030904958779317,2.412975182584054,147.817072296075,1.3656948226580453E-2,5.6741710728172361,-151186.60561991413,3125.9466512272679,3.363475262917753E-3,0.59508045801233156,-153636.75155805569,6670.6653373199451,2.1450325443148244,1.7260411466811364E-2,6.5835601418646288,-150328.87656651673,2766.6225833197295]
["KBM","KBMS-17H03-C (120 V)",5.05,6.14,4.4762327744595565,5.2723589805177342,1600,18.8,2239,2.1,8.8000000000000007,51.34,0.17499999999999999,160,10,2239,2239,2239,4.2470844887593415,642.85714285714289,1.9662064068853717,1.5492914340425532,5.6866437906885337E-2,-22.551455506172839,9,29.12667896,9,-2353.8651999999997,7.5,2365.8651999999997,9,0.50222865738339562,0.7377797393333333,12.053487777201495,35.413427487999996,26.521203270714416,23.030904958779317,2.412975182584054,147.817072296075,1.0955224928801929E-2,4.2684542281114854,-151935.8973450101,3534.363102979074,2.7505846253614743E-3,0.50138812579135317,-153640.1561506624,7383.1859498492558,2.6849627079425651,1.3835596459616727E-2,4.9525516173088899,-151337.58975767042,3133.167308005759]
["KBM","KBMS-17H03-C (240 V)",5.05,6.14,3.8063629746453294,4.4833486156010949,3575,18.8,4700,2.1,8.8000000000000007,51.34,0.17499999999999999,325,10,3534.363102979074,4700,4700,3.415008665967286,642.85714285714289,1.9661135438290385,1.5492914340425532,4.0637457868331055E-2,-22.551455506172839,9,29.12667896,9,-2353.8651999999997,7.5,2365.8651999999997,9,0.50222865738339562,0.7377797393333333,12.053487777201495,35.413427487999996,26.521203270714416,23.030904958779317,2.412975182584054,147.817072296075,1.0955224928801929E-2,4.2684542281114854,-151935.8973450101,3534.363102979074,2.7975768830157742E-3,0.59523436676717578,-153630.39497089791,7304.8804551432968,3.187514811471102,1.3835596459616727E-2,4.9525516173088899,-151337.58975767042,3133.167308005759]
["KBM","KBMS-17H03-C (400 V)",5.05,6.14,1.429447174066097,1.6836833616797373,6480,18.8,7200,2.1,8.8000000000000007,51.34,0.17499999999999999,565,10,3534.363102979074,7200,7200,1.0271635267401082,642.85714285714289,1.9679393336927349,1.5492914340425532,4.0637457868331055E-2,-22.551455506172839,9,29.12667896,9,-2353.8651999999997,7.5,2365.8651999999997,9,0.50222865738339562,0.7377797393333333,12.053487777201495,35.413427487999996,26.521203270714416,23.030904958779317,2.412975182584054,147.817072296075,1.0955224928801929E-2,4.2684542281114854,-151935.8973450101,3534.363102979074,2.6850283901855353E-3,0.32836063356906242,-153653.77341929721,7503.8957196752772,1.7583903777095209,1.3835596459616727E-2,4.9525516173088899,-151337.58975767042,3133.167308005759]
["KBM","KBMS-17H03-D (120 V)",5,10.38,4.0139416156057672,8.0278832312115345,2950,19,3838,0.74,2.9,30,0.17499999999999999,160,10,3838,3838,3838,3.7171213290491307,642.85714285714289,1.9856849429862753,1.5329831031578947,3.3174558226554525E-2,-22.551455506172839,9,29.12667896,9,-2353.8651999999997,7.5,2365.8651999999997,9,0.8575349834325805,1.2597288650200003,20.580839602381932,60.466985520960009,45.283874731191503,23.030904958779317,2.412975182584054,147.817072296075,3.5903972108365162E-3,1.5166820675931789,-153025.0209738448,6320.6504837280818,9.0414252997404547E-4,5.9514005347201734E-2,-153663.01613421319,13003.786341272755,1.5477669823315203,4.4460239496934275E-3,1.7412341739157799,-152821.80654210772,5670.2728014161685]
["KBM","KBMS-17H03-D (240 V)",5,10.38,1.4103576495527956,2.8207152991055913,6500,19,8030,0.74,2.9,30,0.17499999999999999,325,10,6320.6504837280818,8030,8030,0.56541106552445353,642.85714285714289,1.9876103928135078,1.5329831031578947,2.2454643529975615E-2,-22.551455506172839,9,29.12667896,9,-2353.8651999999997,7.5,2365.8651999999997,9,0.8575349834325805,1.2597288650200003,20.580839602381932,60.466985520960009,45.283874731191503,23.030904958779317,2.412975182584054,147.817072296075,3.5903972108365162E-3,1.5166820675931789,-153025.0209738448,6320.6504837280818,9.1082957552895841E-4,-9.6225918931582999E-2,-153661.42793681272,13041.5763368015,-2.5025252341517366,4.4460239496934275E-3,1.7412341739157799,-152821.80654210772,5670.2728014161685]
["KBM","KBMS-17H04-A (120 V)",5.98,3.15,5.4908455366703892,2.8014518044236678,600,23.7,960,8.64,34,118,0.24,160,10,960,960,960,5.1973528586726223,468.75,1.6630293053305765,1.2295367210126582,0.13262911924324611,-22.56792628148148,9,29.140020287999999,9,-2355.2265600000001,7.5,2367.2265600000001,9,0.21761240253215308,0.31978492163879596,5.222697660771674,15.349676238662205,11.494621348387765,23.03354480882064,2.4152574217871821,147.95688057911107,5.0969185492360604E-2,22.045202524812183,-144938.2215893424,1483.8612147317745,1.454025045470241E-2,2.8433271530470328,-153518.84578247531,3153.0344692275717,1.6101652711137364,4.5329497753776184E-2,20.297897104226156,-146266.6173000978,1586.3200240002059]
["KBM","KBMS-17H04-A (240 V)",5.98,3.15,5.2862177526950962,2.6970498738240285,1400,23.7,2018,8.64,34,118,0.24,325,10,1483.8612147317745,2018,2018,4.9799624463847882,468.75,1.6610531666738664,1.2295367210126582,8.0263725192376276E-2,-22.56792628148148,9,29.140020287999999,9,-2355.2265600000001,7.5,2367.2265600000001,9,0.21761240253215308,0.31978492163879596,5.222697660771674,15.349676238662205,11.494621348387765,23.03354480882064,2.4152574217871821,147.95688057911107,5.0969185492360604E-2,22.045202524812183,-144938.2215893424,1483.8612147317745,1.5173099595343102E-2,4.0480581262293462,-153369.78184082641,3048.7104083918875,2.2923998046862888,4.5329497753776184E-2,20.297897104226156,-146266.6173000978,1586.3200240002059]
["KBM","KBMS-17H04-A (400 V)",5.98,3.15,4.703912762493796,2.3999554910682632,2700,23.7,3377,8.64,34,118,0.24,565,10,1483.8612147317745,3028.7175970716567,3322.0338983050847,4.5485526401357044,468.75,1.6609115872804767,1.2295367210126582,8.0263725192376276E-2,-22.56792628148148,9,29.140020287999999,9,-2355.2265600000001,7.5,2367.2265600000001,9,0.21761240253215308,0.31978492163879596,5.222697660771674,15.349676238662205,11.494621348387765,23.03354480882064,2.4152574217871821,147.95688057911107,5.0969185492360604E-2,22.045202524812183,-144938.2215893424,1483.8612147317745,1.5308726530424165E-2,4.2621645505985377,-153337.83570352665,3028.7175970716567,2.4136474523486995,4.5329497753776184E-2,20.297897104226156,-146266.6173000978,1586.3200240002059]
["KBM","KBMS-17H04-A (480 V)",5.98,3.15,4.332815167158464,2.2106199832441145,3350,23.7,4058,8.64,34,118,0.24,679,10,1483.8612147317745,3029.8718976675736,3322.0338983050847,4.4902211834952741,468.75,1.6610293247209895,1.2295367210126582,8.0263725192376276E-2,-22.56792628148148,9,29.140020287999999,9,-2355.2265600000001,7.5,2367.2265600000001,9,0.21761240253215308,0.31978492163879596,5.222697660771674,15.349676238662205,11.494621348387765,23.03354480882064,2.4152574217871821,147.95688057911107,5.0969185492360604E-2,22.045202524812183,-144938.2215893424,1483.8612147317745,1.5300776386291452E-2,4.2499117347228497,-153339.70831382982,3029.8718976675736,2.4067087296712044,4.5329497753776184E-2,20.297897104226156,-146266.6173000978,1586.3200240002059]
["KBM","KBMS-17H04-B (120 V)",6.12,5.53,5.4510568008974154,4.7816287727170312,1200,23.7,1660,2.8,12,69.3,0.24,160,10,1660,1660,1660,5.1946285745747582,468.75,1.6233517286909562,1.2295367210126582,7.6701177393684497E-2,-22.56792628148148,9,29.140020287999999,9,-2355.2265600000001,7.5,2367.2265600000001,9,0.37329139870820538,0.54855770762745093,8.9589935689969291,26.330769966117646,19.71782504504484,23.03354480882064,2.4152574217871821,147.95688057911107,1.838140627174089E-2,7.1973719747136995,-150967.36953630333,2676.7424399270685,5.0041301443439802E-3,0.87706118839638625,-153623.95638053431,5453.7661220101918,2.6096243723790291,1.6314178193836036E-2,6.6269074007894284,-151377.89936789885,2849.792207575646]
["KBM","KBMS-17H04-B (240 V)",6.12,5.53,4.8647359963937822,4.267312277538406,2650,23.7,3485,2.8,12,69.3,0.24,325,10,2676.7424399270685,3485,3485,4.469209414125408,468.75,1.6228579127578511,1.2295367210126582,4.4678329225214759E-2,-22.56792628148148,9,29.140020287999999,9,-2355.2265600000001,7.5,2367.2265600000001,9,0.37329139870820538,0.54855770762745093,8.9589935689969291,26.330769966117646,19.71782504504484,23.03354480882064,2.4152574217871821,147.95688057911107,1.838140627174089E-2,7.1973719747136995,-150967.36953630333,2676.7424399270685,5.1246810023667733E-3,1.1086592816538476,-153600.01624351132,5367.6236505435572,3.2987256993528455,1.6314178193836036E-2,6.6269074007894284,-151377.89936789885,2849.792207575646]
["KBM","KBMS-17H04-B (400 V)",6.12,5.53,2.902986161996171,2.5464790894703255,5000,23.7,5822,2.8,12,69.3,0.24,565,10,2676.7424399270685,5438.8676694340584,5656.5656565656564,2.6206174888718001,468.75,1.6238587198482151,1.2295367210126582,4.4678329225214759E-2,-22.56792628148148,9,29.140020287999999,9,-2355.2265600000001,7.5,2367.2265600000001,9,0.37329139870820538,0.54855770762745093,8.9589935689969291,26.330769966117646,19.71782504504484,23.03354480882064,2.4152574217871821,147.95688057911107,1.838140627174089E-2,7.1973719747136995,-150967.36953630333,2676.7424399270685,5.02409550952501E-3,0.91945752192389862,-153619.99146824761,5438.8676694340584,2.7357712213522429,1.6314178193836036E-2,6.6269074007894284,-151377.89936789885,2849.792207575646]
["KBM","KBMS-17H04-B (480 V)",6.12,5.53,1.8009638297240791,1.5797928330912976,5700,23.7,6987,2.8,12,69.3,0.24,679,10,2676.7424399270685,5490.211310280949,5656.5656565656564,1.9599260997260748,468.75,1.6245335635406331,1.2295367210126582,4.4678329225214759E-2,-22.56792628148148,9,29.140020287999999,9,-2355.2265600000001,7.5,2367.2265600000001,9,0.37329139870820538,0.54855770762745093,8.9589935689969291,26.330769966117646,19.71782504504484,23.03354480882064,2.4152574217871821,147.95688057911107,1.838140627174089E-2,7.1973719747136995,-150967.36953630333,2676.7424399270685,4.9570507144434161E-3,0.76787574828483374,-153633.30586191727,5490.211310280949,2.2847519582376532,1.6314178193836036E-2,6.6269074007894284,-151377.89936789885,2849.792207575646]
["KBM","KBMS-17H04-C (120 V)",6.1,6.2,5.4052622182153129,5.3517447705102104,1325,23.7,1868,2.23,9.1,61.4,0.24,160,10,1868,1868,1868,5.1205508102839286,468.75,1.6284884284923737,1.2295367210126582,6.8160575199955178E-2,-22.56792628148148,9,29.140020287999999,9,-2355.2265600000001,7.5,2367.2265600000001,9,0.41989057695977666,0.61703594872131151,10.077373847034639,29.617725538622953,22.179265215343474,23.03354480882064,2.4152574217871821,147.95688057911107,1.3650068039579633E-2,5.7127347815458362,-151499.82991037812,3128.7999276186952,3.9033685091200386E-3,0.66382710399336098,-153634.77777854432,6189.2616027740032,2.7991174331804727,1.2145939407852382E-2,5.2599427312604892,-151829.29899944959,3325.6861796055941]
["KBM","KBMS-17H04-C (240 V)",6.1,6.2,4.6473243382833438,4.601311226023113,3000,23.7,3922,2.23,9.1,61.4,0.24,325,10,3128.7999276186952,3922,3922,4.2008686849157586,468.75,1.6282504709428578,1.2295367210126582,3.8285017766954817E-2,-22.56792628148148,9,29.140020287999999,9,-2355.2265600000001,7.5,2367.2265600000001,9,0.41989057695977666,0.61703594872131151,10.077373847034639,29.617725538622953,22.179265215343474,23.03354480882064,2.4152574217871821,147.95688057911107,1.3650068039579633E-2,5.7127347815458362,-151499.82991037812,3128.7999276186952,3.9632327342043732E-3,0.79900318502704837,-153621.66492948975,6125.9040607845473,3.3691057971599507,1.2145939407852382E-2,5.2599427312604892,-151829.29899944959,3325.6861796055941]
["KBM","KBMS-17H04-C (400 V)",6.1,6.2,1.6122189040477708,1.5962563406413572,5775,23.7,6548,2.23,9.1,61.4,0.24,565,10,3128.7999276186952,6268.6504177782617,6384.3648208469058,1.2286007199933628,468.75,1.6299898271998137,1.2295367210126582,3.8285017766954817E-2,-22.56792628148148,9,29.140020287999999,9,-2355.2265600000001,7.5,2367.2265600000001,9,0.41989057695977666,0.61703594872131151,10.077373847034639,29.617725538622953,22.179265215343474,23.03354480882064,2.4152574217871821,147.95688057911107,1.3650068039579633E-2,5.7127347815458362,-151499.82991037812,3128.7999276186952,3.835714235491664E-3,0.46604202599344774,-153649.59698445129,6268.6504177782617,1.9651297027577428,1.2145939407852382E-2,5.2599427312604892,-151829.29899944959,3325.6861796055941]
["KBM","KBMS-17H04-D (120 V)",6.07,9.56,5.5993602705966818,8.48387919787376,2200,24,2881,0.94,3.8,40,0.24,160,10,2881,2881,2881,5.4536758816313817,468.75,1.6346942534350957,1.2141675119999999,4.4194361150127134E-2,-22.56792628148148,9,29.140020287999999,9,-2355.2265600000001,7.5,2367.2265600000001,9,0.65064406882038406,0.95613191225041183,15.615457651689217,45.89433178801977,34.368019086410428,23.03354480882064,2.4152574217871821,147.95688057911107,5.8421555307359733E-3,2.4616647977020558,-152717.15725371163,4906.440667596582,1.6902127822147339E-3,0.35897950975402926,-153643.86464243388,9428.656244690419,5.5121520369693808,5.1069914169651794E-3,2.2382210360148069,-152881.24478030324,5256.6040084086617]
["KBM","KBMS-17H04-D (240 V)",6.07,9.56,3.9629580829881941,6.0044819439215056,5000,24,6037,0.94,3.8,40,0.24,325,10,4906.440667596582,6037,6037,3.5259575893999453,468.75,1.635935833534969,1.2141675119999999,2.4221713157362448E-2,-22.56792628148148,9,29.140020287999999,9,-2355.2265600000001,7.5,2367.2265600000001,9,0.65064406882038406,0.95613191225041183,15.615457651689217,45.89433178801977,34.368019086410428,23.03354480882064,2.4152574217871821,147.95688057911107,5.8421555307359733E-3,2.4616647977020558,-152717.15725371163,4906.440667596582,1.6401078344869991E-3,0.23935925733914043,-153655.04799155093,9606.4543476589315,3.6753758419622784,5.1069914169651794E-3,2.2382210360148069,-152881.24478030324,5256.6040084086617]
["KBM","KBMS-25H01-A (120 V)",4.9000000000000004,3.1,4.4336019861313707,2.6870315067462855,700,14.37,1132,8.98,37,100.3,0.434,160,10,1132,1132,1132,4.1457677832867308,259.21658986175117,2.0302534026533117,2.0306081434098822,0.11247699158437832,-22.617085210864197,9,29.179839020800003,9,-2359.2896959999998,7.5,2371.2896959999998,9,0.26144994534099902,0.38459821838639457,6.274798688183977,18.46071448254694,13.821498372222859,23.041430996654391,2.4220690280242105,148.3741545315572,3.3325286234856297E-2,14.182744492534097,-148665.28126735182,1910.0159915136342,1.0509748274555501E-2,1.9717334935656416,-153567.38722194213,3729.8972859108426,1.2638930239130319,6.3834073554578638E-2,21.56219771464616,-142110.21742237167,1332.6961511271277]
["KBM","KBMS-25H01-A (240 V)",4.9000000000000004,3.1,4.1090912580089336,2.4903583381872325,1650,14.37,2379,8.98,37,100.3,0.434,325,10,1910.0159915136342,2379,2379,3.7596533956383351,259.21658986175117,2.0285311832058142,2.0306081434098822,9.5538622487828184E-2,-22.617085210864197,9,29.179839020800003,9,-2359.2896959999998,7.5,2371.2896959999998,9,0.26144994534099902,0.38459821838639457,6.274798688183977,18.46071448254694,13.821498372222859,23.041430996654395,2.4220690280242105,148.3741545315572,3.3325286234856297E-2,14.182744492534097,-148665.28126735182,1910.0159915136342,1.1130534747861603E-2,3.0422089999073121,-153434.00614310813,3578.6643497812502,1.9500742594350455,6.3834073554578638E-2,21.56219771464616,-142110.21742237167,1332.6961511271277]
["KBM","KBMS-25H01-A (400 V)",4.9000000000000004,3.1,3.304359770860303,2.0026422853698809,3150,14.37,3979,8.98,37,100.3,0.434,565,10,1910.0159915136342,3562.7665402776902,3908.2751744765701,3.0952718670793842,259.21658986175117,2.0287817081673789,2.0306081434098822,9.5538622487828184E-2,-22.617085210864197,9,29.179839020800003,9,-2359.2896959999998,7.5,2371.2896959999998,9,0.26144994534099902,0.38459821838639457,6.274798688183977,18.46071448254694,13.821498372222859,23.041430996654391,2.4220690280242105,148.3741545315572,3.3325286234856297E-2,14.182744492534097,-148665.28126735182,1910.0159915136342,1.1203886897470851E-2,3.1447156071848834,-153418.24583055242,3562.7665402776902,2.0157816109944222,6.3834073554578638E-2,21.56219771464616,-142110.21742237167,1332.6961511271277]
["KBM","KBMS-25H01-A (480 V)",4.9000000000000004,3.1,2.7893997920842706,1.6905453285359218,3800,14.37,4779,8.98,37,100.3,0.434,679,10,1910.0159915136342,3579.7330571055081,3908.2751744765701,2.9117407014185011,259.21658986175117,2.0292317385072454,2.0306081434098822,9.5538622487828184E-2,-22.617085210864197,9,29.179839020800003,9,-2359.2896959999998,7.5,2371.2896959999998,9,0.26144994534099902,0.38459821838639457,6.274798688183977,18.46071448254694,13.821498372222859,23.041430996654391,2.4220690280242105,148.3741545315572,3.3325286234856297E-2,14.182744492534097,-148665.28126735182,1910.0159915136342,1.1125656557063964E-2,3.0352691638118157,-153435.05426251687,3579.7330571055081,1.9456257827738637,6.3834073554578638E-2,21.56219771464616,-142110.21742237167,1332.6961511271277]
["KBM","KBMS-25H01-B (120 V)",4.96,5.34,4.2630788328186258,4.4874514029669745,1400,14.64,1989,2.87,12,57.5,0.434,160,10,1989,1989,1989,3.9698741417687478,259.21658986175117,2.0041056305622118,1.9931584030601095,6.4014054536710038E-2,-22.617085210864197,9,29.179839020800003,9,-2359.2896959999998,7.5,2371.2896959999998,9,0.44492060807704092,0.65448731674677429,10.678094593848982,31.415391203845164,23.520637773646161,23.041430996654391,2.4220690280242105,148.3741545315572,1.0661921313160422E-2,4.5051683668662887,-152129.28982882324,3571.9927187594176,3.4133048569001873E-3,0.54350439006404405,-153641.66374124622,6629.9984580107584,1.9014840533811195,1.9686449521709008E-2,6.7229435158037729,-150246.38415752831,2597.1232603278445]
["KBM","KBMS-25H01-B (240 V)",4.96,5.34,3.3346749981159021,3.510184208543055,3150,14.64,4173,2.87,12,57.5,0.434,325,10,3571.9927187594176,4173,4173,2.8068313546468762,259.21658986175117,2.0042689372669238,1.9931584030601095,4.9024994854284923E-2,-22.617085210864197,9,29.179839020800003,9,-2359.2896959999998,7.5,2371.2896959999998,9,0.44492060807704092,0.65448731674677429,10.678094593848982,31.415391203845164,23.520637773646161,23.041430996654391,2.4220690280242105,148.3741545315572,1.0661921313160422E-2,4.5051683668662887,-152129.28982882324,3571.9927187594176,3.4318952803662601E-3,0.58880699208769227,-153637.78497739648,6605.6263404691445,2.0599780359494804,1.9686449521709008E-2,6.7229435158037729,-150246.38415752831,2597.1232603278445]
["KBM","KBMS-25H01-B (400 V)",4.96,5.34,1.4226503076377583,1.497526639618693,4900,14.64,6970,2.87,12,57.5,0.434,565,10,3571.9927187594176,6752.9979943203571,6817.391304347826,8.4956045360826238E-2,259.21658986175117,2.006121108959189,1.9931584030601095,4.9024994854284923E-2,-22.617085210864197,9,29.179839020800003,9,-2359.2896959999998,7.5,2371.2896959999998,9,0.44492060807704092,0.65448731674677429,10.678094593848982,31.415391203845164,23.520637773646161,23.041430996654391,2.4220690280242105,148.3741545315572,1.0661921313160422E-2,4.5051683668662887,-152129.28982882324,3571.9927187594176,3.3308840523264302E-3,0.26071606851076046,-153658.86027460266,6752.9979943203571,0.91213144879108299,1.9686449521709008E-2,6.7229435158037729,-150246.38415752831,2597.1232603278445]
["KBM","KBMS-25H01-C (120 V)",4.8499999999999996,6.45,3.9834208613857238,5.2002883307907624,1750,15.1,2470,1.97,7.9,46.3,0.434,160,10,2470,2470,2470,3.6268854443558505,259.21658986175117,2.0496387616820173,1.932439670251656,5.1548159705877034E-2,-22.617085210864197,9,29.179839020800003,9,-2359.2896959999998,7.5,2371.2896959999998,9,0.54959265197886775,0.80846203472577338,13.190223647492827,38.806177666837122,29.054104160565586,23.041430996654391,2.4220690280242105,148.3741545315572,7.3185968558146762E-3,3.1725083064621877,-152490.22849449178,4353.0458910691596,2.1689100070932141E-3,0.22147468947117219,-153658.27960221903,8366.096034090504,1.4018974858829534,1.2976164339433754E-2,4.5900279882245272,-151206.9799862988,3241.3158535449952]
["KBM","KBMS-25H01-C (240 V)",4.8499999999999996,6.45,2.3166932544737429,3.0244037264670274,4225,15.1,5178,1.97,7.9,46.3,0.434,325,10,4353.0458910691596,5178,5178,1.7452751885597726,259.21658986175117,2.0506204054961414,1.932439670251656,3.9281563484244622E-2,-22.617085210864197,9,29.179839020800003,9,-2359.2896959999998,7.5,2371.2896959999998,9,0.54959265197886775,0.80846203472577338,13.190223647492827,38.806177666837122,29.054104160565586,23.041430996654391,2.4220690280242105,148.3741545315572,7.3185968558146762E-3,3.1725083064621877,-152490.22849449178,4353.0458910691596,2.1503152948842705E-3,0.11351522276042314,-153662.49725172503,8427.0744507834206,0.71853224301729668,1.2976164339433754E-2,4.5900279882245272,-151206.9799862988,3241.3158535449952]
["KBM","KBMS-25H01-D (120 V)",4.75,7.95,3.6744032513824534,5.9941325471165632,2300,15.2,3097,1.3,5.2,37.1,0.434,160,10,3097,3097,3097,3.3016855954484603,259.21658986175117,2.0926193091676253,1.9197262513684212,4.1112029213276162E-2,-22.617085210864197,9,29.179839020800003,9,-2359.2896959999998,7.5,2371.2896959999998,9,0.69166605234353951,1.0174549132252633,16.599985256244949,48.837835834812637,36.564785676736271,23.041430996654391,2.4220690280242105,148.3741545315572,4.9747269056431677E-3,2.1251764578237542,-152843.68211200001,5333.4432197968008,1.3772716784303245E-3,3.2886518709925802E-2,-153663.80356087344,10550.792928923116,0.39367697345812402,8.8098742929681589E-3,3.0545055701875454,-151969.37334836519,3983.5582529892836]
["KBM","KBMS-25H01-D (240 V)",4.75,7.95,1.3252085057447611,2.1618409555379463,4900,15.2,6489,1.3,5.2,37.1,0.434,325,10,5333.4432197968008,6489,6489,0.21459754975056189,259.21658986175117,2.0948873204934966,1.9197262513684212,3.1962367910139552E-2,-22.617085210864197,9,29.179839020800003,9,-2359.2896959999998,7.5,2371.2896959999998,9,0.69166605234353951,1.0174549132252633,16.599985256244949,48.837835834812637,36.564785676736271,23.041430996654391,2.4220690280242105,148.3741545315572,4.9747269056431677E-3,2.1251764578237542,-152843.68211200001,5333.4432197968008,1.4124631024484383E-3,-0.21272405986575513,-153655.78087821839,10505.612481348415,-2.5464709356542352,8.8098742929681589E-3,3.0545055701875454,-151969.37334836519,3983.5582529892836]
["KBM","KBMS-25H01-E (120 V)",5.09,10.44,3.6221469807121007,7.2733875114700819,2900,15.32,3815,0.75,3.4,30,0.434,160,10,3815,3815,3815,3.1590140453160913,259.21658986175117,1.9528801951934103,1.9046892311227155,3.3374562116255904E-2,-22.617085210864197,9,29.179839020800003,9,-2359.2896959999998,7.5,2371.2896959999998,9,0.84762870928855749,1.2468791723033401,20.34308902292538,59.850200270560322,44.809719927082369,23.041430996654391,2.4220690280242105,148.3741545315572,3.2469255087942362E-3,1.2245728517823724,-153247.45036963266,6684.0723498953557,9.064733254580831E-4,-6.4312989210696711E-2,-153662.85106650522,13055.40104106591,-1.6502720725860112,5.6726633441243251E-3,1.7462860106993598,-152816.91254689882,5038.6575808907637]
["KBM","KBMS-25H01-E (240 V)",5.09,10.44,1.4421386680163577,2.8958607791493125,4900,15.32,6918,0.75,3.4,30,0.434,325,10,6684.0723498953557,6918,6918,-6.0184631563844349E-2,259.21658986175117,1.9549152760262754,1.9046892311227155,2.526941996542801E-2,-22.617085210864197,9,29.179839020800003,9,-2359.2896959999998,7.5,2371.2896959999998,9,0.84762870928855749,1.2468791723033401,20.34308902292538,59.850200270560322,44.809719927082369,23.041430996654391,2.4220690280242105,148.3741545315572,3.2469255087942362E-3,1.2245728517823724,-153247.45036963266,6684.0723498953557,1.003764727610282E-3,-0.2574896930932018,-153645.583071653,12501.045409573962,-6.607188605373965,5.6726633441243251E-3,1.7462860106993598,-152816.91254689882,5038.6575808907637]
["KBM","KBMS-25H01-F (120 V)",4.63,12,2.4658943081579734,6.2905467044846262,3950,15.73,4765,0.56000000000000005,2.1,23.7,0.434,160,10,4765,4765,4765,2.0193762983222134,259.21658986175117,2.147804979981315,1.8550438029752068,2.6720662009132479E-2,-22.617085210864197,9,29.179839020800003,9,-2359.2896959999998,7.5,2371.2896959999998,9,1.0710831732774155,1.5755852603023761,25.705996158657975,75.62809249451405,56.622594878193013,23.041430996654388,2.4220690280242105,148.3741545315572,2.0688350544394588E-3,0.93718640071617698,-153273.07335465855,8383.8392899637893,6.2455388671766503E-4,-0.19140314347884466,-153647.69422486887,15838.747164404838,-8.3263002118182285,3.4689015395585436E-3,1.3016276588528888,-152909.92098742595,6454.3296260716206]
["KBM","KBMS-25H02-A (120 V)",8.6999999999999993,3.33,8.0801740338962258,3.0262824096989611,390,29.4,707,8.9600000000000009,45,162,0.67800000000000005,160,10,707,707,707,7.576366774268287,165.92920353982299,1.1451591720301457,0.99421497665306136,0.18009045894415313,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.15824686844930272,0.23308341629379314,3.7979248427832655,11.188003982102071,8.3742867807637129,23.051365115686874,2.4306362028790298,148.89897331710799,7.8970404630503171E-2,28.291499266412547,-146039.31501732377,1192.5062070467523,2.7652128251120685E-2,4.6234161923159816,-153460.37272055165,2273.658430231148,1.8389898748961822,5.544375411464067E-2,21.053847892156774,-149441.46807778851,1462.834105805794]
["KBM","KBMS-25H02-A (240 V)",8.6999999999999993,3.33,8.0691556147590937,3.0221556609584623,1000,29.4,1484,8.9600000000000009,45,162,0.67800000000000005,325,10,1192.5062070467523,1484,1484,7.7638269323024955,165.92920353982299,1.1423557062038898,0.99421497665306136,8.7039230195812653E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.15824686844930272,0.23308341629379314,3.7979248427832655,11.188003982102071,8.3742867807637129,23.051365115686874,2.4306362028790298,148.89897331710799,7.8970404630503171E-2,28.291499266412547,-146039.31501732377,1192.5062070467523,2.9371349624219775E-2,6.8901726109948918,-153211.75873905176,2169.6526720753591,2.7406050290184676,5.544375411464067E-2,21.053847892156774,-149441.46807778851,1462.834105805794]
["KBM","KBMS-25H02-A (400 V)",8.6999999999999993,3.33,7.5170103891095179,2.8153596962956997,1950,29.4,2482,8.9600000000000009,45,162,0.67800000000000005,565,10,1192.5062070467523,2159.2573549353597,2419.7530864197533,7.3900620419859528,165.92920353982299,1.1422851485479819,0.99421497665306136,8.7039230195812653E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.15824686844930272,0.23308341629379314,3.7979248427832655,11.188003982102071,8.3742867807637129,23.051365115686874,2.4306362028790298,148.89897331710799,7.8970404630503171E-2,28.291499266412547,-146039.31501732377,1192.5062070467523,2.9566231827116322E-2,7.1016105331379134,-153183.57712082405,2159.2573549353597,2.8247056554419196,5.544375411464067E-2,21.053847892156774,-149441.46807778851,1462.834105805794]
["KBM","KBMS-25H02-A (480 V)",8.6999999999999993,3.33,7.4404935895461071,2.7867017189311265,2400,29.4,2982,8.9600000000000009,45,162,0.67800000000000005,679,10,{"$f":"IF(AQ955<I955,IF(AQ955<0,0,AQ955),I955)","v":1192.5062070467523},{"$f":"IF(AU955<I955,IF(AU955<0,0,AU955),I955)","v":2150.2987083140774},{"$f":"IF(UAC_V*0.98/L955*1000<I955,IF(UAC_V*0.98/L955*1000<0,0,UAC_V*0.98/L955*1000),I955)","v":2419.7530864197533},{"$f":"C955+(E955-C955)/G955*Q955","v":7.5715354135365391},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M955,(inertia/gear^2+gear_inertia)/M955),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M955,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M955))","v":165.92920353982299},{"$f":"IF((C955+(E955-C955)/G955*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X955^2*time1+Y955^2*time2+Z955^2*time3+AA955^2*time4)/time)/(C955+(E955-C955)/G955*mspeed),SQRT((((X955-Y955)*2/PI()+Y955)^2*time1+Y955^2*time2+((Z955-Y955)*2/PI()+Y955)^2*time3+AA955^2*time4)/time)/(C955+(E955-C955)/G955*mspeed)),IF(AccType=1,SQRT((X955^2*time1+Y955^2*time2+Z955^2*time3+AA955^2*time4+AB955^2*time5+AC955^2*time6+AD955^2*time7+AE955^2*time8)/time)/(C955+(E955-C955)/G955*mspeed),SQRT((((X955-Y955)*2/PI()+Y955)^2*time1+Y955^2*time2+((Z955-Y955)*2/PI()+Y955)^2*time3+AA955^2*time4+((AB955-AC955)*2/PI()+AC955)^2*time5+AC955^2*time6+((AD955-AC955)*2/PI()+AC955)^2*time7+AE955^2*time8)/time)/(C955+(E955-C955)/G955*mspeed))))","v":1.1420463540065295},{"$f":"IF(move1,MAX(ABS(X955),ABS(Z955))/H955,MAX(ABS(X955),ABS(Z955),ABS(AB955),ABS(AD955))/H955)","v":0.99421497665306136},{"$f":"IF(AZ955>0,speed/(MIN(AZ955,I955)),\"NA\")","v":8.7039230195812653E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M955+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M955+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.678913967407407},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M955+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M955+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.229920313600001},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M955+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M955+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2364.400032},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M955+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M955+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2376.400032},9,{"$f":"AH955/Irms","v":0.15824686844930272},{"$f":"AI955/Ipeak","v":0.23308341629379314},{"$f":"IF(move1,IF(AccType=1,SQRT((X955^2*time1+Y955^2*time2+Z955^2*time3+AA955^2*time4)/time)/(C955/D955),SQRT((((X955-Y955)*2/PI()+Y955)^2*time1+Y955^2*time2+((Z955-AA955)*2/PI()+AA955)^2*time3+AA955^2*time4)/time)/(C955/D955)),IF(AccType=1,SQRT((X955^2*time1+Y955^2*time2+Z955^2*time3+AA955^2*time4+AB955^2*time5+AC955^2*time6+AD955^2*time7+AE955^2*time8)/time)/(C955/D955),SQRT((((X955-Y955)*2/PI()+Y955)^2*time1+Y955^2*time2+((Z955-AA955)*2/PI()+AA955)^2*time3+AA955^2*time4+((AB955-AC955)*2/PI()+AC955)^2*time5+AC955^2*time6+((AD955-AE955)*2/PI()+AE955)^2*time7+AE955^2*time8)/time)/(C955/D955)))","v":3.7979248427832655},{"$f":"IF(move1,MAX(ABS(X955),ABS(Z955))/(C955/D955),MAX(ABS(X955),ABS(Z955),ABS(AB955),ABS(AD955))/(C955/D955))","v":11.188003982102071},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X955),ABS(Z955))/(C955/D955),MAX(ABS((X955-Y955)*2/PI()+Y955),ABS((Z955-Y955)*2/PI()+Y955))/(C955/D955)),IF(AccType=1,MAX(ABS(X955),ABS(Z955),ABS(AB955),ABS(AD955))/(C955/D955),MAX(ABS((X955-Y955)*2/PI()+Y955),ABS((Z955-Y955)*2/PI()+Y955),ABS((AB955-AC955)*2/PI()+AC955),ABS((AD955-AC955)*2/PI()+AC955))/(C955/D955)))","v":8.3742867807637129},{"$f":"IF((C955+(E955-C955)/G955*mspeed)<0,\"NA\",U955*(C955+(E955-C955)/G955*mspeed)*mspeed/9.55)","v":23.051365115686874},{"$f":"IF(move1,IF(speed1>speed2,AM955/2*time1/time,AM955/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z955*-speed/30*PI(),((Z955-AA955)*2/PI()+AA955)*-speed/30*PI()),IF(AccType=1,X955*-speed/30*PI(),((X955-Y955)*2/PI()+Y955)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z955*-speed/30*PI(),((Z955-AA955)*2/PI()+AA955)*-speed/30*PI()),IF(AccType=1,X955*-speed/30*PI(),((X955-Y955)*2/PI()+Y955)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD955*-speed/30*PI(),((AD955-AE955)*2/PI()+AE955)*-speed/30*PI()),IF(AccType=1,AB955*-speed/30*PI(),((AB955-AC955)*2/PI()+AC955)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD955*-speed/30*PI(),((AD955-AE955)*2/PI()+AE955)*-speed/30*PI()),IF(AccType=1,AB955*-speed/30*PI(),((AB955-AC955)*2/PI()+AC955)*-speed/30*PI()),0)/2*time7/time)))","v":2.4306362028790298},{"$f":"IF(move1,MAX(IF(AccType=1,Z955*-speed/30*PI(),((Z955-AA955)*2/PI()+AA955)*-speed/30*PI()),IF(AccType=1,X955*-speed/30*PI(),((X955-Y955)*2/PI()+Y955)*-speed/30*PI()),0),MAX(IF(AccType=1,Z955*-speed/30*PI(),((Z955-AA955)*2/PI()+AA955)*-speed/30*PI()),IF(AccType=1,X955*-speed/30*PI(),((X955-Y955)*2/PI()+Y955)*-speed/30*PI()),IF(AccType=1,AD955*-speed/30*PI(),((AD955-AE955)*2/PI()+AE955)*-speed/30*PI()),IF(AccType=1,AB955*-speed/30*PI(),((AB955-AC955)*2/PI()+AC955)*-speed/30*PI()),0))","v":148.89897331710799},{"$f":"(L955^2)/1000000+((K955/1000)^2*(D955/C955*H955)^2*PI()*PI()*(O955/2)^2)/1200","v":7.8970404630503171E-2},{"$f":"SQRT(3)*L955*J955*D955/C955*H955/1000","v":28.291499266412547},{"$f":"0.75*J955^2*(D955/C955*H955)^2-(UAC_V*0.98)^2","v":-146039.31501732377},{"$f":"-AO955/2/AN955+SQRT((AO955/2/AN955)^2-AP955/AN955)","v":1192.5062070467523},{"$f":"(L955^2)/1000000+((K955/1000)^2*AV955^2*PI()*PI()*(O955/2)^2)/1200","v":2.9737466374039338E-2},{"$f":"SQRT(3)*L955*J955*AV955/1000","v":7.2823268524686267},{"$f":"0.75*J955^2*AV955^2-(UAC_V*0.98)^2","v":-153158.81515407155},{"$f":"-AS955/2/AR955+SQRT((AS955/2/AR955)^2-AT955/AR955)","v":2150.2987083140774},{"$f":"D955+(F955-D955)*((0.85*UAC_V-D955*J955)/L955*1000)/G955","v":2.8965865910215505},{"$f":"(L955^2)/1000000+((K955/1000)^2*AJ955^2*PI()*PI()*(O955/2)^2)/1200","v":5.544375411464067E-2},{"$f":"SQRT(3)*L955*J955*AJ955/1000","v":21.053847892156774},{"$f":"0.75*J955^2*AJ955^2-(UAC_V*0.98)^2","v":-149441.46807778851},{"$f":"IF(((AX955/2/AW955)^2-AY955/AW955)>0,-AX955/2/AW955+SQRT((AX955/2/AW955)^2-AY955/AW955),-9999)","v":1462.834105805794}]
["KBM","KBMS-25H02-B (120 V)",8.75,5.18,8.0214091318315255,4.6636099603671664,750,29.7,1098,3.7,19,104,0.67800000000000005,160,10,1098,1098,1098,7.6833429690013535,165.92920353982299,1.1368008503480278,0.98417240113131321,0.11595988567715507,-22.678913967407407,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},29.229920313600001,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},-2364.400032,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},2376.400032,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},0.24475515653492153,0.3605023505344,5.8741237568381166,17.304112825651199,12.952230220914538,23.051365115686874,2.4306362028790298,148.89897331710799,3.3762794270852589E-2,11.718549173790825,-150489.89694113919,1944.8030327709869,1.1509201863706504E-2,2.0367733159706503,-153568.11322252566,3565.4040365460501,3.0559553592876858,2.3268450395245589E-2,8.6325727292091319,-151941.52145143572,2376.5987109371663]
["KBM","KBMS-25H02-B (240 V)",8.75,5.18,7.6956096012669404,4.4741916286435703,1700,29.7,2303,3.7,19,104,0.67800000000000005,325,10,1944.8030327709869,2303,2303,7.321611124539861,165.92920353982299,1.1357868835874787,0.98417240113131321,5.5286128733615401E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.24475515653492153,0.3605023505344,5.8741237568381166,17.304112825651199,12.952230220914538,23.051365115686874,2.4306362028790298,148.89897331710799,3.3762794270852589E-2,11.718549173790825,-150489.89694113919,1944.8030327709869,1.1944533254788855E-2,2.5987829949010828,-153507.89624041726,3477.7954492784393,3.8991893494583216,2.3268450395245589E-2,8.6325727292091319,-151941.52145143572,2376.5987109371663]
["KBM","KBMS-25H02-B (400 V)",8.75,5.18,6.7906109052542005,3.9480295960780238,3150,29.7,3845,3.7,19,104,0.67800000000000005,565,10,1944.8030327709869,3469.6120037877195,3769.2307692307691,6.5918031989775301,165.92920353982299,1.1357920715476388,0.98417240113131321,5.3574023198602383E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.24475515653492153,0.3605023505344,5.8741237568381166,17.304112825651199,12.952230220914538,23.051365115686874,2.4306362028790298,148.89897331710799,3.3762794270852589E-2,11.718549173790825,-150489.89694113919,1944.8030327709869,1.198794278886975E-2,2.6482930531648887,-153501.89163980581,3469.6120037877195,3.9734737711480363,2.3268450395245589E-2,8.6325727292091319,-151941.52145143572,2376.5987109371663]
["KBM","KBMS-25H02-B (480 V)",8.75,5.18,6.0876765732649973,3.5393468449215102,4000,29.7,4614,3.7,19,104,0.67800000000000005,679,10,1944.8030327709869,3476.0956985344624,3769.2307692307691,6.4363772470547325,165.92920353982299,1.1359177083189396,0.98417240113131321,5.3574023198602383E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.24475515653492153,0.3605023505344,5.8741237568381166,17.304112825651199,12.952230220914538,23.051365115686874,2.4306362028790298,148.89897331710799,3.3762794270852589E-2,11.718549173790825,-150489.89694113919,1944.8030327709869,1.1953512052455815E-2,2.609100687412218,-153506.65425302665,3476.0956985344624,3.9146699174123745,2.3268450395245589E-2,8.6325727292091319,-151941.52145143572,2376.5987109371663]
["KBM","KBMS-25H02-C (120 V)",8.75,6.5,7.9912534584035866,5.7907633756547732,950,29.7,1380,2.35,12,83.4,0.67800000000000005,160,10,1380,1380,1380,7.6478208132599468,165.92920353982299,1.1363018354203602,0.98417240113131321,9.2263735125736421E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.30712519642412928,0.45236781437714285,7.3710047141791026,21.713655090102858,16.252798539757624,23.051365115686874,2.4306362028790298,148.89897331710799,2.1368232093066306E-2,7.4895598082909327,-151647.86089251022,2494.505989375738,7.337838989681553E-3,1.2197596284211623,-153610.52430749193,4493.0123449513167,3.593186131004622,1.4776830465209091E-2,5.5172503691357671,-152569.90938631367,3031.977388964061]
["KBM","KBMS-25H02-C (240 V)",8.75,6.5,7.4617759365874656,5.4070840120199026,2150,29.7,2895,2.35,12,83.4,0.67800000000000005,325,10,2494.505989375738,2895,2895,7.015391319265448,165.92920353982299,1.1357261545140895,0.98417240113131321,4.3980640578071252E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.30712519642412928,0.45236781437714285,7.3710047141791026,21.713655090102858,16.252798539757624,23.051365115686874,2.4306362028790298,148.89897331710799,2.1368232093066306E-2,7.4895598082909327,-151647.86089251022,2494.505989375738,7.5606839064013415E-3,1.5346388756595384,-153579.35129886432,4406.636928024066,4.5207621203678707,1.4776830465209091E-2,5.5172503691357671,-152569.90938631367,3031.977388964061]
["KBM","KBMS-25H02-C (400 V)",8.75,6.5,6.0399300903374282,4.3767609350271224,4000,29.7,4826,2.35,12,83.4,0.67800000000000005,565,10,2494.505989375738,4415.235536774805,4700.2398081534775,5.7586007569284323,165.92920353982299,1.135952146924025,0.98417240113131321,4.1993701845190599E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.30712519642412928,0.45236781437714285,7.3710047141791026,21.713655090102858,16.252798539757624,23.051365115686874,2.4306362028790298,148.89897331710799,2.1368232093066306E-2,7.4895598082909327,-151647.86089251022,2494.505989375738,7.537482105573764E-3,1.5049305823702706,-153582.59691894855,4415.235536774805,4.4332469862910138,1.4776830465209091E-2,5.5172503691357671,-152569.90938631367,3031.977388964061]
["KBM","KBMS-25H02-C (480 V)",8.75,6.5,4.8414933688554562,3.5083285281561278,5000,29.7,5791,2.35,12,83.4,0.67800000000000005,679,10,2494.505989375738,4440.5276033819109,4700.2398081534775,5.2788336832802827,165.92920353982299,1.1362528186967695,0.98417240113131321,4.1993701845190599E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.30712519642412928,0.45236781437714285,7.3710047141791026,21.713655090102858,16.252798539757624,23.051365115686874,2.4306362028790298,148.89897331710799,2.1368232093066306E-2,7.4895598082909327,-151647.86089251022,2494.505989375738,7.4705072927413975E-3,1.4156810862161993,-153591.96579506644,4440.5276033819109,4.1703344875431618,1.4776830465209091E-2,5.5172503691357671,-152569.90938631367,3031.977388964061]
["KBM","KBMS-25H02-D (120 V)",8.6199999999999992,8,7.7953441514397719,7.0228325688646587,1225,29.8,1717,1.57,7.8,67,0.67800000000000005,160,10,1717,1717,1717,7.4641354351200722,165.92920353982299,1.1531007313809614,0.98086980918120803,7.4154894859357168E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.38370094145438255,0.56515700529002333,9.2088225949051807,27.127536253921118,20.305120431608675,23.051365115686874,2.4306362028790298,148.89897331710799,1.4057540157768531E-2,5.0388806019076311,-152249.97027621514,3116.6232925234358,4.6994494575990581E-3,0.74728304918279265,-153632.89998019626,5638.7091612250952,4.101569251892097,9.6467329578765939E-3,3.6994797303877234,-152901.79515061542,3794.0869818711853]
["KBM","KBMS-25H02-D (240 V)",8.6199999999999992,8,6.9736147541916713,6.2825358145870904,2725,29.8,3597,1.57,7.8,67,0.67800000000000005,325,10,3116.6232925234358,3597,3597,6.4467714755330068,165.92920353982299,1.1528956015256069,0.98086980918120803,3.5397262850574443E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.38370094145438255,0.56515700529002333,9.2088225949051807,27.127536253921118,20.305120431608675,23.051365115686874,2.4306362028790298,148.89897331710799,1.4057540157768531E-2,5.0388806019076311,-152249.97027621514,3116.6232925234358,4.791791456787548E-3,0.89636116935619969,-153619.25376776958,5569.2937863000743,4.9198057079468542,9.6467329578765939E-3,3.6994797303877234,-152901.79515061542,3794.0869818711853]
["KBM","KBMS-25H02-D (400 V)",8.6199999999999992,8,4.4612543893712751,4.0191480985326802,5180,29.8,5995,1.57,7.8,67,0.67800000000000005,565,10,3116.6232925234358,5627.1628417135989,5850.746268656716,4.1022512030367775,165.92920353982299,1.1534863312899279,0.98086980918120803,3.355852279662868E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.38370094145438255,0.56515700529002333,9.2088225949051807,27.127536253921118,20.305120431608675,23.051365115686874,2.4306362028790298,148.89897331710799,1.4057540157768531E-2,5.0388806019076311,-152249.97027621514,3116.6232925234358,4.7143399008942842E-3,0.77326842204578106,-153630.69948471079,5627.1628417135989,4.2441936650248966,9.6467329578765939E-3,3.6994797303877234,-152901.79515061542,3794.0869818711853]
["KBM","KBMS-25H02-D (480 V)",8.6199999999999992,8,2.8488734813449264,2.5665526858963297,6000,29.8,7193,1.57,7.8,67,0.67800000000000005,679,10,3116.6232925234358,5679.2397708312928,5850.746268656716,3.1573981254591601,165.92920353982299,1.1539595682556307,0.98086980918120803,3.355852279662868E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.38370094145438255,0.56515700529002333,9.2088225949051807,27.127536253921118,20.305120431608675,23.051365115686874,2.4306362028790298,148.89897331710799,1.4057540157768531E-2,5.0388806019076311,-152249.97027621514,3116.6232925234358,4.6488202397724819E-3,0.65121907745134822,-153640.38191764109,5679.2397708312928,3.5743084862435177,9.6467329578765939E-3,3.6994797303877234,-152901.79515061542,3794.0869818711853]
["KBM","KBMS-25H02-E (120 V)",8.85,10.199999999999999,7.8184865793893579,8.7848163813363573,1600,29.8,2143,0.96,5,54,0.67800000000000005,160,10,2143,2143,2143,7.4684167122696214,165.92920353982299,1.1230021335745954,0.98086980918120803,5.9413884495341233E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.47650454204004417,0.70184836911186432,11.43610900896106,33.688721717369489,25.216206339389277,23.051365115686874,2.4306362028790298,148.89897331710799,8.9797996966562328E-3,3.0838893371993312,-152848.6387650813,3957.5574936335047,3.0340101497143687E-3,0.43021548935557813,-153648.13191295599,7045.7687550613282,4.7913778662999542,6.1845716974301378E-3,2.264150908717423,-153224.49559864146,4797.7936483238091]
["KBM","KBMS-25H02-E (240 V)",8.85,10.199999999999999,6.5120897548433847,7.3169547807229041,3600,29.8,4480,0.96,5,54,0.67800000000000005,325,10,3957.5574936335047,4480,4480,5.940600583805101,165.92920353982299,1.1230154534126859,0.98086980918120803,2.8420525552124168E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.47650454204004417,0.70184836911186432,11.43610900896106,33.688721717369489,25.216206339389277,23.051365115686874,2.4306362028790298,148.89897331710799,8.9797996966562328E-3,3.0838893371993312,-152848.6387650813,3957.5574936335047,3.0605500849525047E-3,0.47614095370788578,-153644.56325378962,7007.9501022700379,5.3028570176592016,6.1845716974301378E-3,2.264150908717423,-153224.49559864146,4797.7936483238091]
["KBM","KBMS-25H02-E (400 V)",8.85,10.199999999999999,2.9443664472000637,3.3082769069663636,6000,29.8,"",0.96,5,54,0.67800000000000005,565,10,3957.5574936335047,7147.507999926459,7259.2592592592591,1.8149061561213902,165.92920353982299,1.1239604884112133,0.98086980918120803,2.6538022225695151E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.47650454204004417,0.70184836911186432,11.43610900896106,33.688721717369489,25.216206339389277,23.051365115686874,2.4306362028790298,148.89897331710799,8.9797996966562328E-3,3.0838893371993312,-152848.6387650813,3957.5574936335047,2.9678587304904289E-3,0.28519197605017149,-153657.02688072674,7147.507999926459,3.1762280891837928,6.1845716974301378E-3,2.264150908717423,-153224.49559864146,4797.7936483238091]
["KBM","KBMS-25H02-F (120 V)",8.93,12.74,7.639437268410977,10.669605123479018,2100,30.1,2666,0.61,3.2,43.3,0.67800000000000005,160,10,2666,2666,2666,7.2915998845636496,165.92920353982299,1.1128420340792722,0.9710936981262458,4.7758422533201901E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.58983170421879261,0.86876909480044795,14.155960901251023,41.700916550421503,31.213381294159383,23.051365115686874,2.4306362028790298,148.89897331710799,5.7575324103834452E-3,1.9645488096689794,-153149.3762053278,4989.7163539131598,1.9312868643388522E-3,0.23676996249479956,-153656.52489277508,8858.6503788610935,5.1754515421341818,3.9262415783708282E-3,1.4279703052357142,-153392.10415642583,6071.2698413604685]
["KBM","KBMS-25H02-F (240 V)",8.93,12.74,5.6022539968347154,7.8243770905512786,4500,30.1,5564,0.61,3.2,43.3,0.67800000000000005,325,10,4989.7163539131598,5564,5564,4.8154269418640796,165.92920353982299,1.1131881166355215,0.9710936981262458,2.288352884139401E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.58983170421879261,0.86876909480044795,14.155960901251023,41.700916550421503,31.213381294159383,23.051365115686874,2.4306362028790298,148.89897331710799,5.7575324103834452E-3,1.9645488096689794,-153149.3762053278,4989.7163539131598,1.9148898061164185E-3,0.19940133863754547,-153658.69823644983,8905.9950216216039,4.3586270601279153,3.9262415783708282E-3,1.4279703052357142,-153392.10415642583,6071.2698413604685]
["KBM","KBMS-25H02-G (120 V)",8.74,14.37,7.341021750113673,11.615540743850747,2400,30,3027,0.49,2.5,38.200000000000003,0.67800000000000005,160,10,3027,3027,3027,6.9755386823308703,165.92920353982299,1.1369805729322187,0.97433067711999999,4.2062753377441781E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.67975980259424318,1.0012251022750571,16.314235262261835,48.058804909202742,35.972298123442599,23.051365115686874,2.4306362028790298,148.89897331710799,4.5858355526250377E-3,1.5991406403466366,-153225.88653209747,5608.6583819447242,1.483742185209655E-3,0.1415641275568448,-153660.56663704893,10128.990042004445,4.366496802678645,3.1221735423393009E-3,1.1662408631413475,-153430.98182772184,6825.881386586243]
["KBM","KBMS-25H02-G (240 V)",8.74,14.37,4.3692536263907114,6.9133759911245436,5300,30,6316,0.49,2.5,38.200000000000003,0.67800000000000005,325,10,5608.6583819447242,6316,6316,3.5313897932610816,165.92920353982299,1.137679798860562,0.97433067711999999,2.0158954159834749E-2,-22.678913967407407,9,29.229920313600001,9,-2364.400032,7.5,2376.400032,9,0.67975980259424318,1.0012251022750571,16.314235262261835,48.058804909202742,35.972298123442599,23.051365115686874,2.4306362028790298,148.89897331710799,4.5858355526250377E-3,1.5991406403466366,-153225.88653209747,5608.6583819447242,1.464945669019559E-3,6.831311594752025E-2,-153663.20049446792,10218.46079764567,2.1070945550530471,3.1221735423393009E-3,1.1662408631413475,-153430.98182772184,6825.881386586243]
["KBM","KBMS-25H03-A (120 V)",11.86,5.3,11.285532328334398,4.9281800560412217,550,42.2,827,3.97,21,139,0.93099999999999994,160,10,827,827,827,10.996209519150085,120.83780880773362,0.83864941141879745,0.69388267457819908,0.15395883249518291,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.1848398838996359,0.27261417755087125,4.4361572135912617,13.08548052244182,9.7919627190440064,23.061683764075173,2.4395193800850512,149.44315017261758,5.1569116979886337E-2,18.024763117748442,-149460.12745909963,1536.6078992554526,2.0595275169771693E-2,3.5830180496259696,-153497.88517230027,2644.4289247351535,3.748720503529785,2.8015339608531975E-2,9.3591344381539052,-152530.60372869627,2172.2887543519437]
["KBM","KBMS-25H03-A (240 V)",11.86,5.3,11.018419137131216,4.8115367411053347,1300,42.2,1735,3.97,21,139,0.93099999999999994,325,10,1536.6078992554526,1735,1735,10.736813233017431,120.83780880773362,0.83802564945966718,0.69388267457819908,7.3385564538049716E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.1848398838996359,0.27261417755087125,4.4361572135912617,13.08548052244182,9.7919627190440064,23.061683764075173,2.4395193800850512,149.44315017261758,5.1569116979886337E-2,18.024763117748442,-149460.12745909963,1536.6078992554526,2.1106797944968027E-2,4.2416374520940385,-153431.20293624804,2597.5513817883689,4.4377988234987074,2.8015339608531975E-2,9.3591344381539052,-152530.60372869627,2172.2887543519437]
["KBM","KBMS-25H03-A (400 V)",11.86,5.3,9.9869726790164322,4.3611234406185293,2400,42.2,2899,3.97,21,139,0.93099999999999994,565,10,1536.6078992554526,2600.0443571597552,2820.1438848920861,9.8308524513627589,120.83780880773362,0.83823454407891174,0.69388267457819908,5.8612812969010962E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.1848398838996359,0.27261417755087125,4.4361572135912617,13.08548052244182,9.7919627190440064,23.061683764075173,2.4395193800850512,149.44315017261758,5.1569116979886337E-2,18.024763117748442,-149460.12745909963,1536.6078992554526,2.107836527132264E-2,4.2077352424953629,-153434.90942664797,2600.0443571597552,4.4023287514875467,2.8015339608531975E-2,9.3591344381539052,-152530.60372869627,2172.2887543519437]
["KBM","KBMS-25H03-A (480 V)",11.86,5.3,9.3846535409358971,4.09810198294144,2900,42.2,3479,3.97,21,139,0.93099999999999994,679,10,1536.6078992554526,2603.7784812154614,2820.1438848920861,9.6374986745986213,120.83780880773362,0.83834941408572061,0.69388267457819908,5.8612812969010962E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.1848398838996359,0.27261417755087125,4.4361572135912617,13.08548052244182,9.7919627190440064,23.061683764075173,2.4395193800850512,149.44315017261758,5.1569116979886337E-2,18.024763117748442,-149460.12745909963,1536.6078992554526,2.1036030724186586E-2,4.1567445685157649,-153440.42816872982,2603.7784812154614,4.3489799314736262,2.8015339608531975E-2,9.3591344381539052,-152530.60372869627,2172.2887543519437]
["KBM","KBMS-25H03-B (120 V)",11.84,7.27,10.742958658702936,6.4716618425921304,800,42.3,1144,2.1,11.4,100,0.93099999999999994,160,10,1144,1144,1144,10.271230881945197,120.83780880773362,0.8405846030320917,0.69224229000472814,0.1112971630013254,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.25397280465277899,0.3745760157385698,6.0953473116666963,17.97964875545135,13.454305328180077,23.061683764075173,2.4395193800850512,149.44315017261758,2.8026622426156465E-2,9.4471975711842582,-151432.76145127526,2162.0355844575142,1.0433862742216306E-2,1.4656220666618673,-153610.29879894285,3767.3717961543398,4.0294156891308797,1.4837163522009037E-2,4.8937434858800364,-153065.28186736017,3051.2225142357938]
["KBM","KBMS-25H03-B (240 V)",11.84,7.27,10.02022080068974,6.0362775907769519,1825,42.3,2399,2.1,11.4,100,0.93099999999999994,325,10,2162.0355844575142,2399,2399,9.447862849783391,120.83780880773362,0.83999415631331464,0.69224229000472814,5.3073761764700404E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.25397280465277899,0.3745760157385698,6.0953473116666963,17.97964875545135,13.454305328180077,23.061683764075173,2.4395193800850512,149.44315017261758,2.8026622426156465E-2,9.4471975711842582,-151432.76145127526,2162.0355844575142,1.0688176899723806E-2,1.8458476881723964,-153578.82115780172,3705.2848174621886,5.0747650459494356,1.4837163522009037E-2,4.8937434858800364,-153065.28186736017,3051.2225142357938]
["KBM","KBMS-25H03-B (400 V)",11.84,7.27,5.2661562052465376,3.1723832561726133,3400,42.3,4000,2.1,11.4,100,0.93099999999999994,565,10,2162.0355844575142,3803.0268751757112,3920,4.4869104045133819,120.83780880773362,0.84147331584759455,0.69224229000472814,4.1728832911881453E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.25397280465277899,0.3745760157385698,6.0953473116666963,17.97964875545135,13.454305328180077,23.061683764075173,2.4395193800850512,149.44315017261758,2.8026622426156465E-2,9.4471975711842582,-151432.76145127526,2162.0355844575142,1.0301030167183634E-2,1.2208177263761331,-153626.74010197414,3803.0268751757112,3.3563782997844158,1.4837163522009037E-2,4.8937434858800364,-153065.28186736017,3051.2225142357938]
["KBM","KBMS-25H03-B (480 V)",11.84,7.27,6.6499920800324466,4.006019325320751,4150,42.3,4800,2.1,11.4,100,0.93099999999999994,679,10,2162.0355844575142,3727.4565184104436,3920,7.1784267826783417,120.83780880773362,0.84039404596885292,0.69224229000472814,4.1728832911881453E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.25397280465277899,0.3745760157385698,6.0953473116666963,17.97964875545135,13.454305328180077,23.061683764075173,2.4395193800850512,149.44315017261758,2.8026622426156465E-2,9.4471975711842582,-151432.76145127526,2162.0355844575142,1.0594306353178483E-2,1.7153431130487291,-153590.43995011289,3727.4565184104436,4.7159705146250204,1.4837163522009037E-2,4.8937434858800364,-153065.28186736017,3051.2225142357938]
["KBM","KBMS-25H03-C (120 V)",11.9,8.1999999999999993,10.769484482551585,7.2278419345983789,900,42.4,1276,1.66,9.1,90,0.93099999999999994,160,10,1276,1276,1276,10.297180221928691,120.83780880773362,0.83615549393945521,0.6906096430943397,9.9783663380498641E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.28501741539570941,0.42036267631484586,6.8404179694970253,20.177408463112602,15.098905317147102,23.061683764075173,2.4395193800850512,149.44315017261758,2.26347239484481E-2,7.5603860555854405,-151899.81983612682,2428.9135688196961,8.4123043512300474E-3,1.1082292183040663,-153626.09345678077,4208.0524417693268,4.282707078391307,1.1981791601926721E-2,3.9071194295068152,-153192.84005443117,3416.3488700726371]
["KBM","KBMS-25H03-C (240 V)",11.9,8.1999999999999993,9.8753701274580923,6.6277651862134848,2050,42.4,2676,1.66,9.1,90,0.93099999999999994,325,10,2428.9135688196961,2676,2676,9.257117298086758,120.83780880773362,0.83573615043191363,0.6906096430943397,4.7579953091747486E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.28501741539570941,0.42036267631484586,6.8404179694970253,20.177408463112602,15.098905317147102,23.061683764075173,2.4395193800850512,149.44315017261758,2.26347239484481E-2,7.5603860555854405,-151899.81983612682,2428.9135688196961,8.5999469531840862E-3,1.4021760393026821,-153603.31797391374,4145.4868600693262,5.4186527024273552,1.1981791601926721E-2,3.9071194295068152,-153192.84005443117,3416.3488700726371]
["KBM","KBMS-25H03-C (400 V)",11.9,8.1999999999999993,7.4635291734146705,5.0090799821574974,3800,42.4,4459,1.66,9.1,90,0.93099999999999994,565,10,2428.9135688196961,4160.7603526307767,4355.5555555555547,7.042344231352808,120.83780880773362,0.83601701767205261,0.6906096430943397,3.7269014177351609E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.28501741539570941,0.42036267631484586,6.8404179694970253,20.177408463112602,15.098905317147102,23.061683764075173,2.4395193800850512,149.44315017261758,2.26347239484481E-2,7.5603860555854405,-151899.81983612682,2428.9135688196961,8.5524340414915093E-3,1.3338844680192115,-153609.0849452462,4160.7603526307767,5.1547426819193607,1.1981791601926721E-2,3.9071194295068152,-153192.84005443117,3416.3488700726371]
["KBM","KBMS-25H03-C (480 V)",11.9,8.1999999999999993,5.2243241637149138,3.5062578279965866,4725,42.4,5351,1.66,9.1,90,0.93099999999999994,679,10,2428.9135688196961,4191.564491416907,4355.5555555555547,5.9779839594534536,120.83780880773362,0.83640043944381948,0.6906096430943397,3.7269014177351609E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.28501741539570941,0.42036267631484586,6.8404179694970253,20.177408463112602,15.098905317147102,23.061683764075173,2.4395193800850512,149.44315017261758,2.26347239484481E-2,7.5603860555854405,-151899.81983612682,2428.9135688196961,8.4598957961167526E-3,1.1896767258783445,-153620.31695333036,4191.564491416907,4.5974576836311574,1.1981791601926721E-2,3.9071194295068152,-153192.84005443117,3416.3488700726371]
["KBM","KBMS-25H03-D (120 V)",11.9,10.24,10.663381187156988,8.9608245270226785,1200,42.6,1595,1.06,5.7,72.099999999999994,0.93099999999999994,160,10,1595,1595,1595,10.256327494596164,120.83780880773362,0.83580310893977272,0.68736734430046953,7.9826930704398918E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.35592418703073953,0.52494070798341741,8.542180488737749,25.197153983204036,18.855218347266625,23.061683764075173,2.4395193800850512,149.44315017261758,1.4175455120792279E-2,4.8524866773580868,-152531.60437547549,3113.5879934132313,5.3913178962383193E-3,0.71133249754351313,-153639.66592852134,5272.7525463276661,5.3736687637724874,7.5734523132938922E-3,2.495935300126976,-153364.40392050552,4338.2633675152902]
["KBM","KBMS-25H03-D (240 V)",11.9,10.24,9.1956189341983965,7.7274108690742835,2700,42.6,3338,1.06,5.7,72.099999999999994,0.93099999999999994,325,10,3113.5879934132313,3338,3338,8.5565837045756474,120.83780880773362,0.83575800224976771,0.68736734430046953,3.8143785042994691E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.35592418703073953,0.52494070798341741,8.542180488737749,25.197153983204036,18.855218347266625,23.061683764075173,2.4395193800850512,149.44315017261758,1.4175455120792279E-2,4.8524866773580868,-152531.60437547549,3113.5879934132313,5.4382463304319664E-3,0.79314964287930156,-153633.74621297669,5242.7067088522444,5.9917457386755864,7.5734523132938922E-3,2.495935300126976,-153364.40392050552,4338.2633675152902]
["KBM","KBMS-25H03-D (400 V)",11.9,10.199999999999999,5.0010749128257421,4.2025839603577664,4850,42.6,5560,1.06,5.7,72.099999999999994,0.93099999999999994,565,10,3121.6326928012982,5309.3687432366978,5436.8932038834955,4.3476418103557695,120.83780880773362,0.83641547619108192,0.68736734430046953,2.9310043532792349E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.35453385817515071,0.52289015834285713,8.508812596203617,25.098727600457142,18.781565150597615,23.061683764075173,2.4395193800850512,149.44315017261758,1.4105458934623991E-2,4.833531651274658,-152540.43393730611,3121.6326928012982,5.3369637662603773E-3,0.60284659940540364,-153646.52234710159,5309.3687432366978,4.5541261670996818,7.5549335354909569E-3,2.4861855528608552,-153366.73994340317,4344.0383952710627]
["KBM","KBMS-25H03-E (120 V)",11.8,12.7,10.269407475568853,10.80990260586195,1525,42.6,2006,0.69,3.6,57.4,0.93099999999999994,160,10,2006,2006,2006,9.7866435383548325,120.83780880773362,0.84285730685102456,0.68736734430046953,6.3471562549110808E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.44517033886682061,0.65656687961412419,10.684088132803694,31.515210221477961,23.583066975821016,23.061683764075173,2.4395193800850512,149.44315017261758,8.8965411141455411E-3,3.1452337211898,-152913.37664952004,3972.8357508514664,3.3767764324775722E-3,0.38057503238453844,-153653.01002233286,6689.4648679916218,5.5477729988906699,4.7768141722677746E-3,1.6177890623579017,-153465.40879379038,5501.2726921900512]
["KBM","KBMS-25H03-E (240 V)",11.8,12.7,8.0747728480446916,8.4997608926786228,3400,42.6,4193,0.69,3.6,57.4,0.93099999999999994,325,10,3972.8357508514664,4193,4193,7.2059183976033507,120.83780880773362,0.84300338207691905,0.68736734430046953,3.036583698390562E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.44517033886682061,0.65656687961412419,10.684088132803694,31.515210221477961,23.583066975821016,23.061683764075173,2.4395193800850512,149.44315017261758,8.8965411141455411E-3,3.1452337211898,-152913.37664952004,3972.8357508514664,3.3774678314679625E-3,0.38217579070360652,-153652.91737675885,6688.5488286995205,5.571107802870408,4.7768141722677746E-3,1.6177890623579017,-153465.40879379038,5501.2726921900512]
["KBM","KBMS-25H03-F (120 V)",11.75,14.79,9.936430230872384,12.20691674554347,1850,42,2347,0.51,2.7,49.4,0.93099999999999994,160,10,2347,2347,2347,9.4492171631662085,120.83780880773362,0.84641334063193707,0.69718687779047617,5.4249661045384007E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.52063674236699797,0.76786976018774478,12.495281816807951,36.857748489011747,27.580928227537179,23.061683764075173,2.4395193800850512,149.44315017261758,6.6296963679867288E-3,2.3069455819869047,-153118.79376831197,4634.981843088075,2.4839608818044093E-3,0.23534900718339147,-153658.32571883019,7817.8947162901541,5.3933004941987086,3.5806197451413507E-3,1.2035569096380661,-153515.6049645608,6381.9175947390322]
["KBM","KBMS-25H03-F (240 V)",11.75,14.79,6.7427350280639562,8.2834582654348363,4100,42,4902,0.51,2.7,49.4,0.93099999999999994,325,10,4634.981843088075,4902,4902,5.7632651481876858,120.83780880773362,0.84679935189537381,0.69718687779047617,2.5973878921565947E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.52063674236699797,0.76786976018774478,12.495281816807951,36.857748489011747,27.580928227537179,23.061683764075173,2.4395193800850512,149.44315017261758,6.6296963679867288E-3,2.3069455819869047,-153118.79376831197,4634.981843088075,2.4656792051405228E-3,0.17934520424414416,-153660.70492240024,7858.0063287233515,4.1099071980719639,3.5806197451413507E-3,1.2035569096380661,-153515.6049645608,6381.9175947390322]
["KBM","KBMS-25H03-G (120 V)",11.2,20,8.5422798546777301,14.856138877700401,2750,42,3324,0.28000000000000003,1.3,34.6,0.93099999999999994,160,10,3324,3324,3324,7.9875411770722824,120.83780880773362,0.88803471664495748,0.69718687779047617,3.8304438770612598E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.73861220453156406,1.0893544965476192,17.726692908757538,52.289015834285721,39.128260730411704,23.061683764075173,2.4395193800850512,149.44315017261758,3.1518043091219939E-3,1.2585081167795462,-153333.25,6778.1169748221164,1.1984438699627735E-3,3.2253932320982594E-2,-153663.78275331823,11309.953018095399,1.9221528187389829,1.7291779679991974E-3,0.65657644966252693,-153573.97597767811,9236.1400131705541]
["KBM","KBMS-25H03-G (240 V)",11.2,20,3.5388569699256727,6.1545338607403011,5100,42,6937,0.28000000000000003,1.3,34.6,0.93099999999999994,325,10,6778.1169748221164,6937,6937,0.77934329419105808,120.83780880773362,0.88897995178848821,0.69718687779047617,1.8354325280887453E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.73861220453156406,1.0893544965476192,17.726692908757538,52.289015834285721,39.128260730411704,23.061683764075173,2.4395193800850512,149.44315017261758,3.1518043091219939E-3,1.2585081167795462,-153333.25,6778.1169748221164,1.2106810194487652E-3,-0.10467111968701767,-153661.71207622695,11309.264960412585,-6.2378095713954558,1.7291779679991974E-3,0.65657644966252693,-153573.97597767811,9236.1400131705541]
["KBM","KBMS-25H03-H (120 V)",11,21.1,7.9793274858614645,15.198719020688504,2950,42.6,3642,0.25,1.1000000000000001,31.8,0.93099999999999994,160,10,3642,3642,3642,7.2707493910194758,120.83780880773362,0.90431744067739206,0.68736734430046953,3.4959899635781513E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.79340380079499651,1.1701647937460609,19.041691219079915,56.167910099810918,42.030866253685879,23.061683764075173,2.4395193800850512,149.44315017261758,2.6725191589977554E-3,1.1251932683351202,-153351.00311224174,7367.4173284860999,1.0112404717056555E-3,5.9957202112164711E-4,-153663.99991112726,12326.74469637485,4.3542524250710812E-2,1.4507619410977785E-3,0.57875678690825294,-153581.1909194671,10091.414003540554]
["KBM","KBMS-25H03-H (240 V)",11,21.1,3.0300652627110845,5.7715528813544461,5200,42.6,7600,0.25,1.1000000000000001,31.8,0.93099999999999994,325,10,7367.4173284860999,7600,7600,-0.64836615449918433,120.83780880773362,0.90524819017280544,0.68736734430046953,1.6753151904410034E-2,-22.743023292839506,9,29.281848867200001,9,-2369.698864,7.5,2381.698864,9,0.79340380079499651,1.1701647937460609,19.041691219079915,56.167910099810918,42.030866253685879,23.061683764075173,2.4395193800850512,149.44315017261758,2.6725191589977554E-3,1.1251932683351202,-153351.00311224174,7367.4173284860999,1.0357633792879802E-3,-0.13670864363181437,-153659.37961976294,12246.228278814366,-9.9281474467140427,1.4507619410977785E-3,0.57875678690825294,-153581.1909194671,10091.414003540554]
["KBM","KBMS-25H04-A (120 V)",14.82,5.5,13.687325105903,4.9772091294192728,450,54.4,685,4.08,23,167,1.18,160,10,685,685,685,13.095817105652344,95.33898305084746,0.6726647146265532,0.53920875764705889,0.18587438609272447,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.15357146800495095,0.22679270733243365,3.6857152321188225,10.886049951956815,8.1439940261893575,23.071857247979214,2.4482621118016494,149.97872344147882,7.222341182475106E-2,23.825973101413155,-148575.28227769674,1278.7882818883591,2.906696095120611E-2,3.8836994951700072,-153528.79327182058,2232.4032337460185,3.2908520444229445,3.510321486321321E-2,9.611135675874884,-152835.95015077561,1954.1883141039134]
["KBM","KBMS-25H04-A (240 V)",14.82,5.5,13.187123856185615,4.7953177658856783,1050,54.4,1437,4.08,23,167,1.18,325,10,1278.7882818883591,1437,1437,12.585292363179741,95.33898305084746,0.67169378638973976,0.53920875764705889,8.860400450488258E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.15357146800495095,0.22679270733243365,3.6857152321188225,10.886049951956815,8.1439940261893575,23.071857247979214,2.4482621118016494,149.97872344147882,7.222341182475106E-2,23.825973101413155,-148575.28227769674,1278.7882818883591,2.9829546847520979E-2,4.9847368622416433,-153441.26342298227,2186.0094194731246,4.2238158524930487,3.510321486321321E-2,9.611135675874884,-152835.95015077561,1954.1883141039134]
["KBM","KBMS-25H04-A (400 V)",14.82,5.5,12.032113697747288,4.3753140719081047,2000,54.4,2400,4.08,23,167,1.18,565,10,1278.7882818883591,2175.092493782206,2347.3053892215567,11.788044715225949,95.33898305084746,0.67153137667094687,0.53920875764705889,6.5154393542620398E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.15357146800495095,0.22679270733243365,3.6857152321188225,10.886049951956815,8.1439940261893575,23.071857247979214,2.4482621118016494,149.97872344147882,7.222341182475106E-2,23.825973101413155,-148575.28227769674,1278.7882818883591,3.0024273699432738E-2,5.2288591933188382,-153418.91261372267,2175.092493782206,4.4306728642968194,3.510321486321321E-2,9.611135675874884,-152835.95015077561,1954.1883141039134]
["KBM","KBMS-25H04-A (480 V)",14.82,5.5,11.399472798957003,4.1452628359843651,2400,54.4,2888,4.08,23,167,1.18,679,10,1278.7882818883591,2175.3083435338385,2347.3053892215567,11.719707766786133,95.33898305084746,0.6715628862578773,0.53920875764705889,6.5154393542620398E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.15357146800495095,0.22679270733243365,3.6857152321188225,10.886049951956815,8.1439940261893575,23.071857247979214,2.4482621118016494,149.97872344147882,7.222341182475106E-2,23.825973101413155,-148575.28227769674,1278.7882818883591,3.0020369982609905E-2,5.2240772949933652,-153419.36068356642,2175.3083435338385,4.4266209236407059,3.510321486321321E-2,9.611135675874884,-152835.95015077561,1954.1883141039134]
["KBM","KBMS-25H04-B (120 V)",14.9,6.2,13.641852265019601,5.5681029653141225,525,53.8,772,3.2,18,148,1.18,160,10,772,772,772,13.049923711609775,95.33898305084746,0.66891895042492,0.54522223821561344,0.16492740216776719,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.17218744070978539,0.25428457743176736,4.1324985770348492,12.205659716724833,9.1312110689735579,23.071857247979214,2.4482621118016494,149.97872344147882,5.5291116436579142E-2,18.363692750852262,-149815.10012500337,1488.3686188128727,2.2765615054083959E-2,2.9500352209808911,-153564.67216256133,2533.2199812172807,3.596291446267303,2.7458695819515738E-2,7.4903257052877859,-153023.6491602984,2228.2362428006272]
["KBM","KBMS-25H04-B (240 V)",14.9,6.2,13.130282805081366,5.359299104114843,1200,53.8,1618,3.2,18,148,1.18,325,10,1488.3686188128727,1618,1618,12.513831315518042,95.33898305084746,0.66799889554754399,0.54522223821561344,7.8692184470652821E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.17218744070978539,0.25428457743176736,4.1324985770348492,12.205659716724833,9.1312110689735579,23.071857247979214,2.4482621118016494,149.97872344147882,5.5291116436579142E-2,18.363692750852262,-149815.10012500337,1488.3686188128727,2.3365920452134509E-2,3.8426641876223324,-153495.46836127152,2482.1363157890073,4.6844662228232439,2.7458695819515738E-2,7.4903257052877859,-153023.6491602984,2228.2362428006272]
["KBM","KBMS-25H04-B (400 V)",14.9,6.2,11.735024470642415,4.7898059063846592,2250,53.8,2704,3.2,18,148,1.18,565,10,1488.3686188128727,2474.1425475094811,2648.6486486486488,11.419733058217803,95.33898305084746,0.66793100954204032,0.54522223821561344,5.7141137922379917E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.17218744070978539,0.25428457743176736,4.1324985770348492,12.205659716724833,9.1312110689735579,23.071857247979214,2.4482621118016494,149.97872344147882,5.5291116436579142E-2,18.363692750852262,-149815.10012500337,1488.3686188128727,2.3467306863276863E-2,3.9736780670287875,-153483.78043530422,2474.1425475094811,4.8441809579222603,2.7458695819515738E-2,7.4903257052877859,-153023.6491602984,2228.2362428006272]
["KBM","KBMS-25H04-B (480 V)",14.9,6.2,10.92863942564348,4.4606691533238694,2700,53.8,3245,3.2,18,148,1.18,679,10,1488.3686188128727,2476.0417866190878,2648.6486486486488,11.258053803022843,95.33898305084746,0.66799501784371096,0.54522223821561344,5.7141137922379917E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.17218744070978539,0.25428457743176736,4.1324985770348492,12.205659716724833,9.1312110689735579,23.071857247979214,2.4482621118016494,149.97872344147882,5.5291116436579142E-2,18.363692750852262,-149815.10012500337,1488.3686188128727,2.3443046209509603E-2,3.9427241386994654,-153486.57722751686,2476.0417866190878,4.8064460363567818,2.7458695819515738E-2,7.4903257052877859,-153023.6491602984,2228.2362428006272]
["KBM","KBMS-25H04-C (120 V)",15.1,8.6300000000000008,13.687325105903,7.646550338493296,750,54.4,1060,1.66,9.6,108,1.18,160,10,1060,1060,1060,13.103419483009572,95.33898305084746,0.6595290153968234,0.53920875764705889,0.12011693818256251,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.23649932106974125,0.34925967697306848,5.6759837056737901,16.764464494707287,12.541711575796871,23.071857247979214,2.4482621118016494,149.97872344147882,2.9981511393068736E-2,9.6543984552800897,-151666.24173668306,2093.8958751652181,1.2078311157655085E-2,1.4519621607983648,-153618.81408358217,3506.7103491465787,4.6758742993646072,1.4644674774062954E-2,3.894478224570411,-153338.91939639804,3105.5997984119704]
["KBM","KBMS-25H04-C (240 V)",15.1,8.6300000000000008,12.638774892591691,7.0607680964199391,1700,54.4,2223,1.66,9.6,108,1.18,325,10,2093.8958751652181,2223,2223,11.8815862271949,95.33898305084746,0.65910582605382628,0.53920875764705889,5.7275733006530036E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.23649932106974125,0.34925967697306848,5.6759837056737901,16.764464494707287,12.541711575796871,23.071857247979214,2.4482621118016494,149.97872344147882,2.9981511393068736E-2,9.6543984552800897,-151666.24173668306,2093.8958751652181,1.2311718967845687E-2,1.8154541763515164,-153593.35798468723,3459.0909537136813,5.8464578169231292,1.4644674774062954E-2,3.894478224570411,-153338.91939639804,3105.5997984119704]
["KBM","KBMS-25H04-C (400 V)",15.1,8.6300000000000008,10.064655448858906,5.6227125412619587,3150,54.4,3707,1.66,9.6,108,1.18,565,10,2093.8958751652181,3463.1823413966049,3629.6296296296296,9.56402656115573,95.33898305084746,0.65925214954845945,0.53920875764705889,4.0998184807528197E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.23649932106974125,0.34925967697306848,5.6759837056737901,16.764464494707287,12.541711575796871,23.071857247979214,2.4482621118016494,149.97872344147882,2.9981511393068736E-2,9.6543984552800897,-151666.24173668306,2093.8958751652181,1.2290765966627306E-2,1.785848802773123,-153595.64317673256,3463.1823413966049,5.751117174325266,1.4644674774062954E-2,3.894478224570411,-153338.91939639804,3105.5997984119704]
["KBM","KBMS-25H04-C (480 V)",15.1,8.6300000000000008,8.0858978879934362,4.517261389940467,3850,54.4,4450,1.66,9.6,108,1.18,679,10,2093.8958751652181,3477.5732865809937,3629.6296296296296,8.7644015236193873,95.33898305084746,0.65946904479642732,0.53920875764705889,4.0998184807528197E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.23649932106974125,0.34925967697306848,5.6759837056737901,16.764464494707287,12.541711575796871,23.071857247979214,2.4482621118016494,149.97872344147882,2.9981511393068736E-2,9.6543984552800897,-151666.24173668306,2093.8958751652181,1.2218355273905961E-2,1.679523464171863,-153603.54048639609,3477.5732865809937,5.4087088584890566,1.4644674774062954E-2,3.894478224570411,-153338.91939639804,3105.5997984119704]
["KBM","KBMS-25H04-D (120 V)",15,10.7,13.369015219719209,9.284038347027229,1000,54.8,1325,1.08,6.2,87,1.18,160,10,1325,1325,1325,12.838945166127953,95.33898305084746,0.66368952193333985,0.53527292729927012,9.6093550546050011E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.29518111475657077,0.43592032451555557,7.084346754157699,20.924175576746666,15.653644954047895,23.071857247979214,2.4482621118016494,149.97872344147882,1.9646805771190295E-2,6.361751671399408,-152327.23542315519,2627.2716701826521,7.7956048882860483E-3,0.87139954541850662,-153638.91950165955,4383.8760334509388,5.354435527023119,9.5057467926309321E-3,2.5475288717658211,-153449.6419820161,3886.0484188911396]
["KBM","KBMS-25H04-D (240 V)",15,10.7,11.777465788800255,8.1787956866668434,2250,54.8,2776,1.08,6.2,87,1.18,325,10,2627.2716701826521,2776,2776,11.024108902093115,95.33898305084746,0.66349400937214364,0.53527292729927012,4.5865977836281074E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.29518111475657077,0.43592032451555557,7.084346754157699,20.924175576746666,15.653644954047895,23.071857247979214,2.4482621118016494,149.97872344147882,1.9646805771190295E-2,6.361751671399408,-152327.23542315519,2627.2716701826521,7.899837578543397E-3,1.0529072320323314,-153627.38308761836,4343.7268349425221,6.46973471525724,9.5057467926309321E-3,2.5475288717658211,-153449.6419820161,3886.0484188911396]
["KBM","KBMS-25H04-D (400 V)",15,10.7,6.9376214952587638,4.8177927050408087,4150,54.8,4626,1.08,6.2,87,1.18,565,10,2627.2716701826521,4384.0602005486962,4505.7471264367814,6.4829029579770214,95.33898305084746,0.66399643706964273,0.53527292729927012,3.2764376752116582E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.29518111475657077,0.43592032451555557,7.084346754157699,20.924175576746666,15.653644954047895,23.071857247979214,2.4482621118016494,149.97872344147882,1.9646805771190295E-2,6.361751671399408,-152327.23542315519,2627.2716701826521,7.7951457174341241E-3,0.87051623665072408,-153638.9703224246,4384.0602005486962,5.3490079136253241,9.5057467926309321E-3,2.5475288717658211,-153449.6419820161,3886.0484188911396]
["KBM","KBMS-25H04-D (480 V)",15,10.7,4.0432128096111288,2.8077866733410617,4700,54.8,5551,1.08,6.2,87,1.18,679,10,2627.2716701826521,4415.6954329426435,4505.7471264367814,4.7059925199309376,95.33898305084746,0.6643792904401491,0.53527292729927012,3.2764376752116582E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.29518111475657077,0.43592032451555557,7.084346754157699,20.924175576746666,15.653644954047895,23.071857247979214,2.4482621118016494,149.97872344147882,1.9646805771190295E-2,6.361751671399408,-152327.23542315519,2627.2716701826521,7.7192966386971963E-3,0.70967143686942813,-153647.36525471302,4415.6954329426435,4.3606747032008597,9.5057467926309321E-3,2.5475288717658211,-153449.6419820161,3886.0484188911396]
["KBM","KBMS-25H04-E (120 V)",14.6,13.8,12.584608714480584,11.65241547637091,1400,53.8,1837,0.65,3.5,65.5,1.18,160,10,1837,1837,1837,11.955518720357738,95.33898305084746,0.68171918397648101,0.54522223821561344,6.9310808096633786E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.39113103798879895,0.57761814860273986,9.3871449117311752,27.725671132931513,20.741931285929557,23.071857247979214,2.4482621118016494,149.97872344147882,1.0803707883045573E-2,3.7499354350619143,-152844.58296328111,3591.758642260118,4.3823648527384126E-3,0.44594655851381121,-153652.41161161644,5870.6165566707805,6.047383807448881,5.3739098405337499E-3,1.5295528063717041,-153527.67159329413,5204.5867300931504]
["KBM","KBMS-25H04-E (240 V)",14.6,13.8,9.9719703688069501,9.233305897043472,3050,53.8,3681,0.65,3.5,65.5,1.18,325,10,3591.758642260118,3681,3681,9.014499320517503,95.33898305084746,0.68179998814833287,0.54522223821561344,3.4589501351131827E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.39113103798879895,0.57761814860273986,9.3871449117311752,27.725671132931513,20.741931285929557,23.071857247979214,2.4482621118016494,149.97872344147882,1.0803707883045573E-2,3.7499354350619143,-152844.58296328111,3591.758642260118,4.3881039049424352E-3,0.45962862305915048,-153651.68961767174,5865.2499807781651,6.2329232941974766,5.3739098405337499E-3,1.5295528063717041,-153527.67159329413,5204.5867300931504]
["KBM","KBMS-25H04-E (400 V)",14.6,13.8,4.5670548887239537,4.2287545265962532,4600,53.8,6135,0.65,3.5,65.5,1.18,565,10,3591.758642260118,5937.8229472675985,5984.7328244274813,1.6491626716497461,95.33898305084746,0.68248989219573986,0.54522223821561344,2.4463797238179073E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.39113103798879895,0.57761814860273986,9.3871449117311752,27.725671132931513,20.741931285929557,23.071857247979214,2.4482621118016494,149.97872344147882,1.0803707883045573E-2,3.7499354350619143,-152844.58296328111,3591.758642260118,4.3174200170493712E-3,0.24219375527942125,-153660.58191159627,5937.8229472675985,3.2843365779593707,5.3739098405337499E-3,1.5295528063717041,-153527.67159329413,5204.5867300931504]
["KBM","KBMS-25H04-F (120 V)",14.5,19.399999999999999,11.793381283109445,15.316079588453825,2000,54.1,2495,0.33,1.8,46.3,1.18,160,10,2495,2495,2495,11.123493150679034,95.33898305084746,0.68634029286880194,0.54219882469500924,5.1031645079565639E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.55364295452247569,0.81761401504367814,13.287430908539417,39.245472722096551,29.360043065600632,23.071857247979214,2.4482621118016494,149.97872344147882,5.6340120734180987E-3,1.9155193835389135,-153236.09128783623,5047.9819894634711,2.1583274594738104E-3,0.12404711036354542,-153662.20546748952,8409.0272861507765,4.6873900491254776,2.7179610122725654E-3,0.77698430560872533,-153593.59515937913,7375.7765716533722]
["KBM","KBMS-25H04-F (240 V)",14.5,19.399999999999999,4.8481044203377346,6.2962395069321229,4550,54.1,5206,0.33,1.8,46.3,1.18,325,10,5047.9819894634711,5206,5206,3.4565344202809332,95.33898305084746,0.68714941771424942,0.54219882469500924,2.4457156064832168E-2,-22.806119032098767,9,29.332956416000002,9,-2374.91392,7.5,2386.91392,9,0.55364295452247569,0.81761401504367814,13.287430908539417,39.245472722096551,29.360043065600632,23.071857247979214,2.4482621118016494,149.97872344147882,5.6340120734180987E-3,1.9155193835389135,-153236.09128783623,5047.9819894634711,2.1449049110676211E-3,-3.5737654290870384E-2,-153663.85105356487,8472.4553689827499,-1.350425049089587,2.7179610122725654E-3,0.77698430560872533,-153593.59515937913,7375.7765716533722]
["KBM","KBMS-25H04-G (120 V)",14,20.3,11.77006323330761,16.577553849729028,2150,54.5,2701,0.3,1.5,42.8,1.18,160,10,{"$f":"IF(AQ1019<I1019,IF(AQ1019<0,0,AQ1019),I1019)","v":2701},{"$f":"IF(AU1019<I1019,IF(AU1019<0,0,AU1019),I1019)","v":2701},{"$f":"IF(UAC_V*0.98/L1019*1000<I1019,IF(UAC_V*0.98/L1019*1000<0,0,UAC_V*0.98/L1019*1000),I1019)","v":2701},{"$f":"C1019+(E1019-C1019)/G1019*Q1019","v":11.198577113099468},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M1019,(inertia/gear^2+gear_inertia)/M1019),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M1019,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M1019))","v":95.33898305084746},{"$f":"IF((C1019+(E1019-C1019)/G1019*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X1019^2*time1+Y1019^2*time2+Z1019^2*time3+AA1019^2*time4)/time)/(C1019+(E1019-C1019)/G1019*mspeed),SQRT((((X1019-Y1019)*2/PI()+Y1019)^2*time1+Y1019^2*time2+((Z1019-Y1019)*2/PI()+Y1019)^2*time3+AA1019^2*time4)/time)/(C1019+(E1019-C1019)/G1019*mspeed)),IF(AccType=1,SQRT((X1019^2*time1+Y1019^2*time2+Z1019^2*time3+AA1019^2*time4+AB1019^2*time5+AC1019^2*time6+AD1019^2*time7+AE1019^2*time8)/time)/(C1019+(E1019-C1019)/G1019*mspeed),SQRT((((X1019-Y1019)*2/PI()+Y1019)^2*time1+Y1019^2*time2+((Z1019-Y1019)*2/PI()+Y1019)^2*time3+AA1019^2*time4+((AB1019-AC1019)*2/PI()+AC1019)^2*time5+AC1019^2*time6+((AD1019-AC1019)*2/PI()+AC1019)^2*time7+AE1019^2*time8)/time)/(C1019+(E1019-C1019)/G1019*mspeed))))","v":0.71054839645604284},{"$f":"IF(move1,MAX(ABS(X1019),ABS(Z1019))/H1019,MAX(ABS(X1019),ABS(Z1019),ABS(AB1019),ABS(AD1019))/H1019)","v":0.5382193837798166},{"$f":"IF(AZ1019>0,speed/(MIN(AZ1019,I1019)),\"NA\")","v":4.7139561078680586E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M1019+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M1019+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-22.806119032098767},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M1019+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M1019+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.332956416000002},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M1019+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M1019+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2374.91392},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M1019+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M1019+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2386.91392},9,{"$f":"AH1019/Irms","v":0.60001768653788934},{"$f":"AI1019/Ipeak","v":0.88609972506666679},{"$f":"IF(move1,IF(AccType=1,SQRT((X1019^2*time1+Y1019^2*time2+Z1019^2*time3+AA1019^2*time4)/time)/(C1019/D1019),SQRT((((X1019-Y1019)*2/PI()+Y1019)^2*time1+Y1019^2*time2+((Z1019-AA1019)*2/PI()+AA1019)^2*time3+AA1019^2*time4)/time)/(C1019/D1019)),IF(AccType=1,SQRT((X1019^2*time1+Y1019^2*time2+Z1019^2*time3+AA1019^2*time4+AB1019^2*time5+AC1019^2*time6+AD1019^2*time7+AE1019^2*time8)/time)/(C1019/D1019),SQRT((((X1019-Y1019)*2/PI()+Y1019)^2*time1+Y1019^2*time2+((Z1019-AA1019)*2/PI()+AA1019)^2*time3+AA1019^2*time4+((AB1019-AC1019)*2/PI()+AC1019)^2*time5+AC1019^2*time6+((AD1019-AE1019)*2/PI()+AE1019)^2*time7+AE1019^2*time8)/time)/(C1019/D1019)))","v":14.400424476909345},{"$f":"IF(move1,MAX(ABS(X1019),ABS(Z1019))/(C1019/D1019),MAX(ABS(X1019),ABS(Z1019),ABS(AB1019),ABS(AD1019))/(C1019/D1019))","v":42.532786803200004},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X1019),ABS(Z1019))/(C1019/D1019),MAX(ABS((X1019-Y1019)*2/PI()+Y1019),ABS((Z1019-Y1019)*2/PI()+Y1019))/(C1019/D1019)),IF(AccType=1,MAX(ABS(X1019),ABS(Z1019),ABS(AB1019),ABS(AD1019))/(C1019/D1019),MAX(ABS((X1019-Y1019)*2/PI()+Y1019),ABS((Z1019-Y1019)*2/PI()+Y1019),ABS((AB1019-AC1019)*2/PI()+AC1019),ABS((AD1019-AC1019)*2/PI()+AC1019))/(C1019/D1019)))","v":31.819325023415118},{"$f":"IF((C1019+(E1019-C1019)/G1019*mspeed)<0,\"NA\",U1019*(C1019+(E1019-C1019)/G1019*mspeed)*mspeed/9.55)","v":23.071857247979214},{"$f":"IF(move1,IF(speed1>speed2,AM1019/2*time1/time,AM1019/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z1019*-speed/30*PI(),((Z1019-AA1019)*2/PI()+AA1019)*-speed/30*PI()),IF(AccType=1,X1019*-speed/30*PI(),((X1019-Y1019)*2/PI()+Y1019)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z1019*-speed/30*PI(),((Z1019-AA1019)*2/PI()+AA1019)*-speed/30*PI()),IF(AccType=1,X1019*-speed/30*PI(),((X1019-Y1019)*2/PI()+Y1019)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD1019*-speed/30*PI(),((AD1019-AE1019)*2/PI()+AE1019)*-speed/30*PI()),IF(AccType=1,AB1019*-speed/30*PI(),((AB1019-AC1019)*2/PI()+AC1019)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD1019*-speed/30*PI(),((AD1019-AE1019)*2/PI()+AE1019)*-speed/30*PI()),IF(AccType=1,AB1019*-speed/30*PI(),((AB1019-AC1019)*2/PI()+AC1019)*-speed/30*PI()),0)/2*time7/time)))","v":2.4482621118016494},{"$f":"IF(move1,MAX(IF(AccType=1,Z1019*-speed/30*PI(),((Z1019-AA1019)*2/PI()+AA1019)*-speed/30*PI()),IF(AccType=1,X1019*-speed/30*PI(),((X1019-Y1019)*2/PI()+Y1019)*-speed/30*PI()),0),MAX(IF(AccType=1,Z1019*-speed/30*PI(),((Z1019-AA1019)*2/PI()+AA1019)*-speed/30*PI()),IF(AccType=1,X1019*-speed/30*PI(),((X1019-Y1019)*2/PI()+Y1019)*-speed/30*PI()),IF(AccType=1,AD1019*-speed/30*PI(),((AD1019-AE1019)*2/PI()+AE1019)*-speed/30*PI()),IF(AccType=1,AB1019*-speed/30*PI(),((AB1019-AC1019)*2/PI()+AC1019)*-speed/30*PI()),0))","v":149.97872344147882},{"$f":"(L1019^2)/1000000+((K1019/1000)^2*(D1019/C1019*H1019)^2*PI()*PI()*(O1019/2)^2)/1200","v":4.7209896331133934E-3},{"$f":"SQRT(3)*L1019*J1019*D1019/C1019*H1019/1000","v":1.7574790454747957},{"$f":"0.75*J1019^2*(D1019/C1019*H1019)^2-(UAC_V*0.98)^2","v":-153242.46583281251},{"$f":"-AO1019/2/AN1019+SQRT((AO1019/2/AN1019)^2-AP1019/AN1019)","v":5514.2570011714552},{"$f":"(L1019^2)/1000000+((K1019/1000)^2*AV1019^2*PI()*PI()*(O1019/2)^2)/1200","v":1.8531850785698056E-3},{"$f":"SQRT(3)*L1019*J1019*AV1019/1000","v":0.15106157794804662},{"$f":"0.75*J1019^2*AV1019^2-(UAC_V*0.98)^2","v":-153660.88569957908},{"$f":"-AS1019/2/AR1019+SQRT((AS1019/2/AR1019)^2-AT1019/AR1019)","v":9065.221183557007},{"$f":"D1019+(F1019-D1019)*((0.85*UAC_V-D1019*J1019)/L1019*1000)/G1019","v":6.7924799604761965},{"$f":"(L1019^2)/1000000+((K1019/1000)^2*AJ1019^2*PI()*PI()*(O1019/2)^2)/1200","v":2.300246541709604E-3},{"$f":"SQRT(3)*L1019*J1019*AJ1019/1000","v":0.70764690882383907},{"$f":"0.75*J1019^2*AJ1019^2-(UAC_V*0.98)^2","v":-153595.65831246617},{"$f":"IF(((AX1019/2/AW1019)^2-AY1019/AW1019)>0,-AX1019/2/AW1019+SQRT((AX1019/2/AW1019)^2-AY1019/AW1019),-9999)","v":8019.1370701392279}]
["KBM","KBMS-25H04-G (240 V)",14,20.3,4.8473059841683774,6.8271915269977148,4600,54.5,5637,0.3,1.5,42.8,1.18,325,10,5514.2570011714552,5637,5637,2.7839703984254651,95.33898305084746,0.71162435937103763,0.5382193837798166,2.2587183692303756E-2,-22.806119032098767,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},29.332956416000002,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},-2374.91392,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},2386.91392,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},0.60001768653788934,0.88609972506666679,14.400424476909345,42.532786803200004,31.819325023415118,23.071857247979214,2.4482621118016494,149.97872344147882,4.7209896331133934E-3,1.7574790454747957,-153242.46583281251,5514.2570011714552,1.8348482714517621E-3,-5.6710522568628755E-2,-153663.56108566115,9166.8210548026746,-2.5499871862057759,2.300246541709604E-3,0.70764690882383907,-153595.65831246617,8019.1370701392279]
["KBM","KBMS-35H01-A (120 V)",12.6,5.41,11.650141834326739,4.9156716600534764,500,40.799999999999997,798,4.13,32,144,2.17,160,10,798,798,798,11.084026367585476,51.843317972350235,0.79223847231496014,0.7239253701960785,0.15955382766104795,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.1779863919745828,0.26420403292433869,4.2716734073899874,12.681793580368257,9.4776855648405416,23.112481974676097,2.4830223704339081,152.10811113695127,8.5350833684642746E-2,18.045131622824574,-149738.13706494667,1223.0318494915673,2.2931403343415226E-2,3.3262209868483215,-153530.61185796018,2516.0015688726317,3.2290734835570714,3.9649114737245444E-2,9.7628241639750293,-152514.87847636122,1842.0239838558869]
["KBM","KBMS-35H01-A (240 V)",12.6,5.41,11.459155902616464,4.8350868787411239,1200,40.799999999999997,1675,4.13,32,144,2.17,325,10,1223.0318494915673,1675,1675,11.007571780735482,51.843317972350235,0.79091241053703798,0.7239253701960785,7.6014301178218668E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.1779863919745828,0.26420403292433869,4.2716734073899874,12.681793580368257,9.4776855648405416,23.112481974676097,2.4830223704339081,152.10811113695127,8.5350833684642746E-2,18.045131622824574,-149738.13706494667,1223.0318494915673,2.4725920104490172E-2,4.4841077355320698,-153421.58075106266,2401.9349895356108,4.3531423328368373,3.9649114737245444E-2,9.7628241639750293,-152514.87847636122,1842.0239838558869]
["KBM","KBMS-35H01-A (400 V)",12.6,5.41,10.926171907145932,4.6101991169392118,2150,40.799999999999997,2795,4.13,32,144,2.17,565,10,1223.0318494915673,2376.5134786033295,2722.2222222222222,10.749825570449953,51.843317972350235,0.79067229973170405,0.7239253701960785,6.9121768005968393E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.1779863919745828,0.26420403292433869,4.2716734073899874,12.681793580368257,9.4776855648405416,23.112481974676097,2.4830223704339081,152.10811113695127,8.5350833684642746E-2,18.045131622824574,-149738.13706494667,1223.0318494915673,2.5170734542057597E-2,4.7274588048231685,-153394.55475078005,2376.5134786033295,4.5893859522927141,3.9649114737245444E-2,9.7628241639750293,-152514.87847636122,1842.0239838558869]
["KBM","KBMS-35H01-A (480 V)",12.6,5.41,10.504226244065093,4.4321629721793636,2700,40.799999999999997,3353,4.13,32,144,2.17,679,10,1223.0318494915673,2374.1594881620031,2722.2222222222222,10.757147723076379,51.843317972350235,0.79066907626999805,0.7239253701960785,6.9121768005968393E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.1779863919745828,0.26420403292433869,4.2716734073899874,12.681793580368257,9.4776855648405416,23.112481974676097,2.4830223704339081,152.10811113695127,8.5350833684642746E-2,18.045131622824574,-149738.13706494667,1223.0318494915673,2.5212777695955181E-2,4.7498150947366824,-153392.00029617347,2374.1594881620031,4.6110892916787254,3.9649114737245444E-2,9.7628241639750293,-152514.87847636122,1842.0239838558869]
["KBM","KBMS-35H01-B (120 V)",12.45,6.1,11.632779476898532,5.5394187985231103,550,41.4,901,3.3,25,127,2.17,160,10,901,901,901,11.111244197610141,51.843317972350235,0.80122302547584234,0.71343369816425128,0.1413140449206618,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.20310497572050024,0.3014902043748327,4.8745194172920057,14.471529809991969,10.81523747505577,23.112481974676097,2.4830223704339081,152.10811113695127,6.9005192470452642E-2,14.724451059951607,-150303.44666413122,1373.0151110400286,1.7732973108812052E-2,2.5645287194197586,-153562.05927905126,2871.3138733588553,3.532883193752145,3.1160788104857069E-2,7.8508078504197556,-152708.65273879017,2091.3538361175724]
["KBM","KBMS-35H01-B (240 V)",12.45,6.1,11.275515583664278,5.3692931350782276,1300,41.4,1892,3.3,25,127,2.17,325,10,1373.0151110400286,1892,1892,10.740673449456011,51.843317972350235,0.80039013429606887,0.71343369816425128,6.7295959024057217E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.20310497572050024,0.3014902043748327,4.8745194172920057,14.471529809991969,10.81523747505577,23.112481974676097,2.4830223704339081,152.10811113695127,6.9005192470452642E-2,14.724451059951607,-150303.44666413122,1373.0151110400286,1.8948868779574017E-2,3.4003488537781155,-153484.78287049118,2757.7297708727929,4.6843052399604641,3.1160788104857069E-2,7.8508078504197556,-152708.65273879017,2091.3538361175724]
["KBM","KBMS-35H01-B (400 V)",12.45,6.1,10.646449810232319,5.0697380048725327,2350,41.4,3153,3.3,25,127,2.17,565,10,1373.0151110400286,2724.9402708575922,3086.6141732283463,10.358695088250721,51.843317972350235,0.8001959183725873,0.71343369816425128,6.0881115512180756E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.20310497572050024,0.3014902043748327,4.8745194172920057,14.471529809991969,10.81523747505577,23.112481974676097,2.4830223704339081,152.10811113695127,6.9005192470452642E-2,14.724451059951607,-150303.44666413122,1373.0151110400286,1.933636059122246E-2,3.626460236670805,-153460.15577766518,2724.9402708575922,4.9957952609099578,3.1160788104857069E-2,7.8508078504197556,-152708.65273879017,2091.3538361175724]
["KBM","KBMS-35H01-B (480 V)",12.45,6.1,10.207868763825012,4.8608898875357198,2900,41.4,3783,3.3,25,127,2.17,679,10,1373.0151110400286,2721.9561594250072,3086.6141732283463,10.345523128087684,51.843317972350235,0.80020402973335514,0.71343369816425128,6.0881115512180756E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.20310497572050024,0.3014902043748327,4.8745194172920057,14.471529809991969,10.81523747505577,23.112481974676097,2.4830223704339081,152.10811113695127,6.9005192470452642E-2,14.724451059951607,-150303.44666413122,1373.0151110400286,1.9372456275620578E-2,3.6468092638449914,-153457.86171171701,2721.9561594250072,5.0238279889385034,3.1160788104857069E-2,7.8508078504197556,-152708.65273879017,2091.3538361175724]
["KBM","KBMS-35H01-C (120 V)",12.45,8.32,11.482589759268032,7.5049606269725704,815,40.799999999999997,1242,1.75,13.4,93,2.17,160,10,1242,1242,1242,10.975738013510302,51.843317972350235,0.80079542889395949,0.7239253701960785,0.10251526125081825,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.2770218685236987,0.41121286891780467,6.6485248445687688,19.738217708054624,14.751274720076069,23.112481974676097,2.4830223704339081,152.10811113695127,3.6096094692917982E-2,7.6859182800421619,-151956.48063916387,1948.0695590381824,9.5069223338159915E-3,1.3588501263301223,-153610.62753885341,3948.8412916595526,4.820476105837499,1.6682914529049964E-2,4.1582555492043394,-153164.19975683637,2907.9360230368725]
["KBM","KBMS-35H01-C (240 V)",12.45,8.32,10.976501238239955,7.1741838158431079,1840,40.799999999999997,2600,1.75,13.4,93,2.17,325,10,1948.0695590381824,2600,2600,10.367882184469501,51.843317972350235,0.8002435367396179,0.7239253701960785,4.8970751720583176E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.2770218685236987,0.41121286891780467,6.6485248445687688,19.738217708054624,14.751274720076069,23.112481974676097,2.4830223704339081,152.10811113695127,3.6096094692917982E-2,7.6859182800421619,-151956.48063916387,1948.0695590381824,1.004127976823984E-2,1.7310548471013316,-153577.38446977476,3825.5843320865429,6.1408601041840871,1.6682914529049964E-2,4.1582555492043394,-153164.19975683637,2907.9360230368725]
["KBM","KBMS-35H01-C (400 V)",12.45,8.32,9.6876921882023268,6.3318249596093636,3450,40.799999999999997,4334,1.75,13.4,93,2.17,565,10,1948.0695590381824,3809.476529532737,4215.0537634408602,9.3998704995976325,51.843317972350235,0.80024332879239246,0.7239253701960785,4.3784991645224307E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.2770218685236987,0.41121286891780467,6.6485248445687688,19.738217708054624,14.751274720076069,23.112481974676097,2.4830223704339081,152.10811113695127,3.6096094692917982E-2,7.6859182800421619,-151956.48063916387,1948.0695590381824,1.0115950451454019E-2,1.776868526393804,-153572.73910972109,3809.476529532737,6.3033826238281794,1.6682914529049964E-2,4.1582555492043394,-153164.19975683637,2907.9360230368725]
["KBM","KBMS-35H01-C (480 V)",12.45,8.32,8.8330993416001924,5.7732675435295375,4200,40.799999999999997,5201,1.75,13.4,93,2.17,679,10,1948.0695590381824,3819.9300660591666,4215.0537634408602,9.1604029592927088,51.843317972350235,0.80032973373276683,0.7239253701960785,4.3784991645224307E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.2770218685236987,0.41121286891780467,6.6485248445687688,19.738217708054624,14.751274720076069,23.112481974676097,2.4830223704339081,152.10811113695127,3.6096094692917982E-2,7.6859182800421619,-151956.48063916387,1948.0695590381824,1.0067362518938132E-2,1.7471942644427734,-153575.76182802342,3819.9300660591666,6.1981141560835962,1.6682914529049964E-2,4.1582555492043394,-153164.19975683637,2907.9360230368725]
["KBM","KBMS-35H01-D (120 V)",12.65,10.57,11.589373583328015,9.4222549457951352,1100,41.2,1556,1.08,8.5,74,2.17,160,10,1556,1556,1556,11.149695723325811,51.843317972350235,0.78779974041066303,0.71689696854368934,8.1827734237478314E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.34637340682178203,0.51415869474519116,8.3129617637227682,24.679617347769174,18.444209141271003,23.112481974676097,2.4830223704339081,152.10811113695127,2.3081960173350388E-2,4.7653826622573376,-152627.25456913153,2470.3032777851363,5.9996264964296275E-3,0.82182382998011749,-153633.16570455063,4992.3218640052155,5.9369395578762525,1.052978120146581E-2,2.553148882461568,-153366.40279327909,3697.1041282261453]
["KBM","KBMS-35H01-D (240 V)",12.65,10.57,10.757574928986886,8.745995877225111,2450,41.2,3252,1.08,8.5,74,2.17,325,10,2470.3032777851363,3252,3252,10.138095375128716,51.843317972350235,0.787534394234496,0.71689696854368934,3.9152507525681508E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.34637340682178203,0.51415869474519116,8.3129617637227682,24.679617347769174,18.444209141271003,23.112481974676097,2.4830223704339081,152.10811113695127,2.3081960173350388E-2,4.7653826622573376,-152627.25456913153,2470.3032777851363,6.2599230279906121E-3,1.0055522310922813,-153617.83787027691,4874.1099677034554,7.2642123536706382,1.052978120146581E-2,2.553148882461568,-153366.40279327909,3697.1041282261453]
["KBM","KBMS-35H01-D (400 V)",12.65,10.57,8.4999233343583658,6.9105067759011103,4550,41.2,5420,1.08,8.5,74,2.17,565,10,2470.3032777851363,4898.7690987405831,5297.2972972972975,8.1818093786704189,51.843317972350235,0.78772763864698436,0.71689696854368934,3.4438833762198022E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.34637340682178203,0.51415869474519116,8.3129617637227682,24.679617347769174,18.444209141271003,23.112481974676097,2.4830223704339081,152.10811113695127,2.3081960173350388E-2,4.7653826622573376,-152627.25456913153,2470.3032777851363,6.20366704898845E-3,0.96880032860589516,-153621.15056260469,4898.7690987405831,6.9987128442393836,1.052978120146581E-2,2.553148882461568,-153366.40279327909,3697.1041282261453]
["KBM","KBMS-35H01-D (480 V)",12.65,10.57,6.1741141716683536,5.0196050176165476,5800,41.2,6505,1.08,8.5,74,2.17,679,10,2470.3032777851363,4959.4986865065393,5297.2972972972975,7.1125608173142911,51.843317972350235,0.78801061771566627,0.71689696854368934,3.4438833762198022E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.34637340682178203,0.51415869474519116,8.3129617637227682,24.679617347769174,18.444209141271003,23.112481974676097,2.4830223704339081,152.10811113695127,2.3081960173350388E-2,4.7653826622573376,-152627.25456913153,2470.3032777851363,6.0695197202148927E-3,0.87495456126241389,-153629.04996876032,4959.4986865065393,6.3207614048241441,1.052978120146581E-2,2.553148882461568,-153366.40279327909,3697.1041282261453]
["KBM","KBMS-35H01-E (120 V)",12.2,12.8,10.777063289365486,11.226107593089049,1400,41.1,1996,0.74,5.4,57.8,2.17,160,10,1996,1996,1996,10.171298803981079,51.843317972350235,0.81698662535923727,0.71864124340632607,6.3789556349457044E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.43492084024212468,0.6455990186666668,10.438100165810992,30.988752896000005,23.159315291922706,23.112481974676097,2.4830223704339081,152.10811113695127,1.4489686842120434E-2,3.1945680687306601,-152900.32491037034,3140.0728816593228,3.5842248470563456E-3,0.47200210952729532,-153647.32859465,6481.8265441972562,6.3712369071742074,6.5567024020869473E-3,1.7157179731750909,-153443.71945951646,4708.5528056889425]
["KBM","KBMS-35H01-E (240 V)",12.2,12.8,9.5955028593145926,9.9953154784527012,3100,41.1,4166,0.74,5.4,57.8,2.17,325,10,3140.0728816593228,4166,4166,8.6998919070659984,51.843317972350235,0.81672440864009621,0.71864124340632607,3.0562639095899249E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.43492084024212468,0.6455990186666668,10.438100165810992,30.988752896000005,23.159315291922706,23.112481974676097,2.4830223704339081,152.10811113695127,1.4489686842120434E-2,3.1945680687306601,-152900.32491037034,3140.0728816593228,3.689555911852562E-3,0.56497997359066743,-153640.11361434861,6376.9428756120224,7.6262821434424275,6.5567024020869473E-3,1.7157179731750909,-153443.71945951646,4708.5528056889425]
["KBM","KBMS-35H01-E (400 V)",12.2,12.8,5.1268764455012183,5.3404962973971024,6100,41.1,6943,0.74,5.4,57.8,2.17,565,10,3140.0728816593228,6524.9228409219431,6782.0069204152251,4.6341663217357203,51.843317972350235,0.81719974669588835,0.71864124340632607,2.7040995339307143E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.43492084024212468,0.6455990186666668,10.438100165810992,30.988752896000005,23.159315291922706,23.112481974676097,2.4830223704339081,152.10811113695127,1.4489686842120434E-2,3.1945680687306601,-152900.32491037034,3140.0728816593228,3.5430287252557055E-3,0.43020518341046066,-153650.15045169528,6524.9228409219431,5.8070485001590253,6.5567024020869473E-3,1.7157179731750909,-153443.71945951646,4708.5528056889425]
["KBM","KBMS-35H01-F (120 V)",12.4,14.58,11.071215728829969,12.725535320494217,1600,41.1,2288,0.56999999999999995,4.4000000000000004,52.6,2.17,160,10,2288,2288,2288,10.499838492226855,51.843317972350235,0.80351767950755904,0.71864124340632607,5.5648581500662701E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.4874116644336452,0.72351670264838708,11.697879946407484,34.72880172712258,25.954425194468516,23.112481974676097,2.4830223704339081,152.10811113695127,1.2063253765421899E-2,2.5095675373278952,-153094.92920741139,3459.946232924819,2.9772247416614862E-3,0.37759737978873181,-153651.11671944591,7120.7948783069487,7.2712276988300211,5.4483148903683686E-3,1.347822314645831,-153499.85267679006,5185.6511725892033]
["KBM","KBMS-35H01-F (240 V)",12.4,14.58,9.4962449378164226,10.915224066455659,3600,41.1,4576,0.56999999999999995,4.4000000000000004,52.6,2.17,325,10,3459.946232924819,4576,4576,8.7090046765133202,51.843317972350235,0.80348328225454346,0.71864124340632607,2.7824290750331351E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.4874116644336452,0.72351670264838708,11.697879946407484,34.72880172712258,25.954425194468516,23.112481974676097,2.4830223704339081,152.10811113695127,1.2063253765421899E-2,2.5095675373278952,-153094.92920741139,3459.946232924819,3.0318624896363763E-3,0.42378560420389039,-153647.77215241559,7049.2804928002743,8.1606541480156203,5.4483148903683686E-3,1.347822314645831,-153499.85267679006,5185.6511725892033]
["KBM","KBMS-35H01-F (400 V)",12.4,14.58,3.7039695846841094,4.2574363042346084,6600,41.1,7200,0.56999999999999995,4.4000000000000004,52.6,2.17,565,10,3459.946232924819,7200,7200,2.9134213651099383,51.843317972350235,0.80421959817512245,0.71864124340632607,2.455312751203495E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.4874116644336452,0.72351670264838708,11.697879946407484,34.72880172712258,25.954425194468516,23.112481974676097,2.4830223704339081,152.10811113695127,1.2063253765421899E-2,2.5095675373278952,-153094.92920741139,3459.946232924819,2.8553485020913318E-3,0.24497850269222521,-153658.57718895195,7293.0502228390733,4.7174439488702458,5.4483148903683686E-3,1.347822314645831,-153499.85267679006,5185.6511725892033]
["KBM","KBMS-35H01-G (120 V)",12.4,20.100000000000001,10.605814505613111,16.834626199385891,2350,41.2,3026,0.3,2.2000000000000002,38.1,2.17,160,10,3026,3026,3026,10.089699869780969,51.843317972350235,0.80342121532366029,0.71689696854368934,4.2076653824691432E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.67194612175008706,0.99744072175806464,16.126706922002089,47.877154644387105,35.780791934761126,23.112481974676097,2.4830223704339081,152.10811113695127,5.8902206027177956E-3,1.3221430488509529,-153362.94423405308,4991.6363046666393,1.5140342757535077E-3,0.15679480852903671,-153659.765975024,10022.591147644687,7.9199934306015045,2.7257107365560394E-3,0.70836452954003115,-153577.5821076752,7377.4507561437495]
["KBM","KBMS-35H01-G (240 V)",12.4,20.100000000000001,7.1259373576805212,11.31101167885797,5300,41.2,6316,0.3,2.2000000000000002,38.1,2.17,325,10,4991.6363046666393,6316,6316,6.1149095002094658,51.843317972350235,0.80375476136821999,0.71689696854368934,2.0158954159834749E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.67194612175008706,0.99744072175806464,16.126706922002089,47.877154644387105,35.780791934761126,23.112481974676097,2.4830223704339081,152.10811113695127,5.8902206027177956E-3,1.3221430488509529,-153362.94423405308,4991.6363046666393,1.4824188195792208E-3,0.11015201660221281,-153661.91034321176,10144.084169031068,5.5639804406883382,2.7257107365560394E-3,0.70836452954003115,-153577.5821076752,7377.4507561437495]
["KBM","KBMS-35H01-H (120 V)",12.2,21.2,10.313240312354818,17.450491222258577,2500,41.4,3237,0.27,1.6,35.700000000000003,2.17,160,10,3237,3237,3237,9.7570235564370194,51.843317972350235,0.81659731147572501,0.71343369816425128,3.9333937124966412E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.72033764165101888,1.0692733746666667,17.288103399624454,51.325121984000006,38.357615952246981,23.112481974676097,2.4830223704339081,152.10811113695127,3.9987667004109289E-3,1.2010718241405245,-153381.0292574394,6044.9498918775498,1.3014497319819411E-3,0.11948163479422873,-153661.1996914348,10820.161396958167,7.1566297345849677,2.0489548051665155E-3,0.64038951723823367,-153583.55630609329,8502.9105088926899]
["KBM","KBMS-35H01-H (240 V)",12.2,21.2,6.3605136185653901,10.762290386743469,5600,41.4,6756,0.27,1.6,35.700000000000003,2.17,325,10,6044.9498918775498,6756,6756,5.1550767869692455,51.843317972350235,0.81702589589223418,0.71343369816425128,1.8846056020354687E-2,-23.056981609876544,9,29.536155104000002,9,-2395.6484799999998,7.5,2407.6484799999998,9,0.72033764165101888,1.0692733746666667,17.288103399624454,51.325121984000006,38.357615952246981,23.112481974676097,2.4830223704339081,152.10811113695127,3.9987667004109289E-3,1.2010718241405245,-153381.0292574394,6044.9498918775498,1.2818828891783486E-3,6.2567740117303636E-2,-153663.2321002708,10924.278471337606,3.7476399625803296,2.0489548051665155E-3,0.64038951723823367,-153583.55630609329,8502.9105088926899]
["KBM","KBMS-35H02-A (120 V)",17.3,4.97,16.160348067792452,4.5522107233218172,325,58.8,531,5.5,44,215,2.94,160,10,531,531,531,15.43798407383936,38.265306122448983,0.57846833368545436,0.5050033763265307,0.23978145851886304,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.11925245180386546,0.17772178068901734,2.8620588432927709,8.5306454730728323,6.370315011701603,23.144272670531002,2.5100581271478877,153.76430156676318,0.15981473447468164,34.597872067302063,-147190.1614300411,857.53146581675219,5.005183974008047E-2,6.3503839498350283,-153445.89628820811,1688.6360668889681,3.100546201179478,6.2379208292969474E-2,13.047361200524579,-152743.3205284102,1463.718290155211]
["KBM","KBMS-35H02-A (240 V)",17.3,4.97,15.875705573416559,4.4720297389905799,800,58.8,1114,5.5,44,215,2.94,325,10,857.53146581675219,1114,1114,15.316670010982557,38.265306122448983,0.57718479384110821,0.5050033763265307,0.11429439360279736,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.11925245180386546,0.17772178068901734,2.8620588432927709,8.5306454730728323,6.370315011701603,23.144272670531002,2.5100581271478877,153.76430156676318,0.15981473447468164,34.597872067302063,-147190.1614300411,857.53146581675219,5.2802152501024095E-2,8.3252791049951913,-153289.14725702503,1626.8323976123518,4.064779815938893,6.2379208292969474E-2,13.047361200524579,-152743.3205284102,1463.718290155211]
["KBM","KBMS-35H02-A (400 V)",17.3,4.97,15.311803145737517,4.3131839847147937,1450,58.8,1863,5.5,44,215,2.94,565,10,857.53146581675219,1610.1495498953313,1823.2558139534885,15.092210848279965,38.265306122448983,0.57688137325798738,0.5050033763265307,8.6986652643395598E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.11925245180386546,0.17772178068901734,2.8620588432927709,8.5306454730728323,6.370315011701603,23.144272670531002,2.5100581271478877,153.76430156676318,0.15981473447468164,34.597872067302063,-147190.1614300411,857.53146581675219,5.362397440525446E-2,8.8300997322324388,-153242.30902498015,1610.1495498953313,4.3112562007405,6.2379208292969474E-2,13.047361200524579,-152743.3205284102,1463.718290155211]
["KBM","KBMS-35H02-A (480 V)",17.3,4.97,15.006037491521562,4.2270528145131161,1750,58.8,2235,5.5,44,215,2.94,679,10,857.53146581675219,1607.3225630716925,1823.2558139534885,15.193064172161183,38.265306122448983,0.57683666212924523,0.5050033763265307,8.6986652643395598E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.11925245180386546,0.17772178068901734,2.8620588432927709,8.5306454730728323,6.370315011701603,23.144272670531002,2.5100581271478877,153.76430156676318,0.15981473447468164,34.597872067302063,-147190.1614300411,857.53146581675219,5.3766592406847689E-2,8.9147952846383145,-153234.18077356945,1607.3225630716925,4.352608420597325,6.2379208292969474E-2,13.047361200524579,-152743.3205284102,1463.718290155211]
["KBM","KBMS-35H02-B (120 V)",17.600000000000001,6.3,16.472536610011169,5.7395597944289785,400,58.8,661,3.43,28,174,2.94,160,10,661,661,661,15.736866748043456,38.265306122448983,0.56806946846405804,0.5050033763265307,0.19262322915811841,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.14858840225561662,0.22144111118181817,3.5661216541347986,10.629173336727272,7.9374043479668659,23.144272670531002,2.5100581271478877,153.76430156676318,0.10169026752584735,21.757510581125761,-149755.05176800271,1111.2584359485968,3.2526294475423566E-2,3.862214476207408,-153540.82734954893,2114.1147632211291,3.7362195762648978,4.0432207847809723E-2,8.2050739659353855,-153108.08740597774,1847.1429105577213]
["KBM","KBMS-35H02-B (240 V)",17.600000000000001,6.3,16.083025828233634,5.6038417519977815,950,58.8,1386,3.43,28,174,2.94,325,10,1111.2584359485968,1386,1386,15.386814524138753,38.265306122448983,0.56719275416763071,0.5050033763265307,9.1864325016967008E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.14858840225561662,0.22144111118181817,3.5661216541347986,10.629173336727272,7.9374043479668659,23.144272670531002,2.5100581271478877,153.76430156676318,0.10169026752584735,21.757510581125761,-149755.05176800271,1111.2584359485968,3.4240428290349845E-2,5.1263351208187977,-153447.00211577702,2043.4103647544835,4.9591015079269551,4.0432207847809723E-2,8.2050739659353855,-153108.08740597774,1847.1429105577213]
["KBM","KBMS-35H02-B (400 V)",17.600000000000001,6.3,15.305400360670603,5.3328921117319172,1800,58.8,2313,3.43,28,174,2.94,565,10,1111.2584359485968,2021.2269895976979,2252.8735632183907,15.0233851548146,38.265306122448983,0.56696213185597977,0.5050033763265307,6.8930213112245023E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.14858840225561662,0.22144111118181817,3.5661216541347986,10.629173336727272,7.9374043479668659,23.144272670531002,2.5100581271478877,153.76430156676318,0.10169026752584735,21.757510581125761,-149755.05176800271,1111.2584359485968,3.4833068348206632E-2,5.4961614478324536,-153414.5632294504,2021.2269895976979,5.3168631939541404,4.0432207847809723E-2,8.2050739659353855,-153108.08740597774,1847.1429105577213]
["KBM","KBMS-35H02-B (480 V)",17.600000000000001,6.3,14.823112654331526,5.16484761474966,2200,58.8,2776,3.43,28,174,2.94,679,10,1111.2584359485968,2018.7762202641377,2252.8735632183907,15.051857209187311,38.265306122448983,0.56695314381901241,0.5050033763265307,6.8930213112245023E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.14858840225561662,0.22144111118181817,3.5661216541347986,10.629173336727272,7.9374043479668659,23.144272670531002,2.5100581271478877,153.76430156676318,0.10169026752584735,21.757510581125761,-149755.05176800271,1111.2584359485968,3.4900136742243348E-2,5.5364584438365148,-153410.89215797721,2018.7762202641377,5.3558456032073121,4.0432207847809723E-2,8.2050739659353855,-153108.08740597774,1847.1429105577213]
["KBM","KBMS-35H02-C (120 V)",17.5,8.6999999999999993,16.119212636347161,7.8630305543156886,625,59.2,923,1.8,14.6,124,2.94,160,10,923,923,923,15.460853221357487,38.265306122448983,0.57088458665107844,0.50159119135135133,0.13794577949460052,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.20636604220752849,0.3075470561828571,4.9527850129806836,14.762258696777142,11.023812732523234,23.144272670531002,2.5100581271478877,153.76430156676318,5.3339831827869243E-2,11.37778514160213,-151559.19389424328,1582.3588978511495,1.6559892901456714E-2,2.0092265861243424,-153598.36213133472,2985.4802653506345,5.1972558707967824,2.070232758886624E-2,4.2617369960748226,-153368.69559339696,2620.8326343818303]
["KBM","KBMS-35H02-C (240 V)",17.5,8.6999999999999993,15.48350232079725,7.5529279613645128,1400,59.2,1935,1.8,14.6,124,2.94,325,10,1582.3588978511495,1935,1935,14.712912136244771,38.265306122448983,0.5703270737049837,0.50159119135135133,6.5800493267967067E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.20636604220752849,0.3075470561828571,4.9527850129806836,14.762258696777142,11.023812732523234,23.144272670531002,2.5100581271478877,153.76430156676318,5.3339831827869243E-2,11.37778514160213,-151559.19389424328,1582.3588978511495,1.726035169202407E-2,2.5348583103583557,-153559.52701200583,2910.2010335656405,6.5569046946369021,2.070232758886624E-2,4.2617369960748226,-153368.69559339696,2620.8326343818303]
["KBM","KBMS-35H02-C (400 V)",17.5,8.6999999999999993,14.155427879702691,6.9050867705866787,2550,59.2,3224,1.8,14.6,124,2.94,565,10,1582.3588978511495,2892.351613556963,3161.2903225806449,13.706400561255077,38.265306122448983,0.57023382056044158,0.50159119135135133,4.8581490020841361E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.20636604220752849,0.3075470561828571,4.9527850129806836,14.762258696777142,11.023812732523234,23.144272670531002,2.5100581271478877,153.76430156676318,5.3339831827869243E-2,11.37778514160213,-151559.19389424328,1582.3588978511495,1.7437914362831139E-2,2.6516000574379022,-153549.68251065613,2892.351613556963,6.8588799594310039,2.070232758886624E-2,4.2617369960748226,-153368.69559339696,2620.8326343818303]
["KBM","KBMS-35H02-C (480 V)",17.5,8.6999999999999993,13.100441253251635,6.3904591479276274,3200,59.2,3869,1.8,14.6,124,2.94,679,10,1582.3588978511495,2895.1341733706049,3161.2903225806449,13.519589726417893,38.265306122448983,0.57027963644474466,0.50159119135135133,4.8581490020841361E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.20636604220752849,0.3075470561828571,4.9527850129806836,14.762258696777142,11.023812732523234,23.144272670531002,2.5100581271478877,153.76430156676318,5.3339831827869243E-2,11.37778514160213,-151559.19389424328,1582.3588978511495,1.740994789043911E-2,2.6335563715177921,-153551.23303912004,2895.1341733706049,6.8122064517108036,2.070232758886624E-2,4.2617369960748226,-153368.69559339696,2620.8326343818303]
["KBM","KBMS-35H02-D (120 V)",17.45,10.92,15.952942531093511,9.7274039823740921,850,59.4,1165,1.1399999999999999,9.3000000000000007,99,2.94,160,10,1165,1165,1165,15.398150645557577,38.265306122448983,0.57219811973965762,0.49990233212121216,0.10929094804593671,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.25976715519453747,0.38713066848825223,6.2344117246688988,18.582272087436106,13.876432586932717,23.144272670531002,2.5100581271478877,153.76430156676318,3.4373633840441876E-2,7.2663167473263588,-152317.21500172239,2002.0026704673478,1.0501885974165558E-2,1.2271909822872074,-153625.5856109834,3766.7256867838596,6.2778579121974181,1.3225365125620886E-2,2.7125546922484518,-153476.31626980822,3305.5583462678205]
["KBM","KBMS-35H02-D (240 V)",17.45,10.92,15.020785439916175,9.1590155121440091,1850,59.4,2437,1.1399999999999999,9.3000000000000007,99,2.94,325,10,2002.0026704673478,2437,2437,14.250002225446334,38.265306122448983,0.57187154420376596,0.49990233212121216,5.2246185668246313E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.25976715519453747,0.38713066848825223,6.2344117246688988,18.582272087436106,13.876432586932717,23.144272670530995,2.5100581271478877,153.76430156676318,3.4373633840441876E-2,7.2663167473263588,-152317.21500172239,2002.0026704673478,1.0874825046858716E-2,1.5189911219318206,-153605.14544361524,3689.1116414379985,7.7706001519049126,1.3225365125620886E-2,2.7125546922484518,-153476.31626980822,3305.5583462678205]
["KBM","KBMS-35H02-D (400 V)",17.45,10.92,12.441369265697876,7.5862007717669977,3500,59.4,4061,1.1399999999999999,9.3000000000000007,99,2.94,565,10,2002.0026704673478,3689.2264070400279,3959.5959595959598,12.170579209114376,38.265306122448983,0.57195745834159051,0.49990233212121216,3.8518138582328422E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.25976715519453747,0.38713066848825223,6.2344117246688988,18.582272087436106,13.876432586932717,23.144272670531002,2.5100581271478877,153.76430156676318,3.4373633840441876E-2,7.2663167473263588,-152317.21500172239,2002.0026704673478,1.0874248519556684E-2,1.518583300642991,-153605.17704211327,3689.2264070400279,7.7685138881189211,1.3225365125620886E-2,2.7125546922484518,-153476.31626980822,3305.5583462678205]
["KBM","KBMS-35H02-D (480 V)",17.45,10.92,10.548641577020971,6.4320985225737637,4300,59.4,4873,1.1399999999999999,9.3000000000000007,99,2.94,679,10,2002.0026704673478,3705.6481239737191,3959.5959595959598,11.502556769073845,38.265306122448983,0.57208419663224752,0.49990233212121216,3.8518138582328422E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.25976715519453747,0.38713066848825223,6.2344117246688988,18.582272087436106,13.876432586932717,23.144272670531002,2.5100581271478877,153.76430156676318,3.4373633840441876E-2,7.2663167473263588,-152317.21500172239,2002.0026704673478,1.0792507720717708E-2,1.4596089607688871,-153609.65711870327,3705.6481239737191,7.466822846105857,1.3225365125620886E-2,2.7125546922484518,-153476.31626980822,3305.5583462678205]
["KBM","KBMS-35H02-E (120 V)",17.100000000000001,12,15.580431271101332,10.671528267877624,950,59.4,1305,0.94,7.4,88.4,2.94,160,10,1305,1305,1305,15.012592430302355,38.265306122448983,0.58381384103583622,0.49990233212121216,9.7566248638709788E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.29130112834295213,0.43412570947368417,6.9912270802308507,20.838034054736841,15.560937513140278,23.144272670531002,2.5100581271478877,153.76430156676318,2.7378895815966042E-2,5.9994622722815141,-152512.5101030471,2253.1561378740516,8.3352040953843035E-3,0.97870148199852725,-153633.35666912576,4234.9272816847788,6.8000091952456856,1.0540984432527377E-2,2.2396311781526377,-153503.53198215403,3711.3339060882158]
["KBM","KBMS-35H02-E (240 V)",17.100000000000001,12,14.533563583806249,9.9544956053467466,2050,59.4,2728,0.94,7.4,88.4,2.94,325,10,2253.1561378740516,2728,2728,13.684761686157778,38.265306122448983,0.5835501016839334,0.49990233212121216,4.6673003839265495E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.29130112834295213,0.43412570947368417,6.9912270802308507,20.838034054736841,15.560937513140278,23.144272670531002,2.5100581271478877,153.76430156676318,2.7378895815966042E-2,5.9994622722815141,-152512.5101030471,2253.1561378740516,8.5882898943108812E-3,1.1930934477932444,-153618.46090454335,4160.4085627941186,8.2896026674185102,1.0540984432527377E-2,2.2396311781526377,-153503.53198215403,3711.3339060882158]
["KBM","KBMS-35H02-E (400 V)",17.100000000000001,12,11.496360954248335,7.8742198316769416,3850,59.4,4547,0.94,7.4,88.4,2.94,565,10,2253.1561378740516,4174.7848500237424,4434.3891402714926,11.023639638128428,38.265306122448983,0.58370451911458077,0.49990233212121216,3.4306790414262947E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.29130112834295213,0.43412570947368417,6.9912270802308507,20.838034054736841,15.560937513140278,23.144272670531002,2.5100581271478877,153.76430156676318,2.7378895815966042E-2,5.9994622722815141,-152512.5101030471,2253.1561378740516,8.5378926312561099E-3,1.153582876953219,-153621.42711509031,4174.7848500237424,8.0150835725123244,1.0540984432527377E-2,2.2396311781526377,-153503.53198215403,3711.3339060882158]
["KBM","KBMS-35H02-E (480 V)",17.100000000000001,12,9.1226258870120436,6.2483738952137289,4700,59.4,5457,0.94,7.4,88.4,2.94,679,10,2253.1561378740516,4203.5162500050792,4434.3891402714926,9.9653145284436739,38.265306122448983,0.58388805905263086,0.49990233212121216,3.4306790414262947E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.29130112834295213,0.43412570947368417,6.9912270802308507,20.838034054736841,15.560937513140278,23.144272670531002,2.5100581271478877,153.76430156676318,2.7378895815966042E-2,5.9994622722815141,-152512.5101030471,2253.1561378740516,8.4393973669149754E-3,1.0721690564651323,-153627.22420949992,4203.5162500050792,7.449421071615137,1.0540984432527377E-2,2.2396311781526377,-153503.53198215403,3711.3339060882158]
["KBM","KBMS-35H02-F (120 V)",17.3,14.92,15.597184423005743,13.106877666391382,1200,59.4,1607,0.61,4.9000000000000004,72.099999999999994,2.94,160,10,1607,1607,1607,15.019646139808524,38.265306122448983,0.5769168322268321,0.49990233212121216,7.9230836635666629E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.35799729998263036,0.53352293116300575,8.5919351995831281,25.609100695824278,19.123762570339622,23.144272670531002,2.5100581271478877,153.76430156676318,1.8154352086988401E-2,3.9024279373386861,-152931.61529938379,2796.916872940772,5.513236410808457E-3,0.60832543053478261,-153646.20322033876,5224.191013076359,7.9856495094279758,7.0039094242916331E-3,1.4567971065236665,-153561.93716686565,4579.588487398375]
["KBM","KBMS-35H02-F (240 V)",17.3,14.92,13.873506360085971,11.658408705954598,2650,59.4,3356,0.61,4.9000000000000004,72.099999999999994,2.94,325,10,2796.916872940772,3356,3356,12.960636733754157,38.265306122448983,0.5768234584312173,0.49990233212121216,3.7939199783526896E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.35799729998263036,0.53352293116300575,8.5919351995831281,25.609100695824278,19.123762570339622,23.144272670531002,2.5100581271478877,153.76430156676318,1.8154352086988401E-2,3.9024279373386861,-152931.61529938379,2796.916872940772,5.6227734078775574E-3,0.70626771998621352,-153640.01121822372,5164.8664220732444,9.2713639583907526,7.0039094242916331E-3,1.4567971065236665,-153561.93716686565,4579.588487398375]
["KBM","KBMS-35H02-F (400 V)",17.3,14.92,7.6956096012669395,6.4668988245940673,5100,59.4,5593,0.61,4.9000000000000004,72.099999999999994,2.94,565,10,2796.916872940772,5252.861306938913,5436.8932038834955,7.4077390779920602,38.265306122448983,0.57726110428427357,0.49990233212121216,2.780248811085817E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.35799729998263036,0.53352293116300575,8.5919351995831281,25.609100695824278,19.123762570339622,23.144272670531002,2.5100581271478877,153.76430156676318,1.8154352086988401E-2,3.9024279373386861,-152931.61529938379,2796.916872940772,5.4624426417988767E-3,0.55709492685418871,-153649.07453444772,5252.861306938913,7.3131330798172112,7.0039094242916331E-3,1.4567971065236665,-153561.93716686565,4579.588487398375]
["KBM","KBMS-35H02-F (480 V)",17.3,14.92,6.2689363695640994,5.2680137559362183,5400,59.4,6711,0.61,4.9000000000000004,72.099999999999994,2.94,679,10,2796.916872940772,5276.8328104900702,5436.8932038834955,6.5205410185763206,38.265306122448983,0.57737954771261635,0.49990233212121216,2.780248811085817E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.35799729998263036,0.53352293116300575,8.5919351995831281,25.609100695824278,19.123762570339622,23.144272670531002,2.5100581271478877,153.76430156676318,1.8154352086988401E-2,3.9024279373386861,-152931.61529938379,2796.916872940772,5.4211388999505124E-3,0.51166849754218746,-153651.40938809284,5276.8328104900702,6.7168082761154437,7.0039094242916331E-3,1.4567971065236665,-153561.93716686565,4579.588487398375]
["KBM","KBMS-35H02-G (120 V)",17.100000000000001,18.64,15.094049441618461,16.057499405977087,1550,59.4,2032,0.39,3.1,57,2.94,160,10,2032,2032,2032,14.470263526044331,38.265306122448983,0.58358213702074835,0.49990233212121216,6.2659426414132025E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.4524877526927189,0.67434193538245613,10.859706064625254,32.368412898357896,24.1713229370779,23.144272670531002,2.5100581271478877,153.76430156676318,1.1533272593584727E-2,2.4930806770391358,-153185.74120789274,3537.977740736279,3.4060161806484233E-3,0.34322692288443074,-153654.93530928035,6666.4100638283626,8.91417707244503,4.4034702267088475E-3,0.93068027775485584,-153597.35135584782,5801.281655197814]
["KBM","KBMS-35H02-G (240 V)",17.100000000000001,18.64,12.44217172759582,13.236352901697682,3400,59.4,4241,0.39,3.1,57,2.94,325,10,3537.977740736279,4241,4241,11.290044204921728,38.265306122448983,0.58363962230165001,0.49990233212121216,3.0022153848978134E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.4524877526927189,0.67434193538245613,10.859706064625254,32.368412898357896,24.1713229370779,23.144272670531002,2.5100581271478877,153.76430156676318,1.1533272593584727E-2,2.4930806770391358,-153185.74120789274,3537.977740736279,3.4222112164554144E-3,0.36049325899491452,-153654.00035474141,6648.2119964169224,9.3626126910373095,4.4034702267088475E-3,0.93068027775485584,-153597.35135584782,5801.281655197814]
["KBM","KBMS-35H02-G (400 V)",17.100000000000001,18.64,3.6056826762543186,3.8358326343131051,5800,59.4,7068,0.39,3.1,57,2.94,565,10,3537.977740736279,6826.1425239818409,6877.1929824561403,1.218252876599097,38.265306122448983,0.58436622409385153,0.49990233212121216,2.1947556081755994E-2,-23.252096948148147,9,29.694198528000001,9,-2411.7753600000001,7.5,2423.7753600000001,9,0.4524877526927189,0.67434193538245613,10.859706064625254,32.368412898357896,24.1713229370779,23.144272670531002,2.5100581271478877,153.76430156676318,1.1533272593584727E-2,2.4930806770391358,-153185.74120789274,3537.977740736279,3.2766455911482596E-3,0.14401975994174171,-153662.40399420948,6826.1425239818409,3.7404339708047623,4.4034702267088475E-3,0.93068027775485584,-153597.35135584782,5801.281655197814]
["KBM","KBMS-35H03-A (120 V)",21.8,10.199999999999999,20.567715722644937,9.3489616921113345,650,76.099999999999994,867,1.41,12,132,3.7,160,10,867,867,867,20.156322356204864,30.405405405405403,0.45850281604321186,0.39224953272010515,0.14685577217245244,-23.444678320987656,9,29.850189440000001,9,-2427.6928000000003,7.5,2439.6928000000003,9,0.19448772903621947,0.29097088330275228,4.6677054968692673,13.966602398532109,10.421612712025697,23.175815942689891,2.5367427701383081,155.39898302995414,5.4962565284357029E-2,11.478417209983911,-151773.58933588077,1560.603075234483,1.88625219325293E-2,2.2469914249745417,-153591.55724196642,2794.5981024722278,6.9702401895327348,2.0639813543084352E-2,3.3596079563360424,-153502.05432707362,2646.947336505199]
["KBM","KBMS-35H03-A (240 V)",21.8,10.199999999999999,19.644267261628229,8.9292123916491946,1400,76.099999999999994,1818,1.41,12,132,3.7,325,10,1560.603075234483,1818,1818,19.000627058314372,30.405405405405403,0.4583364322780018,0.39224953272010515,7.0035178478281779E-2,-23.444678320987656,9,29.850189440000001,9,-2427.6928000000003,7.5,2439.6928000000003,9,0.19448772903621947,0.29097088330275228,4.6677054968692673,13.966602398532109,10.421612712025697,23.175815942689891,2.5367427701383081,155.39898302995414,5.4962565284357029E-2,11.478417209983911,-151773.58933588077,1560.603075234483,1.9300471651469815E-2,2.5663398933577954,-153569.50246142907,2755.075047787926,7.9608694834633518,2.0639813543084352E-2,3.3596079563360424,-153502.05432707362,2646.947336505199]
["KBM","KBMS-35H03-A (400 V)",21.8,10.199999999999999,17.188733853924695,7.8130608426930426,2550,76.099999999999994,3029,1.41,12,132,3.7,565,10,1560.603075234483,2757.9518566478291,2969.6969696969695,16.812686263111502,30.405405405405403,0.4584619197132826,0.39224953272010515,4.8102186514078452E-2,-23.444678320987656,9,29.850189440000001,9,-2427.6928000000003,7.5,2439.6928000000003,9,0.19448772903621947,0.29097088330275228,4.6677054968692673,13.966602398532109,10.421612712025697,23.175815942689891,2.5367427701383081,155.39898302995414,5.4962565284357029E-2,11.478417209983911,-151773.58933588077,1560.603075234483,1.9267648967005745E-2,2.5437960485275015,-153571.15538429029,2757.9518566478291,7.8909377465122486,2.0639813543084352E-2,3.3596079563360424,-153502.05432707362,2646.947336505199]
["KBM","KBMS-35H03-A (480 V)",21.8,10.199999999999999,15.586916362161105,7.0849619828005022,3100,76.099999999999994,3635,1.41,12,132,3.7,679,10,1560.603075234483,2764.8805111003335,2969.6969696969695,16.258569721258993,30.405405405405403,0.45855350045529114,0.39224953272010515,4.8102186514078452E-2,-23.444678320987656,9,29.850189440000001,9,-2427.6928000000003,7.5,2439.6928000000003,9,0.19448772903621947,0.29097088330275228,4.6677054968692673,13.966602398532109,10.421612712025697,23.175815942689891,2.5367427701383081,155.39898302995414,5.4962565284357029E-2,11.478417209983911,-151773.58933588077,1560.603075234483,1.9189200506992642E-2,2.4890876667742283,-153575.10598294181,2764.8805111003335,7.7212305740848821,2.0639813543084352E-2,3.3596079563360424,-153502.05432707362,2646.947336505199]
["KBM","KBMS-35H03-B (120 V)",21.7,14,19.629109648000426,12.345351979874481,900,76.599999999999994,1197,0.75,6.2,96.2,3.7,160,10,1197,1197,1197,18.945715831840566,30.405405405405403,0.46081109327959729,0.38968915718015668,0.10636921844069863,-23.444678320987656,9,29.850189440000001,9,-2427.6928000000003,7.5,2439.6928000000003,9,0.26817409822831029,0.40121222365591397,6.4361783574794469,19.258186735483871,14.370092164589515,23.175815942689891,2.5367427701383081,155.39898302995414,2.8557938666551951E-2,6.1758115339889281,-152633.66623309054,2206.2605912194163,9.7234107021318961E-3,0.96260668921243664,-153638.96845735353,3925.8475876381681,7.7028583664661774,1.0886593475389178E-2,1.7957940006339632,-153576.88300284208,3674.3532324855669]
["KBM","KBMS-35H03-B (240 V)",21.7,14,17.910753839658661,11.264625056389095,2050,76.599999999999994,2504,0.75,6.2,96.2,3.7,325,10,2206.2605912194163,2504,2504,17.07157444610014,30.405405405405403,0.46059746666647783,0.38968915718015668,5.0848224629998509E-2,-23.444678320987656,9,29.850189440000001,9,-2427.6928000000003,7.5,2439.6928000000003,9,0.26817409822831029,0.40121222365591397,6.4361783574794469,19.258186735483871,14.370092164589515,23.175815942689891,2.5367427701383081,155.39898302995414,2.8557938666551951E-2,6.1758115339889281,-152633.66623309054,2206.2605912194163,9.9572516567399006E-3,1.1784074983211812,-153626.48708100923,3869.1984581713355,9.4297142948136852,1.0886593475389178E-2,1.7957940006339632,-153576.88300284208,3674.3532324855669]
["KBM","KBMS-35H03-B (400 V)",21.7,14,13.105153077224749,8.2422346397639927,3800,76.599999999999994,4173,0.75,6.2,96.2,3.7,565,10,2206.2605912194163,3890.3310601911166,4074.8440748440748,12.900842120720895,30.405405405405403,0.46079258805448997,0.38968915718015668,3.465207246484199E-2,-23.444678320987656,9,29.850189440000001,9,-2427.6928000000003,7.5,2439.6928000000003,9,0.26817409822831029,0.40121222365591397,6.4361783574794469,19.258186735483871,14.370092164589515,23.175815942689891,2.5367427701383081,155.39898302995414,2.8557938666551951E-2,6.1758115339889281,-152633.66623309054,2206.2605912194163,9.8679382305438077E-3,1.1009882307676908,-153631.25422920543,3890.3310601911166,8.810198910718448,1.0886593475389178E-2,1.7957940006339632,-153576.88300284208,3674.3532324855669]
["KBM","KBMS-35H03-B (480 V)",21.7,14,10.26549382942725,6.4562854273127357,4800,76.599999999999994,5007,0.75,6.2,96.2,3.7,679,10,2206.2605912194163,3896.7407182090428,4074.8440748440748,12.417227960940959,30.405405405405403,0.46084944229724217,0.38968915718015668,3.465207246484199E-2,-23.444678320987656,9,29.850189440000001,9,-2427.6928000000003,7.5,2439.6928000000003,9,0.26817409822831029,0.40121222365591397,6.4361783574794469,19.258186735483871,14.370092164589515,23.175815942689891,2.5367427701383081,155.39898302995414,2.8557938666551951E-2,6.1758115339889281,-152633.66623309054,2206.2605912194163,9.8413264746536177E-3,1.0768446872285196,-153632.67464480799,3896.7407182090428,8.6170002778489838,1.0886593475389178E-2,1.7957940006339632,-153576.88300284208,3674.3532324855669]
["KBM","KBMS-35H03-C (120 V)",20.7,20.2,18.044877685729375,17.185597795932736,1450,75.2,1813,0.36,2.8,63.6,3.7,160,10,1813,1813,1813,17.380181547743007,30.405405405405403,0.48288375302028957,0.39694400851063832,7.0228325688646592E-2,-23.444678320987656,9,29.850189440000001,9,-2427.6928000000003,7.5,2439.6928000000003,9,0.40562951765837657,0.60685771607085348,9.7351084238010372,29.129170371400967,21.735632158130326,23.175815942689891,2.5367427701383081,155.39898302995414,1.2726010844285641E-2,2.9101750186989843,-153140.56351116823,3356.5016857011433,4.1851083187243619E-3,0.36976593975609601,-153655.54955486557,6015.2611869870007,9.3240943769801277,4.8065462984151833E-3,0.86197073154754189,-153618.07905504352,5564.3781375966628]
["KBM","KBMS-35H03-C (240 V)",20.7,20.2,14.724399251211478,14.023237382106169,3100,75.2,3783,0.36,2.8,63.6,3.7,325,10,{"$f":"IF(AQ1083<I1083,IF(AQ1083<0,0,AQ1083),I1083)","v":3356.5016857011433},{"$f":"IF(AU1083<I1083,IF(AU1083<0,0,AU1083),I1083)","v":3783},{"$f":"IF(UAC_V*0.98/L1083*1000<I1083,IF(UAC_V*0.98/L1083*1000<0,0,UAC_V*0.98/L1083*1000),I1083)","v":3783},{"$f":"C1083+(E1083-C1083)/G1083*Q1083","v":13.407839473333233},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M1083,(inertia/gear^2+gear_inertia)/M1083),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M1083,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M1083))","v":30.405405405405403},{"$f":"IF((C1083+(E1083-C1083)/G1083*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X1083^2*time1+Y1083^2*time2+Z1083^2*time3+AA1083^2*time4)/time)/(C1083+(E1083-C1083)/G1083*mspeed),SQRT((((X1083-Y1083)*2/PI()+Y1083)^2*time1+Y1083^2*time2+((Z1083-Y1083)*2/PI()+Y1083)^2*time3+AA1083^2*time4)/time)/(C1083+(E1083-C1083)/G1083*mspeed)),IF(AccType=1,SQRT((X1083^2*time1+Y1083^2*time2+Z1083^2*time3+AA1083^2*time4+AB1083^2*time5+AC1083^2*time6+AD1083^2*time7+AE1083^2*time8)/time)/(C1083+(E1083-C1083)/G1083*mspeed),SQRT((((X1083-Y1083)*2/PI()+Y1083)^2*time1+Y1083^2*time2+((Z1083-Y1083)*2/PI()+Y1083)^2*time3+AA1083^2*time4+((AB1083-AC1083)*2/PI()+AC1083)^2*time5+AC1083^2*time6+((AD1083-AC1083)*2/PI()+AC1083)^2*time7+AE1083^2*time8)/time)/(C1083+(E1083-C1083)/G1083*mspeed))))","v":0.48293379687482568},{"$f":"IF(move1,MAX(ABS(X1083),ABS(Z1083))/H1083,MAX(ABS(X1083),ABS(Z1083),ABS(AB1083),ABS(AD1083))/H1083)","v":0.39694400851063832},{"$f":"IF(AZ1083>0,speed/(MIN(AZ1083,I1083)),\"NA\")","v":3.3656874034765069E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M1083+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M1083+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-23.444678320987656},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M1083+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M1083+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.850189440000001},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M1083+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M1083+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2427.6928000000003},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M1083+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M1083+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2439.6928000000003},9,{"$f":"AH1083/Irms","v":0.40562951765837657},{"$f":"AI1083/Ipeak","v":0.60685771607085348},{"$f":"IF(move1,IF(AccType=1,SQRT((X1083^2*time1+Y1083^2*time2+Z1083^2*time3+AA1083^2*time4)/time)/(C1083/D1083),SQRT((((X1083-Y1083)*2/PI()+Y1083)^2*time1+Y1083^2*time2+((Z1083-AA1083)*2/PI()+AA1083)^2*time3+AA1083^2*time4)/time)/(C1083/D1083)),IF(AccType=1,SQRT((X1083^2*time1+Y1083^2*time2+Z1083^2*time3+AA1083^2*time4+AB1083^2*time5+AC1083^2*time6+AD1083^2*time7+AE1083^2*time8)/time)/(C1083/D1083),SQRT((((X1083-Y1083)*2/PI()+Y1083)^2*time1+Y1083^2*time2+((Z1083-AA1083)*2/PI()+AA1083)^2*time3+AA1083^2*time4+((AB1083-AC1083)*2/PI()+AC1083)^2*time5+AC1083^2*time6+((AD1083-AE1083)*2/PI()+AE1083)^2*time7+AE1083^2*time8)/time)/(C1083/D1083)))","v":9.7351084238010372},{"$f":"IF(move1,MAX(ABS(X1083),ABS(Z1083))/(C1083/D1083),MAX(ABS(X1083),ABS(Z1083),ABS(AB1083),ABS(AD1083))/(C1083/D1083))","v":29.129170371400967},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X1083),ABS(Z1083))/(C1083/D1083),MAX(ABS((X1083-Y1083)*2/PI()+Y1083),ABS((Z1083-Y1083)*2/PI()+Y1083))/(C1083/D1083)),IF(AccType=1,MAX(ABS(X1083),ABS(Z1083),ABS(AB1083),ABS(AD1083))/(C1083/D1083),MAX(ABS((X1083-Y1083)*2/PI()+Y1083),ABS((Z1083-Y1083)*2/PI()+Y1083),ABS((AB1083-AC1083)*2/PI()+AC1083),ABS((AD1083-AC1083)*2/PI()+AC1083))/(C1083/D1083)))","v":21.735632158130326},{"$f":"IF((C1083+(E1083-C1083)/G1083*mspeed)<0,\"NA\",U1083*(C1083+(E1083-C1083)/G1083*mspeed)*mspeed/9.55)","v":23.175815942689891},{"$f":"IF(move1,IF(speed1>speed2,AM1083/2*time1/time,AM1083/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z1083*-speed/30*PI(),((Z1083-AA1083)*2/PI()+AA1083)*-speed/30*PI()),IF(AccType=1,X1083*-speed/30*PI(),((X1083-Y1083)*2/PI()+Y1083)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z1083*-speed/30*PI(),((Z1083-AA1083)*2/PI()+AA1083)*-speed/30*PI()),IF(AccType=1,X1083*-speed/30*PI(),((X1083-Y1083)*2/PI()+Y1083)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD1083*-speed/30*PI(),((AD1083-AE1083)*2/PI()+AE1083)*-speed/30*PI()),IF(AccType=1,AB1083*-speed/30*PI(),((AB1083-AC1083)*2/PI()+AC1083)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD1083*-speed/30*PI(),((AD1083-AE1083)*2/PI()+AE1083)*-speed/30*PI()),IF(AccType=1,AB1083*-speed/30*PI(),((AB1083-AC1083)*2/PI()+AC1083)*-speed/30*PI()),0)/2*time7/time)))","v":2.5367427701383081},{"$f":"IF(move1,MAX(IF(AccType=1,Z1083*-speed/30*PI(),((Z1083-AA1083)*2/PI()+AA1083)*-speed/30*PI()),IF(AccType=1,X1083*-speed/30*PI(),((X1083-Y1083)*2/PI()+Y1083)*-speed/30*PI()),0),MAX(IF(AccType=1,Z1083*-speed/30*PI(),((Z1083-AA1083)*2/PI()+AA1083)*-speed/30*PI()),IF(AccType=1,X1083*-speed/30*PI(),((X1083-Y1083)*2/PI()+Y1083)*-speed/30*PI()),IF(AccType=1,AD1083*-speed/30*PI(),((AD1083-AE1083)*2/PI()+AE1083)*-speed/30*PI()),IF(AccType=1,AB1083*-speed/30*PI(),((AB1083-AC1083)*2/PI()+AC1083)*-speed/30*PI()),0))","v":155.39898302995414},{"$f":"(L1083^2)/1000000+((K1083/1000)^2*(D1083/C1083*H1083)^2*PI()*PI()*(O1083/2)^2)/1200","v":1.2726010844285641E-2},{"$f":"SQRT(3)*L1083*J1083*D1083/C1083*H1083/1000","v":2.9101750186989843},{"$f":"0.75*J1083^2*(D1083/C1083*H1083)^2-(UAC_V*0.98)^2","v":-153140.56351116823},{"$f":"-AO1083/2/AN1083+SQRT((AO1083/2/AN1083)^2-AP1083/AN1083)","v":3356.5016857011433},{"$f":"(L1083^2)/1000000+((K1083/1000)^2*AV1083^2*PI()*PI()*(O1083/2)^2)/1200","v":4.1990247384286186E-3},{"$f":"SQRT(3)*L1083*J1083*AV1083/1000","v":0.38768998647315311},{"$f":"0.75*J1083^2*AV1083^2-(UAC_V*0.98)^2","v":-153654.71044425585},{"$f":"-AS1083/2/AR1083+SQRT((AS1083/2/AR1083)^2-AT1083/AR1083)","v":6003.2227110025178},{"$f":"D1083+(F1083-D1083)*((0.85*UAC_V-D1083*J1083)/L1083*1000)/G1083","v":9.7760708443569762},{"$f":"(L1083^2)/1000000+((K1083/1000)^2*AJ1083^2*PI()*PI()*(O1083/2)^2)/1200","v":4.8065462984151833E-3},{"$f":"SQRT(3)*L1083*J1083*AJ1083/1000","v":0.86197073154754189},{"$f":"0.75*J1083^2*AJ1083^2-(UAC_V*0.98)^2","v":-153618.07905504352},{"$f":"IF(((AX1083/2/AW1083)^2-AY1083/AW1083)>0,-AX1083/2/AW1083+SQRT((AX1083/2/AW1083)^2-AY1083/AW1083),-9999)","v":5564.3781375966628}]
["KBM","KBMS-35H03-C (400 V)",20.7,20.2,5.7009300615516914,5.4294572014778009,5000,75.2,6305,0.36,2.8,63.6,3.7,565,10,3356.5016857011433,6112.9947454684125,6163.5220125786154,2.3621528558704554,30.405405405405403,0.48349056018737324,0.39694400851063832,2.2881973748913723E-2,-23.444678320987656,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},29.850189440000001,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},-2427.6928000000003,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},2439.6928000000003,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},0.40562951765837657,0.60685771607085348,9.7351084238010372,29.129170371400967,21.735632158130326,23.175815942689891,2.5367427701383081,155.39898302995414,1.2726010844285641E-2,2.9101750186989843,-153140.56351116823,3356.5016857011433,4.0812606379096363E-3,0.18818720276219852,-153661.81120064948,6112.9947454684125,4.7453674079663699,4.8065462984151833E-3,0.86197073154754189,-153618.07905504352,5564.3781375966628]
["KBM","KBMS-35H03-D (120 V)",20,21.5,17.188733853924695,17.904931097838226,1550,75.7,1996,0.32,2.2999999999999998,57.8,3.7,160,10,1996,1996,1996,16.379814691892705,30.405405405405403,0.49980941824906372,0.39432218546895642,6.3789556349457044E-2,-23.444678320987656,9,29.850189440000001,9,-2427.6928000000003,7.5,2439.6928000000003,9,0.44684509117292204,0.66851986766666671,10.724282188150129,32.088953648,23.944166069247281,23.175815942689891,2.5367427701383081,155.39898302995414,1.0543996780891933E-2,2.60701054511095,-153155.40755152001,3689.5949146101025,3.4127796385887933E-3,0.26053464347203975,-153658.92056635089,6671.9728114760919,8.1325555007463954,3.9644507771488813E-3,0.76707558522214936,-153619.96878678387,6128.90665708897]
["KBM","KBMS-35H03-D (240 V)",20,21.5,13.298799803649256,13.852916462134642,3400,75.7,4166,0.32,2.2999999999999998,57.8,3.7,325,10,3689.5949146101025,4166,4166,11.789058818236118,30.405405405405403,0.49989677864260301,0.39432218546895642,3.0562639095899249E-2,-23.444678320987656,9,29.850189440000001,9,-2427.6928000000003,7.5,2439.6928000000003,9,0.44684509117292204,0.66851986766666671,10.724282188150129,32.088953648,23.944166069247281,23.175815942689891,2.5367427701383081,155.39898302995414,1.0543996780891933E-2,2.60701054511095,-153155.40755152001,3689.5949146101025,3.4201216214621356E-3,0.27350647729833161,-153658.40217182474,6662.9516482848067,8.5374696309092801,3.9644507771488813E-3,0.76707558522214936,-153619.96878678387,6128.90665708897]
["KBM","KBMS-35H04-A (120 V)",25.6,10.86,23.786429676643269,9.7485367527226519,550,92.3,778,1.35,11,147,4.46,160,10,778,778,778,23.034622342597206,25.224215246636771,0.3913419459447795,0.32509404498374861,0.16365546847495663,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.1765761899360633,0.26519134002499994,4.2378285584655195,12.729184321199998,9.4910247784557882,23.20752290289068,2.5634274131287293,157.03366449314512,5.9753067325012302E-2,13.458705545314521,-151568.38295437687,1484.0215552265863,2.2624089883763143E-2,2.1955434754160708,-153608.23144115365,2557.6131313940546,6.3874911390727886,2.3850145706355155E-2,3.2623070738812343,-153540.87251325496,2469.7986417408665]
["KBM","KBMS-35H04-A (240 V)",25.6,10.86,22.612734314496489,9.2675140633182327,1250,92.3,1633,1.35,11,147,4.46,325,10,1484.0215552265863,1633,1633,21.697436108458213,25.224215246636771,0.39103349632601231,0.32509404498374861,7.7969353627382901E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.1765761899360633,0.26519134002499994,4.2378285584655195,12.729184321199998,9.4910247784557882,23.20752290289068,2.5634274131287293,157.03366449314512,5.9753067325012302E-2,13.458705545314521,-151568.38295437687,1484.0215552265863,2.3217427070613264E-2,2.7636973262577511,-153575.63377630658,2513.0710444826059,8.0404202331749151,2.3850145706355155E-2,3.2623070738812343,-153540.87251325496,2469.7986417408665]
["KBM","KBMS-35H04-A (400 V)",25.6,10.86,20.136560191191975,8.252688602947531,2300,92.3,2721,1.35,11,147,4.46,565,10,1484.0215552265863,2504.1080083553388,2666.6666666666665,19.651720270259332,25.224215246636771,0.39102860497554254,0.32509404498374861,5.1552362335000108E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.1765761899360633,0.26519134002499994,4.2378285584655195,12.729184321199998,9.4910247784557882,23.20752290289068,2.5634274131287293,157.03366449314512,5.9753067325012302E-2,13.458705545314521,-151568.38295437687,1484.0215552265863,2.334412569546845E-2,2.8704848699729633,-153568.6730136894,2504.1080083553388,8.351097064165474,2.3850145706355155E-2,3.2623070738812343,-153540.87251325496,2469.7986417408665]
["KBM","KBMS-35H04-A (480 V)",25.6,10.86,18.416500557776462,7.5477461302362556,2800,92.3,3266,1.35,11,147,4.46,679,10,1484.0215552265863,2507.2779194360105,2666.6666666666665,19.167489451511436,25.224215246636771,0.39109317894077655,0.32509404498374861,5.1552362335000108E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.1765761899360633,0.26519134002499994,4.2378285584655195,12.729184321199998,9.4910247784557882,23.20752290289068,2.5634274131287293,157.03366449314512,5.9753067325012302E-2,13.458705545314521,-151568.38295437687,1484.0215552265863,2.3299050716221834E-2,2.832954896368796,-153571.14941176292,2507.2779194360105,8.2419111716835118,2.3850145706355155E-2,3.2623070738812343,-153540.87251325496,2469.7986417408665]
["KBM","KBMS-35H04-B (120 V)",25.9,13.3,23.708598419206478,11.795322596620139,725,93,948,0.9,7.6,122,4.46,160,10,948,948,948,23.034553519183092,25.224215246636771,0.38670490939195945,0.32264710055913975,0.1343079688539201,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.21374411125603807,0.32101206457657655,5.1298586701449134,15.408579099675675,11.488812035839173,23.20752290289068,2.5634274131287293,157.03366449314512,4.1970652956830092E-2,9.0823407759937265,-152278.47000182615,1799.6587277287767,1.5591757137014354E-2,1.468122349044181,-153627.79697608566,3092.2444533172966,7.7196797215297233,1.6451602476508103E-2,2.1849328368821137,-153583.81437278813,2989.7205066301194]
["KBM","KBMS-35H04-B (240 V)",25.9,13.3,22.117403059351133,11.003683114105042,1550,93,1984,0.9,7.6,122,4.46,325,10,1799.6587277287767,1984,1984,21.05827591596945,25.224215246636771,0.38651163793030968,0.32264710055913975,6.4175380278990057E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.21374411125603807,0.32101206457657655,5.1298586701449134,15.408579099675675,11.488812035839173,23.20752290289068,2.5634274131287293,157.03366449314512,4.1970652956830092E-2,9.0823407759937265,-152278.47000182615,1799.6587277287767,1.5914862276834321E-2,1.7718234485654178,-153611.26957919769,3051.6100806818349,9.3166005918555115,1.6451602476508103E-2,2.1849328368821137,-153583.81437278813,2989.7205066301194]
["KBM","KBMS-35H04-B (400 V)",25.9,13.3,18.327948183424581,9.1183821808082506,2850,93,3307,0.9,7.6,122,4.46,565,10,1799.6587277287767,3050.5805694773012,3213.1147540983607,17.795033634133237,25.224215246636771,0.38658347341855309,0.32264710055913975,4.2587243252724713E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.21374411125603807,0.32101206457657655,5.1298586701449134,15.408579099675675,11.488812035839173,23.20752290289068,2.5634274131287293,157.03366449314512,4.1970652956830092E-2,9.0823407759937265,-152278.47000182615,1799.6587277287767,1.5923364894834594E-2,1.7791154996881311,-153610.83465531393,3050.5805694773012,9.3549436490380522,1.6451602476508103E-2,2.1849328368821137,-153583.81437278813,2989.7205066301194]
["KBM","KBMS-35H04-B (480 V)",25.9,13.3,16.149545696089383,8.0345998488006884,3400,93,3968,0.9,7.6,122,4.46,679,10,1799.6587277287767,3056.4254084698982,3213.1147540983607,17.134842271000856,25.224215246636771,0.38665349128940524,0.32264710055913975,4.2587243252724713E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.21374411125603807,0.32101206457657655,5.1298586701449134,15.408579099675675,11.488812035839173,23.20752290289068,2.5634274131287293,157.03366449314512,4.1970652956830092E-2,9.0823407759937265,-152278.47000182615,1799.6587277287767,1.587529290397462E-2,1.7374852237340437,-153613.2936223009,3056.4254084698982,9.1360433664466978,1.6451602476508103E-2,2.1849328368821137,-153583.81437278813,2989.7205066301194]
["KBM","KBMS-35H04-C (120 V)",25.3,14.7,22.977994908892388,13.055678925507038,800,93,1080,0.73,6.1,107,4.46,160,10,1080,1080,1080,22.165293127004723,25.224215246636771,0.39585834218260807,0.32264710055913975,0.11789255043844099,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.24184610383224273,0.36321710406324104,5.8043064919738256,17.43442099503557,12.999302821495579,23.20752290289068,2.5634274131287293,157.03366449314512,3.3788718806741905E-2,7.3104990884043923,-152497.01168395576,2019.0145978646967,1.1985639969863468E-2,1.1330515896012832,-153635.96685508126,3533.3154094680863,8.3749537864810435,1.27418802455496E-2,1.758682029909175,-153596.46216957102,3403.627007129161]
["KBM","KBMS-35H04-C (240 V)",25.3,14.7,21.088029959676135,11.98183520436144,1800,93,2260,0.73,6.1,107,4.46,325,10,2019.0145978646967,2260,2260,20.011637616037813,25.224215246636771,0.39566266946292233,0.32264710055913975,5.6338032952883303E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.24184610383224273,0.36321710406324104,5.8043064919738256,17.43442099503557,12.999302821495579,23.20752290289068,2.5634274131287293,157.03366449314512,3.3788718806741905E-2,7.3104990884043923,-152497.01168395576,2019.0145978646967,1.222223533958201E-2,1.3600786505357374,-153623.60752171275,3490.1025050413737,10.053024900856112,1.27418802455496E-2,1.758682029909175,-153596.46216957102,3403.627007129161]
["KBM","KBMS-35H04-C (400 V)",25.3,14.7,16.14699240823229,9.1744275046774373,3300,93,3766,0.73,6.1,107,4.46,565,10,2019.0145978646967,3503.6277551873309,3663.5514018691588,15.582202593346151,25.224215246636771,0.39581349867330939,0.32264710055913975,3.7408315954370545E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.24184610383224273,0.36321710406324104,5.8043064919738256,17.43442099503557,12.999302821495579,23.20752290289068,2.5634274131287293,157.03366449314512,3.3788718806741905E-2,7.3104990884043923,-152497.01168395576,2019.0145978646967,1.2146403494992009E-2,1.2916660235544664,-153627.56884626593,3503.6277551873309,9.5473527896846075,1.27418802455496E-2,1.758682029909175,-153596.46216957102,3403.627007129161]
["KBM","KBMS-35H04-C (480 V)",25.3,14.7,11.206042017217307,6.3670693279643791,4150,93,4520,0.73,6.1,107,4.46,679,10,2019.0145978646967,3529.7485461682049,3663.5514018691588,13.312499349522174,25.224215246636771,0.39603020941941558,0.32264710055913975,3.7408315954370545E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.24184610383224273,0.36321710406324104,5.8043064919738256,17.43442099503557,12.999302821495579,23.20752290289068,2.5634274131287293,157.03366449314512,3.3788718806741905E-2,7.3104990884043923,-152497.01168395576,2019.0145978646967,1.2004522202082415E-2,1.1528130563516019,-153634.98047989138,3529.7485461682049,8.5210207196250494,1.27418802455496E-2,1.758682029909175,-153596.46216957102,3403.627007129161]
["KBM","KBMS-35H04-D (120 V)",24.7,19.2,21.838826104261813,16.544565230501373,1150,91.5,1443,0.43,3.4,80,4.46,160,10,1443,1443,1443,21.109848755173736,25.224215246636771,0.40534814873623032,0.32793639728961749,8.8235588685735458E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.32355383898634016,0.48593004618623481,7.7652921356721638,23.324642216939271,17.391118837119429,23.20752290289068,2.5634274131287293,157.03366449314512,1.842450150702819E-2,4.2378388639899969,-152962.46569386157,2768.6290962387889,6.6201880446799697E-3,0.57346612150568321,-153651.15377372989,4774.5050867673162,9.6247331285592104,7.1189048069825681E-3,1.03620716906675,-153622.05760557714,4573.1602915009871]
["KBM","KBMS-35H04-D (240 V)",24.7,19.2,18.65932552809381,14.13585267279834,2500,91.5,3015,0.43,3.4,80,4.46,325,10,2768.6290962387889,3015,3015,17.414946586881136,25.224215246636771,0.40532198389404328,0.32793639728961749,4.2230167321232595E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.32355383898634016,0.48593004618623481,7.7652921356721638,23.324642216939271,17.391118837119429,23.20752290289068,2.5634274131287293,157.03366449314512,1.842450150702819E-2,4.2378388639899969,-152962.46569386157,2768.6290962387889,6.6772449572880775E-3,0.64349136977810095,-153647.82495535238,4748.9995667035519,10.799997545424059,7.1189048069825681E-3,1.03620716906675,-153622.05760557714,4573.1602915009871]
["KBM","KBMS-35H04-D (400 V)",24.7,19.2,10.111019914073351,7.6598635712676897,4250,91.5,5025,0.43,3.4,80,4.46,565,10,2768.6290962387889,4807.5046312580234,4900,8.1972730991944829,25.224215246636771,0.40569317798441978,0.32793639728961749,2.7841568271757742E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.32355383898634016,0.48593004618623481,7.7652921356721638,23.324642216939271,17.391118837119429,23.20752290289068,2.5634274131287293,157.03366449314512,1.842450150702819E-2,4.2378388639899969,-152962.46569386157,2768.6290962387889,6.549853424255076E-3,0.47309050801491925,-153655.25724106352,4807.5046312580234,7.9400852370194901,7.1189048069825681E-3,1.03620716906675,-153622.05760557714,4573.1602915009871]
["KBM","KBMS-35H04-E (120 V)",24.7,20.7,22.042959618227506,17.776580337280247,1200,92.1,1536,0.37,2.8,75,4.46,160,10,1536,1536,1536,21.298988311331208,25.224215246636771,0.4052482703748016,0.32580000382193269,8.2893199527028824E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.34883148265714797,0.52389333104453439,8.3719555837715518,25.146879890137651,18.749799996269385,23.20752290289068,2.5634274131287293,157.03366449314512,1.5228744898188632E-2,3.7098524518699181,-153052.3108793491,3050.7437804982533,5.7831473378660656E-3,0.47606611672611726,-153653.92715788912,5113.5420567201427,9.9047531763561665,6.1917190997923749E-3,0.90119807275188968,-153627.90409038524,4908.9049456582607]
["KBM","KBMS-35H04-E (240 V)",24.7,20.7,18.657856405542191,15.046658391566282,2600,92.1,3208,0.37,2.8,75,4.46,325,10,3050.7437804982533,3208,3208,17.244924364992055,25.224215246636771,0.40528828522306498,0.32580000382193269,3.9689511992991353E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.34883148265714797,0.52389333104453439,8.3719555837715518,25.146879890137651,18.749799996269385,23.20752290289068,2.5634274131287293,157.03366449314512,1.5228744898188632E-2,3.7098524518699181,-153052.3108793491,3050.7437804982533,5.8223660705325024E-3,0.53182968768802819,-153651.42920814638,5091.637998738116,11.064937418007846,6.1917190997923749E-3,0.90119807275188968,-153627.90409038524,4908.9049456582607]
["KBM","KBMS-35H04-E (400 V)",24.7,20.7,6.8402026628842849,5.5162924700679721,4600,92.1,5347,0.37,2.8,75,4.46,565,10,3050.7437804982533,5173.5807363495733,5226.666666666667,4.6132383786066811,25.224215246636771,0.40585768229782282,0.32580000382193269,2.5937343640383474E-2,-23.637259693827161,9,30.006180351999998,9,-2443.61024,7.5,2455.61024,9,0.34883148265714797,0.52389333104453439,8.3719555837715518,25.146879890137651,18.749799996269385,23.20752290289068,2.5634274131287293,157.03366449314512,1.5228744898188632E-2,3.7098524518699181,-153052.3108793491,3050.7437804982533,5.6844623195075484E-3,0.29191556518468803,-153660.21268012456,5173.5807363495733,6.0734245095503194,6.1917190997923749E-3,0.90119807275188968,-153627.90409038524,4908.9049456582607]
["KBM","KBMS-45H01-A (120 V)",30.7,10.24,28.329579870357374,9.1979155423238232,450,118,617,1.36,21,187,8.35,160,10,617,617,617,27.449890622245555,13.473053892215569,0.32896156138135541,0.26105599593220341,0.20635973172368924,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.13982263068061571,0.21406024769598264,3.3557431363347772,10.274891889407167,7.6320502080031201,23.372350673615067,2.7000106515928572,165.40065250868835,0.1754392238223442,17.337430403901937,-151515.05026587733,881.21957338010338,3.8456892304321241E-2,2.7319586825711104,-153610.64132343451,1963.3851580952091,6.2020174614555126,4.0250770601715349E-2,3.3618811880415942,-153583.19811030835,1912.0557476152533]
["KBM","KBMS-45H01-A (240 V)",30.7,10.24,27.341143907997175,8.876994775323757,950,118,1293,1.36,21,187,8.35,325,10,881.21957338010338,1293,1293,26.128420076884577,13.473053892215569,0.32854876590008658,0.26105599593220341,9.8471735865055116E-2,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.13982263068061571,0.21406024769598264,3.3557431363347772,10.274891889407167,7.6320502080031201,23.372350673615067,2.7000106515928572,165.40065250868835,0.1754392238223442,17.337430403901937,-151515.05026587733,881.21957338010338,4.0398752061809769E-2,3.4086514346795891,-153580.93425174337,1908.0445814256541,7.738226735553102,4.0250770601715349E-2,3.3618811880415942,-153583.19811030835,1912.0557476152533]
["KBM","KBMS-45H01-A (400 V)",30.7,10.24,24.99187334951591,8.1142445939986718,1750,118,2155,1.36,21,187,8.35,565,10,881.21957338010338,1893.3525871280328,2096.2566844919784,24.524287793515128,13.473053892215569,0.32848359107299013,0.26105599593220341,6.6590084850986567E-2,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.13982263068061571,0.21406024769598264,3.3557431363347772,10.274891889407167,7.6320502080031201,23.372350673615067,2.7000106515928572,165.40065250868835,0.1754392238223442,17.337430403901937,-151515.05026587733,881.21957338010338,4.0950510992111867E-2,3.5776516034744095,-153572.49330123936,1893.3525871280328,8.1218862705750503,4.0250770601715349E-2,3.3618811880415942,-153583.19811030835,1912.0557476152533]
["KBM","KBMS-45H01-A (480 V)",30.7,10.24,23.64587725936731,7.6772328764179578,2100,118,2586,1.36,21,187,8.35,679,10,881.21957338010338,1893.7334450945198,2096.2566844919784,24.338748495362886,13.473053892215569,0.32850674949420072,0.26105599593220341,6.6590084850986567E-2,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.13982263068061571,0.21406024769598264,3.3557431363347772,10.274891889407167,7.6320502080031201,23.372350673615067,2.7000106515928572,165.40065250868835,0.1754392238223442,17.337430403901937,-151515.05026587733,881.21957338010338,4.0936013818488784E-2,3.5733134604023684,-153572.71508274262,1893.7334450945198,8.1120379374890721,4.0250770601715349E-2,3.3618811880415942,-153583.19811030835,1912.0557476152533]
["KBM","KBMS-45H01-B (120 V)",30.2,12.5,27.738432938873189,11.184851991481125,525,118,763,0.92,14,150,8.35,160,10,763,763,763,26.622522537829035,13.473053892215569,0.33428638497723706,0.26105599593220341,0.16687281058127951,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.17350778185691187,0.26563023868653424,4.1641867645658852,12.750251456953643,9.470713690375355,23.372350673615067,2.7000106515928572,165.40065250868835,0.11863570911371593,11.674137148365727,-152149.71690934608,1084.339697934495,2.4482624226236947E-2,1.676496412377797,-153632.77066421427,2471.0255745874833,7.0139540216069776,2.6114764384614828E-2,2.2637185068022196,-153607.06198357735,2382.3291371948376]
["KBM","KBMS-45H01-B (240 V)",30.2,12.5,26.101410667070837,10.52476236575437,1200,118,1596,0.92,14,150,8.35,325,10,1084.339697934495,1596,1596,24.748876187204214,13.473053892215569,0.3339729259123983,0.26105599593220341,7.9776913830523974E-2,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.17350778185691187,0.26563023868653424,4.1641867645658852,12.750251456953643,9.470713690375355,23.372350673615067,2.7000106515928572,165.40065250868835,0.11863570911371593,11.674137148365727,-152149.71690934608,1084.339697934495,2.568878446802977E-2,2.1261554160842771,-153613.77181274063,2404.3299736778872,8.895191317501725,2.6114764384614828E-2,2.2637185068022196,-153607.06198357735,2382.3291371948376]
["KBM","KBMS-45H01-B (400 V)",30.2,12.5,23.09597313705644,9.3128923939743711,2150,118,2660,0.92,14,150,8.35,565,10,1084.339697934495,2390.705568383235,2613.3333333333335,22.300634149217089,13.473053892215569,0.33394555403382792,0.26105599593220341,5.3445156878465003E-2,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.17350778185691187,0.26563023868653424,4.1641867645658852,12.750251456953643,9.470713690375355,23.372350673615067,2.7000106515928572,165.40065250868835,0.11863570911371593,11.674137148365727,-152149.71690934608,1084.339697934495,2.5950927040498811E-2,2.2118227097726146,-153609.64267000594,2390.705568383235,9.2535973687459876,2.6114764384614828E-2,2.2637185068022196,-153607.06198357735,2382.3291371948376]
["KBM","KBMS-45H01-B (480 V)",30.2,12.5,20.720171836492035,8.3549079985854977,2650,118,3192,0.92,14,150,8.35,679,10,1084.339697934495,2397.5487113569716,2613.3333333333335,21.623264227432436,13.473053892215569,0.33401272848184765,0.26105599593220341,5.3445156878465003E-2,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.17350778185691187,0.26563023868653424,4.1641867645658852,12.750251456953643,9.470713690375355,23.372350673615067,2.7000106515928572,165.40065250868835,0.11863570911371593,11.674137148365727,-152149.71690934608,1084.339697934495,2.5818590111406043E-2,2.1689983990431627,-153611.72717716609,2397.5487113569716,9.0744334026046189,2.6114764384614828E-2,2.2637185068022196,-153607.06198357735,2382.3291371948376]
["KBM","KBMS-45H01-C (120 V)",31.3,14.3,28.427521373798537,12.69085775616006,650,119,854,0.69,11,135,8.35,160,10,854,854,854,27.526005004959924,13.473053892215569,0.32243732734666569,0.25886224806722691,0.14909128158491367,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.19151711354051362,0.29320146933972313,4.5964107249723272,14.07367052830671,10.453731410416614,23.372350673615067,2.7000106515928572,165.40065250868835,9.1764589441662964E-2,8.7716672376422391,-152608.55217931513,1242.6816076419614,1.9916763280895779E-2,1.3304279028309061,-153639.71963779654,2744.2263174994464,8.246085967115544,2.0943858171524631E-2,1.6866105947211096,-153624.97866531927,2668.3704487829532]
["KBM","KBMS-45H01-C (240 V)",31.3,14.3,26.601611916788226,11.875719605709028,1400,119,1783,0.69,11,135,8.35,325,10,1242.6816076419614,1783,1783,25.316267176881006,13.473053892215569,0.32219375301678277,0.25886224806722691,7.1409957640783103E-2,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.19151711354051362,0.29320146933972313,4.5964107249723272,14.07367052830671,10.453731410416614,23.372350673615067,2.7000106515928572,165.40065250868835,9.1764589441662964E-2,8.7716672376422391,-152608.55217931513,1242.6816076419614,2.0745623510874483E-2,1.6239607888176342,-153627.82374974462,2682.4119892465224,10.065423495193325,2.0943858171524631E-2,1.6866105947211096,-153624.97866531927,2668.3704487829532]
["KBM","KBMS-45H01-C (400 V)",31.3,14.3,22.23076245107594,9.9244475228017581,2500,119,2972,0.69,11,135,8.35,565,10,1242.6816076419614,2684.038231512895,2903.7037037037039,21.563127875206209,13.473053892215569,0.32225596368535603,0.25886224806722691,4.7715996304631865E-2,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.19151711354051362,0.29320146933972313,4.5964107249723272,14.07367052830671,10.453731410416614,23.372350673615067,2.7000106515928572,165.40065250868835,9.1764589441662964E-2,8.7716672376422391,-152608.55217931513,1242.6816076419614,2.0722903504055458E-2,1.6166253181219135,-153628.14982964069,2684.038231512895,10.019957730504039,2.0943858171524631E-2,1.6866105947211096,-153624.97866531927,2668.3704487829532]
["KBM","KBMS-45H01-C (480 V)",31.3,14.3,18.621128341751753,8.3130037239963173,3100,119,3567,0.69,11,135,8.35,679,10,1242.6816076419614,2699.6715471470766,2903.7037037037039,20.258455140096043,13.473053892215569,0.32236186120851401,0.25886224806722691,4.7715996304631865E-2,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.19151711354051362,0.29320146933972313,4.5964107249723272,14.07367052830671,10.453731410416614,23.372350673615067,2.7000106515928572,165.40065250868835,9.1764589441662964E-2,8.7716672376422391,-152608.55217931513,1242.6816076419614,2.0507013043603577E-2,1.5451854451049976,-153631.24831193738,2699.6715471470766,9.5771683594123687,2.0943858171524631E-2,1.6866105947211096,-153624.97866531927,2668.3704487829532]
["KBM","KBMS-45H01-D (120 V)",29.7,20.2,26.335954793732576,17.326286048508273,950,118,1263,0.35,5,91.2,8.35,160,10,1263,1263,1263,25.227590425772888,13.473053892215569,0.33964169763762075,0.26105599593220341,0.10081073196636284,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.28510892186933473,0.43648503921436593,6.8426141248640331,20.951281882289564,15.562327756704596,23.372350673615067,2.7000106515928572,165.40065250868835,4.1426920880529877E-2,4.4371124731678089,-153072.23236778559,1869.4291339814943,8.7484891262132672E-3,0.50627634514378839,-153656.29583448597,4162.0778734294272,9.1572300799845276,9.5623777383637525E-3,0.86039537608816374,-153641.74915709661,3963.6696136917517]
["KBM","KBMS-45H01-D (240 V)",29.7,20.2,22.804629703024432,15.003045857252916,2100,118,2635,0.35,5,91.2,8.35,325,10,1869.4291339814943,2635,2635,21.047952032128276,13.473053892215569,0.33957618280117863,0.26105599593220341,4.8320286327710162E-2,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.28510892186933473,0.43648503921436593,6.8426141248640331,20.951281882289564,15.562327756704596,23.372350673615067,2.7000106515928572,165.40065250868835,4.1426920880529877E-2,4.4371124731678089,-153072.23236778559,1869.4291339814943,8.9583270142866486E-3,0.61732659570674109,-153652.5453899948,4107.1760183923088,11.16584198650383,9.5623777383637525E-3,0.86039537608816374,-153641.74915709661,3963.6696136917517]
["KBM","KBMS-45H01-D (400 V)",29.7,20.2,12.723792477454767,8.3709161035886623,3700,118,4392,0.35,5,91.2,8.35,565,10,1869.4291339814943,4177.6347928738414,4298.2456140350869,10.532325622369839,13.473053892215569,0.33990826529386042,0.26105599593220341,3.2122746566388784E-2,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.28510892186933473,0.43648503921436593,6.8426141248640331,20.951281882289564,15.562327756704596,23.372350673615067,2.7000106515928572,165.40065250868835,4.1426920880529877E-2,4.4371124731678089,-153072.23236778559,1869.4291339814943,8.6913752066192663E-3,0.47154422455342859,-153657.31663481463,4177.6347928738414,8.5290158201984756,9.5623777383637525E-3,0.86039537608816374,-153641.74915709661,3963.6696136917517]
["KBM","KBMS-45H01-E (120 V)",31.2,23.4,27.345712949425653,19.960374415639162,1100,118,1394,0.26,3.2,82.7,8.35,160,10,1394,1394,1394,26.315567137726692,13.473053892215569,0.32326297583937835,0.26105599593220341,9.1337126595061879E-2,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.31439610072472429,0.48132199250000002,7.5455064173933826,23.10345564,17.160933206960138,23.372350673615067,2.7000106515928572,165.40065250868835,2.3330214601692188E-2,3.2959662470946212,-153266.90492500001,2493.4316135688764,7.083716855870106E-3,0.4012681717532543,-153658.11429601384,4629.2015980656179,10.774452933632702,7.4593593526799049E-3,0.63911702394108327,-153649.06897023335,4495.8816992510792]
["KBM","KBMS-45H01-E (240 V)",31.2,23.4,23.167423890072417,16.910528386914173,2300,118,2909,0.26,3.2,82.7,8.35,325,10,2493.4316135688764,2909,2909,21.04053743313942,13.473053892215569,0.32326033200667903,0.26105599593220341,4.3768977130806554E-2,-24.622972246913577,9,30.804607520000001,9,-2525.0823999999998,7.5,2537.0823999999998,9,0.31439610072472429,0.48132199250000002,7.5455064173933826,23.10345564,17.160933206960138,23.372350673615067,2.7000106515928572,165.40065250868835,2.3330214601692188E-2,3.2959662470946212,-153266.90492500001,2493.4316135688764,7.1428710734378099E-3,0.44719567913717512,-153656.6898853741,4606.8937016335212,12.00765257791301,7.4593593526799049E-3,0.63911702394108327,-153649.06897023335,4495.8816992510792]
["KBM","KBMS-45H02-A (120 V)",43.7,13.3,40.226411866476546,12.00788413924673,400,171,568,0.95,16,202,11.5,160,10,568,568,568,38.767504850396691,9.7826086956521738,0.23259178300342079,0.18392484678362575,0.22416189167872583,-25.42117135802469,9,31.451148800000002,9,-2591.056,7.5,2603.056,9,0.12832634888051223,0.199418515942029,3.0798323731322936,9.5720887652173925,7.0891268117011697,23.508890873334074,2.8106114745136814,172.17597699428256,0.18337496924834726,17.298239926827986,-151830.66806828923,863.9889508548714,4.4227732883788937E-2,2.6806264745974939,-153619.97393456331,1833.6436985481287,8.0649318223329907,4.3449355013079061E-2,2.3562878684977999,-153629.98316023411,1853.4631912555126]
["KBM","KBMS-45H02-A (240 V)",43.7,13.3,38.46847317687061,11.483126321453913,880,171,1188,0.95,16,202,11.5,325,10,863.9889508548714,1188,1188,36.63743878877532,9.7826086956521738,0.23226736508397766,0.18392484678362575,0.10717504585312818,-25.42117135802469,9,31.451148800000002,9,-2591.056,7.5,2603.056,9,0.12832634888051223,0.199418515942029,3.0798323731322936,9.5720887652173925,7.0891268117011697,23.508890873334074,2.8106114745136814,172.17597699428256,0.18337496924834726,17.298239926827986,-151830.66806828923,863.9889508548714,4.6019497755223432E-2,3.3085236760941479,-153596.93348130528,1791.3300259637037,9.9540231110641315,4.3449355013079061E-2,2.3562878684977999,-153629.98316023411,1853.4631912555126]
["KBM","KBMS-45H02-A (400 V)",43.7,13.3,34.85493253712508,10.40445747376868,1600,171,1980,0.95,16,202,11.5,565,10,863.9889508548714,1781.4762894002708,1940.5940594059405,33.851701272964078,9.7826086956521738,0.2322180838849468,0.18392484678362575,6.8695162156022435E-2,-25.42117135802469,9,31.451148800000002,9,-2591.056,7.5,2603.056,9,0.12832634888051223,0.199418515942029,3.0798323731322936,9.5720887652173925,7.0891268117011697,23.508890873334074,2.8106114745136814,172.17597699428256,0.18337496924834726,17.298239926827986,-151830.66806828923,863.9889508548714,4.6461397291574134E-2,3.4458367982177625,-153591.25105847497,1781.4762894002708,10.367143319617215,4.3449355013079061E-2,2.3562878684977999,-153629.98316023411,1853.4631912555126]
["KBM","KBMS-45H02-A (480 V)",43.7,13.3,32.565549894187811,9.7210596699068095,1950,171,2376,0.95,16,202,11.5,679,10,863.9889508548714,1782.4761066244373,1940.5940594059405,33.522107038968123,9.7826086956521738,0.23223958025999186,0.18392484678362575,6.8695162156022435E-2,-25.42117135802469,9,31.451148800000002,9,-2591.056,7.5,2603.056,9,0.12832634888051223,0.199418515942029,3.0798323731322936,9.5720887652173925,7.0891268117011697,23.508890873334074,2.8106114745136814,172.17597699428256,0.18337496924834726,17.298239926827986,-151830.66806828923,863.9889508548714,4.6416137330960366E-2,3.4320255343126402,-153591.83306006656,1782.4761066244373,10.325590756128568,4.3449355013079061E-2,2.3562878684977999,-153629.98316023411,1853.4631912555126]
["KBM","KBMS-45H02-B (120 V)",43.5,14.9,39.894839068368434,13.387529888714239,450,171,638,0.76,12,180,11.5,160,10,638,638,638,38.388682945820136,9.7826086956521738,0.23358545379632331,0.18392484678362575,0.19956732676099728,-25.42117135802469,9,31.451148800000002,9,-2591.056,7.5,2603.056,9,0.14442508952824809,0.22443587984674329,3.466202148677954,10.772922232643678,7.9784688288012831,23.508890873334074,2.8106114745136814,172.17597699428256,0.13397977436369921,13.878414256467329,-152177.80877874911,1015.2165380078853,3.4673565661469549E-2,2.076299385125898,-153630.73596345159,2075.2126579468704,8.7628070827535929,3.4284777572581214E-2,1.89045471012249,-153636.42423602604,2089.4905544026074]
["KBM","KBMS-45H02-B (240 V)",43.5,14.9,37.515093728803905,12.588957627115404,1050,171,1334,0.76,12,180,11.5,325,10,1015.2165380078853,1334,1334,35.896319080213722,9.7826086956521738,0.23330926609379418,0.18392484678362575,9.5445243233520438E-2,-25.42117135802469,9,31.451148800000002,9,-2591.056,7.5,2603.056,9,0.14442508952824809,0.22443587984674329,3.466202148677954,10.772922232643678,7.9784688288012831,23.508890873334074,2.8106114745136814,172.17597699428256,0.13397977436369921,13.878414256467329,-152177.80877874911,1015.2165380078853,3.5905593124238293E-2,2.5782022251605698,-153612.71044202297,2032.799501673029,10.881036174866573,3.4284777572581214E-2,1.89045471012249,-153636.42423602604,2089.4905544026074]
["KBM","KBMS-45H02-B (400 V)",43.5,14.9,32.769165125026028,10.996364135914774,1900,171,2223,0.76,12,180,11.5,565,10,1015.2165380078853,2027.0852984448106,2177.7777777777774,32.051411781527051,9.7826086956521738,0.23330304830302759,0.18392484678362575,6.0935405620878069E-2,-25.42117135802469,9,31.451148800000002,9,-2591.056,7.5,2603.056,9,0.14442508952824809,0.22443587984674329,3.466202148677954,10.772922232643678,7.9784688288012831,23.508890873334074,2.8106114745136814,172.17597699428256,0.13397977436369921,13.878414256467329,-152177.80877874911,1015.2165380078853,3.6080015771448933E-2,2.6415635583491195,-153610.15850283334,2027.0852984448106,11.14844613665475,3.4284777572581214E-2,1.89045471012249,-153636.42423602604,2089.4905544026074]
["KBM","KBMS-45H02-B (480 V)",43.5,14.9,29.257419325829272,9.8179259482648558,2350,171,2667,0.76,12,180,11.5,679,10,1015.2165380078853,2031.3080686626404,2177.7777777777774,31.188906790629112,9.7826086956521738,0.23335232733475109,0.18392484678362575,6.0935405620878069E-2,-25.42117135802469,9,31.451148800000002,9,-2591.056,7.5,2603.056,9,0.14442508952824809,0.22443587984674329,3.466202148677954,10.772922232643678,7.9784688288012831,23.508890873334074,2.8106114745136814,172.17597699428256,0.13397977436369921,13.878414256467329,-152177.80877874911,1015.2165380078853,3.5950928388171356E-2,2.5948196713502698,-153612.04715179917,2031.3080686626404,10.951168390004492,3.4284777572581214E-2,1.89045471012249,-153636.42423602604,2089.4905544026074]
["KBM","KBMS-45H02-C (120 V)",41.8,21.1,37.242256683503506,18.345939252957393,750,168,941,0.38,5.9,123,11.5,160,10,941,941,941,36.081551385569064,9.7826086956521738,0.24287547058698955,0.18720921904761906,0.13530707170405554,-25.42117135802469,9,31.451148800000002,9,-2591.056,7.5,2603.056,9,0.21283929293134859,0.33075121594896334,5.1081430303523661,15.876058365550241,11.757871639503,23.508890873334074,2.8106114745136814,172.17597699428256,6.6603654677383994E-2,6.8653833220766289,-152885.14005950413,1464.4104450032271,1.6025061124486862E-2,0.90580953448853596,-153650.44175238334,3068.3379969812563,11.188904120057463,1.611850948309964E-2,0.95187090014133335,-153649.02779082331,3058.0819545543413]
["KBM","KBMS-45H02-C (240 V)",41.8,21.1,33.243488738319641,16.376102826758444,1600,168,1964,0.38,5.9,123,11.5,325,10,1464.4104450032271,1964,1964,31.296882426287361,9.7826086956521738,0.24278120564715608,0.18720921904761906,6.4828897389774071E-2,-25.42117135802469,9,31.451148800000002,9,-2591.056,7.5,2603.056,9,0.21283929293134859,0.33075121594896334,5.1081430303523661,15.876058365550241,11.757871639503,23.508890873334074,2.8106114745136814,172.17597699428256,6.6603654677383994E-2,6.8653833220766289,-152885.14005950413,1464.4104450032271,1.6363170222055044E-2,1.0630546746116374,-153645.32584372375,3031.951415207378,13.131255938175414,1.611850948309964E-2,0.95187090014133335,-153649.02779082331,3058.0819545543413]
["KBM","KBMS-45H02-C (400 V)",41.8,21.1,22.654882933908411,11.160040854142075,2900,168,3274,0.38,5.9,123,11.5,565,10,1464.4104450032271,3056.4104002292602,3186.9918699186992,21.622298305376194,9.7826086956521738,0.24294335690755614,0.18720921904761906,4.163523292235357E-2,-25.42117135802469,9,31.451148800000002,9,-2591.056,7.5,2603.056,9,0.21283929293134859,0.33075121594896334,5.1081430303523661,15.876058365550241,11.757871639503,23.508890873334074,2.8106114745136814,172.17597699428256,6.6603654677383994E-2,6.8653833220766289,-152885.14005950413,1464.4104450032271,1.6133880593906788E-2,0.95923562451027045,-153648.79521145928,3056.4104002292602,11.848843517913638,1.611850948309964E-2,0.95187090014133335,-153649.02779082331,3058.0819545543413]
["KBM","KBMS-45H02-C (480 V)",41.8,21.1,12.34587629984274,6.0817124629767196,3500,168,3929,0.38,5.9,123,11.5,679,10,1464.4104450032271,3096.3833606721769,3186.9918699186992,15.74249756332944,9.7826086956521738,0.24317827522066748,0.18720921904761906,4.163523292235357E-2,-25.42117135802469,9,31.451148800000002,9,-2591.056,7.5,2603.056,9,0.21283929293134859,0.33075121594896334,5.1081430303523661,15.876058365550241,11.757871639503,23.508890873334074,2.8106114745136814,172.17597699428256,6.6603654677383994E-2,6.8653833220766289,-152885.14005950413,1464.4104450032271,1.5777495396456218E-2,0.77058671684522706,-153654.18765469996,3096.3833606721769,9.5185804108802277,1.611850948309964E-2,0.95187090014133335,-153649.02779082331,3058.0819545543413]
["KBM","KBMS-45H03-A (120 V)",54.6,14.1,50.202016335272141,12.67727685234145,350,218,480,0.93,16,240,14.5,160,10,480,480,480,48.568479545516077,7.7586206896551726,0.18733937236507689,0.14709588256880735,0.26525823848649221,-26.181360987654323,9,32.066902400000004,9,-2653.8879999999999,7.5,2665.8879999999999,9,0.10949991726766095,0.17252110952380953,2.6279980144238628,8.2810132571428579,6.1164163147819854,23.641434624372383,2.9159455915811323,178.62866698056268,0.22442625491965246,21.763953091181758,-151608.14212606268,774.85134692641111,6.1460082687145083E-2,3.3105784588722567,-153616.43086053667,1554.2616738179361,8.5634559337064236,5.9569212343868909E-2,2.3645682600538565,-153639.73271242858,1586.2580259294346]
["KBM","KBMS-45H03-A (240 V)",54.6,14.1,47.7464829275686,12.05719265847692,800,218,1005,0.93,16,240,14.5,325,10,774.85134692641111,1005,1005,45.990269177758051,7.7586206896551726,0.18703391116530813,0.14709588256880735,0.12669050196369777,-26.181360987654323,9,32.066902400000004,9,-2653.8879999999999,7.5,2665.8879999999999,9,0.10949991726766095,0.17252110952380953,2.6279980144238628,8.2810132571428579,6.1164163147819854,23.641434624372383,2.9159455915811323,178.62866698056268,0.22442625491965246,21.763953091181758,-151608.14212606268,774.85134692641111,6.3539020590363843E-2,4.1064165014054721,-153590.81138679245,1522.7780632806696,10.622046023705963,5.9569212343868909E-2,2.3645682600538565,-153639.73271242858,1586.2580259294346]
["KBM","KBMS-45H03-A (400 V)",54.6,14.1,43.688031878725276,11.032331282506384,1400,218,1676,0.93,16,240,14.5,565,10,774.85134692641111,1514.7039861644841,1633.3333333333333,42.793998849860998,7.7586206896551726,0.18697500544651707,0.14709588256880735,8.026686225837279E-2,-26.181360987654323,9,32.066902400000004,9,-2653.8879999999999,7.5,2665.8879999999999,9,0.10949991726766095,0.17252110952380953,2.6279980144238628,8.2810132571428579,6.1164163147819854,23.641434624372383,2.9159455915811323,178.62866698056268,0.22442625491965246,21.763953091181758,-151608.14212606268,774.85134692641111,6.4103678014459833E-2,4.2971953484070902,-153583.85291726401,1514.7039861644841,11.115532666501977,5.9569212343868909E-2,2.3645682600538565,-153639.73271242858,1586.2580259294346]
["KBM","KBMS-45H03-A (480 V)",54.6,14.1,40.837285986285153,10.312445956132615,1700,218,2011,0.93,16,240,14.5,679,10,774.85134692641111,1515.53208788746,1633.3333333333333,42.330685468115725,7.7586206896551726,0.18699798372785728,0.14709588256880735,8.026686225837279E-2,-26.181360987654323,9,32.066902400000004,9,-2653.8879999999999,7.5,2665.8879999999999,9,0.10949991726766095,0.17252110952380953,2.6279980144238628,8.2810132571428579,6.1164163147819854,23.641434624372383,2.9159455915811323,178.62866698056268,0.22442625491965246,21.763953091181758,-151608.14212606268,774.85134692641111,6.4045186990435682E-2,4.2778282274938686,-153584.57372246552,1515.53208788746,11.065435836427261,5.9569212343868909E-2,2.3645682600538565,-153639.73271242858,1586.2580259294346]
["KBM","KBMS-45H03-B (120 V)",53,19.899999999999999,49.482718670389282,18.125537974501569,550,216,699,0.47,7.7,165,14.5,160,10,699,699,699,48.529855182912925,7.7586206896551726,0.19252487729980003,0.14845788148148151,0.18215158007656118,-26.181360987654323,9,32.066902400000004,9,-2653.8879999999999,7.5,2665.8879999999999,9,0.15920786847049956,0.25083779786163524,3.8209888432919894,12.04021429735849,8.8929894054104341,23.641434624372383,2.9159455915811323,178.62866698056268,0.10741161384298485,10.893649239278348,-152574.27002985831,1142.2004448178975,2.9425390557169421E-2,1.8045641969638115,-153634.09686004624,2254.5238478256624,13.434759830909318,2.8189129803676993E-2,1.1945111402781194,-153650.89754945593,2313.5852169281093]
["KBM","KBMS-45H03-B (240 V)",53,19.899999999999999,45.50447416401321,16.668305554583593,1150,216,1459,0.47,7.7,165,14.5,325,10,1142.2004448178975,1459,1459,43.490458961126322,7.7586206896551726,0.1925348003409118,0.14845788148148151,8.7267960571292852E-2,-26.181360987654323,9,32.066902400000004,9,-2653.8879999999999,7.5,2665.8879999999999,9,0.15920786847049956,0.25083779786163524,3.8209888432919894,12.04021429735849,8.8929894054104341,23.641434624372383,2.9159455915811323,178.62866698056268,0.10741161384298485,10.893649239278348,-152574.27002985831,1142.2004448178975,2.9707019996305706E-2,1.9165717762077612,-153630.26953743474,2242.0671849388332,14.268642564987623,2.8189129803676993E-2,1.1945111402781194,-153650.89754945593,2313.5852169281093]
["KBM","KBMS-45H03-B (400 V)",53,19.899999999999999,33.533576381687716,12.283361311973522,2150,216,2432,0.47,7.7,165,14.5,565,10,1142.2004448178975,2263.6843197462658,2375.757575757576,32.504261438924701,7.7586206896551726,0.19273999313712803,0.14845788148148151,5.5033181203747568E-2,-26.181360987654323,9,32.066902400000004,9,-2653.8879999999999,7.5,2665.8879999999999,9,0.15920786847049956,0.25083779786163524,3.8209888432919894,12.04021429735849,8.8929894054104341,23.641434624372383,2.9159455915811323,178.62866698056268,0.10741161384298485,10.893649239278348,-152574.27002985831,1142.2004448178975,2.9222645771087748E-2,1.719418877108154,-153636.85214623547,2263.6843197462658,12.800863333953796,2.8189129803676993E-2,1.1945111402781194,-153650.89754945593,2313.5852169281093]
["KBM","KBMS-45H03-B (480 V)",53,19.899999999999999,24.699622899069141,9.0474809154099418,2600,216,2918,0.47,7.7,165,14.5,679,10,1142.2004448178975,2281.1243314531234,2375.757575757576,28.170508156064543,7.7586206896551726,0.19288836575292453,0.14845788148148151,5.5033181203747568E-2,-26.181360987654323,9,32.066902400000004,9,-2653.8879999999999,7.5,2665.8879999999999,9,0.15920786847049956,0.25083779786163524,3.8209888432919894,12.04021429735849,8.8929894054104341,23.641434624372383,2.9159455915811323,178.62866698056268,0.10741161384298485,10.893649239278348,-152574.27002985831,1142.2004448178975,2.8847242961019343E-2,1.5494601081834931,-153641.95384181035,2281.1243314531234,11.535541077476807,2.8189129803676993E-2,1.1945111402781194,-153650.89754945593,2313.5852169281093]
["KBM","KBMS-43H01-A (400 V)",6.12,5.12,4.82490774847009,3.9875270648513141,4750,18,5478,2.9,6.8,72.8,2.85,565,16,3505.2149373042757,5061.9311014268451,5384.6153846153848,4.73985942163449,39.473684210526315,1.6292075962841546,1.6486514400000001,4.1198050302491643E-2,-23.229291259259259,9,29.675725920000001,9,-2409.8903999999998,7.5,2421.8903999999998,9,0.34722075342199016,0.51722398117647062,8.3332980821277634,24.826751096470588,18.541239992658745,23.140548154174382,2.5068981036358635,153.57072086717474,1.0819322829054226E-2,5.5065685307322925,-152233.65979238754,3505.2149373042757,5.700088493422531E-3,1.4828482471209443,-153560.27805160204,5061.9311014268451,4.0551479473410481,1.3667303939535604E-2,6.7799857316156427,-151495.62291121468,3090.5334970624995]
["KBM","KBMS-43H02-A (400 V)",11.6,5.12,9.9780405138429078,4.3194980579406526,2450,34.5,2866,3.55,12,139,3.73,565,16,1857.4406026742151,2630.4569208447001,2820.1438848920861,9.8585736507381068,30.160857908847184,0.86114327999398144,0.86540136162318848,5.6799728281920314E-2,-23.452280217283953,9,29.856346976000001,9,-2428.3211200000001,7.5,2440.3211200000001,9,0.18347795622773169,0.27454112161839078,4.4034709494655608,13.177973837682758,9.83285533319963,23.177064434467763,2.5377961113089835,155.46350992981701,3.6897123643143917E-2,13.014720551425221,-151472.30506920334,1857.4406026742151,2.0764225009738554E-2,3.7294116319948825,-153484.0337570408,2630.4569208447001,4.3635156746401194,2.6649587283080464E-2,8.4039494274034059,-152750.14504970817,2241.6296402256598]
["KBM","KBMS-43H02-A (480 V)",11.6,5.12,6.8754935415698784,2.9764041305497306,3000,34.5,3439,3.55,12,139,3.73,679,16,1857.4406026742151,2682.7115802976487,2820.1438848920861,7.3751706042594938,30.160857908847184,0.86265123053760218,0.86540136162318848,5.6799728281920314E-2,-23.452280217283953,9,29.856346976000001,9,-2428.3211200000001,7.5,2440.3211200000001,9,0.18347795622773169,0.27454112161839078,4.4034709494655608,13.177973837682758,9.83285533319963,23.177064434467763,2.5377961113089835,155.46350992981701,3.6897123643143917E-2,13.014720551425221,-151472.30506920334,1857.4406026742151,2.0231400278668727E-2,2.962030246405813,-153550.47555534623,2682.7115802976487,3.4656580405516459,2.6649587283080464E-2,8.4039494274034059,-152750.14504970817,2241.6296402256598]
["KBM","KBMS-43H03-A (400 V)",21,4.78,18.636530433018713,4.2068917456024186,1240,64.5,1491,4.83,19,268,5.69,565,16,1016.1125416515356,1366.0453605652117,1462.686567164179,18.396284970313019,19.77152899824253,0.47772207186280535,0.46912619113178294,9.5066588970505378E-2,-23.948937441975307,9,30.258639328000001,9,-2469.3713600000001,7.5,2481.3713600000001,9,9.4954719648281172E-2,0.14348838887682544,2.2789132715587481,6.8874426660876207,5.1290925343150242,23.259183233679568,2.6066144011263832,159.67926738751993,0.11278233636413708,32.916289147443393,-149892.69064923251,1016.1125416515356,7.5229627786043307E-2,9.4915754593880362,-153350.42095712695,1366.0453605652117,4.2334628461043602,7.68230415192694E-2,11.499609326306761,-153203.70464379009,1339.313378678379]
["KBM","KBMS-43H03-A (480 V)",21,4.78,16.182532804310163,3.652941942282204,1490,64.5,1790,4.83,19,268,5.69,679,16,1016.1125416515356,1375.958854137958,1462.686567164179,16.551250575551283,19.77152899824253,0.47839419530451438,0.46912619113178294,9.5066588970505378E-2,-23.948937441975307,9,30.258639328000001,9,-2469.3713600000001,7.5,2481.3713600000001,9,9.4954719648281172E-2,0.14348838887682544,2.2789132715587481,6.8874426660876207,5.1290925343150242,23.259183233679568,2.6066144011263832,159.67926738751993,0.11278233636413708,32.916289147443393,-149892.69064923251,1016.1125416515356,7.4692842395100545E-2,8.7115023800268521,-153399.84639633962,1375.958854137958,3.8855321561096443,7.68230415192694E-2,11.499609326306761,-153203.70464379009,1339.313378678379]
["KBM","KBMS-43S01-A (240 V)",6.12,5.12,4.9618894022767375,4.1007350432039154,2550,18,3284,2.9,6.8,72.8,2.85,325,16,{"$f":"IF(AQ1147<I1147,IF(AQ1147<0,0,AQ1147),I1147)","v":3284},{"$f":"IF(AU1147<I1147,IF(AU1147<0,0,AU1147),I1147)","v":3284},{"$f":"IF(UAC_V*0.98/L1147*1000<I1147,IF(UAC_V*0.98/L1147*1000<0,0,UAC_V*0.98/L1147*1000),I1147)","v":3284},{"$f":"C1147+(E1147-C1147)/G1147*Q1147","v":4.6285352145399239},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M1147,(inertia/gear^2+gear_inertia)/M1147),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M1147,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M1147))","v":39.473684210526315},{"$f":"IF((C1147+(E1147-C1147)/G1147*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X1147^2*time1+Y1147^2*time2+Z1147^2*time3+AA1147^2*time4)/time)/(C1147+(E1147-C1147)/G1147*mspeed),SQRT((((X1147-Y1147)*2/PI()+Y1147)^2*time1+Y1147^2*time2+((Z1147-Y1147)*2/PI()+Y1147)^2*time3+AA1147^2*time4)/time)/(C1147+(E1147-C1147)/G1147*mspeed)),IF(AccType=1,SQRT((X1147^2*time1+Y1147^2*time2+Z1147^2*time3+AA1147^2*time4+AB1147^2*time5+AC1147^2*time6+AD1147^2*time7+AE1147^2*time8)/time)/(C1147+(E1147-C1147)/G1147*mspeed),SQRT((((X1147-Y1147)*2/PI()+Y1147)^2*time1+Y1147^2*time2+((Z1147-Y1147)*2/PI()+Y1147)^2*time3+AA1147^2*time4+((AB1147-AC1147)*2/PI()+AC1147)^2*time5+AC1147^2*time6+((AD1147-AC1147)*2/PI()+AC1147)^2*time7+AE1147^2*time8)/time)/(C1147+(E1147-C1147)/G1147*mspeed))))","v":1.6302813875210758},{"$f":"IF(move1,MAX(ABS(X1147),ABS(Z1147))/H1147,MAX(ABS(X1147),ABS(Z1147),ABS(AB1147),ABS(AD1147))/H1147)","v":1.6486514400000001},{"$f":"IF(AZ1147>0,speed/(MIN(AZ1147,I1147)),\"NA\")","v":4.1198050302491643E-2},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M1147+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M1147+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-23.229291259259259},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M1147+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M1147+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":29.675725920000001},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M1147+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M1147+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-2409.8903999999998},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M1147+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M1147+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":2421.8903999999998},9,{"$f":"AH1147/Irms","v":0.34722075342199016},{"$f":"AI1147/Ipeak","v":0.51722398117647062},{"$f":"IF(move1,IF(AccType=1,SQRT((X1147^2*time1+Y1147^2*time2+Z1147^2*time3+AA1147^2*time4)/time)/(C1147/D1147),SQRT((((X1147-Y1147)*2/PI()+Y1147)^2*time1+Y1147^2*time2+((Z1147-AA1147)*2/PI()+AA1147)^2*time3+AA1147^2*time4)/time)/(C1147/D1147)),IF(AccType=1,SQRT((X1147^2*time1+Y1147^2*time2+Z1147^2*time3+AA1147^2*time4+AB1147^2*time5+AC1147^2*time6+AD1147^2*time7+AE1147^2*time8)/time)/(C1147/D1147),SQRT((((X1147-Y1147)*2/PI()+Y1147)^2*time1+Y1147^2*time2+((Z1147-AA1147)*2/PI()+AA1147)^2*time3+AA1147^2*time4+((AB1147-AC1147)*2/PI()+AC1147)^2*time5+AC1147^2*time6+((AD1147-AE1147)*2/PI()+AE1147)^2*time7+AE1147^2*time8)/time)/(C1147/D1147)))","v":8.3332980821277634},{"$f":"IF(move1,MAX(ABS(X1147),ABS(Z1147))/(C1147/D1147),MAX(ABS(X1147),ABS(Z1147),ABS(AB1147),ABS(AD1147))/(C1147/D1147))","v":24.826751096470588},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X1147),ABS(Z1147))/(C1147/D1147),MAX(ABS((X1147-Y1147)*2/PI()+Y1147),ABS((Z1147-Y1147)*2/PI()+Y1147))/(C1147/D1147)),IF(AccType=1,MAX(ABS(X1147),ABS(Z1147),ABS(AB1147),ABS(AD1147))/(C1147/D1147),MAX(ABS((X1147-Y1147)*2/PI()+Y1147),ABS((Z1147-Y1147)*2/PI()+Y1147),ABS((AB1147-AC1147)*2/PI()+AC1147),ABS((AD1147-AC1147)*2/PI()+AC1147))/(C1147/D1147)))","v":18.541239992658745},{"$f":"IF((C1147+(E1147-C1147)/G1147*mspeed)<0,\"NA\",U1147*(C1147+(E1147-C1147)/G1147*mspeed)*mspeed/9.55)","v":23.140548154174382},{"$f":"IF(move1,IF(speed1>speed2,AM1147/2*time1/time,AM1147/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z1147*-speed/30*PI(),((Z1147-AA1147)*2/PI()+AA1147)*-speed/30*PI()),IF(AccType=1,X1147*-speed/30*PI(),((X1147-Y1147)*2/PI()+Y1147)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z1147*-speed/30*PI(),((Z1147-AA1147)*2/PI()+AA1147)*-speed/30*PI()),IF(AccType=1,X1147*-speed/30*PI(),((X1147-Y1147)*2/PI()+Y1147)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD1147*-speed/30*PI(),((AD1147-AE1147)*2/PI()+AE1147)*-speed/30*PI()),IF(AccType=1,AB1147*-speed/30*PI(),((AB1147-AC1147)*2/PI()+AC1147)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD1147*-speed/30*PI(),((AD1147-AE1147)*2/PI()+AE1147)*-speed/30*PI()),IF(AccType=1,AB1147*-speed/30*PI(),((AB1147-AC1147)*2/PI()+AC1147)*-speed/30*PI()),0)/2*time7/time)))","v":2.5068981036358635},{"$f":"IF(move1,MAX(IF(AccType=1,Z1147*-speed/30*PI(),((Z1147-AA1147)*2/PI()+AA1147)*-speed/30*PI()),IF(AccType=1,X1147*-speed/30*PI(),((X1147-Y1147)*2/PI()+Y1147)*-speed/30*PI()),0),MAX(IF(AccType=1,Z1147*-speed/30*PI(),((Z1147-AA1147)*2/PI()+AA1147)*-speed/30*PI()),IF(AccType=1,X1147*-speed/30*PI(),((X1147-Y1147)*2/PI()+Y1147)*-speed/30*PI()),IF(AccType=1,AD1147*-speed/30*PI(),((AD1147-AE1147)*2/PI()+AE1147)*-speed/30*PI()),IF(AccType=1,AB1147*-speed/30*PI(),((AB1147-AC1147)*2/PI()+AC1147)*-speed/30*PI()),0))","v":153.57072086717474},{"$f":"(L1147^2)/1000000+((K1147/1000)^2*(D1147/C1147*H1147)^2*PI()*PI()*(O1147/2)^2)/1200","v":1.0819322829054226E-2},{"$f":"SQRT(3)*L1147*J1147*D1147/C1147*H1147/1000","v":5.5065685307322925},{"$f":"0.75*J1147^2*(D1147/C1147*H1147)^2-(UAC_V*0.98)^2","v":-152233.65979238754},{"$f":"-AO1147/2/AN1147+SQRT((AO1147/2/AN1147)^2-AP1147/AN1147)","v":3505.2149373042757},{"$f":"(L1147^2)/1000000+((K1147/1000)^2*AV1147^2*PI()*PI()*(O1147/2)^2)/1200","v":5.5705097572272657E-3},{"$f":"SQRT(3)*L1147*J1147*AV1147/1000","v":1.2194155305114529},{"$f":"0.75*J1147^2*AV1147^2-(UAC_V*0.98)^2","v":-153593.8575883398},{"$f":"-AS1147/2/AR1147+SQRT((AS1147/2/AR1147)^2-AT1147/AR1147)","v":5142.656832276868},{"$f":"D1147+(F1147-D1147)*((0.85*UAC_V-D1147*J1147)/L1147*1000)/G1147","v":3.334737991638868},{"$f":"(L1147^2)/1000000+((K1147/1000)^2*AJ1147^2*PI()*PI()*(O1147/2)^2)/1200","v":1.3667303939535604E-2},{"$f":"SQRT(3)*L1147*J1147*AJ1147/1000","v":6.7799857316156427},{"$f":"0.75*J1147^2*AJ1147^2-(UAC_V*0.98)^2","v":-151495.62291121468},{"$f":"IF(((AX1147/2/AW1147)^2-AY1147/AW1147)>0,-AX1147/2/AW1147+SQRT((AX1147/2/AW1147)^2-AY1147/AW1147),-9999)","v":3090.5334970624995}]
["KBM","KBMS-43S02-A (240 V)",11.6,5.12,10.136945606160719,4.3882881411951162,1300,34.5,1717,3.55,12,139,3.73,325,16,1717,1717,1717,9.6676427736753503,30.160857908847184,0.86190815408101018,0.86540136162318848,7.4154894859357168E-2,-23.452280217283953,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},29.856346976000001,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},-2428.3211200000001,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},2440.3211200000001,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},0.18347795622773169,0.27454112161839078,4.4034709494655608,13.177973837682758,9.83285533319963,23.177064434467763,2.5377961113089835,155.46350992981701,3.6897123643143917E-2,13.014720551425221,-151472.30506920334,1857.4406026742151,2.0425249167109714E-2,3.2621718677296756,-153526.30312490804,2662.9292754976691,3.8168321126285392,2.6649587283080464E-2,8.4039494274034059,-152750.14504970817,2241.6296402256598]
["KBM","KBMS-43S03-A (240 V)",21,4.78,18.813539541609121,4.2468486549907727,670,64.5,893,4.83,19,268,5.69,325,16,893,893,893,18.085807180084991,19.77152899824253,0.47840949853707948,0.46912619113178294,0.14258001620774499,-23.948937441975307,9,30.258639328000001,9,-2469.3713600000001,7.5,2481.3713600000001,9,9.4954719648281172E-2,0.14348838887682544,2.2789132715587481,6.8874426660876207,5.1290925343150242,23.259183233679568,2.6066144011263832,159.67926738751993,0.11278233636413708,32.916289147443393,-149892.69064923251,1016.1125416515356,7.4624569867563051E-2,8.6072203320760323,-153406.13270687757,1377.2623448214838,3.8390199435265577,7.68230415192694E-2,11.499609326306761,-153203.70464379009,1339.313378678379]
["KBM","KBMS-57H01-A (400 V)",18.8,5.67,13.222102964557459,3.9468964073305846,1625,46.1,1975,3.39,13,203,9.49,565,24,1279.4377584448944,1806.623322877077,1931.0344827586207,12.598671460407754,11.854583772391992,0.53844765171909159,0.67328837067245118,7.6873791589564769E-2,-24.911844306172839,9,31.038593888000001,9,-2548.95856,7.5,2560.95856,9,0.12669296593344906,0.19502307994787235,3.0406311824027776,9.3611078374978725,6.9458117138121453,23.421451151630073,2.7400376160784883,167.8526747034748,7.9900891930766382E-2,16.572289009537378,-151997.85447950911,1279.4377584448944,4.4402546088286456E-2,4.7611198014252611,-153526.47990873642,1806.623322877077,3.9944109725749914,5.0865365788522195E-2,8.2790283510272129,-153248.17875684248,1656.272597471306]
["KBM","KBMS-57H01-A (480 V)",18.8,5.67,10.713844949600761,3.1981626715226152,2050,46.1,2370,3.39,13,203,9.49,679,24,1279.4377584448944,1816.8301527896365,1931.0344827586207,11.633575455757295,11.854583772391992,0.53877445579909866,0.67328837067245118,7.6873791589564769E-2,-24.911844306172839,9,31.038593888000001,9,-2548.95856,7.5,2560.95856,9,0.12669296593344906,0.19502307994787235,3.0406311824027776,9.3611078374978725,6.9458117138121453,23.421451151630073,2.7400376160784883,167.8526747034748,7.9900891930766382E-2,16.572289009537378,-151997.85447950911,1279.4377584448944,4.4045717923545849E-2,4.4872533640461318,-153541.84559954656,1816.8301527896365,3.7646467263235648,5.0865365788522195E-2,8.2790283510272129,-153248.17875684248,1656.272597471306]
["KBM","KBMS-57H02-A (400 V)",33.5,5.22,26.795904964199107,4.1479729046747842,825,115,1023,4.4000000000000004,22,390,14.9,565,24,591.24074264297644,935.5831883411937,1005.1282051282051,25.897286535106705,7.5503355704697981,0.30565055280483772,0.27955654678260872,0.13462330070171652,-26.282719604938272,9,32.149002880000005,9,-2662.2656000000002,7.5,2674.2656000000002,9,6.612122476682325E-2,0.10436430039402987,1.586909394403758,5.0094864189134336,3.6987381960504746,23.659289559824217,2.9299901405234592,179.48902564540006,0.33616593689141883,53.260034962049318,-149001.55535148139,591.24074264297644,0.16203764956574188,12.37532386519517,-153412.27639584406,935.5831883411937,4.1636926368760099,0.15994212097278476,10.99338665474491,-153465.35675519277,945.77947361153065]
["KBM","KBMS-57H02-A (480 V)",33.5,5.22,24.931661036070302,3.8593902532616569,1015,115,1228,4.4000000000000004,22,390,14.9,679,24,591.24074264297644,936.33113238928058,1005.1282051282051,25.595761059318733,7.5503355704697981,0.30571478381585376,0.27955654678260872,0.13462330070171652,-26.282719604938272,9,32.149002880000005,9,-2662.2656000000002,7.5,2674.2656000000002,9,6.612122476682325E-2,0.10436430039402987,1.586909394403758,5.0094864189134336,3.6987381960504746,23.659289559824217,2.9299901405234592,179.48902564540006,0.33616593689141883,53.260034962049318,-149001.55535148139,591.24074264297644,0.1618789006580636,12.276081173041625,-153416.29755265103,936.33113238928058,4.1303023134319812,0.15994212097278476,10.99338665474491,-153465.35675519277,945.77947361153065]
["KBM","KBMS-57H03-A (400 V)",59.9,5.47,51.264644827494706,4.635139676988671,475,218,597,5.92,35,669,25.2,565,24,313.42017937668498,532.89566684649765,585.94917787742895,50.212119256613555,4.4642857142857144,0.1746029947456092,0.15717013871559632,0.22584593664494718,-28.892703999999995,9,34.263090239999997,9,-2877.9887999999996,7.5,2889.9887999999996,9,3.9526974889276575E-2,6.5184718841402325E-2,0.94864739734263781,3.1288665043873118,2.2905495106120344,24.13345938965346,3.2916372757883727,201.64326126496181,1.0225387978968383,136.56061042339675,-143247.09575722038,313.42017937668498,0.47909136956578102,31.978967846445947,-153092.76256838508,532.89566684649765,4.6618252571789167,0.45517295912027211,15.712602920445223,-153526.09371988647,563.76464578011201]
["KBM","KBMS-57H03-A (480 V)",59.9,5.47,49.392913373346836,4.465905368295374,580,218,717,5.92,35,669,25.2,679,24,313.42017937668498,532.7223754069621,585.94917787742895,50.249379058004486,4.4642857142857144,0.17459882604532911,0.15717013871559632,0.22584593664494718,-28.892703999999995,9,34.263090239999997,9,-2877.9887999999996,7.5,2889.9887999999996,9,3.9526974889276575E-2,6.5184718841402325E-2,0.94864739734263781,3.1288665043873118,2.2905495106120344,24.13345938965346,3.2916372757883727,201.64326126496181,1.0225387978968383,136.56061042339675,-143247.09575722038,313.42017937668498,0.47925580945897855,32.062249134471863,-153089.78340183743,532.7223754069621,4.6739658244990956,0.45517295912027211,15.712602920445223,-153526.09371988647,563.76464578011201]
["KBM","KBMS-57S01-A (240 V)",18.8,5.67,16.00592325412811,4.7778875385457047,880,46.1,1183,3.39,13,203,9.49,325,24,1183,1183,1183,15.043871829129039,11.854583772391992,0.53828343684789226,0.67328837067245118,0.10762802575952347,-24.911844306172839,9,31.038593888000001,9,-2548.95856,7.5,2560.95856,9,0.12669296593344906,0.19502307994787235,3.0406311824027776,9.3611078374978725,6.9458117138121453,23.421451151630073,2.7400376160784883,167.8526747034748,7.9900891930766382E-2,16.572289009537378,-151997.85447950911,1279.4377584448944,4.4521396058562819E-2,4.8489046602847843,-153521.362005845,1803.2915969892933,4.0680593616261254,5.0865365788522195E-2,8.2790283510272129,-153248.17875684248,1656.272597471306]
["KBM","KBMS-57S02-A (240 V)",33.5,5.22,29.506253494564866,4.5675315007066359,445,115,612,4.4000000000000004,22,390,14.9,325,24,591.24074264297644,612,612,28.007476716120671,7.5503355704697981,0.30582334256688265,0.27955654678260872,0.20804567724430761,-26.282719604938272,9,32.149002880000005,9,-2662.2656000000002,7.5,2674.2656000000002,9,6.612122476682325E-2,0.10436430039402987,1.586909394403758,5.0094864189134336,3.6987381960504746,23.659289559824217,2.9299901405234592,179.48902564540006,0.33616593689141883,53.260034962049318,-149001.55535148139,591.24074264297644,0.16140096261223713,11.972330126947202,-153428.40386477875,938.6056364574207,4.028104907703983,0.15994212097278476,10.99338665474491,-153465.35675519277,945.77947361153065]
["KBM","KBMS-57S03-A (240 V)",59.9,5.47,53.858032742297389,4.8696232135892759,250,218,357,5.92,35,669,25.2,325,24,313.42017937668498,357,357,51.272070756000673,4.4642857142857144,0.17499374831029474,0.15717013871559632,0.35664973241881309,-28.892703999999995,9,34.263090239999997,9,-2877.9887999999996,7.5,2889.9887999999996,9,3.9526974889276575E-2,6.5184718841402325E-2,0.94864739734263781,3.1288665043873118,2.2905495106120344,24.13345938965346,3.2916372757883727,201.64326126496181,1.0225387978968383,136.56061042339675,-143247.09575722038,313.42017937668498,0.4752134762472352,29.947938027772931,-153163.01857394,537.08168707618631,4.3657460918901076,0.45517295912027211,15.712602920445223,-153526.09371988647,563.76464578011201]
["KBM","KBMS-79H01-A (400 V)",43.4,4.95,35.571129781038607,4.0102739324733498,600,152,744,6.26,23,534,44.5,565,32,409.12559339504384,673.0517250586347,734.08239700374531,34.617942323113105,2.5280898876404496,0.25054387039328657,0.25147656842105265,0.18466871461227594,-33.783257283950618,9,38.224438400000004,9,-3282.2080000000001,7.5,3294.2080000000001,9,5.1329994534655254E-2,9.0827078571428591E-2,1.2319198688317261,4.3596997714285726,3.1484800424609016,25.092403038945097,3.9692867622556416,243.15556684336411,0.61991499195707211,100.37724576294784,-144830.5969969462,409.12559339504384,0.30336834734728069,23.4127329527272,-153183.4243989994,673.0517250586347,4.0436717499856032,0.2961971936297495,18.229600966347167,-153372.65214883059,689.47225165259454]
["KBM","KBMS-79H01-A (480 V)",43.4,4.95,33.814974895278034,3.8122857830076704,730,152,894,6.26,23,534,44.5,679,32,409.12559339504384,672.96696093434559,734.08239700374531,34.563828472323081,2.5280898876404496,0.25055445072127774,0.25147656842105265,0.18466871461227594,-33.783257283950618,9,38.224438400000004,9,-3282.2080000000001,7.5,3294.2080000000001,9,5.1329994534655254E-2,9.0827078571428591E-2,1.2319198688317261,4.3596997714285726,3.1484800424609016,25.092403038945097,3.9692867622556416,243.15556684336411,0.61991499195707211,100.37724576294784,-144830.5969969462,409.12559339504384,0.30340849346855064,23.438523505370419,-153182.36504920834,672.96696093434559,4.0481261009300429,0.2961971936297495,18.229600966347167,-153372.65214883059,689.47225165259454]
["KBM","KBMS-79H02-A (400 V)",79.31,5.39,67.254331666546648,4.5137135346675601,350,319,443,6.4,32,901,71.5,565,32,223.17093581699675,397.09663857401756,435.07214206437294,65.632098940064125,1.5734265734265733,0.14561861095622095,0.1371981843260188,0.30340976022310295,-40.624963950617285,9,43.766220799999999,9,-3847.6959999999999,7.5,3859.6959999999999,9,3.2388398578033432E-2,6.1966736569579288E-2,0.77732156587280232,2.9744033553398057,2.1158256796353347,26.571444581883924,4.9172938158627009,301.22977671988542,1.8251555411105096,216.52940908268576,-139225.42915637666,223.17093581699675,0.85626161383676169,45.354868163047946,-153030.51221602107,397.09663857401756,4.5410733461077477,0.82145301946242788,21.132227436516498,-153526.4752136211,419.6435684201212]
["KBM","KBMS-79H02-A (480 V)",79.31,5.39,64.846386115581552,4.3521064507101714,430,319,532,6.4,32,901,71.5,679,32,223.17093581699675,396.78800261876535,435.07214206437294,65.963515200354792,1.5734265734265733,0.14558536572506883,0.1371981843260188,0.30340976022310295,-40.624963950617285,9,43.766220799999999,9,-3847.6959999999999,7.5,3859.6959999999999,9,3.2388398578033432E-2,6.1966736569579288E-2,0.77732156587280232,2.9744033553398057,2.1158256796353347,26.571444581883924,4.9172938158627009,301.22977671988542,1.8251555411105096,216.52940908268576,-139225.42915637666,223.17093581699675,0.85686097909777736,45.659555012536835,-153021.97228509732,396.78800261876535,4.5715795604825651,0.82145301946242788,21.132227436516498,-153526.4752136211,419.6435684201212]
["KBM","KBMS-79H03-A (400 V)",143,6.76,122.74824985962429,5.7358995261506687,240,637,307,5.75,34,1300,125,565,32,140.14450962597201,273.42334490160994,301.53846153846155,119.92791140211177,0.9,9.1156008567524857E-2,8.5945306122448981E-2,0.43312756040998651,-54.181679012345683,9,54.747160000000001,9,-4968.2,7.5,4980.2,9,2.5339473355087114E-2,5.3917657575757581E-2,0.60814736052209073,2.5880475636363638,1.8022040204131751,29.886388112495933,6.7957522368989078,416.30274814188124,3.8970718944828411,389.87188259144398,-131178.78034979338,140.14450962597201,1.771078475922266,74.725092824458883,-152837.98823999646,273.42334490160994,5.771578924069714,1.6979054065116088,23.333279243979867,-153583.46125439683,293.96410229123944]
["KBM","KBMS-79H03-A (480 V)",143,6.76,119.2070523758296,5.5704230082163368,300,637,369,5.75,34,1300,125,679,32,140.14450962597201,273.02566928828185,301.53846153846155,121.3463818352328,0.9,9.1083377218548769E-2,8.5945306122448981E-2,0.43312756040998651,-54.181679012345683,9,54.747160000000001,9,-4968.2,7.5,4980.2,9,2.5339473355087114E-2,5.3917657575757581E-2,0.60814736052209073,2.5880475636363638,1.8022040204131751,29.886388112495933,6.7957522368989078,416.30274814188124,3.8970718944828411,389.87188259144398,-131178.78034979338,140.14450962597201,1.7730546928429931,75.630289570175592,-152817.85492596618,273.02566928828185,5.8414940524722709,1.6979054065116088,23.333279243979867,-153583.46125439683,293.96410229123944]
["KBM","KBMS-79S01-A (240 V)",43.4,4.95,38.505228167394037,4.3410629275528798,310,152,445,6.26,23,534,44.5,325,32,409.12559339504384,445,445,36.373633982226927,2.5280898876404496,0.25089784799830989,0.25147656842105265,0.28612124600790173,-33.783257283950618,9,38.224438400000004,9,-3282.2080000000001,7.5,3294.2080000000001,9,5.1329994534655254E-2,9.0827078571428591E-2,1.2319198688317261,4.3596997714285726,3.1484800424609016,25.092403038945097,3.9692867622556416,243.15556684336411,0.61991499195707211,100.37724576294784,-144830.5969969462,409.12559339504384,0.30135230222879755,22.078882354739797,-153236.62248906351,677.39681103880525,3.8132990723202731,0.2961971936297495,18.229600966347167,-153372.65214883059,689.47225165259454]
["KBM","KBMS-79S02-A (240 V)",79.31,5.39,71.354466152866408,4.7888903458299605,180,319,265,6.4,32,901,71.5,325,32,223.17093581699675,265,265,67.597686280608883,1.5734265734265733,0.14602085800629638,0.1371981843260188,0.48046775273025005,-40.624963950617285,9,43.766220799999999,9,-3847.6959999999999,7.5,3859.6959999999999,9,3.2388398578033432E-2,6.1966736569579288E-2,0.77732156587280232,2.9744033553398057,2.1158256796353347,26.571444581883924,4.9172938158627009,301.22977671988542,1.8251555411105096,216.52940908268576,-139225.42915637666,223.17093581699675,0.85088529294532522,42.524313532912494,-153107.11560300941,399.93880271540075,4.2576692330277242,0.82145301946242788,21.132227436516498,-153526.4752136211,419.6435684201212]
["KBM","KBMS-79S03-A (240 V)",143,6.76,128.72451797272495,6.0151643912488302,125,637,184,5.75,34,1300,125,325,32,140.14450962597201,184,184,121.98649045585114,0.9,9.1585369262742133E-2,8.5945306122448981E-2,0.69197801344302323,-54.181679012345683,9,54.747160000000001,9,-4968.2,7.5,4980.2,9,2.5339473355087114E-2,5.3917657575757581E-2,0.60814736052209073,2.5880475636363638,1.8022040204131751,29.886388112495933,6.7957522368989078,416.30274814188124,3.8970718944828411,389.87188259144398,-131178.78034979338,140.14450962597201,1.7604431513559573,69.651915293527239,-152946.33886034664,275.63382249434324,5.3797394039185242,1.6979054065116088,23.333279243979867,-153583.46125439683,293.96410229123944]
["KBM","KBMS-118H01-A (400 V)",325,43.7,109.48238123518914,14.443585914932603,785,994,872,0.27600000000000002,2.5,648,315,565,38,424.00805538635876,587.9353912273682,604.93827160493834,163.58543247786005,0.35714285714285715,5.9479008845675641E-2,0.10294469036440868,0.21189916948141124,-102.32702222222223,9,93.744888000000003,9,-8947.56,7.5,8959.56,9,0.10627161303276267,0.28664685071225077,2.550518712786304,13.759048834188036,8.4643903266282745,44.066210284047393,13.466912984504134,824.97311393962366,0.75139721169624418,41.402748804354658,-152643.41695687795,424.00805538635876,0.4313529871939909,7.6944111806974762,-153628.75148878217,587.9353912273682,24.838803712825154,0.42123352675993497,2.6220465494225071,-153659.90672623544,600.87047431625592]
["KBM","KBMS-118H02-A (400 V)",445,46.5,239.54167706034417,24.797275058006644,590,1451,685,0.29199999999999998,2.7,585,403,565,38,399.83122280328899,645.45776489990044,670.08547008547009,220.22937304286069,0.27915632754342434,5.0488729493943424E-2,8.588967472411535E-2,0.19137014723778223,-124.62591802469137,9,111.8069936,9,-10790.632,7.5,10802.632,9,9.6123566093090751E-2,0.27130642266611182,2.306965586234178,13.022708287973368,7.9487728549683068,51.288906340090811,16.55671375181603,1014.2520202038413,0.83981762885279965,44.860044415419679,-152193.89730078646,399.83122280328899,0.356828607882751,7.6851581969995841,-153620.85465957125,645.45776489990044,25.97487503689597,0.34359258208494498,2.3517948315699582,-153659.95957416188,665.32819413737002]
["KBM","KBMS-118H02-A (480 V)",445,46.5,139.13728616498514,14.403445772772789,710,1451,822,0.29199999999999998,2.7,585,403,679,38,399.83122280328899,651.75229819667891,670.08547008547009,164.22996243007879,0.27915632754342434,5.0701103840529588E-2,8.588967472411535E-2,0.19137014723778223,-124.62591802469137,9,111.8069936,9,-10790.632,7.5,10802.632,9,9.6123566093090751E-2,0.27130642266611182,2.306965586234178,13.022708287973368,7.9487728549683068,51.288906340090811,16.55671375181603,1014.2520202038413,0.83981762885279965,44.860044415419679,-152193.89730078646,399.83122280328899,0.35202238757371207,6.2947411281110615,-153635.05430208932,651.75229819667891,21.275438969640152,0.34359258208494498,2.3517948315699582,-153659.95957416188,665.32819413737002]
["KBM","KBMS-118H03-A (400 V)",560,44,374.83733148884318,29.284166522565872,435,1932,516,0.373,4.3,775,591,565,38,265.09524922361442,474.83301675429266,505.80645161290329,357.8819575185571,0.19035532994923857,5.2637397310205232E-2,8.9163803389310639E-2,0.25427346164345932,-172.26446814814815,9,150.39421920000001,9,-14728.103999999999,7.5,14740.103999999999,9,9.4874508883473707E-2,0.2819805282186949,2.276988213203369,13.535065354497355,8.3597284925632334,67.324230364327263,23.157651754709626,1418.6205926773971,1.8656705274531626,76.005134736652323,-151259.51279653001,265.09524922361442,0.64962323848073444,14.958225946889472,-153570.86846057099,474.83301675429266,29.875069712136579,0.60446160384488357,4.1856540872140977,-153656.70772106646,500.73630826660604]
["KBM","KBMS-118H03-A (480 V)",560,44,302.72162633703306,23.650127057580708,535,1932,619,0.373,4.3,775,591,679,38,265.09524922361442,477.52563124887513,505.80645161290329,330.36071441104252,0.19035532994923857,5.2754815794514631E-2,8.9163803389310639E-2,0.25427346164345932,-172.26446814814815,9,150.39421920000001,9,-14728.103999999999,7.5,14740.103999999999,9,9.4874508883473707E-2,0.2819805282186949,2.276988213203369,13.535065354497355,8.3597284925632334,67.324230364327263,23.157651754709626,1418.6205926773971,1.8656705274531626,76.005134736652323,-151259.51279653001,265.09524922361442,0.6440299123351505,14.078594398635271,-153581.49976264671,477.52563124887513,28.118240130982034,0.60446160384488357,4.1856540872140977,-153656.70772106646,500.73630826660604]
["KBM","KBMS-118H04-A (400 V)",672,42.8,502.32108656444967,31.395067910278105,340,2400,413,0.45500000000000002,4.5,970,698,565,38,229.22256954278296,379.61233386752502,404.12371134020617,482.55232841948526,0.16117478510028654,4.9928684941926989E-2,8.307412427983539E-2,0.31819980149721711,-199.37789827160495,9,172.3560976,9,-16969.112000000001,7.5,16981.112000000001,9,8.7572451458126657E-2,0.26455152672447579,2.1017388349950399,12.698473282774838,7.8758044330709192,76.661889180524312,26.91456859678204,1648.7665355213887,2.3457249252312979,116.85020965642296,-150036.09812499999,229.22256954278296,1.0013785537261357,24.24482715828627,-153507.81665322161,379.61233386752502,31.715775430593695,0.94462941381920551,6.0205848546927623,-153654.36894409807,400.13838435606255]
["KBM","KBMS-118H04-A (480 V)",672,42.8,450.74953525668928,28.17184595354308,420,2400,495,0.45500000000000002,4.5,970,698,679,38,229.22256954278296,380.07080505983259,404.12371134020617,471.78370891701854,0.16117478510028654,4.9975205793493717E-2,8.307412427983539E-2,0.31819980149721711,-199.37789827160495,9,172.3560976,9,-16969.112000000001,7.5,16981.112000000001,9,8.7572451458126657E-2,0.26455152672447579,2.1017388349950399,12.698473282774838,7.8758044330709192,76.661889180524312,26.91456859678204,1648.7665355213887,2.3457249252312979,116.85020965642296,-150036.09812499999,229.22256954278296,0.99976998151047247,23.92022958061802,-153511.97072399047,380.07080505983259,31.291154384156478,0.94462941381920551,6.0205848546927623,-153654.36894409807,400.13838435606255]
["KBM","KBMS-118S01-A (240 V)",325,43.7,252.45952847951898,33.306006395714903,400,994,523,0.27600000000000002,2.5,648,315,325,38,424.00805538635876,523,523,230.15333348697106,0.35714285714285715,5.9095871087106733E-2,0.10294469036440868,0.24344924373521273,-102.32702222222223,9,93.744888000000003,9,-8947.56,7.5,8959.56,9,0.10627161303276267,0.28664685071225077,2.550518712786304,13.759048834188036,8.4643903266282745,44.066210284047393,13.466912984504134,824.97311393962366,0.75139721169624418,41.402748804354658,-152643.41695687795,424.00805538635876,0.43722271502306459,9.4634542956203305,-153610.68009401835,582.00988198255095,30.549560996153815,0.42123352675993497,2.6220465494225071,-153659.90672623544,600.87047431625592]
["KBM","KBMS-118S02-A (240 V)",445,46.5,356.90495988357532,36.946683217761418,320,1451,411,0.29199999999999998,2.7,585,403,325,38,399.83122280328899,411,411,331.85293285046703,0.27915632754342434,5.0302578354958431E-2,8.588967472411535E-2,0.30979064348787411,-124.62591802469137,9,111.8069936,9,-10790.632,7.5,10802.632,9,9.6123566093090751E-2,0.27130642266611182,2.306965586234178,13.022708287973368,7.9487728549683068,51.288906340090811,16.55671375181603,1014.2520202038413,0.83981762885279965,44.860044415419679,-152193.89730078646,399.83122280328899,0.36150040949692719,8.8292646921229725,-153607.05214770723,639.757679432945,29.841812122372421,0.34359258208494498,2.3517948315699582,-153659.95957416188,665.32819413737002]
["KBM","KBMS-118S03-A (240 V)",560,44,467.30600312088416,36.508281493819069,235,1932,309,0.373,4.3,775,591,325,38,265.09524922361442,309,309,438.11725516746043,0.19035532994923857,5.2571260834321364E-2,8.9163803389310639E-2,0.41205163260037625,-172.26446814814815,9,150.39421920000001,9,-14728.103999999999,7.5,14740.103999999999,9,9.4874508883473707E-2,0.2819805282186949,2.276988213203369,13.535065354497355,8.3597284925632334,67.324230364327263,23.157651754709626,1418.6205926773971,1.8656705274531626,76.005134736652323,-151259.51279653001,265.09524922361442,0.65233012942540403,15.365852863225449,-153565.72344049354,473.55703039923333,30.689195838143718,0.60446160384488357,4.1856540872140977,-153656.70772106646,500.73630826660604]
["KBM","KBMS-118S04-A (240 V)",672,42.8,577.08722068131567,36.067951292582229,185,2400,247,0.45500000000000002,4.5,970,698,325,38,229.22256954278296,247,247,545.27861355829714,0.16117478510028654,4.995213723062595E-2,8.307412427983539E-2,0.51548159705877028,-199.37789827160495,9,172.3560976,9,-16969.112000000001,7.5,16981.112000000001,9,8.7572451458126657E-2,0.26455152672447579,2.1017388349950399,12.698473282774838,7.8758044330709192,76.661889180524312,26.91456859678204,1648.7665355213887,2.3457249252312979,116.85020965642296,-150036.09812499999,229.22256954278296,0.99784570121316019,23.526041914563411,-153516.94009773468,380.62379286090191,30.775499336897255,0.94462941381920551,6.0205848546927623,-153654.36894409807,400.13838435606255]
["KBM","KBMS-60H01-A (400 V)",54,13.7,34.759439571269944,8.6038216760569171,1250,127,1639,0.91600000000000004,7.8,245,25.6,565,38,761.29308542055537,1435.4252920298613,1600,31.905290342217572,4.39453125,0.19375229538533675,0.27043457259842518,8.5346607446859971E-2,-28.994062617283944,9,34.345190719999998,9,-2886.3663999999999,7.5,2898.3663999999999,9,0.1099008313581336,0.18153129354320985,2.6376199525952062,8.7135020900740727,6.3769059035347571,24.152421342923351,3.3056818247307,202.50361992979919,0.24755724953138974,12.524278422296174,-153010.69908371847,761.29308542055537,7.232290207237474E-2,3.2072310465352643,-153621.15813833461,1435.4252920298613,8.2510280192071122,6.7370729367431631E-2,2.4787469569902219,-153638.40988556106,1491.8455259371965]
["KBM","KBMS-60H01-A (480 V)",54,13.7,24.858012674165401,6.1529734341993567,1600,127,1895,0.91600000000000004,7.8,245,25.6,679,38,761.29308542055537,1462.0374544251308,1600,27.370826895779597,4.39453125,0.19397857328841264,0.27043457259842518,8.5346607446859971E-2,-28.994062617283944,9,34.345190719999998,9,-2886.3663999999999,7.5,2898.3663999999999,9,0.1099008313581336,0.18153129354320985,2.6376199525952062,8.7135020900740727,6.3769059035347571,24.152421342923351,3.3056818247307,202.50361992979919,0.24755724953138974,12.524278422296174,-153010.69908371847,761.29308542055537,6.9905415095751225E-2,2.8747648585239767,-153629.57987092127,1462.0374544251308,7.3957145750186903,6.7370729367431631E-2,2.4787469569902219,-153638.40988556106,1491.8455259371965]
["KBM","KBMS-60H02-A (400 V)",108,16.399999999999999,88.643815200699777,13.055053785080968,725,255,974,0.92100000000000004,11,411,42,565,38,446.96442055897234,803.66743274534781,953.77128953771285,86.543537454623262,2.6785714285714284,0.10004401717359644,0.14788749176470589,0.13704390652848286,-33.149765925925927,9,37.711310400000002,9,-3229.848,7.5,3241.848,9,6.7988472955146151E-2,0.11930275666666666,1.6317233509235076,5.7265323199999996,4.1422433464449702,24.963283009110185,3.8815083313660983,237.77832518813062,0.70760195024155381,25.38764123306548,-152710.10390747918,446.96442055897234,0.2273496500025925,8.361216514288067,-153560.53456112798,803.66743274534781,12.752854073449626,0.17508527903711146,2.7157994026294898,-153653.0842962164,929.07417556032362]
["KBM","KBMS-60H02-A (480 V)",108,16.399999999999999,84.001439455620698,12.371346017028085,885,255,1169,0.92100000000000004,11,411,42,679,38,446.96442055897234,802.82589553852665,953.77128953771285,86.229756089630655,2.6785714285714284,0.10005267305892385,0.14788749176470589,0.13704390652848286,-33.149765925925927,9,37.711310400000002,9,-3229.848,7.5,3241.848,9,6.7988472955146151E-2,0.11930275666666666,1.6317233509235076,5.7265323199999996,4.1422433464449702,24.963283009110185,3.8815083313660983,237.77832518813062,0.70760195024155381,25.38764123306548,-152710.10390747918,446.96442055897234,0.22779646739523066,8.3931257039457385,-153559.74333700037,802.82589553852665,12.801523216104993,0.17508527903711146,2.7157994026294898,-153653.0842962164,929.07417556032362]
["KBM","KBMS-60H03-A (400 V)",154,18.7,119.77083853017209,14.090686885902599,590,393,778,0.86699999999999999,11,515,52.9,565,38,358.38962772909792,662.73310691202528,761.1650485436893,115.55118893577553,2.1266540642722118,7.1979336010658368E-2,0.10165025058524174,0.16976986766897922,-35.911788246913581,9,39.948548480000007,9,-3458.1376,7.5,3470.1376,9,5.5615150297258283E-2,0.10106031609523809,1.3347636071341988,4.8508951725714287,3.4852984578825654,25.53634490980976,4.2642222900445041,261.22309880494851,1.0833844362918668,36.906289996527782,-152380.1143922068,358.38962772909792,0.33352633394232695,10.663407620725721,-153556.81905732327,662.73310691202528,13.788247075183261,0.26958906308388764,2.6954229884072904,-153657.15175314693,749.97970029507906]
["KBM","KBMS-60H03-A (480 V)",154,18.7,110.74531456811052,13.028860537424766,720,393,930,0.86699999999999999,11,515,52.9,679,38,358.38962772909792,663.16787201296358,761.1650485436893,114.15955876047738,2.1266540642722118,7.2000888501637286E-2,0.10165025058524174,0.16976986766897922,-35.911788246913581,9,39.948548480000007,9,-3458.1376,7.5,3470.1376,9,5.5615150297258283E-2,0.10106031609523809,1.3347636071341988,4.8508951725714287,3.4852984578825654,25.53634490980976,4.2642222900445041,261.22309880494851,1.0833844362918668,36.906289996527782,-152380.1143922068,358.38962772909792,0.33312710985346489,10.632197921680245,-153557.44553431447,663.16787201296358,13.747891584997859,0.26958906308388764,2.6954229884072904,-153657.15175314693,749.97970029507906]
["KBM","KBMS-60S01-A (240 V)",54,13.7,44.708070377632424,11.066354053869413,660,127,983,0.91600000000000004,7.8,245,25.6,325,38,761.29308542055537,983,983,40.160656335170714,4.39453125,0.19364710659197532,0.27043457259842518,0.12952589468312947,-28.994062617283944,9,34.345190719999998,9,-2886.3663999999999,7.5,2898.3663999999999,9,0.1099008313581336,0.18153129354320985,2.6376199525952062,8.7135020900740727,6.3769059035347571,24.152421342923351,3.3056818247307,202.50361992979919,0.24755724953138974,12.524278422296174,-153010.69908371847,761.29308542055537,7.2670226109468605E-2,3.2522058880969,-153619.94817518294,1431.7325874256796,8.3667317750326671,6.7370729367431631E-2,2.4787469569902219,-153638.40988556106,1491.8455259371965]
["KBM","KBMS-60S02-A (240 V)",108,16.399999999999999,95.989033210228826,14.136823742301742,385,255,584,0.92100000000000004,11,411,42,325,38,446.96442055897234,584,584,89.780767259152299,2.6785714285714284,0.10013707798134101,0.14788749176470589,0.21802046998889771,-33.149765925925927,9,37.711310400000002,9,-3229.848,7.5,3241.848,9,6.7988472955146151E-2,0.11930275666666666,1.6317233509235076,5.7265323199999996,4.1422433464449702,24.963283009110185,3.8815083313660983,237.77832518813062,0.70760195024155381,25.38764123306548,-152710.10390747918,446.96442055897234,0.21854809297479377,7.7057685726332714,-153576.12035612063,820.83441596643695,11.753139266593166,0.17508527903711146,2.7157994026294898,-153653.0842962164,929.07417556032362]
["KBM","KBMS-60S03-A (240 V)",154,18.7,133.38699992463609,15.692588226427775,315,393,467,0.86699999999999999,11,515,52.9,325,38,358.38962772909792,467,467,123.44040941207953,2.1266540642722118,7.2057038255803937E-2,0.10165025058524174,0.27264230079982071,-35.911788246913581,9,39.948548480000007,9,-3458.1376,7.5,3470.1376,9,5.5615150297258283E-2,0.10106031609523809,1.3347636071341988,4.8508951725714287,3.4852984578825654,25.53634490980976,4.2642222900445041,261.22309880494851,1.0833844362918668,36.906289996527782,-152380.1143922068,358.38962772909792,0.32314721536459268,9.8198306951795189,-153573.10634849468,674.35129848966801,12.697465639261475,0.26958906308388764,2.6954229884072904,-153657.15175314693,749.97970029507906]
["KBM","KBMS-88H01-A (400 V)",205,17,162.33804195373327,13.306396881453548,425,414,542,0.93,13,738,146,565,46,315.00667676066973,466.356594627199,531.16531165311653,158.18662241274026,0.77054794520547942,6.644291623879843E-2,0.14372706864674659,0.24323891384701504,-59.503006419753092,9,59.0574352,9,-5408.0240000000003,7.5,5420.0240000000003,9,4.6552447403057966E-2,0.10279990946502059,1.1172587376733911,4.9343956543209879,3.3890165904370351,31.299252364547094,7.5330910563710658,461.47157804584231,1.4113098397515564,40.812701158126359,-152899.42874987031,315.00667676066973,0.67241775662622771,15.670769818796241,-153551.2781914821,466.356594627199,13.182275801047108,0.55308916746132031,4.0287807433525149,-153656.54968645665,523.45224067887671]
["KBM","KBMS-88H01-A (480 V)",205,17,151.31962281660205,12.403247771852628,520,414,651,0.93,13,738,146,679,46,315.00667676066973,466.84395218769458,531.16531165311653,156.80700107841608,0.77054794520547942,6.6463644417627463E-2,0.14372706864674659,0.24323891384701504,-59.503006419753092,9,59.0574352,9,-5408.0240000000003,7.5,5420.0240000000003,9,4.6552447403057966E-2,0.10279990946502059,1.1172587376733911,4.9343956543209879,3.3890165904370351,31.299252364547094,7.5330910563710658,461.47157804584231,1.4113098397515564,40.812701158126359,-152899.42874987031,315.00667676066973,0.67115140053170197,15.592920538203897,-153552.3953688507,466.84395218769458,13.11678886584559,0.55308916746132031,4.0287807433525149,-153656.54968645665,523.45224067887671]
["KBM","KBMS-88H01-B (400 V)",205,32,66.998273370021394,10.197606296806908,935,414,1006,0.26100000000000001,3.7,397,146,565,46,600.40243190909291,952.6645847028816,987.40554156171288,64.391061402963459,0.77054794520547942,6.6787933369485034E-2,0.14372706864674659,0.13041186209870609,-59.503006419753092,9,59.0574352,9,-5408.0240000000003,7.5,5420.0240000000003,9,8.7628136288109115E-2,0.19350571193415642,2.1030752709146188,9.2882741728395075,6.3793253467050075,31.299252364547094,7.5330910563710658,461.47157804584231,0.4063632653612248,11.59813340574218,-153450.62909716862,600.40243190909291,0.1669461829669705,2.2470398076081426,-153655.99095880156,952.6645847028816,12.520426549720277,0.16003296934474243,1.1448969364426342,-153661.92082147105,976.32188072851352]
["KBM","KBMS-88H01-B (480 V)",205,32,67.048252621692072,10.20521348884202,940,414,1068,0.26100000000000001,3.7,397,146,679,46,600.40243190909291,952.13716301534157,987.40554156171288,65.267036827881725,0.77054794520547942,6.6781776637564266E-2,0.14372706864674659,0.13041186209870609,-59.503006419753092,9,59.0574352,9,-5408.0240000000003,7.5,5420.0240000000003,9,8.7628136288109115E-2,0.19350571193415642,2.1030752709146188,9.2882741728395075,6.3793253467050075,31.299252364547094,7.5330910563710658,461.47157804584231,0.4063632653612248,11.59813340574218,-153450.62909716862,600.40243190909291,0.16711153472301887,2.2668488568680969,-153655.84912704877,952.13716301534157,12.630801873485925,0.16003296934474243,1.1448969364426342,-153661.92082147105,976.32188072851352]
["KBM","KBMS-88H02-A (400 V)",385,15,331.71240770731868,12.907097576160259,190,789,257,1.66,29,1560,247,565,46,149.19769377310638,215.66783868864522,251.28205128205127,324.51357969113531,0.45546558704453444,4.3979424496109483E-2,0.10785305105697163,0.51232944803983316,-85.096057283950614,9,79.787806400000008,9,-7523.3680000000004,7.5,7535.3680000000004,9,2.7042897955173954E-2,6.9071475068141722E-2,0.64902955092417491,3.3154308032708029,2.1064253453286401,38.699843242509104,11.079339664308581,678.71214091727381,5.8912834617309935,137.87986404702104,-151711.0437921572,149.19769377310638,3.0307669411326721,57.300196178495682,-153326.71033837792,215.66783868864522,12.775055486666997,2.4498353744895836,9.4479891417032729,-153654.82999477917,248.51968779201803]
["KBM","KBMS-88H02-A (480 V)",385,15,323.05067172269821,12.570065047575806,235,789,309,1.66,29,1560,247,679,46,149.19769377310638,215.13076300222383,251.28205128205127,328.28848400097371,0.45546558704453444,4.3936070001107289E-2,0.10785305105697163,0.51232944803983316,-85.096057283950614,9,79.787806400000008,9,-7523.3680000000004,7.5,7535.3680000000004,9,2.7042897955173954E-2,6.9071475068141722E-2,0.64902955092417491,3.3154308032708029,2.1064253453286401,38.699843242509104,11.079339664308581,678.71214091727381,5.8912834617309935,137.87986404702104,-151711.0437921572,149.19769377310638,3.0435838744744936,57.911845800952499,-153319.47112466375,215.13076300222383,12.911422521797972,2.4498353744895836,9.4479891417032729,-153654.82999477917,248.51968779201803]
["KBM","KBMS-88H02-B (400 V)",385,31.7,273.02307055855135,22.563890128805898,440,789,545,0.36899999999999999,6.4,733,247,565,46,333.13202353645516,486.78463189451486,534.7885402455662,261.11670822992357,0.45546558704453444,4.3912632863589859E-2,0.10785305105697163,0.23973110892546487,-85.096057283950614,9,79.787806400000008,9,-7523.3680000000004,7.5,7535.3680000000004,9,5.7150657678600947E-2,0.1459710506440062,1.3716157842864227,7.0066104309122972,4.451578896461192,38.699843242509104,11.079339664308581,678.71214091727381,1.2894056295513745,30.434523324444495,-153233.01210987655,333.13202353645516,0.62670872655903109,10.493988338004364,-153612.75951711362,486.78463189451486,22.400082046974838,0.54082052487084431,2.0854752642068553,-153661.97631857454,531.11152342394882]
["KBM","KBMS-88H02-B (480 V)",385,31.7,233.08964847367582,19.263607311874036,550,789,654,0.36899999999999999,6.4,733,247,679,46,333.13202353645516,489.59321572574953,534.7885402455662,249.77404089854167,0.45546558704453444,4.3968452565963309E-2,0.10785305105697163,0.23973110892546487,-85.096057283950614,9,79.787806400000008,9,-7523.3680000000004,7.5,7535.3680000000004,9,5.7150657678600947E-2,0.1459710506440062,1.3716157842864227,7.0066104309122972,4.451578896461192,38.699843242509104,11.079339664308581,678.71214091727381,1.2894056295513745,30.434523324444495,-153233.01210987655,333.13202353645516,0.6202234764432768,10.106283158454405,-153616.47578152592,489.59321572574953,21.572500811678005,0.54082052487084431,2.0854752642068553,-153661.97631857454,531.11152342394882]
["KBM","KBMS-88H03-A (400 V)",538,18.100000000000001,462.41745283790686,15.413915094596895,165,1200,221,1.41,26,1812,315,565,46,126.22164547992375,188.19735362708036,216.3355408388521,451.79130087090959,0.35714285714285715,3.5936063205761037E-2,8.5272518518518525E-2,0.59363818298226667,-102.32702222222223,9,93.744888000000003,9,-8947.56,7.5,8959.56,9,2.6589826021676453E-2,7.1720845036486305E-2,0.63815582452023489,3.4426005617513429,2.117843700134868,44.066210284047393,13.466912984504134,824.97311393962366,8.0771003636998877,178.65512478481151,-151233.72970149666,126.22164547992375,3.9695658068161701,67.594250552412674,-153316.10904585826,188.19735362708036,15.274669559949619,3.2965359403268648,9.3719904797886304,-153657.31213805551,214.48073611754137]
["KBM","KBMS-88H03-A (480 V)",538,18.100000000000001,443.08736156783664,14.769578718927887,225,1200,265,1.41,26,1812,315,679,46,126.22164547992375,187.52927190618459,216.3355408388521,458.89378675609532,0.35714285714285715,3.5881404238794525E-2,8.5272518518518525E-2,0.59363818298226667,-102.32702222222223,9,93.744888000000003,9,-8947.56,7.5,8959.56,9,2.6589826021676453E-2,7.1720845036486305E-2,0.63815582452023489,3.4426005617513429,2.117843700134868,44.066210284047393,13.466912984504134,824.97311393962366,8.0771003636998877,178.65512478481151,-151233.72970149666,126.22164547992375,3.9927981537812891,68.728943437255907,-153304.33104161479,187.52927190618459,15.531082771522501,3.2965359403268648,9.3719904797886304,-153657.31213805551,214.48073611754137]
["KBM","KBMS-88H03-B (400 V)",545,35.5,400.51687418082179,25.839798334246566,345,1200,426,0.37,7,940,315,565,46,254.02977245253496,379.58806696605825,417.02127659574467,386.03167988720105,0.35714285714285715,3.5408028164731389E-2,8.5272518518518525E-2,0.30696311074720145,-102.32702222222223,9,93.744888000000003,9,-8947.56,7.5,8959.56,9,5.148148281088738E-2,0.13886121134896365,1.2355555874612971,6.6653381447502547,4.1004305163845949,44.066210284047393,13.466912984504134,824.97311393962366,2.1861561239418492,47.087247227828627,-153036.67744129282,254.02977245253496,1.0251064874372537,15.520054954632348,-153595.84922312279,379.58806696605825,25.763392483883763,0.88718450479243194,2.4701291567773769,-153662.27367076415,414.78584890408388]
["KBM","KBMS-88H03-B (480 V)",545,35.5,359.5029302781636,23.193737437300879,425,1200,511,0.37,7,940,315,679,46,254.02977245253496,380.34619657053793,417.02127659574467,378.99269425016382,0.35714285714285715,3.543396135521016E-2,8.5272518518518525E-2,0.30696311074720145,-102.32702222222223,9,93.744888000000003,9,-8947.56,7.5,8959.56,9,5.148148281088738E-2,0.13886121134896365,1.2355555874612971,6.6653381447502547,4.1004305163845949,44.066210284047393,13.466912984504134,824.97311393962366,2.1861561239418492,47.087247227828627,-153036.67744129282,254.02977245253496,1.0214808271420253,15.31993841096463,-153597.59537321306,380.34619657053793,25.431197715753072,0.88718450479243194,2.4701291567773769,-153662.27367076415,414.78584890408388]
["KBM","KBMS-88S01-A (240 V)",205,17,179.31456921686876,14.697915509579408,225,414,325,0.93,13,738,146,325,46,315.00667676066973,325,325,167.89882220214378,0.77054794520547942,6.6543217853561709E-2,0.14372706864674659,0.39176601376466541,-59.503006419753092,9,59.0574352,9,-5408.0240000000003,7.5,5420.0240000000003,9,4.6552447403057966E-2,0.10279990946502059,1.1172587376733911,4.9343956543209879,3.3890165904370351,31.299252364547087,7.5330910563710658,461.47157804584231,1.4113098397515564,40.812701158126359,-152899.42874987031,315.00667676066973,0.65963465812842459,14.866227669365211,-153562.55542101015,471.35594379950959,12.505493700996979,0.55308916746132031,4.0287807433525149,-153656.54968645665,523.45224067887671]
["KBM","KBMS-88S01-B (240 V)",205,32,156.03550620729419,23.74969653079059,500,414,604,0.26100000000000001,3.7,397,146,325,46,600.40243190909291,604,604,145.85089149841139,0.77054794520547942,6.6425095026534792E-2,0.14372706864674659,0.2108012491283382,-59.503006419753092,9,59.0574352,9,-5408.0240000000003,7.5,5420.0240000000003,9,8.7628136288109115E-2,0.19350571193415642,2.1030752709146188,9.2882741728395075,6.3793253467050075,31.299252364547087,7.5330910563710658,461.47157804584231,0.4063632653612248,11.59813340574218,-153450.62909716862,600.40243190909291,0.17737260676206618,3.2691581732212933,-153647.04761282424,921.54965995594273,18.215634030446537,0.16003296934474243,1.1448969364426342,-153661.92082147105,976.32188072851352]
["KBM","KBMS-88S02-A (240 V)",385,15,346.63946605414804,13.487916967087473,100,789,154,1.66,29,1560,247,325,46,149.19769377310638,154,154,325.92477772338799,0.45546558704453444,4.424673796574459E-2,0.10785305105697163,0.82677892515270301,-85.096057283950614,9,79.787806400000008,9,-7523.3680000000004,7.5,7535.3680000000004,9,2.7042897955173954E-2,6.9071475068141722E-2,0.64902955092417491,3.3154308032708029,2.1064253453286401,38.699843242509104,11.079339664308581,678.71214091727381,5.8912834617309935,137.87986404702104,-151711.0437921572,149.19769377310638,2.9557552361836645,53.580658768006025,-153369.07817697921,218.90647626978839,11.945786130315788,2.4498353744895836,9.4479891417032729,-153654.82999477917,248.51968779201803]
["KBM","KBMS-88S02-B (240 V)",385,31.7,323.45702476889028,26.731985518090106,235,789,327,0.36899999999999999,6.4,733,247,325,46,327,327,327,299.36360467841325,0.45546558704453444,4.3931624928835823E-2,0.10785305105697163,0.38936989135631883,-85.096057283950614,9,79.787806400000008,9,-7523.3680000000004,7.5,7535.3680000000004,9,5.7150657678600947E-2,0.1459710506440062,1.3716157842864227,7.0066104309122972,4.451578896461192,38.699843242509104,11.079339664308581,678.71214091727381,1.2894056295513745,30.434523324444495,-153233.01210987655,333.13202353645516,0.62536711268951861,10.414967247959693,-153613.52830656496,487.36102802333812,22.231406530724104,0.54082052487084431,2.0854752642068553,-153661.97631857454,531.11152342394882]
["KBM","KBMS-88S03-A (240 V)",538,18.100000000000001,482.76999404541584,16.092333134847195,90,1200,132,1.41,26,1812,315,325,46,126.22164547992375,132,132,456.99599126660991,0.35714285714285715,3.6172623750920674E-2,8.5272518518518525E-2,0.9645754126781535,-102.32702222222223,9,93.744888000000003,9,-8947.56,7.5,8959.56,9,2.6589826021676453E-2,7.1720845036486305E-2,0.63815582452023489,3.4426005617513429,2.117843700134868,44.066210284047393,13.466912984504134,824.97311393962366,8.0771003636998877,178.65512478481151,-151233.72970149666,126.22164547992375,3.8787830169156052,62.96455584522618,-153362.13281118378,190.89251651404209,14.228470271729279,3.2965359403268648,9.3719904797886304,-153657.31213805551,214.48073611754137]
["KBM","KBMS-88S03-B (240 V)",545,35.5,463.67140087438844,29.914283927379898,180,1200,255,0.37,7,940,315,325,46,254.02977245253496,255,255,429.7844845720503,0.35714285714285715,3.5456535324261747E-2,8.5272518518518525E-2,0.49930962538633827,-102.32702222222223,9,93.744888000000003,9,-8947.56,7.5,8959.56,9,5.148148281088738E-2,0.13886121134896365,1.2355555874612971,6.6653381447502547,4.1004305163845949,44.066210284047393,13.466912984504134,824.97311393962366,2.1861561239418492,47.087247227828627,-153036.67744129282,254.02977245253496,1.0137647819533937,14.885102408964276,-153601.31148887353,381.97794510331005,24.709367115384339,0.88718450479243194,2.4701291567773769,-153662.27367076415,414.78584890408388]
["KBM","KBMS-163H01-A (400 V)",776,43.2,534.60145384567647,29.535991925175495,300,1966,365,0.37,4.2,1100,1230,565,56,228.8884452378488,334.35835300342399,356.36363636363637,506.95459896806454,9.1463414634146339E-2,7.0419693740717326E-2,0.16998212576768021,0.36300176357262487,-334.18485925925927,9,281.54973600000005,9,-28111.32,7.5,28123.32,9,0.12383938543283736,0.38758553264604817,2.9721452503880967,18.604105567010311,11.661676718564975,124.02900755002838,45.593818690076674,2793.0435597550672,2.5725241885138996,77.154378213855807,-152434.08304182507,228.8884452378488,1.310900278111971,20.995907309246878,-153572.91980914495,334.35835300342399,29.783765938265645,1.2254687470776564,8.2208369472450382,-153650.03674377827,350.75299144667343]
["KBM","KBMS-163H01-A (480 V)",776,43.2,440.54088247836631,24.339275275047861,375,1966,438,0.37,4.2,1100,1230,679,56,228.8884452378488,335.89645601928447,356.36363636363637,475.52125676033756,9.1463414634146339E-2,7.0605432443991978E-2,0.16998212576768021,0.36300176357262487,-334.18485925925927,9,281.54973600000005,9,-28111.32,7.5,28123.32,9,0.12383938543283736,0.38758553264604817,2.9721452503880967,18.604105567010311,11.661676718564975,124.02900755002838,45.593818690076674,2793.0435597550672,2.5725241885138996,77.154378213855807,-152434.08304182507,228.8884452378488,1.3016456276355377,20.009873361916778,-153581.27375372729,335.89645601928447,28.385026466714926,1.2254687470776564,8.2208369472450382,-153650.03674377827,350.75299144667343]
["KBM","KBMS-163H02-A (400 V)",1090,40.6,843.68035333013711,31.017660048902101,200,2915,243,0.50900000000000001,6.3,1645,1720,565,56,149.45650791721917,220.2829668136086,238.29787234042556,818.69988723541405,6.5406976744186052E-2,6.8136404894790698E-2,0.15723813565423631,0.54375212019344143,-458.3491654320988,9,382.12282400000004,9,-38373.879999999997,7.5,38385.879999999997,9,0.11237463482450087,0.35567614901649863,2.6969912357880208,17.072455152791935,10.746846792780378,168.21133742845828,62.798391144427008,3846.9829241808247,5.7231399054328129,157.46440871065298,-151373.27467312798,149.45650791721917,2.9567405867374492,45.391773224812034,-153473.64578334524,220.2829668136086,31.299171138760283,2.7355831858962518,15.585666161478015,-153641.55813511543,234.15808370222149]
["KBM","KBMS-163H02-A (480 V)",1090,40.6,781.87301838940914,28.74533155843416,245,2915,291,0.50900000000000001,6.3,1645,1720,679,56,149.45650791721917,220.35873143153665,238.29787234042556,812.86338454066026,6.5406976744186052E-2,6.8173499986409453E-2,0.15723813565423631,0.54375212019344143,-458.3491654320988,9,382.12282400000004,9,-38373.879999999997,7.5,38385.879999999997,9,0.11237463482450087,0.35567614901649863,2.6969912357880208,17.072455152791935,10.746846792780378,168.21133742845828,62.798391144427008,3846.9829241808247,5.7231399054328129,157.46440871065298,-151373.27467312798,149.45650791721917,2.955266442853512,45.258130447919079,-153474.76501772518,220.35873143153665,31.207019899708328,2.7355831858962518,15.585666161478015,-153641.55813511543,234.15808370222149]
["KBM","KBMS-163H03-A (400 V)",1375,38.6,1115.3578411880026,30.810990088066365,150,3930,183,0.64,8.4,2190,1830,565,56,108.18501456669327,164.06954844696992,178.99543378995435,1091.0041883061276,6.1475409836065573E-2,5.7376916515100566E-2,0.1237208104796909,0.7225686176357452,-486.22278518518522,9,404.70045600000003,9,-40677.72,7.5,40689.72,9,8.9703858824012397E-2,0.28436665921436588,2.1528926117762976,13.649599642289562,8.5977953509433629,178.16115732580599,66.660642103566872,4083.5815570110967,10.334029821388199,267.83163534448545,-149924.8272924198,108.18501456669327,5.2368434273326256,75.558107454145812,-153366.41302297427,164.06954844696992,31.124067978103419,4.8297331342920291,20.872372642688209,-153641.29113551974,176.21019148343595]
["KBM","KBMS-163H03-A (480 V)",1375,38.6,1063.9507945693204,29.390905927329289,180,3930,220,0.64,8.4,2190,1830,679,56,{"$f":"IF(AQ1211<I1211,IF(AQ1211<0,0,AQ1211),I1211)","v":108.18501456669327},{"$f":"IF(AU1211<I1211,IF(AU1211<0,0,AU1211),I1211)","v":163.99705862597972},{"$f":"IF(UAC_V*0.98/L1211*1000<I1211,IF(UAC_V*0.98/L1211*1000<0,0,UAC_V*0.98/L1211*1000),I1211)","v":178.99543378995435},{"$f":"C1211+(E1211-C1211)/G1211*Q1211","v":1091.6046956745579},{"$f":"IF(move1,IF(kgcm2,(inertia/10/gear^2+gear_inertia/10)/M1211,(inertia/gear^2+gear_inertia)/M1211),IF(kgcm2,(MAX(inertia,inertia2)/10/gear^2+gear_inertia/10)/M1211,(MAX(inertia,inertia2)/gear^2+gear_inertia)/M1211))","v":6.1475409836065573E-2},{"$f":"IF((C1211+(E1211-C1211)/G1211*mspeed)<0,\"NA\",IF(move1,IF(AccType=1,SQRT((X1211^2*time1+Y1211^2*time2+Z1211^2*time3+AA1211^2*time4)/time)/(C1211+(E1211-C1211)/G1211*mspeed),SQRT((((X1211-Y1211)*2/PI()+Y1211)^2*time1+Y1211^2*time2+((Z1211-Y1211)*2/PI()+Y1211)^2*time3+AA1211^2*time4)/time)/(C1211+(E1211-C1211)/G1211*mspeed)),IF(AccType=1,SQRT((X1211^2*time1+Y1211^2*time2+Z1211^2*time3+AA1211^2*time4+AB1211^2*time5+AC1211^2*time6+AD1211^2*time7+AE1211^2*time8)/time)/(C1211+(E1211-C1211)/G1211*mspeed),SQRT((((X1211-Y1211)*2/PI()+Y1211)^2*time1+Y1211^2*time2+((Z1211-Y1211)*2/PI()+Y1211)^2*time3+AA1211^2*time4+((AB1211-AC1211)*2/PI()+AC1211)^2*time5+AC1211^2*time6+((AD1211-AC1211)*2/PI()+AC1211)^2*time7+AE1211^2*time8)/time)/(C1211+(E1211-C1211)/G1211*mspeed))))","v":5.7374157967056492E-2},{"$f":"IF(move1,MAX(ABS(X1211),ABS(Z1211))/H1211,MAX(ABS(X1211),ABS(Z1211),ABS(AB1211),ABS(AD1211))/H1211)","v":0.1237208104796909},{"$f":"IF(AZ1211>0,speed/(MIN(AZ1211,I1211)),\"NA\")","v":0.7225686176357452},{"$f":"IF(kgcm2,(accel1*gear*(inertia/10/gear^2+M1211+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel1*gear*(inertia/gear^2+M1211+gear_inertia)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":-486.22278518518522},9,{"$f":"IF(kgcm2,(accel3*gear*(inertia/10/gear^2+M1211+gear_inertia/10)/1000+(torque+IF(accel1>=0,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad,(accel3*gear*(inertia/gear^2+M1211+gear_inertia)/1000+(torque+IF(accel1>=1,IF(AND(speed1=0,speed2=0),0,DryTorq),-DryTorq))/gear)/Wirkungsgrad)","v":404.70045600000003},9,{"$f":"IF(kgcm2,(accel5*gear*(inertia2/10/gear^2+M1211+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel5*gear*(inertia2/gear^2+M1211+gear_inertia)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":-40677.72},7.5,{"$f":"IF(kgcm2,(accel7*gear*(inertia2/10/gear^2+M1211+gear_inertia/10)/1000+(torque2+IF(accel5>=0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad,(accel7*gear*(inertia2/gear^2+M1211+gear_inertia)/1000+(torque2+IF(accel5>0,IF(AND(speed1=0,speed6=0),0,DryTorq2),-DryTorq2))/gear)/Wirkungsgrad)","v":40689.72},9,{"$f":"AH1211/Irms","v":8.9703858824012397E-2},{"$f":"AI1211/Ipeak","v":0.28436665921436588},{"$f":"IF(move1,IF(AccType=1,SQRT((X1211^2*time1+Y1211^2*time2+Z1211^2*time3+AA1211^2*time4)/time)/(C1211/D1211),SQRT((((X1211-Y1211)*2/PI()+Y1211)^2*time1+Y1211^2*time2+((Z1211-AA1211)*2/PI()+AA1211)^2*time3+AA1211^2*time4)/time)/(C1211/D1211)),IF(AccType=1,SQRT((X1211^2*time1+Y1211^2*time2+Z1211^2*time3+AA1211^2*time4+AB1211^2*time5+AC1211^2*time6+AD1211^2*time7+AE1211^2*time8)/time)/(C1211/D1211),SQRT((((X1211-Y1211)*2/PI()+Y1211)^2*time1+Y1211^2*time2+((Z1211-AA1211)*2/PI()+AA1211)^2*time3+AA1211^2*time4+((AB1211-AC1211)*2/PI()+AC1211)^2*time5+AC1211^2*time6+((AD1211-AE1211)*2/PI()+AE1211)^2*time7+AE1211^2*time8)/time)/(C1211/D1211)))","v":2.1528926117762976},{"$f":"IF(move1,MAX(ABS(X1211),ABS(Z1211))/(C1211/D1211),MAX(ABS(X1211),ABS(Z1211),ABS(AB1211),ABS(AD1211))/(C1211/D1211))","v":13.649599642289562},{"$f":"IF(move1,IF(AccType=1,MAX(ABS(X1211),ABS(Z1211))/(C1211/D1211),MAX(ABS((X1211-Y1211)*2/PI()+Y1211),ABS((Z1211-Y1211)*2/PI()+Y1211))/(C1211/D1211)),IF(AccType=1,MAX(ABS(X1211),ABS(Z1211),ABS(AB1211),ABS(AD1211))/(C1211/D1211),MAX(ABS((X1211-Y1211)*2/PI()+Y1211),ABS((Z1211-Y1211)*2/PI()+Y1211),ABS((AB1211-AC1211)*2/PI()+AC1211),ABS((AD1211-AC1211)*2/PI()+AC1211))/(C1211/D1211)))","v":8.5977953509433629},{"$f":"IF((C1211+(E1211-C1211)/G1211*mspeed)<0,\"NA\",U1211*(C1211+(E1211-C1211)/G1211*mspeed)*mspeed/9.55)","v":178.16115732580599},{"$f":"IF(move1,IF(speed1>speed2,AM1211/2*time1/time,AM1211/2*time3/time),(IF(speed1>speed2,MAX(IF(AccType=1,Z1211*-speed/30*PI(),((Z1211-AA1211)*2/PI()+AA1211)*-speed/30*PI()),IF(AccType=1,X1211*-speed/30*PI(),((X1211-Y1211)*2/PI()+Y1211)*-speed/30*PI()),0)/2*time1/time,MAX(IF(AccType=1,Z1211*-speed/30*PI(),((Z1211-AA1211)*2/PI()+AA1211)*-speed/30*PI()),IF(AccType=1,X1211*-speed/30*PI(),((X1211-Y1211)*2/PI()+Y1211)*-speed/30*PI()),0)/2*time3/time)+IF(speed1>speed6,MAX(IF(AccType=1,AD1211*-speed/30*PI(),((AD1211-AE1211)*2/PI()+AE1211)*-speed/30*PI()),IF(AccType=1,AB1211*-speed/30*PI(),((AB1211-AC1211)*2/PI()+AC1211)*-speed/30*PI()),0)/2*time5/time,MAX(IF(AccType=1,AD1211*-speed/30*PI(),((AD1211-AE1211)*2/PI()+AE1211)*-speed/30*PI()),IF(AccType=1,AB1211*-speed/30*PI(),((AB1211-AC1211)*2/PI()+AC1211)*-speed/30*PI()),0)/2*time7/time)))","v":66.660642103566872},{"$f":"IF(move1,MAX(IF(AccType=1,Z1211*-speed/30*PI(),((Z1211-AA1211)*2/PI()+AA1211)*-speed/30*PI()),IF(AccType=1,X1211*-speed/30*PI(),((X1211-Y1211)*2/PI()+Y1211)*-speed/30*PI()),0),MAX(IF(AccType=1,Z1211*-speed/30*PI(),((Z1211-AA1211)*2/PI()+AA1211)*-speed/30*PI()),IF(AccType=1,X1211*-speed/30*PI(),((X1211-Y1211)*2/PI()+Y1211)*-speed/30*PI()),IF(AccType=1,AD1211*-speed/30*PI(),((AD1211-AE1211)*2/PI()+AE1211)*-speed/30*PI()),IF(AccType=1,AB1211*-speed/30*PI(),((AB1211-AC1211)*2/PI()+AC1211)*-speed/30*PI()),0))","v":4083.5815570110967},{"$f":"(L1211^2)/1000000+((K1211/1000)^2*(D1211/C1211*H1211)^2*PI()*PI()*(O1211/2)^2)/1200","v":10.334029821388199},{"$f":"SQRT(3)*L1211*J1211*D1211/C1211*H1211/1000","v":267.83163534448545},{"$f":"0.75*J1211^2*(D1211/C1211*H1211)^2-(UAC_V*0.98)^2","v":-149924.8272924198},{"$f":"-AO1211/2/AN1211+SQRT((AO1211/2/AN1211)^2-AP1211/AN1211)","v":108.18501456669327},{"$f":"(L1211^2)/1000000+((K1211/1000)^2*AV1211^2*PI()*PI()*(O1211/2)^2)/1200","v":5.239968638031379},{"$f":"SQRT(3)*L1211*J1211*AV1211/1000","v":75.825516874116474},{"$f":"0.75*J1211^2*AV1211^2-(UAC_V*0.98)^2","v":-153364.30290187721},{"$f":"-AS1211/2/AR1211+SQRT((AS1211/2/AR1211)^2-AT1211/AR1211)","v":163.99705862597972},{"$f":"D1211+(F1211-D1211)*((0.85*UAC_V-D1211*J1211)/L1211*1000)/G1211","v":31.234219876365337},{"$f":"(L1211^2)/1000000+((K1211/1000)^2*AJ1211^2*PI()*PI()*(O1211/2)^2)/1200","v":4.8297331342920291},{"$f":"SQRT(3)*L1211*J1211*AJ1211/1000","v":20.872372642688209},{"$f":"0.75*J1211^2*AJ1211^2-(UAC_V*0.98)^2","v":-153641.29113551974},{"$f":"IF(((AX1211/2/AW1211)^2-AY1211/AW1211)>0,-AX1211/2/AW1211+SQRT((AX1211/2/AW1211)^2-AY1211/AW1211),-9999)","v":176.21019148343595}]
["KBM","KBMS-163S01-A (240 V)",776,43.2,580.77085597351629,32.086787622846202,165,1966,219,0.37,4.2,1100,1230,325,56,219,219,219,516.8776815648489,9.1463414634146339E-2,7.1208507157037637E-2,0.16998212576768021,0.58138791997039396,-334.18485925925927,{"$f":"(torque+IF(speed2=0,0,IF(speed2>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},281.54973600000005,{"$f":"(torque+IF(speed1=0,0,IF(speed4>0,DryTorq,-DryTorq)))/gear/Wirkungsgrad","v":9},-28111.32,{"$f":"(torque2+IF(speed6=0,0,IF(speed6>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":7.5},28123.32,{"$f":"(torque2+IF(speed1=0,0,IF(speed2>0,DryTorq2,-DryTorq2)))/gear/Wirkungsgrad","v":9},0.12383938543283736,0.38758553264604817,2.9721452503880967,18.604105567010311,11.661676718564975,124.02900755002838,45.593818690076674,2793.0435597550672,2.5725241885138996,77.154378213855807,-152434.08304182507,228.8884452378488,1.2720725501734422,16.467901446960873,-153607.9686408953,341.08431583107301,23.360558558700465,1.2254687470776564,8.2208369472450382,-153650.03674377827,350.75299144667343]
["KBM","KBMS-163S02-A (240 V)",1090,40.6,945.38036196585824,34.756630954627141,110,2915,146,0.50900000000000001,6.3,1645,1720,325,56,146,146,146,898.05029860923003,6.5406976744186052E-2,6.8254858147303227E-2,0.15723813565423631,0.87208187995559083,-458.3491654320988,9,382.12282400000004,9,-38373.879999999997,7.5,38385.879999999997,9,0.11237463482450087,0.35567614901649863,2.6969912357880208,17.072455152791935,10.746846792780378,168.21133742845828,62.798391144427008,3846.9829241808247,5.7231399054328129,157.46440871065298,-151373.27467312798,149.45650791721917,2.9407998340771555,43.925048799963939,-153485.74869854498,221.10915143796859,30.287814773382017,2.7355831858962518,15.585666161478015,-153641.55813511543,234.15808370222149]
["KBM","KBMS-163S03-A (240 V)",1375,38.6,1209.1796801406749,33.402753595046264,80,3930,110,0.64,8.4,2190,1830,325,56,108.18501456669327,110,110,1146.9970601934281,6.1475409836065573E-2,5.7704307216404765E-2,0.1237208104796909,1.1574904952137843,-486.22278518518522,9,404.70045600000003,9,-40677.72,7.5,40689.72,9,8.9703858824012397E-2,0.28436665921436588,2.1528926117762976,13.649599642289562,8.5977953509433629,178.16115732580599,66.660642103566872,4083.5815570110967,10.334029821388199,267.83163534448545,-149924.8272924198,108.18501456669327,5.1852808644107755,71.000905633190328,-153401.22771623125,165.28974737676293,29.246855008582799,4.8297331342920291,20.872372642688209,-153641.29113551974,176.21019148343595]
["KBM","KBMS-260H01-A (400 V)",1932,33.1,1710.4475354640751,28.84397193025422,85,6494,111,1.06,16,3584,5450,565,58,54.516705088836581,96.945501843353469,109.375,1679.3115898933293,2.0642201834862386E-2,0.11648469711972388,0.21612538829764988,1.2257414592844313,-1403.5182716049383,9,1147.7098000000001,9,-116495,7.5,116507,9,0.15584325409062308,0.5009538344345611,3.7402380981749541,24.045784052858934,15.25199104745421,507.17010034806481,193.76381003162436,11869.827473789137,34.764057805170467,732.0953520520244,-143232.67909925466,54.516705088836581,14.317874763451499,189.77190515237746,-152963.08098522181,96.945501843353469,28.840143963831196,13.256970939880198,100.3600884264758,-153467.96840331078,103.87504926842075]
["KBM","KBMS-260H01-A (480 V)",1932,33.1,1680.6761990504149,28.341925784998566,105,6494,134,1.06,16,3584,5450,679,58,54.516705088836581,96.720490843809401,109.375,1700.4937010611836,2.0642201834862386E-2,0.11619180949076607,0.21612538829764988,1.2257414592844313,-1403.5182716049383,9,1147.7098000000001,9,-116495,7.5,116507,9,0.15584325409062308,0.5009538344345611,3.7402380981749541,24.045784052858934,15.25199104745421,507.17010034806481,193.76381003162436,11869.827473789137,34.764057805170467,732.0953520520244,-143232.67909925466,54.516705088836581,14.359490941533707,192.43433970804284,-152943.27571707609,96.720490843809401,29.244761263836768,13.256970939880198,100.3600884264758,-153467.96840331078,103.87504926842075]
["KBM","KBMS-260H02-A (400 V)",2706,31,2428.9938042061262,27.322764951699956,55,9741,74,1.48,24,5380,7860,565,58,32.531595539804037,63.446898902972372,72.862453531598504,2386.4511981812566,1.4312977099236641E-2,0.12056049201267173,0.20677588961510529,1.861020380109677,-2014.2039407407406,9,1642.365192,9,-166970.04,7.5,166982.04,9,0.14929364122143376,0.48072433298659578,3.5830473893144106,23.074767983356598,14.652387508660192,726.59752623167151,278.38221740914327,17053.488429434183,78.559271215097397,1539.012202733609,-133206.16912284453,32.531595539804037,31.92352823683802,377.12100979870769,-152435.60818645751,63.446898902972372,27.344885527522781,29.799769519164133,202.07519858388986,-153311.30322719837,68.41620641790746]
["KBM","KBMS-260H02-A (480 V)",2706,31,2406.2823087173174,27.067292561499631,68,9741,89,1.48,24,5380,7860,679,58,32.531595539804037,63.241336387467889,72.862453531598504,2427.2566568281854,1.4312977099236641E-2,0.11991558544967441,0.20677588961510529,1.861020380109677,-2014.2039407407406,9,1642.365192,9,-166970.04,7.5,166982.04,9,0.14929364122143376,0.48072433298659578,3.5830473893144106,23.074767983356598,14.652387508660192,726.59752623167151,278.38221740914327,17053.488429434183,78.559271215097397,1539.012202733609,-133206.16912284453,32.531595539804037,32.032002700034298,383.92539092926717,-152390.88062457513,63.241336387467889,27.838268336399167,29.799769519164133,202.07519858388986,-153311.30322719837,68.41620641790746]
["KBM","KBMS-260H03-A (400 V)",3444,29.5,3366.1270463935866,28.286781902467116,40,12812,55,1.9,32,7180,10200,565,58,21.740132594661269,45.940391551555592,54.596100278551532,3354.5621505011313,1.1029411764705883E-2,0.11894211192678691,0.20349296377238929,2.5118360625240439,-2607.1518518518515,9,2122.6529999999998,9,-215979,7.5,215991,9,0.14436614692751623,0.46524740871581988,3.4647875262603893,22.331875618359355,14.188900375710247,939.70816053716703,360.54282872175503,22086.586618732697,136.85574434483163,2593.07140327052,-121056.30713575242,21.740132594661269,57.22527223347371,668.70250151465632,-151495.51203662701,45.940391551555592,28.300510867707303,52.978375062432313,335.26437806485961,-153118.91284984202,50.689595699797977]
["KBM","KBMS-260H03-A (480 V)",3444,29.5,3288.7777440509253,27.636787765133825,50,12812,67,1.9,32,7180,10200,679,58,21.740132594661269,46.036809926411763,54.596100278551532,3301.0812501304722,1.1029411764705883E-2,0.1198472002070924,0.20349296377238929,2.5118360625240439,-2607.1518518518515,9,2122.6529999999998,9,-215979,7.5,215991,9,0.14436614692751623,0.46524740871581988,3.4647875262603893,22.331875618359355,14.188900375710247,939.70816053716703,360.54282872175503,22086.586618732697,136.85574434483163,2593.07140327052,-121056.30713575242,21.740132594661269,57.115872100034501,662.22321884636699,-151537.33086539499,46.036809926411763,28.026297732339135,52.978375062432313,335.26437806485961,-153118.91284984202,50.689595699797977]
["KBM","KBMS-260S01-A (240 V)",1932,33.1,1761.3147035503084,29.701765658521222,45,6494,67,1.06,16,3584,5450,325,58,54.516705088836581,67,67,1677.8685586193481,2.0642201834862386E-2,0.11814409859723583,0.21612538829764988,1.9003575294554667,-1403.5182716049383,9,1147.7098000000001,9,-116495,7.5,116507,9,0.15584325409062308,0.5009538344345611,3.7402380981749541,24.045784052858934,15.25199104745421,507.17010034806481,193.76381003162436,11869.827473789137,34.764057805170467,732.0953520520244,-143232.67909925466,54.516705088836581,14.105067112297689,175.52721049961201,-153064.35680603932,98.135153643726284,26.675339620550218,13.256970939880198,100.3600884264758,-153467.96840331078,103.87504926842075]
["KBM","KBMS-260S02-A (240 V)",2706,31,2482.8171122335671,27.928201487441697,28,9741,44,1.48,24,5380,7860,325,58,32.531595539804037,44,44,2355.2840335098908,1.4312977099236641E-2,0.12366375094283437,0.20677588961510529,2.8937262380344606,-2014.2039407407406,9,1642.365192,9,-166970.04,7.5,166982.04,9,0.14929364122143376,0.48072433298659578,3.5830473893144106,23.074767983356598,14.652387508660192,726.59752623167151,278.38221740914327,17053.488429434183,78.559271215097397,1539.012202733609,-133206.16912284453,32.531595539804037,31.434980748370013,344.81523220754104,-152637.05226259361,64.41337476865958,25.002407205830799,29.799769519164133,202.07519858388986,-153311.30322719837,68.41620641790746]
["KBM","KBMS-260S03-A (240 V)",3444,29.5,3317.1240770731874,27.874992244312498,19,12812,33,1.9,32,7180,10200,325,58,21.740132594661269,33,33,3223.6365549165885,1.1029411764705883E-2,0.12272990911982505,0.20349296377238929,3.858301650712614,-2607.1518518518515,9,2122.6529999999998,9,-215979,7.5,215991,9,0.14436614692751623,0.46524740871581988,3.4647875262603893,22.331875618359355,14.188900375710247,939.70816053716703,360.54282872175503,22086.586618732697,136.85574434483163,2593.07140327052,-121056.30713575242,21.740132594661269,56.383905302603416,617.12434165373304,-151817.12937389166,46.705154499549089,26.117644390650447,52.978375062432313,335.26437806485961,-153118.91284984202,50.689595699797977]

{"sheet":"LinMotor","index":4,"n_rows":392,"n_cols":51,"rows_kept":392,"cut":false,"hidden":true,"merged":[[0,0,1,0]]}
["Motor\nLinie","Typ","Fn","In","Fmax","Imax","Vmax","RU-V","LU-V","KE eff","G","UDCmax","PolPitch","Vmax","Vmax","Vmax",null,"Gext/Gmot","Frms","Fpk","v","F (t1)","F (t2)","F (t3)","F (t4)","F (t5)","F (t6)","F (t7)","F (t8)","Irms","Ipeak","Irms","Ipeak","Ipeak","P","PbrRMS","PbrPEAK","Koeff","Koeff","Koeff","nmax","Koeff","Koeff","Koeff","nmax","Koeff","Koeff","Koeff","nmax",null,"KE Peak"]
[null,"Kein Motor","[N]","[A]","[N]","[A] ","[m/s]","[W]","[mH]","[V/m/s]","[kg]","[V]","[mm]","bei F=0","bei Fmax","bei Fn",null," "," "," "," "," "," "," "," "," "," "," "," "," "," "," "," ","trapez"," "," "," ","A","B","C","theo","A","B","C","theo","A","B","C","theo",null,"[V/m/s]"]
["Other","power_linear_test",175.16066937328301,2.86372222365137,404.68872564616998,8.9,"NA",3.8,47,34.699696967550501,2.5,675,32,{"$f":"IFERROR(IF(G3=\"NA\",(UAC_V*0.98)/J3,(IF((UAC_V*0.98)/J3<G3,(UAC_V*0.98)/J3,G3))),0)","v":11.296928626396353},{"$f":"IFERROR(IF(AO3<G3,IF(AO3<0,0,AO3),G3),0)","v":4.8588177741146783},{"$f":"IFERROR(IF(AS3<G3,IF(AS3<0,0,AS3),G3),0)","v":9.3334888176471171},null,{"$f":"IFERROR(IF(move1,Gewicht/K3,MAX(Gewicht,Gewicht2)/K3),0)","v":2},{"$f":"IFERROR(IF(move1,IF(AccType=1,SQRT((V3^2*Ltime1+W3^2*Ltime2+X3^2*Ltime3+Y3^2*Ltime4)/ltime)/C3,SQRT((((V3-W3)*2/PI()+W3)^2*Ltime1+W3^2*Ltime2+((X3-W3)*2/PI()+W3)^2*Ltime3+Y3^2*Ltime4)/ltime)/C3),IF(AccType=1,SQRT((V3^2*Ltime1+W3^2*Ltime2+X3^2*Ltime3+Y3^2*Ltime4+Z3^2*Ltime5+AA3^2*Ltime6+AB3^2*Ltime7+AC3^2*Ltime8)/ltime)/C3,SQRT((((V3-W3)*2/PI()+W3)^2*Ltime1+W3^2*Ltime2+((X3-W3)*2/PI()+W3)^2*Ltime3+Y3^2*Ltime4+((Z3-AA3)*2/PI()+AA3)^2*Ltime5+AA3^2*Ltime6+((AB3-AA3)*2/PI()+AA3)^2*Ltime7+AC3^2*Ltime8)/ltime)/C3)),0)","v":0.86726809642745961},{"$f":"IFERROR( IF(move1,MAX(ABS(V3),ABS(X3))/E3,MAX(ABS(V3),ABS(X3),ABS(Z3),ABS(AB3))/E3),0)","v":0.97037543947628513},{"$f":"IFERROR(IF(AW3>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW3,G3),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW3,G3)),\"NA\"),0)","v":0.13435993963318454},{"$f":"((Gewicht+K3)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":235.62},{"$f":"(Ltorque+IF(Lspeed2=0,0,IF(Lspeed2>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},{"$f":"((Gewicht+K3)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-392.7},{"$f":"(Ltorque+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},{"$f":"((Gewicht2+K3)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},{"$f":"(Ltorque2+IF(Lspeed6=0,0,IF(Lspeed6>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},{"$f":"((Gewicht2+K3)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},{"$f":"(Ltorque2+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},{"$f":"AF3/Irms","v":0.10348395506679731},{"$f":"AG3/Ipeak","v":0.17884818151792384},{"$f":"D3*S3","v":2.4836149216031354},{"$f":"IFERROR(IF(move1,IF(MAX(ABS(V3),ABS(X3))<=C3,MAX(ABS(V3),ABS(X3))/C3*D3,D3+(MAX(ABS(V3),ABS(X3))-C3)/(E3-C3)*(F3-D3)),IF(MAX(ABS(V3),ABS(X3),ABS(Z3),ABS(AB3))<=C3,MAX(ABS(V3),ABS(X3),ABS(Z3),ABS(AB3))/C3*D3,D3+(MAX(ABS(V3),ABS(X3),ABS(Z3),ABS(AB3))-C3)/(E3-C3)*(F3-D3))),0)","v":8.5847127128603447},{"$f":"IFERROR(IF(AccType=1,IF(move1,IF(MAX(ABS(V3),ABS(X3))<=C3,MAX(ABS(V3),ABS(X3))/C3*D3,D3+(MAX(ABS(V3),ABS(X3))-C3)/(E3-C3)*(F3-D3)),IF(MAX(ABS(V3),ABS(X3),ABS(Z3),ABS(AB3))<=C3,MAX(ABS(V3),ABS(X3),ABS(Z3),ABS(AB3))/C3*D3,D3+(MAX(ABS(V3),ABS(X3),ABS(Z3),ABS(AB3))-C3)/(E3-C3)*(F3-D3))),IF(move1,IF(MAX(ABS((V3-W3)*2/PI()+W3),ABS((X3-W3)*2/PI()+W3))<=C3,MAX(ABS((V3-W3)*2/PI()+W3),ABS((X3-W3)*2/PI()+W3))/C3*D3,D3+(MAX(ABS((V3-W3)*2/PI()+W3),ABS((X3-W3)*2/PI()+W3))-C3)/(E3-C3)*(F3-D3)),IF(MAX(ABS((V3-W3)*2/PI()+W3),ABS((X3-W3)*2/PI()+W3),ABS((Z3-AA3)*2/PI()+AA3),ABS((AB3-AA3)*2/PI()+AA3))<=C3,MAX(ABS((V3-W3)*2/PI()+W3),ABS((X3-W3)*2/PI()+W3),ABS((Z3-AA3)*2/PI()+AA3),ABS((AB3-AA3)*2/PI()+AA3))/C3*D3,D3+(MAX(ABS((V3-W3)*2/PI()+W3),ABS((X3-W3)*2/PI()+W3),ABS((Z3-AA3)*2/PI()+AA3),ABS((AB3-AA3)*2/PI()+AA3))-C3)/(E3-C3)*(F3-D3)))),0)","v":4.8319108819588612},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V3)+Ltime2*ABS(Lspeed2)*ABS(W3)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X3)+Ltime4*ABS(Lspeed1)*ABS(Y3))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V3)+Ltime2*ABS(Lspeed2)*ABS(W3)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X3)+Ltime4*ABS(Lspeed1)*ABS(Y3)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z3)+Ltime6*ABS(Lspeed6)*ABS(AA3)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB3)+Ltime8*ABS(Lspeed1)*ABS(AC3))/ltime)","v":181.24615384615385},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK3/2*Ltime1/ltime,AK3/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X3*-ABS(Lspeed2-Lspeed1),((X3-Y3)*2/PI()+Y3)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V3*-ABS(Lspeed2-Lspeed1),((V3-W3)*2/PI()+W3)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X3*-ABS(Lspeed2-Lspeed1),((X3-Y3)*2/PI()+Y3)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V3*-ABS(Lspeed2-Lspeed1),((V3-W3)*2/PI()+W3)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB3*-ABS(Lspeed6-Lspeed1),((AB3-AC3)*2/PI()+AB3)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z3*-ABS(Lspeed6-Lspeed1),((Z3-AA3)*2/PI()+AA3)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB3*-ABS(Lspeed6-Lspeed1),((AB3-AC3)*2/PI()+AB3)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z3*-ABS(Lspeed6-Lspeed1),((Z3-AA3)*2/PI()+AA3)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":28.846221301009521},{"$f":"IF(move1,MAX(IF(AccType=1,X3*-ABS(Lspeed2-Lspeed1),((X3-Y3)*2/PI()+Y3)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V3*-ABS(Lspeed2-Lspeed1),((V3-W3)*2/PI()+W3)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X3*-ABS(Lspeed2-Lspeed1),((X3-Y3)*2/PI()+Y3)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V3*-ABS(Lspeed2-Lspeed1),((V3-W3)*2/PI()+W3)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB3*-ABS(Lspeed6-Lspeed1),((AB3-AC3)*2/PI()+AB3)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z3*-ABS(Lspeed6-Lspeed1),((Z3-AA3)*2/PI()+AA3)*-ABS(Lspeed6-Lspeed1)),0))","v":250.00058460874919},{"$f":"IFERROR((J3^2)+3*(I3/1000)^2*(F3/2)^2*(2000*PI()/M3)^2,0)","v":6263.4428302573924},{"$f":"SQRT(3)*H3*F3/2*J3","v":1016.3187012017462},{"$f":"3*F3^2*H3^2/4-(UAC_V*0.98)^2","v":-152806.1557},{"$f":"IFERROR(-AM3/2/AL3+SQRT((AM3/2/AL3)^2-AN3/AL3),0)","v":4.8588177741146783},{"$f":"IFERROR((J3^2)+3*(I3/1000)^2*(D3/2)^2*(2000*PI()/M3)^2,0)","v":1727.8847032599797},{"$f":"SQRT(3)*H3*D3/2*J3","v":327.01735403864456},{"$f":"3*D3^2*H3^2/4-(UAC_V*0.98)^2","v":-153575.18419912903},{"$f":"IFERROR(-AQ3/2/AP3+SQRT((AQ3/2/AP3)^2-AR3/AP3),0)","v":9.3334888176471171},{"$f":"IFERROR((J3^2)+3*(I3/1000)^2*(AH3/2)^2*(2000*PI()/M3)^2,0)","v":2695.3331650561522},{"$f":"SQRT(3)*H3*AH3/2*J3","v":551.77094290730486},{"$f":"3*AH3^2*H3^2/4-(UAC_V*0.98)^2","v":-153411.148061188},{"$f":"IFERROR(IF((AU3/2/AT3)^2-AV3/AT3>=0,-AU3/2/AT3+SQRT((AU3/2/AT3)^2-AV3/AT3),-9999),0)","v":7.4426946211057814},null,36.299999999999997]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,{"$f":"IFERROR(IF(AO4<G4,IF(AO4<0,0,AO4),G4),0)","v":0},{"$f":"IFERROR(IF(AS4<G4,IF(AS4<0,0,AS4),G4),0)","v":0},null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,{"$f":"IFERROR((J4^2)+3*(I4/1000)^2*(F4/2)^2*(2000*PI()/M4)^2,0)","v":0},0,-153664,{"$f":"IFERROR(-AM4/2/AL4+SQRT((AM4/2/AL4)^2-AN4/AL4),0)","v":0},{"$f":"IFERROR((J4^2)+3*(I4/1000)^2*(D4/2)^2*(2000*PI()/M4)^2,0)","v":0},0,-153664,{"$f":"IFERROR(-AQ4/2/AP4+SQRT((AQ4/2/AP4)^2-AR4/AP4),0)","v":0},{"$f":"IFERROR((J4^2)+3*(I4/1000)^2*(AH4/2)^2*(2000*PI()/M4)^2,0)","v":0},0,-153664,{"$f":"IFERROR(IF((AU4/2/AT4)^2-AV4/AT4>=0,-AU4/2/AT4+SQRT((AU4/2/AT4)^2-AV4/AT4),-9999),0)","v":0},null,36.4]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-153664,0,0,0,-153664,0,0,0,-153664,0,null,72.8]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-153664,0,0,0,-153664,0,0,0,-153664,0,null,30.9]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-153664,0,0,0,-153664,0,0,0,-153664,0,null,51.4]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-153664,0,0,0,-153664,0,0,0,-153664,0,null,61.7]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-153664,0,0,0,-153664,0,0,0,-153664,0,null,103]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-153664,0,0,0,-153664,0,0,0,-153664,0,null,103]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-153664,0,0,0,-153664,0,0,0,-153664,0,null,154]
["Other",null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,null,0,0,0,"NA",157.08000000000001,0,-261.8,0,0,0,0,0,0,0,0,0,0,120.83076923076923,19.230814200673017,166.6670564058328,0,0,-153664,0,0,0,-153664,0,0,0,-153664,0,null,154]
["Leerzeile"]
["ALT","L1S040P 2608-GL-X0",110,1.8,600,15,"NA",11.1,25,30.1,1.8,330,24,{"$f":"IF(G14=\"NA\",(UAC_V*0.98)/J14,(IF((UAC_V*0.98)/J14<G14,(UAC_V*0.98)/J14,G14)))","v":13.023255813953488},{"$f":"IF(AO14<G14,IF(AO14<0,0,AO14),G14)","v":3.7835541351793798},{"$f":"IF(AS14<G14,IF(AS14<0,0,AS14),G14)","v":12.066843788672312},null,{"$f":"IF(move1,Gewicht/K14,MAX(Gewicht,Gewicht2)/K14)","v":2.7777777777777777},{"$f":"IF(move1,IF(AccType=1,SQRT((V14^2*Ltime1+W14^2*Ltime2+X14^2*Ltime3+Y14^2*Ltime4)/ltime)/C14,SQRT((((V14-W14)*2/PI()+W14)^2*Ltime1+W14^2*Ltime2+((X14-W14)*2/PI()+W14)^2*Ltime3+Y14^2*Ltime4)/ltime)/C14),IF(AccType=1,SQRT((V14^2*Ltime1+W14^2*Ltime2+X14^2*Ltime3+Y14^2*Ltime4+Z14^2*Ltime5+AA14^2*Ltime6+AB14^2*Ltime7+AC14^2*Ltime8)/ltime)/C14,SQRT((((V14-W14)*2/PI()+W14)^2*Ltime1+W14^2*Ltime2+((X14-W14)*2/PI()+W14)^2*Ltime3+Y14^2*Ltime4+((Z14-AA14)*2/PI()+AA14)^2*Ltime5+AA14^2*Ltime6+((AB14-AA14)*2/PI()+AA14)^2*Ltime7+AC14^2*Ltime8)/ltime)/C14))","v":1.2521170545636631},{"$f":" IF(move1,MAX(ABS(V14),ABS(X14))/E14,MAX(ABS(V14),ABS(X14),ABS(Z14),ABS(AB14))/E14)","v":0.59341333333333335},{"$f":"IF(AW14>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW14,G14),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW14,G14)),\"NA\")","v":0.11050875778057588},213.62879999999998,0,-356.048,0,0,0,0,0,9.3908779092274741E-2,0.17558816326530613,2.2538106982145938,{"$f":"IF(move1,IF(MAX(ABS(V14),ABS(X14))<=C14,MAX(ABS(V14),ABS(X14))/C14*D14,D14+(MAX(ABS(V14),ABS(X14))-C14)/(E14-C14)*(F14-D14)),IF(MAX(ABS(V14),ABS(X14),ABS(Z14),ABS(AB14))<=C14,MAX(ABS(V14),ABS(X14),ABS(Z14),ABS(AB14))/C14*D14,D14+(MAX(ABS(V14),ABS(X14),ABS(Z14),ABS(AB14))-C14)/(E14-C14)*(F14-D14)))","v":8.4282318367346942},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V14),ABS(X14))<=C14,MAX(ABS(V14),ABS(X14))/C14*D14,D14+(MAX(ABS(V14),ABS(X14))-C14)/(E14-C14)*(F14-D14)),IF(MAX(ABS(V14),ABS(X14),ABS(Z14),ABS(AB14))<=C14,MAX(ABS(V14),ABS(X14),ABS(Z14),ABS(AB14))/C14*D14,D14+(MAX(ABS(V14),ABS(X14),ABS(Z14),ABS(AB14))-C14)/(E14-C14)*(F14-D14))),IF(move1,IF(MAX(ABS((V14-W14)*2/PI()+W14),ABS((X14-W14)*2/PI()+W14))<=C14,MAX(ABS((V14-W14)*2/PI()+W14),ABS((X14-W14)*2/PI()+W14))/C14*D14,D14+(MAX(ABS((V14-W14)*2/PI()+W14),ABS((X14-W14)*2/PI()+W14))-C14)/(E14-C14)*(F14-D14)),IF(MAX(ABS((V14-W14)*2/PI()+W14),ABS((X14-W14)*2/PI()+W14),ABS((Z14-AA14)*2/PI()+AA14),ABS((AB14-AA14)*2/PI()+AA14))<=C14,MAX(ABS((V14-W14)*2/PI()+W14),ABS((X14-W14)*2/PI()+W14),ABS((Z14-AA14)*2/PI()+AA14),ABS((AB14-AA14)*2/PI()+AA14))/C14*D14,D14+(MAX(ABS((V14-W14)*2/PI()+W14),ABS((X14-W14)*2/PI()+W14),ABS((Z14-AA14)*2/PI()+AA14),ABS((AB14-AA14)*2/PI()+AA14))-C14)/(E14-C14)*(F14-D14))))","v":4.9428714216275722},164.32984615384612,26.153907312915297,226.6671967119326,{"$f":"(J14^2)+3*(I14/1000)^2*(F14/2)^2*(2000*PI()/M14)^2","v":8134.7241609541206},4340.2162148762818,-132872.3125,{"$f":"-AM14/2/AL14+SQRT((AM14/2/AL14)^2-AN14/AL14)","v":3.7835541351793798},{"$f":"(J14^2)+3*(I14/1000)^2*(D14/2)^2*(2000*PI()/M14)^2","v":1010.1034839177395},520.82594578515386,-153364.59969999999,{"$f":"-AQ14/2/AP14+SQRT((AQ14/2/AP14)^2-AR14/AP14)","v":12.066843788672312},{"$f":"(J14^2)+3*(I14/1000)^2*(AH14/2)^2*(2000*PI()/M14)^2","v":1690.9512647063507},1430.2087128131045,-151406.3020030612,{"$f":"IF((AU14/2/AT14)^2-AV14/AT14>=0,-AU14/2/AT14+SQRT((AU14/2/AT14)^2-AV14/AT14),-9999)","v":9.0490565642370289},null,30.1]
["ALT","L1S050P 1708-KL-X0",80,1,460,7,"NA",23.5,57,41.5,1.3,330,24,9.4457831325301207,3.3829820723509618,8.7857036548783594,null,3.8461538461538458,1.5950682331114312,0.7171043478260869,0.15679352071561398,197.92079999999999,0,-329.86799999999999,0,0,0,0,0,6.6461176379642967E-2,0.10302675438596491,1.5950682331114312,4.9452842105263155,3.0526393327055157,152.24676923076922,24.230825892847999,210.00049107134933,9905.8483867595151,5912.138925285416,-133368.8125,3.3829820723509618,1889.2622119746841,844.59127504077378,-153249.8125,8.7857036548783594,3278.5711501534888,2578.2325462493682,-149804.34950643664,6.3778145642495092,null,41.5]
["ALT","L1S050P 2608-GL-X0",130,2,725,17,"NA",9.4,23,32.6,2,330,24,12.024539877300613,3.6383276534300526,11.21856396331043,null,2.5,1.090644945717218,0.50554482758620689,0.10785680641963592,219.91200000000001,0,-366.52,0,0,0,0,0,9.0887078809768165E-2,0.16588935574229691,2.1812898914344361,7.9626890756302515,4.605055772306704,169.16307692307691,26.92313988094222,233.33387896816592,8921.4839085569893,4511.5420205069577,-134511.97,3.6383276534300526,1171.5312651703389,530.76964947140675,-153398.92000000001,11.21856396331043,1639.4255101476365,1222.1119190317538,-152258.6426826005,9.271552099450485,null,32.6]
["ALT","L1S075P 3208-KL-X0",240,2.4,1400,22,"NA",9.1,25.5,47.5,3.5,330,24,8.2526315789473692,2.3756697090428136,7.7310250537002858,null,1.4285714285714286,0.71735872917709864,0.31790000000000002,0.13382526428992675,267.036,0,-445.06,0,0,0,0,0,7.1735872917709859E-2,0.12218347701149425,1.7216609500250366,5.8648068965517242,3.1321951029675419,205.41230769230768,32.692384141144124,283.33399588991574,18434.227951641893,8235.4685772881185,-123603.97,2.3756697090428136,2448.7813078542504,898.41475388597644,-153306.26079999999,7.7310250537002858,2584.1764820604244,1172.5042885647688,-153054.68529342813,7.4724306004996368,null,47.5]
["ALT","L1S080P 4111-IL-X0",450,4.5,2400,31,"NA",4,27,51.1,13.2,330,24,7.6712328767123283,1.8485951015631727,6.6300598701857547,null,0.37878787878787878,0.81919553700537717,0.39706333333333332,0.17062396519838693,571.77120000000002,0,-952.952,0,0,0,0,0,0.15359916318850822,0.23614559829059831,3.6863799165241975,11.334988717948718,6.6290791081572475,439.82400000000001,70.000163690449781,606.66808531723143,38623.39169618109,5487.483368539717,-142132,1.8485951015631727,3370.0514977603198,796.57016640092661,-153421,6.6300598701857547,4257.9781107800572,1173.4503662821612,-153136.66372213353,5.8608414054689542,null,51.1]
["ALT","L1S120P 4711-IL-X0",1000,10.4,4200,50,"NA",2.73,20.3,55,21.5,330,24,7.127272727272727,1.522626160355518,5.2400672954268259,null,0.23255813953488372,0.536753119713688,0.33036666666666664,0.18118869958685505,832.524,0,-1387.54,0,0,0,0,0,0.23259301854259815,0.31657932291666668,5.5822324450223553,15.195807500000001,9.1866881490895036,640.40307692307692,101.92331526356698,883.33539895091383,55982.88121933482,6501.6857189116727,-139689.8125,1.522626160355518,5316.1697730733022,1352.3506295336281,-153059.42075200001,5.2400672954268259,4812.7572201240218,1194.5791828606068,-153192.25804161193,5.5191079922765143,null,55]
["ALT","L1S160P 5611-IL-X0",1750,16.2,6550,84,"NA",1.36,11.6,56.6,32.200000000000003,330,24,6.925795053003533,1.6102683790114463,5.4201998381609853,null,0.15527950310559005,0.43055991489701767,0.29737282442748092,0.16625220400947788,1168.6752000000001,0,-1947.7920000000001,0,0,0,0,0,0.29062794255548691,0.39570441666666673,6.9750706213316862,18.993812000000002,11.478883985418411,898.9809230769232,143.07725765300725,1240.0028996593962,52009.543331738962,5599.70640446372,-143875.91680000001,1.6102683790114463,5018.8437677978418,1079.9433780037173,-153299.94323199999,5.4201998381609853,4114.9700817530502,765.21881153861329,-153481.21590058168,6.0149578524865213,null,56.6]
["ALT","L1S200P 7411-IL-X0",2500,23,10900,130,"NA",0.82,7.5,59,48,330,24,6.6440677966101696,1.613920998077514,5.4377164567820548,null,0.10416666666666667,0.42940249577095035,0.25459449541284401,0.16851003043912563,1665.048,0,-2775.08,0,0,0,0,0,0.41151072511382741,0.55216656746031745,9.8762574027318575,26.503995238095236,16.253371340696813,1280.8061538461538,203.84663052713395,1766.6707979018277,52347.10772804985,5446.7801745618472,-145141.33000000002,1.613920998077514,5010.5959164578917,963.66110780709619,-153397.22529999999,5.4377164567820548,4244.8497820722996,680.98877529460856,-153530.77802008696,5.9343648410368708,null,59]
["ICH","ICH11-030-A1",175.16066937328333,2.8637222236513655,404.68872564617027,8.9,"NA",3.8,47,34.699696967550494,2.5,675,32,11.296928626396356,4.8588177741146792,9.3334888176471242,null,2,0.86726809642745806,0.97037543947628446,0.13435993963318435,235.62,0,-392.7,0,0,0,0,0,{"$f":"AF22/Irms","v":0.10348395506679696},{"$f":"AG22/Ipeak","v":0.1788481815179237},2.4836149216031269,8.5847127128603375,4.8319108819588505,{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V22)+Ltime2*ABS(Lspeed2)*ABS(W22)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X22)+Ltime4*ABS(Lspeed1)*ABS(Y22))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V22)+Ltime2*ABS(Lspeed2)*ABS(W22)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X22)+Ltime4*ABS(Lspeed1)*ABS(Y22)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z22)+Ltime6*ABS(Lspeed6)*ABS(AA22)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB22)+Ltime8*ABS(Lspeed1)*ABS(AC22))/ltime)","v":181.24615384615385},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK22/2*Ltime1/ltime,AK22/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X22*-ABS(Lspeed2-Lspeed1),((X22-Y22)*2/PI()+Y22)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V22*-ABS(Lspeed2-Lspeed1),((V22-W22)*2/PI()+W22)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X22*-ABS(Lspeed2-Lspeed1),((X22-Y22)*2/PI()+Y22)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V22*-ABS(Lspeed2-Lspeed1),((V22-W22)*2/PI()+W22)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB22*-ABS(Lspeed6-Lspeed1),((AB22-AC22)*2/PI()+AB22)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z22*-ABS(Lspeed6-Lspeed1),((Z22-AA22)*2/PI()+AA22)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB22*-ABS(Lspeed6-Lspeed1),((AB22-AC22)*2/PI()+AB22)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z22*-ABS(Lspeed6-Lspeed1),((Z22-AA22)*2/PI()+AA22)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":28.846221301009521},{"$f":"IF(move1,MAX(IF(AccType=1,X22*-ABS(Lspeed2-Lspeed1),((X22-Y22)*2/PI()+Y22)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V22*-ABS(Lspeed2-Lspeed1),((V22-W22)*2/PI()+W22)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X22*-ABS(Lspeed2-Lspeed1),((X22-Y22)*2/PI()+Y22)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V22*-ABS(Lspeed2-Lspeed1),((V22-W22)*2/PI()+W22)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB22*-ABS(Lspeed6-Lspeed1),((AB22-AC22)*2/PI()+AB22)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z22*-ABS(Lspeed6-Lspeed1),((Z22-AA22)*2/PI()+AA22)*-ABS(Lspeed6-Lspeed1)),0))","v":250.00058460874919},6263.4428302573915,1016.318701201746,-152806.1557,{"$f":"-AM22/2/AL22+SQRT((AM22/2/AL22)^2-AN22/AL22)","v":4.8588177741146792},1727.8847032599774,327.01735403864399,-153575.18419912903,{"$f":"-AQ22/2/AP22+SQRT((AQ22/2/AP22)^2-AR22/AP22)","v":9.3334888176471242},2695.3331650561454,551.77094290730361,-153411.148061188,{"$f":"IF((AU22/2/AT22)^2-AV22/AT22>=0,-AU22/2/AT22+SQRT((AU22/2/AT22)^2-AV22/AT22),-9999)","v":7.4426946211057921},null,49.072782061746295]
["ICH","ICH11-030-A5",175.16066937328333,4.9601123901282884,404.68872564617027,15.5,"NA",1.3,16,20.033879385013719,2.5,675,32,{"$f":"IF(G23=\"NA\",(UAC_V*0.98)/J23,(IF((UAC_V*0.98)/J23<G23,(UAC_V*0.98)/J23,G23)))","v":19.566854350397776},{"$f":"IF(AO23<G23,IF(AO23<0,0,AO23),G23)","v":8.3080933178235448},{"$f":"IF(AS23<G23,IF(AS23<0,0,AS23),G23)","v":16.131199096642032},null,{"$f":"IF(move1,Gewicht/K23,MAX(Gewicht,Gewicht2)/K23)","v":2},{"$f":"IF(move1,IF(AccType=1,SQRT((V23^2*Ltime1+W23^2*Ltime2+X23^2*Ltime3+Y23^2*Ltime4)/ltime)/C23,SQRT((((V23-W23)*2/PI()+W23)^2*Ltime1+W23^2*Ltime2+((X23-W23)*2/PI()+W23)^2*Ltime3+Y23^2*Ltime4)/ltime)/C23),IF(AccType=1,SQRT((V23^2*Ltime1+W23^2*Ltime2+X23^2*Ltime3+Y23^2*Ltime4+Z23^2*Ltime5+AA23^2*Ltime6+AB23^2*Ltime7+AC23^2*Ltime8)/ltime)/C23,SQRT((((V23-W23)*2/PI()+W23)^2*Ltime1+W23^2*Ltime2+((X23-W23)*2/PI()+W23)^2*Ltime3+Y23^2*Ltime4+((Z23-AA23)*2/PI()+AA23)^2*Ltime5+AA23^2*Ltime6+((AB23-AA23)*2/PI()+AA23)^2*Ltime7+AC23^2*Ltime8)/ltime)/C23))","v":0.86726809642745806},{"$f":" IF(move1,MAX(ABS(V23),ABS(X23))/E23,MAX(ABS(V23),ABS(X23),ABS(Z23),ABS(AB23))/E23)","v":0.97037543947628446},{"$f":"IF(AW23>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW23,G23),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW23,G23)),\"NA\")","v":7.8154487733728517E-2},{"$f":"((Gewicht+K23)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":235.62},0,{"$f":"((Gewicht+K23)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-392.7},0,{"$f":"((Gewicht2+K23)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K23)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,0.17923946794386705,0.3114474967907998,{"$f":"D23*S23","v":4.3017472306528095},{"$f":"IF(move1,IF(MAX(ABS(V23),ABS(X23))<=C23,MAX(ABS(V23),ABS(X23))/C23*D23,D23+(MAX(ABS(V23),ABS(X23))-C23)/(E23-C23)*(F23-D23)),IF(MAX(ABS(V23),ABS(X23),ABS(Z23),ABS(AB23))<=C23,MAX(ABS(V23),ABS(X23),ABS(Z23),ABS(AB23))/C23*D23,D23+(MAX(ABS(V23),ABS(X23),ABS(Z23),ABS(AB23))-C23)/(E23-C23)*(F23-D23)))","v":14.94947984595839},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V23),ABS(X23))<=C23,MAX(ABS(V23),ABS(X23))/C23*D23,D23+(MAX(ABS(V23),ABS(X23))-C23)/(E23-C23)*(F23-D23)),IF(MAX(ABS(V23),ABS(X23),ABS(Z23),ABS(AB23))<=C23,MAX(ABS(V23),ABS(X23),ABS(Z23),ABS(AB23))/C23*D23,D23+(MAX(ABS(V23),ABS(X23),ABS(Z23),ABS(AB23))-C23)/(E23-C23)*(F23-D23))),IF(move1,IF(MAX(ABS((V23-W23)*2/PI()+W23),ABS((X23-W23)*2/PI()+W23))<=C23,MAX(ABS((V23-W23)*2/PI()+W23),ABS((X23-W23)*2/PI()+W23))/C23*D23,D23+(MAX(ABS((V23-W23)*2/PI()+W23),ABS((X23-W23)*2/PI()+W23))-C23)/(E23-C23)*(F23-D23)),IF(MAX(ABS((V23-W23)*2/PI()+W23),ABS((X23-W23)*2/PI()+W23),ABS((Z23-AA23)*2/PI()+AA23),ABS((AB23-AA23)*2/PI()+AA23))<=C23,MAX(ABS((V23-W23)*2/PI()+W23),ABS((X23-W23)*2/PI()+W23),ABS((Z23-AA23)*2/PI()+AA23),ABS((AB23-AA23)*2/PI()+AA23))/C23*D23,D23+(MAX(ABS((V23-W23)*2/PI()+W23),ABS((X23-W23)*2/PI()+W23),ABS((Z23-AA23)*2/PI()+AA23),ABS((AB23-AA23)*2/PI()+AA23))-C23)/(E23-C23)*(F23-D23))))","v":8.3967480159548877},181.24615384615385,28.846221301009521,250.00058460874919,{"$f":"(J23^2)+3*(I23/1000)^2*(F23/2)^2*(2000*PI()/M23)^2","v":2179.7356662345665},{"$f":"SQRT(3)*H23*F23/2*J23","v":349.5994469480712},{"$f":"3*F23^2*H23^2/4-(UAC_V*0.98)^2","v":-153359.483125},8.3080933178235448,{"$f":"(J23^2)+3*(I23/1000)^2*(D23/2)^2*(2000*PI()/M23)^2","v":583.47062082317848},{"$f":"SQRT(3)*H23*D23/2*J23","v":111.87435796058872},{"$f":"3*D23^2*H23^2/4-(UAC_V*0.98)^2","v":-153632.81605883548},16.131199096642032,{"$f":"(J23^2)+3*(I23/1000)^2*(AH23/2)^2*(2000*PI()/M23)^2","v":923.25145937003572},{"$f":"SQRT(3)*H23*AH23/2*J23","v":189.38699758323503},{"$f":"3*AH23^2*H23^2/4-(UAC_V*0.98)^2","v":-153574.63443434393},12.795170552547015,null,28.332183933233065]
["ICH","ICH11-050-A1",298.57480806320996,2.9348587565849433,674.48120941028378,8.9,"NA",5.0999999999999996,78,57.714632204180219,3.5,675,32,6.7920384316614912,2.9032910106585463,5.5512444512051191,null,1.4285714285714286,0.57662632731578334,0.65985529884387351,0.17721885386201372,267.036,0,-445.06,0,0,0,0,0,7.0513201083339264E-2,0.10957055214502472,1.6923168260001424,5.2593865029611866,2.7850482908111887,205.41230769230768,32.692384141144124,283.33399588991574,17265.44258576358,2268.6983063372681,-152118.810925,2.9032910106585463,4846.2300492097247,748.12461689925408,-153495.97417906908,5.5512444512051191,4695.4855843492178,709.93644274503902,-153512.69019364321,5.6427404771425778,null,81.620815610526378]
["ICH","ICH11-050-A5",298.57480806320996,5.083324479443541,674.48120941028378,15.5,"NA",1.7,26,33.321558439263704,3.5,675,32,11.764155650598132,5.0706069135537497,9.6744866267149785,null,1.4285714285714286,0.57662632731578334,0.65985529884387351,0.10171356053559229,267.036,0,-445.06,0,0,0,0,0,0.12213244688066438,0.1904697836462412,2.9311787251359451,9.1425496150195773,4.8238451412178396,205.41230769230768,32.692384141144124,283.33399588991574,5806.3592094868563,760.39027929007466,-153143.25812499999,5.0706069135537497,1615.410016403242,249.37487229975144,-153607.99139302303,9.6744866267149785,1565.1618614497397,236.64548091501308,-153613.56339788108,9.8315307687028941,null,47.12379986421422]
["ICH","ICH11-075-A1",454.73089841680786,2.9839137873774302,1011.7218141154258,8.9,"NA",6.7,117,86.454612708295386,4.8,675,32,4.534171025930549,1.9153938265145567,3.6667296715587301,null,1.0416666666666667,0.43651614792753829,0.50718289636627134,0.24957182263617905,307.8768,0,-513.12800000000004,0,0,0,0,0,5.4271939675577807E-2,7.5087069934995573E-2,1.3025265522138674,3.6041793568797877,2.1435698636604563,236.8283076923077,37.692395833319111,326.6674305554323,38826.943642965867,4464.6108531582267,-150997.19732499999,1.9153938265145567,10998.638704487381,1496.8554921363757,-153364.23328336855,3.6667296715587301,9293.1293122144234,1075.303963797907,-153509.30148165696,4.0068625914463931,null,122.26528582178425]
["ICH","ICH11-075-A5",454.73089841680786,5.1682902851429846,1011.7218141154258,15.5,"NA",2.2000000000000002,39,49.914593919819197,4.8,675,32,7.8534145871184107,3.3647564317014305,6.405340105348853,null,1.0416666666666667,0.43651614792753829,0.50718289636627134,0.14315936267833529,307.8768,0,-513.12800000000004,0,0,0,0,0,9.4001756943413908E-2,0.1302397303575262,2.2560421666419339,6.2515070571612572,3.7127719134334014,236.8283076923077,37.692395833319111,326.6674305554323,13057.54082967803,1474.0511466764369,-152791.89249999999,3.3647564317014305,3666.2129014957954,491.50478846269067,-153567.03825516845,6.405340105348853,3097.7097707381431,353.08488363513379,-153613.9616287293,6.9852224911541381,null,70.589895681753688]
["ICH","ICH11-100-A1",611.81557163638524,3.0134151426335043,1348.9624188205676,8.9,"NA",8.3000000000000007,156,115.18118325320502,6.1,675,32,3.4033336776742327,1.4198392943979277,2.7289594022551755,null,0.81967213114754101,0.36747784080949153,0.43084669512747031,0.32379069199069488,348.7176,0,-581.19600000000003,0,0,0,0,0,4.6140137086566085E-2,5.9637553524834484E-2,1.107363290077586,2.8626025691920551,1.8223893959778996,268.2443076923077,42.69240752549409,370.00086522094881,69004.560236807534,7368.5199964111671,-149571.41732499999,1.4198392943979277,19656.518331788568,2494.8774984250767,-153194.8244403119,2.7289594022551755,15603.672081840174,1508.7991803944744,-153492.4069050345,3.0884149073338341,null,162.89079148686278]
["ICH","ICH11-100-A5",611.81557163638524,5.2193881313386443,1348.9624188205676,15.5,"NA",2.8,52,66.49988715681755,6.1,675,32,5.8947468448420111,2.5081112059477291,4.7764399151095871,null,0.81967213114754101,0.36747784080949153,0.43084669512747031,0.18567770490653313,348.7176,0,-581.19600000000003,0,0,0,0,0,7.9917061702125494E-2,0.1032952727441217,1.9180094808510117,4.9581730917178417,3.1564710250084795,268.2443076923077,42.69240752549409,370.00086522094881,23206.366802531826,2499.4316765945491,-152251.32999999999,2.5081112059477291,6552.1727772628574,841.64542115544771,-153503.81696670252,4.7764399151095871,5201.22402728006,508.99249459090703,-153605.41574112949,5.3856762205423765,null,94.045042313451447]
["ICH","ICH11-150-A1",927.18464906955387,6.0944012777031107,2023.4436282308516,17.899999999999999,"NA",2.9,59,86.308816616386423,8.6,675,32,4.5418303177797901,1.9061709884525577,3.6447043848081058,null,0.58139534883720934,0.29709912937022914,0.35192282605006581,0.23516343766564426,427.25759999999997,0,-712.096,0,0,0,0,0,7.5443388068266934E-2,9.7512911276679048E-2,1.8106413136384063,4.6806197412805943,2.9797750742332596,328.65969230769224,52.307814625830595,453.33439342386521,39699.316510951685,3880.0455370404484,-151643.01392500001,1.9061709884525577,11187.623803502884,1321.0365630438862,-153429.72855736589,3.6447043848081058,8342.9123911101942,645.90295967391796,-153607.99533224775,4.2523617188391398,null,122.05909901126559]
["ICH","ICH11-150-A5",927.18464906955387,10.555812654694471,2023.4436282308516,30.9,"NA",1,20,49.830418506908735,8.6,675,32,7.8666808697512982,3.3137180766024117,6.3209644616414025,null,0.58139534883720934,0.29709912937022914,0.35192282605006581,0.13550944772354268,427.25759999999997,0,-712.096,0,0,0,0,0,0.13067178122937392,0.16889731672516425,3.1361227495049744,8.1070712028078837,5.1611218236993288,328.65969230769224,52.307814625830595,453.33439342386521,13526.348317406637,1333.4712167231698,-152947.89249999999,3.3137180766024117,3771.8078603226631,455.52984932547804,-153580.43111439925,6.3209644616414025,2791.1546874208452,222.72515850824755,-153644.0221161407,7.3795592617286223,null,70.470853671197361]
["ICH","ICH11-200-A1",1250.5593222258879,10.578973306845628,2697.9248376411351,30.6,"NA",1.2,27,67.062656446351482,11.2,675,32,5.8452799333052159,2.4661452781576672,4.6787690728351414,null,0.44642857142857145,0.2623852514697389,0.31440164239031615,0.18030132312940497,508.93919999999997,0,-848.23199999999997,0,0,0,0,0,0.11565694047534773,0.149490170893432,2.7757665714083455,7.1755282028847365,4.5680831311376409,391.49169230769229,62.307838010180561,540.00126275489822,24234.867246387279,2132.6228427731326,-152652.73120000001,2.4661452781576672,6856.441571014193,737.28627866883051,-153543.1321496749,4.6787690728351414,4937.2620158679001,318.3659618676715,-153641.46322582758,5.546271001473932,null,94.84091827519741]
["ICH","ICH11-200-A5",1250.5593222258879,18.323319259371566,2697.9248376411351,53,"NA",0.4,9,38.718642751872416,11.2,675,32,10.124321828947453,4.3128915386951148,8.1450228921279599,null,0.44642857142857145,0.2623852514697389,0.31440164239031615,0.10383795300177794,508.93919999999997,0,-848.23199999999997,0,0,0,0,0,0.2003236971512716,0.2589245712195784,4.8077687316305182,12.428379418539762,7.9121520763287165,391.49169230769229,62.307838010180561,540.00126275489822,8078.101713858041,710.8641583313256,-153326.92000000001,4.3128915386951148,2285.4805236713973,245.76209288961013,-153623.7107165583,8.1450228921279599,1645.7540052892998,106.12198728922385,-153656.48774194252,9.630390152075492,null,54.756429696376514]
["ICH","ICH11-250-A1",1568.82610601437,10.620308277258449,3372.4060470514191,30.6,"NA",1.5,33,83.802632253092327,13.8,675,32,4.677657365416886,1.9959286289433951,3.7553965195672667,null,0.36231884057971014,0.24272345482797436,0.29188893219446638,0.22377028853993999,590.62080000000003,0,-984.36800000000005,0,0,0,0,0,0.10740824651642931,0.13882847895779613,2.5777979163943034,6.6637669899742136,4.2422858242679862,454.32369230769234,72.307861394530534,626.66813208593135,36507.24598941439,3331.2020671749046,-152083.89249999999,1.9959286289433951,10574.473995864924,1156.1566303018985,-153473.665275412,3.7553965195672667,7589.5753817369559,461.82716690680746,-153633.63008103755,4.4688685281894047,null,118.51481909488771]
["ICH","ICH11-250-A5",1568.82610601437,18.39491352825593,3372.4060470514191,53,"NA",0.5,11,48.383472290122072,13.8,675,32,8.1019402173008235,3.5021216905200099,6.5468311007122697,null,0.36231884057971014,0.24272345482797436,0.29188893219446638,0.12881659839326093,590.62080000000003,0,-984.36800000000005,0,0,0,0,0,0.18603654011833845,0.24045797909240971,4.4648769628401226,11.541982996435665,7.3478545878613675,454.32369230769234,72.307861394530534,626.66813208593135,12168.802100659146,1110.3848773534733,-153137.3125,3.5021216905200099,3524.8246652883081,385.38554343396623,-153600.55509180401,6.5468311007122697,2529.8584605789852,153.94238896893586,-153653.87669367919,7.7629747445055592,null,68.424562707393221]
["ICH","ICH22-030-A1",342.42727740624485,2.8200649546478425,710.11417896403464,8.9,"NA",7.5,94,69.489983101853994,4.9000000000000004,675,32,5.6411008105359786,2.3700552699981223,4.6355922765456876,null,1.0204081632653061,0.58559255299412794,0.72997274995441797,0.21330802357813911,311.01840000000004,0,-518.36400000000003,0,0,0,0,0,6.8808709850062488E-2,0.11936020281472941,1.6514090364014997,5.7292897351070113,2.7177262812724416,239.2449230769231,38.077012117332572,330.00077168354898,25066.353193966188,4017.0210525400244,-150322.328125,2.3700552699981223,6860.7233332588894,1272.8382350955856,-153328.4926696755,4.6355922765456876,6715.92848397329,1226.6476052710909,-153352.40160034716,4.6880561885365717,null,98.273676551718765]
["ICH","ICH22-030-A5",342.42727740624485,4.8844957820944845,710.11417896403464,15.5,"NA",2.5,31,40.120060449837951,4.9000000000000004,675,32,9.7706732144662887,4.2102360905649148,8.1271279995507992,null,1.0204081632653061,0.58559255299412794,0.72997274995441797,0.1217197261645032,311.01840000000004,0,-518.36400000000003,0,0,0,0,0,0.11918018146357329,0.20758275842430521,2.8603243551257589,9.9639724043666504,4.7072400002290937,239.2449230769231,38.077012117332572,330.00077168354898,8285.4885811371605,1346.3684225984211,-152537.828125,4.2102360905649148,2272.5740345890254,424.27941169852852,-153552.16422322518,8.1271279995507992,2225.330536344301,408.88253509036366,-153560.13386678239,8.2155952162471042,null,56.738333611389045]
["ICH","ICH22-050-A1",583.67665954224049,2.890117015516144,1183.5236316067244,8.9,"NA",10.1,156,115.57658677919602,6.8,675,32,3.3916904013517786,1.3979233954864445,2.7455934697293913,null,0.73529411764705888,0.4094853642431639,0.52204111814922016,0.32974275302506917,370.70880000000005,0,-617.84800000000007,0,0,0,0,0,4.9310859116833083E-2,6.7343345766521498E-2,1.183460618803994,3.2324805967930321,1.9476228818410022,285.16061538461543,45.384721513588318,393.33425311776546,69095.802672728169,8997.2932723875565,-147603.840925,1.3979233954864445,19235.561853783965,2921.7112786647422,-153024.949962379,2.7455934697293913,16027.140408162546,1968.913960891698,-153373.78908166321,3.032667104359299,null,163.44997651592939]
["ICH","ICH22-050-A5",583.67665954224049,5.0058295106932906,1183.5236316067244,15.5,"NA",3.4,52,66.728173488986982,6.8,675,32,5.8745800986849561,2.4893895914379001,4.8159102311152129,null,0.73529411764705888,0.4094853642431639,0.52204111814922016,0.18868855073842047,370.70880000000005,0,-617.84800000000007,0,0,0,0,0,8.5408913355225879E-2,0.11674267576471901,2.0498139205254211,5.6036484367065125,3.3733817853323318,285.16061538461543,45.384721513588318,393.33425311776546,23236.780947838703,3045.4430616318159,-151581.0325,2.4893895914379001,6411.8539512613243,983.54637103565619,-153446.7442867886,4.8159102311152129,5342.3801360541838,662.80271950809663,-153565.33796051447,5.2997386226486158,null,94.36788794050986]
["ICH","ICH22-075-A1",888.92530223322842,5.8768484107682353,1775.2854474100868,17.899999999999999,"NA",3.3,59,86.563288020543851,9.3000000000000007,675,32,4.528478630651918,1.8945892767217551,3.6736514643129596,null,0.5376344086021505,0.32583630544733377,0.42176203330699696,0.23770633201213387,449.24880000000002,0,-748.74800000000005,0,0,0,0,0,7.978710724328153E-2,0.10312730258875445,1.9148905738387567,4.9501105242602135,3.1513382351489057,345.57600000000002,55.000128613924829,476.66778132068185,39743.307518158297,4428.2420016453707,-151047.05132500001,1.8945892767217551,10969.477181860942,1453.8607245735616,-153381.91621639158,3.6736514643129596,8492.7771854884777,779.60270023895987,-153582.88910739889,4.2068715272967756,null,122.41897592226115]
["ICH","ICH22-075-A5",888.92530223322842,10.179000035830994,1775.2854474100868,30.9,"NA",1.1000000000000001,20,49.977337640600098,9.3000000000000007,675,32,7.8435550692790583,3.3052920339168912,6.3806369453220562,null,0.5376344086021505,0.32583630544733377,0.42176203330699696,0.13686382564048488,449.24880000000002,0,-748.74800000000005,0,0,0,0,0,0.13819532353431038,0.17862172773125207,3.316687764823449,8.5738429311000992,5.458277935112342,345.57600000000002,55.000128613924829,476.66778132068185,13541.011986475507,1471.1430799091427,-152797.50992499999,3.3052920339168912,3696.1052109145839,484.62024152452045,-153569.97207213053,6.3806369453220562,2842.316071113677,259.86756674631994,-153636.96303579962,7.3065325722138503,null,70.678628702635791]
["ICH","ICH22-100-A1",1202.9831045137794,10.239008031593199,2367.0472632134488,30.6,"NA",1.4,27,67.237972465825109,11.8,675,32,5.8300389738735943,2.454649146859357,4.7140712362058812,null,0.42372881355932202,0.28286450722955631,0.37162249088588545,0.18166979485764065,527.78880000000004,0,-879.64800000000002,0,0,0,0,0,0.12067716505733665,0.15597896635698566,2.8962519613760795,7.4869903851353117,4.7663661147031133,405.99138461538467,64.615535714261327,560.00130952359825,24258.412298060965,2494.5643001769172,-152287.5508,2.454649146859357,6730.8027948695726,834.70143479859883,-153509.88919035759,4.7140712362058812,4999.8212684021119,388.56231213435768,-153630.6041784691,5.5044923719081424,null,95.08885256763827]
["ICH","ICH22-100-A5",1202.9831045137794,17.734482129825221,2367.0472632134488,53,"NA",0.5,9,38.819861502908779,11.8,675,32,10.097923712855787,4.2971197708529525,8.2081058656509533,null,0.42372881355932202,0.28286450722955631,0.37162249088588545,0.10460000232026664,527.78880000000004,0,-879.64800000000002,0,0,0,0,0,0.20901898119268261,0.27016349464237577,5.0164555486243829,12.967847742834037,8.2555882781404595,405.99138461538467,64.615535714261327,560.00130952359825,8085.950064415937,890.90313517218283,-153137.3125,4.2971197708529525,2243.6009316231912,298.10765528521398,-153605.02902692254,8.2081058656509533,1666.6070894673712,138.77225433369921,-153651.22098665909,9.5602292334389958,null,54.899574626858602]
["ICH","ICH22-150-A1",1823.0643897122618,10.353804682819181,3550.5708948201736,30.6,"NA",1.9,40,100.76622866476333,16.8,675,32,3.8901922320039888,1.6343719552192064,3.1293383109808661,null,0.29761904761904762,0.24220504721961481,0.32148294846477393,0.26912112308201563,684.86880000000008,0,-1141.4480000000001,0,0,0,0,0,0.10448932300437036,0.13505568008512009,2.5077437521048886,6.4826726440857643,4.1269975830114269,526.82215384615392,83.846349914934351,726.66836592943105,53473.377106525775,5073.6518602411443,-151128.80530000001,1.6343719552192064,15113.367871085928,1716.7189669790525,-153373.75255765751,3.1293383109808661,10941.802425763957,684.27937791688328,-153617.88556474663,3.7157989998995595,null,142.50496720689634]
["ICH","ICH22-150-A5",1823.0643897122618,17.933315762287386,3550.5708948201736,53,"NA",0.6,13,58.177409244824503,16.8,675,32,6.7380105970406809,2.9428714012676678,5.512183314414612,null,0.29761904761904762,0.24220504721961481,0.32148294846477393,0.15450033130326635,684.86880000000008,0,-1141.4480000000001,0,0,0,0,0,0.18098081629204496,0.23392329975819617,4.3435395910090788,11.228318388393417,7.1481694964897455,526.82215384615392,83.846349914934351,726.66836592943105,17111.100607248991,1602.183035769737,-152905.57,2.9428714012676678,4956.1636096308193,542.12177904601651,-153577.16697015794,5.512183314414612,3634.2988091444195,216.08822460533159,-153650.20399166935,6.4724780300769398,null,82.275281177760405]
["ICH","ICH22-200-A1",2444.5479347532541,10.417697510043947,4734.0945264268976,30.6,"NA",2.5,53,134.28879580831176,21.7,675,32,2.9190819505117438,1.2131994206826318,2.3326590836226808,null,0.2304147465437788,0.22122866930384436,0.2953071579361054,0.35718285896186802,838.80719999999997,0,-1398.0119999999999,0,0,0,0,0,9.6028889889874791E-2,0.12412030874536058,2.304693357356995,5.9577748197773079,3.7928372495839375,645.23630769230772,102.6925478315939,890.00208120714717,94086.355583760698,8896.7594089418708,-149274.8125,1.2131994206826318,26848.357924610704,3028.880664771038,-153155.27302463699,2.3326590836226808,19201.906640304009,1102.7438067588594,-153596.56743249143,2.7996864208614154,null,189.91303630686505]
["ICH","ICH22-200-A5",2444.5479347532541,18.043981385279899,4734.0945264268976,53,"NA",0.8,18,77.531672409079505,21.7,675,32,5.055998249743598,2.1270612986253381,4.062795558026318,null,0.2304147465437788,0.22122866930384436,0.2953071579361054,0.20549352623791589,838.80719999999997,0,-1398.0119999999999,0,0,0,0,0,0.16632691628370042,0.21498268099810014,3.9918459908088102,10.319168687908807,6.5693868211191786,645.23630769230772,102.6925478315939,890.00208120714717,32327.033895792491,2846.9224711362099,-152315.68,2.1270612986253381,9061.3776285086824,969.24181272673252,-153507.7190731685,4.062795558026318,6415.4713813224571,352.87801816283519,-153643.28471526137,4.8663333502887189,null,109.64634263438774]
["ICH","ICH22-250-A1",3066.6708916086786,10.458402331377483,5917.6181580336224,30.6,"NA",3,66,167.80882279225321,26.7,675,32,2.3359915973267671,0.95963574270006591,1.8560213053087715,null,0.18726591760299627,0.20937305725982022,0.28048649907339446,0.44561098244626907,995.88720000000001,0,-1659.8119999999999,0,0,0,0,0,9.1237819590572297E-2,0.11792770227607707,2.189707670173735,5.6605297092516995,3.6036051349837481,766.06707692307691,121.92336203226692,1056.66913761298,146097.26027439127,13340.991382883771,-147343.57,0.95963574270006591,41936.323465044428,4559.6554046287101,-152925.6972895565,1.8560213053087715,29795.424382817342,1571.1001651350946,-153576.34470271005,2.2441098612747457,null,237.31751307866699]
["ICH","ICH22-250-A5",3066.6708916086786,18.114484203942595,5917.6181580336224,53,"NA",1,22,96.884469011501594,26.7,675,32,4.0460561326239386,1.7190720120911207,3.2589449149617935,null,0.18726591760299627,0.20937305725982022,0.28048649907339446,0.25596501170493424,995.88720000000001,0,-1659.8119999999999,0,0,0,0,0,0.15802853910267425,0.20425677196202138,3.7926849384641819,9.8043250541770259,6.2416271842079531,766.06707692307691,121.92336203226692,1056.66913761298,48697.96717488116,4446.9338039947097,-151557.25,1.7190720120911207,13978.774488348139,1519.8851348762362,-153417.89909651884,3.2589449149617935,9931.8081276057801,523.70005504503138,-153634.78156757003,3.9067839519908998,null,137.01533005938091]
["ICH","ICH33-030-A1",511.19187514079709,2.8053615583674194,1065.171268446052,8.9,"NA",11.3,141,104.28169119278212,7.2,675,32,3.7590491246955571,1.5307376838516951,3.0596028474402606,null,0.69444444444444442,0.48339771313324809,0.59970825248780446,0.30699262861025778,383.27519999999998,0,-638.79199999999992,0,0,0,0,0,5.6504390076113985E-2,8.7690879104648345E-2,1.3561053618267356,4.2091621970231206,2.231744589482159,294.8270769230769,46.923186649642155,406.66761763023197,56409.035863584788,9082.5364106771831,-146078.25632499999,1.5307376838516951,15398.820662455146,2862.8987077512552,-152910.30465400859,3.0596028474402606,13737.848468897062,2277.5170217194959,-153187.01235339214,3.2574072039675879,null,147.47658199203488]
["ICH","ICH33-030-A5",511.19187514079709,4.8590287526929732,1065.171268446052,15.5,"NA",3.8,47,60.207062481702174,7.2,675,32,6.5108640721200217,2.7421054048798164,5.3739257963908509,null,0.69444444444444442,0.48339771313324809,0.59970825248780446,0.17523227439128811,383.27519999999998,0,-638.79199999999992,0,0,0,0,0,9.7868474462520075E-2,0.15229173041707469,2.3488433871004819,7.3100030600195849,3.8654950185000465,294.8270769230769,46.923186649642155,406.66761763023197,18970.359000542881,3071.095805627433,-151062.0925,2.7421054048798164,5132.940220818381,962.74469818183786,-153408.30196265684,5.3739257963908509,4579.2828229656861,765.89067987027283,-153502.17757967694,5.7067112977546115,null,85.145644312267251]
["ICH","ICH33-050-A1",768.78560211416482,8.7788455646958372,1908.9090832366524,30.6,"NA",1.3,20,50.560016241167531,10.199999999999999,675,32,7.7531620664477057,3.3105664524049945,6.6018960926483654,null,0.49019607843137258,0.40046729112412499,0.41692504215578385,0.13949775645002493,477.52319999999997,0,-795.87199999999996,0,0,0,0,0,0.14648502093711588,0.193692916679819,3.5156405024907813,9.2972600006313115,5.7856947482526033,367.32553846153849,58.461675170045964,506.66785147373167,13386.201309108725,1741.8173623584621,-152477.1637,3.3105664524049945,3447.6808082345478,499.71064137420876,-153566.31614592366,6.6018960926483654,2943.4766569950789,329.33410345792669,-153621.57137073495,7.16857407207298,null,71.502660682062825]
["ICH","ICH33-050-A5",768.78560211416482,15.20540654985388,1908.9090832366524,53,"NA",0.4,7,29.190838987069938,10.199999999999999,675,32,13.428870618403128,5.5779080881165726,11.347086319688367,null,0.49019607843137258,0.40046729112412499,0.41692504215578385,8.077720519181246E-2,477.52319999999997,0,-795.87199999999996,0,0,0,0,0,0.25371949881087547,0.33548559921389592,6.0892679714610107,16.103308762267005,10.021117261057933,367.32553846153849,58.461675170045964,506.66785147373167,4831.9748640805865,535.93617215637607,-153326.92000000001,5.5779080881165726,1179.6819262473703,153.75712042283354,-153636.25547339843,11.347086319688367,994.38690066686536,101.33357029474672,-153651.9492650608,12.37973011848347,null,41.282080392563458]
["ICH","ICH33-075-A1",1170.8433585035712,8.9255805782743938,2863.3636248549783,30.6,"NA",1.7,30,75.735883204766836,13.8,675,32,5.1758820708560433,2.1884060043519211,4.3701818720686756,null,0.36231884057971014,0.32522787075702958,0.34378029791792708,0.20473354930939713,590.62080000000003,0,-984.36800000000005,0,0,0,0,0,0.12095198194760325,0.15633417568313165,2.9028475667424778,7.504040432790319,4.777220512160099,454.32369230769234,72.307861394530534,626.66813208593135,30103.167655109683,3411.9501233123901,-151634.43969999999,2.1884060043519211,7809.1015821296896,995.21685472803904,-153491.32396958105,4.3701818720686756,6329.825104828622,532.6679122730435,-153614.53367085624,4.8843973221447037,null,107.10671318648558]
["ICH","ICH33-075-A5",1170.8433585035712,15.45955904862125,2863.3636248549783,53,"NA",0.6,10,43.726132555586183,13.8,675,32,8.9648907207074835,3.8441089309683885,7.6144840665830174,null,0.36231884057971014,0.32522787075702958,0.34378029791792708,0.11779927617653174,590.62080000000003,0,-984.36800000000005,0,0,0,0,0,0.20949497800940245,0.27077873524258289,5.027879472225659,12.997379291643979,8.2743886460215048,454.32369230769234,72.307861394530534,626.66813208593135,10034.157899516744,1204.2005429557923,-152905.57,3.8441089309683885,2603.0338607098961,351.25300755107253,-153599.47054918599,7.6144840665830174,2109.9417016095404,188.00043962578002,-153645.51431298433,8.489016507210275,null,61.838089690233488]
["ICH","ICH33-100-A1",1575.2892534803184,9.0138259976361308,3817.8181664733047,30.6,"NA",2.1,40,100.89984816513028,17.5,675,32,3.8850405340398746,1.6259360960757994,3.2584635259099946,null,0.2857142857142857,0.28930165039983513,0.30857938975345844,0.27058100860979883,706.86,0,-1178.0999999999999,0,0,0,0,0,0.1086547807305447,0.14043966296393315,2.6077147375330729,6.7411038222687916,4.2915199808389906,543.73846153846159,86.538663903028564,750.00175382624752,53500.323626952748,5615.1565081904509,-150566.98929999999,1.6259360960757994,13939.667194585236,1654.05371615434,-153395.26873697495,3.2584635259099946,11032.825873670223,787.50184151756264,-153603.08529706032,3.6957508774833725,null,142.69393371651279]
["ICH","ICH33-100-A5",1575.2892534803184,15.612404598491,3817.8181664733047,53,"NA",0.7,13,58.254554499330339,17.5,675,32,6.7290875944215864,2.9316966174252297,5.7278615946173757,null,0.2857142857142857,0.28930165039983513,0.30857938975345844,0.15527385404292035,706.86,0,-1178.0999999999999,0,0,0,0,0,0.18819560071055927,0.24324863165138136,4.5166944170534222,11.675934319266306,7.4331306485101463,543.73846153846159,86.538663903028564,750.00175382624752,17120.08278072465,1871.6921834631667,-152631.6925,2.9316966174252297,4584.6907025800228,551.35123871811334,-153574.42291232498,5.7278615946173757,3663.5853590150782,262.50061383918751,-153643.69509902011,6.4402342954892005,null,82.384381042955283]
["ICH","ICH33-150-A1",2387.2665234552542,9.1148862796546126,5726.7272497099566,30.6,"NA",2.9,60,151.21296389849255,24.9,675,32,2.5923703225812367,1.060869887171586,2.1501885133302041,null,0.20080321285140562,0.2536874503807538,0.27337848158898986,0.40311093910579571,939.33839999999998,0,-1565.5639999999999,0,0,0,0,0,9.6347177533170555E-2,0.12453170536361792,2.3123322607960932,5.9775218574536604,3.8054086042143913,722.56799999999998,115.00026892002462,996.6689973068801,120334.33505218121,11620.881752758818,-147757.9093,1.060869887171586,31513.566999203613,3461.5364590101303,-153139.96563444729,2.1501885133302041,24372.752207249749,1445.170046094981,-153572.66024322648,2.4807066814367742,null,213.84742435188062]
["ICH","ICH33-150-A5",2387.2665234552542,15.78744614157425,5726.7272497099566,53,"NA",1,20,87.30284541175584,24.9,675,32,4.4901171107444213,1.8945245969904656,3.7659846526256771,null,0.20080321285140562,0.2536874503807538,0.27337848158898986,0.23158722085620884,939.33839999999998,0,-1565.5639999999999,0,0,0,0,0,0.16687820665331002,0.21569524084298389,4.0050769596794407,10.353371560463227,6.5911610460590904,722.56799999999998,115.00026892002462,996.6689973068801,40110.519741981137,4007.1435433100528,-151557.25,1.8945245969904656,10504.522333067873,1193.6332617276312,-153477.06740824517,3.7659846526256771,8124.2507357499162,498.33449865344181,-153631.41744704868,4.3180275504963817,null,123.4648680150664]
["ICH","ICH33-200-A1",3201.0792522061433,13.756700702128253,7635.6363329466094,45.9,"NA",1.7,35,134.34500088183421,32.200000000000003,675,32,2.91786071254554,1.2203691775718515,2.4339384773261195,null,0.15527950310559005,0.23538306667993056,0.25509229552952567,0.35565550750268682,1168.6752000000001,0,-1947.7920000000001,0,0,0,0,0,0.13492059994437092,0.17438904625898755,3.2380943986649022,8.3706742204314022,5.328936716774221,898.9809230769232,143.07725765300725,1240.0028996593962,92673.262940994799,9078.4927090477304,-149097.489325,1.2203691775718515,24751.833778263797,2720.9173643752315,-153253.8075302043,2.4339384773261195,19054.440929418106,1054.0024647104906,-153602.44827454322,2.8117095866776234,null,189.99252228411467]
["ICH","ICH33-200-A5",3201.0792522061433,23.827304560604581,7635.6363329466094,79.5,"NA",0.6,12,77.564122423407497,32.200000000000003,675,32,5.0538830035380027,2.1189415191682142,4.2230911556788033,null,0.15527950310559005,0.23538306667993056,0.25509229552952567,0.20484680677522663,1168.6752000000001,0,-1947.7920000000001,0,0,0,0,0,0.23368933409132508,0.30205068840404564,5.608544018191802,14.498433043394192,9.2299891437722312,898.9809230769232,143.07725765300725,1240.0028996593962,32332.066756557018,3204.128271031746,-151957.5325,2.1189415191682142,8380.1163126618085,960.32377566184641,-153510.71008049158,4.2230911556788033,6370.9132835178571,372.00086989782017,-153640.99797110958,4.8816967945088621,null,109.69223388474958]
["ICH","ICH33-250-A1",4015.7289257162465,13.810451931099834,9544.5454161832604,45.9,"NA",2,44,167.87880569164045,39.6,675,32,2.3350178027834261,0.95954392759343377,1.9338361369007946,null,0.12626262626262627,0.22495682467769296,0.24466916947563108,0.44421833143079675,1401.1536000000001,0,-2335.2559999999999,0,0,0,0,0,0.12944814224100548,0.16731572550607043,3.1067554137841316,8.0311548242913808,5.1127919560891817,1077.8104615384614,171.53886267000328,1486.6701431400286,146120.75266792095,13346.555102610415,-147343.57,0.95954392759343377,38860.119708755214,4015.7289257162606,-153091.81425237635,1.9338361369007946,29646.624622680392,1486.6701431400338,-153585.57807524124,2.251145279797591,null,237.41648384411462]
["ICH","ICH33-250-A5",4015.7289257162465,23.920404420152629,9544.5454161832604,79.5,"NA",0.7,15,96.92487365730149,39.6,675,32,4.0443694709987383,1.6853005060887873,3.3672033103106926,null,0.12626262626262627,0.22495682467769296,0.24466916947563108,0.25560556410872154,1401.1536000000001,0,-2335.2559999999999,0,0,0,0,0,0.22421075930682444,0.28979933748176184,5.3810582233637865,13.910368199124569,8.8556154364759259,1077.8104615384614,171.53886267000328,1486.6701431400286,50512.983741677104,4671.2277683698949,-151341.30812500001,1.6853005060887873,13116.981628372785,1405.505124000691,-153453.7217377483,3.3672033103106926,9904.6318437134305,520.33455009901172,-153635.17994265116,3.9122779016447824,null,137.07247085745402]
["ICH","ICH44-030-A1",599.91929812416197,4.2717615244621898,1527.1272665893216,15.3,"NA",5.0999999999999996,64,81.082140536308216,9.6,675,32,4.8346034947666947,2.0066045337954099,4.1026219843468459,null,0.52083333333333337,0.49293394567377158,0.50058434337783264,0.23237523222342465,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,8.7737344301273043E-2,0.1297659547882947,2.1056962632305529,6.2287658298381459,3.4653474389536467,352.82584615384616,56.153977465965212,486.66780470503181,34298.821844961727,5479.2036686226365,-149097.489325,2.0066045337954099,8735.5136735873893,1529.794210216618,-153308.02818322452,4.1026219843468459,7996.5589841628016,1241.0029019978354,-153429.74159423655,4.3033846181959605,null,114.66746281268797]
["ICH","ICH44-030-A5",599.91929812416197,7.3989079981863934,1527.1272665893216,26.5,"NA",1.7,21,46.812795665108624,9.6,675,32,8.3737788873859689,3.613533896085007,7.2019487732612797,null,0.52083333333333337,0.49293394567377158,0.50058434337783264,0.13272912198050019,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.15196553805096857,0.22475983171784555,3.6471729132232458,10.788471922456587,6.0021578301464036,352.82584615384616,56.153977465965212,486.66780470503181,11146.144850434186,1826.3752155803427,-152141.87312500001,3.613533896085007,2889.5012684521448,509.93140340553953,-153545.34272774152,7.2019487732612797,2650.8203470388812,413.66763399927856,-153585.91386474553,7.534141604183251,null,66.203290522196809]
["ICH","ICH44-050-A1",1022.575911581599,4.3778745761609796,2545.2121109822028,15.3,"NA",6.8,106,134.85641663498313,13.5,675,32,2.9067953144641927,1.1799545014817625,2.4332293716615321,null,0.37037037037037035,0.36644168694010099,0.3805812473625988,0.37199572510032508,581.19600000000003,0,-968.66,0,0,0,0,0,6.6843156037525372E-2,8.63968455160362E-2,1.6042357449006091,4.1470485847697374,2.6400931260334106,447.0738461538462,71.15401254249015,616.66810870158133,94239.128011742403,12150.736160907079,-145545.75880000001,1.1799545014817625,24412.974070659635,3476.7580993774491,-152999.3305482966,2.4332293716615321,20450.747589258492,2096.6715695853841,-153422.277219354,2.6882029349404641,null,190.71577337822913]
["ICH","ICH44-050-A5",1022.575911581599,7.5827011950748808,2545.2121109822028,26.5,"NA",2.2999999999999998,35,77.859388446155833,13.5,675,32,5.0347171718551342,2.1429808765926808,4.2806791306274334,null,0.37037037037037035,0.36644168694010099,0.3805812473625988,0.2127831836711839,581.19600000000003,0,-968.66,0,0,0,0,0,0.11577574239524829,0.14964372604745402,2.778617817485959,7.1828988502777928,4.57277543100321,447.0738461538462,71.15401254249015,616.66810870158133,30936.270514906533,4109.7492969511104,-150877.823125,2.1429808765926808,8098.6809818064557,1175.9622983188428,-153435.87923446079,4.2806791306274334,6802.7409391623469,709.16832500682085,-153581.03848337257,4.6996195035097816,null,110.10980309862825]
["ICH","ICH44-075-A1",1557.3551744449078,8.9020981182865899,3817.8181664733047,30.6,"NA",2.2000000000000002,40,101.00309132098027,18.3,675,32,3.881069330385674,1.6214750248579559,3.2644374296573906,null,0.27322404371584696,0.30303790451791829,0.319551101389137,0.27178789961528649,731.99279999999999,0,-1219.9880000000001,0,0,0,0,0,{"$f":"AF68/Irms","v":0.11240304831576965},{"$f":"AG68/Ipeak","v":0.14528441468887629},2.6976731595784718,6.9736519050660615,4.4395646883739071,{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V68)+Ltime2*ABS(Lspeed2)*ABS(W68)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X68)+Ltime4*ABS(Lspeed1)*ABS(Y68))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V68)+Ltime2*ABS(Lspeed2)*ABS(W68)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X68)+Ltime4*ABS(Lspeed1)*ABS(Y68)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z68)+Ltime6*ABS(Lspeed6)*ABS(AA68)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB68)+Ltime8*ABS(Lspeed1)*ABS(AC68))/ltime)","v":563.07138461538466},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK68/2*Ltime1/ltime,AK68/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X68*-ABS(Lspeed2-Lspeed1),((X68-Y68)*2/PI()+Y68)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V68*-ABS(Lspeed2-Lspeed1),((V68-W68)*2/PI()+W68)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X68*-ABS(Lspeed2-Lspeed1),((X68-Y68)*2/PI()+Y68)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V68*-ABS(Lspeed2-Lspeed1),((V68-W68)*2/PI()+W68)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB68*-ABS(Lspeed6-Lspeed1),((AB68-AC68)*2/PI()+AB68)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z68*-ABS(Lspeed6-Lspeed1),((Z68-AA68)*2/PI()+AA68)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB68*-ABS(Lspeed6-Lspeed1),((AB68-AC68)*2/PI()+AB68)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z68*-ABS(Lspeed6-Lspeed1),((Z68-AA68)*2/PI()+AA68)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":89.615594175136266},{"$f":"IF(move1,MAX(IF(AccType=1,X68*-ABS(Lspeed2-Lspeed1),((X68-Y68)*2/PI()+Y68)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V68*-ABS(Lspeed2-Lspeed1),((V68-W68)*2/PI()+W68)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X68*-ABS(Lspeed2-Lspeed1),((X68-Y68)*2/PI()+Y68)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V68*-ABS(Lspeed2-Lspeed1),((V68-W68)*2/PI()+W68)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB68*-ABS(Lspeed6-Lspeed1),((AB68-AC68)*2/PI()+AB68)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z68*-ABS(Lspeed6-Lspeed1),((Z68-AA68)*2/PI()+AA68)*-ABS(Lspeed6-Lspeed1)),0))","v":776.6684828511809},53521.168723600684,5888.5640750391212,-150265.01319999999,{"$f":"-AM68/2/AL68+SQRT((AM68/2/AL68)^2-AN68/AL68)","v":1.6214750248579559},13867.905721827114,1713.0906918894045,-153376.33211620542,{"$f":"-AQ68/2/AP68+SQRT((AQ68/2/AP68)^2-AR68/AP68)","v":3.2644374296573906},11113.471098138622,854.33533113630199,-153592.45366332121,{"$f":"IF((AU68/2/AT68)^2-AV68/AT68>=0,-AU68/2/AT68+SQRT((AU68/2/AT68)^2-AV68/AT68),-9999)","v":3.6793396667603364},null,142.83994158773805]
["ICH","ICH44-075-A5",1557.3551744449078,15.41888623483567,3817.8181664733047,53,"NA",0.7,13,58.31416196315233,18.3,675,32,6.7222092679253072,2.9310578661305748,5.7424796856473872,null,0.27322404371584696,0.30303790451791829,0.319551101389137,0.15584993557694296,731.99279999999999,0,-1219.9880000000001,0,0,0,0,0,0.19468779060853236,0.25163998778903979,4.6725069746047767,12.078719413873911,7.689551603752296,563.07138461538466,89.615594175136266,776.6684828511809,17127.031146273963,1873.6073440041844,-152631.6925,2.9310578661305748,4562.2943614487904,545.07431105571959,-153576.62979562438,5.7424796856473872,3689.4828900675002,271.83396899791427,-153642.27001757897,6.4164287030218308,null,82.468678726711005]
["ICH","ICH44-100-A1",2095.3102447660631,8.9901113712910679,5090.4242219644057,30.6,"NA",2.8,53,134.56206312578115,23.2,675,32,2.9131539075287525,1.2024829605884657,2.4330751002642557,null,0.21551724137931036,0.2726022745991778,0.29006462636825098,0.35999485045066332,885.93119999999999,0,-1476.5519999999999,0,0,0,0,0,0.10211353369641162,0.13198489896127355,2.4507248087138787,6.33527515014113,4.0331614239688411,681.48553846153845,108.4617920917958,940.00219812889691,94159.823736780963,9984.6472617043455,-148158.20319999999,1.2024829605884657,24671.468086482346,2933.4343426724986,-153188.76603748687,2.4330751002642557,19428.134920628898,1316.0030773804604,-153568.35362049786,2.7778175125231361,null,190.29949465338356]
["ICH","ICH44-100-A5",2095.3102447660631,15.57132966077884,5090.4242219644057,53,"NA",0.9,18,77.689443368381149,23.2,675,32,5.0457305781076069,2.1182406231479725,4.2424618182017282,null,0.21551724137931036,0.2726022745991778,0.29006462636825098,0.20695731219615662,885.93119999999999,0,-1476.5519999999999,0,0,0,0,0,0.17686582850258148,0.22860455083277051,4.2447798840619555,10.973018439972984,6.9856405014408738,681.48553846153845,108.4617920917958,940.00219812889691,32351.523280132573,3209.3052055498797,-151957.5325,2.1182406231479725,8307.1742512266719,942.88961014473159,-153516.70171825169,4.2424618182017282,6492.8204465952904,423.00098915800504,-153634.35450227166,4.8319143179255635,null,109.86946446478075]
["ICH","ICH44-150-A1",3175.3235352486199,18.181811544229408,7635.6363329466094,61.2,"NA",1,20,100.83010119097844,33,675,32,3.8877279241992211,1.6302028509789122,3.2552389932779762,null,0.15151515151515152,0.24239536862641561,0.26057815134736489,0.26690776360189117,1193.808,0,-1989.68,0,0,0,0,0,0.18363278798164609,0.23735105514800373,4.4071869115595064,11.392850647104179,7.2529139855773153,918.31384615384616,146.15418792511494,1266.6696286843294,53486.253573389353,5344.0714607696264,-150854.92000000001,1.6302028509789122,13990.158632738754,1587.6617676243154,-153416.0662967276,3.2552389932779762,10775.132958685555,633.33481434216685,-153624.54642903837,3.7466126369091293,null,142.59529659973276]
["ICH","ICH44-150-A5",3175.3235352486199,31.491821368247681,7635.6363329466094,106,"NA",0.3,7,58.21428606502861,33,675,32,6.733742290717335,2.7728853121142785,5.6108683229367324,null,0.15151515151515152,0.24239536862641561,0.26057815134736489,0.1539515375606684,1193.808,0,-1989.68,0,0,0,0,0,0.31806131871973453,0.41110408674642501,7.6334716492736288,19.7329961638284,12.562415525946793,918.31384615384616,146.15418792511494,1266.6696286843294,19308.382235307159,1603.1986089365571,-152905.57,2.7728853121142785,4794.0207295702421,476.29853028729462,-153597.05790011646,5.6108683229367324,3612.4987943556912,190.00044430265007,-153653.34753584035,6.4955505858843754,null,82.327432877030247]
["ICH","ICH44-200-A1",4257.7776655133157,18.294010622656721,10180.848443928811,61.2,"NA",1.2,27,134.37343686076341,42.7,675,32,{"$f":"IF(G74=\"NA\",(UAC_V*0.98)/J74,(IF((UAC_V*0.98)/J74<G74,(UAC_V*0.98)/J74,G74)))","v":2.9172432376362227},{"$f":"IF(AO74<G74,IF(AO74<0,0,AO74),G74)","v":1.1986511983693238},{"$f":"IF(AS74<G74,IF(AS74<0,0,AS74),G74)","v":2.4204981402339563},null,{"$f":"IF(move1,Gewicht/K74,MAX(Gewicht,Gewicht2)/K74)","v":0.11709601873536299},{"$f":"IF(move1,IF(AccType=1,SQRT((V74^2*Ltime1+W74^2*Ltime2+X74^2*Ltime3+Y74^2*Ltime4)/ltime)/C74,SQRT((((V74-W74)*2/PI()+W74)^2*Ltime1+W74^2*Ltime2+((X74-W74)*2/PI()+W74)^2*Ltime3+Y74^2*Ltime4)/ltime)/C74),IF(AccType=1,SQRT((V74^2*Ltime1+W74^2*Ltime2+X74^2*Ltime3+Y74^2*Ltime4+Z74^2*Ltime5+AA74^2*Ltime6+AB74^2*Ltime7+AC74^2*Ltime8)/ltime)/C74,SQRT((((V74-W74)*2/PI()+W74)^2*Ltime1+W74^2*Ltime2+((X74-W74)*2/PI()+W74)^2*Ltime3+Y74^2*Ltime4+((Z74-AA74)*2/PI()+AA74)^2*Ltime5+AA74^2*Ltime6+((AB74-AA74)*2/PI()+AA74)^2*Ltime7+AC74^2*Ltime8)/ltime)/C74))","v":0.22691546891003742},{"$f":" IF(move1,MAX(ABS(V74),ABS(X74))/E74,MAX(ABS(V74),ABS(X74),ABS(Z74),ABS(AB74))/E74)","v":0.2453206148539995},{"$f":"IF(AW74>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW74,G74),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW74,G74)),\"NA\")","v":0.35518046318839541},{"$f":"((Gewicht+K74)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":1498.5432000000001},0,{"$f":"((Gewicht+K74)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-2497.5720000000001},0,{"$f":"((Gewicht2+K74)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K74)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"AF74/Irms","v":0.1729664166118898},{"$f":"AG74/Ipeak","v":0.22356444042065368},{"$f":"D74*S74","v":4.151193998685355},{"$f":"IF(move1,IF(MAX(ABS(V74),ABS(X74))<=C74,MAX(ABS(V74),ABS(X74))/C74*D74,D74+(MAX(ABS(V74),ABS(X74))-C74)/(E74-C74)*(F74-D74)),IF(MAX(ABS(V74),ABS(X74),ABS(Z74),ABS(AB74))<=C74,MAX(ABS(V74),ABS(X74),ABS(Z74),ABS(AB74))/C74*D74,D74+(MAX(ABS(V74),ABS(X74),ABS(Z74),ABS(AB74))-C74)/(E74-C74)*(F74-D74)))","v":10.731093140191376},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V74),ABS(X74))<=C74,MAX(ABS(V74),ABS(X74))/C74*D74,D74+(MAX(ABS(V74),ABS(X74))-C74)/(E74-C74)*(F74-D74)),IF(MAX(ABS(V74),ABS(X74),ABS(Z74),ABS(AB74))<=C74,MAX(ABS(V74),ABS(X74),ABS(Z74),ABS(AB74))/C74*D74,D74+(MAX(ABS(V74),ABS(X74),ABS(Z74),ABS(AB74))-C74)/(E74-C74)*(F74-D74))),IF(move1,IF(MAX(ABS((V74-W74)*2/PI()+W74),ABS((X74-W74)*2/PI()+W74))<=C74,MAX(ABS((V74-W74)*2/PI()+W74),ABS((X74-W74)*2/PI()+W74))/C74*D74,D74+(MAX(ABS((V74-W74)*2/PI()+W74),ABS((X74-W74)*2/PI()+W74))-C74)/(E74-C74)*(F74-D74)),IF(MAX(ABS((V74-W74)*2/PI()+W74),ABS((X74-W74)*2/PI()+W74),ABS((Z74-AA74)*2/PI()+AA74),ABS((AB74-AA74)*2/PI()+AA74))<=C74,MAX(ABS((V74-W74)*2/PI()+W74),ABS((X74-W74)*2/PI()+W74),ABS((Z74-AA74)*2/PI()+AA74),ABS((AB74-AA74)*2/PI()+AA74))/C74*D74,D74+(MAX(ABS((V74-W74)*2/PI()+W74),ABS((X74-W74)*2/PI()+W74),ABS((Z74-AA74)*2/PI()+AA74),ABS((AB74-AA74)*2/PI()+AA74))-C74)/(E74-C74)*(F74-D74))))","v":6.8316260721639477},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V74)+Ltime2*ABS(Lspeed2)*ABS(W74)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X74)+Ltime4*ABS(Lspeed1)*ABS(Y74))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V74)+Ltime2*ABS(Lspeed2)*ABS(W74)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X74)+Ltime4*ABS(Lspeed1)*ABS(Y74)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z74)+Ltime6*ABS(Lspeed6)*ABS(AA74)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB74)+Ltime8*ABS(Lspeed1)*ABS(AC74))/ltime)","v":1152.7255384615385},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK74/2*Ltime1/ltime,AK74/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X74*-ABS(Lspeed2-Lspeed1),((X74-Y74)*2/PI()+Y74)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V74*-ABS(Lspeed2-Lspeed1),((V74-W74)*2/PI()+W74)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X74*-ABS(Lspeed2-Lspeed1),((X74-Y74)*2/PI()+Y74)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V74*-ABS(Lspeed2-Lspeed1),((V74-W74)*2/PI()+W74)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB74*-ABS(Lspeed6-Lspeed1),((AB74-AC74)*2/PI()+AB74)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z74*-ABS(Lspeed6-Lspeed1),((Z74-AA74)*2/PI()+AA74)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB74*-ABS(Lspeed6-Lspeed1),((AB74-AC74)*2/PI()+AB74)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z74*-ABS(Lspeed6-Lspeed1),((Z74-AA74)*2/PI()+AA74)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":183.46196747442056},{"$f":"IF(move1,MAX(IF(AccType=1,X74*-ABS(Lspeed2-Lspeed1),((X74-Y74)*2/PI()+Y74)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V74*-ABS(Lspeed2-Lspeed1),((V74-W74)*2/PI()+W74)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X74*-ABS(Lspeed2-Lspeed1),((X74-Y74)*2/PI()+Y74)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V74*-ABS(Lspeed2-Lspeed1),((V74-W74)*2/PI()+W74)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB74*-ABS(Lspeed6-Lspeed1),((AB74-AC74)*2/PI()+AB74)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z74*-ABS(Lspeed6-Lspeed1),((Z74-AA74)*2/PI()+AA74)*-ABS(Lspeed6-Lspeed1)),0))","v":1590.003718111645},{"$f":"(J74^2)+3*(I74/1000)^2*(F74/2)^2*(2000*PI()/M74)^2","v":97006.089960757206},{"$f":"SQRT(3)*H74*F74/2*J74","v":8546.2722801756208},{"$f":"3*F74^2*H74^2/4-(UAC_V*0.98)^2","v":-149618.92480000001},{"$f":"-AM74/2/AL74+SQRT((AM74/2/AL74)^2-AN74/AL74)","v":1.1986511983693238},{"$f":"(J74^2)+3*(I74/1000)^2*(D74/2)^2*(2000*PI()/M74)^2","v":25110.72358497079},{"$f":"SQRT(3)*H74*D74/2*J74","v":2554.6665993079982},{"$f":"3*D74^2*H74^2/4-(UAC_V*0.98)^2","v":-153302.55550936516},{"$f":"-AQ74/2/AP74+SQRT((AQ74/2/AP74)^2-AR74/AP74)","v":2.4204981402339563},{"$f":"(J74^2)+3*(I74/1000)^2*(AH74/2)^2*(2000*PI()/M74)^2","v":19039.997718476039},{"$f":"SQRT(3)*H74*AH74/2*J74","v":954.0022308669902},{"$f":"3*AH74^2*H74^2/4-(UAC_V*0.98)^2","v":-153613.59519602693},{"$f":"IF((AU74/2/AT74)^2-AV74/AT74>=0,-AU74/2/AT74+SQRT((AU74/2/AT74)^2-AV74/AT74),-9999)","v":2.8154701726079407},null,190.0327368311757]
["ICH","ICH44-200-A5",4257.7776655133157,31.686155872646193,10180.848443928811,106,"NA",0.4,9,77.58053994349693,42.7,675,32,{"$f":"IF(G75=\"NA\",(UAC_V*0.98)/J75,(IF((UAC_V*0.98)/J75<G75,(UAC_V*0.98)/J75,G75)))","v":5.052813505622666},{"$f":"IF(AO75<G75,IF(AO75<0,0,AO75),G75)","v":2.1267898406859329},{"$f":"IF(AS75<G75,IF(AS75<0,0,AS75),G75)","v":4.2324210391892096},null,{"$f":"IF(move1,Gewicht/K75,MAX(Gewicht,Gewicht2)/K75)","v":0.11709601873536299},{"$f":"IF(move1,IF(AccType=1,SQRT((V75^2*Ltime1+W75^2*Ltime2+X75^2*Ltime3+Y75^2*Ltime4)/ltime)/C75,SQRT((((V75-W75)*2/PI()+W75)^2*Ltime1+W75^2*Ltime2+((X75-W75)*2/PI()+W75)^2*Ltime3+Y75^2*Ltime4)/ltime)/C75),IF(AccType=1,SQRT((V75^2*Ltime1+W75^2*Ltime2+X75^2*Ltime3+Y75^2*Ltime4+Z75^2*Ltime5+AA75^2*Ltime6+AB75^2*Ltime7+AC75^2*Ltime8)/ltime)/C75,SQRT((((V75-W75)*2/PI()+W75)^2*Ltime1+W75^2*Ltime2+((X75-W75)*2/PI()+W75)^2*Ltime3+Y75^2*Ltime4+((Z75-AA75)*2/PI()+AA75)^2*Ltime5+AA75^2*Ltime6+((AB75-AA75)*2/PI()+AA75)^2*Ltime7+AC75^2*Ltime8)/ltime)/C75))","v":0.22691546891003742},{"$f":" IF(move1,MAX(ABS(V75),ABS(X75))/E75,MAX(ABS(V75),ABS(X75),ABS(Z75),ABS(AB75))/E75)","v":0.2453206148539995},{"$f":"IF(AW75>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW75,G75),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW75,G75)),\"NA\")","v":0.20427808804995617},{"$f":"((Gewicht+K75)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":1498.5432000000001},0,{"$f":"((Gewicht+K75)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-2497.5720000000001},0,{"$f":"((Gewicht2+K75)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K75)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,0.29958662157491861,0.38722496957427732,{"$f":"D75*S75","v":7.1900789177980471},{"$f":"IF(move1,IF(MAX(ABS(V75),ABS(X75))<=C75,MAX(ABS(V75),ABS(X75))/C75*D75,D75+(MAX(ABS(V75),ABS(X75))-C75)/(E75-C75)*(F75-D75)),IF(MAX(ABS(V75),ABS(X75),ABS(Z75),ABS(AB75))<=C75,MAX(ABS(V75),ABS(X75),ABS(Z75),ABS(AB75))/C75*D75,D75+(MAX(ABS(V75),ABS(X75),ABS(Z75),ABS(AB75))-C75)/(E75-C75)*(F75-D75)))","v":18.586798539565311},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V75),ABS(X75))<=C75,MAX(ABS(V75),ABS(X75))/C75*D75,D75+(MAX(ABS(V75),ABS(X75))-C75)/(E75-C75)*(F75-D75)),IF(MAX(ABS(V75),ABS(X75),ABS(Z75),ABS(AB75))<=C75,MAX(ABS(V75),ABS(X75),ABS(Z75),ABS(AB75))/C75*D75,D75+(MAX(ABS(V75),ABS(X75),ABS(Z75),ABS(AB75))-C75)/(E75-C75)*(F75-D75))),IF(move1,IF(MAX(ABS((V75-W75)*2/PI()+W75),ABS((X75-W75)*2/PI()+W75))<=C75,MAX(ABS((V75-W75)*2/PI()+W75),ABS((X75-W75)*2/PI()+W75))/C75*D75,D75+(MAX(ABS((V75-W75)*2/PI()+W75),ABS((X75-W75)*2/PI()+W75))-C75)/(E75-C75)*(F75-D75)),IF(MAX(ABS((V75-W75)*2/PI()+W75),ABS((X75-W75)*2/PI()+W75),ABS((Z75-AA75)*2/PI()+AA75),ABS((AB75-AA75)*2/PI()+AA75))<=C75,MAX(ABS((V75-W75)*2/PI()+W75),ABS((X75-W75)*2/PI()+W75),ABS((Z75-AA75)*2/PI()+AA75),ABS((AB75-AA75)*2/PI()+AA75))/C75*D75,D75+(MAX(ABS((V75-W75)*2/PI()+W75),ABS((X75-W75)*2/PI()+W75),ABS((Z75-AA75)*2/PI()+AA75),ABS((AB75-AA75)*2/PI()+AA75))-C75)/(E75-C75)*(F75-D75))))","v":11.832723455300162},1152.7255384615385,183.46196747442056,1590.003718111645,{"$f":"(J75^2)+3*(I75/1000)^2*(F75/2)^2*(2000*PI()/M75)^2","v":32334.613847168195},{"$f":"SQRT(3)*H75*F75/2*J75","v":2848.7168614481839},{"$f":"3*F75^2*H75^2/4-(UAC_V*0.98)^2","v":-152315.68},2.1267898406859329,{"$f":"(J75^2)+3*(I75/1000)^2*(D75/2)^2*(2000*PI()/M75)^2","v":8370.2411949902635},{"$f":"SQRT(3)*H75*D75/2*J75","v":851.55553310266612},{"$f":"3*D75^2*H75^2/4-(UAC_V*0.98)^2","v":-153543.51850312171},4.2324210391892096,{"$f":"(J75^2)+3*(I75/1000)^2*(AH75/2)^2*(2000*PI()/M75)^2","v":6346.6659061586797},{"$f":"SQRT(3)*H75*AH75/2*J75","v":318.00074362233011},{"$f":"3*AH75^2*H75^2/4-(UAC_V*0.98)^2","v":-153647.19839867565},4.895287642184365,null,109.7154517643206]
["ICH","ICH44-250-A1",5341.3447862142475,18.365490374602974,12726.060554911015,61.2,"NA",1.5,33,167.91421232181924,52.5,675,32,{"$f":"IF(G76=\"NA\",(UAC_V*0.98)/J76,(IF((UAC_V*0.98)/J76<G76,(UAC_V*0.98)/J76,G76)))","v":2.3345254376008673},{"$f":"IF(AO76<G76,IF(AO76<0,0,AO76),G76)","v":0.95949747251001527},{"$f":"IF(AS76<G76,IF(AS76<0,0,AS76),G76)","v":1.9350500511232744},null,{"$f":"IF(move1,Gewicht/K76,MAX(Gewicht,Gewicht2)/K76)","v":9.5238095238095233E-2},{"$f":"IF(move1,IF(AccType=1,SQRT((V76^2*Ltime1+W76^2*Ltime2+X76^2*Ltime3+Y76^2*Ltime4)/ltime)/C76,SQRT((((V76-W76)*2/PI()+W76)^2*Ltime1+W76^2*Ltime2+((X76-W76)*2/PI()+W76)^2*Ltime3+Y76^2*Ltime4)/ltime)/C76),IF(AccType=1,SQRT((V76^2*Ltime1+W76^2*Ltime2+X76^2*Ltime3+Y76^2*Ltime4+Z76^2*Ltime5+AA76^2*Ltime6+AB76^2*Ltime7+AC76^2*Ltime8)/ltime)/C76,SQRT((((V76-W76)*2/PI()+W76)^2*Ltime1+W76^2*Ltime2+((X76-W76)*2/PI()+W76)^2*Ltime3+Y76^2*Ltime4+((Z76-AA76)*2/PI()+AA76)^2*Ltime5+AA76^2*Ltime6+((AB76-AA76)*2/PI()+AA76)^2*Ltime7+AC76^2*Ltime8)/ltime)/C76))","v":0.21804490109140398},{"$f":" IF(move1,MAX(ABS(V76),ABS(X76))/E76,MAX(ABS(V76),ABS(X76),ABS(Z76),ABS(AB76))/E76)","v":0.23657753214431815},{"$f":"IF(AW76>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW76,G76),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW76,G76)),\"NA\")","v":0.44342712917860633},{"$f":"((Gewicht+K76)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":1806.42},0,{"$f":"((Gewicht+K76)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-3010.7},0,{"$f":"((Gewicht2+K76)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K76)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,0.16685423050939321,0.21566425093579147,{"$f":"D76*S76","v":4.0045015322254374},{"$f":"IF(move1,IF(MAX(ABS(V76),ABS(X76))<=C76,MAX(ABS(V76),ABS(X76))/C76*D76,D76+(MAX(ABS(V76),ABS(X76))-C76)/(E76-C76)*(F76-D76)),IF(MAX(ABS(V76),ABS(X76),ABS(Z76),ABS(AB76))<=C76,MAX(ABS(V76),ABS(X76),ABS(Z76),ABS(AB76))/C76*D76,D76+(MAX(ABS(V76),ABS(X76),ABS(Z76),ABS(AB76))-C76)/(E76-C76)*(F76-D76)))","v":10.351884044917991},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V76),ABS(X76))<=C76,MAX(ABS(V76),ABS(X76))/C76*D76,D76+(MAX(ABS(V76),ABS(X76))-C76)/(E76-C76)*(F76-D76)),IF(MAX(ABS(V76),ABS(X76),ABS(Z76),ABS(AB76))<=C76,MAX(ABS(V76),ABS(X76),ABS(Z76),ABS(AB76))/C76*D76,D76+(MAX(ABS(V76),ABS(X76),ABS(Z76),ABS(AB76))-C76)/(E76-C76)*(F76-D76))),IF(move1,IF(MAX(ABS((V76-W76)*2/PI()+W76),ABS((X76-W76)*2/PI()+W76))<=C76,MAX(ABS((V76-W76)*2/PI()+W76),ABS((X76-W76)*2/PI()+W76))/C76*D76,D76+(MAX(ABS((V76-W76)*2/PI()+W76),ABS((X76-W76)*2/PI()+W76))-C76)/(E76-C76)*(F76-D76)),IF(MAX(ABS((V76-W76)*2/PI()+W76),ABS((X76-W76)*2/PI()+W76),ABS((Z76-AA76)*2/PI()+AA76),ABS((AB76-AA76)*2/PI()+AA76))<=C76,MAX(ABS((V76-W76)*2/PI()+W76),ABS((X76-W76)*2/PI()+W76),ABS((Z76-AA76)*2/PI()+AA76),ABS((AB76-AA76)*2/PI()+AA76))/C76*D76,D76+(MAX(ABS((V76-W76)*2/PI()+W76),ABS((X76-W76)*2/PI()+W76),ABS((Z76-AA76)*2/PI()+AA76),ABS((AB76-AA76)*2/PI()+AA76))-C76)/(E76-C76)*(F76-D76))))","v":6.5902140642512892},1389.5538461538461,221.15436330773969,1916.6711486670772,{"$f":"(J76^2)+3*(I76/1000)^2*(F76/2)^2*(2000*PI()/M76)^2","v":146132.64196712643},{"$f":"SQRT(3)*H76*F76/2*J76","v":13349.369969792322},{"$f":"3*F76^2*H76^2/4-(UAC_V*0.98)^2","v":-147343.57},0.95949747251001527,{"$f":"(J76^2)+3*(I76/1000)^2*(D76/2)^2*(2000*PI()/M76)^2","v":38815.903226360802},{"$f":"SQRT(3)*H76*D76/2*J76","v":4006.0085896607002},{"$f":"3*D76^2*H76^2/4-(UAC_V*0.98)^2","v":-153094.82103806938},1.9350500511232744,{"$f":"(J76^2)+3*(I76/1000)^2*(AH76/2)^2*(2000*PI()/M76)^2","v":29562.74766533625},{"$f":"SQRT(3)*H76*AH76/2*J76","v":1437.5033615003133},{"$f":"3*AH76^2*H76^2/4-(UAC_V*0.98)^2","v":-153590.71032011614},2.2551619740821356,null,237.46655638071138]
["ICH","ICH44-250-A5",5341.3447862142475,31.80996243472952,12726.060554911015,106,"NA",0.5,11,96.945315684766314,52.5,675,32,{"$f":"IF(G77=\"NA\",(UAC_V*0.98)/J77,(IF((UAC_V*0.98)/J77<G77,(UAC_V*0.98)/J77,G77)))","v":4.0435166694866691},{"$f":"IF(AO77<G77,IF(AO77<0,0,AO77),G77)","v":1.718841341578933},{"$f":"IF(AS77<G77,IF(AS77<0,0,AS77),G77)","v":3.3928665981723491},null,{"$f":"IF(move1,Gewicht/K77,MAX(Gewicht,Gewicht2)/K77)","v":9.5238095238095233E-2},{"$f":"IF(move1,IF(AccType=1,SQRT((V77^2*Ltime1+W77^2*Ltime2+X77^2*Ltime3+Y77^2*Ltime4)/ltime)/C77,SQRT((((V77-W77)*2/PI()+W77)^2*Ltime1+W77^2*Ltime2+((X77-W77)*2/PI()+W77)^2*Ltime3+Y77^2*Ltime4)/ltime)/C77),IF(AccType=1,SQRT((V77^2*Ltime1+W77^2*Ltime2+X77^2*Ltime3+Y77^2*Ltime4+Z77^2*Ltime5+AA77^2*Ltime6+AB77^2*Ltime7+AC77^2*Ltime8)/ltime)/C77,SQRT((((V77-W77)*2/PI()+W77)^2*Ltime1+W77^2*Ltime2+((X77-W77)*2/PI()+W77)^2*Ltime3+Y77^2*Ltime4+((Z77-AA77)*2/PI()+AA77)^2*Ltime5+AA77^2*Ltime6+((AB77-AA77)*2/PI()+AA77)^2*Ltime7+AC77^2*Ltime8)/ltime)/C77))","v":0.21804490109140398},{"$f":" IF(move1,MAX(ABS(V77),ABS(X77))/E77,MAX(ABS(V77),ABS(X77),ABS(Z77),ABS(AB77))/E77)","v":0.23657753214431815},{"$f":"IF(AW77>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW77,G77),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW77,G77)),\"NA\")","v":0.25482047346298092},{"$f":"((Gewicht+K77)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":1806.42},0,{"$f":"((Gewicht+K77)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-3010.7},0,{"$f":"((Gewicht2+K77)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K77)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,0.28900000470007808,0.37354143999707462,{"$f":"D77*S77","v":6.9360001128018745},{"$f":"IF(move1,IF(MAX(ABS(V77),ABS(X77))<=C77,MAX(ABS(V77),ABS(X77))/C77*D77,D77+(MAX(ABS(V77),ABS(X77))-C77)/(E77-C77)*(F77-D77)),IF(MAX(ABS(V77),ABS(X77),ABS(Z77),ABS(AB77))<=C77,MAX(ABS(V77),ABS(X77),ABS(Z77),ABS(AB77))/C77*D77,D77+(MAX(ABS(V77),ABS(X77),ABS(Z77),ABS(AB77))-C77)/(E77-C77)*(F77-D77)))","v":17.929989119859581},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V77),ABS(X77))<=C77,MAX(ABS(V77),ABS(X77))/C77*D77,D77+(MAX(ABS(V77),ABS(X77))-C77)/(E77-C77)*(F77-D77)),IF(MAX(ABS(V77),ABS(X77),ABS(Z77),ABS(AB77))<=C77,MAX(ABS(V77),ABS(X77),ABS(Z77),ABS(AB77))/C77*D77,D77+(MAX(ABS(V77),ABS(X77),ABS(Z77),ABS(AB77))-C77)/(E77-C77)*(F77-D77))),IF(move1,IF(MAX(ABS((V77-W77)*2/PI()+W77),ABS((X77-W77)*2/PI()+W77))<=C77,MAX(ABS((V77-W77)*2/PI()+W77),ABS((X77-W77)*2/PI()+W77))/C77*D77,D77+(MAX(ABS((V77-W77)*2/PI()+W77),ABS((X77-W77)*2/PI()+W77))-C77)/(E77-C77)*(F77-D77)),IF(MAX(ABS((V77-W77)*2/PI()+W77),ABS((X77-W77)*2/PI()+W77),ABS((Z77-AA77)*2/PI()+AA77),ABS((AB77-AA77)*2/PI()+AA77))<=C77,MAX(ABS((V77-W77)*2/PI()+W77),ABS((X77-W77)*2/PI()+W77),ABS((Z77-AA77)*2/PI()+AA77),ABS((AB77-AA77)*2/PI()+AA77))/C77*D77,D77+(MAX(ABS((V77-W77)*2/PI()+W77),ABS((X77-W77)*2/PI()+W77),ABS((Z77-AA77)*2/PI()+AA77),ABS((AB77-AA77)*2/PI()+AA77))-C77)/(E77-C77)*(F77-D77))))","v":11.414585592038218},1389.5538461538461,221.15436330773969,1916.6711486670772,{"$f":"(J77^2)+3*(I77/1000)^2*(F77/2)^2*(2000*PI()/M77)^2","v":48709.761072459543},{"$f":"SQRT(3)*H77*F77/2*J77","v":4449.7266265282096},{"$f":"3*F77^2*H77^2/4-(UAC_V*0.98)^2","v":-151557.25},1.718841341578933,{"$f":"(J77^2)+3*(I77/1000)^2*(D77/2)^2*(2000*PI()/M77)^2","v":12938.634408786933},{"$f":"SQRT(3)*H77*D77/2*J77","v":1335.3361965535667},{"$f":"3*D77^2*H77^2/4-(UAC_V*0.98)^2","v":-153474.27367935647},3.3928665981723491,{"$f":"(J77^2)+3*(I77/1000)^2*(AH77/2)^2*(2000*PI()/M77)^2","v":9854.2492217787512},{"$f":"SQRT(3)*H77*AH77/2*J77","v":479.16778716677101},{"$f":"3*AH77^2*H77^2/4-(UAC_V*0.98)^2","v":-153639.57010670539},3.9243314573986736,null,137.10138024993716]
["IL","IL06-015A1",21,2.5,60,7.2,"NA",4.2,0.5,4.8790367901871781,0.23,330,32,{"$f":"IF(G78=\"NA\",(UAC_V*0.98)/J78,(IF((UAC_V*0.98)/J78<G78,(UAC_V*0.98)/J78,G78)))","v":80.343727021775834},{"$f":"IF(AO78<G78,IF(AO78<0,0,AO78),G78)","v":76.942289135179664},{"$f":"IF(AS78<G78,IF(AS78<0,0,AS78),G78)","v":79.32127838373971},null,{"$f":"IF(move1,Gewicht/K78,MAX(Gewicht,Gewicht2)/K78)","v":21.739130434782609},{"$f":"IF(move1,IF(AccType=1,SQRT((V78^2*Ltime1+W78^2*Ltime2+X78^2*Ltime3+Y78^2*Ltime4)/ltime)/C78,SQRT((((V78-W78)*2/PI()+W78)^2*Ltime1+W78^2*Ltime2+((X78-W78)*2/PI()+W78)^2*Ltime3+Y78^2*Ltime4)/ltime)/C78),IF(AccType=1,SQRT((V78^2*Ltime1+W78^2*Ltime2+X78^2*Ltime3+Y78^2*Ltime4+Z78^2*Ltime5+AA78^2*Ltime6+AB78^2*Ltime7+AC78^2*Ltime8)/ltime)/C78,SQRT((((V78-W78)*2/PI()+W78)^2*Ltime1+W78^2*Ltime2+((X78-W78)*2/PI()+W78)^2*Ltime3+Y78^2*Ltime4+((Z78-AA78)*2/PI()+AA78)^2*Ltime5+AA78^2*Ltime6+((AB78-AA78)*2/PI()+AA78)^2*Ltime7+AC78^2*Ltime8)/ltime)/C78))","v":5.0444183577764381},{"$f":" IF(move1,MAX(ABS(V78),ABS(X78))/E78,MAX(ABS(V78),ABS(X78),ABS(Z78),ABS(AB78))/E78)","v":4.564046666666667},{"$f":"IF(AW78>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW78,G78),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW78,G78)),\"NA\")","v":1.4828253838631178E-2},{"$f":"((Gewicht+K78)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":164.30568000000002},0,{"$f":"((Gewicht+K78)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-273.84280000000001},0,{"$f":"((Gewicht2+K78)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K78)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,0.52546024560171223,0.68689164529914537,{"$f":"D78*S78","v":12.611045894441094},{"$f":"IF(move1,IF(MAX(ABS(V78),ABS(X78))<=C78,MAX(ABS(V78),ABS(X78))/C78*D78,D78+(MAX(ABS(V78),ABS(X78))-C78)/(E78-C78)*(F78-D78)),IF(MAX(ABS(V78),ABS(X78),ABS(Z78),ABS(AB78))<=C78,MAX(ABS(V78),ABS(X78),ABS(Z78),ABS(AB78))/C78*D78,D78+(MAX(ABS(V78),ABS(X78),ABS(Z78),ABS(AB78))-C78)/(E78-C78)*(F78-D78)))","v":32.970798974358978},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V78),ABS(X78))<=C78,MAX(ABS(V78),ABS(X78))/C78*D78,D78+(MAX(ABS(V78),ABS(X78))-C78)/(E78-C78)*(F78-D78)),IF(MAX(ABS(V78),ABS(X78),ABS(Z78),ABS(AB78))<=C78,MAX(ABS(V78),ABS(X78),ABS(Z78),ABS(AB78))/C78*D78,D78+(MAX(ABS(V78),ABS(X78),ABS(Z78),ABS(AB78))-C78)/(E78-C78)*(F78-D78))),IF(move1,IF(MAX(ABS((V78-W78)*2/PI()+W78),ABS((X78-W78)*2/PI()+W78))<=C78,MAX(ABS((V78-W78)*2/PI()+W78),ABS((X78-W78)*2/PI()+W78))/C78*D78,D78+(MAX(ABS((V78-W78)*2/PI()+W78),ABS((X78-W78)*2/PI()+W78))-C78)/(E78-C78)*(F78-D78)),IF(MAX(ABS((V78-W78)*2/PI()+W78),ABS((X78-W78)*2/PI()+W78),ABS((Z78-AA78)*2/PI()+AA78),ABS((AB78-AA78)*2/PI()+AA78))<=C78,MAX(ABS((V78-W78)*2/PI()+W78),ABS((X78-W78)*2/PI()+W78),ABS((Z78-AA78)*2/PI()+AA78),ABS((AB78-AA78)*2/PI()+AA78))/C78*D78,D78+(MAX(ABS((V78-W78)*2/PI()+W78),ABS((X78-W78)*2/PI()+W78),ABS((Z78-AA78)*2/PI()+AA78),ABS((AB78-AA78)*2/PI()+AA78))-C78)/(E78-C78)*(F78-D78))))","v":20.978681607752698},126.38898461538462,20.115431653903975,174.33374100050111,{"$f":"(J78^2)+3*(I78/1000)^2*(F78/2)^2*(2000*PI()/M78)^2","v":24.179736542103861},{"$f":"SQRT(3)*H78*F78/2*J78","v":127.77518294254169},{"$f":"3*F78^2*H78^2/4-(UAC_V*0.98)^2","v":-152978.1568},76.942289135179664,{"$f":"(J78^2)+3*(I78/1000)^2*(D78/2)^2*(2000*PI()/M78)^2","v":23.850179463505963},{"$f":"SQRT(3)*H78*D78/2*J78","v":44.366382966160316},{"$f":"3*D78^2*H78^2/4-(UAC_V*0.98)^2","v":-153581.3125},79.32127838373971,{"$f":"(J78^2)+3*(I78/1000)^2*(AH78/2)^2*(2000*PI()/M78)^2","v":26.98639383855738},{"$f":"SQRT(3)*H78*AH78/2*J78","v":372.29928893387995},{"$f":"3*AH78^2*H78^2/4-(UAC_V*0.98)^2","v":-147841.40976514714},67.438823942624907,null,6.9]
["IL","IL06-015A4",21,4.9000000000000004,60,14.4,"NA",1.1000000000000001,0.13,2.4041630560342613,0.23,330,32,163.05050483830979,158.76135704715449,161.90777809522871,null,21.739130434782609,5.0444183577764381,4.564046666666667,6.9404349830376119E-3,164.30568000000002,0,-273.84280000000001,0,0,0,0,0,1.0299020813793562,1.3852065170940173,24.717649953104548,66.489912820512828,42.250526653968215,126.38898461538462,20.115431653903975,174.33374100050111,5.881328760984883,32.979929896832708,-153475.82079999999,158.76135704715449,5.7917327524655029,11.222337256561131,-153642.21092499999,161.90777809522871,6.6523123109210225,96.765236607787045,-152044.01539519706,144.08318822148684,null,3.4]
["IL","IL06-030A1",38,2.2999999999999998,120,7.1,"NA",6.1,1.3,9.6873629022556997,0.27,330,32,40.465088791989295,37.919304884007239,39.769497057086987,null,18.518518518518519,2.8090257605671654,2.2994766666666662,2.7464199130080306E-2,165.56232,0,-275.93719999999996,0,0,0,0,0,0.2691983020543533,0.33808398373983733,6.4607592493044796,16.228031219512193,10.358560631321819,127.35563076923074,20.269278167509356,175.66707745174776,96.30834049057097,363.34934760279248,-152257.182925,37.919304884007239,94.103501709881357,117.70471823752433,-153516.36932500001,39.769497057086987,99.088322528182317,530.10933063306379,-150669.53143562007,36.411038066817135,null,13.7]
["IL","IL06-030A4",38,4.5,120,14.2,"NA",1.5,0.33,4.8790367901871781,0.27,330,32,80.343727021775834,77.385527909046488,79.632181871554835,null,18.518518518518519,2.8090257605671654,2.2994766666666662,1.3265600803628711E-2,165.56232,0,-275.93719999999996,0,0,0,0,0,0.52669233010634353,0.68012978658536571,12.640615922552245,32.646229756097554,20.785007942462844,127.35563076923074,20.269278167509356,175.66707745174776,24.439929655439482,90.000376874210914,-153323.73250000001,77.385527909046488,23.868763764742361,28.521246192531631,-153629.828125,79.632181871554835,25.16534577721248,131.73651747571293,-152934.97206315357,75.382940795750244,null,6.9]
["IL","IL06-050A1",61,2.1,200,7,"NA",8.6,3,16.475588001646557,0.32,330,32,23.79277753005379,21.584613497007631,23.25578631196791,null,15.625,1.7664872235551008,1.392776,4.5681181074183515E-2,167.13312000000002,0,-278.55520000000001,0,0,0,0,0,0.15456763206107133,0.20352525179856118,3.7096231694657118,9.7692120863309366,6.2009738509169061,128.56393846153847,20.46158630951609,177.33374801580612,284.19645177992305,858.95032065306305,-150945.97,21.584613497007631,272.59263066019309,257.68509619591896,-153419.37729999999,23.25578631196791,281.4515265688741,760.90406822947648,-151531.06330546457,21.890852567407563,null,23.3]
["IL","IL06-050A4",61,4.3,200,14,"NA",2.2000000000000002,0.75,8.2024386617639511,0.32,330,32,47.790665211228728,45.062391500874234,47.179212355459917,null,15.625,1.7664872235551008,1.392776,2.1993167165375971E-2,167.13312000000002,0,-278.55520000000001,0,0,0,0,0,0.31649562755362221,0.40587311750599525,7.5958950612869334,19.481909640287771,12.418254357937549,128.56393846153847,20.46158630951609,177.33374801580612,70.467862944980766,218.78842382539347,-152952.51999999999,45.062391500874234,67.58073258088109,67.199301603513703,-153596.88130000001,47.179212355459917,69.788214489735054,194.06930697399855,-153104.20666008667,45.46866726745516,null,11.6]
["IL","IL06-075A1",87,2,300,7,"NA",11.7,5,24.678026663410506,0.38,330,32,15.884576402586054,13.889517812293899,15.422438682886954,null,13.157894736842104,1.2525403530946178,0.93898933333333334,6.7494461677004985E-2,169.01808,0,-281.6968,0,0,0,0,0,0.10437836275788481,0.1368822378716745,2.5050807061892355,6.5703474178403756,4.167458983396152,130.0139076923077,20.692356079924163,179.33375269267609,644.42569938867507,1750.3502566736461,-148633.29250000001,13.889517812293899,611.89648566438154,500.10007333532741,-153253.32999999999,15.422438682886954,621.55962428697455,1042.0732716091923,-151880.900184067,14.816030458699027,null,34.9]
["IL","IL06-075A4",87,4.0999999999999996,300,14,"NA",2.9,1.25,12.37436867076458,0.38,330,32,31.678383797157334,29.36251370919803,31.177914822154722,null,13.157894736842104,1.2525403530946178,0.93898933333333334,3.2802086411969432E-2,169.01808,0,-281.6968,0,0,0,0,0,0.21397564365366384,0.27394349765258214,5.1354154476879321,13.149287887323943,8.3915687871243811,130.0139076923077,20.692356079924163,179.33375269267609,161.98017484716877,435.09061556186191,-152427.73000000001,29.36251370919803,153.88446678153522,127.4193945574024,-153557.970925,31.177914822154722,156.30646673964839,260.79234493711812,-153219.83577353272,30.485865668444234,null,17.5]
["IL","IL06-100A1",113,2,400,7,"NA",14.7,7,32.880465325174455,0.45,330,32,11.921972396779642,10.052559622902207,11.486829185802709,null,11.111111111111111,0.97689247034216065,0.71340500000000007,8.9411820296708591E-2,171.21720000000002,0,-285.36200000000002,0,0,0,0,0,8.1407705861846716E-2,0.10422546457607434,1.9537849406843213,5.0028222996515685,3.1962907923755708,131.70553846153848,20.961587478733588,181.66709148235776,1150.5495708018032,2930.1102489390219,-145722.6925,10.052559622902207,1086.7923119021877,837.17435683972042,-153015.73000000001,11.486829185802709,1095.5997039842057,1337.9263441898695,-152008.27387908217,11.184203572654608,null,46.5]
["IL","IL06-100A4",113,4,400,14,"NA",3.7,1.75,16.475588001646557,0.45,330,32,23.79277753005379,21.671322535873426,23.3344381393883,null,11.111111111111111,0.97689247034216065,0.71340500000000007,4.3482093504876231E-2,171.21720000000002,0,-285.36200000000002,0,0,0,0,0,0.16281541172369343,0.20845092915214869,3.9075698813686426,10.005644599303137,6.3925815847511416,131.70553846153848,20.961587478733588,181.66709148235776,288.80114270045084,739.09678753868218,-151651.57,21.671322535873426,272.86182797554699,211.17051072533778,-153499.72,23.3344381393883,275.06367599605147,337.48117952632191,-153244.41759275552,22.997972714626922,null,23.3]
["IL","IL12-015A1",41,2.4,120,7.1,"NA",8.5,1,9.6873629022556997,0.35,330,32,40.465088791989295,37.228193988663293,39.488166134754699,null,14.285714285714286,2.6430089189767423,2.3343833333333333,2.832488072338761E-2,168.07559999999998,0,-280.12599999999998,0,0,0,0,0,0.26430089189767419,0.34638507383966233,6.3432214055441811,16.626483544303792,10.570488945125735,129.28892307692306,20.576971194720127,178.33375035424109,95.302597923414766,506.30646797110433,-150932.40812499999,37.228193988663293,94.011549574268358,171.14584832826063,-153351.88,39.488166134754699,97.075808346588815,753.78970739918532,-147609.34687004157,35.304649991846517,null,13.7]
["IL","IL12-015A2",41,4.9000000000000004,120,14.3,"NA",2.1,0.25,4.8790367901871781,0.35,330,32,80.343727021775834,76.970480513673309,79.34346464614606,null,14.285714285714286,2.6430089189767423,2.3343833333333333,1.335415595682771E-2,168.07559999999998,0,-280.12599999999998,0,0,0,0,0,0.53961432095775164,0.6948534810126582,12.950743702986038,33.352967088607592,21.240977890251472,129.28892307692306,20.576971194720127,178.33375035424109,24.174549939693378,126.88785528321849,-152987.64932500001,76.970480513673309,23.848390356751128,43.479055306837104,-153584.58692500001,79.34346464614606,24.620361262745195,188.47707193092813,-152171.7249887143,74.88305537488651,null,6.9]
["IL","IL12-015A4",41,9.8000000000000007,120,28.6,"NA",0.5,0.06,2.4041630560342613,0.35,330,32,163.05050483830979,159.26361306569831,162.02150437279059,null,14.285714285714286,2.6430089189767423,2.3343833333333333,6.3846987265077561E-3,168.07559999999998,0,-280.12599999999998,0,0,0,0,0,1.0792286419155033,1.3897069620253164,25.901487405972077,66.705934177215184,42.481955780502943,129.28892307692306,20.576971194720127,178.33375035424109,5.8651443061053525,29.773547823529526,-153510.63250000001,159.26361306569831,5.7899971381954582,10.202124778691935,-153645.99249999999,162.02150437279059,5.9678592349364923,44.225123848526948,-153325.61564369939,156.62446151894952,null,3.4]
["IL","IL12-030A1",76,2.2999999999999998,240,7.1,"NA",12.2,2.6,19.445436482630054,0.42,330,32,20.15897150728194,17.743915967776662,19.479267453774145,null,11.904761904761905,1.4444895277299847,1.1824633333333334,5.4298261166321742E-2,170.27472,0,-283.7912,0,0,0,0,0,0.13843024640745685,0.17461861788617886,3.3223259137789647,8.3816936585365855,5.3634269993343242,130.98055384615387,20.846202593529551,180.66708914392277,387.97836196228388,1458.7017604491668,-148036.7317,17.743915967776662,379.15900683952543,472.53719000465969,-153073.4773,19.479267453774145,383.74779807134064,1101.9211839393763,-150452.81244135046,18.416796017406273,null,27.5]
["IL","IL12-030A2",76,4.5,240,14.2,"NA",3.1,0.65,9.7580735803743561,0.42,330,32,40.171863510887917,37.615884993980771,39.488051764139847,null,11.904761904761905,1.4444895277299847,1.1824633333333334,2.6075263663583759E-2,170.27472,0,-283.7912,0,0,0,0,0,0.27084178644937212,0.34979352642276423,6.5002028747849314,16.790089268292682,10.690675394488114,130.98055384615387,20.846202593529551,180.66708914392277,97.683340490570998,372.00155774673851,-152210.67970000001,37.615884993980771,95.467384670373249,117.8878175957974,-153518.048125,39.488051764139847,96.616233464752526,280.06675352917648,-152840.25093013683,38.350523043668467,null,13.8]
["IL","IL12-030A4",76,9,240,28.5,"NA",0.8,0.16,4.8790367901871781,0.42,330,32,80.343727021775834,77.298132509326877,79.597724280582682,null,11.904761904761905,1.4444895277299847,1.1824633333333334,1.2782654259917007E-2,170.27472,{"$f":"(Ltorque+IF(Lspeed2=0,0,IF(Lspeed2>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},-283.7912,{"$f":"(Ltorque+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},0,{"$f":"(Ltorque2+IF(Lspeed6=0,0,IF(Lspeed6>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},0,0,0.54168357289874425,0.70222667682926831,13.000405749569863,33.706880487804881,21.445172184795695,130.98055384615387,20.846202593529551,180.66708914392277,24.406243963108864,96.338431583662398,-153274.12,77.298132509326877,23.864957846736619,30.422662605367073,-153625.12,79.597724280582682,24.145423932219565,72.491026432449118,-153443.25020318295,78.231013658542977,null,6.9]
["IL","IL12-050A1",122,2.1,400,7,"NA",17.2,6,32.880465325174455,0.52,330,32,11.921972396779642,9.8180758210203543,11.394595759513235,null,9.615384615384615,0.91644825883685666,0.72256799999999999,9.023780882856404E-2,173.41631999999998,0,-289.02719999999999,0,0,0,0,0,8.0189222648224964E-2,0.10508342925659471,1.924541343557399,5.0440046043165463,3.1928133393273135,133.39716923076921,21.230818877543008,184.00043027203941,1132.130807119692,3428.4283184864744,-142791.88,9.8180758210203543,1085.7155226407722,1028.5284955459424,-152685.5092,11.394595759513235,1091.7363491044564,1563.7616668844466,-151402.1426284498,11.08182936821775,null,46.5]
["IL","IL12-050A2",122,4.3,400,14,"NA",4.3,1.5,16.475588001646557,0.52,330,32,23.79277753005379,21.584613497007631,23.241538985311021,null,9.615384615384615,0.91644825883685666,0.72256799999999999,4.3634297269761424E-2,173.41631999999998,0,-289.02719999999999,0,0,0,0,0,0.16419697970827016,0.21099848920863309,3.9407275129984836,10.127927482014389,6.4633243656071304,133.39716923076921,21.230818877543008,184.00043027203941,284.19645177992305,858.95032065306305,-150945.97,21.584613497007631,272.64793032352435,263.82045562915505,-153407.58992500001,23.241538985311021,274.16278730164333,396.54818116592855,-153084.69126347508,22.917751919268337,null,23.3]
["IL","IL12-050A4",122,8.6,400,28.1,"NA",1.1000000000000001,0.38,8.2024386617639511,0.52,330,32,47.790665211228728,45.022613469519229,47.176424043374489,null,9.615384615384615,0.91644825883685666,0.72256799999999999,2.1375732194671752E-2,173.41631999999998,0,-289.02719999999999,0,0,0,0,0,0.32839395941654032,0.4232486810551559,7.8814550259969671,20.315936690647483,12.948951044261758,133.39716923076921,21.230818877543008,184.00043027203941,70.576862817433252,219.56981105334131,-152947.42892499999,45.022613469519229,67.588805579941194,67.199301603513703,-153596.88130000001,47.176424043374489,67.980095707060514,101.18144961307904,-153511.83463516939,46.782023225818023,null,11.6]
["IL","IL12-075A1",174,2,600,7,"NA",23.3,10,49.356053326821012,0.65,330,32,7.9422882012930272,5.9758628345424016,7.4849939900739573,null,7.6923076923076916,0.65770009247068695,0.4930566666666667,0.13436701754109157,177.50040000000001,0,-295.834,0,0,0,0,0,5.4808341039223912E-2,7.145784428794992E-2,1.3154001849413739,3.4299765258215964,2.1682367809693788,136.53876923076925,21.73082004676051,188.33377373859108,2577.7027975547003,6971.4805094864887,-133712.79250000001,5.9758628345424016,2447.5859426575262,1991.8515741389967,-152035.32999999999,7.4849939900739573,2449.6135991145975,2159.4029226399639,-151749.8034899935,7.4423025702284731,null,69.8]
["IL","IL12-075A2",174,4.0999999999999996,600,14,"NA",5.8,2.5,24.678026663410506,0.65,330,32,15.884576402586054,13.904452670813622,15.413485986736379,null,7.6923076923076916,0.65770009247068695,0.4930566666666667,6.505881564358991E-2,177.50040000000001,0,-295.834,0,0,0,0,0,0.11235709913040902,0.14440319835680751,2.6965703791298163,6.931353521126761,4.4331088263193701,136.53876923076925,21.73082004676051,188.33377373859108,644.42569938867507,1735.3899980695976,-148718.92000000001,13.904452670813622,612.04286712614089,508.221356577525,-153239.88370000001,15.413485986736379,612.55654928896445,549.51233696776342,-153168.16858896107,15.370707107216262,null,34.9]
["IL","IL12-075A4",174,8.1,600,28.1,"NA",1.5,0.63,12.37436867076458,0.65,330,32,31.678383797157334,29.28602874507509,31.16914952722572,null,7.6923076923076916,0.65770009247068695,0.4930566666666667,3.2134154327859037E-2,177.50040000000001,0,-295.834,0,0,0,0,0,0.22197378120885683,0.28791471048513301,5.3273707490125641,13.819906103286385,8.7729471238775147,136.53876923076925,21.73082004676051,188.33377373859108,162.18680645595052,451.70121788011045,-152331.53312499999,29.28602874507509,153.87796047615265,130.2056891398183,-153553.28312499999,31.16914952722572,154.00826936130662,141.02316371008132,-153534.12223541029,31.119536857798671,null,17.5]
["IL","IL12-100A2",226,4,800,14,"NA",7.4,3.5,32.880465325174455,0.77,330,32,11.921972396779642,10.040714324827764,11.483951390897259,null,6.4935064935064934,0.51712564714442799,0.37764649999999994,8.6542089933652255E-2,181.27032,0,-302.11719999999997,0,0,0,0,0,8.6187607857404661E-2,0.11096007549361207,2.068502588577712,5.3260836236933793,3.4041377538465669,139.43870769230767,22.192359587576657,192.33378309233103,1150.5495708018032,2950.0429717209199,-145614.28,10.040714324827764,1086.7923119021877,842.86942049169147,-153006.88,11.483951390897259,1085.2296051389008,717.31090396463594,-153188.07452149698,11.555071073123528,null,46.5]
["IL","IL12-100A4",226,7.9,800,28.1,"NA",1.8,0.88,16.475588001646557,0.77,330,32,23.79277753005379,21.695341797717376,23.351150821927849,null,6.4935064935064934,0.51712564714442799,0.37764649999999994,4.2688901300954395E-2,181.27032,0,-302.11719999999997,0,0,0,0,0,0.17022052551837422,0.22038935249709637,4.0852926124409814,10.578688919860626,6.7231720638469703,139.43870769230767,22.192359587576657,192.33378309233103,289.12568258878332,721.68948868159362,-151745.24770000001,21.695341797717376,272.84246381171204,202.8949096293448,-153512.3437,23.351150821927849,272.45712660287268,172.67055548313502,-153554.16146648178,23.42529251221659,null,23.3]
["IL","IL18-015A1",62,2.4,180,7.1,"NA",12.7,1.5,14.637110370561532,0.46,330,32,26.781242340591948,23.550753494247562,25.812165383751797,null,10.869565217391305,1.7837322176729984,1.5882533333333333,4.253768817142841E-2,171.53136000000001,0,-285.88560000000001,0,0,0,0,0,0.17837322176729983,0.23578077683615817,4.2809573224151958,11.317477288135592,7.1796779686211547,131.94720000000001,21.000049107134934,182.00042559516942,217.52459532768322,1143.0047863024784,-147566.02832499999,23.550753494247562,214.61973654210382,386.36781508816171,-152967.22719999999,25.812165383751797,217.59861722766814,1155.8318707386529,-147428.39443900576,23.508564827734975,null,20.7]
["IL","IL18-015A2",62,4.9000000000000004,180,14.2,"NA",3.2,0.38,7.2831998462214393,0.46,330,32,53.822496742743034,50.537778409317319,52.81701705229306,null,10.869565217391305,1.7837322176729984,1.5882533333333333,1.9803806562592955E-2,171.53136000000001,0,-285.88560000000001,0,0,0,0,0,0.36417866110823721,0.46969210451977395,8.7402878665976935,22.545221016949149,14.357660661314199,131.94720000000001,21.000049107134934,182.00042559516942,53.886908560564379,286.60989582357411,-152115.40479999999,50.537778409317319,53.145249080237797,98.900597854613608,-153479.60320000001,52.81701705229306,53.905707537253498,289.79208636686553,-152080.82621696935,50.495342743292674,null,10.3]
["IL","IL18-015A3",62,7.3,180,21.3,"NA",1.4,0.17,4.8790367901871781,0.46,330,32,80.343727021775834,76.975941534478778,79.348000416377516,null,10.869565217391305,1.7837322176729984,1.5882533333333333,1.2998674188650772E-2,171.53136000000001,0,-285.88560000000001,0,0,0,0,0,0.54255188287553702,0.70547288135593222,13.021245189012888,33.862698305084749,21.537338629935356,131.94720000000001,21.000049107134934,182.00042559516942,24.184121219880186,126.00052762389528,-152997.07569999999,76.975941534478778,23.849531221334864,43.183279420396033,-153585.6637,79.348000416377516,24.192617127836787,127.40450849701205,-152982.13027576706,76.930922760807917,null,6.9]
["IL","IL18-015A4",62,14.7,180,42.6,"NA",0.4,0.04,2.4041630560342613,0.46,330,32,163.05050483830979,158.7674641884951,161.84214979174905,null,10.869565217391305,1.7837322176729984,1.5882533333333333,6.3009170025955484E-3,171.53136000000001,0,-285.88560000000001,0,0,0,0,{"$f":"(Ltorque2+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},1.0925359833247115,1.4090763135593223,26.220863599793073,67.635663050847469,43.072981983942597,131.94720000000001,21.000049107134934,182.00042559516942,5.8639576403886906,35.478409434471544,-153446.22880000001,158.7674641884951,5.7899971381954582,12.242549734430321,-153638.0692,161.84214979174905,5.8658323305848361,35.872321370655683,-153441.36618676133,158.7070579707792,null,3.4]
["IL","IL18-030A1",114,2.2999999999999998,360,7.1,"NA",18.2,3.8,29.132799384885757,0.56999999999999995,330,32,13.455624185685759,11.001638072291037,12.774377445471517,null,8.7719298245614041,0.98964411678425757,0.81012555555555554,8.1268566054067917E-2,174.98712,0,-291.64519999999999,0,0,0,0,0,9.4840894525158023E-2,0.12013016260162601,2.2761814686037924,5.7662478048780486,3.6983824553384927,134.60547692307691,21.423127019549739,185.66710083609775,869.76771401410952,3260.1875649931549,-141140.64370000002,11.001638072291037,850.92873650336514,1056.1170985189092,-152349.80530000001,12.774377445471517,854.4309962776116,1698.2282382370995,-150265.96631498507,12.304880577500294,null,41.2]
["IL","IL18-030A2",114,4.5,360,14.3,"NA",4.5999999999999996,0.95,14.566399692442879,0.56999999999999995,330,32,26.911248371371517,24.458562034761485,26.242878054261013,null,8.7719298245614041,0.98964411678425757,0.81012555555555554,3.8809801747827256E-2,174.98712,0,-291.64519999999999,0,0,0,0,0,0.18555827189704829,0.24118588753387535,4.4533985255291588,11.576922601626016,7.3550308463160894,134.60547692307691,21.423127019549739,185.66710083609775,217.51630112917235,829.80629169342888,-150418.74369999999,24.458562034761485,212.70843707695113,261.12785402940068,-153342.63250000001,26.242878054261013,213.59168321501915,426.80076027079269,-152805.48888223336,25.766686634929393,null,20.6]
["IL","IL18-030A3",114,6.8,360,21.4,"NA",2,0.42,9.6873629022556997,0.56999999999999995,330,32,40.465088791989295,37.968727199130491,39.794262224371856,null,8.7719298245614041,0.98964411678425757,0.81012555555555554,2.5436490051127598E-2,174.98712,0,-291.64519999999999,0,0,0,0,0,0.2803991664222063,0.36131605013550133,6.7295799941329513,17.343170406504065,11.053413301654581,134.60547692307691,21.423127019549739,185.66710083609775,96.180861942853397,359.07070139458602,-152290.12,37.968727199130491,94.080850852121429,114.09723221884042,-153525.28,39.794262224371856,94.468178472843064,185.46527416025032,-153297.46616314841,39.313600185795686,null,13.7]
["IL","IL18-030A4",114,13.6,360,42.8,"NA",0.5,0.11,4.8790367901871781,0.56999999999999995,330,32,80.343727021775834,77.367020873932191,79.626087025672575,null,8.7719298245614041,0.98964411678425757,0.81012555555555554,1.2647854975161325E-2,174.98712,0,-291.64519999999999,0,0,0,0,0,0.56079833284441261,0.72263210027100266,13.459159988265903,34.68634081300813,22.106826603309162,134.60547692307691,21.423127019549739,185.66710083609775,24.445905431032347,90.422913854841013,-153320.53,77.367020873932191,23.869711911806569,28.732514682846681,-153629.32,79.626087025672575,23.975985476675767,46.704758821376913,-153572.3665407871,79.064790192792742,null,6.9]
["IL","IL18-050A1",184,2.2000000000000002,600,7,"NA",25.7,9,49.356053326821012,0.72,330,32,7.9422882012930272,5.7726712826585933,7.3835602507261475,null,6.9444444444444446,0.62966116586593412,0.49916533333333329,0.135835668201919,179.69952000000001,0,-299.49919999999997,0,0,0,0,0,5.7718940204377296E-2,7.35975641025641E-2,1.3852545649050552,3.5326830769230768,2.2769282214800697,138.23039999999997,22.000051445569927,190.6671125282727,2550.7830660193072,7689.5729224808038,-129390.99249999999,5.7726712826585933,2447.3557803986414,2416.7229184939674,-151266.42129999999,7.3835602507261475,2448.1624057842987,2501.2293711893603,-151095.81567996144,7.361836645979503,null,69.8]
["IL","IL18-050A2",184,4.3,600,14,"NA",6.4,2.25,24.678026663410506,0.72,330,32,15.884576402586054,13.788430219103539,15.346635326695731,null,6.9444444444444446,0.62966116586593412,0.49916533333333329,6.5251935835327818E-2,179.69952000000001,0,-299.49919999999997,0,0,0,0,0,0.11281429221764654,0.14569021634615384,2.7075430132235168,6.9931303846153838,4.4554591142409734,138.23039999999997,22.000051445569927,190.6671125282727,637.69576650482679,1914.9131013181773,-147642.88,13.788430219103539,611.71159322792971,588.15188111915438,-153095.9872,15.346635326695731,611.91083536572899,609.41550216053724,-153054.17371897836,15.325215829973791,null,34.9]
["IL","IL18-050A3",184,6.5,600,21,"NA",2.9,1,16.475588001646557,0.72,330,32,23.79277753005379,21.563354576843022,23.230752838328726,null,6.9444444444444446,0.62966116586593412,0.49916533333333329,4.308804846710737E-2,179.69952000000001,0,-299.49919999999997,0,0,0,0,0,0.17053323242202381,0.21928778044871797,4.0927975781285717,10.525813461538462,6.7323873357210431,138.23039999999997,22.000051445569927,190.6671125282727,284.19645177992305,868.93811507926137,-150882.39249999999,21.563354576843022,272.66665269320123,268.95703561977137,-153397.50812499999,23.230752838328726,272.75556701194722,278.57276007071113,-153378.11231500519,23.208291755505748,null,23.3]
["IL","IL18-050A4",184,12.9,600,42.1,"NA",0.7,0.25,8.2024386617639511,0.72,330,32,47.790665211228728,45.131681488166805,47.202506397500791,null,6.9444444444444446,0.62966116586593412,0.49916533333333329,2.1196729282132405E-2,179.69952000000001,0,-299.49919999999997,0,0,0,0,0,0.33844287665293965,0.43764907051282048,8.1226290396705512,21.007155384615384,13.367980014003757,138.23039999999997,22.000051445569927,190.6671125282727,70.483061316504177,209.34074188747874,-153012.639325,45.131681488166805,67.58073258088109,64.144787894263075,-153602.84432500001,47.202506397500791,67.602948027262784,66.471801749846421,-153598.32668805186,47.177089761812503,null,11.6]
["IL","IL18-075A1",260,2,900,7,"NA",35,15,74.246212024587479,0.91,330,32,5.2797306328595557,3.1720732942221077,4.8134542947737708,null,5.4945054945054945,0.46040797351348278,0.34383066666666667,0.20255802099817294,185.66856000000001,0,-309.44760000000002,0,0,0,0,0,3.8367331126123567E-2,4.9714778645833339E-2,0.92081594702696556,2.3863093750000002,1.5153881590130338,142.82196923076924,22.730822385195506,197.00046067169438,5831.2862944980752,15753.280908274312,-108645.25,3.1720732942221077,5538.5233709794329,4500.9374023640885,-149989,4.8134542947737708,5527.4400255578266,3410.3336220007118,-151554.18133091184,4.9368570796266811,null,105]
["IL","IL18-075A2",260,4.0999999999999996,900,14,"NA",8.8000000000000007,3.75,37.052395334175088,0.91,330,32,10.579612909355978,8.6293146715028097,10.108598135481801,null,5.4945054945054945,0.46040797351348278,0.34383066666666667,9.7737563301753511E-2,185.66856000000001,0,-309.44760000000002,0,0,0,0,0,7.8653028808553307E-2,0.10135192838541666,1.8876726914052793,4.8648925624999997,3.1065457259767189,142.82196923076924,22.730822385195506,197.00046067169438,1452.5765736245191,3953.2804856726266,-142280.32000000001,8.6293146715028097,1379.715201033817,1157.7464279469834,-152687.6752,10.108598135481801,1376.8040910879231,877.2176140252476,-153103.4916217323,10.231480775846792,null,52.4]
["IL","IL18-075A3",260,6.1,900,21,"NA",3.9,1.67,24.678026663410506,0.91,330,32,15.884576402586054,13.888125763941678,15.413754052009669,null,5.4945054945054945,0.46040797351348278,0.34383066666666667,6.4361163058804127E-2,185.66856000000001,0,-309.44760000000002,0,0,0,0,0,0.11702035993467687,0.15106670703125,2.8084886384322449,7.2512019375000003,4.6219338849897529,142.82196923076924,22.730822385195506,197.00046067169438,644.56752386902735,1750.3502566736461,-148633.29250000001,13.888125763941678,612.00563835185142,508.43507455758288,-153239.52692500001,15.413754052009669,610.72766743235854,385.23824580573506,-153420.30987260945,15.537320217261167,null,34.9]
["IL","IL18-075A4",260,12.2,900,42.1,"NA",1,0.42,12.37436867076458,0.91,330,32,31.678383797157334,29.289775398337262,31.166717475516684,null,5.4945054945054945,0.46040797351348278,0.34383066666666667,3.1942866384801052E-2,185.66856000000001,0,-309.44760000000002,0,0,0,0,0,0.23404071986935374,0.30229437630208333,5.6169772768644899,14.5101300625,9.2438677699795058,142.82196923076924,22.730822385195506,197.00046067169438,162.16532025970136,451.1653919988766,-152334.6925,29.289775398337262,153.88417043316946,130.74151502105209,-153552.37,31.166717475516684,153.5608399871893,99.062071877163532,-153599.91318148834,31.305894341273536,null,17.5]
["IL","IL18-100A1",338,2,1200,7,"NA",44.2,21,98.994949366116643,1.1000000000000001,330,32,3.9597979746446668,1.8053869903983075,3.5078672337116168,null,4.545454545454545,0.3655458334546719,0.26616333333333331,0.27002539663563463,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,3.0462152787889326E-2,3.9373274161735694E-2,0.7310916669093438,1.8899171597633133,1.2031586320421064,147.41353846153845,23.461593324821077,203.33380881511599,10424.821137216228,26525.524424599029,-81867.729999999981,1.8053869903983075,9851.0058071196909,7578.7212641711521,-147803.07999999999,3.5078672337116168,9818.4588829297863,4559.2019544142931,-151542.94668763928,3.7033553601233087,null,140]
["IL","IL18-100A2",338,4,1200,14,"NA",11.1,5.25,49.42676400493967,1.1000000000000001,330,32,{"$f":"IF(G119=\"NA\",(UAC_V*0.98)/J119,(IF((UAC_V*0.98)/J119<G119,(UAC_V*0.98)/J119,G119)))","v":7.9309258433512628},{"$f":"IF(AO119<G119,IF(AO119<0,0,AO119),G119)","v":6.0544790805790907},{"$f":"IF(AS119<G119,IF(AS119<0,0,AS119),G119)","v":7.4947105035726098},null,{"$f":"IF(move1,Gewicht/K119,MAX(Gewicht,Gewicht2)/K119)","v":4.545454545454545},{"$f":"IF(move1,IF(AccType=1,SQRT((V119^2*Ltime1+W119^2*Ltime2+X119^2*Ltime3+Y119^2*Ltime4)/ltime)/C119,SQRT((((V119-W119)*2/PI()+W119)^2*Ltime1+W119^2*Ltime2+((X119-W119)*2/PI()+W119)^2*Ltime3+Y119^2*Ltime4)/ltime)/C119),IF(AccType=1,SQRT((V119^2*Ltime1+W119^2*Ltime2+X119^2*Ltime3+Y119^2*Ltime4+Z119^2*Ltime5+AA119^2*Ltime6+AB119^2*Ltime7+AC119^2*Ltime8)/ltime)/C119,SQRT((((V119-W119)*2/PI()+W119)^2*Ltime1+W119^2*Ltime2+((X119-W119)*2/PI()+W119)^2*Ltime3+Y119^2*Ltime4+((Z119-AA119)*2/PI()+AA119)^2*Ltime5+AA119^2*Ltime6+((AB119-AA119)*2/PI()+AA119)^2*Ltime7+AC119^2*Ltime8)/ltime)/C119))","v":0.3655458334546719},{"$f":" IF(move1,MAX(ABS(V119),ABS(X119))/E119,MAX(ABS(V119),ABS(X119),ABS(Z119),ABS(AB119))/E119)","v":0.26616333333333331},{"$f":"IF(AW119>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW119,G119),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW119,G119)),\"NA\")","v":0.1302163316155355},{"$f":"((Gewicht+K119)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":191.63759999999999},0,{"$f":"((Gewicht+K119)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-319.39599999999996},0,{"$f":"((Gewicht2+K119)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K119)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"AF119/Irms","v":6.0924305575778652E-2},{"$f":"AG119/Ipeak","v":7.8746548323471388E-2},{"$f":"D119*S119","v":1.4621833338186876},{"$f":"IF(move1,IF(MAX(ABS(V119),ABS(X119))<=C119,MAX(ABS(V119),ABS(X119))/C119*D119,D119+(MAX(ABS(V119),ABS(X119))-C119)/(E119-C119)*(F119-D119)),IF(MAX(ABS(V119),ABS(X119),ABS(Z119),ABS(AB119))<=C119,MAX(ABS(V119),ABS(X119),ABS(Z119),ABS(AB119))/C119*D119,D119+(MAX(ABS(V119),ABS(X119),ABS(Z119),ABS(AB119))-C119)/(E119-C119)*(F119-D119)))","v":3.7798343195266266},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V119),ABS(X119))<=C119,MAX(ABS(V119),ABS(X119))/C119*D119,D119+(MAX(ABS(V119),ABS(X119))-C119)/(E119-C119)*(F119-D119)),IF(MAX(ABS(V119),ABS(X119),ABS(Z119),ABS(AB119))<=C119,MAX(ABS(V119),ABS(X119),ABS(Z119),ABS(AB119))/C119*D119,D119+(MAX(ABS(V119),ABS(X119),ABS(Z119),ABS(AB119))-C119)/(E119-C119)*(F119-D119))),IF(move1,IF(MAX(ABS((V119-W119)*2/PI()+W119),ABS((X119-W119)*2/PI()+W119))<=C119,MAX(ABS((V119-W119)*2/PI()+W119),ABS((X119-W119)*2/PI()+W119))/C119*D119,D119+(MAX(ABS((V119-W119)*2/PI()+W119),ABS((X119-W119)*2/PI()+W119))-C119)/(E119-C119)*(F119-D119)),IF(MAX(ABS((V119-W119)*2/PI()+W119),ABS((X119-W119)*2/PI()+W119),ABS((Z119-AA119)*2/PI()+AA119),ABS((AB119-AA119)*2/PI()+AA119))<=C119,MAX(ABS((V119-W119)*2/PI()+W119),ABS((X119-W119)*2/PI()+W119),ABS((Z119-AA119)*2/PI()+AA119),ABS((AB119-AA119)*2/PI()+AA119))/C119*D119,D119+(MAX(ABS((V119-W119)*2/PI()+W119),ABS((X119-W119)*2/PI()+W119),ABS((Z119-AA119)*2/PI()+AA119),ABS((AB119-AA119)*2/PI()+AA119))-C119)/(E119-C119)*(F119-D119))))","v":2.4063172640842128},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V119)+Ltime2*ABS(Lspeed2)*ABS(W119)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X119)+Ltime4*ABS(Lspeed1)*ABS(Y119))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V119)+Ltime2*ABS(Lspeed2)*ABS(W119)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X119)+Ltime4*ABS(Lspeed1)*ABS(Y119)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z119)+Ltime6*ABS(Lspeed6)*ABS(AA119)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB119)+Ltime8*ABS(Lspeed1)*ABS(AC119))/ltime)","v":147.41353846153845},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK119/2*Ltime1/ltime,AK119/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X119*-ABS(Lspeed2-Lspeed1),((X119-Y119)*2/PI()+Y119)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V119*-ABS(Lspeed2-Lspeed1),((V119-W119)*2/PI()+W119)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X119*-ABS(Lspeed2-Lspeed1),((X119-Y119)*2/PI()+Y119)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V119*-ABS(Lspeed2-Lspeed1),((V119-W119)*2/PI()+W119)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB119*-ABS(Lspeed6-Lspeed1),((AB119-AC119)*2/PI()+AB119)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z119*-ABS(Lspeed6-Lspeed1),((Z119-AA119)*2/PI()+AA119)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB119*-ABS(Lspeed6-Lspeed1),((AB119-AC119)*2/PI()+AB119)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z119*-ABS(Lspeed6-Lspeed1),((Z119-AA119)*2/PI()+AA119)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":23.461593324821077},{"$f":"IF(move1,MAX(IF(AccType=1,X119*-ABS(Lspeed2-Lspeed1),((X119-Y119)*2/PI()+Y119)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V119*-ABS(Lspeed2-Lspeed1),((V119-W119)*2/PI()+W119)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X119*-ABS(Lspeed2-Lspeed1),((X119-Y119)*2/PI()+Y119)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V119*-ABS(Lspeed2-Lspeed1),((V119-W119)*2/PI()+W119)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB119*-ABS(Lspeed6-Lspeed1),((AB119-AC119)*2/PI()+AB119)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z119*-ABS(Lspeed6-Lspeed1),((Z119-AA119)*2/PI()+AA119)*-ABS(Lspeed6-Lspeed1)),0))","v":203.33380881511599},{"$f":"(J119^2)+3*(I119/1000)^2*(F119/2)^2*(2000*PI()/M119)^2","v":2599.210284304057},{"$f":"SQRT(3)*H119*F119/2*J119","v":6651.8710878481397},{"$f":"3*F119^2*H119^2/4-(UAC_V*0.98)^2","v":-135552.13},{"$f":"-AM119/2/AL119+SQRT((AM119/2/AL119)^2-AN119/AL119)","v":6.0544790805790907},{"$f":"(J119^2)+3*(I119/1000)^2*(D119/2)^2*(2000*PI()/M119)^2","v":2455.7564517799228},{"$f":"SQRT(3)*H119*D119/2*J119","v":1900.5345965280399},{"$f":"3*D119^2*H119^2/4-(UAC_V*0.98)^2","v":-152185.48000000001},{"$f":"-AQ119/2/AP119+SQRT((AQ119/2/AP119)^2-AR119/AP119)","v":7.4947105035726098},{"$f":"(J119^2)+3*(I119/1000)^2*(AH119/2)^2*(2000*PI()/M119)^2","v":2447.6197207324467},{"$f":"SQRT(3)*H119*AH119/2*J119","v":1143.3223026536864},{"$f":"3*AH119^2*H119^2/4-(UAC_V*0.98)^2","v":-153128.92705182947},{"$f":"IF((AU119/2/AT119)^2-AV119/AT119>=0,-AU119/2/AT119+SQRT((AU119/2/AT119)^2-AV119/AT119),-9999)","v":7.6795282710966388},null,69.900000000000006]
["IL","IL18-100A3",338,5.9,1200,21,"NA",4.9000000000000004,2.33,32.951176003293114,1.1000000000000001,330,32,11.896388765026895,10.032903405135935,11.470364158179276,null,4.545454545454545,0.3655458334546719,0.26616333333333331,8.5830607926347155E-2,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,8.9863350724273525E-2,0.1161511587771203,2.1567204173825645,5.5752556213017748,3.5493179645242141,147.41353846153845,23.461593324821077,203.33380881511599,1155.0063565680243,2936.4115613023323,-145722.6925,10.032903405135935,1091.2443298687822,824.99181960398857,-153037.158925,11.470364158179276,1087.7575282665541,496.29801456033158,-153437.14767332561,11.650855378516235,null,46.6]
["IL","IL18-100A4",338,11.9,1200,42.1,"NA",1.2,0.57999999999999996,16.475588001646557,1.1000000000000001,330,32,23.79277753005379,21.712733210414164,23.350351142166147,null,4.545454545454545,0.3655458334546719,0.26616333333333331,4.247658181620264E-2,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,0.1812498090879415,0.23427098126232737,4.3499954181105958,11.245007100591714,7.1587938606505332,147.41353846153845,23.461593324821077,203.33380881511599,288.68515722995204,720.83339201649085,-151749.7972,21.712733210414164,272.82243449051487,203.75100629444751,-153511.0612,23.350351142166147,271.94349033746693,122.57239100521504,-153608.65180409758,23.542383997069916,null,23.3]
["IL","IL24-015A1",83,2.4,240,7.1,"NA",16.899999999999999,2,19.445436482630054,0.56999999999999995,330,32,20.15897150728194,16.836900205437928,19.178857970655365,null,8.7719298245614041,1.3592702326916308,1.2151883333333333,5.6470490157060911E-2,174.98712,0,-291.64519999999999,0,0,0,0,0,0.13592702326916309,0.18012638535031844,3.2622485584599139,8.6460664968152852,5.4734737192971927,134.60547692307691,21.423127019549739,185.66710083609775,383.95539169365907,2020.660635376305,-142865.799925,16.836900205437928,378.79119829707344,683.040214775089,-152430.1648,19.178857970655365,381.59003087834537,1557.7511103310667,-147246.57581028054,17.708364089256321,null,27.5]
["IL","IL24-015A2",83,4.9000000000000004,240,14.2,"NA",4.2,0.5,9.7580735803743561,0.56999999999999995,330,32,40.171863510887917,36.999555131835358,39.19258626146928,null,8.7719298245614041,1.3592702326916308,1.2151883333333333,2.6451779163739506E-2,174.98712,0,-291.64519999999999,0,0,0,0,0,0.27751767250787468,0.35956745753715502,6.6604241401889919,17.259237961783441,10.981554380736998,134.60547692307691,21.423127019549739,185.66710083609775,96.677597923414794,504.00211049558112,-150996.3028,36.999555131835358,95.393561427004514,173.91622122734842,-153346.34770000001,39.19258626146928,96.091743434577609,389.76947777559451,-152068.53428055599,37.804640429284049,null,13.8]
["IL","IL24-015A3",83,9.8000000000000007,240,28.4,"NA",1.1000000000000001,0.13,4.8790367901871781,0.56999999999999995,330,32,80.343727021775834,76.81613284076542,79.292722546918057,null,8.7719298245614041,1.3592702326916308,1.2151883333333333,1.2863387380993449E-2,174.98712,0,-291.64519999999999,0,0,0,0,0,0.55503534501574936,0.71913491507431004,13.320848280377984,34.518475923566882,21.963108761473997,134.60547692307691,21.423127019549739,185.66710083609775,24.199134478491359,132.00055274884269,-152932.04680000001,76.81613284076542,23.851931009862017,45.549486511924599,-153576.8437,79.292722546918057,24.040719424709788,102.08248227456046,-153226.24183207998,77.740020601227457,null,6.9]
["IL","IL24-030A1",152,2.2999999999999998,480,7.1,"NA",24.3,5.0999999999999996,38.890872965260108,0.72,330,32,10.07948575364097,7.5187881280564852,9.3878385594964495,null,6.9444444444444446,0.76222141131139398,0.6239566666666666,0.10873193015960766,179.69952000000001,0,-299.49919999999997,0,0,0,0,0,7.3046218584008588E-2,9.2885934959349561E-2,1.7531092460162061,4.4585248780487792,2.8658601833405757,138.23039999999997,22.000051445569927,190.6671125282727,1550.4121219880183,5810.8938981827469,-131339.049325,7.5187881280564852,1516.4784789787066,1882.402248707087,-151321.23092500001,9.3878385594964495,1518.676911698866,2345.5224580871327,-150026.66075941085,9.1969304557741172,null,55]
["IL","IL24-030A2",152,4.5,480,14.2,"NA",6.1,1.28,19.445436482630054,0.72,330,32,20.15897150728194,17.750139854993193,19.495926391983996,null,6.9444444444444446,0.76222141131139398,0.6239566666666666,5.1782388394989644E-2,179.69952000000001,0,-299.49919999999997,0,0,0,0,0,0.14291651462088636,0.18462539634146338,3.429996350901273,8.8620190243902428,5.643509120500747,138.23039999999997,22.000051445569927,190.6671125282727,387.67751375089102,1458.7017604491668,-148036.7317,17.750139854993193,379.0843255477858,462.26464239586278,-153098.87312500001,19.495926391983996,379.63382699383851,579.73216121023734,-152775.16858514646,19.311585096695886,null,27.5]
["IL","IL24-030A3",152,9,480,28.5,"NA",1.5,0.32,9.7580735803743561,0.72,330,32,40.171863510887917,37.689649308694314,39.510416594911057,null,6.9444444444444446,0.76222141131139398,0.6239566666666666,2.5430957069552906E-2,179.69952000000001,0,-299.49919999999997,0,0,0,0,0,0.28583302924177273,0.37018765243902435,6.8599927018025459,17.769007317073168,11.29880699482109,138.23039999999997,22.000051445569927,190.6671125282727,97.624975852435455,361.26911843873398,-152293.328125,37.689649308694314,95.459831386946476,114.08498477012652,-153527.3125,39.510416594911057,95.597995108970096,143.22491376941812,-153448.56862083325,39.322153596698307,null,13.8]
["IL","IL24-050A1",245,2.1,800,7,"NA",34.299999999999997,12,65.831641328467569,0.92,330,32,5.9545834205182953,3.6502043158821049,5.413448010994415,null,5.4347826086956523,0.48942294473700931,0.38746400000000003,0.18086202100670476,185.98272,0,-309.97120000000001,0,0,0,0,0,4.2824507664488316E-2,5.5700408408408418E-2,1.0277881839477196,2.673619603603604,1.6914325267243377,143.06363076923077,22.769284013596849,197.33379478450604,4537.8282284787683,13688.550890563158,-110427.99250000001,3.6502043158821049,4352.167090563089,4106.5652671689468,-149772.75932499999,5.413448010994415,4345.7172250987514,3307.6086028599893,-151139.5960017321,5.5290767759524755,null,93.1]
["IL","IL24-050A2",245,4.3,800,14,"NA",8.6,3,32.880465325174455,0.92,330,32,11.921972396779642,9.8180758210203543,11.380831966607433,null,5.4347826086956523,0.48942294473700931,0.38746400000000003,8.6999561668912193E-2,185.98272,0,-309.97120000000001,0,0,0,0,0,8.768827759871417E-2,0.11324026426426426,2.1045186623691401,5.4355326846846843,3.4634094594831675,143.06363076923077,22.769284013596849,197.33379478450604,1132.130807119692,3428.4283184864744,-142791.88,9.8180758210203543,1085.9367212940972,1053.017269249417,-152638.3597,11.380831966607433,1084.2465567187628,848.14650495757314,-152998.62597398844,11.494310785215518,null,46.5]
["IL","IL24-050A3",245,8.6,800,28.1,"NA",2.1,0.75,16.475588001646557,0.92,330,32,23.79277753005379,21.617407044546553,23.253474747435195,null,5.4347826086956523,0.48942294473700931,0.38746400000000003,4.2793149565862526E-2,185.98272,0,-309.97120000000001,0,0,0,0,0,0.17537655519742834,0.2267244144144144,4.2090373247382802,10.882771891891892,6.9268189189663349,143.06363076923077,22.769284013596849,197.33379478450604,284.28769622441973,841.97107012852575,-151052.364925,21.617407044546553,272.64793032352435,257.6850961959189,-153419.37729999999,23.253474747435195,272.22538917969075,207.55093017041293,-153505.30343673818,23.36822622651108,null,23.3]
["IL","IL24-075A1",348,2,1200,7,"NA",46.6,20,98.994949366116643,1.17,330,32,3.9597979746446668,1.6418206516744414,3.4813210933008767,null,4.2735042735042734,0.35911589119859627,0.26921766666666663,0.27071211305886644,193.83672000000001,0,-323.06119999999999,0,0,0,0,0,2.9926324266549689E-2,3.8680699233716469E-2,0.71823178239719254,1.8566735632183906,1.181995101176998,149.10516923076921,23.730824723630498,205.66714760479766,10366.731190218801,27965.824393355542,-73859.17,1.6418206516744414,9846.2637706301048,7990.2355409587262,-147149.32,3.4813210933008767,9816.1589221266586,4722.2096333317777,-151388.56491621106,3.6939610448186695,null,140]
["IL","IL24-075A2",348,4.0999999999999996,1200,14,"NA",11.7,5,49.42676400493967,1.17,330,32,7.9309258433512628,5.958434324799212,7.4596587333905662,null,4.2735042735042734,0.35911589119859627,0.26921766666666663,0.13047272323250633,193.83672000000001,0,-323.06119999999999,0,0,0,0,0,6.1348964746426864E-2,7.9295433429118753E-2,1.4723751539142447,3.8061808045977004,2.4230899574128459,149.10516923076921,23.730824723630498,205.66714760479766,2584.6877975547004,7011.4316871912815,-133541.17000000001,5.958434324799212,2455.1564685045637,2053.347851248875,-151938.15932500002,7.4596587333905662,2447.24924188983,1213.5235505942428,-153061.20163984646,7.6644372496002084,null,69.900000000000006]
["IL","IL24-075A3",348,8.1,1200,28,"NA",2.9,1.25,24.678026663410506,1.17,33,32,15.884576402586054,13.904452670813622,15.419851503793804,null,4.2735042735042734,0.35911589119859627,0.26921766666666663,6.4011010033422425E-2,193.83672000000001,0,-323.06119999999999,0,0,0,0,0,0.12120161327952624,0.15665683189655169,2.9088387187086298,7.5195279310344816,4.787080159766842,149.10516923076921,23.730824723630498,205.66714760479766,644.42569938867507,1735.3899980695976,-148718.92000000001,13.904452670813622,611.96922460062615,502.02353515584792,-153250.16492499999,15.419851503793804,610.04033875071286,296.69467961488533,-153519.45646930358,15.622312465900233,null,34.9]
["IL","IL24-075A4",348,16.3,1200,56.1,"NA",0.73,0.31,12.37436867076458,1.17,330,32,31.678383797157334,29.358706525149628,31.179707615108882,null,4.2735042735042734,0.35911589119859627,0.26921766666666663,3.1843875750095875E-2,193.83672000000001,0,-323.06119999999999,0,0,0,0,0,0.24389954277237999,0.31524769875478925,5.8535890265371195,15.131889540229885,9.6332600745925347,149.10516923076921,23.730824723630498,205.66714760479766,161.87020820648439,438.87354628337272,-152406.13884325,29.358706525149628,153.86327751194892,127.51584321602451,-153557.81034925001,31.179707615108882,153.38286417019114,75.361551001897553,-153626.91028003651,31.403212594088497,null,17.5]
["IL","IL24-100A1",450,2,1600,7,"NA",58.9,28,131.52186130069782,1.42,330,32,2.9804930991949106,0.47049984480935736,2.5102766806025447,null,3.5211267605633805,0.28896897514145714,0.21009450000000002,0.36005644045065799,201.69072,0,-336.15120000000002,0,0,0,0,0,2.4080747928454761E-2,3.1125111111111114E-2,0.57793795028291428,1.4940053333333334,0.95111333522261932,155.1467076923077,24.692365433664154,214.00050042508934,18408.793132828851,46961.49487415194,-26170.532500000001,0.47049984480935736,17388.676990435004,13417.56996404341,-143256.37,2.5102766806025447,17318.506977162258,6380.8148595420844,-151310.27134514088,2.77734234873946,null,186]
["IL","IL24-100A2",450,3.9,1600,14,"NA",14.7,7,65.831641328467569,1.42,330,32,5.9545834205182953,4.0242637810956383,5.5287075504620216,null,3.5211267605633805,0.28896897514145714,0.21009450000000002,0.17349046101064755,201.69072,0,-336.15120000000002,0,0,0,0,0,4.6957458460486788E-2,6.0693966666666675E-2,1.1269790030516829,2.9133104000000003,1.8546710036841076,155.1467076923077,24.692365433664154,214.00050042508934,4611.5032832072129,11733.043620482707,-121898.77,4.0242637810956383,4355.3549535080692,3268.4907228487541,-151198.95332500001,5.5287075504620216,4338.6786112912177,1554.3525562764341,-153106.51947902521,5.7640056644879598,null,93.1]
["IL","IL24-100A3",450,7.9,1600,28.1,"NA",3.7,1.75,32.951176003293114,1.42,330,32,11.896388765026895,10.01215128432175,11.465458558433053,null,3.5211267605633805,0.28896897514145714,0.21009450000000002,8.5449028232729554E-2,201.69072,0,-336.15120000000002,0,0,0,0,0,9.5118954317396309E-2,0.1229441888888889,2.2828549036175114,5.9013210666666671,3.7568976741293465,155.1467076923077,24.692365433664154,214.00050042508934,1155.7013461107294,2966.9456756909958,-145556.679325,10.01215128432175,1091.3065146221181,834.12351736508424,-153023.20532499999,11.465458558433053,1087.0298441842742,396.67300029436382,-153519.0816287254,11.702883235563466,null,46.6]
["IL","IL24-100A4",450,15.8,1600,56.1,"NA",0.92,0.44,16.475588001646557,1.42,330,32,23.79277753005379,21.66753924868982,23.342492700033777,null,3.5211267605633805,0.28896897514145714,0.21009450000000002,4.238116104425791E-2,201.69072,0,-336.15120000000002,0,0,0,0,0,0.19023790863479262,0.24588837777777781,4.5657098072350228,11.802642133333334,7.513795348258693,155.1467076923077,24.692365433664154,214.00050042508934,289.06281798933799,736.4143513213603,-151666.15109199999,21.66753924868982,272.84246381171204,207.40368539888581,-153505.528528,23.342492700033777,271.76104223226184,98.632205478598564,-153628.16101988405,23.595389445695396,null,23.3]
["IC/ICD","ICD05-030A1",57,2.1,170,7.9,"NA",3.2,9.1,15.414927829866736,0.62,330,32,25.429895250011619,19.462732957455209,24.70020034036887,null,8.064516129032258,1.9970556324335824,1.7309599999999998,5.3785019132017955E-2,176.55792,0,-294.26319999999998,0,0,0,0,0,0.17474236783793848,0.29746064896755159,4.1938168281105233,14.278111150442477,8.7896980010699579,135.81378461538463,21.615435161556469,187.33377140015605,387.05695538207198,337.48089880169516,-153184.6912,19.462732957455209,248.1794772189543,89.710112339691122,-153630.1312,24.70020034036887,422.6114836736092,375.48799767044972,-153070.6524855039,18.592537776094328,null,21.8]
["IC/ICD","ICD05-030A5",57,3.7,170,13.7,"NA",1.1000000000000001,3,8.9095454429504972,0.62,330,32,43.997755273829632,34.148411466998539,42.851842556749638,null,8.064516129032258,1.9970556324335824,1.7309599999999998,3.0604563746290486E-2,176.55792,0,-294.26319999999998,0,0,0,0,0,0.30787941000017732,0.51451548672566372,7.3891058400042553,24.696743362831857,15.233962070810271,135.81378461538463,21.615435161556469,187.33377140015605,128.22326499130119,116.27850283478882,-153493.671325,34.148411466998539,82.942599487084593,31.403683247351729,-153651.576325,42.851842556749638,139.7733739708876,129.29797823618816,-153453.3932076598,32.674865366156638,null,12.6]
["IC/ICD","ICD05-050A1",87,2,280,8.5,"NA",4.5,14.4,25.667976157071671,0.95,330,32,15.271948111577228,11.436919456155206,14.852605233872367,null,5.2631578947368425,1.3852444425488804,1.1126500000000001,7.6705676548166721E-2,186.92520000000002,0,-311.54200000000003,0,0,0,0,0,0.11543703687907336,0.19921448618307427,2.7704888850977607,9.5622953367875656,5.7495838409280671,143.78861538461538,22.884668898800893,198.33379712294106,1092.0404426720638,850.26381765271799,-152566.703125,11.436919456155206,682.8281386946469,200.06207474181602,-153603.25,14.852605233872367,857.05193700921177,575.1368360590443,-153161.93596340262,13.036844794297043,null,36.299999999999997]
["IC/ICD","ICD05-050A5",87,3.4,280,14.7,"NA",1.5,4.8,14.849242404917497,0.95,330,32,26.398653164297777,20.123743860645828,25.804434775436132,null,5.2631578947368425,1.3852444425488804,1.1126500000000001,4.3795610195631406E-2,186.92520000000002,0,-311.54200000000003,0,0,0,0,0,0.19624296269442473,0.34472415803108808,4.7098311046661934,16.546759585492229,9.9185072926903306,143.78861538461538,22.884668898800893,198.33379712294106,364.45879001461935,283.55905634893764,-153299.34812499999,20.123743860645828,228.20125231417001,65.585087863019595,-153644.49249999999,25.804434775436132,286.03844791443942,191.32534478267527,-153497.98917208068,22.83333867328442,null,21]
["IC/ICD","ICD05-075A1",125,1.9,425,8.5,"NA",6.1,21,38.395898218429529,1.36,330,32,10.209423875695272,7.6046721303653175,9.9244229018840322,null,3.6764705882352939,1.030565989850281,0.78355200000000003,0.10662028474050225,199.80576000000002,0,-333.00960000000003,0,0,0,0,0,8.1586474196480574E-2,0.1349210666666667,1.9580753807155338,6.4762112000000016,3.8140109064608256,153.69673846153847,24.46159566325608,212.00049574821935,2395.5373910994413,1724.107035941903,-151647.68312500001,7.6046721303653175,1520.2777409255223,385.38863156348418,-153563.253925,9.9244229018840322,1659.7362783079791,773.61918105744292,-153258.03855037663,9.3790783098530426,null,54.3]
["IC/ICD","ICD05-075A5",125,3.3,425,14.7,"NA",2,7,22.203152929257591,1.36,330,32,17.655150205422078,13.488263831466291,17.258976920472922,null,3.6764705882352939,1.030565989850281,0.78355200000000003,6.0946393244708713E-2,199.80576000000002,0,-333.00960000000003,0,0,0,0,0,0.14170282360441364,0.23342426666666669,3.400867766505927,11.2043648,6.6060188384323348,153.69673846153847,24.46159566325608,212.00049574821935,799.14235723595277,565.31773773692953,-153015.73000000001,13.488263831466291,508.40925665370685,126.90806357359644,-153631.32999999999,17.258976920472922,554.80964303588758,254.04759355034741,-153533.08154531883,16.407861839909923,null,31.4]
["IC/ICD","ICD05-100A1",157,1.8,550,8.5,"NA",7.7,27.6,51.194530957906039,1.71,330,32,7.657067906771454,5.641874764980682,7.4380980799796026,null,2.9239766081871346,0.86566841323851618,0.63879200000000003,0.13872659483163363,210.80135999999999,0,-351.3356,0,0,0,0,0,6.4925130992888713E-2,0.10652292832909245,1.5582031438293291,5.1131005597964378,2.9365653205277482,162.15489230769231,25.807752657303187,223.66718969662762,4212.2715914827904,2901.7757763393779,-150451.22312499999,5.641874764980682,2692.2448270782593,614.49369381304473,-153519.9253,7.4380980799796026,2810.8209207479345,1002.5004838524353,-153280.53825427935,7.2084231665431995,null,72.400000000000006]
["IC/ICD","ICD05-100A5",157,3.1,550,14.7,"NA",2.6,9.1999999999999993,29.557063453597682,1.71,330,32,13.26248125479075,10.087078583196186,12.970930800611841,null,2.9239766081871346,0.86566841323851618,0.63879200000000003,7.9205168448324689E-2,210.80135999999999,0,-351.3356,0,0,0,0,0,0.11181550337664169,0.18408571670907548,2.6835720810394004,8.8361144020356228,5.0677847340480415,162.15489230769231,25.807752657303187,223.66718969662762,1402.4686105398168,978.3237537778582,-152568.42370000001,10.087078583196186,897.13906681145625,206.31317256539867,-153615.27729999999,12.970930800611841,936.47401372338686,337.27443430966019,-153533.79001849901,12.625438713035798,null,41.8]
["IC/ICD","ICD10-030A1",104,1.9,340,7.9,"NA",6.4,18.3,30.900566337852126,1.1000000000000001,330,32,12.685851635017237,9.440979410525328,12.292032193061127,null,4.545454545454545,1.1880239587276837,0.9393999999999999,8.898250840453184E-2,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,9.4051896732608289E-2,0.15367019774011295,2.2572455215825991,7.3761694915254221,4.4254358173334571,147.41353846153845,23.461593324821077,203.33380881511599,1559.1795246697509,1353.0197502416586,-151746.7648,9.440979410525328,989.8016997926261,325.40981334925959,-153553.10079999999,12.292032193061127,1144.48734457823,757.93697016189924,-153062.36470763508,11.238163746225325,null,43.7]
["IC/ICD","ICD10-030A4",104,3.9,340,15.8,"NA",1.6,4.5999999999999996,15.414927829866736,1.1000000000000001,330,32,25.429895250011619,19.382032291056241,24.775617983305512,null,4.545454545454545,1.1880239587276837,0.9393999999999999,4.3800842202789313E-2,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,0.1930538932932486,0.30752228107344631,4.6332934390379661,14.761069491525422,8.908781037711357,147.41353846153845,23.461593324821077,203.33380881511599,390.35932983381923,337.48089880169516,-153184.6912,19.382032291056241,246.92606155572983,83.302247172570318,-153634.79680000001,24.775617983305512,286.17939604255224,190.28755897685613,-153511.61655121046,22.830611232774842,null,21.8]
["IC/ICD","ICD10-030A5",104,3.4,340,13.7,"NA",2.1,6.1,17.819090885900994,1.1000000000000001,330,32,21.998877636914816,16.74247538333433,21.411270088948864,null,4.545454545454545,1.1880239587276837,0.9393999999999999,5.0708125747679619E-2,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,0.16830339415308851,0.2666824505649717,4.0392814596741244,12.800757627118641,7.7353314864224334,147.41353846153845,23.461593324821077,203.33380881511599,519.45976559181304,443.97246536919369,-153043.215325,16.74247538333433,329.95765618968159,110.18294760987288,-153625.7653,21.411270088948864,381.89816186418227,250.67694820984801,-153466.09456927501,19.720705217462303,null,25.2]
["IC/ICD","ICD10-030A8",104,6.8,340,27.4,"NA",0.5,1.5,8.9095454429504972,1.1000000000000001,330,32,43.997755273829632,34.192447331325091,43.02689076217932,null,4.545454545454545,1.1880239587276837,0.9393999999999999,2.5056533545547224E-2,191.63759999999999,0,-319.39599999999996,0,0,0,0,0,0.33660678830617702,0.53336490112994339,8.0785629193482489,25.601515254237281,15.470662972844867,147.41353846153845,23.461593324821077,203.33380881511599,128.22326499130119,105.70772984980803,-153523.23250000001,34.192447331325091,82.388301685222629,26.234035145207834,-153655.32999999999,43.02689076217932,94.951175941350186,59.684987669011427,-153619.12348509638,39.909750412291537,null,12.6]
["IC/ICD","ICD10-050A1",171,1.9,560,7.9,"NA",9,29,51.477373670380658,1.9,330,32,7.614996105085897,5.6285673998337709,7.348630687954028,null,2.6315789473684212,0.81730034779310312,0.64515,0.13993699654202982,216.77040000000002,0,-361.28399999999999,0,0,0,0,0,6.4702944200287327E-2,0.10072857754927163,1.5528706608068958,4.8349717223650384,2.8100340026742812,166.74646153846155,26.538523596928759,230.00053784004925,4167.5685868412329,3169.6887169562879,-149872.5925,5.6285673998337709,2737.7057939191927,762.33019774898048,-153444.6925,7.348630687954028,2841.9372251788677,1127.4598826000233,-153184.30031590673,7.1460730522371314,null,72.8]
["IC/ICD","ICD10-050A4",171,3.8,560,15.8,"NA",2.2000000000000002,7.3,25.738686835190329,1.9,330,32,15.229992210171794,11.713799721594979,14.842489809488434,null,2.6315789473684212,0.81730034779310312,0.64515,6.8957755907867443E-2,216.77040000000002,0,-361.28399999999999,0,0,0,0,0,0.12940588840057465,0.20145715509854326,3.1057413216137917,9.6699434447300767,5.6200680053485623,166.74646153846155,26.538523596928759,230.00053784004925,1047.1434634614473,774.81279747820372,-152757.80679999999,11.713799721594979,684.73020194032722,186.34738167197307,-153611.5828,14.842489809488434,711.1487178586533,275.60130463556129,-153549.34585328339,14.501632004035519,null,36.4]
["IC/ICD","ICD10-050A5",171,3.3,560,13.7,"NA",3,9.6999999999999993,29.698484809834994,1.9,330,32,13.199326582148888,10.088293764880195,12.841061814574028,null,2.6315789473684212,0.81730034779310312,0.64515,7.9768311509657935E-2,216.77040000000002,0,-361.28399999999999,0,0,0,0,0,0.11237879782155168,0.17473508997429307,2.6970911477172401,8.3872843187660671,4.877392271302087,166.74646153846155,26.538523596928759,230.00053784004925,1392.6292003368367,1057.0772984980804,-152397.0925,10.088293764880195,911.62732160300561,254.62445876231132,-153590.49249999999,12.841061814574028,946.720204893659,376.33435371265887,-153503.42455126494,12.536306474017884,null,42]
["IC/ICD","ICD10-050A8",171,6.6,560,27.4,"NA",0.7,2.4,14.849242404917497,1.9,330,32,26.398653164297777,20.715285164490023,25.843343393124748,null,2.6315789473684212,0.81730034779310312,0.64515,3.9509710522269634E-2,216.77040000000002,0,-361.28399999999999,0,0,0,0,0,0.22475759564310335,0.34947017994858615,5.3941822954344802,16.774568637532134,9.7547845426041739,166.74646153846155,26.538523596928759,230.00053784004925,345.53875837773109,246.65136964955204,-153388.09570000001,20.715285164490023,227.75489945513073,59.412373711205966,-153647.99170000001,25.843343393124748,236.34816155542464,87.811349199620395,-153629.03023560881,25.310233529459811,null,21]
["IC/ICD","ICD10-075A1",246,1.8,850,7.9,"NA",12.2,42.4,77.216060505570979,2.7,330,32,5.0766640700572649,3.6570404487474955,4.8822205729486319,null,1.8518518518518516,0.63399279364862671,0.47432000000000002,0.20548745275333946,241.9032,0,-403.17200000000003,0,0,0,0,0,4.7549459523647003E-2,7.0569439845474632E-2,1.1411870285675281,3.3873331125827821,1.9077323309211813,186.07938461538461,29.615453869036447,256.66726686498254,9206.5149149580193,6445.0337244777857,-146697.17170000001,3.6570404487474955,6130.7415914831581,1468.4886967164575,-153302.31880000001,4.8822205729486319,6151.5054082177267,1556.3796468434971,-153257.72901737769,4.8664771819443784,null,109.2]
["IC/ICD","ICD10-075A4",246,3.7,850,15.8,"NA",3,10.6,38.60803025278549,2.7,330,32,10.15332814011453,7.7889510257421284,9.8819900685626276,null,1.8518518518518516,0.63399279364862671,0.47432000000000002,0.10144050105976871,241.9032,0,-403.17200000000003,0,0,0,0,0,9.7740555687496622E-2,0.14268009105960267,2.3457733364999189,6.8486443708609279,3.9136985580567694,186.07938461538461,29.615453869036447,256.66726686498254,2301.6287287395048,1584.8443584781439,-151978.93,7.7889510257421284,1535.0570753743141,371.13443837779323,-153571.5925,9.8819900685626276,1540.3431104910351,392.56981522280489,-153560.61000427749,9.8579954707715842,null,54.6]
["IC/ICD","ICD10-075A5",246,3.2,850,13.7,"NA",4.0999999999999996,14.1,44.61843789287115,2.7,330,32,8.7856056489739025,6.6758158119655153,8.5321033744797763,null,1.8518518518518516,0.63399279364862671,0.47432000000000002,0.11750513102303198,241.9032,{"$f":"(Ltorque+IF(Lspeed2=0,0,IF(Lspeed2>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},-403.17200000000003,{"$f":"(Ltorque+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},0,{"$f":"(Ltorque2+IF(Lspeed6=0,0,IF(Lspeed6>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},0,0,8.4532372486483556E-2,0.1235894729580574,2.0287769396756055,5.9322947019867556,3.3854408974872792,186.07938461538461,29.615453869036447,256.66726686498254,3069.7527236578439,2170.4481578923678,-151297.698325,6.6758158119655153,2049.6702815294175,506.96599308434872,-153534.89920000001,8.5321033744797763,2056.6904841270198,536.34481456968979,-153519.50279403769,8.5102666691549977,null,63.1]
["IC/ICD","ICD10-075A8",246,6.4,850,27.4,"NA",1,3.5,22.273863607376246,2.7,330,32,17.599102109531852,13.831614297166059,17.225087793114159,null,1.8518518518518516,0.63399279364862671,0.47432000000000002,5.8176594672566397E-2,241.9032,0,-403.17200000000003,0,0,0,0,0,0.16906474497296711,0.24717894591611481,4.0575538793512109,11.864589403973511,6.7708817949745583,186.07938461538461,29.615453869036447,256.66726686498254,762.0494427304177,528.53864924904019,-153100.93,13.831614297166059,510.63331846960131,123.45428303627217,-153633.28,17.225087793114159,512.36356306133462,130.60849336280182,-153629.61636978886,17.189043216232754,null,31.5]
["IC/ICD","ICD10-100A1",315,1.8,1130,7.9,"NA",15.4,55.8,103.02545801887996,3.4,330,32,3.8048848074828645,2.6479482322244134,3.6349356854919663,null,1.4705882352941178,0.5401289254980508,0.38922477876106198,0.27332408323388468,263.89440000000002,0,-439.82400000000001,0,0,0,0,0,4.0509669412353809E-2,5.6963865030674854E-2,0.97223206589649147,2.734265521472393,1.6000037414959949,202.99569230769234,32.307767857130663,280.00065476179913,16233.045649146652,10854.829287747527,-142563.13329999999,2.6479482322244134,10905.943671739064,2473.2522427779172,-153087.70120000001,3.6349356854919663,10844.724040772286,2198.4515789489051,-153208.65067039785,3.6586604011191186,null,145.69999999999999]
["IC/ICD","ICD10-100A4",315,3.5,1130,15.8,"NA",3.9,13.9,51.477373670380658,3.4,330,32,7.614996105085897,5.7762745182492505,7.4040137821549434,null,1.4705882352941178,0.5401289254980508,0.38922477876106198,0.13447359152246108,263.89440000000002,0,-439.82400000000001,0,0,0,0,0,7.8768801635132404E-2,0.1121634764826176,1.8904512392431778,5.3838468711656446,3.1111183862422123,202.99569230769234,32.307767857130663,280.00065476179913,4044.5686728351702,2747.0635546954495,-150816.2317,5.7762745182492505,2718.3563332888589,608.52673679962493,-153524.25812499999,7.4040137821549434,2703.9934051216328,540.91391982208245,-153553.58615027726,7.4364043428777631,null,72.8]
["IC/ICD","ICD10-100A5",315,3.1,1130,13.7,"NA",5.0999999999999996,18.600000000000001,59.46768029778864,3.4,330,32,6.5918158912039635,4.9418774964075149,6.3889310948377904,null,1.4705882352941178,0.5401289254980508,0.38922477876106198,0.15577312354793274,263.89440000000002,0,-439.82400000000001,0,0,0,0,0,6.9766652876831564E-2,9.8405787321063407E-2,1.6743996690439575,4.7234777914110433,2.7555619992431026,202.99569230769234,32.307767857130663,280.00065476179913,5413.9401062656179,3598.3414611016788,-150002.63732499999,4.9418774964075149,3632.5375183611936,814.22325032227775,-153476.53292500001,6.3889310948377904,3612.3619129568474,723.75569273815256,-153515.87717391789,6.4195926564462278,null,84.1]
["IC/ICD","ICD10-100A8",315,6.1,1130,27.4,"NA",1.3,4.5999999999999996,29.698484809834994,3.4,330,32,13.199326582148888,10.334031352903956,12.917977181226238,null,1.4705882352941178,0.5401289254980508,0.38922477876106198,7.7131727616210233E-2,263.89440000000002,0,-439.82400000000001,0,0,0,0,0,0.13728276856408791,0.19504732106339465,3.2947864455381097,9.3622714110429435,5.4222349017364273,202.99569230769234,32.307767857130663,280.00065476179913,1341.3437720959705,916.13365869833626,-152712.4117,10.334031352903956,904.7665056205592,203.95676343284129,-153616.83632500001,12.917977181226238,899.9884342492212,181.29532477553309,-153626.73469978973,12.964833420765194,null,42]
["IC/ICD","IC11-015A1",73,3.9,190,11.3,"NA",1.4,9.1,10.889444430272832,1.7,330,32,35.998163405860602,18.843278137211765,31.318304102183294,null,2.9411764705882355,1.8590053771422639,1.8463789473684211,6.0406737191274033E-2,210.4872,0,-350.81200000000001,0,0,0,0,0,0.30208837378561787,0.44731282051282051,7.2501209708548293,21.471015384615384,13.408295139489216,161.91323076923078,25.769291028901844,223.33385558381596,424.32595149393956,149.19107176369502,-153476.29569999999,18.843278137211765,154.99942142863827,51.490723883045185,-153641.64129999999,31.318304102183294,549.05798880801092,177.02636481277335,-153399.71990353495,16.554444859909658,null,15.4]
["IC/ICD","IC11-015A5",73,6.7,190,19.100000000000001,"NA",0.47,3,6.293250352560273,1.7,330,32,62.288956904522841,33.607524772779932,54.568851396861803,null,2.9411764705882355,1.8590053771422639,1.8463789473684211,3.3743084141005901E-2,210.4872,0,-350.81200000000001,0,0,0,0,0,0.51897233445221536,0.7529858974358975,12.455336026853168,36.143323076923082,22.632818882387337,161.91323076923078,25.769291028901844,223.33385558381596,134.5408596700762,48.925679461646212,-153603.56010325,33.607524772779932,51.286891232668289,17.162411120053907,-153656.56284925001,54.568851396861803,172.90828410091217,57.975185442574684,-153579.13389402599,29.635702410046193,null,8.9]
["IC/ICD","IC11-030A1",151,4,375,11.3,"NA",1.9,16.7,21.849599538664314,2.5,330,32,17.940832247581014,9.9522621745120112,15.797891638166799,null,2,1.0060348363995151,1.0471999999999999,7.7353369317755022E-2,235.62,0,-392.7,0,0,0,0,0,0.1676724727332525,0.24743396577380952,4.0241393455980603,11.876830357142858,7.226358337695844,181.24615384615385,28.846221301009521,250.00058460874919,1507.1053793279168,406.26195840661103,-153318.27932500001,9.9522621745120112,606.43002991030346,143.80954279880035,-153620.68,15.797891638166799,898.51249629323252,259.80482216108459,-153522.61366006188,12.927685100466189,null,30.9]
["IC/ICD","IC11-030A5",151,6.9,375,19.100000000000001,"NA",0.63,5.6,12.586500705120546,2.5,330,32,31.144478452261421,17.583080145068589,27.490420794256249,null,2,1.0060348363995151,1.0471999999999999,4.4128913807789369E-2,235.62,0,-392.7,0,0,0,0,0,0.28923501546486058,0.41800037202380952,6.9416403711566543,20.064017857142858,12.291996126012233,181.24615384615385,28.846221301009521,250.00058460874919,489.21872880595447,131.16245983334943,-153555.40518325,17.583080145068589,201.59131514610752,47.38329700785922,-153649.82769325,27.490420794256249,295.42673818617902,84.41091351569456,-153619.02334098879,22.660879539334729,null,17.8]
["IC/ICD","IC11-050A1",276,4.4000000000000004,625,11.3,"NA",2.6,26.7,36.345288552988542,3.6,330,32,10.785441954285083,6.1057322996349113,9.3447100952003179,null,1.3888888888888888,0.63112890751130923,0.72047359999999994,0.10827097738720122,270.17759999999998,0,-450.29599999999999,0,0,0,0,0,0.11570696637707338,0.16345764087870104,2.776967193049761,7.8459667621776505,4.610901505514108,207.82892307692308,33.077000425157586,286.66733701803241,3953.0682907923506,924.76321106216142,-153016.61170000001,6.1057322996349113,1720.0498512784079,360.08479014809831,-153565.84479999999,9.3447100952003179,1759.2232712672253,377.34443204695407,-153556.20970764369,9.236085460130063,null,51.4]
["IC/ICD","IC11-050A5",276,7.6,625,19.100000000000001,"NA",0.87,8.9,21.001071401240459,3.6,330,32,18.665714358594389,10.846246589050706,16.264960231942823,null,1.3888888888888888,0.63112890751130923,0.72047359999999994,6.2164097552153776E-2,270.17759999999998,0,-450.29599999999999,0,0,0,0,0,0.19985748737858125,0.27798495702005727,4.7965796970859502,13.34327793696275,7.9515025091901794,207.82892307692308,33.077000425157586,286.66733701803241,1276.5860493851928,302.22104508952339,-153456.90648325,10.846246589050706,573.33537310514703,120.25549438117159,-153631.21109200001,16.264960231942823,585.85530138676813,125.81735069944625,-153628.10795783417,16.086455677427484,null,29.7]
["IC/ICD","IC11-075A1",435,4.5999999999999996,940,11.3,"NA",3.5,39.4,54.51793282948281,5,330,32,7.1902946361900559,4.0798135595333997,6.1592770963688599,null,1,0.46562838405004381,0.55702127659574474,0.15352897576166499,314.16000000000003,0,-523.6,0,0,0,0,{"$f":"(Ltorque2+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},8.92454402762584E-2,0.12032260726072608,2.1418905666302015,5.7754851485148517,3.524912457318762,241.66153846153847,38.461628401346033,333.33411281166559,8703.732415301678,1867.3103300293646,-152490.84812499999,4.0798135595333997,3921.9984067490282,760.14402815354651,-153469.5925,6.1592770963688599,3529.9172172689805,582.48720743367392,-153549.84524054569,6.5134284589534293,null,77.099999999999994]
["IC/ICD","IC11-075A5",435,8,940,19.100000000000001,"NA",1.2,13.1,31.466251762801363,5,330,32,12.457791380904569,7.2874714031653944,10.7380742478489,null,1,0.46562838405004381,0.55702127659574474,8.8170598926068433E-2,314.16000000000003,0,-523.6,0,0,0,0,0,0.15520946135001459,0.20723844884488452,3.7250270724003505,9.9474455445544567,6.1302825344674128,241.66153846153847,38.461628401346033,333.33411281166559,2800.3408753313083,624.58314206356852,-153270.00520000001,7.2874714031653944,1307.698027113302,261.60550452924338,-153594.88,10.7380742478489,1176.6017178184698,200.46445691701953,-153623.41320693141,11.341649168545468,null,44.5]
["IC/ICD","IC11-100A1",599,4.8,1250,11.3,"NA",4.4000000000000004,52,72.831998462214386,6.5,330,32,5.3822496742743038,3.0502900771618777,4.5523990265143377,null,0.76923076923076927,0.3888657748264347,0.48171199999999997,0.2011800556724106,361.28399999999999,0,-602.14,0,0,0,0,0,7.7773154965286931E-2,0.10065316180235534,1.8665557191668865,4.8313517665130563,3.0717934936901403,277.91076923076923,44.230872661547934,383.33422973341544,15288.041273271494,3136.0572227878747,-151809.9412,3.0502900771618777,7105.9001952868284,1332.1305017152033,-153329.45920000001,4.5523990265143377,6042.2543231885293,852.5062099822801,-153526.99051031042,4.9706716535974094,null,103]
["IC/ICD","IC11-100A5",599,8.1999999999999993,1250,19.100000000000001,"NA",1.5,17.3,41.93143212436226,6.5,330,32,9.3485955556535139,5.4752468968196482,8.0055042555288018,null,0.76923076923076927,0.3888657748264347,0.48171199999999997,0.11493821176461425,361.28399999999999,0,-602.14,0,0,0,0,0,0.13286247306569851,0.17192863543266768,3.188699353576764,8.2525745007680484,5.2476472183873231,277.91076923076923,44.230872661547934,383.33422973341544,4915.2842711841222,1040.3870877631916,-153048.38312499999,5.4752468968196482,2340.1350813969466,446.65833087215543,-153550.5325,8.0055042555288018,1996.5551346909581,285.84211555741354,-153617.5299602579,8.7003267638088282,null,59.3]
["IC/ICD","IC11-150A1",905,4.8,1875,11.3,"NA",6.2,77.3,108.89444430272832,9.4,330,32,3.5998163405860604,2.0076484615660104,3.0206956405787144,null,0.53191489361702127,0.32228687267287015,0.4021248,0.29567959699428575,452.3904,0,-753.98400000000004,0,0,0,0,0,6.4457374534574022E-2,8.3313149171270709E-2,1.5469769888297766,3.9990311602209943,2.5458623069107542,347.99261538461542,55.384744897938283,480.00112244879847,33919.595538005335,6607.0331781064942,-149982.6973,2.0076484615660104,15838.728022520501,2806.5273676912539,-152999.7568,3.0206956405787144,12977.824212729269,1488.5483830663798,-153477.14080884386,3.3820392416840512,null,154]
["IC/ICD","IC11-150A5",905,8.3000000000000007,1875,19.100000000000001,"NA",2.1,25.8,62.932503525602726,9.4,330,32,6.2288956904522843,3.6277277311403564,5.2983485606535465,null,0.53191489361702127,0.32228687267287015,0.4021248,0.1696150338562043,452.3904,0,-753.98400000000004,0,0,0,0,0,0.11145754346603427,0.14406232044198897,2.6749810431848227,6.9149913812154704,4.4022202390331797,347.99261538461542,55.384744897938283,480.00112244879847,10981.956181198837,2186.0409972224902,-152457.39092500001,3.6277277311403564,5286.4179198015072,949.95498832181511,-153436.14632500001,5.2983485606535465,4333.495839526161,503.84470792299066,-153599.90216141852,5.8957038021038679,null,89]
["IC/ICD","IC11-200A1",1255,5,2500,11.3,"NA",8,103,145.66399692442877,12.3,330,32,2.6911248371371519,1.4714760975642687,2.2117001304126105,null,0.4065040650406504,0.27921007204530712,0.36233119999999996,0.39345875869467656,543.49680000000001,0,-905.82799999999997,0,0,0,0,0,5.8168765009438982E-2,7.5184926958831347E-2,1.3960503602265355,3.6088764940239044,2.2974821321282133,418.07446153846155,66.538617134328632,576.6680151641815,60387.892517802247,11403.844446501362,-147534.88,1.4714760975642687,28886.94285335622,5045.9488701333457,-152464,2.2117001304126105,22837.197325702291,2318.5954737527818,-153410.63564092247,2.5415624329156148,null,206]
["IC/ICD","IC11-200A5",1255,8.6,2500,19.100000000000001,"NA",2.7,34.200000000000003,84.145706961199153,12.3,330,32,4.6585858525231369,2.6996580117654627,3.9120306173015429,null,0.4065040650406504,0.27921007204530712,0.36233119999999996,0.22512647202655134,543.49680000000001,0,-905.82799999999997,0,0,0,0,0,0.10005027581623505,0.12931807436918991,2.4012066195896411,6.2072675697211155,3.9516692672605265,418.07446153846155,66.538617134328632,576.6680151641815,19418.364322723108,3758.0255345510232,-151669.40132500001,2.6996580117654627,9581.8251975236453,1692.0952668659054,-153259.6237,3.9120306173015429,7608.6222129291973,777.51172829662778,-153578.62121493695,4.4419476350256151,null,119]
["IC/ICD","IC11-250A1",1496,4.9000000000000004,3125,11.3,"NA",9.6999999999999993,128,174.65537495307723,15.2,330,32,2.2444199046568958,1.1730050478353728,1.8210350197342999,null,0.32894736842105265,0.27349442584543682,0.33845503999999998,0.47326078025755708,634.60320000000002,0,-1057.672,0,0,0,0,0,5.5838445276776692E-2,7.217291666666667E-2,1.3401226866426406,3.4643000000000002,2.2054418774130125,488.15630769230768,77.692489370718974,673.33490787956453,90996.489726804808,16579.169241124157,-144653.23592499999,1.1730050478353728,41879.021680167461,7189.1972815494146,-151969.674325,1.8210350197342999,32808.763902079998,3235.7870917781356,-153320.76152360084,2.112999939390249,null,247]
["IC/ICD","IC11-250A5",1496,8.6,3125,19.100000000000001,"NA",3.2,42.6,101.11626970967629,15.2,330,32,3.8767252898619113,2.177216439428951,3.210175378476023,null,0.32894736842105265,0.27349442584543682,0.33845503999999998,0.27133903532034181,634.60320000000002,0,-1057.672,0,0,0,0,0,9.8002169261281524E-2,0.12667083333333332,2.3520520622707566,6.0801999999999996,3.8707755399493684,488.15630769230768,77.692489370718974,673.33490787956453,29367.366743874161,5352.2330675709554,-150862.2592,2.177216439428951,14105.441926967276,2409.9059885398015,-153095.9872,3.210175378476023,11010.705753510667,1084.6750179089963,-153548.93130280444,3.6854262373985516,null,143]
["IC/ICD","IC22-015A1",143,3.8,375,11,"NA",2.9,18.3,21.849599538664314,3.2,330,32,17.940832247581014,9.4477731075327949,15.605671245205297,null,1.5625,1.1614660460884658,1.1449386666666665,8.5097659082857477E-2,257.6112,0,-429.35199999999998,0,0,0,0,0,0.18389879063067374,0.26430804597701146,4.41357097513617,12.686786206896549,7.8448474225865246,198.16246153846154,31.538535289103745,273.33397250556578,1649.0838573151716,603.62163358970145,-152900.79250000001,9.4477731075327949,617.23179917050459,208.52383705826048,-153572.9197,15.605671245205297,1073.3308511191524,430.48360149851243,-153275.8261619398,11.751204566347999,null,30.9]
["IC/ICD","IC22-015A2",143,7.6,375,22,"NA",0.73,4.5999999999999996,10.889444430272832,3.2,330,32,35.998163405860602,19.055399156492761,31.424613311817488,null,1.5625,1.1614660460884658,1.1449386666666665,4.2221504090547278E-2,257.6112,0,-429.35199999999998,0,0,0,0,0,0.36779758126134748,0.52861609195402293,8.8271419502723401,25.373572413793099,15.689694845173049,198.16246153846154,31.538535289103745,273.33397250556578,414.70976942624782,151.45440028602667,-153470.55729999999,19.055399156492761,153.91978405384313,52.320611007900119,-153640.91477199999,31.424613311817488,269.19412415636504,108.01242379302036,-153565.61339438654,23.684613363262066,null,15.4]
["IC/ICD","IC22-015A6",143,13.1,375,38.1,"NA",0.24,1.5,6.293250352560273,3.2,330,32,62.288956904522841,33.665733444714057,54.845526252555885,null,1.5625,1.1614660460884658,1.1449386666666665,2.3986642720513009E-2,257.6112,0,-429.35199999999998,0,0,0,0,0,0.63396688348995422,0.91576867816091945,15.215205203758902,43.956896551724135,27.144609106203209,198.16246153846154,31.538535289103745,273.33397250556578,134.04446386864348,49.835848612820868,-153601.29044800001,33.665733444714057,50.76967673445202,17.135160546665443,-153656.58644799999,54.845526252555885,87.541988314820145,35.505895802386924,-153632.16895248755,41.68986930150151,null,8.9]
["IC/ICD","IC22-030A1",298,3.9,750,11,"NA",3.9,33.4,43.628488399209978,4.8,330,32,8.9849548857415442,4.9835181957785686,7.8879346166943751,null,1.0416666666666667,0.66609859100850222,0.6841706666666667,0.13010089749719184,307.8768,0,-513.12800000000004,0,0,0,0,0,0.10824102103888161,0.15165047935103246,2.5977845049331587,7.2792230088495575,4.3503069843884274,236.8283076923077,37.692395833319111,326.6674305554323,5806.4521547866852,1620.9069712162691,-152283.6925,4.9835181957785686,2394.0626762339293,574.68519888576816,-153490.49192500001,7.8879346166943751,2513.9001840162709,641.04026526600251,-153448.11111343259,7.6863420563381171,null,61.7]
["IC/ICD","IC22-030A2",298,7.9,750,22,"NA",1,8.4,21.849599538664314,4.8,330,32,{"$f":"IF(G183=\"NA\",(UAC_V*0.98)/J183,(IF((UAC_V*0.98)/J183<G183,(UAC_V*0.98)/J183,G183)))","v":17.940832247581014},{"$f":"IF(AO183<G183,IF(AO183<0,0,AO183),G183)","v":10.088806988242318},{"$f":"IF(AS183<G183,IF(AS183<0,0,AS183),G183)","v":15.815000908212035},null,{"$f":"IF(move1,Gewicht/K183,MAX(Gewicht,Gewicht2)/K183)","v":1.0416666666666667},{"$f":"IF(move1,IF(AccType=1,SQRT((V183^2*Ltime1+W183^2*Ltime2+X183^2*Ltime3+Y183^2*Ltime4)/ltime)/C183,SQRT((((V183-W183)*2/PI()+W183)^2*Ltime1+W183^2*Ltime2+((X183-W183)*2/PI()+W183)^2*Ltime3+Y183^2*Ltime4)/ltime)/C183),IF(AccType=1,SQRT((V183^2*Ltime1+W183^2*Ltime2+X183^2*Ltime3+Y183^2*Ltime4+Z183^2*Ltime5+AA183^2*Ltime6+AB183^2*Ltime7+AC183^2*Ltime8)/ltime)/C183,SQRT((((V183-W183)*2/PI()+W183)^2*Ltime1+W183^2*Ltime2+((X183-W183)*2/PI()+W183)^2*Ltime3+Y183^2*Ltime4+((Z183-AA183)*2/PI()+AA183)^2*Ltime5+AA183^2*Ltime6+((AB183-AA183)*2/PI()+AA183)^2*Ltime7+AC183^2*Ltime8)/ltime)/C183))","v":0.66609859100850222},{"$f":" IF(move1,MAX(ABS(V183),ABS(X183))/E183,MAX(ABS(V183),ABS(X183),ABS(Z183),ABS(AB183))/E183)","v":0.6841706666666667},{"$f":"IF(AW183>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW183,G183),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW183,G183)),\"NA\")","v":6.4849647843917391E-2},{"$f":"((Gewicht+K183)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":307.8768},0,{"$f":"((Gewicht+K183)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-513.12800000000004},0,{"$f":"((Gewicht2+K183)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K183)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"AF183/Irms","v":0.21925745287363199},{"$f":"AG183/Ipeak","v":0.3043927359882006},{"$f":"D183*S183","v":5.262178868967168},{"$f":"IF(move1,IF(MAX(ABS(V183),ABS(X183))<=C183,MAX(ABS(V183),ABS(X183))/C183*D183,D183+(MAX(ABS(V183),ABS(X183))-C183)/(E183-C183)*(F183-D183)),IF(MAX(ABS(V183),ABS(X183),ABS(Z183),ABS(AB183))<=C183,MAX(ABS(V183),ABS(X183),ABS(Z183),ABS(AB183))/C183*D183,D183+(MAX(ABS(V183),ABS(X183),ABS(Z183),ABS(AB183))-C183)/(E183-C183)*(F183-D183)))","v":14.610851327433629},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V183),ABS(X183))<=C183,MAX(ABS(V183),ABS(X183))/C183*D183,D183+(MAX(ABS(V183),ABS(X183))-C183)/(E183-C183)*(F183-D183)),IF(MAX(ABS(V183),ABS(X183),ABS(Z183),ABS(AB183))<=C183,MAX(ABS(V183),ABS(X183),ABS(Z183),ABS(AB183))/C183*D183,D183+(MAX(ABS(V183),ABS(X183),ABS(Z183),ABS(AB183))-C183)/(E183-C183)*(F183-D183))),IF(move1,IF(MAX(ABS((V183-W183)*2/PI()+W183),ABS((X183-W183)*2/PI()+W183))<=C183,MAX(ABS((V183-W183)*2/PI()+W183),ABS((X183-W183)*2/PI()+W183))/C183*D183,D183+(MAX(ABS((V183-W183)*2/PI()+W183),ABS((X183-W183)*2/PI()+W183))-C183)/(E183-C183)*(F183-D183)),IF(MAX(ABS((V183-W183)*2/PI()+W183),ABS((X183-W183)*2/PI()+W183),ABS((Z183-AA183)*2/PI()+AA183),ABS((AB183-AA183)*2/PI()+AA183))<=C183,MAX(ABS((V183-W183)*2/PI()+W183),ABS((X183-W183)*2/PI()+W183),ABS((Z183-AA183)*2/PI()+AA183),ABS((AB183-AA183)*2/PI()+AA183))/C183*D183,D183+(MAX(ABS((V183-W183)*2/PI()+W183),ABS((X183-W183)*2/PI()+W183),ABS((Z183-AA183)*2/PI()+AA183),ABS((AB183-AA183)*2/PI()+AA183))-C183)/(E183-C183)*(F183-D183))))","v":8.7942716168840604},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V183)+Ltime2*ABS(Lspeed2)*ABS(W183)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X183)+Ltime4*ABS(Lspeed1)*ABS(Y183))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V183)+Ltime2*ABS(Lspeed2)*ABS(W183)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X183)+Ltime4*ABS(Lspeed1)*ABS(Y183)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z183)+Ltime6*ABS(Lspeed6)*ABS(AA183)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB183)+Ltime8*ABS(Lspeed1)*ABS(AC183))/ltime)","v":236.8283076923077},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK183/2*Ltime1/ltime,AK183/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X183*-ABS(Lspeed2-Lspeed1),((X183-Y183)*2/PI()+Y183)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V183*-ABS(Lspeed2-Lspeed1),((V183-W183)*2/PI()+W183)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X183*-ABS(Lspeed2-Lspeed1),((X183-Y183)*2/PI()+Y183)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V183*-ABS(Lspeed2-Lspeed1),((V183-W183)*2/PI()+W183)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB183*-ABS(Lspeed6-Lspeed1),((AB183-AC183)*2/PI()+AB183)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z183*-ABS(Lspeed6-Lspeed1),((Z183-AA183)*2/PI()+AA183)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB183*-ABS(Lspeed6-Lspeed1),((AB183-AC183)*2/PI()+AB183)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z183*-ABS(Lspeed6-Lspeed1),((Z183-AA183)*2/PI()+AA183)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":37.692395833319111},{"$f":"IF(move1,MAX(IF(AccType=1,X183*-ABS(Lspeed2-Lspeed1),((X183-Y183)*2/PI()+Y183)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V183*-ABS(Lspeed2-Lspeed1),((V183-W183)*2/PI()+W183)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X183*-ABS(Lspeed2-Lspeed1),((X183-Y183)*2/PI()+Y183)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V183*-ABS(Lspeed2-Lspeed1),((V183-W183)*2/PI()+W183)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB183*-ABS(Lspeed6-Lspeed1),((AB183-AC183)*2/PI()+AB183)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z183*-ABS(Lspeed6-Lspeed1),((Z183-AA183)*2/PI()+AA183)*-ABS(Lspeed6-Lspeed1)),0))","v":326.6674305554323},{"$f":"(J183^2)+3*(I183/1000)^2*(F183/2)^2*(2000*PI()/M183)^2","v":1464.8774258372423},{"$f":"SQRT(3)*H183*F183/2*J183","v":416.29078178600105},{"$f":"3*F183^2*H183^2/4-(UAC_V*0.98)^2","v":-153301},{"$f":"-AM183/2/AL183+SQRT((AM183/2/AL183)^2-AN183/AL183)","v":10.088806988242318},{"$f":"(J183^2)+3*(I183/1000)^2*(D183/2)^2*(2000*PI()/M183)^2","v":604.7358968935996},{"$f":"SQRT(3)*H183*D183/2*J183","v":149.48623527770039},{"$f":"3*D183^2*H183^2/4-(UAC_V*0.98)^2","v":-153617.1925},{"$f":"-AQ183/2/AP183+SQRT((AQ183/2/AP183)^2-AR183/AP183)","v":15.815000908212035},{"$f":"(J183^2)+3*(I183/1000)^2*(AH183/2)^2*(2000*PI()/M183)^2","v":635.19495979666124},{"$f":"SQRT(3)*H183*AH183/2*J183","v":166.40791848323204},{"$f":"3*AH183^2*H183^2/4-(UAC_V*0.98)^2","v":-153605.99559004634},{"$f":"IF((AU183/2/AT183)^2-AV183/AT183>=0,-AU183/2/AT183+SQRT((AU183/2/AT183)^2-AV183/AT183),-9999)","v":15.420284199643431},null,30.9]
["IC/ICD","IC22-030A6",298,13.7,750,38.1,"NA",0.33,2.8,12.586500705120546,4.8,330,32,31.144478452261421,17.607443333223891,27.528041534385576,null,1.0416666666666667,0.66609859100850222,0.6841706666666667,3.724772600677137E-2,307.8768,0,-513.12800000000004,0,0,0,0,0,0.38023127903402004,0.52735634218289096,9.1255506968164806,25.313104424778764,15.247533861841919,236.8283076923077,37.692395833319111,326.6674305554323,487.48906521340666,137.0485836852574,-153545.43975324999,17.607443333223891,200.96791083686682,49.279936915696226,-153648.67041925,27.528041534385576,211.12311917236531,54.846533345365827,-153645.0116006817,26.847276524161693,null,17.8]
["IC/ICD","IC22-050A1",548,4.4000000000000004,1250,11,"NA",5.3,53.4,72.831998462214386,6.9,330,32,5.3822496742743038,3.0266457117569843,4.6072226314270219,null,0.72463768115942029,0.43984038869252773,0.49846720000000005,0.20354592959774725,373.85040000000004,0,-623.08400000000006,0,0,0,0,0,8.0637404593630099E-2,0.10637329059829061,1.9352977102471223,5.1059179487179494,3.1849222895654772,287.57723076923077,45.769337797601786,396.66759424588213,15281.246281960197,3677.2352391096761,-151114.83249999999,3.0266457117569843,6900.7794051136307,1470.8940956438705,-153256.13320000001,4.6072226314270219,6140.8753757738614,1064.7007706378222,-153450.29696842365,4.9128960818633214,null,103]
["IC/ICD","IC22-050A2",548,8.6999999999999993,1250,22,"NA",1.3,13.4,36.345288552988542,6.9,330,32,10.785441954285083,6.20195450506192,9.3623646678165802,null,0.72463768115942029,0.43984038869252773,0.49846720000000005,0.10054057366761256,373.85040000000004,0,-623.08400000000006,0,0,0,0,0,0.15944214090104128,0.21088607549857552,3.8266113816249909,10.122531623931625,6.297459981640829,287.57723076923077,45.769337797601786,396.66759424588213,3833.8846029384245,900.21197537024568,-153050.53,6.20195450506192,1713.9588210669615,355.9929175327789,-153568.06292500001,9.3623646678165802,1526.8824304192237,257.68404044945282,-153613.73348218569,9.9462332819584169,null,51.4]
["IC/ICD","IC22-050A6",548,15.1,1250,38.1,"NA",0.44,4.5,21.001071401240459,6.9,330,32,18.665714358594389,10.785023839943195,16.247338082249669,null,0.72463768115942029,0.43984038869252773,0.49846720000000005,5.795496114300068E-2,373.85040000000004,0,-623.08400000000006,0,0,0,0,0,0.27673291121904869,0.36583368945868949,6.6415898692571682,17.560017094017095,10.930074221008796,287.57723076923077,45.769337797601786,396.66759424588213,1291.000174817791,304.89460190652767,-153453.22622800001,10.785023839943195,574.55074838297094,120.83749314405689,-153630.89294799999,16.247338082249669,510.99573676580405,87.467733029482346,-153646.65346093639,17.254778198065821,null,29.7]
["IC/ICD","IC22-075A1",864,4.5999999999999996,1875,11,"NA",7.1,78.900000000000006,108.89444430272832,9.6,330,32,3.5998163405860604,1.9986345812534965,3.0268973408591515,null,0.52083333333333337,0.34226919758123014,0.4077098666666667,0.29755381270080655,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,6.5601596203069115E-2,8.479209104938272E-2,1.5744383088736587,4.0700203703703703,2.5910554417166041,352.82584615384616,56.153977465965212,486.66780470503181,33638.127622045999,7365.2482330875982,-149089.29250000001,1.9986345812534965,15666.822318037133,3080.0128974729955,-152863.9933,3.0268973408591515,13066.449375354998,1734.8878649032022,-153410.17676642028,3.3607366375960721,null,154]
["IC/ICD","IC22-075A2",864,9.1999999999999993,1875,22,"NA",1.8,19.7,54.51793282948281,9.6,330,32,7.1902946361900559,4.150006188094804,6.1563221933049492,null,0.52083333333333337,0.34226919758123014,0.4077098666666667,0.14742819084557021,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.13120319240613823,0.16958418209876544,3.1488766177473173,8.1400407407407407,5.1821108834332081,352.82584615384616,56.153977465965212,486.66780470503181,8403.4432900109878,1869.6710257689717,-152487.88,4.150006188094804,3921.9984067490282,781.86242895793362,-153458.3248,6.1563221933049492,3273.5520183858989,440.40193504895996,-153598.74411610409,6.7829632464763243,null,77.099999999999994]
["IC/ICD","IC22-075A6",864,15.9,1875,38.1,"NA",0.59,6.6,31.466251762801363,9.6,330,32,12.457791380904569,7.2668063807075178,10.736991649930665,null,0.52083333333333337,0.34226919758123014,0.4077098666666667,8.474248572999539E-2,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.22675334339756495,0.29308570601851852,5.442080241541559,14.06811388888889,8.9560394615856538,352.82584615384616,56.153977465965212,486.66780470503181,2818.4730204969378,612.56563919925645,-153285.02091925,7.2668063807075178,1308.5470713978484,255.63762895716999,-153597.99762924999,10.736991649930665,1091.1528036488398,143.99375426456641,-153643.05900642122,11.800456304600004,null,44.5]
["IC/ICD","IC22-100A1",1198,4.8,2500,11,"NA",8.8000000000000007,104,145.66399692442877,12.5,330,32,2.6911248371371519,1.4757109638679831,2.2231427453016108,null,0.4,0.2958761330201134,0.36651999999999996,0.39521375658773894,549.78,0,-916.3,0,0,0,0,0,5.9175226604022683E-2,7.6485809682804676E-2,1.4202054384965443,3.6713188647746242,2.3372341799816283,422.90769230769229,67.307849702355554,583.33469742041473,59059.913824601797,12211.196265722698,-146636.32,1.4757109638679831,28423.600781147314,5328.5220068608132,-152325.83679999999,2.2231427453016108,22926.410294718236,2594.5841173373742,-153346.72849741072,2.530276295627873,null,206]
["IC/ICD","IC22-100A2",1198,9.5,2500,22,"NA",2.2000000000000002,26,72.831998462214386,12.5,330,32,5.3822496742743038,3.1058296344249494,4.5652295140080774,null,0.4,0.2958761330201134,0.36651999999999996,0.19513157408751208,549.78,0,-916.3,0,0,0,0,0,0.11711763598712821,0.1513781649972176,2.810823263691077,7.2661519198664442,4.6257759812136392,422.90769230769229,67.307849702355554,583.33469742041473,14764.978456150449,3052.7990664306744,-151907.07999999999,3.1058296344249494,7068.5664889825985,1318.2541423223367,-153336.39249999999,4.5652295140080774,5722.7509469898032,641.88929986211065,-153586.32597355501,5.1247472618220291,null,103]
["IC/ICD","IC22-100A6",1198,16.5,2500,38.1,"NA",0.73,8.6999999999999993,41.938503192174132,12.5,330,32,9.3470193297968862,5.4677309222615689,7.9830904316763913,null,0.4,0.2958761330201134,0.36651999999999996,0.11190429251466763,549.78,0,-916.3,0,0,0,0,0,0.20341484145132796,0.26291997078464108,4.8819561948318713,12.620158597662771,8.0342424936868468,422.90769230769229,67.307849702355554,583.33469742041473,4935.7816145411662,1010.1628521981629,-153083.82777325,5.4677309222615689,2354.6750072036102,437.47210134566114,-153555.18848124999,7.9830904316763913,1900.1078792033543,213.01557251113874,-153638.20135746311,8.9362076961339714,null,59.31]
["IC/ICD","IC22-150A1",1810,4.8,3750,11,"NA",12.4,155,217.78888860545663,18.100000000000001,330,32,1.7999081702930302,0.93759503057075422,1.4569109260696185,null,0.27624309392265189,0.25850092912303119,0.32253760000000004,0.58899489763319801,725.70960000000002,0,-1209.5160000000001,0,0,0,0,0,5.1700185824606233E-2,6.6824088397790055E-2,1.2408044597905497,3.2075562430939226,2.0419937253346676,558.23815384615386,88.84636160710933,770.00180059494755,131488.21113499062,25726.500870503161,-139710.28,0.93759503057075422,63437.414087191595,11226.109470765015,-151007.02720000001,1.4569109260696185,50328.631480730168,4775.7593956713026,-153183.14577067501,1.697807576972864,null,308]
["IC/ICD","IC22-150A2",1810,9.6,3750,22,"NA",3.1,38.700000000000003,108.89444430272832,18.100000000000001,330,32,3.5998163405860604,2.0434196414873838,3.0197413336518051,null,0.27624309392265189,0.25850092912303119,0.32253760000000004,0.29015361428155872,725.70960000000002,0,-1209.5160000000001,0,0,0,0,0,0.10340037164921247,0.13364817679558011,2.4816089195810993,6.4151124861878452,4.0839874506693352,558.23815384615386,88.84636160710933,770.00180059494755,32817.857957088709,6431.6252176257904,-150175.57,2.0434196414873838,15849.034110176231,2806.5273676912539,-152999.7568,3.0197413336518051,12580.290281352718,1193.9398489178257,-153543.78644266876,3.44645026213467,null,154]
["IC/ICD","IC22-150A6",1810,16.600000000000001,3750,38.1,"NA",1,12.9,62.932503525602726,18.100000000000001,330,32,6.2288956904522843,3.6399604580288081,5.3029292621153967,null,0.27624309392265189,0.25850092912303119,0.32253760000000004,0.16661163807166887,725.70960000000002,0,-1209.5160000000001,0,0,0,0,0,0.17879647597676326,0.23109997237569066,4.2911154234423181,11.092798674033151,7.0618949667823925,558.23815384615386,88.84636160710933,770.00180059494755,10945.242747724871,2076.4936922008696,-152575.29250000001,3.6399604580288081,5286.4179198015072,904.71903649696674,-153457.32999999999,5.3029292621153967,4200.4622756673834,384.88137410784009,-153626.5972296086,6.0019816837155444,null,89]
["IC/ICD","IC22-200A1",2513,5,5000,11,"NA",15.9,205,290.62088706767099,23.7,330,32,1.3488362930663098,0.66237051190776519,1.0549827986533973,null,0.2109704641350211,0.23132262477806492,0.30054639999999999,0.78746543862843699,901.63919999999996,0,-1502.732,0,0,0,0,0,4.8192213495430188E-2,6.2289925719591459E-2,1.1566131238903246,2.9899164345403899,1.9034399199551935,693.56861538461533,110.38487351186312,956.66890376948027,231493.26890522285,44019.718930312913,-130721.49249999999,0.66237051190776519,114839.17126140966,20008.963150142237,-148923.8125,1.0549827986533973,88863.078539057737,7617.17184337863,-152977.03618979806,1.2698970023900271,null,411]
["IC/ICD","IC22-200A2",2513,10,5000,22,"NA",4,51.3,145.66399692442877,23.7,330,32,2.6911248371371519,1.5032167110040158,2.213892795087443,null,0.2109704641350211,0.23132262477806492,0.30054639999999999,0.38765084821512802,901.63919999999996,0,-1502.732,0,0,0,0,0,9.6384426990860375E-2,0.12457985143918292,2.3132262477806491,5.9798328690807798,3.8068798399103869,693.56861538461533,110.38487351186312,956.66890376948027,58047.950515187244,11101.087514293362,-147856,1.5032167110040158,28827.493908096534,5045.9488701333457,-152464,2.213892795087443,22320.793281661194,1920.9321026929231,-153490.09199061382,2.5796409439172616,null,206]
["IC/ICD","IC22-200A6",2513,17.3,5000,38.1,"NA",1.3,17.100000000000001,84.145706961199153,23.7,330,32,4.6585858525231369,2.7091342344199325,3.9092538764923561,null,0.2109704641350211,0.23132262477806492,0.30054639999999999,0.22222582077701197,901.63919999999996,0,-1502.732,0,0,0,0,0,0.16674505869418846,0.21552314298978645,4.0018814086605232,10.345110863509749,6.5859021230449697,693.56861538461533,110.38487351186312,956.66890376948027,19353.85272436891,3609.3660020615112,-151824.084325,2.7091342344199325,9610.9949241713475,1638.8984733770117,-153284.64992500001,3.9092538764923561,7447.2277791870883,623.90895579588562,-153609.02331966354,4.4999271304455206,null,119]
["IC/ICD","IC22-250A1",3000,5,6250,11,"NA",19.3,256,349.31074990615446,29.3,330,32,1.1222099523284479,0.49981159245743151,0.84836050264670471,null,0.17064846416382251,0.23158027680728926,0.28735168,0.95608201992314112,1077.5688,0,-1795.9479999999999,0,0,0,0,0,4.8245891001518597E-2,6.235930555555555E-2,1.1579013840364463,2.9932466666666664,1.9055600115733551,828.8990769230769,131.92338541661687,1143.336006944013,351308.64944610791,64223.294040519293,-119860.5325,0.49981159245743151,169392.10112522892,29192.406382054221,-146679.8125,0.84836050264670471,128898.91566656852,11125.576448648266,-152649.57219988268,1.0459353686835251,null,494]
["IC/ICD","IC22-250A2",3000,9.9,6250,22,"NA",4.8,63.9,174.65537495307723,29.3,330,32,2.2444199046568958,1.1996462943877098,1.8169787993251265,null,0.17064846416382251,0.23158027680728926,0.28735168,0.46704062857595452,1077.5688,0,-1795.9479999999999,0,0,0,0,0,9.5526864183006821E-2,0.12347142499999998,2.2926447403921637,5.9266283999999994,3.7730088229152434,828.8990769230769,131.92338541661687,1143.336006944013,87648.168989553349,15972.632714740545,-145300.48000000001,1.1996462943877098,42076.092970384547,7187.6847216332462,-151970.3872,1.8169787993251265,32185.231738774251,2739.3129162682153,-153418.00890841568,2.1411413457734558,null,247]
["IC/ICD","IC22-250A6",3000,17.2,6250,38.1,"NA",1.6,21.3,101.11626970967629,29.3,330,32,3.8767252898619113,2.1811264720553338,3.210175378476023,null,0.17064846416382251,0.23158027680728926,0.28735168,0.26804297095079782,1077.5688,0,-1795.9479999999999,0,0,0,0,0,0.16596586504522395,0.21451601111111107,3.9831807610853751,10.296768533333331,6.5551264398123408,828.8990769230769,131.92338541661687,1143.336006944013,29267.273494473273,5338.2219862422362,-150876.9088,2.1811264720553338,14105.441926967276,2409.9059885398015,-153095.9872,3.210175378476023,10788.192681697983,918.44409668252024,-153581.49820932749,3.7307450982684447,null,143]
["IC/ICD","IC33-015A1",216,3.8,565,11.1,"NA",4.3,27.4,32.739043968937146,5,330,32,11.973471197629662,6.1905702458877405,10.359291090711759,null,1,0.93772382898967155,0.9267256637168142,0.11452393486144659,314.16000000000003,0,-523.6,0,0,0,0,0,0.14847293959003133,0.21320916905444123,3.5633505501607519,10.23404011461318,6.2542665430520312,241.66153846153847,38.461628401346033,333.33411281166559,3746.5021909236548,1353.2812332717003,-151955.38532500001,6.1905702458877405,1385.3102206552842,463.28546724616763,-153463.75330000001,10.359291090711759,1920.9764784430113,762.50284149471963,-153121.56095024233,8.7317991755157607,null,46.3]
["IC/ICD","IC33-015A3",216,11.4,565,33.299999999999997,"NA",0.48,3,10.889444430272832,5,330,32,35.998163405860602,19.230778774918502,31.582474558648006,null,1,0.93772382898967155,0.9267256637168142,3.7269637832614735E-2,314.16000000000003,0,-523.6,0,0,0,0,0,0.44541881877009398,0.63962750716332373,10.690051650482255,30.702120343839539,18.762799629156092,241.66153846153847,38.461628401346033,333.33411281166559,407.15055845385484,150.73767958728828,-153472.38380800001,19.230778774918502,152.39997292487351,51.603890309161763,-153641.542912,31.582474558648006,210.19336479551913,84.932759118925617,-153603.16703009314,26.831492285790283,null,15.4]
["IC/ICD","IC33-015A5",216,6.6,565,19.100000000000001,"NA",1.4,9.1,18.879751057680817,5,330,32,20.762985634840948,10.981554380750014,18.095259006475992,null,1,0.93772382898967155,0.9267256637168142,6.5173791715104026E-2,314.16000000000003,0,-523.6,0,0,0,0,0,0.25787405297215965,0.36702483285577853,6.1889772713318321,17.617191977077368,10.802511203856218,241.66153846153847,38.461628401346033,333.33411281166559,1229.9603932532236,437.20819944449806,-153127.72930000001,10.981554380750014,460.74677497905861,151.07717886563802,-153599.96679999999,18.095259006475992,635.86229174750963,247.27468444591588,-153492.45945498513,15.343590938690928,null,26.7]
["IC/ICD","IC33-015A7",216,19.8,565,57.7,"NA",0.16,1,6.293250352560273,5,330,32,62.288956904522841,33.438038204381108,54.752321245748661,null,1,0.93772382898967155,0.9267256637168142,2.1471654370845972E-2,314.16000000000003,0,-523.6,0,0,0,0,0,0.77362215891647912,1.1084192932187202,18.566931813995499,53.204126074498575,32.542013970092057,241.66153846153847,38.461628401346033,333.33411281166559,135.87094307569177,50.315458704457818,-153600.077632,33.438038204381108,50.940780398641806,17.265963298930068,-153656.472832,54.752321245748661,70.225332184721367,28.377233276812071,-153643.66753267398,46.573029852687618,null,8.9]
["IC/ICD","IC33-030A1",450,4,1125,11.1,"NA",5.8,50.1,65.478087937874292,7.3,330,32,5.986735598814831,3.2383065622102412,5.1842657341248257,null,0.68493150684931503,0.55363214863550214,0.57246933333333339,0.18901454202224816,386.41680000000002,0,-644.02800000000002,0,0,0,0,0,9.2272024772583686E-2,0.12585181481481481,2.2145285945420086,6.0408871111111111,3.6444529667408774,297.2436923076923,47.307802933655616,410.0009587583487,13229.540338577286,3650.7121641748195,-150555.4117,3.2383065622102412,5448.6052691927316,1315.5719510539889,-153260.32,5.1842657341248257,5251.3448428967477,1198.6350249949485,-153328.89419572218,5.2905982222378105,null,92.6]
["IC/ICD","IC33-030A3",450,11.9,1125,33.1,"NA",0.64,5.6,21.849599538664314,7.3,330,32,17.940832247581014,10.074572717120256,15.805621428824276,null,0.68493150684931503,0.55363214863550214,0.57246933333333339,6.2084245565561705E-2,386.41680000000002,0,-644.02800000000002,0,0,0,0,0,0.27450927369843647,0.37487325925925924,6.5882225687624754,17.993916444444444,10.84224757605411,297.2436923076923,47.307802933655616,410.0009587583487,1470.8711749049962,400.85017824339297,-153327.42860799999,10.074572717120256,605.81268615501529,144.11229973100836,-153620.497408,15.805621428824276,583.999730837372,131.30262457463098,-153627.88730905586,16.107145877193403,null,30.9]
["IC/ICD","IC33-030A5",450,6.9,1125,19.100000000000001,"NA",1.9,16.7,37.830212793480293,7.3,330,32,10.362088157948659,5.7743947314321833,9.0797123864566007,null,0.68493150684931503,0.55363214863550214,0.57246933333333339,0.10803083658808216,386.41680000000002,0,-644.02800000000002,0,0,0,0,0,0.15916924273270686,0.21680992592592596,3.8200618255849648,10.406876444444446,6.286681367628014,297.2436923076923,47.307802933655616,410.0009587583487,4372.9763225986171,1188.9302694899206,-152676.27692500001,5.7743947314321833,1815.0551046268474,429.50884081049486,-153535.095925,9.0797123864566007,1749.8358761827374,391.33119228331083,-153556.99320321155,9.2566162734901827,null,53.5]
["IC/ICD","IC33-030A7",450,20.6,1125,57.3,"NA",0.21,1.9,12.586500705120546,7.3,330,32,31.144478452261421,17.374285083712646,27.414966328930849,null,0.68493150684931503,0.55363214863550214,0.57246933333333339,3.5781949715177529E-2,386.41680000000002,0,-644.02800000000002,0,0,0,0,0,0.47520092757880605,0.64894529629629627,11.404822261891345,31.149374222222221,18.76893277871552,297.2436923076923,47.307802933655616,410.0009587583487,501.13845340897501,131.1624598333494,-153555.40518325,17.374285083712646,202.71581392098557,47.154392191396127,-153649.964293,27.414966328930849,195.19116614678094,42.962991129199118,-153652.34857589466,27.947051738654498,null,17.8]
["IC/ICD","IC33-050A1",824,4.4000000000000004,1875,11.1,"NA",7.9,80.2,108.89444430272832,10.4,330,32,3.5998163405860604,1.9468530587717117,3.0392833791535314,null,0.48076923076923073,0.37854909523680136,0.43005013333333336,0.30077659099567655,483.8064,0,-806.34400000000005,0,0,0,0,0,6.9400667460080251E-2,8.9702508090614905E-2,1.665616019041926,4.3057203883495152,2.7411067335095223,372.15876923076922,59.230907738072894,513.33453372996507,34772.782404907819,8269.6365884692896,-147896.84792500001,1.9468530587717117,15458.602121248401,3278.0541431770162,-152757.80679999999,3.0392833791535314,13255.403005485299,2042.158246516206,-153312.30407287789,3.3247268236189775,null,154]
["IC/ICD","IC33-050A3",824,13.1,1875,33.1,"NA",0.88,8.9,36.345288552988542,10.4,330,32,10.785441954285083,6.2021966185971955,9.3600880052888247,null,0.48076923076923073,0.37854909523680136,0.43005013333333336,9.8675520090120844E-2,483.8064,0,-806.34400000000005,0,0,0,0,0,0.20662471448342076,0.26706883090614891,4.9589931476020981,12.819303883495147,8.161022320221532,372.15876923076922,59.230907738072894,513.33453372996507,3830.305756193392,916.83127337708117,-153027.669712,6.2021966185971955,1714.0262418381978,362.85467314923756,-153564.328912,9.3600880052888247,1473.5222640835877,226.05076996699358,-153625.31739269127,10.134225784538,null,51.4]
["IC/ICD","IC33-050A5",824,7.6,1875,19.100000000000001,"NA",2.6,26.7,62.932503525602726,10.4,330,32,6.2288956904522843,3.5204916427889277,5.3530559101807027,null,0.48076923076923073,0.37854909523680136,0.43005013333333336,0.17191068878337257,483.8064,0,-806.34400000000005,0,0,0,0,0,0.11987388015832041,0.15494069579288025,2.8769731237996901,7.4371533980582525,4.7346389033346288,372.15876923076922,59.230907738072894,513.33453372996507,11480.369444466736,2706.5269489421303,-151814.41329999999,3.5204916427889277,5151.113357946324,1076.9426603120519,-153371.1568,5.3530559101807027,4422.5801268062014,670.9124494965962,-153550.34679588702,5.8169739594267815,null,89]
["IC/ICD","IC33-050A7",824,22.7,1875,57.3,"NA",0.28999999999999998,3,21.001071401240459,10.4,330,32,18.665714358594389,10.767763632100737,16.240045355494384,null,0.48076923076923073,0.37854909523680136,0.43005013333333336,5.6892460226049456E-2,483.8064,0,-806.34400000000005,0,0,0,0,0,0.35804435257814132,0.46278339401294505,8.5930644618753913,22.213602912621361,14.141618829696853,372.15876923076922,59.230907738072894,513.33453372996507,1295.4677370306856,302.22104508952333,-153456.90648325,10.767763632100737,575.1408283199296,119.72805800230681,-153631.49808324999,16.240045355494384,493.08793815511609,74.588042268214053,-153651.38592195942,17.577021560092916,null,29.7]
["IC/ICD","IC33-075A1",1301,4.5999999999999996,2815,11.1,"NA",10.6,118,163.34166645409246,14.4,330,32,2.3998775603907072,1.2657225126921203,1.9815495019870757,null,0.34722222222222221,0.30203212398142343,0.36084689165186495,0.44476577505088932,609.47039999999993,0,-1015.7839999999999,0,0,0,0,0,5.7889490429772816E-2,7.4823955931334854E-2,1.3893477703145476,3.5915498847040732,2.28645167004712,468.82338461538455,74.6155590986113,646.66817885463115,76286.135258166352,16643.952121096419,-143281.09330000001,1.2657225126921203,35199.737416303869,6897.4936718057224,-151880.8468,1.9815495019870757,28785.291638868766,3428.4317228347036,-153223.44813335061,2.2483744390754477,null,231]
["IC/ICD","IC33-075A3",1301,13.8,2815,33.1,"NA",1.2,13.1,54.51793282948281,14.4,330,32,7.1902946361900559,4.1483130251757929,6.1600445320967001,null,0.34722222222222221,0.30203212398142343,0.36084689165186495,0.14572978257414032,609.47039999999993,0,-1015.7839999999999,0,0,0,0,0,0.17366847128931848,0.2244718677940046,4.1680433109436432,10.774649654112221,6.8593550101413605,468.82338461538455,74.6155590986113,646.66817885463115,8408.7078786813254,1875.3366955440295,-152480.74119999999,4.1483130251757929,3917.1832388040189,781.86242895793362,-153458.3248,6.1600445320967001,3205.6745230046263,388.62840357347068,-153613.18518875242,6.8620153158552055,null,77.099999999999994]
["IC/ICD","IC33-075A5",1301,8,2815,19.100000000000001,"NA",3.5,39.4,94.752308678997366,14.4,330,32,4.1371023615690543,2.3291282816482703,3.4983925586624851,null,0.34722222222222221,0.30203212398142343,0.36084689165186495,0.25495346564520149,609.47039999999993,0,-1015.7839999999999,0,0,0,0,0,0.10067737466047448,0.13012861901101716,2.4162569918513874,6.2461737125288233,3.9764376870384699,468.82338461538455,74.6155590986113,646.66817885463115,25352.959013048832,5485.5710417193577,-150312.30812500001,2.3291282816482703,11850.721079014076,2297.621378730621,-153076,3.4983925586624851,9687.7441956881394,1142.0435301162163,-153518.72672926262,3.9222843959753053,null,134]
["IC/ICD","IC33-075A7",1301,23.9,2815,57.3,"NA",0.39,4.4000000000000004,31.466251762801363,14.4,330,32,12.457791380904569,7.2553640143959903,10.732210203962156,null,0.34722222222222221,0.30203212398142343,0.36084689165186495,8.3828189656358007E-2,609.47039999999993,0,-1015.7839999999999,0,0,0,0,0,0.30077365679816748,0.38875924929541372,7.2185677631560194,18.660443966179859,11.879607590027428,468.82338461538455,74.6155590986113,646.66817885463115,2828.0832432126745,608.96856351197937,-153289.45869325,7.2553640143959903,1309.8835739016388,254.00259455386225,-153598.83921924999,10.732210203962156,1069.125635845264,126.2531861986913,-153647.90115689905,11.929161348937162,null,44.5]
["IC/ICD","IC33-100A1",1796,4.8,3750,11.1,"NA",13.2,156,217.78888860545663,18.899999999999999,330,32,1.7999081702930302,0.91492124216999215,1.4475163910120223,null,0.26455026455026459,0.26953816786059465,0.33370773333333331,0.59264824941041017,750.8424,0,-1251.404,0,0,0,0,0,5.3907633572118925E-2,6.9677282850779509E-2,1.2937832057308543,3.3445095768374165,2.1291809254874319,577.57107692307693,91.923291879217018,796.66852961988081,134131.4211176915,27635.241257669521,-137562.9172,0.91492124216999215,63644.601757581462,11950.374597911145,-150653.13279999999,1.4475163910120223,50622.034455281842,5300.9395096462385,-153071.5737964891,1.6873415233991484,null,308]
["IC/ICD","IC33-100A3",1796,14.3,3750,33.1,"NA",1.5,17.3,72.831998462214386,18.899999999999999,330,32,5.3822496742743038,3.1001608215709981,4.5607988260810339,null,0.26455026455026459,0.26953816786059465,0.33370773333333331,0.19380299045740351,750.8424,0,-1251.404,0,0,0,0,0,0.16059982501693765,0.20758023849294729,3.8543958004065035,9.9638514476614706,6.3431848405146418,577.57107692307693,91.923291879217018,796.66852961988081,14785.829447937384,3131.6420175265084,-151815.15812499999,3.1001608215709981,7074.1416232132915,1352.9450408045036,-153318.923125,4.5607988260810339,5652.6993720663259,600.13849460703432,-153596.10176025843,5.1598791001101336,null,103]
["IC/ICD","IC33-100A5",1796,8.1999999999999993,3750,19.100000000000001,"NA",4.4000000000000004,52,125.86500705120545,18.899999999999999,330,32,3.1144478452261422,1.7283968406055512,2.5985188844817961,null,0.26455026455026459,0.26953816786059465,0.33370773333333331,0.33734077387597694,750.8424,{"$f":"(Ltorque+IF(Lspeed2=0,0,IF(Lspeed2>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},-1251.404,{"$f":"(Ltorque+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},0,{"$f":"(Ltorque2+IF(Lspeed6=0,0,IF(Lspeed6>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},0,0,9.2092207352369837E-2,0.11903202487008165,2.2102129764568761,5.7135371937639192,3.6373507477076963,577.57107692307693,91.923291879217018,796.66852961988081,44364.951616431783,9160.5527502656751,-148366.95879999999,1.7283968406055512,21099.211333814514,3932.8027514229589,-152687.6752,2.5985188844817961,16876.422823944591,1744.5101254238034,-153471.89574689395,2.9643614927131496,null,178]
["IC/ICD","IC33-100A7",1796,24.7,3750,57.3,"NA",0.49,5.8,41.93143212436226,18.899999999999999,330,32,9.3485955556535139,5.4578609660357564,7.9876641140113547,null,0.26455026455026459,0.26953816786059465,0.33370773333333331,0.11110676261325532,750.8424,0,-1251.404,0,0,0,0,0,0.27739969775652867,0.35854768466963621,6.6575927461566877,17.210288864142537,10.956410179070744,577.57107692307693,91.923291879217018,796.66852961988081,4951.8873193013615,1019.5793460079275,-153072.76155324999,5.4578609660357564,2351.6769668937454,439.50453484111358,-153554.13804324999,7.9876641140113547,1875.010245305027,194.95514005185953,-153642.38327045852,9.0003522421118358,null,59.3]
["IC/ICD","IC33-150A1",2718,4.8,5625,11.1,"NA",18.5,232,327.39043968937148,27.3,330,32,1.1973471197629661,0.54893058801476713,0.93211985233149253,null,0.18315018315018314,0.24070314974595802,0.30066275555555555,0.89268852746492,1014.7367999999999,0,-1691.2279999999998,0,0,0,0,0,4.8140629949191605E-2,6.2223252391464305E-2,1.1553751187805985,2.9867161147902865,1.9014025331243793,780.56676923076918,124.23105973634766,1076.6691843816798,298937.85479284299,58222.564687270824,-122037.533125,0.54893058801476713,143041.95714168577,25177.325270171172,-147749.92000000001,0.93211985233149253,112811.08843958197,9973.3812595833133,-152735.98957172906,1.1202115510992685,null,463]
["IC/ICD","IC33-150A3",2718,14.4,5625,33.1,"NA",2.1,25.8,108.89444430272832,27.3,330,32,3.5998163405860604,2.0369012947019982,3.018135049808726,null,0.18315018315018314,0.24070314974595802,0.30066275555555555,0.2888350073139721,1014.7367999999999,0,-1691.2279999999998,0,0,0,0,0,0.14442188984757481,0.18666975717439291,3.4661253563417955,8.9601483443708592,5.704207599373138,780.56676923076918,124.23105973634766,1076.6691843816798,32945.079868104651,6555.1652328030596,-150040.269925,2.0369012947019982,15849.034110176231,2851.7939381378869,-152978.1568,3.018135049808726,12484.254848400531,1129.6683787341933,-153556.38061680621,3.4621842043993327,null,154]
["IC/ICD","IC33-150A5",2718,8.3000000000000007,5625,19.100000000000001,"NA",6.2,77.3,188.79751057680818,27.3,330,32,2.0762985634840949,1.1103265533020448,1.6997860778714307,null,0.18315018315018314,0.24070314974595802,0.30066275555555555,0.50557132998151721,1014.7367999999999,0,-1691.2279999999998,0,0,0,0,0,8.324317262047716E-2,0.10759437392690703,1.9978361428914517,5.1645299484915377,3.2878418801942395,780.56676923076918,124.23105973634766,1076.6691843816798,98674.421436445497,19362.07740397063,-143146.52770000001,1.1103265533020448,47546.945897197802,8413.887039421792,-151677.9013,1.6997860778714307,37512.17746032017,3332.9554437872875,-153352.35046107334,1.9779602613869702,null,267]
["IC/ICD","IC33-150A7",2718,24.9,5625,57.3,"NA",0.69,8.6,62.932503525602726,27.3,330,32,6.2288956904522843,3.629529960989939,5.2997243207142466,null,0.18315018315018314,0.24070314974595802,0.30066275555555555,0.16593526292687319,1014.7367999999999,0,-1691.2279999999998,0,0,0,0,0,0.24972951786143141,0.32278312178072105,5.9935084286743541,15.493589845474609,9.8635256405827167,780.56676923076918,124.23105973634766,1076.6691843816798,10981.956181198835,2154.8118401193115,-152491.61922324999,3.629529960989939,5286.4179198015063,936.38420277436035,-153442.60992925,5.2997243207142466,4168.5569854663991,370.92568648600439,-153629.26048102634,6.0264465934567193,null,89]
["IC/ICD","IC33-200A1",3765,5,7500,11.1,"NA",23.9,308,436.28488399209976,35.700000000000003,330,32,0.89849548857415451,0.35229146414311008,0.6609529542574536,null,0.14005602240896359,0.21895664609333332,0.2841402666666667,1.1985624530949848,1278.6312,0,-2131.0520000000001,0,0,0,0,0,4.5615967936111113E-2,5.8960048694112442E-2,1.0947832304666667,2.8300823373173971,1.8016863733645141,983.56246153846166,156.53882759347835,1356.6698391434791,528306.93774279603,100235.52689835991,-100879.91192500001,0.35229146414311008,258918.97401647508,45151.138242504458,-142953.8125,0.6609529542574536,199248.41210514115,16269.638102683537,-152273.35764368137,0.83433282714451185,null,617]
["IC/ICD","IC33-200A3",3765,14.9,7500,33.1,"NA",2.7,34.200000000000003,145.66399692442877,35.700000000000003,330,32,2.6911248371371519,1.498128874411061,2.2170474992333373,null,0.14005602240896359,0.21895664609333332,0.2841402666666667,0.38623089384773623,1278.6312,0,-2131.0520000000001,0,0,0,0,0,0.1359355844496111,0.1757009451084551,3.2624540267906665,8.4336453652058445,5.3690253926262521,983.56246153846166,156.53882759347835,1356.6698391434791,58271.500536220658,11273.91126309543,-147673.75232500001,1.498128874411061,28726.372189051162,5074.9630761366134,-152450.160325,2.2170474992333373,22192.909206127286,1828.6983639206787,-153506.39147392751,2.5891248367983475,null,206]
["IC/ICD","IC33-200A5",3765,8.6,7500,19.100000000000001,"NA",8,103,251.73001410241091,35.700000000000003,330,32,1.5572239226130711,0.79144097454356721,1.2364759426346732,null,0.14005602240896359,0.21895664609333332,0.2841402666666667,0.67578800707668008,1278.6312,0,-2131.0520000000001,0,0,0,0,0,7.8459464850111099E-2,0.10141128375387339,1.8830271564026664,4.8677416201859227,3.0989005621869641,983.56246153846166,156.53882759347835,1356.6698391434791,175276.28169331537,33311.100910056994,-136153.12,0.79144097454356721,86055.800537369039,14998.715593009954,-150113.92000000001,1.2364759426346732,66313.85098523942,5404.5963003791785,-153203.04713467252,1.479753990198486,null,356]
["IC/ICD","IC33-200A7",3765,25.9,7500,57.3,"NA",0.89,11.4,84.145706961199153,35.700000000000003,330,32,4.6585858525231369,2.7011020155590098,3.9088617034447197,null,0.14005602240896359,0.21895664609333332,0.2841402666666667,0.22157872001872544,1278.6312,0,-2131.0520000000001,0,0,0,0,0,0.23629071390905554,0.30541305223550247,5.6709771338173329,14.659826507304118,9.332735414028182,983.56246153846166,156.53882759347835,1356.6698391434791,19418.3643227231,3716.2696952782326,-151713.47949324999,2.7011020155590098,9601.2528930815988,1679.7798448116271,-153265.48854925,3.9088617034447197,7407.8019956870039,605.28729132989338,-153612.25609702061,4.5130687636226563,null,119]
["IC/ICD","IC33-250A1",4496,5,9375,11.1,"NA",29,384,523.96612485923163,44.1,330,32,0.74813996821896533,0.23007917140456505,0.52134646164778953,null,0.11337868480725623,0.22119937368178072,0.27422677333333334,1.4612874330403494,1542.5256000000002,0,-2570.8760000000002,0,0,0,0,0,4.6083202850370986E-2,5.9563964264531442E-2,1.1059968684089037,2.8590702846975091,1.8201406738270443,1186.5581538461538,188.84659545060902,1636.6704939052781,799867.16996755078,146067.91110440285,-75949.292499999996,0.23007917140456505,381132.22753176495,65796.356353334617,-137895.25,0.52134646164778953,288665.6608388279,23951.724877664565,-151574.38071025829,0.68432806399997814,null,741]
["IC/ICD","IC33-250A3",4496,14.9,9375,33.1,"NA",3.2,42.6,174.65537495307723,44.1,330,32,2.2444199046568958,1.1969668321836093,1.8150258666066448,null,0.11337868480725623,0.22119937368178072,0.27422677333333334,0.46565565618948979,1542.5256000000002,0,-2570.8760000000002,0,0,0,0,0,0.13732794449410554,0.17750061350830371,3.2958706678585328,8.5200294483985779,5.4240192080045917,1186.5581538461538,188.84659545060902,1636.6704939052781,87995.018991409146,16021.034632057943,-145249.71520000001,1.1969668321836093,42154.147339183415,7211.8856802919436,-151958.9632,1.8150258666066448,32048.270292423043,2625.3292923380377,-153438.05452004759,2.1475096172633386,null,247]
["IC/ICD","IC33-250A5",4496,8.6,9375,19.100000000000001,"NA",9.6999999999999993,128,302.64170234784234,44.1,330,32,1.2952610197435823,0.60975719967859188,0.99982168027979501,null,0.11337868480725623,0.22119937368178072,0.27422677333333334,0.8196003530240864,1542.5256000000002,0,-2570.8760000000002,0,0,0,0,{"$f":"(Ltorque2+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},7.9263108902638088E-2,0.10245001853499408,1.902314613663314,4.9176008896797159,3.1306419589825158,1186.5581538461538,188.84659545060902,1636.6704939052781,264417.45831494767,48558.415217062015,-127920.27032499999,0.60975719967859188,126629.88519221931,21863.998474698077,-148444.82769999999,0.99982168027979501,96235.09731395432,7959.1105832580843,-152972.37364315082,1.2201068439151979,null,428]
["IC/ICD","IC33-250A7",4496,25.7,9375,57.3,"NA",1.1000000000000001,14.2,101.11626970967629,44.1,330,32,3.8767252898619113,2.1731497592363898,3.2108992355888724,null,0.11337868480725623,0.22119937368178072,0.27422677333333334,0.26732693247376033,1542.5256000000002,0,-2570.8760000000002,0,0,0,0,0,0.23686766265090686,0.30615877631969163,5.6848239036217647,14.695621263345197,9.3555230634710078,1186.5581538461538,188.84659545060902,1636.6704939052781,29367.366743874154,5519.4903509325477,-150684.41432499999,2.1731497592363898,14075.415409744932,2475.5829322681757,-153064.60532500001,3.2108992355888724,10734.809766047823,901.18183729066561,-153584.57032579955,3.7407379449063023,null,143]
["IC/ICD","IC44-015A1",286,3.8,750,11.1,"NA",5.8,36.5,43.628488399209978,6.4,330,32,8.9849548857415442,4.5788543886156656,7.7271261584494608,null,0.78125,0.80736054423222625,0.79587200000000002,0.14333889460105909,358.14240000000001,0,-596.904,0,0,0,0,0,0.12783208617010247,0.18107036637931037,3.0679700680824595,8.6913775862068974,5.2788932905575017,275.49415384615384,43.846256377534473,380.00088860529877,6649.7181666684946,2432.4939582028765,-150555.4117,4.5788543886156656,2459.7000485081817,832.74567938476855,-153299.67879999999,7.7271261584494608,2976.9214927540506,1156.8356788539481,-152960.92279636685,6.9764735020679538,null,61.7]
["IC/ICD","IC44-015A2",286,7.6,750,22.1,"NA",1.5,9.1,21.849599538664314,6.4,330,32,17.940832247581014,9.4450285057190708,15.618661728244939,null,0.78125,0.80736054423222625,0.79587200000000002,7.0572643241101365E-2,358.14240000000001,0,-596.904,0,0,0,0,0,0.25566417234020494,0.36074479166666668,6.1359401361649191,17.315750000000001,10.537527768915586,275.49415384615384,43.846256377534473,380.00088860529877,1646.8730880973844,627.27451891845169,-152839.80812500001,9.4450285057190708,615.70781273623561,215.71431419820053,-153566.53,15.618661728244939,743.28231988534526,299.09152316001581,-153476.62085812638,14.169796596446623,null,30.9]
["IC/ICD","IC44-015A3",286,15.1,750,44.1,"NA",0.36,2.2999999999999998,10.889444430272832,6.4,330,32,35.998163405860602,19.027148818377885,31.475294342189546,null,0.78125,0.80736054423222625,0.79587200000000002,3.5016973996841345E-2,358.14240000000001,0,-596.904,0,0,0,0,0,0.50796434241277566,0.71940625000000002,12.191144217906617,34.531500000000001,20.975055537831174,275.49415384615384,43.846256377534473,380.00088860529877,416.05734342864724,149.71918175223905,-153474.96446799999,19.027148818377885,153.45631649115637,51.264391030812007,-153641.837428,31.475294342189546,185.87502431187636,71.210162184395784,-153621.23657279197,28.557578964139037,null,15.4]
["IC/ICD","IC44-015A7",286,26.2,750,76.400000000000006,"NA",0.12,0.8,6.293250352560273,6.4,330,32,62.288956904522841,32.088133713894919,54.0355294716339,null,0.78125,0.80736054423222625,0.79587200000000002,2.0499981780046094E-2,358.14240000000001,0,-596.904,0,0,0,0,0,0.88136859412018032,1.2465957614942529,21.152846258884328,59.836596551724142,36.369923724107757,275.49415384615384,43.846256377534473,380.00088860529877,147.62091144684229,49.96665136508549,-153600.96083200001,32.088133713894919,52.307921084532083,17.135160546665443,-153656.58644799999,54.0355294716339,64.083556164402012,23.78643061383827,-153649.71406940167,48.780531159952645,null,8.9]
["IC/ICD","IC44-030A1",597,3.9,1500,11.1,"NA",7.8,66.8,86.974134085945337,9.6,330,32,4.5070871256118155,2.3768235154015978,3.8886096255265334,null,0.52083333333333337,0.49534436634871498,0.50963733333333339,0.24677273351356574,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,8.0493459531666187E-2,0.10906661129568107,1.9318430287599884,5.2351973421926914,3.1792369151584992,352.82584615384616,56.153977465965212,486.66780470503181,23461.673935248509,6521.3622743526512,-148041.9277,2.3768235154015978,9526.9707049357166,2291.2894477455261,-152969.96770000001,3.8886096255265334,8868.626600793019,1867.8338450219765,-153202.7926138397,4.0523115571235806,null,123]
["IC/ICD","IC44-030A2",597,7.9,1500,22.1,"NA",2,16.7,43.628488399209978,9.6,330,32,8.9849548857415442,4.9632282106452354,7.862552957546292,null,0.52083333333333337,0.49534436634871498,0.50963733333333339,0.12232350045647773,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.16305085392311869,0.21944387227759321,3.9132204941548485,10.533305869324474,6.4399927255774738,352.82584615384616,56.153977465965212,486.66780470503181,5842.0146786557134,1670.0253642834289,-152198.76999999999,4.9632282106452354,2406.7232572938779,596.97739266240217,-153476.76999999999,7.862552957546292,2237.8900244719443,486.64937545317429,-153539.57948108352,8.1750440125427613,null,61.7]
["IC/ICD","IC44-030A3",597,15.8,1500,44.1,"NA",0.49,4.2,21.849599538664314,9.6,330,32,17.940832247581014,10.076491537226923,15.817550010468956,null,0.52083333333333337,0.49534436634871498,0.50963733333333339,6.0872759290315985E-2,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.32610170784623738,0.43850140273163535,7.826440988309697,21.048067331118496,12.879985451154948,352.82584615384616,56.153977465965212,486.66780470503181,1469.3710374444872,408.892159255168,-153313.78833924999,10.076491537226923,604.7358968935996,146.49651057214638,-153619.04607700001,15.817550010468956,562.02058652780795,119.42233701355774,-153634.12663340816,16.427709400041707,null,30.9]
["IC/ICD","IC44-030A7",597,27.3,1500,76.400000000000006,"NA",0.16,1.4,12.586500705120546,9.6,330,32,31.144478452261421,17.580768096901334,27.55343280763655,null,0.52083333333333337,0.49534436634871498,0.50963733333333339,3.496454176000869E-2,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.56345421672166329,0.75844383536360294,13.52290120131992,36.405304097452941,22.254658406109495,352.82584615384616,56.153977465965212,486.66780470503181,489.21872880595447,133.244403640228,-153551.930368,17.580768096901334,200.65790887581716,47.612201824322305,-153649.690432,27.55343280763655,186.48848550059199,38.81294093637495,-153654.49081944115,28.600403427673907,null,17.8]
["IC/ICD","IC44-050A1",1096,4.4000000000000004,2500,11.1,"NA",10.6,107,145.66399692442877,13.9,330,32,2.6911248371371519,1.4051341488632638,2.2417872794176144,null,0.35971223021582732,0.34928501454994842,0.39584159999999996,0.40157896840208684,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,6.4035586000823888E-2,8.2767974452554752E-2,1.5368540640197732,3.9728627737226279,2.5292029946549368,456.74030769230768,72.692477678543995,630.00147321404791,62006.2015276319,14842.658601497238,-143281.09330000001,1.4051341488632638,27627.05431032346,5883.5763825754821,-152032.53279999999,2.2417872794176144,23335.658732972614,3381.9906832024931,-153124.9359514908,2.4901702496499651,null,206]
["IC/ICD","IC44-050A2",1096,8.6999999999999993,2500,22.1,"NA",2.7,26.7,72.831998462214386,13.9,330,32,5.3822496742743038,3.0140659706382329,4.6181826393654779,null,0.35971223021582732,0.34928501454994842,0.39584159999999996,0.19749495979512866,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.12661581777435629,0.1636548585766423,3.0387796265845513,7.8554332116788306,5.0009241030677156,456.74030769230768,72.692477678543995,630.00147321404791,15372.150106554091,3763.6471135107104,-150993.61832499999,3.0140659706382329,6864.7064588462126,1481.6167369929037,-153250.16492499999,4.6181826393654779,5820.0183078249202,851.6612473030292,-153527.26196999571,5.0634203578529284,null,103]
["IC/ICD","IC44-050A3",1096,17.399999999999999,2500,44.1,"NA",0.66,6.7,36.345288552988542,13.9,330,32,10.785441954285083,6.1904136296835999,9.3606929521941957,null,0.35971223021582732,0.34928501454994842,0.39584159999999996,9.7856568813926445E-2,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.25323163554871259,0.32730971715328461,6.0775592531691025,15.710866423357661,10.001848206135431,456.74030769230768,72.692477678543995,630.00147321404791,3845.319876467292,916.13880262679629,-153028.630573,6.1904136296835999,1713.9588210669615,361.4697316486679,-153565.08830800001,9.3606929521941957,1450.8267748923997,207.77961994611982,-153631.31792270514,10.219038048447139,null,51.4]
["IC/ICD","IC44-050A7",1096,30.2,2500,76.400000000000006,"NA",0.22,2.2000000000000002,21.001071401240459,13.9,330,32,18.665714358594389,10.924033162916665,16.330402426886277,null,0.35971223021582732,0.34928501454994842,0.39584159999999996,5.6305615357956161E-2,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.43951697664201844,0.56808927919708019,10.548407439408443,27.268285401459849,17.359529645131612,456.74030769230768,72.692477678543995,630.00147321404791,1257.9153303167445,305.69485020549496,-153452.11835199999,10.924033162916665,568.68308833058359,120.83749314405689,-153630.89294799999,16.330402426886277,483.21875907983974,69.459670346941834,-153653.06087631715,17.76021793994472,null,29.7]
["IC/ICD","IC44-075A1",1732,4.5999999999999996,3750,11.1,"NA",14.1,158,217.78888860545663,19.2,330,32,{"$f":"IF(G247=\"NA\",(UAC_V*0.98)/J247,(IF((UAC_V*0.98)/J247<G247,(UAC_V*0.98)/J247,G247)))","v":1.7999081702930302},{"$f":"IF(AO247<G247,IF(AO247<0,0,AO247),G247)","v":0.89367532130654148},{"$f":"IF(AS247<G247,IF(AS247<0,0,AS247),G247)","v":1.4547915688832074},null,{"$f":"IF(move1,Gewicht/K247,MAX(Gewicht,Gewicht2)/K247)","v":0.26041666666666669},{"$f":"IF(move1,IF(AccType=1,SQRT((V247^2*Ltime1+W247^2*Ltime2+X247^2*Ltime3+Y247^2*Ltime4)/ltime)/C247,SQRT((((V247-W247)*2/PI()+W247)^2*Ltime1+W247^2*Ltime2+((X247-W247)*2/PI()+W247)^2*Ltime3+Y247^2*Ltime4)/ltime)/C247),IF(AccType=1,SQRT((V247^2*Ltime1+W247^2*Ltime2+X247^2*Ltime3+Y247^2*Ltime4+Z247^2*Ltime5+AA247^2*Ltime6+AB247^2*Ltime7+AC247^2*Ltime8)/ltime)/C247,SQRT((((V247-W247)*2/PI()+W247)^2*Ltime1+W247^2*Ltime2+((X247-W247)*2/PI()+W247)^2*Ltime3+Y247^2*Ltime4+((Z247-AA247)*2/PI()+AA247)^2*Ltime5+AA247^2*Ltime6+((AB247-AA247)*2/PI()+AA247)^2*Ltime7+AC247^2*Ltime8)/ltime)/C247))","v":0.28300635097545096},{"$f":" IF(move1,MAX(ABS(V247),ABS(X247))/E247,MAX(ABS(V247),ABS(X247),ABS(Z247),ABS(AB247))/E247)","v":0.3378965333333333},{"$f":"IF(AW247>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW247,G247),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW247,G247)),\"NA\")","v":0.59486752123969866},{"$f":"((Gewicht+K247)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":760.2672},0,{"$f":"((Gewicht+K247)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-1267.1119999999999},0,{"$f":"((Gewicht2+K247)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K247)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"AF247/Irms","v":5.4242883936961424E-2},{"$f":"AG247/Ipeak","v":7.0110604311008448E-2},{"$f":"D247*S247","v":1.3018292144870742},{"$f":"IF(move1,IF(MAX(ABS(V247),ABS(X247))<=C247,MAX(ABS(V247),ABS(X247))/C247*D247,D247+(MAX(ABS(V247),ABS(X247))-C247)/(E247-C247)*(F247-D247)),IF(MAX(ABS(V247),ABS(X247),ABS(Z247),ABS(AB247))<=C247,MAX(ABS(V247),ABS(X247),ABS(Z247),ABS(AB247))/C247*D247,D247+(MAX(ABS(V247),ABS(X247),ABS(Z247),ABS(AB247))-C247)/(E247-C247)*(F247-D247)))","v":3.3653090069284057},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V247),ABS(X247))<=C247,MAX(ABS(V247),ABS(X247))/C247*D247,D247+(MAX(ABS(V247),ABS(X247))-C247)/(E247-C247)*(F247-D247)),IF(MAX(ABS(V247),ABS(X247),ABS(Z247),ABS(AB247))<=C247,MAX(ABS(V247),ABS(X247),ABS(Z247),ABS(AB247))/C247*D247,D247+(MAX(ABS(V247),ABS(X247),ABS(Z247),ABS(AB247))-C247)/(E247-C247)*(F247-D247))),IF(move1,IF(MAX(ABS((V247-W247)*2/PI()+W247),ABS((X247-W247)*2/PI()+W247))<=C247,MAX(ABS((V247-W247)*2/PI()+W247),ABS((X247-W247)*2/PI()+W247))/C247*D247,D247+(MAX(ABS((V247-W247)*2/PI()+W247),ABS((X247-W247)*2/PI()+W247))-C247)/(E247-C247)*(F247-D247)),IF(MAX(ABS((V247-W247)*2/PI()+W247),ABS((X247-W247)*2/PI()+W247),ABS((Z247-AA247)*2/PI()+AA247),ABS((AB247-AA247)*2/PI()+AA247))<=C247,MAX(ABS((V247-W247)*2/PI()+W247),ABS((X247-W247)*2/PI()+W247),ABS((Z247-AA247)*2/PI()+AA247),ABS((AB247-AA247)*2/PI()+AA247))/C247*D247,D247+(MAX(ABS((V247-W247)*2/PI()+W247),ABS((X247-W247)*2/PI()+W247),ABS((Z247-AA247)*2/PI()+AA247),ABS((AB247-AA247)*2/PI()+AA247))-C247)/(E247-C247)*(F247-D247))))","v":2.1424222539373332},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V247)+Ltime2*ABS(Lspeed2)*ABS(W247)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X247)+Ltime4*ABS(Lspeed1)*ABS(Y247))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V247)+Ltime2*ABS(Lspeed2)*ABS(W247)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X247)+Ltime4*ABS(Lspeed1)*ABS(Y247)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z247)+Ltime6*ABS(Lspeed6)*ABS(AA247)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB247)+Ltime8*ABS(Lspeed1)*ABS(AC247))/ltime)","v":584.82092307692312},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK247/2*Ltime1/ltime,AK247/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X247*-ABS(Lspeed2-Lspeed1),((X247-Y247)*2/PI()+Y247)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V247*-ABS(Lspeed2-Lspeed1),((V247-W247)*2/PI()+W247)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X247*-ABS(Lspeed2-Lspeed1),((X247-Y247)*2/PI()+Y247)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V247*-ABS(Lspeed2-Lspeed1),((V247-W247)*2/PI()+W247)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB247*-ABS(Lspeed6-Lspeed1),((AB247-AC247)*2/PI()+AB247)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z247*-ABS(Lspeed6-Lspeed1),((Z247-AA247)*2/PI()+AA247)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB247*-ABS(Lspeed6-Lspeed1),((AB247-AC247)*2/PI()+AB247)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z247*-ABS(Lspeed6-Lspeed1),((Z247-AA247)*2/PI()+AA247)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":93.077140731257387},{"$f":"IF(move1,MAX(IF(AccType=1,X247*-ABS(Lspeed2-Lspeed1),((X247-Y247)*2/PI()+Y247)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V247*-ABS(Lspeed2-Lspeed1),((V247-W247)*2/PI()+W247)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X247*-ABS(Lspeed2-Lspeed1),((X247-Y247)*2/PI()+Y247)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V247*-ABS(Lspeed2-Lspeed1),((V247-W247)*2/PI()+W247)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB247*-ABS(Lspeed6-Lspeed1),((AB247-AC247)*2/PI()+AB247)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z247*-ABS(Lspeed6-Lspeed1),((Z247-AA247)*2/PI()+AA247)*-ABS(Lspeed6-Lspeed1)),0))","v":806.66855300423072},{"$f":"(J247^2)+3*(I247/1000)^2*(F247/2)^2*(2000*PI()/M247)^2","v":136368.73359558065},{"$f":"SQRT(3)*H247*F247/2*J247","v":29519.462252510628},{"$f":"3*F247^2*H247^2/4-(UAC_V*0.98)^2","v":-135292.46492500001},{"$f":"-AM247/2/AL247+SQRT((AM247/2/AL247)^2-AN247/AL247)","v":0.89367532130654148},{"$f":"(J247^2)+3*(I247/1000)^2*(D247/2)^2*(2000*PI()/M247)^2","v":62705.932983381921},{"$f":"SQRT(3)*H247*D247/2*J247","v":12233.290663202602},{"$f":"3*D247^2*H247^2/4-(UAC_V*0.98)^2","v":-150508.88529999999},{"$f":"-AQ247/2/AP247+SQRT((AQ247/2/AP247)^2-AR247/AP247)","v":1.4547915688832074},{"$f":"(J247^2)+3*(I247/1000)^2*(AH247/2)^2*(2000*PI()/M247)^2","v":50745.182501951567},{"$f":"SQRT(3)*H247*AH247/2*J247","v":5697.5813382019687},{"$f":"3*AH247^2*H247^2/4-(UAC_V*0.98)^2","v":-152979.60058387951},{"$f":"IF((AU247/2/AT247)^2-AV247/AT247>=0,-AU247/2/AT247+SQRT((AU247/2/AT247)^2-AV247/AT247),-9999)","v":1.6810465596037398},null,308]
["IC/ICD","IC44-075A2",1732,9.1999999999999993,3750,22.1,"NA",305,39.4,108.89444430272832,19.2,330,32,3.5998163405860604,{"$error":"#NUM!"},{"$error":"#NUM!"},null,0.26041666666666669,0.28300635097545096,0.3378965333333333,"NA",760.2672,0,-1267.1119999999999,0,0,0,0,0,0.10848576787392285,0.1402212086220169,2.6036584289741485,6.7306180138568115,4.2848445078746664,584.82092307692312,93.077140731257387,806.66855300423072,33780.901596894764,635665.24603235547,33922091.187500007,{"$error":"#NUM!"},15657.173626996115,264620.82640260947,5751562.9999999991,{"$error":"#NUM!"},12682.107032323271,123245.55376961704,1127282.7468358551,-9999,null,154]
["IC/ICD","IC44-075A3",1732,18.3,3750,44.1,"NA",0.88,9.9,54.51793282948281,19.2,330,32,7.1902946361900559,4.1336378311692323,6.1598185619114227,null,0.26041666666666669,0.28300635097545096,0.3378965333333333,0.1449891747001302,760.2672,0,-1267.1119999999999,0,0,0,0,0,0.21579234261878136,0.27891827367205541,5.1790162228507528,13.388077136258659,8.523114618924609,584.82092307692312,93.077140731257387,806.66855300423072,8483.6897692706461,1832.2776052535924,-152534.454352,4.1336378311692323,3921.2648744252888,760.33288381271529,-153469.495888,6.1598185619114227,3178.0726421240906,354.12045449580648,-153621.8086651855,6.8970666401006975,null,77.099999999999994]
["IC/ICD","IC44-075A7",1732,31.8,3750,76.400000000000006,"NA",0.28999999999999998,3.3,31.466251762801363,19.2,330,32,12.457791380904569,7.2564239000653856,10.73871067858094,null,0.26041666666666669,0.28300635097545096,0.3378965333333333,8.3409203455829223E-2,760.2672,0,-1267.1119999999999,0,0,0,0,0,0.37498341504247251,0.48467765588914546,8.9996019610193407,23.264527482678982,14.810658190262435,584.82092307692312,93.077140731257387,806.66855300423072,2828.0832432126754,603.76370399478299,-153295.833748,7.2564239000653856,1308.5470713978484,251.30478778840444,-153600.21603700001,10.73871067858094,1059.1963018276533,117.04368910410363,-153650.16414578049,11.989084640156852,null,44.5]
["IC/ICD","IC44-100A1",2397,4.8,5000,11.1,"NA",17.600000000000001,208,290.62088706767099,25,330,32,1.3488362930663098,0.62818462642799278,1.0542039158844327,null,0.2,0.25350231171685739,0.31415999999999999,0.79499249920414683,942.48,0,-1570.8,0,0,0,0,0,5.0700462343371472E-2,6.553191489361701E-2,1.2168110962409153,3.1455319148936165,2.0025078116345365,724.98461538461538,115.38488520403808,1000.0023384349968,238592.8042092293,49169.195484424999,-125039.85279999999,0.62818462642799278,113282.90312458924,21262.354804075672,-148311.34719999999,1.0542039158844327,89476.946111000419,8870.4232476888865,-152732.3880797161,1.2578735032105115,null,411]
["IC/ICD","IC44-100A2",2397,9.5,5000,22.1,"NA",4.4000000000000004,52.1,145.66399692442877,25,330,32,2.6911248371371519,1.4692253712432457,2.2288936627328146,null,0.2,0.25350231171685739,0.31415999999999999,0.38975463711064312,942.48,0,-1570.8,0,0,0,0,0,0.10034466505458939,0.12969858156028366,2.4082719613101453,6.2255319148936161,3.9632967105266874,724.98461538461538,115.38488520403808,1000.0023384349968,59551.726277169684,12266.701703294166,-146572.2868,1.4692253712432457,28301.431536034401,5273.016569289347,-152353.57,2.2288936627328146,22450.848365484238,2199.845181433388,-153435.92389375644,2.5657167478834153,null,206]
["IC/ICD","IC44-100A3",2397,19,5000,44.1,"NA",1.1000000000000001,13,72.831998462214386,25,330,32,5.3822496742743038,3.101145958669385,4.5652295140080774,null,0.2,0.25350231171685739,0.31415999999999999,0.19293131771191344,942.48,0,-1570.8,0,0,0,0,0,0.20068933010917878,0.25939716312056732,4.8165439226202906,12.451063829787232,7.9265934210533748,724.98461538461538,115.38488520403808,1000.0023384349968,14808.029497058862,3059.7372461271079,-151899.084925,3.101145958669385,7068.5664889825985,1318.2541423223367,-153336.39249999999,4.5652295140080774,5611.5300710162965,549.961295358347,-153606.98097343912,5.1831916759787431,null,103]
["IC/ICD","IC44-100A7",2397,33,5000,76.400000000000006,"NA",0.37,4.3,41.93143212436226,25,330,32,9.3485955556535139,5.496934262615004,8.0056831954393441,null,0.2,0.25350231171685739,0.31415999999999999,0.11061779104770761,942.48,0,-1570.8,0,0,0,0,0,0.34856567861067894,0.45053191489361694,8.3655762866562942,21.625531914893614,13.767241204987441,724.98461538461538,115.38488520403808,1000.0023384349968,4878.8921916439267,1026.515259926349,-153064.69013199999,5.496934262615004,2340.4632765857968,443.390099182847,-153552.18692499999,8.0056831954393441,1859.578209333974,184.97752858647152,-153644.53929567157,9.0401371291957613,null,59.3]
["IC/ICD","IC44-150A1",3617,4.8,7500,11.1,"NA",24.7,309,436.28488399209976,36.200000000000003,330,32,0.89849548857415451,0.34159054896000435,0.66768141053363539,null,0.13812154696132595,0.23071583906400014,0.28763093333333334,1.2024026517813893,1294.3392000000001,0,-2157.232,0,0,0,0,0,4.6143167812800027E-2,5.9641470832181361E-2,1.1074360275072006,2.8627905999447054,1.8225091000728499,995.64553846153854,158.46190901354564,1373.3365447840622,530505.06162632722,103590.69097863973,-97287.108325000008,0.34159054896000435,253953.7796028778,44795.97447724962,-143121.64480000001,0.66768141053363539,199514.67055855526,17008.556485712197,-152144.17151150855,0.83166815917985148,null,617]
["IC/ICD","IC44-150A2",3617,9.6,7500,22.1,"NA",6.2,77.400000000000006,217.78888860545663,36.200000000000003,330,32,1.7999081702930302,0.93496673829962129,1.4573579906712908,null,0.13812154696132595,0.23071583906400014,0.28763093333333334,0.58368707458639335,1294.3392000000001,0,-2157.232,0,0,0,0,0,9.2286335625600055E-2,0.11928294166436272,2.2148720550144012,5.7255811998894108,3.6450182001456999,995.64553846153854,158.46190901354564,1373.3365447840622,132035.34070100577,25843.439510823631,-139583.1397,0.93496673829962129,63396.136440704926,11226.109470765015,-151007.02720000001,1.4573579906712908,49733.45436161627,4262.43472268401,-153280.96007410309,1.7132467781792329,null,308]
["IC/ICD","IC44-150A3",3617,19.2,7500,44.1,"NA",1.5,19.3,108.89444430272832,36.200000000000003,330,32,3.5998163405860604,2.0480979502614476,3.0248574479160153,null,0.13812154696132595,0.23071583906400014,0.28763093333333334,0.28787782879381851,1294.3392000000001,0,-2157.232,0,0,0,0,0,0.18457267125120011,0.23856588332872544,4.4297441100288024,11.451162399778822,7.2900364002913998,995.64553846153854,158.46190901354564,1373.3365447840622,32804.566286150628,6238.2992396766285,-150382.13312499999,2.0480979502614476,15828.435258830717,2715.9942267979877,-153041.92000000001,3.0248574479160153,12430.393976829948,1031.2342071009703,-153574.31843566408,3.4736957833463853,null,154]
["IC/ICD","IC44-150A7",3617,33.200000000000003,7500,76.400000000000006,"NA",0.51,6.4,62.932503525602726,36.200000000000003,330,32,6.2288956904522843,3.6489180099099641,5.3112285921139897,null,0.13812154696132595,0.23071583906400014,0.28763093333333334,0.16547305980192675,1294.3392000000001,0,-2157.232,0,0,0,0,0,0.31915691070520019,0.41252017325592116,7.659765856924805,19.800968316284216,12.605687942170547,995.64553846153854,158.46190901354564,1373.3365447840622,10873.518332597905,2123.5826830161336,-152525.35502799999,3.6489180099099641,5265.9407306068078,922.81341722690615,-153448.98053199999,5.3112285921139897,4148.6976062059957,350.38246886778336,-153633.00192539077,6.0432798015399731,null,89]
["IC/ICD","IC44-200A1",5025,5,10000,11.1,"NA",31.8,410,581.94888091652854,47.4,330,32,0.67359868341464557,0.17573806907647824,0.46092881454961954,null,0.10548523206751055,0.21121459474699894,0.27436639999999995,1.6226052188833782,1646.1984,0,-2743.6639999999998,0,0,0,0,0,4.4003040572291451E-2,5.6875290215588716E-2,1.0560729737349948,2.7300139303482585,1.7379808468986344,1266.3064615384615,201.53893282305319,1746.6707511331276,937537.47377892572,177895.74799561495,-60217.839699999997,0.17573806907647824,460179.18504563865,80133.219817844569,-134703.25,0.46092881454961954,353346.28057423944,27854.00024874639,-151373.10346417423,0.61629285322289673,null,823]
["IC/ICD","IC44-200A2",5025,10,10000,22.1,"NA",8,103,290.62088706767099,47.4,330,32,1.3488362930663098,0.65659323618432786,1.0529920629462446,null,0.10548523206751055,0.21121459474699894,0.27436639999999995,0.78210892485194017,1646.1984,0,-2743.6639999999998,0,0,0,0,0,8.8006081144582901E-2,0.11375058043117743,2.1121459474699895,5.4600278606965169,3.4759616937972688,1266.3064615384615,201.53893282305319,1746.6707511331276,234284.03516030853,44497.920565347762,-130220.31999999999,0.65659323618432786,115136.27141342487,20134.805685677718,-148864,1.0529920629462446,88166.841704035833,6998.7813275467206,-153084.0491345562,1.2785942830013204,null,411]
["IC/ICD","IC44-200A3",5025,20,10000,44.1,"NA",2,25.7,145.66399692442877,47.4,330,32,2.6911248371371519,1.4990881218459362,2.2127967041300014,null,0.10548523206751055,0.21121459474699894,0.27436639999999995,0.38552264266931396,1646.1984,0,-2743.6639999999998,0,0,0,0,0,0.1760121622891658,0.22750116086235486,4.224291894939979,10.920055721393034,6.9519233875945377,1266.3064615384615,201.53893282305319,1746.6707511331276,58359.93016279531,11126.317258644029,-147829.57,1.4990881218459362,28857.189465869735,5045.9488701333457,-152464,2.2127967041300014,22140.990529587572,1753.9524981443119,-153519.01228363905,2.5938813686172004,null,206]
["IC/ICD","IC44-200A7",5025,34.6,10000,76.400000000000006,"NA",0.66,8.6,84.145706961199153,47.4,330,32,4.6585858525231369,2.692864345443557,3.9019268877641347,null,0.10548523206751055,0.21121459474699894,0.27436639999999995,0.22122074731186669,1646.1984,0,-2743.6639999999998,0,0,0,0,0,0.3045010407602568,0.39357700829187392,7.3080249782461637,18.891696398009948,12.02682746053855,1266.3064615384615,201.53893282305319,1746.6707511331276,19563.088766575711,3674.5138560054443,-151757.065168,2.692864345443557,9640.6778953074499,1664.1122960443504,-153272.88782800001,3.9019268877641347,7389.8286220986793,578.43905952271825,-153616.7446161173,4.5203716746795299,null,119]
["IC/ICD","IC44-250A1",6029,5,12500,11.1,"NA",38.6,512,698.62149981230891,58.5,330,32,0.56110497616422395,4.8658709214415966E-2,0.35312844138117261,null,8.5470085470085472E-2,0.21333255993402445,0.26598880000000003,1.9866245296877676,1994.9159999999999,0,-3324.86,0,0,0,0,0,4.4444283319588419E-2,5.7445610106706478E-2,1.0666627996701221,2.7573892851219108,1.7554085390231189,1534.5507692307692,244.23134034854732,2116.6716163540768,1421986.0799423126,259228.56867264147,-15980.521299999993,4.8658709214415966E-2,677568.40450091567,116769.62552821689,-125727.25,0.35312844138117261,511429.01709733409,40995.679550152781,-150220.56185608104,0.50336638104290765,null,988]
["IC/ICD","IC44-250A2",6029,10,12500,22.1,"NA",9.6999999999999993,128,349.31074990615446,58.5,330,32,1.1222099523284479,0.49621962470217812,0.84772609936423493,null,8.5470085470085472E-2,0.21333255993402445,0.26598880000000003,0.94909748452897558,1994.9159999999999,0,-3324.86,0,0,0,0,0,8.8888566639176839E-2,0.11489122021341296,2.1333255993402442,5.5147785702438217,3.5108170780462378,1534.5507692307692,244.23134034854732,2116.6716163540768,353397.84730573057,64849.493845813078,-119198.12732500001,0.49621962470217812,169392.10112522892,29343.662373671075,-146607.25,0.84772609936423493,127857.25427433352,10302.023099390723,-152794.19652886968,1.0536325470257533,null,494]
["IC/ICD","IC44-250A3",6029,19.899999999999999,12500,44.1,"NA",2.4,32,174.65537495307723,58.5,330,32,2.2444199046568958,1.1964993311130157,1.8132982209617667,null,8.5470085470085472E-2,0.21333255993402445,0.26598880000000003,0.46463377825340163,1994.9159999999999,0,-3324.86,0,0,0,0,0,0.1768882476119619,0.22863352822469174,4.2453179426870857,10.974409354785204,6.9865259853120127,1534.5507692307692,244.23134034854732,2116.6716163540768,88088.016005847778,16008.934152728592,-145262.42079999999,1.1964993311130157,42229.886116626185,7223.9861596212913,-151953.23680000001,1.8132982209617667,31949.751928236761,2536.2093980768086,-153453.13412411633,2.1522326761499908,null,247]
["IC/ICD","IC44-250A7",6029,34.5,12500,76.400000000000006,"NA",0.8,10.7,101.11626970967629,58.5,330,32,3.8767252898619113,2.1708347305914133,3.2033424318012695,null,8.5470085470085472E-2,0.21333255993402445,0.26598880000000003,0.26684223342155827,1994.9159999999999,0,-3324.86,0,0,0,0,0,0.30666555490516018,0.39637470973627464,7.3599733177238438,19.025986067341183,12.11231891925952,1534.5507692307692,244.23134034854732,2116.6716163540768,29547.533908670266,5352.2330675709554,-150862.2592,2.1708347305914133,14164.777320693438,2416.911529204162,-153092.68,3.2033424318012695,10710.172142382151,848.53342728568191,-153593.58003059111,3.7475327169076587,null,143]
["IC/ICD","IC55-015A1",359,3.8,940,11.1,"NA",7.2,45.6,54.588643507601468,8,330,32,7.1809807830343688,3.6082062582777872,6.1418197077005141,null,0.625,0.73346198100362037,0.72412765957446801,0.17364596730493598,408.40800000000002,0,-680.68,0,0,0,0,0,0.11613148032557323,0.16337005163511184,2.7871555278137574,7.8417624784853688,4.7339771610717829,314.16000000000003,50.000116921749836,433.33434665516523,10387.846869464291,3778.2301506943695,-148873.59520000001,3.6082062582777872,3848.1162827291973,1293.4481596971714,-153102.57279999999,6.1418197077005141,4327.340174164261,1611.3563281675627,-152792.67821407097,5.7588437872785221,null,77.2]
["IC/ICD","IC55-015A3",359,19,940,55.5,"NA",0.28999999999999998,1.8,10.889444430272832,8,330,32,35.998163405860602,19.229336653556096,31.581272786107313,null,0.625,0.73346198100362037,0.72412765957446801,3.3580717939800636E-2,408.40800000000002,0,-680.68,0,0,0,0,0,0.58065740162786617,0.81685025817555934,13.935777639068787,39.20881239242685,23.669885805358916,314.16000000000003,50.000116921749836,433.33434665516523,407.15055845385484,151.78446902886671,-153469.71323125,19.229336653556096,152.39997292487351,51.962250658530941,-153641.22992499999,31.581272786107313,171.06780110577543,64.733712593519144,-153628.66138011351,29.778994058217474,null,15.4]
["IC/ICD","IC55-015A5",359,6.6,940,19.2,"NA",2.4,15.2,31.466251762801363,8,330,32,12.457791380904569,6.4571191945231998,10.778036228189599,null,0.625,0.73346198100362037,0.72412765957446801,9.8684709279939942E-2,408.40800000000002,0,-680.68,0,0,0,0,0,0.2017020447759956,0.28283734939759031,4.8408490746238941,13.576192771084335,8.2120701684252708,314.16000000000003,50.000116921749836,433.33434665516523,3452.8202728939,1255.7064217403681,-152071.47519999999,6.4571191945231998,1281.1270781446892,431.64908247325155,-153475.82079999999,10.778036228189599,1440.6444263866806,537.08068991011032,-153372.66742333106,10.13328211935336,null,44.5]
["IC/ICD","IC55-015A7",359,32.9,940,96.1,"NA",0.1,0.6,6.293250352560273,8,330,32,62.288956904522841,33.446246829658989,54.782489465349528,null,0.625,0.73346198100362037,0.72412765957446801,1.9348786205600134E-2,408.40800000000002,0,-680.68,0,0,0,0,0,1.0054541322924628,1.4144103557085483,24.13089917501911,67.891697074010324,40.985939257498181,314.16000000000003,50.000116921749836,433.33434665516523,135.7375183611945,52.375602052625602,-153594.73592499999,33.446246829658989,50.872182792740013,17.93087728960856,-153655.88192499999,54.782489465349528,57.091114924824211,22.3378069126307,-153651.40114587385,51.68282854407525,null,8.9]
["IC/ICD","IC55-030A1",748,4,1875,11.1,"NA",9.6999999999999993,83.5,108.89444430272832,12,330,32,3.5998163405860604,1.8540259327568245,3.0610542680041988,null,0.41666666666666669,0.46033715241311146,0.47473066666666669,0.30851694066206281,534.072,0,-890.12,0,0,0,0,0,7.6722858735518581E-2,0.10198632061520259,1.8413486096524458,4.8953433895297245,3.0303101164696873,410.82461538461536,65.384768282288249,566.66799177983148,36697.3342738258,10153.857583310391,-144969.378325,1.8540259327568245,15083.625747757591,3659.047777769511,-152534.92000000001,3.0610542680041988,13709.263104687501,2772.0123744052189,-153015.99421455088,3.2413130956570719,null,154]
["IC/ICD","IC55-030A3",748,19.8,1875,55.5,"NA",0.39,3.3,21.849599538664314,12,330,32,17.940832247581014,10.151632853312595,15.86852993258557,null,0.41666666666666669,0.46033715241311146,0.47473066666666669,6.0098015885875204E-2,534.072,0,-890.12,0,0,0,0,0,0.37977815074081694,0.50629037267080745,9.1146756177796071,24.301937888198758,15.000035076524952,410.82461538461536,65.384768282288249,566.66799177983148,1447.3227103587897,409.57336235263608,-153312.62048124999,10.151632853312595,600.8516485412091,146.11806440688639,-153619.27803700001,15.86852993258557,548.25395884171849,110.69576219278929,-153638.33300495922,16.639484436540762,null,30.9]
["IC/ICD","IC55-030A5",748,6.9,1875,19.2,"NA",3.2,27.8,63.003214203721377,12,330,32,6.2219047861981291,3.3804847953368911,5.4003784145263793,null,0.41666666666666669,0.46033715241311146,0.47473066666666669,0.17575973548716967,534.072,0,-890.12,0,0,0,0,0,0.13234693131876954,0.17606433007985803,3.1763263516504692,8.4510878438331858,5.2272849509102111,410.82461538461536,65.384768282288249,566.66799177983148,12207.240070564931,3352.3128742192303,-150832.84479999999,3.3804847953368911,5033.3246172677846,1204.7374391725359,-153298.35519999999,5.4003784145263793,4580.0136966754681,912.68201240358019,-153454.14777888247,5.6895852581264226,null,89.1]
["IC/ICD","IC55-030A7",748,34.299999999999997,1875,96.1,"NA",0.13,1.1000000000000001,12.586500705120546,12,330,32,31.144478452261421,17.716139126168724,27.624765076842461,null,0.41666666666666669,0.46033715241311146,0.47473066666666669,3.454026808453927E-2,534.072,0,-890.12,0,0,0,0,0,0.65789851365707175,0.87694313812481506,15.789564327769721,42.093270629991125,25.984909248727565,410.82461538461536,65.384768282288249,566.66799177983148,481.53207560290377,136.17656533682657,-153546.94371324999,17.716139126168724,199.5818280283892,48.604122695662348,-153649.08798924999,27.624765076842461,182.04374916042966,36.821391176699883,-153655.44164342768,28.951715069276332,null,17.8]
["IC/ICD","IC55-050A1",1374,4.4000000000000004,3125,11.1,"NA",13.2,134,181.7264427649427,17.3,330,32,2.1570883908570169,1.0779535646044278,1.7700122329445187,null,0.28901734104046239,0.32873567245105167,0.37364095999999997,0.50140414381194576,700.57680000000005,0,-1167.6279999999999,0,0,0,0,0,6.0268206616026145E-2,7.7898520135856394E-2,1.4464369587846275,3.7391289665211067,2.3804034315196962,538.90523076923068,85.769431335001642,743.33507157001429,96994.536390091584,23059.275984483982,-137562.9172,1.0779535646044278,43076.11841175369,9140.6139037594166,-151134.03520000001,1.7700122329445187,35966.42621035326,4945.079250614901,-152923.52523747939,1.9943991535400141,null,257]
["IC/ICD","IC55-050A3",1374,21.8,3125,55.5,"NA",0.53,5.3,36.345288552988542,17.3,330,32,10.785441954285083,6.2067352273323486,9.3789233988164273,null,0.28901734104046239,0.32873567245105167,0.37364095999999997,9.7252652278159199E-2,700.57680000000005,0,-1167.6279999999999,0,0,0,0,0,0.29860156914303865,0.38595175885492483,7.1664376594329271,18.525684425036392,11.793817001620313,538.90523076923068,85.769431335001642,743.33507157001429,3822.8154898051803,925.8648690739783,-153015.06833124999,6.2067352273323486,1706.9786358818324,363.67304767230138,-153563.87881299999,9.3789233988164273,1433.9547924705835,196.74740241599369,-153634.69634638113,10.282495917333227,null,51.4]
["IC/ICD","IC55-050A5",1374,7.6,3125,19.2,"NA",4.4000000000000004,44.5,104.65180361560903,17.3,330,32,3.7457548408800898,2.0347348799185787,3.1692305993042607,null,0.28901734104046239,0.32873567245105167,0.37364095999999997,0.28413446316610863,700.57680000000005,0,-1167.6279999999999,0,0,0,0,0,0.1040996296094997,0.13455198932557011,2.4983911106279928,6.4584954876273653,4.111605927170384,538.90523076923068,85.769431335001642,743.33507157001429,32059.826844477771,7656.5170584019461,-148311.34719999999,2.0347348799185787,14259.259327628677,3030.7046689507706,-152825.3248,3.1692305993042607,11919.974758075658,1639.6135895211769,-153418.53499607902,3.5194604303082633,null,148]
["IC/ICD","IC55-050A7",1374,37.799999999999997,3125,96.1,"NA",0.18,1.8,21.001071401240459,17.3,330,32,18.665714358594389,10.718455346311787,16.239768572194528,null,0.28901734104046239,0.32873567245105167,0.37364095999999997,5.6123179552348329E-2,700.57680000000005,0,-1167.6279999999999,0,0,0,0,0,0.51775868411040638,0.66921910480349345,12.426208418649752,32.122517030567685,20.449829479873753,538.90523076923068,85.769431335001642,743.33507157001429,1306.2376652507508,314.60670626217575,-153439.584397,10.718455346311787,574.90464020492027,123.74748695848326,-153629.27918799999,16.239768572194528,480.22328631126925,66.94748695407101,-153653.83784872413,17.817949873407656,null,29.7]
["IC/ICD","IC55-075A1",2164,4.5999999999999996,4690,11.1,"NA",17.7,197,272.23611075682078,23.9,330,32,1.4399265362344242,0.66498092700944877,1.1384862234960349,null,0.20920502092050211,0.27050125832186345,0.32264477611940295,0.74702412247485217,907.92239999999993,0,-1513.204,0,0,0,0,0,5.1846074511690488E-2,6.701265403573628E-2,1.2443057882805717,3.2166073937153414,2.0477558667829401,698.40184615384612,111.15410607989003,963.33558602571361,212373.42349426734,46320.432789843799,-124713.65432500001,0.66498092700944877,97857.335168725709,19195.855030025356,-148692.0877,1.1384862234960349,78818.044160116362,8545.3097294889649,-152678.7098212461,1.3386448575275613,null,385]
["IC/ICD","IC55-075A3",2164,22.9,4690,55.5,"NA",0.71,7.9,54.51793282948281,23.9,330,32,7.1902946361900559,4.1204149857702834,6.1609285923525157,null,0.20920502092050211,0.27050125832186345,0.32264477611940295,0.14453176839258267,907.92239999999993,0,-1513.204,0,0,0,0,0,0.25810328398211135,0.33360647335181759,6.1944788155706725,16.013110720887244,10.194262902028115,698.40184615384612,111.15410607989003,963.33558602571361,8530.7508497237923,1860.464312384503,-152499.43448125001,4.1204149857702834,3918.5428066889544,767.65104060549766,-153465.73368924999,6.1609285923525157,3159.7419657494033,341.73085261781239,-153624.70931324357,6.9188941028090252,null,77.099999999999994]
["IC/ICD","IC55-075A5",2164,7.9,4690,19.2,"NA",5.9,65.7,157.68481220460009,23.9,330,32,2.4859718226468757,1.3206317698631682,2.0625000257999129,null,0.20920502092050211,0.27050125832186345,0.32264477611940295,0.42433388008293915,907.92239999999993,0,-1513.204,0,0,0,0,0,8.9039997530946713E-2,0.11508694932224277,2.1369599407427211,5.5241735674676526,3.5167981190402671,698.40184615384612,111.15410607989003,963.33558602571361,70874.71259735887,15469.40954198317,-144039.73120000001,1.3206317698631682,32653.935135094311,6365.0174677951591,-152034.630925,2.0625000257999129,26408.142259468055,2833.4786656203109,-153341.10585981919,2.3566348268126567,null,223]
["IC/ICD","IC55-075A7",2164,39.700000000000003,4690,96.1,"NA",0.24,2.6,31.466251762801363,23.9,330,32,12.457791380904569,7.2931546252148891,10.777728742562038,null,0.20920502092050211,0.27050125832186345,0.32264477611940295,8.3089381528555203E-2,907.92239999999993,0,-1513.204,0,0,0,0,0,0.44745416480741579,0.57834834026494153,10.738899955377979,27.760720332717192,17.673023458974505,698.40184615384612,111.15410607989003,963.33558602571361,2795.2800670046522,628.50722463150714,-153265.03892799999,7.2931546252148891,1298.1945349164082,259.64346324527406,-153595.912912,10.777728742562038,1051.17553122647,115.58400546355448,-153650.50709524655,12.035232199391585,null,44.5]
["IC/ICD","IC55-100A1",2989,4.7,6250,11.1,"NA",22.1,260,363.45288552988541,31.2,330,32,1.0785441954285084,0.44578594230702701,0.82283022472015177,null,0.16025641025641027,0.24530780072385544,0.30326912,0.99996047180141578,1137.2592000000002,0,-1895.432,0,0,0,0,0,4.8039444308421692E-2,6.2092466822794699E-2,1.1529466634021206,2.9804384074941455,1.8974060205345193,874.81476923076934,139.23109481287264,1206.6694883782295,372929.72532692086,77213.636251075164,-108531.25292499999,0.44578594230702701,175276.09278850481,32694.062196401199,-145572.26732499999,0.82283022472015177,139135.01194084244,13198.704350464182,-152345.23819792151,1.0000395297611244,null,514]
["IC/ICD","IC55-100A3",2989,23.7,6250,55.5,"NA",0.88,10.4,72.831998462214386,31.2,330,32,5.3822496742743038,3.0871555674229989,4.5677929441675458,null,0.16025641025641027,0.24530780072385544,0.30326912,0.19251331325772766,1137.2592000000002,0,-1895.432,0,0,0,0,0,0.24224145321480725,0.31310456674473069,5.8137948771553738,15.029019203747072,9.5677707843974691,874.81476923076934,139.23109481287264,1206.6694883782295,14937.769013076831,3080.551785216408,-151874.9908,3.0871555674229989,7061.1466591851713,1315.4788704437633,-153337.770448,4.5677929441675458,5590.7920226022125,531.06330397147769,-153610.83226829578,5.194445948064109,null,103]
["IC/ICD","IC55-100A5",2989,8.1999999999999993,6250,19.2,"NA",7.4,86.7,210.01071401240461,31.2,330,32,1.8665714358594387,0.9570757566525222,1.5118699497096399,null,0.16025641025641027,0.24530780072385544,0.30326912,0.56555628993730522,1137.2592000000002,{"$f":"(Ltorque+IF(Lspeed2=0,0,IF(Lspeed2>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},-1895.432,{"$f":"(Ltorque+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},0,{"$f":"(Ltorque2+IF(Lspeed6=0,0,IF(Lspeed6>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},0,0,8.3813498580650611E-2,0.10833153786104605,2.0115239659356146,5.1999138173302102,3.3103679507197996,874.81476923076934,139.23109481287264,1206.6694883782295,124228.32907662494,25840.745072106569,-138523.9552,0.9570757566525222,58719.100333963375,11036.151541212179,-150902.45319999999,1.5118699497096399,46486.335565653331,4455.3319952824049,-153213.93292774691,1.7681705920216271,null,297]
["IC/ICD","IC55-100A7",2989,41.1,6250,96.1,"NA",0.28999999999999998,3.5,41.93143212436226,31.2,330,32,9.3485955556535139,5.4172986005829795,7.9809432958450905,null,0.16025641025641027,0.24530780072385544,0.30326912,0.11047047532373445,1137.2592000000002,0,-1895.432,0,0,0,0,0,0.42008960873960244,0.54297880562060896,10.082150609750459,26.062982669789228,16.592210094461436,874.81476923076934,139.23109481287264,1206.6694883782295,5029.4209720128683,1012.0260994370813,-153081.48912925,5.4172986005829795,2356.5749961434394,432.8228167207497,-153557.45307925,7.9809432958450905,1855.7586939940645,174.73204644056582,-153646.63536193574,9.0521924257996851,null,59.3]
["IC/ICD","IC55-150A1",4532,4.8,9375,11.1,"NA",30.9,387,545.17932829482811,45.1,330,32,0.71902946361900555,0.19962160385996325,0.50618123968311179,null,0.11086474501108647,0.22391156636793089,0.27981183999999998,1.520327855083015,1573.9416000000001,0,-2623.2359999999999,0,0,0,0,0,4.4782313273586172E-2,5.7882524271844656E-2,1.0747755185660681,2.7783611650485436,1.7687596524481319,1210.7243076923078,192.69275829074363,1670.0039051864446,830787.46258117747,161939.00634558071,-65432.394925000001,0.19962160385996325,396996.3527544057,70027.678419710574,-137164.88320000001,0.50618123968311179,310768.66943380225,25804.610863207668,-151423.65001807892,0.65775286340813421,null,771]
["IC/ICD","IC55-150A3",4532,24,9375,55.5,"NA",1.2,15.5,108.89444430272832,45.1,330,32,3.5998163405860604,2.0338418893831856,3.0219887709813649,null,0.11086474501108647,0.22391156636793089,0.27981183999999998,0.287439930196839,1573.9416000000001,0,-2623.2359999999999,0,0,0,0,0,0.22391156636793089,0.2894126213592233,5.3738775928303415,13.891805825242718,8.843798262240659,1210.7243076923078,192.69275829074363,1670.0039051864446,33255.863169302043,6280.7366494703456,-150337.32999999999,2.0338418893831856,15859.353521797899,2715.9942267979877,-153041.92000000001,3.0219887709813649,12401.328009546534,1000.8210426338211,-153579.53021088053,3.4789877638614772,null,154]
["IC/ICD","IC55-150A5",4532,8.3000000000000007,9375,19.2,"NA",10.3,129,314.66251762801363,45.1,330,32,1.2457791380904568,0.58026005778596967,0.97440720948037152,null,0.11086474501108647,0.22391156636793089,0.27981183999999998,0.85129554424988463,1573.9416000000001,0,-2623.2359999999999,0,0,0,0,0,7.7436083368909434E-2,0.10008853155339807,1.8584660008538265,4.8042495145631072,3.0584802323582285,1210.7243076923078,192.69275829074363,1670.0039051864446,276391.79378561018,53890.73393302413,-124332.23679999998,0.58026005778596967,132160.44799503766,23296.515189796894,-148182.59492499998,0.97440720948037152,103513.52909092707,8584.5700229912054,-152919.70162878788,1.1746801762966417,null,445]
["IC/ICD","IC55-150A7",4532,41.6,9375,96.1,"NA",0.41,5.2,62.932503525602726,45.1,330,32,6.2288956904522843,3.5983264912435655,5.2870843366596683,null,0.11086474501108647,0.22391156636793089,0.27981183999999998,0.16535802528093457,1573.9416000000001,0,-2623.2359999999999,0,0,0,0,0,0.38811338170441356,0.50164854368932044,9.3147211609059255,24.079130097087379,15.329250321217144,1210.7243076923078,192.69275829074363,1670.0039051864446,11181.120268018609,2147.3996841576491,-152499.67089924999,3.5983264912435655,5313.5517022376625,929.57155942724478,-153445.819648,5.2870843366596683,4144.2255529124104,342.53930591212531,-153634.3741507146,6.0474839264744045,null,89]
["IC/ICD","IC55-200A1",6303,5,12500,11.1,"NA",39.799999999999997,513,726.90577105977081,59,330,32,0.53927209771425422,2.3331846534652645E-2,0.33721615794839821,null,8.4745762711864403E-2,0.20566546425437443,0.26808320000000002,2.0597935888729606,2010.624,0,-3351.04,0,0,0,0,0,4.2846971719661342E-2,5.5381035485747528E-2,1.0283273212718722,2.6582897033158814,1.6923197858120418,1546.6338461538462,246.15442176861461,2133.33832199466,1465957.7444165745,278108.84369165532,-7286.8237000000372,2.3331846534652645E-2,718629.34770241333,125274.25391516006,-123963.25,0.33721615794839821,550185.18159918848,42400.819710693402,-150261.5459277606,0.48548553864912325,null,1028]
["IC/ICD","IC55-200A3",6303,25,12500,55.5,"NA",1.6,20.5,145.66399692442877,59,330,32,2.6911248371371519,1.4945934024391179,2.2144406578198108,null,8.4745762711864403E-2,0.20566546425437443,0.26808320000000002,0.3849063419406229,2010.624,0,-3351.04,0,0,0,0,0,0.21423485859830671,0.27690517742873766,5.141636606359361,13.291448516579408,8.4615989290602087,1546.6338461538462,246.15442176861461,2133.33832199466,58647.560861182879,11202.006491696027,-147749.92000000001,1.4945934024391179,28812.667815352419,5045.9488701333466,-152464,2.2144406578198108,22088.028818654457,1707.8718222245157,-153526.53057964236,2.5980346152734053,null,206]
["IC/ICD","IC55-200A5",6303,8.6999999999999993,12500,19.2,"NA",13.3,171,420.02142802480921,59,330,32,0.93328571792971937,0.37779227695655337,0.69032001076771055,null,8.4745762711864403E-2,0.20566546425437443,0.26808320000000002,1.1453324701343488,2010.624,0,-3351.04,0,0,0,0,0,7.4553730792210726E-2,9.6363001745200697E-2,1.7892895390130574,4.6254240837696337,2.9446364273129522,1546.6338461538462,246.15442176861461,2133.33832199466,488102.87047563423,92887.002556491178,-104757.4528,0.37779227695655337,240413.84376709186,42089.423033410065,-143622.39692500001,0.69032001076771055,183749.22628996702,14245.752674570584,-152513.65553818183,0.87310892345756941,null,594]
["IC/ICD","IC55-200A7",6303,43.3,12500,96.1,"NA",0.53,6.8,84.145706961199153,59,330,32,4.6585858525231369,2.700603360543782,3.9120736215063014,null,8.4745762711864403E-2,0.20566546425437443,0.26808320000000002,0.22084949329150072,2010.624,0,-3351.04,0,0,0,0,0,0.3710547750922672,0.47959976730657355,8.9053146022144123,23.020788830715532,14.655489345132281,1546.6338461538462,246.15442176861461,2133.33832199466,19428.187913948983,3711.6058668079741,-151718.37213325,2.700603360543782,9587.2709984920548,1672.3468681871516,-153269.00754925,3.9120736215063014,7367.6702967767123,566.02913875478384,-153618.75051395813,4.5279705427265498,null,119]
["IC/ICD","IC55-250A1",7496,5,15625,11.1,"NA",48.3,639,873.27687476538608,73,330,32,0.44888398093137921,{"$error":"#NUM!"},0.24739112147472953,null,6.8493150684931503E-2,0.210762687711019,0.26138112000000002,2.542320523065468,2450.4479999999999,0,-4084.08,0,0,0,0,0,4.3908893273128961E-2,5.6753601921024542E-2,1.053813438555095,2.7241728922091779,1.7342623265281429,1884.9599999999998,300.00070153049904,2600.0060799309917,2217296.6851658821,405464.37392773892,61912.532674999995,{"$error":"#NUM!"},1057776.0794914945,182641.60987735991,-109922.3125,0.24739112147472953,798122.63634093315,63349.692653351129,-148401.58486875831,0.39334143390945231,null,1235]
["IC/ICD","IC55-250A3",7496,24.8,15625,55.5,"NA",1.9,25.6,174.65537495307723,73,330,32,2.2444199046568958,1.1921485156045406,1.8161282889604848,null,6.8493150684931503E-2,0.210762687711019,0.26138112000000002,0.46409703594606633,2450.4479999999999,0,-4084.08,0,0,0,0,0,0.21778811063471962,0.28149786552828171,5.226914655233271,13.511897545357522,8.6019411395795888,1884.9599999999998,300.00070153049904,2600.0060799309917,88874.129996394549,15949.944315998016,-145324.22312499999,1.1921485156045406,42159.286862424313,7127.182324986502,-151998.77919999999,1.8161282889604848,31906.64816212151,2472.0807601042693,-153463.662892869,2.1547217985598426,null,247]
["IC/ICD","IC55-250A5",7496,8.6,15625,19.2,"NA",16.100000000000001,213,504.16713498600836,73,330,32,0.77751993892041138,0.2542294136877104,0.54954132635789521,null,6.8493150684931503E-2,0.210762687711019,0.26138112000000002,1.3936116186720757,2450.4479999999999,0,-4084.08,0,0,0,0,{"$f":"(Ltorque2+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},7.5523296429781797E-2,9.7616195304162212E-2,1.8125591143147632,4.6855773745997862,2.9829312016284057,1884.9599999999998,300.00070153049904,2600.0060799309917,737780.50863886485,134968.45250078849,-81997.619199999986,0.2542294136877104,351208.04817418195,60454.619349311513,-139285.6213,0.54954132635789521,265857.0763723352,20968.833760422054,-151934.18567508162,0.71756003365763077,null,713]
["IC/ICD","IC55-250A7",7496,42.9,15625,96.1,"NA",0.64,8.5,101.11626970967629,73,330,32,3.8767252898619113,2.1710742346736533,3.2144117186032268,null,6.8493150684931503E-2,0.210762687711019,0.26138112000000002,0.26650699571997083,2450.4479999999999,0,-4084.08,0,0,0,0,0,0.37673830428344646,0.4869459044823905,9.041719302802715,23.373403415154744,14.879970761611466,1884.9599999999998,300.00070153049904,2600.0060799309917,29517.762365545292,5385.8596627598827,-150826.94348799999,2.1710742346736533,14069.297572569893,2404.301556008314,-153098.62604800001,3.2144117186032268,10687.054649325155,833.93792203964244,-153595.98176362505,3.752246717946341,null,143]
["IC/ICD","IC11-030A1AC",296,9.6999999999999993,375,13.8,"NA",1.6,10.3,17.53624817342638,2.5,330,32,22.353698243961823,12.924966025858723,15.849040000145132,null,2,0.51321371721732023,1.0471999999999999,5.8478670555827575E-2,235.62,0,-392.7,0,0,0,0,0,0.2074238773753336,0.30663765822784811,4.9781730570080063,14.71860759493671,8.1925867253542801,181.24615384615385,28.846221301009521,250.00058460874919,891.70939079726395,335.32534782804595,-153298.35519999999,12.924966025858723,596.14833322891491,235.69970100956851,-153483.34719999999,15.849040000145132,513.41110658133516,199.07115893411998,-153535.1325236753,17.100251946482512,null,24.8]
["IC/ICD","IC11-030A5AC",296,16.899999999999999,375,23.9,"NA",0.53,3.4,10.111626970967629,2.5,330,32,38.767252898619113,22.696678522214672,27.67541302200156,null,2,0.51321371721732023,1.0471999999999999,3.3515994290244357E-2,235.62,0,-392.7,0,0,0,0,0,0.36138799254052967,0.53059071729957796,8.673311820972712,25.468354430379744,14.273682026648178,181.24615384615385,28.846221301009521,250.00058460874919,293.17522284622652,110.92397949430838,-153543.66033325001,22.696678522214672,197.71178270182727,78.43578466333939,-153603.82911324999,27.67541302200156,170.34559605842588,66.246594662435172,-153621.07749714539,29.836501084829052,null,14.3]
["IC/ICD","IC11-050A1AC",502,9.9,625,13.8,"NA",2.1,16.5,29.274220741123063,3.6,330,32,13.390621170295974,7.904830385562243,9.5430757496323064,null,1.3888888888888888,0.34699517624127757,0.72047359999999994,8.5951970799304694E-2,270.17759999999998,0,-450.29599999999999,0,0,0,0,0,0.143135510199527,0.18500707171314743,3.4352522447886482,8.880339442231076,5.6533996742600019,207.82892307692308,33.077000425157586,286.66733701803241,2356.1369577203795,734.70730191961468,-153034.11970000001,7.904830385562243,1628.5215533825583,527.07262963798439,-153339.83192500001,9.5430757496323064,1108.5786526039092,300.98507401078217,-153558.28923104706,11.634404548267664,null,41.4]
["IC/ICD","IC11-050A5AC",502,17.2,625,23.9,"NA",0.7,5.5,16.899852070358484,3.6,330,32,23.19546930754198,13.824448044632184,16.634152684616328,null,1.3888888888888888,0.34699517624127757,0.72047359999999994,4.9403282771548776E-2,270.17759999999998,0,-450.29599999999999,0,0,0,0,0,0.24867987630624891,0.32142642762284196,5.968317031349974,15.428468525896415,9.822068120936569,207.82892307692308,33.077000425157586,286.66733701803241,785.22777172131077,244.85528129565628,-153454.08032499999,13.824448044632184,544.36867848257657,176.21384260607903,-153555.2788,16.634152684616328,369.9874840847765,100.62699801912225,-153628.54616435166,20.241569869439878,null,23.9]
["IC/ICD","IC11-075A1AC",754,9.9,940,13.8,"NA",2.8,24.4,43.982041789803255,5,330,32,8.9127285602934609,5.2702382913218626,6.3574264594364678,null,1,0.2686317600288714,0.55702127659574474,0.12295997559334505,314.16000000000003,0,-523.6,0,0,0,0,0,0.11081060101190947,0.14322612732095491,2.6594544242858271,6.8748541114058357,4.3766680594635137,241.66153846153847,38.461628401346033,333.33411281166559,5212.7968093605332,1471.7808109307578,-152544.21280000001,5.2702382913218626,3621.6375545338469,1055.8427556677177,-153087.70120000001,6.3574264594364678,2264.1723621811925,466.77507722695333,-153551.36728697995,8.1327277040718844,null,62.2]
["IC/ICD","IC11-075A5AC",754,17.100000000000001,940,23.9,"NA",0.93,8.1,25.385133444597052,5,330,32,15.44210909332182,9.2782186311629218,11.168308980752537,null,1,0.2686317600288714,0.55702127659574474,7.0507203558568585E-2,314.16000000000003,0,-523.6,0,0,0,0,0,0.19140012902057091,0.24739058355437668,4.5936030964937018,11.87474801061008,7.5596993754369786,241.66153846153847,38.461628401346033,333.33411281166559,1728.0496298391799,488.64215640275415,-153293.47035325001,9.2782186311629218,1199.1371059002374,349.6142625308409,-153474.32094325,11.168308980752537,752.82268555975577,154.56015918703261,-153626.92883697688,14.182947975937306,null,35.9]
["IC/ICD","IC11-100A1AC",1006,9.9,1250,13.8,"NA",3.5,32.1,58.619152160364791,6.5,330,32,6.6872342153227171,3.9511693694431913,4.7659598972464412,null,0.76923076923076927,0.23154135101494472,0.48171199999999997,0.16076152238811275,361.28399999999999,0,-602.14,0,0,0,0,0,9.5510807293664693E-2,0.12345067097415507,2.2922593750479527,5.9256322067594436,3.7723746266012057,277.91076923076923,44.230872661547934,383.33422973341544,9110.2043417985569,2451.9820985964602,-151914.33249999999,3.9511693694431913,6356.3303701411287,1759.0306359496344,-152763.53312499999,4.7659598972464412,3860.2000031945563,670.2750038859175,-153533.25443015352,6.2203939421883909,null,82.9]
["IC/ICD","IC11-100A5AC",1006,17.2,1250,23.9,"NA",1.2,10.7,33.799704140716969,6.5,330,32,11.59773465377099,6.9660797415626883,8.3600790377481058,null,0.76923076923076927,0.23154135101494472,0.48171199999999997,9.219888803951147E-2,361.28399999999999,0,-602.14,0,0,0,0,0,0.16593796822737703,0.21447995361166336,3.9825112374570488,10.295037773359841,6.5540246037919934,277.91076923076923,44.230872661547934,383.33422973341544,3033.388963119764,839.50382158510729,-153047.0932,6.9660797415626883,2121.7870594866181,604.16174607798519,-153344.49280000001,8.3600790377481058,1284.6216820790137,230.21459002703756,-153617.60834241231,10.846117792347496,null,47.8]
["IC/ICD","IC11-150A1AC",1490,9.8000000000000007,1875,13.8,"NA",5,47.7,87.681240867131891,9.4,330,32,4.4707396487923647,2.598221932733892,3.1626320510827322,null,0.53191489361702127,0.19575142266372314,0.4021248,0.23709986837795582,452.3904,0,-753.98400000000004,0,0,0,0,0,7.9931830921020283E-2,0.10331436241610741,1.9183639421044869,4.9590893959731552,3.1570543624149159,347.99261538461542,55.384744897938283,480.00112244879847,20216.987453926919,5239.4585598132171,-150093.25,2.598221932733892,14006.44126798541,3720.7749192876472,-151863.25,3.1626320510827322,8343.7252721019486,1198.6417031123544,-153477.1188953642,4.2176320334599318,null,124]
["IC/ICD","IC11-150A5AC",1490,17,1875,23.9,"NA",1.7,15.9,50.699556211075453,9.4,330,32,7.7318231025139932,4.6230464399424278,5.5826988952794947,null,0.53191489361702127,0.19575142266372314,0.4021248,0.13610425417082578,452.3904,0,-753.98400000000004,0,0,0,0,0,0.13865725772013723,0.17921879194630874,3.3277741852832934,8.6025020134228196,5.4765228735768945,347.99261538461542,55.384744897938283,480.00112244879847,6745.9700551690776,1783.945620868353,-152425.902325,4.6230464399424278,4683.0248584476176,1268.9152951783265,-153037.5925,5.5826988952794947,2789.6876808707748,408.77903756915777,-153598.99168371392,7.3473089147154083,null,71.7]
["IC/ICD","IC11-200A1AC",1991,9.8000000000000007,2500,13.8,"NA",6.4,63.3,117.37972567696688,12.3,330,32,3.3395886533147787,1.9093825779805274,2.3353122503213113,null,0.4065040650406504,0.17599630357451554,0.36233119999999996,0.31574157572757372,543.49680000000001,0,-905.82799999999997,0,0,0,0,0,7.1865157292927181E-2,9.2887937384898714E-2,1.7247637750302525,4.4586209944751385,2.8384462825760823,418.07446153846155,66.538617134328632,576.6680151641815,35842.121294105455,8978.0657644283274,-147813.6832,1.9093825779805274,24905.064740001515,6375.7278616954791,-150713.65119999999,2.3353122503213113,14711.447340717681,1846.6490865047228,-153416.49580137257,3.1671470495948055,null,166]
["IC/ICD","IC11-200A5AC",1991,17,2500,23.9,"NA",2.1,21.1,67.670118959552596,12.3,330,32,5.7928079043913616,3.4453074355769604,4.1652713269302852,null,0.4065040650406504,0.17599630357451554,0.36233119999999996,0.18044387742237467,543.49680000000001,0,-905.82799999999997,0,0,0,0,0,0.12466404836528183,0.16113213627992631,2.991937160766764,7.7343425414364635,4.9238353881421828,418.07446153846155,66.538617134328632,576.6680151641815,11932.536047869249,2941.336872802633,-151774.72292500001,3.4453074355769604,8299.5949813277311,2092.1643028303247,-152708.13250000001,4.1652713269302852,4891.344451001215,605.96897835786888,-153583.8124575706,5.5418893358140737,null,95.7]
["IC/ICD","IC11-250A1AC",2410,9.9,3125,13.8,"NA",7.7,78.900000000000006,140.71424945612296,15.2,330,32,{"$f":"IF(G311=\"NA\",(UAC_V*0.98)/J311,(IF((UAC_V*0.98)/J311<G311,(UAC_V*0.98)/J311,G311)))","v":2.7857875198505191},{"$f":"IF(AO311<G311,IF(AO311<0,0,AO311),G311)","v":1.5231929230739536},{"$f":"IF(AS311<G311,IF(AS311<0,0,AS311),G311)","v":1.8766986038334652},null,{"$f":"IF(move1,Gewicht/K311,MAX(Gewicht,Gewicht2)/K311)","v":0.32894736842105265},{"$f":"IF(move1,IF(AccType=1,SQRT((V311^2*Ltime1+W311^2*Ltime2+X311^2*Ltime3+Y311^2*Ltime4)/ltime)/C311,SQRT((((V311-W311)*2/PI()+W311)^2*Ltime1+W311^2*Ltime2+((X311-W311)*2/PI()+W311)^2*Ltime3+Y311^2*Ltime4)/ltime)/C311),IF(AccType=1,SQRT((V311^2*Ltime1+W311^2*Ltime2+X311^2*Ltime3+Y311^2*Ltime4+Z311^2*Ltime5+AA311^2*Ltime6+AB311^2*Ltime7+AC311^2*Ltime8)/ltime)/C311,SQRT((((V311-W311)*2/PI()+W311)^2*Ltime1+W311^2*Ltime2+((X311-W311)*2/PI()+W311)^2*Ltime3+Y311^2*Ltime4+((Z311-AA311)*2/PI()+AA311)^2*Ltime5+AA311^2*Ltime6+((AB311-AA311)*2/PI()+AA311)^2*Ltime7+AC311^2*Ltime8)/ltime)/C311))","v":0.16977081371982303},{"$f":" IF(move1,MAX(ABS(V311),ABS(X311))/E311,MAX(ABS(V311),ABS(X311),ABS(Z311),ABS(AB311))/E311)","v":0.33845503999999998},{"$f":"IF(AW311>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW311,G311),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW311,G311)),\"NA\")","v":0.38020999736663069},{"$f":"((Gewicht+K311)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":634.60320000000002},0,{"$f":"((Gewicht+K311)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-1057.672},0,{"$f":"((Gewicht2+K311)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K311)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"AF311/Irms","v":7.0030460659427002E-2},{"$f":"AG311/Ipeak","v":9.0516535269709542E-2},{"$f":"D311*S311","v":1.680731055826248},{"$f":"IF(move1,IF(MAX(ABS(V311),ABS(X311))<=C311,MAX(ABS(V311),ABS(X311))/C311*D311,D311+(MAX(ABS(V311),ABS(X311))-C311)/(E311-C311)*(F311-D311)),IF(MAX(ABS(V311),ABS(X311),ABS(Z311),ABS(AB311))<=C311,MAX(ABS(V311),ABS(X311),ABS(Z311),ABS(AB311))/C311*D311,D311+(MAX(ABS(V311),ABS(X311),ABS(Z311),ABS(AB311))-C311)/(E311-C311)*(F311-D311)))","v":4.344793692946058},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V311),ABS(X311))<=C311,MAX(ABS(V311),ABS(X311))/C311*D311,D311+(MAX(ABS(V311),ABS(X311))-C311)/(E311-C311)*(F311-D311)),IF(MAX(ABS(V311),ABS(X311),ABS(Z311),ABS(AB311))<=C311,MAX(ABS(V311),ABS(X311),ABS(Z311),ABS(AB311))/C311*D311,D311+(MAX(ABS(V311),ABS(X311),ABS(Z311),ABS(AB311))-C311)/(E311-C311)*(F311-D311))),IF(move1,IF(MAX(ABS((V311-W311)*2/PI()+W311),ABS((X311-W311)*2/PI()+W311))<=C311,MAX(ABS((V311-W311)*2/PI()+W311),ABS((X311-W311)*2/PI()+W311))/C311*D311,D311+(MAX(ABS((V311-W311)*2/PI()+W311),ABS((X311-W311)*2/PI()+W311))-C311)/(E311-C311)*(F311-D311)),IF(MAX(ABS((V311-W311)*2/PI()+W311),ABS((X311-W311)*2/PI()+W311),ABS((Z311-AA311)*2/PI()+AA311),ABS((AB311-AA311)*2/PI()+AA311))<=C311,MAX(ABS((V311-W311)*2/PI()+W311),ABS((X311-W311)*2/PI()+W311),ABS((Z311-AA311)*2/PI()+AA311),ABS((AB311-AA311)*2/PI()+AA311))/C311*D311,D311+(MAX(ABS((V311-W311)*2/PI()+W311),ABS((X311-W311)*2/PI()+W311),ABS((Z311-AA311)*2/PI()+AA311),ABS((AB311-AA311)*2/PI()+AA311))-C311)/(E311-C311)*(F311-D311))))","v":2.7659815717874232},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V311)+Ltime2*ABS(Lspeed2)*ABS(W311)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X311)+Ltime4*ABS(Lspeed1)*ABS(Y311))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V311)+Ltime2*ABS(Lspeed2)*ABS(W311)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X311)+Ltime4*ABS(Lspeed1)*ABS(Y311)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z311)+Ltime6*ABS(Lspeed6)*ABS(AA311)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB311)+Ltime8*ABS(Lspeed1)*ABS(AC311))/ltime)","v":488.15630769230768},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK311/2*Ltime1/ltime,AK311/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X311*-ABS(Lspeed2-Lspeed1),((X311-Y311)*2/PI()+Y311)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V311*-ABS(Lspeed2-Lspeed1),((V311-W311)*2/PI()+W311)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X311*-ABS(Lspeed2-Lspeed1),((X311-Y311)*2/PI()+Y311)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V311*-ABS(Lspeed2-Lspeed1),((V311-W311)*2/PI()+W311)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB311*-ABS(Lspeed6-Lspeed1),((AB311-AC311)*2/PI()+AB311)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z311*-ABS(Lspeed6-Lspeed1),((Z311-AA311)*2/PI()+AA311)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB311*-ABS(Lspeed6-Lspeed1),((AB311-AC311)*2/PI()+AB311)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z311*-ABS(Lspeed6-Lspeed1),((Z311-AA311)*2/PI()+AA311)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":77.692489370718974},{"$f":"IF(move1,MAX(IF(AccType=1,X311*-ABS(Lspeed2-Lspeed1),((X311-Y311)*2/PI()+Y311)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V311*-ABS(Lspeed2-Lspeed1),((V311-W311)*2/PI()+W311)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X311*-ABS(Lspeed2-Lspeed1),((X311-Y311)*2/PI()+Y311)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V311*-ABS(Lspeed2-Lspeed1),((V311-W311)*2/PI()+W311)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB311*-ABS(Lspeed6-Lspeed1),((AB311-AC311)*2/PI()+AB311)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z311*-ABS(Lspeed6-Lspeed1),((Z311-AA311)*2/PI()+AA311)*-ABS(Lspeed6-Lspeed1)),0))","v":673.33490787956453},{"$f":"(J311^2)+3*(I311/1000)^2*(F311/2)^2*(2000*PI()/M311)^2","v":54079.900862334209},{"$f":"SQRT(3)*H311*F311/2*J311","v":12949.068308389991},{"$f":"3*F311^2*H311^2/4-(UAC_V*0.98)^2","v":-145195.60930000001},{"$f":"-AM311/2/AL311+SQRT((AM311/2/AL311)^2-AN311/AL311)","v":1.5231929230739536},{"$f":"(J311^2)+3*(I311/1000)^2*(D311/2)^2*(2000*PI()/M311)^2","v":37442.403373857254},{"$f":"SQRT(3)*H311*D311/2*J311","v":9289.5490038449916},{"$f":"3*D311^2*H311^2/4-(UAC_V*0.98)^2","v":-149305.74032499999},{"$f":"-AQ311/2/AP311+SQRT((AQ311/2/AP311)^2-AR311/AP311)","v":1.8766986038334652},{"$f":"(J311^2)+3*(I311/1000)^2*(AH311/2)^2*(2000*PI()/M311)^2","v":21177.625799340567},{"$f":"SQRT(3)*H311*AH311/2*J311","v":2595.4263994799458},{"$f":"3*AH311^2*H311^2/4-(UAC_V*0.98)^2","v":-153323.79454078848},{"$f":"IF((AU311/2/AT311)^2-AV311/AT311>=0,-AU311/2/AT311+SQRT((AU311/2/AT311)^2-AV311/AT311),-9999)","v":2.6301254752007881},null,199]
["IC/ICD","IC11-250A5AC",2410,17.2,3125,23.9,"NA",2.6,26.3,81.317279836452954,15.2,330,32,4.8206236213065505,2.7724144280658507,3.3615021576882325,null,0.32894736842105265,0.16977081371982303,0.33845503999999998,0.2175305740458883,634.60320000000002,0,-1057.672,0,0,0,0,0,0.12166908316587316,0.15726105117565697,2.9200579959809558,7.5485304564315348,4.8055437408831994,488.15630769230768,77.692489370718974,673.33490787956453,18036.766941220281,4376.0746627257158,-150767.96530000001,2.7724144280658507,12529.334670069864,3149.3089622963307,-152164.0912,3.3615021576882325,7074.3677192541709,879.89197510874988,-153546.91721922709,4.5970549399140967,null,115]
["IC/ICD","IC22-030A1AC",603,9.9,750,13.8,"NA",3.1,20.6,35.14320702497141,4.8,330,32,11.154360491956806,6.3499927186686955,7.7320783093097285,null,1.0416666666666667,0.32918305160950856,0.6841706666666667,0.10338772034828457,307.8768,0,-513.12800000000004,0,0,0,0,0,0.13578800878892228,0.17551019900497514,3.2589122109341346,8.424489552238807,5.3631966210593358,236.8283076923077,37.692395833319111,326.6674305554323,3571.8025631890559,1302.0054521135846,-152291.4037,6.3499927186686955,2437.65794249191,934.04738955974562,-152957.592925,7.7320783093097285,1587.986658549321,506.00806096930512,-153456.6843493428,9.6723285573110349,null,49.7]
["IC/ICD","IC22-030A2AC",603,19.8,750,27.6,"NA",0.78,5.2,17.606958851545031,4.8,330,32,22.263924355431861,12.831534706794224,15.588391115775366,null,1.0416666666666667,0.32918305160950856,0.6841706666666667,5.1443644236394685E-2,307.8768,0,-513.12800000000004,0,0,0,0,0,0.27157601757784455,0.35102039800995027,6.5178244218682693,16.848979104477614,10.726393242118672,236.8283076923077,37.692395833319111,326.6674305554323,905.59293956670797,328.2605295119107,-153316.40891200001,12.831534706794224,616.52450197927442,235.49124943245766,-153485.11214799999,15.588391115775366,399.96204069350199,127.5743306308281,-153611.50016988144,19.438747290234407,null,24.9]
["IC/ICD","IC22-030A6AC",603,34.299999999999997,750,47.8,"NA",0.26,1.7,10.182337649086284,4.8,330,32,38.498035864600922,22.644367663116597,27.38223209357346,null,1.0416666666666667,0.32918305160950856,0.6841706666666667,2.9508694407675076E-2,307.8768,0,-513.12800000000004,0,0,0,0,0,0.47045744459192257,0.6080807904919846,11.290978670206142,29.187877943615259,18.581580212357093,236.8283076923077,37.692395833319111,326.6674305554323,294.61022284622652,109.59213068391361,-153548.158612,22.644367663116597,201.99213471243371,78.640378294105361,-153604.35195700001,27.38223209357346,132.53254819313076,42.602405166239791,-153646.49455125435,33.88831732724524,null,14.4]
["IC/ICD","IC22-050A1AC",1005,9.9,1250,13.8,"NA",4.2,33,58.619152160364791,6.9,330,32,6.6872342153227171,3.8499756118795689,4.6741863407040558,null,0.72463768115942029,0.23983336617264198,0.49846720000000005,0.16250014486254485,373.85040000000004,0,-623.08400000000006,0,0,0,0,0,9.8931263546214829E-2,0.12787171641791045,2.3743503251091558,6.1378423880597017,3.9074718239146602,287.57723076923077,45.769337797601786,396.66759424588213,9432.8328308815198,2942.378518315752,-151144.47880000001,3.8499756118795689,6522.3712135302339,2110.8367631395613,-152367.32769999999,4.6741863407040558,3916.9786238016572,833.1348663485918,-153461.99991399649,6.1538406679321858,null,82.9]
["IC/ICD","IC22-050A2AC",1005,19.8,1250,27.6,"NA",1.1000000000000001,8.3000000000000007,29.274220741123063,6.9,330,32,13.390621170295974,7.8661842554047823,9.5076361049911622,null,0.72463768115942029,0.23983336617264198,0.49846720000000005,8.0530867713134557E-2,373.85040000000004,0,-623.08400000000006,0,0,0,0,0,0.19786252709242966,0.25574343283582091,4.7487006502183116,12.275684776119403,7.8149436478293204,287.57723076923077,45.769337797601786,396.66759424588213,2374.3636226608915,769.6933639157869,-152972.7028,7.8661842554047823,1637.901911662434,552.17132628741228,-153308.2237,9.5076361049911622,978.63471053699209,217.93877772137898,-153608.57594012149,12.417598722047551,null,41.4]
["IC/ICD","IC22-050A6AC",1005,34.299999999999997,1250,47.8,"NA",0.35,2.8,16.899852070358484,6.9,330,32,23.19546930754198,13.667584288216837,16.51582830009556,null,0.72463768115942029,0.23983336617264198,0.49846720000000005,4.6369984270359758E-2,373.85040000000004,0,-623.08400000000006,0,0,0,0,0,0.3427618524884008,0.44303029021558871,8.2262844597216187,21.265453930348258,13.538008440431598,287.57723076923077,45.769337797601786,396.66759424588213,803.56103706381168,244.85528129565628,-153454.08032499999,13.667584288216837,552.3064311922077,175.70159306361947,-153555.90998125001,16.51582830009556,327.15266939810829,69.348386294243696,-153647.161363836,21.565674772920115,null,23.9]
["IC/ICD","IC22-075A1AC",1493,9.8000000000000007,1875,13.8,"NA",5.7,48.6,87.681240867131891,9.6,330,32,4.4707396487923647,2.5430686409418986,3.1135789305207506,null,0.52083333333333337,0.19807139096462345,0.4077098666666667,0.23833398587218815,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,8.0879151310554578E-2,0.10453880330430899,1.94109963145331,5.0178625586068319,3.1944705198320911,352.82584615384616,56.153977465965212,486.66780470503181,20694.239735012779,5972.9827581870686,-149023.45329999999,2.5430686409418986,14247.122370041103,4241.6834079879181,-151323.74530000001,3.1135789305207506,8384.9335170571376,1382.6461838039102,-153415.33838845114,4.1957927080373336,null,124]
["IC/ICD","IC22-075A2AC",1493,19.600000000000001,1875,27.6,"NA",1.4,12.2,43.982041789803255,9.6,330,32,8.9127285602934609,5.2702382913218626,6.3884277023108877,null,0.52083333333333337,0.19807139096462345,0.4077098666666667,0.11832008794219211,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.16175830262110916,0.20907760660861799,3.88219926290662,10.035725117213664,6.3889410396641821,352.82584615384616,56.153977465965212,486.66780470503181,5212.7968093605332,1471.7808109307578,-152544.21280000001,5.2702382913218626,3587.7244989024657,1045.1776773276397,-153099.28479999999,6.3884277023108877,2110.090349504283,340.69278349078803,-153603.99670561581,8.4516502429289275,null,62.2]
["IC/ICD","IC22-075A6AC",1493,34,1875,47.8,"NA",0.48,4.0999999999999996,25.385133444597052,9.6,330,32,15.44210909332182,9.2026789689090851,11.131457909857252,null,0.52083333333333337,0.19807139096462345,0.4077098666666667,6.8077724183150348E-2,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.28060113719988322,0.36268564411699039,6.7344272927971973,17.40891091761554,11.082856905539908,352.82584615384616,56.153977465965212,486.66780470503181,1754.9714519187082,504.40480660929455,-153269.17964799999,9.2026789689090851,1206.2889036510333,358.7816616049376,-153464.2432,11.131457909857252,704.10745759370604,116.95075929115778,-153642.7750248698,14.689092680444011,null,35.9]
["IC/ICD","IC22-100A1AC",1995,9.8000000000000007,2500,13.8,"NA",7.1,64.099999999999994,117.37972567696688,12.5,330,32,3.3395886533147787,1.8736910687677566,2.3042251132412925,null,0.4,0.17767398865067463,0.36651999999999996,0.31698724060705036,549.78,0,-916.3,0,0,0,0,0,7.2550212032358813E-2,9.3773391812865495E-2,1.7412050887766115,4.501122807017544,2.8655037768020373,422.90769230769229,67.307849702355554,583.33469742041473,36403.348391004853,9960.0417074126744,-146463.93969999999,1.8736910687677566,25188.094830246304,7073.0730965684206,-150032.96770000001,2.3042251132412925,14753.526503354777,2068.1548644707846,-153353.55838703483,3.1547011106344143,null,166]
["IC/ICD","IC22-100A2AC",1995,19.600000000000001,2500,27.6,"NA",1.8,16,58.760573516602093,12.5,330,32,6.671139788811713,3.9496851612633823,4.784600584092173,null,0.4,0.17767398865067463,0.36651999999999996,0.15684577815777617,549.78,0,-916.3,0,0,0,0,0,0.14510042406471763,0.18754678362573099,3.482410177553223,9.0022456140350879,5.7310075536040745,422.90769230769229,67.307849702355554,583.33469742041473,9091.5073864303704,2528.1232625060034,-151812.92319999999,3.9496851612633823,6296.4354200418657,1795.333911054988,-152730.49119999999,4.784600584092173,3695.9262782862411,524.95266354580008,-153584.18799238189,6.3756896216490322,null,83.1]
["IC/ICD","IC22-100A6AC",1995,34,2500,47.8,"NA",0.59,5.3,33.941125496954278,12.5,330,32,11.549410759380278,6.997276154849299,8.4244235427518124,null,0.4,0.17767398865067463,0.36651999999999996,9.0120815025203874E-2,549.78,0,-916.3,0,0,0,0,0,0.25170481725512239,0.32533625730994148,6.0409156141229374,15.616140350877192,9.941543715435639,422.90769230769229,67.307849702355554,583.33469742041473,3007.7889134084789,828.96611671165397,-153067.48539700001,6.997276154849299,2090.9243815322743,589.64117088276646,-153362.1973,8.4244235427518124,1232.2750224654314,172.41010225740231,-153638.19683736077,11.09621567137772,null,48]
["IC/ICD","IC22-150A1AC",2996,9.8000000000000007,3750,13.8,"NA",9.9,95.4,176.06958851545033,18.100000000000001,330,32,2.2263924355431857,1.1900291944148218,1.4879561948769,null,0.27624309392265189,0.15617045451024247,0.32253760000000004,0.47436965146618898,725.70960000000002,0,-1209.5160000000001,0,0,0,0,0,6.3769602258349017E-2,8.2424182242990654E-2,1.5304704542003764,3.9563607476635516,2.5186974785816045,558.23815384615386,88.84636160710933,770.00180059494755,81116.449815707674,20831.918219025105,-139665.2317,1.1900291944148218,56274.265071941642,14793.681054090292,-146604.33970000001,1.4879561948769,32669.936127706238,3802.1231805997618,-153197.68040255952,2.108060658832589,null,249]
["IC/ICD","IC22-150A2AC",2996,19.7,3750,27.6,"NA",2.5,23.9,87.681240867131891,18.100000000000001,330,32,4.4707396487923647,2.5950093310274953,3.1519275864437182,null,0.27624309392265189,0.15617045451024247,0.32253760000000004,0.23299442082755847,725.70960000000002,0,-1209.5160000000001,0,0,0,0,0,0.12818991474382402,0.16568942757009344,3.0765579538517764,7.9530925233644858,5.0630959518426124,558.23815384615386,88.84636160710933,770.00180059494755,20269.574961534734,5239.4585598132171,-150093.25,2.5950093310274953,14097.871123217305,3739.7584647942163,-151844.828125,3.1519275864437182,8111.398349892861,961.15512405932691,-153543.83621585518,4.2919482640320821,null,124]
["IC/ICD","IC22-150A6AC",2996,34.1,3750,47.8,"NA",0.83,8,50.770266889194104,18.100000000000001,330,32,7.72105454666091,4.6069532045023225,5.5588768000475843,null,0.27624309392265189,0.15617045451024247,0.32253760000000004,0.13410123463764276,725.70960000000002,0,-1209.5160000000001,0,0,0,0,0,0.22189218744996952,0.28680251168224297,5.3254124987992686,13.766520560747663,8.7640391856768076,558.23815384615386,88.84636160710933,770.00180059494755,6805.8325474596877,1744.399956190477,-152483.480293,4.6069532045023225,4729.459005055759,1244.4359520103612,-153063.20514325,5.5588768000475843,2719.7578162621157,319.83241781477506,-153624.31502879196,7.4570528951662318,null,71.8]
["IC/ICD","IC22-200A1AC",4023,9.9,5000,13.8,"NA",12.7,127,234.75945135393377,23.7,330,32,1.6697943266573894,0.83690010805380044,1.065961802664773,null,0.2109704641350211,0.14449757794364335,0.30054639999999999,0.63428693145561732,901.63919999999996,0,-1502.732,0,0,0,0,0,5.9605250901752886E-2,7.7041629381058921E-2,1.4305260216420692,3.697998210290828,2.3542187788510698,693.56861538461533,110.38487351186312,956.66890376948027,143927.06913157762,35631.698502574924,-130626.94930000001,0.83690010805380044,100820.70051242344,25561.870664890703,-141807.97532500001,1.065961802664773,57696.771310408127,6078.6096910957549,-152993.55625314481,1.5765735511925372,null,332]
["IC/ICD","IC22-200A2AC",4023,19.8,5000,27.6,"NA",3.2,31.6,117.37972567696688,23.7,330,32,3.3395886533147787,1.9111262061647123,2.3250882228925032,null,0.2109704641350211,0.14449757794364335,0.30054639999999999,0.31151442858292017,901.63919999999996,0,-1502.732,0,0,0,0,0,0.11921050180350577,0.15408325876211784,2.8610520432841384,7.395996420581656,4.7084375577021396,693.56861538461533,110.38487351186312,956.66890376948027,35772.46349606997,8978.0657644283274,-147813.6832,1.9111262061647123,25097.45687486777,6440.7863092637999,-150653.13279999999,2.3250882228925032,14418.101491653826,1531.618189882395,-153493.73912907689,3.2101241812425902,null,166]
["IC/ICD","IC22-200A6AC",4023,34.299999999999997,5000,47.8,"NA",1.1000000000000001,10.5,67.670118959552596,23.7,330,32,5.7928079043913616,3.4471767335196581,4.1494575817198935,null,0.2109704641350211,0.14449757794364335,0.30054639999999999,0.1783347610017583,901.63919999999996,0,-1502.732,0,0,0,0,0,0.2065111218111236,0.26692200886568895,4.9562669234669663,12.81225642555307,8.1565357691506755,693.56861538461533,110.38487351186312,956.66890376948027,11863.001771209854,3081.4005334122826,-151590.50769999999,3.4471767335196581,8329.7338761404226,2211.1305082853828,-152596.33532499999,4.1494575817198935,4791.3305753581917,525.80656213090492,-153603.62486375376,5.6074317445612323,null,95.7]
["IC/ICD","IC22-250A1AC",4806,9.9,6250,13.8,"NA",15.5,158,281.42849891224591,29.3,330,32,1.3928937599252595,0.63156773796294075,0.83578955563645208,null,0.17064846416382251,0.14455697678357632,0.28735168,0.76797258123718615,1077.5688,0,-1795.9479999999999,0,0,0,0,0,5.9629752923225234E-2,7.7073299001248444E-2,1.4311140701574057,3.6995183520599251,2.3551865311580795,828.8990769230769,131.92338541661687,1143.336006944013,216667.39685043733,52132.61267014152,-119349.0925,0.63156773796294075,149948.60546792357,37399.483002492831,-136003.823125,0.83578955563645208,83205.924092578483,8897.2483474491546,-152664.51730819693,1.3021298213394845,null,398]
["IC/ICD","IC22-250A2AC",4806,19.7,6250,27.6,"NA",3.9,39.4,140.71424945612296,29.3,330,32,2.7857875198505191,1.5216377668539696,1.8805573415372165,null,0.17064846416382251,0.14455697678357632,0.28735168,0.37542407952200052,1077.5688,0,-1795.9479999999999,0,0,0,0,0,0.11865718510985222,0.15336807983076708,2.8477724426364532,7.3616678318768196,4.6865832993751679,828.8990769230769,131.92338541661687,1143.336006944013,53993.062642965044,13117.238026680769,-144974.22279999999,1.5216377668539696,37220.411305540198,9362.6662726670693,-149236.86332500001,1.8805573415372165,20786.384794125657,2227.3561112235857,-153413.44495107673,2.6636543965779325,null,199]
["IC/ICD","IC22-250A6AC",4806,34.200000000000003,6250,47.8,"NA",1.3,13.1,81.317279836452954,29.3,330,32,4.8206236213065505,2.7788216700797181,3.3771205987417723,null,0.17064846416382251,0.14455697678357632,0.28735168,0.21502870835078666,1077.5688,0,-1795.9479999999999,0,0,0,0,0,0.20599369191659625,0.26625321473158553,4.9438486059983102,12.780154307116105,8.1360989258188194,828.8990769230769,131.92338541661687,1143.336006944013,17950.055551086825,4376.0746627257158,-150767.96530000001,2.7788216700797181,12416.345553637539,3130.9990264690273,-152181.48130000001,3.3771205987417723,6940.9702762502138,744.85724608170813,-153580.09643598631,4.650541816810116,null,115]
["IC/ICD","IC33-030A1AC",896,9.8000000000000007,1125,13.8,"NA",4.7,31,52.67945519839779,7.3,330,32,7.4412310932919903,4.1399257202030491,5.0958798231640845,null,0.68493150684931503,0.27805186036381241,0.57246933333333339,0.15062495040991628,386.41680000000002,0,-644.02800000000002,0,0,0,0,0,0.11353784298189007,0.146751171875,2.7249082315653617,7.0440562500000006,4.4843854864194395,297.2436923076923,47.307802933655616,410.0009587583487,8066.9150325777218,2959.026475352578,-150508.88529999999,4.1399257202030491,5443.805501621322,2101.3376419170481,-152072.8573,5.0958798231640845,3333.9171645721563,961.5518391305776,-153330.83232671127,6.6390063351294932,null,74.5]
["IC/ICD","IC33-030A3AC",896,29.5,1125,41.4,"NA",0.52,3.4,17.53624817342638,7.3,330,32,22.353698243961823,13.011839676918781,15.821954809607066,null,0.68493150684931503,0.27805186036381241,0.57246933333333339,4.9319599332927545E-2,386.41680000000002,0,-644.02800000000002,0,0,0,0,0,0.34177207836385276,0.44175097656250001,8.2025298807324667,21.204046875,13.498915494834026,297.2436923076923,47.307802933655616,410.0009587583487,880.42097293380448,326.94221413234482,-153316.40891200001,13.011839676918781,598.40606017389177,232.96607045662253,-153487.51329999999,15.821954809607066,368.42832196273912,106.60302705957618,-153627.04563807795,20.275914920751674,null,24.8]
["IC/ICD","IC33-030A5AC",896,17,1125,23.9,"NA",1.6,10.3,30.40559159102154,7.3,330,32,12.8923654988431,7.363928669534789,8.9990883317920307,null,0.68493150684931503,0.27805186036381241,0.57246933333333339,8.6102518858960267E-2,386.41680000000002,0,-644.02800000000002,0,0,0,0,0,0.19695340109103379,0.254568359375,4.7268816261848112,12.21928125,7.7790360478704557,297.2436923076923,47.307802933655616,410.0009587583487,2676.7307389062435,1006.9362434633086,-152567.27679999999,7.363928669534789,1811.0297938479796,716.23080078980115,-153109.12,8.9990883317920307,1110.1295282110596,327.74030693758749,-153547.8142684786,11.614062088451144,null,43]
["IC/ICD","IC33-050A1AC",1492,9.8000000000000007,1875,13.8,"NA",6.4,49.5,87.681240867131891,10.4,330,32,4.4707396487923647,2.488161366706362,3.0647046838139209,null,0.48076923076923073,0.20906464777153105,0.43005013333333336,0.24077425862592464,483.8064,0,-806.34400000000005,0,0,0,0,0,8.5368064506708516E-2,0.11034086237712244,2.0488335481610043,5.2963613941018775,3.3717683850895832,372.15876923076922,59.230907738072894,513.33453372996507,21180.412619483417,6706.5069565609183,-147813.6832,2.488161366706362,14492.302184284748,4762.5918966881891,-150713.65119999999,3.0647046838139209,8493.4654379198,1638.6078355445989,-153314.74978684858,4.1532679020876362,null,124]
["IC/ICD","IC33-050A3AC",1492,29.5,1875,41.4,"NA",0.71,5.5,29.274220741123063,10.4,330,32,13.390621170295974,7.9021692547140594,9.5717067474617217,null,0.48076923076923073,0.20906464777153105,0.43005013333333336,7.9113865239738804E-2,483.8064,0,-806.34400000000005,0,0,0,0,0,0.25697529621917359,0.3321485142984808,6.1674071092601661,15.943128686327078,10.149710955116602,372.15876923076922,59.230907738072894,513.33453372996507,2356.1369577203786,745.20312051846622,-153015.994573,7.9021692547140594,1618.1654083270087,531.00222355784433,-153334.98023125,9.5717067474617217,947.08601258602425,182.69556222496024,-153625.05198667798,12.640009396200012,null,41.4]
["IC/ICD","IC33-050A5AC",1492,17,1875,23.9,"NA",2.1,16.5,50.699556211075453,10.4,330,32,7.7318231025139932,4.4809711196020077,5.4544606516348697,null,0.48076923076923073,0.20906464777153105,0.43005013333333336,0.13775971799199926,483.8064,0,-806.34400000000005,0,0,0,0,0,0.14808745883816785,0.19140761840929402,3.5540990121160281,9.1875656836461133,5.8489859741349903,372.15876923076922,59.230907738072894,513.33453372996507,7067.0499454917972,2203.6975316609069,-151774.72292500001,4.4809711196020077,4845.4731494496409,1567.4835999261682,-152708.13250000001,5.4544606516348697,2839.7535190879053,539.30527003851648,-153550.84831836849,7.2590160213457855,null,71.7]
["IC/ICD","IC33-075A1AC",2240,9.8000000000000007,2815,13.8,"NA",8.5,73.099999999999994,132.22896808188437,14.4,330,32,2.9645546334238144,1.6107574420336284,2.0006294840112768,null,0.34722222222222221,0.1754213362945678,0.36084689165186495,0.35863978429158333,609.47039999999993,0,-1015.7839999999999,0,0,0,0,0,7.1630378986948531E-2,9.2584479166666664E-2,1.7191290956867646,4.4440549999999996,2.8291732824890112,468.82338461538455,74.6155590986113,646.66817885463115,46909.330526516787,13432.450614230822,-143344.5325,1.6107574420336284,32323.613231288979,9538.9866680769592,-148459.83249999999,2.0006294840112768,18721.229993837147,2753.8210431981847,-153230.27124950892,2.7883130756820176,null,187]
["IC/ICD","IC33-075A3AC",2240,29.5,2815,41.4,"NA",0.94,8.1,43.982041789803255,14.4,330,32,8.9127285602934609,5.282218821099204,6.3887123569309408,null,0.34722222222222221,0.1754213362945678,0.36084689165186495,0.11713578011728097,609.47039999999993,0,-1015.7839999999999,0,0,0,0,0,0.21562205919540625,0.27869817708333328,5.1749294206897503,13.377512499999998,8.5163889625944726,468.82338461538455,74.6155590986113,646.66817885463115,5185.9799337531922,1482.2935310088349,-152528.158708,5.282218821099204,3585.3745335647945,1056.2236513227203,-153087.285325,6.3887123569309408,2072.0148116505911,304.92242190359491,-153615.93511058635,8.5371011231475169,null,62.2]
["IC/ICD","IC33-075A5AC",2240,17,2815,23.9,"NA",2.8,24.4,76.367532368147124,14.4,330,32,5.1330714486134568,2.9595087475071566,3.6070592404619419,null,0.34722222222222221,0.1754213362945678,0.36084689165186495,0.20469616559250756,609.47039999999993,0,-1015.7839999999999,0,0,0,0,0,0.12425677987531886,0.16060572916666666,2.9821627170076526,7.7090749999999995,4.9077495716646107,468.82338461538455,74.6155590986113,646.66817885463115,15665.236805685934,4425.8360468503561,-150305.28520000001,2.9595087475071566,10807.062475872683,3148.0842174249397,-151964.68,3.6070592404619419,6246.6345465005252,908.82405703713937,-153522.37428555393,4.8852893609678967,null,108]
["IC/ICD","IC33-100A1AC",3014,9.8000000000000007,3750,13.8,"NA",10.6,96.2,176.06958851545033,18.899999999999999,330,32,2.2263924355431857,1.1668348673561075,1.4687038127118301,null,0.26455026455026459,0.16061398456457465,0.33370773333333331,0.47670927096769494,750.8424,0,-1251.404,0,0,0,0,0,6.5584043697201319E-2,8.4769403892944031E-2,1.5740170487328318,4.0689313868613137,2.5903621732829567,577.57107692307693,91.923291879217018,796.66852961988081,81960.493079176464,22304.882133501626,-137615.62119999999,1.1668348673561075,56699.921000441653,15839.698906399706,-145570.70920000001,1.4687038127118301,32796.027936050319,4186.7915187070621,-153098.55030657191,2.0977146048996533,null,249]
["IC/ICD","IC33-100A3AC",3014,29.7,3750,41.4,"NA",1.2,10.7,58.619152160364791,18.899999999999999,330,32,6.6872342153227171,3.9460904564449697,4.7612824994261747,null,0.26455026455026459,0.16061398456457465,0.33370773333333331,0.15551194770921573,750.8424,0,-1251.404,0,0,0,0,0,0.19875980589866113,0.25690319343065693,4.7702353415678669,12.331353284671533,7.8503833210718179,577.57107692307693,91.923291879217018,796.66852961988081,9110.2043417985533,2522.0387299849303,-151812.92319999999,3.9460904564449697,6356.3303701411269,1809.2886541196237,-152711.34280000001,4.7612824994261747,3640.223864034625,478.23600920219428,-153597.44120024922,6.4303740949206789,null,82.9]
["IC/ICD","IC33-100A5AC",3014,17.100000000000001,3750,23.9,"NA",3.5,32.1,101.82337649086284,18.899999999999999,330,32,3.8498035864600921,2.1971534789331679,2.678068526645581,null,0.26455026455026459,0.16061398456457465,0.33370773333333331,0.27201627050097621,750.8424,0,-1251.404,0,0,0,0,0,0.11443746400225945,0.14791395985401459,2.7464991360542266,7.0998700729927009,4.5199176697080166,577.57107692307693,91.923291879217018,796.66852961988081,27386.720668077884,7376.3934114172625,-148416.00812499999,2.1971534789331679,19080.109575379727,5277.6705998006364,-150977.483125,2.678068526645581,10976.684379475202,1395.0079882419532,-153476.30253788014,3.6762506822047296,null,144]
["IC/ICD","IC33-150A1AC",4464,9.8000000000000007,5625,13.8,"NA",14.9,143,263.7508293825822,27.3,330,32,1.4862512505368721,0.69938850248600959,0.92016632829094092,null,0.18315018315018314,0.14655715972435349,0.30066275555555555,0.71755441743730453,1014.7367999999999,0,-1691.2279999999998,0,0,0,0,0,5.9844173554111008E-2,7.7350444295101559E-2,1.4362601652986642,3.7128213261648746,2.363655467504584,780.56676923076918,124.23105973634766,1076.6691843816798,182167.84482433071,46966.675544957936,-121954.31169999999,0.69938850248600959,126351.02193304306,33353.146401491867,-137672.61969999998,0.92016632829094092,72867.902280644179,8044.4231479966411,-152733.74471484701,1.3936225263185336,null,373]
["IC/ICD","IC33-150A3AC",4464,29.3,5625,41.4,"NA",1.7,15.9,87.681240867131891,27.3,330,32,4.4707396487923647,2.5944464852900948,3.1645276079885325,null,0.18315018315018314,0.14655715972435349,0.30066275555555555,0.23199599398875384,1014.7367999999999,0,-1691.2279999999998,0,0,0,0,0,0.17892186583014821,0.23126204263739544,4.2941247799235569,11.100578046594981,7.0668474691718677,780.56676923076918,124.23105973634766,1076.6691843816798,20216.987453926915,5344.2477310094819,-149948.99170000001,2.5944464852900948,13963.531773974722,3782.2816067289327,-151803.22292500001,3.1645276079885325,8053.0620828450574,912.24597952927195,-153555.75432789186,4.3104192568449076,null,124]
["IC/ICD","IC33-150A5AC",4464,16.98,5625,23.9,"NA",5,47.7,152.02795795510769,27.3,330,32,2.5784730997686203,1.4105752977917794,1.7488858972881274,null,0.18315018315018314,0.14655715972435349,0.30066275555555555,0.40627075887240821,1014.7367999999999,0,-1691.2279999999998,0,0,0,0,0,0.1036891905049801,0.13402148409498207,2.4885405721195224,6.4330312365591391,4.0953948814518197,780.56676923076918,124.23105973634766,1076.6691843816798,60692.225496521693,15733.378804114196,-142953.8125,1.4105752977917794,42081.008056664505,11177.940254973182,-148257.99249999999,1.7488858972881274,24215.941637941589,2695.9999590925449,-153349.52013934334,2.4614126863953212,null,215]
["IC/ICD","IC33-200A1AC",5990,9.8000000000000007,7500,13.8,"NA",19.100000000000001,190,351.43207024971412,35.700000000000003,330,32,1.1154360491956805,0.45052679592646799,0.63789358607862567,null,0.14005602240896359,0.13762466987335559,0.2841402666666667,0.9623546807608977,1278.6312,{"$f":"(Ltorque+IF(Lspeed2=0,0,IF(Lspeed2>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},-2131.0520000000001,{"$f":"(Ltorque+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq,-LDryTorq)))/LWirkungsgrad","v":0},0,{"$f":"(Ltorque2+IF(Lspeed6=0,0,IF(Lspeed6>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},0,0,5.6196740198286875E-2,7.263602392877018E-2,1.3487217647588849,3.4865291485809684,2.2195933929225538,983.56246153846166,156.53882759347835,1356.6698391434791,322290.78530286765,80220.33592054667,-101558.18769999998,0.45052679592646799,223753.58023780407,56968.064639228789,-127386.73569999999,0.63789358607862567,128647.0093752847,12902.646926613999,-152316.04670507665,1.0391179260533523,null,497]
["IC/ICD","IC33-200A3AC",5990,29.5,7500,41.4,"NA",2.1,21.1,117.37972567696688,35.700000000000003,330,32,3.3395886533147787,1.912463390059516,2.3340211893034866,null,0.14005602240896359,0.13762466987335559,0.2841402666666667,0.3104467120765671,1278.6312,0,-2131.0520000000001,0,0,0,0,0,0.16916365671933289,0.21864925570395102,4.0599277612639897,10.49516427378965,6.6814290909403393,983.56246153846166,156.53882759347835,1356.6698391434791,35842.121294105455,8837.7834868591326,-147995.0773,1.912463390059516,24980.887789793967,6297.4544169648416,-150785.64812500001,2.3340211893034866,14352.6781452021,1426.3049200128687,-153516.34825628879,3.2211647316572796,null,166]
["IC/ICD","IC33-200A5AC",5990,17,7500,23.9,"NA",6.4,63.3,202.93964620053913,35.700000000000003,330,32,1.9316087681193495,1.007711026347192,1.270334827083087,null,0.14005602240896359,0.13762466987335559,0.2841402666666667,0.54349562082627523,1278.6312,0,-2131.0520000000001,0,0,0,0,0,9.7484141160293539E-2,0.12600126599888703,2.339619387847045,6.0480607679465779,3.85031506935545,983.56246153846166,156.53882759347835,1356.6698391434791,107364.11943082322,26882.855988276242,-136116.42879999999,1.007711026347192,74667.649831949559,19121.696728062601,-144785.91999999998,1.270334827083087,42902.095927228569,4330.8562978649543,-153208.57826918486,1.8399412280078764,null,287]
["IC/ICD","IC33-250A1AC",7216,9.8000000000000007,9375,13.8,"NA",23.2,237,421.43564158718232,44.1,330,32,0.93015388666149879,0.29486014572520791,0.47553234228909946,null,0.11337868480725623,0.13782045233831569,0.27422677333333334,1.1700956545059349,1542.5256000000002,0,-2570.8760000000002,0,0,0,0,0,5.6276684704812251E-2,7.2739354674796752E-2,1.350640432915494,3.4914890243902441,2.222750947931226,1186.5581538461538,188.84659545060902,1636.6704939052781,486905.14291348396,116850.06677136988,-76787.180799999987,0.29486014572520791,333588.34869465977,82980.482199958307,-114894.57279999999,0.47553234228909946,185632.15563797843,18820.912803035466,-151669.56980125071,0.85463098350044153,null,596]
["IC/ICD","IC33-250A3AC",7216,29.6,9375,41.4,"NA",2.6,26.3,140.71424945612296,44.1,330,32,2.7857875198505191,1.5205058818051311,1.8778148408590702,null,0.11337868480725623,0.13782045233831569,0.27422677333333334,0.37431565237754161,1542.5256000000002,0,-2570.8760000000002,0,0,0,0,0,0.16997855788392269,0.21970254065040651,4.0794853892141445,10.545721951219512,6.713615108037172,1186.5581538461538,188.84659545060902,1636.6704939052781,54079.900862334194,13117.238026680767,-144974.22279999999,1.5205058818051311,37323.80267890892,9378.5083475785214,-149221.8688,1.8778148408590702,20701.95783852696,2127.1518693633748,-153435.48177695836,2.6715420358414019,null,199]
["IC/ICD","IC33-250A5AC",7216,17.100000000000001,9375,23.9,"NA",7.7,78.8,243.24473272817232,44.1,330,32,1.6115456873553875,0.77873257355007408,1.0049890130814718,null,0.11337868480725623,0.13782045233831569,0.27422677333333334,0.65680423065106464,1542.5256000000002,0,-2570.8760000000002,0,0,0,0,0,9.8197072291049944E-2,0.12692275152439025,2.3567297349851986,6.0922920731707322,3.8784735928187719,1186.5581538461538,188.84659545060902,1636.6704939052781,161725.93797147687,38767.045373337387,-128263.719325,0.77873257355007408,111668.7731696566,27737.091041174452,-140661.258325,1.0049890130814718,61868.816984658704,6291.0862657780835,-152995.09507836227,1.522523688692959,null,344]
["IC/ICD","IC44-030A1AC",1201,9.9,1500,13.8,"NA",6.2,41.3,70.28641404994282,9.6,330,32,5.5771802459784032,3.0387513571700882,3.741952192765905,null,0.52083333333333337,0.24622863173204232,0.50963733333333339,0.19846634938727975,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.10156931058946746,0.13128147377185678,2.4376634541472191,6.3015107410491256,4.0116663335385638,352.82584615384616,56.153977465965212,486.66780470503181,14332.639251475019,5208.0218084543385,-148173.61480000001,3.0387513571700882,9774.0118170398364,3736.1895582389825,-150838.37169999999,3.741952192765905,5733.9062700465192,1513.9743299500649,-153200.02535297343,5.0386375478123888,null,99.4]
["IC/ICD","IC44-030A3AC",1201,19.7,1500,27.6,"NA",1.6,10.3,35.14320702497141,9.6,330,32,11.154360491956806,6.3423514425839072,7.7448153572303475,null,0.52083333333333337,0.24622863173204232,0.50963733333333339,9.779809939327104E-2,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.20211266854671806,0.26123687205106855,4.8507040451212333,12.539369858451289,7.9828107849201713,352.82584615384616,56.153977465965212,486.66780470503181,3571.8025631890559,1344.0056279882162,-152201.42079999999,6.3423514425839072,2425.5410127836067,959.30836490463264,-152918.86720000001,7.7448153572303475,1430.5271755281185,388.72980514846887,-153541.64748538655,10.225147586751616,null,49.7]
["IC/ICD","IC44-030A5AC",1201,39.5,1500,55.2,"NA",0.39,2.6,17.53624817342638,9.6,330,32,22.353698243961823,12.849649935603676,15.640269476059842,null,0.52083333333333337,0.24622863173204232,0.50963733333333339,4.8554524230702806E-2,458.67360000000002,0,-764.45600000000002,0,0,0,0,0,0.405251289725653,0.52379981959478206,9.7260309534156715,25.142391340549541,16.0061434519973,352.82584615384616,56.153977465965212,486.66780470503181,903.10793956670818,326.94221413234487,-153316.40891200001,12.849649935603676,612.49337833075901,233.95321482296416,-153486.01448124999,15.640269476059842,357.59732813389377,94.802246012969746,-153634.77436963742,20.595403123477901,null,24.8]
["IC/ICD","IC44-050A1AC",1990,9.8000000000000007,2500,13.8,"NA",8.5,66.099999999999994,117.37972567696688,13.9,330,32,3.3395886533147787,1.7951921240126054,2.2358205246607237,null,0.35971223021582732,0.19237003816419268,0.39584159999999996,0.32177937630098025,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,7.8551098917045356E-2,0.10152972361809044,1.8852263740090884,4.8734267336683414,3.1025198178380249,456.74030769230768,72.692477678543995,630.00147321404791,37837.252786929144,11923.993593381372,-143344.5325,1.7951921240126054,25911.22115971789,8467.7635663143064,-148459.83249999999,2.2358205246607237,14994.054645237873,2680.7555384956049,-153142.41121663703,3.1077193681444575,null,166]
["IC/ICD","IC44-050A3AC",1990,19.600000000000001,2500,27.6,"NA",2.1,16.5,58.619152160364791,13.9,330,32,6.6872342153227171,3.8499756118795689,4.6978308927621875,null,0.35971223021582732,0.19237003816419268,0.39584159999999996,0.15822819468762503,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.15710219783409071,0.20305944723618088,3.7704527480181769,9.7468534673366829,6.2050396356760498,456.74030769230768,72.692477678543995,630.00147321404791,9432.8328308815198,2942.378518315752,-151144.47880000001,3.8499756118795689,6460.3393041265554,2089.5151796735049,-152393.39079999999,4.6978308927621875,3739.2994973265295,661.50635251126835,-153536.65292541837,6.3199861565393292,null,82.9]
["IC/ICD","IC44-050A5AC",1990,39.1,2500,55.2,"NA",0.53,4.0999999999999996,29.274220741123063,13.9,330,32,13.390621170295974,7.9330179280729158,9.626709972757773,null,0.35971223021582732,0.19237003816419268,0.39584159999999996,7.8407932701210853E-2,593.76239999999996,0,-989.60399999999993,0,0,0,0,0,0.31340285384249728,0.40508287688442207,7.5216684922199342,19.443978090452259,12.378420905863956,456.74030769230768,72.692477678543995,630.00147321404791,2338.0204236858522,741.70451431884908,-153022.06484800001,7.9330179280729158,1600.0714625784915,525.3740309758515,-153341.91795325,9.626709972757773,931.45649828598266,166.32483090612527,-153631.71925905393,12.753811579380628,null,41.4]
["IC/ICD","IC44-075A1AC",2980,9.8000000000000007,3750,13.8,"NA",11.3,97.3,176.06958851545033,19.2,330,32,2.2263924355431857,1.1413129232895629,1.4474183790425572,null,0.26041666666666669,0.16448557043271178,0.3378965333333333,0.4790999879400677,760.2672,0,-1267.1119999999999,0,0,0,0,{"$f":"(Ltorque2+IF(Lspeed1=0,0,IF(Lspeed1>0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad","v":0},6.716494126002398E-2,8.6812762863534676E-2,1.6119585902405755,4.1670126174496644,2.6528026239736446,584.82092307692312,93.077140731257387,806.66855300423072,83132.561246121477,23777.846047978146,-135426.0373,1.1413129232895629,57291.001796248209,16885.716758709121,-144466.48929999999,1.4474183790425572,32926.944940008725,4570.8646658346224,-152990.04945748052,2.0872469738510899,null,249]
["IC/ICD","IC44-075A3AC",2980,19.5,3750,27.6,"NA",2.8,24.3,87.681240867131891,19.2,330,32,4.4707396487923647,2.5469164640627335,3.1249110717279396,null,0.26041666666666669,0.16448557043271178,0.3378965333333333,0.23430091067176395,760.2672,0,-1267.1119999999999,0,0,0,0,0,0.1336445259765783,0.17273968120805369,3.2074686234378795,8.2915046979865767,5.2785358334169459,584.82092307692312,93.077140731257387,806.66855300423072,20694.239735012779,5868.1935869908029,-149184.8512,2.5469164640627335,14180.363289275636,4146.0063386348065,-151428.13,3.1249110717279396,8163.7299995357371,1122.2996422593651,-153500.16590959736,4.2680158482222748,null,124]
["IC/ICD","IC44-075A5AC",2980,39.1,3750,55.2,"NA",0.71,6.1,43.982041789803255,19.2,330,32,8.9127285602934609,5.2677033929298025,6.3938202681011482,null,0.26041666666666669,0.16448557043271178,0.3378965333333333,0.11659300982732501,760.2672,0,-1267.1119999999999,0,0,0,0,0,0.26797440849662629,0.34636520693512302,6.4313858039190306,16.625529932885904,10.584141081364235,584.82092307692312,93.077140731257387,806.66855300423072,5212.7968093605332,1492.8062510869117,-152511.99035199999,5.2677033929298025,3579.3000310854059,1057.404427853229,-153085.99515924999,6.3938202681011482,2054.9491111354168,286.23318783779558,-153621.6465101582,8.5768435130116831,null,62.2]
["IC/ICD","IC44-100A1AC",4015,9.9,5000,13.8,"NA",14.1,128,234.05234457274722,25,330,32,1.6748390225083181,0.80336771726611289,1.0406414395817347,null,0.2,0.15134372134129692,0.31415999999999999,0.63788243539947065,942.48,0,-1570.8,0,0,0,0,0,6.2429285053284982E-2,8.0691780821917816E-2,1.4983028412788395,3.873205479452055,2.4657591906616361,724.98461538461538,115.38488520403808,1000.0023384349968,144999.73818288595,39440.446845974628,-125267.96769999999,0.80336771726611289,101211.85651283685,28294.233606894839,-139049.973925,1.0406414395817347,57660.830371723016,7047.1481372654825,-152757.43111383496,1.5676869976420578,null,331]
["IC/ICD","IC44-100A3AC",4015,19.8,5000,27.6,"NA",3.5,32.1,117.37972567696688,25,330,32,3.3395886533147787,1.8751663268992775,2.2934190777148711,null,0.2,0.15134372134129692,0.31415999999999999,0.31320517598479586,942.48,0,-1570.8,0,0,0,0,0,0.12485857010656996,0.16138356164383563,2.996605682557679,7.7464109589041099,4.9315183813232721,724.98461538461538,115.38488520403808,1000.0023384349968,36473.997367194221,9819.7594298434815,-146665.32999999999,1.8751663268992775,25458.501480564511,7044.6100257572807,-150062.13250000001,2.2934190777148711,14502.590141193143,1754.5769611755677,-153440.5611618023,3.1927952558757959,null,166]
["IC/ICD","IC44-100A5AC",4015,39.5,5000,55.1,"NA",0.88,8,58.619152160364791,25,330,32,6.6872342153227171,3.9622112652486687,4.7774353463996926,null,0.2,0.15134372134129692,0.31415999999999999,0.15485185574953039,942.48,0,-1570.8,0,0,0,0,0,0.24908654137421785,0.32195205479452055,5.9780769929812285,15.453698630136985,9.8381301041550113,724.98461538461538,115.38488520403808,1000.0023384349968,9054.4958108283699,2461.526045481266,-151900.68539200001,3.9622112652486687,6323.5269250249385,1764.6148601907444,-152757.80679999999,4.7774353463996926,3615.3176010133238,439.5065969185278,-153607.785062668,6.4577850563023214,null,82.9]
["IC/ICD","IC44-150A1AC",5990,9.8000000000000007,7500,13.8,"NA",19.8,191,351.43207024971412,36.200000000000003,330,32,1.1154360491956805,0.43530565090639239,0.62705087124055015,null,0.13812154696132595,0.13931539063347054,0.28763093333333334,0.96565019010563646,1294.3392000000001,0,-2157.232,0,0,0,0,0,5.6887117842000477E-2,7.3528358375069561E-2,1.3652908282080114,3.5293612020033391,2.2468611250223391,995.64553846153854,158.46190901354564,1373.3365447840622,324388.77906188124,83160.348231770899,-97668.926799999987,0.43530565090639239,224811.61069682357,59055.899468938755,-125425.35879999999,0.62705087124055015,128829.75290959937,13539.837216325088,-152179.62338340236,1.0355716907077974,null,497]
["IC/ICD","IC44-150A3AC",5990,19.600000000000001,7500,27.6,"NA",5,47.7,176.06958851545033,36.200000000000003,330,32,2.2263924355431857,1.1875297179780133,1.4859502066178909,null,0.13812154696132595,0.13931539063347054,0.28763093333333334,0.47055789457139097,1294.3392000000001,0,-2157.232,0,0,0,0,0,0.11377423568400095,0.14705671675013912,2.7305816564160228,7.0587224040066783,4.4937222500446783,995.64553846153854,158.46190901354564,1373.3365447840622,81116.449815707674,21042.341635378889,-139381,1.1875297179780133,56274.265071941642,14943.112175848777,-146461,1.4859502066178909,32329.026596604515,3426.0303913023058,-153285.37113136475,2.1251370161600476,null,249]
["IC/ICD","IC44-150A5AC",5990,39.200000000000003,7500,55.3,"NA",1.2,11.9,87.681240867131891,36.200000000000003,330,32,4.4707396487923647,2.6058226659392627,3.1721464681068507,null,0.13812154696132595,0.13931539063347054,0.28763093333333334,0.23118396259358645,1294.3392000000001,0,-2157.232,0,0,0,0,0,0.22754847136800191,0.29411343350027824,5.4611633128320456,14.117444808013357,8.9874445000893566,995.64553846153854,158.46190901354564,1373.3365447840622,20209.755770210184,5038.9923192638416,-150361.2628,2.6058226659392627,13979.976621595761,3571.9439225161414,-152004.42879999999,3.1721464681068507,8018.7405233533582,818.94509594503302,-153576.76390866644,4.325559562096295,null,124]
["IC/ICD","IC44-200A1AC",8035,9.9,10000,13.8,"NA",25.5,253,468.81179592668099,47.4,330,32,0.83615643506825532,0.22418030508421027,0.40159962505704838,null,0.10548523206751055,0.13209126802783694,0.27436639999999995,1.303888994345477,1646.1984,0,-2743.6639999999998,0,0,0,0,0,5.4487648061482735E-2,7.0426969508400744E-2,1.3077035534755856,3.3804945364032357,2.1520896622548804,1266.3064615384615,201.53893282305319,1746.6707511331276,572252.95805959147,142872.4292604551,-60788.792499999996,0.22418030508421027,401182.49188416591,102495.43838250039,-105865.748125,0.40159962505704838,228356.51275279137,22280.744784975876,-151405.28026237868,0.76693645267094035,null,663]
["IC/ICD","IC44-200A3AC",8035,19.8,10000,27.6,"NA",6.4,63.3,234.75945135393377,47.4,330,32,1.6697943266573894,0.83614663792263533,1.0656479481230972,null,0.10548523206751055,0.13209126802783694,0.27436639999999995,0.63012452843666633,1646.1984,0,-2743.6639999999998,0,0,0,0,0,0.10897529612296547,0.14085393901680149,2.6154071069511713,6.7609890728064714,4.3041793245097608,1266.3064615384615,201.53893282305319,1746.6707511331276,143368.48517642182,35912.26305771331,-130262.7328,0.83614663792263533,100533.22512151387,25763.1452370552,-141620.5312,1.0656479481230972,57258.392674719631,5600.4644981654092,-153094.88251932047,1.5869878966321016,null,332]
["IC/ICD","IC44-200A5AC",8035,39.6,10000,55.2,"NA",1.6,15.8,117.37972567696688,47.4,330,32,3.3395886533147787,1.9111262061647123,2.3250882228925032,null,0.10548523206751055,0.13209126802783694,0.27436639999999995,0.3099307126917959,1646.1984,0,-2743.6639999999998,0,0,0,0,0,0.21795059224593094,0.28170787803360298,5.2308142139023426,13.521978145612943,8.6083586490195216,1266.3064615384615,201.53893282305319,1746.6707511331276,35772.46349606997,8978.0657644283274,-147813.6832,1.9111262061647123,25097.45687486777,6440.7863092637999,-150653.13279999999,2.3250882228925032,14312.904095013348,1400.1161245413523,-153521.72062983012,3.2265276045566642,null,166]
["IC/ICD","IC44-250A3AC",9620,19.8,12500,27.6,"NA",7.7,78.900000000000006,280.72139213105936,58.5,330,32,1.3964023084389252,0.63474604523083877,0.8389561992215282,null,8.5470085470085472E-2,0.13369875299815315,0.26598880000000003,0.76066911852927732,1994.9159999999999,0,-3324.86,0,0,0,0,0,0.11030147122347635,0.14256806133056135,2.6472353093634324,6.8432669438669445,4.3565590440551683,1534.5507692307692,244.23134034854732,2116.6716163540768,215922.10344933684,51666.131843525895,-119790.43719999999,0.63474604523083877,149372.11349542902,37064.833713833788,-136230.9613,0.8389561992215282,82220.84922509703,8155.3099258789643,-152820.02433887482,1.3146320464980348,null,397]
["IC/ICD","IC44-250A5AC",9620,39.5,12500,55,"NA",1.9,19.7,140.71424945612296,58.5,330,32,2.7857875198505191,1.5309956957204545,1.8825471690581554,null,8.5470085470085472E-2,0.13369875299815315,0.26598880000000003,0.37342705427935136,1994.9159999999999,0,-3324.86,0,0,0,0,0,0.22004586430946038,0.28441608194733198,5.2811007434270492,13.651971933471934,8.6911152646555134,1534.5507692307692,244.23134034854732,2116.6716163540768,53745.739312568672,12734.590986511894,-145473.8125,1.5309956957204545,37308.949466920749,9145.7517084949068,-149439.62312500001,1.8825471690581554,20648.126479147402,2012.3236020366917,-153459.48767559839,2.677899173453901,null,199]
["IC/ICD","IC55-030A1AC",1497,9.8000000000000007,1875,13.8,"NA",7.8,51.5,87.681240867131891,12,330,32,{"$f":"IF(G375=\"NA\",(UAC_V*0.98)/J375,(IF((UAC_V*0.98)/J375<G375,(UAC_V*0.98)/J375,G375)))","v":4.4707396487923647},{"$f":"IF(AO375<G375,IF(AO375<0,0,AO375),G375)","v":2.3733957644419301},{"$f":"IF(AS375<G375,IF(AS375<0,0,AS375),G375)","v":2.9622123114071859},null,{"$f":"IF(move1,Gewicht/K375,MAX(Gewicht,Gewicht2)/K375)","v":0.41666666666666669},{"$f":"IF(move1,IF(AccType=1,SQRT((V375^2*Ltime1+W375^2*Ltime2+X375^2*Ltime3+Y375^2*Ltime4)/ltime)/C375,SQRT((((V375-W375)*2/PI()+W375)^2*Ltime1+W375^2*Ltime2+((X375-W375)*2/PI()+W375)^2*Ltime3+Y375^2*Ltime4)/ltime)/C375),IF(AccType=1,SQRT((V375^2*Ltime1+W375^2*Ltime2+X375^2*Ltime3+Y375^2*Ltime4+Z375^2*Ltime5+AA375^2*Ltime6+AB375^2*Ltime7+AC375^2*Ltime8)/ltime)/C375,SQRT((((V375-W375)*2/PI()+W375)^2*Ltime1+W375^2*Ltime2+((X375-W375)*2/PI()+W375)^2*Ltime3+Y375^2*Ltime4+((Z375-AA375)*2/PI()+AA375)^2*Ltime5+AA375^2*Ltime6+((AB375-AA375)*2/PI()+AA375)^2*Ltime7+AC375^2*Ltime8)/ltime)/C375))","v":0.23001482298263684},{"$f":" IF(move1,MAX(ABS(V375),ABS(X375))/E375,MAX(ABS(V375),ABS(X375),ABS(Z375),ABS(AB375))/E375)","v":0.47473066666666669},{"$f":"IF(AW375>0,IF(move1,MAX(ABS(Lspeed1),ABS(Lspeed2))/MIN(AW375,G375),MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6))/MIN(AW375,G375)),\"NA\")","v":0.24631085044795734},{"$f":"((Gewicht+K375)*laccel1+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":534.072},0,{"$f":"((Gewicht+K375)*laccel3+(Ltorque+IF(laccel1>=0,IF(AND(Lspeed1=0,Lspeed2=0),0,LDryTorq),-LDryTorq)))/LWirkungsgrad","v":-890.12},0,{"$f":"((Gewicht2+K375)*laccel5+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"((Gewicht2+K375)*laccel7+(Ltorque2+IF(laccel5>=0,IF(AND(Lspeed1=0,Lspeed6=0),0,LDryTorq2),-LDryTorq2)))/LWirkungsgrad","v":0},0,{"$f":"AF375/Irms","v":9.3922719384576706E-2},{"$f":"AG375/Ipeak","v":0.12139801825873971},{"$f":"D375*S375","v":2.254145265229841},{"$f":"IF(move1,IF(MAX(ABS(V375),ABS(X375))<=C375,MAX(ABS(V375),ABS(X375))/C375*D375,D375+(MAX(ABS(V375),ABS(X375))-C375)/(E375-C375)*(F375-D375)),IF(MAX(ABS(V375),ABS(X375),ABS(Z375),ABS(AB375))<=C375,MAX(ABS(V375),ABS(X375),ABS(Z375),ABS(AB375))/C375*D375,D375+(MAX(ABS(V375),ABS(X375),ABS(Z375),ABS(AB375))-C375)/(E375-C375)*(F375-D375)))","v":5.8271048764195061},{"$f":"IF(AccType=1,IF(move1,IF(MAX(ABS(V375),ABS(X375))<=C375,MAX(ABS(V375),ABS(X375))/C375*D375,D375+(MAX(ABS(V375),ABS(X375))-C375)/(E375-C375)*(F375-D375)),IF(MAX(ABS(V375),ABS(X375),ABS(Z375),ABS(AB375))<=C375,MAX(ABS(V375),ABS(X375),ABS(Z375),ABS(AB375))/C375*D375,D375+(MAX(ABS(V375),ABS(X375),ABS(Z375),ABS(AB375))-C375)/(E375-C375)*(F375-D375))),IF(move1,IF(MAX(ABS((V375-W375)*2/PI()+W375),ABS((X375-W375)*2/PI()+W375))<=C375,MAX(ABS((V375-W375)*2/PI()+W375),ABS((X375-W375)*2/PI()+W375))/C375*D375,D375+(MAX(ABS((V375-W375)*2/PI()+W375),ABS((X375-W375)*2/PI()+W375))-C375)/(E375-C375)*(F375-D375)),IF(MAX(ABS((V375-W375)*2/PI()+W375),ABS((X375-W375)*2/PI()+W375),ABS((Z375-AA375)*2/PI()+AA375),ABS((AB375-AA375)*2/PI()+AA375))<=C375,MAX(ABS((V375-W375)*2/PI()+W375),ABS((X375-W375)*2/PI()+W375),ABS((Z375-AA375)*2/PI()+AA375),ABS((AB375-AA375)*2/PI()+AA375))/C375*D375,D375+(MAX(ABS((V375-W375)*2/PI()+W375),ABS((X375-W375)*2/PI()+W375),ABS((Z375-AA375)*2/PI()+AA375),ABS((AB375-AA375)*2/PI()+AA375))-C375)/(E375-C375)*(F375-D375))))","v":3.7096501799882091},{"$f":"IF(move1,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V375)+Ltime2*ABS(Lspeed2)*ABS(W375)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X375)+Ltime4*ABS(Lspeed1)*ABS(Y375))/ltime,(Ltime1*ABS(Lspeed2-Lspeed1)*ABS(V375)+Ltime2*ABS(Lspeed2)*ABS(W375)+Ltime3*ABS(Lspeed2-Lspeed1)*ABS(X375)+Ltime4*ABS(Lspeed1)*ABS(Y375)+Ltime5*ABS(Lspeed6-Lspeed1)*ABS(Z375)+Ltime6*ABS(Lspeed6)*ABS(AA375)+Ltime7*ABS(Lspeed6-Lspeed1)*ABS(AB375)+Ltime8*ABS(Lspeed1)*ABS(AC375))/ltime)","v":410.82461538461536},{"$f":"IF(move1,IF(Lspeed1>Lspeed2,AK375/2*Ltime1/ltime,AK375/2*Ltime3/ltime),IF(Lspeed1>Lspeed2,MAX(IF(AccType=1,X375*-ABS(Lspeed2-Lspeed1),((X375-Y375)*2/PI()+Y375)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V375*-ABS(Lspeed2-Lspeed1),((V375-W375)*2/PI()+W375)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime1/ltime,MAX(IF(AccType=1,X375*-ABS(Lspeed2-Lspeed1),((X375-Y375)*2/PI()+Y375)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V375*-ABS(Lspeed2-Lspeed1),((V375-W375)*2/PI()+W375)*-ABS(Lspeed2-Lspeed1)),0)/2*Ltime3/ltime)+IF(Lspeed1>Lspeed6,MAX(IF(AccType=1,AB375*-ABS(Lspeed6-Lspeed1),((AB375-AC375)*2/PI()+AB375)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z375*-ABS(Lspeed6-Lspeed1),((Z375-AA375)*2/PI()+AA375)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime5/ltime,MAX(IF(AccType=1,AB375*-ABS(Lspeed6-Lspeed1),((AB375-AC375)*2/PI()+AB375)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z375*-ABS(Lspeed6-Lspeed1),((Z375-AA375)*2/PI()+AA375)*-ABS(Lspeed6-Lspeed1)),0)/2*Ltime7/ltime))","v":65.384768282288249},{"$f":"IF(move1,MAX(IF(AccType=1,X375*-ABS(Lspeed2-Lspeed1),((X375-Y375)*2/PI()+Y375)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V375*-ABS(Lspeed2-Lspeed1),((V375-W375)*2/PI()+W375)*-ABS(Lspeed2-Lspeed1)),0),MAX(IF(AccType=1,X375*-ABS(Lspeed2-Lspeed1),((X375-Y375)*2/PI()+Y375)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,V375*-ABS(Lspeed2-Lspeed1),((V375-W375)*2/PI()+W375)*-ABS(Lspeed2-Lspeed1)),IF(AccType=1,AB375*-ABS(Lspeed6-Lspeed1),((AB375-AC375)*2/PI()+AB375)*-ABS(Lspeed6-Lspeed1)),IF(AccType=1,Z375*-ABS(Lspeed6-Lspeed1),((Z375-AA375)*2/PI()+AA375)*-ABS(Lspeed6-Lspeed1)),0))","v":566.66799177983148},{"$f":"(J375^2)+3*(I375/1000)^2*(F375/2)^2*(2000*PI()/M375)^2","v":22292.734769931594},{"$f":"SQRT(3)*H375*F375/2*J375","v":8173.5553533086195},{"$f":"3*F375^2*H375^2/4-(UAC_V*0.98)^2","v":-144974.22279999999},{"$f":"-AM375/2/AL375+SQRT((AM375/2/AL375)^2-AN375/AL375)","v":2.3733957644419301},{"$f":"(J375^2)+3*(I375/1000)^2*(D375/2)^2*(2000*PI()/M375)^2","v":15053.252716363319},{"$f":"SQRT(3)*H375*D375/2*J375","v":5804.40887408873},{"$f":"3*D375^2*H375^2/4-(UAC_V*0.98)^2","v":-149281.6948},{"$f":"-AQ375/2/AP375+SQRT((AQ375/2/AP375)^2-AR375/AP375)","v":2.9622123114071859},{"$f":"(J375^2)+3*(I375/1000)^2*(AH375/2)^2*(2000*PI()/M375)^2","v":8743.3619126373887},{"$f":"SQRT(3)*H375*AH375/2*J375","v":2197.1761657641237},{"$f":"3*AH375^2*H375^2/4-(UAC_V*0.98)^2","v":-153036.06255158663},{"$f":"IF((AU375/2/AT375)^2-AV375/AT375>=0,-AU375/2/AT375+SQRT((AU375/2/AT375)^2-AV375/AT375),-9999)","v":4.0599104675304938},null,124]
["IC/ICD","IC55-030A3AC",1497,49.2,1875,69.099999999999994,"NA",0.31,2.1,17.53624817342638,12,330,32,22.353698243961823,12.758583176082865,15.595934263014147,null,0.41666666666666669,0.23001482298263684,0.47473066666666669,4.8134381345161119E-2,534.072,0,-890.12,0,0,0,0,0,0.47153038711440559,0.60946760187040749,11.316729290745734,29.25444488977956,18.623958046471415,410.82461538461536,65.384768282288249,566.66799177983148,916.37759473294477,325.31722263698236,-153319.85556925001,12.758583176082865,616.18674236552988,231.62962885296,-153489.53237199999,15.595934263014147,351.7486417228713,87.680091261733153,-153639.0006555552,20.775170928846446,null,24.8]
["IC/ICD","IC55-030A5AC",1497,17,1875,23.9,"NA",2.6,17.2,50.699556211075453,12,330,32,7.7318231025139932,4.3173473323805203,5.3048080368486188,null,0.41666666666666669,0.23001482298263684,0.47473066666666669,0.14046865464706526,534.072,0,-890.12,0,0,0,0,0,0.16292716627936776,0.21058839902026275,3.9102519907048263,10.108243152972612,6.4351074550815861,410.82461538461536,65.384768282288249,566.66799177983148,7456.6731251581023,2728.3874201515987,-150767.96530000001,4.3173473323805203,5042.6004737674266,1940.69398086097,-152198.76999999999,5.3048080368486188,2924.678429538099,734.62201789825815,-153454.04821765068,7.1190259671280511,null,71.7]
["IC/ICD","IC55-050A1AC",2511,9.9,3125,13.9,"NA",10.6,82.5,146.37110370561533,17.3,330,32,2.6781242340591946,1.371187645794032,1.7335100786548703,null,0.28901734104046239,0.17988164633522302,0.37364095999999997,0.4018498616548955,700.57680000000005,0,-1167.6279999999999,0,0,0,0,0,7.4201179113279503E-2,9.5907317801672623E-2,1.7808282987187081,4.6035512544802861,2.9307117517097336,538.90523076923068,85.769431335001642,743.33507157001429,59448.564771208068,18676.979617811601,-137382.19330000001,1.371187645794032,40713.038834563951,13302.309224196752,-145404.6973,1.7335100786548703,23114.844216958798,3937.9024210333541,-152940.19895551447,2.4884915870862976,null,207]
["IC/ICD","IC55-050A3AC",2511,49.5,3125,69.5,"NA",0.42,3.3,29.274220741123063,17.3,330,32,13.390621170295974,7.8678649749005221,9.5430757496323082,null,0.28901734104046239,0.17988164633522302,0.37364095999999997,7.8085844102332214E-2,700.57680000000005,0,-1167.6279999999999,0,0,0,0,0,0.37100589556639751,0.47953658900836316,8.9041414935935403,23.017756272401432,14.653558758548668,538.90523076923068,85.769431335001642,743.33507157001429,2377.9425908483222,740.03126787555391,-153024.957925,7.8678649749005221,1628.5215533825581,527.07262963798439,-153339.83192500001,9.5430757496323082,924.59376867835181,156.03009592773665,-153635.59164643841,12.806418519206771,null,41.4]
["IC/ICD","IC55-050A5AC",2511,17.100000000000001,3125,24.1,"NA",3.5,27.5,84.852813742385692,17.3,330,32,4.6197643037521114,2.5788078367876368,3.1747435610949224,null,0.28901734104046239,0.17988164633522302,0.37364095999999997,0.22918183421568139,700.57680000000005,0,-1167.6279999999999,0,0,0,0,0,0.12816567301384643,0.16565809438470727,3.0759761523323141,7.9515885304659495,5.0621384802259044,538.90523076923068,85.769431335001642,743.33507157001429,19900.491152266877,6198.4337941128315,-148327.80812500001,2.5788078367876368,13594.088631108894,4398.0588331671961,-150977.483125,3.1747435610949224,7760.3436752269281,1301.9639098054445,-153428.56805243946,4.3633475725606905,null,120]
["IC/ICD","IC55-075A1AC",3773,9.9,4690,13.9,"NA",14.1,122,219.91020894901627,23.9,330,32,1.7825457120586923,0.84273102790721421,1.1011172706177108,null,0.20920502092050211,0.15514569918062882,0.32264477611940295,0.60117060338278638,907.92239999999993,0,-1513.204,0,0,0,0,0,6.3997600912009386E-2,8.2718877551020406E-2,1.5359424218882254,3.9705061224489797,2.5277027038575572,698.40184615384612,111.15410607989003,963.33558602571361,131512.04160582711,37325.869711997831,-124854.939925,0.84273102790721421,90540.938863346179,26584.612240919319,-139049.973925,1.1011172706177108,51110.246708250037,6787.6763881188363,-152711.31028939266,1.6634213222885499,null,311]
["IC/ICD","IC55-075A3AC",3773,49.5,4690,69.599999999999994,"NA",0.56000000000000005,4.9000000000000004,43.982041789803255,23.9,330,32,8.9127285602934609,5.2275297744466611,6.3455694320757665,null,0.20920502092050211,0.15514569918062882,0.32264477611940295,0.11626508926689794,907.92239999999993,0,-1513.204,0,0,0,0,0,0.31998800456004695,0.41359438775510204,7.6797121094411267,19.852530612244898,12.638513519287786,698.40184615384612,111.15410607989003,963.33558602571361,5297.4572889526371,1484.5789049388516,-152524.65356800001,5.2275297744466611,3635.4955460711872,1055.8427556677177,-153087.70120000001,6.3455694320757665,2045.3132720792187,269.58147357067719,-153626.43102796056,8.6010341221551183,null,62.2]
["IC/ICD","IC55-075A5AC",3773,17.2,4690,24.1,"NA",4.7,40.5,127.27922061357854,23.9,330,32,3.0798428691680737,1.6774651045994617,2.0758154865267908,null,0.20920502092050211,0.15514569918062882,0.32264477611940295,0.3415805832160802,907.92239999999993,0,-1513.204,0,0,0,0,0,0.11118775107945066,0.14371360544217687,2.6685060259068156,6.8982530612244899,4.3915642935707053,698.40184615384612,111.15410607989003,963.33558602571361,43746.420644635698,12485.416642427277,-144041.43032499999,1.6774651045994617,30230.979293588309,8910.7537862966437,-148762.67079999999,2.0758154865267908,17114.680837035943,2275.1248928314135,-153344.48189642091,2.9275668733413069,null,180]
["IC/ICD","IC55-100A1AC",5001,9.9,6250,13.8,"NA",17.7,161,292.74220741123065,31.2,330,32,1.3390621170295973,0.56814055348601133,0.77710055500213238,null,0.16025641025641027,0.14661568013669343,0.30326912,0.80454879650780275,1137.2592000000002,0,-1895.432,0,0,0,0,0,6.047896805638605E-2,7.8170935812837433E-2,1.4514952333532651,3.7522049190161968,2.3887278414206103,874.81476923076934,139.23109481287264,1206.6694883782295,228433.16070181807,61925.329733224673,-108916.7893,0.56814055348601133,159156.6909282986,44424.693069487264,-130634.83532499999,0.77710055500213238,89974.673921635927,10719.040523398933,-152323.27058108395,1.2429326901495175,null,414]
["IC/ICD","IC55-100A3AC",5001,49.3,6250,69.2,"NA",0.71,6.4,58.619152160364791,31.2,330,32,6.6872342153227171,3.9486480481191251,4.7795021085346345,null,0.16025641025641027,0.14661568013669343,0.30326912,0.15457040138167441,1137.2592000000002,0,-1895.432,0,0,0,0,0,0.30117304294745773,0.38927546823968534,7.2281530307389854,18.685222475504897,11.895382078993544,874.81476923076934,139.23109481287264,1206.6694883782295,9107.642890307905,2494.2191401292189,-151853.53493200001,3.9486480481191251,6314.7619760964408,1776.9509191961054,-152745.09249325001,4.7795021085346345,3603.7910187003749,428.7527407597658,-153610.502344095,6.4695439169543247,null,82.9]
["IC/ICD","IC55-100A5AC",5001,17.100000000000001,6250,24,"NA",5.9,53.5,168.99852070358486,31.2,330,32,2.3195469307541976,1.219420211239699,1.5296039673041788,null,0.16025641025641027,0.14661568013669343,0.30326912,0.45404372686588368,1137.2592000000002,0,-1895.432,0,0,0,0,0,0.10446367209739409,0.13502252549490104,2.507128130337458,6.4810812237552495,4.1259844533628725,874.81476923076934,139.23109481287264,1206.6694883782295,76231.151894967887,20724.152917791354,-138626.07999999999,1.219420211239699,52760.804376054795,14765.958953926342,-146029.905925,1.5296039673041788,29969.411720489912,3562.813864496748,-153219.55250667705,2.2024310453591665,null,239]
["IC/ICD","IC55-150A3AC",7446,48.9,9375,68.7,"NA",1,9.5,87.681240867131891,45.1,330,32,4.4707396487923647,2.6121619315247302,3.1715051242889793,null,0.11086474501108647,0.13628353730586393,0.27981183999999998,0.230991642875396,1573.9416000000001,0,-2623.2359999999999,0,0,0,0,0,0.27767770726069774,0.35890702054794521,6.6642649742567457,17.22753698630137,10.967390674673265,1210.7243076923078,192.69275829074363,1670.0039051864446,20004.341667731191,5216.6783052053343,-150124.23250000001,2.6121619315247302,13928.019865562252,3713.1815010850191,-151870.5925,3.1715051242889793,8001.8881222220461,832.79983984394926,-153573.78725634181,4.329160949512926,null,124]
["IC/ICD","IC55-150A5AC",7446,16.899999999999999,9375,23.8,"NA",8.3000000000000007,79.5,253.85133444597054,45.1,330,32,1.5442109093321819,0.74098533054688376,0.96709018545067582,null,0.11086474501108647,0.13628353730586393,0.27981183999999998,0.68524165975613938,1573.9416000000001,0,-2623.2359999999999,0,0,0,0,0,9.5966324186212495E-2,0.1240394406392694,2.3031917804691,5.9538931506849311,3.7903661022899424,1210.7243076923078,192.69275829074363,1670.0039051864446,167956.91306393326,43427.53029009766,-124397.4613,0.74098533054688376,116635.47693522696,30837.195878262621,-138907.245325,0.96709018545067582,67066.033836845425,6916.2285175527686,-152921.69947615225,1.4593391772996922,null,359]
["IC/ICD","IC55-200A3AC",10033,49.4,12500,69.400000000000006,"NA",1.3,12.7,117.37972567696688,59,330,32,3.3395886533147787,1.895281603451112,2.3200756214276872,null,8.4745762711864403E-2,0.12920456704827291,0.26808320000000002,0.30967153156488764,2010.624,0,-3351.04,0,0,0,0,0,0.2659460671743617,0.34374351307352402,6.3827056121846812,16.499688627529153,10.504028018193582,1546.6338461538462,246.15442176861461,2133.33832199466,36239.94845424097,9171.2080306467797,-147559.26370000001,1.895281603451112,25159.051360320133,6528.2085981837299,-150570.8437,2.3200756214276872,14292.564982974984,1388.10700453308,-153524.15088866063,3.2292280628659049,null,166]
["IC/ICD","IC55-200A5AC",10033,17.100000000000001,12500,24,"NA",10.6,106,338.70414818835621,59,330,32,1.1573522264097147,0.47933629488432139,0.66777108327924461,null,8.4745762711864403E-2,0.12920456704827291,0.26808320000000002,0.92110675475126103,2010.624,0,-3351.04,0,0,0,0,0,9.2058254021894451E-2,0.11898813914083524,2.2093980965254669,5.7114306787600917,3.6360096986054709,1546.6338461538462,246.15442176861461,2133.33832199466,301855.60164795502,74622.235320043837,-105124.48000000001,0.47933629488432139,209720.80394596967,53168.342665531236,-129022.6093,0.66777108327924461,119015.69455056751,11305.298806470795,-152549.9028586557,1.0856504903929878,null,479]
["IC/ICD","IC55-250A3AC",12023,49.4,15625,69.400000000000006,"NA",1.5,15.8,140.71424945612296,73,330,32,2.7857875198505191,1.5210276882767864,1.8821846834520592,null,6.8493150684931503E-2,0.13140456683704552,0.26138112000000002,0.37300298442286123,2450.4479999999999,0,-4084.08,0,0,0,0,0,0.27047440007291867,0.34959652333028363,6.4913856017500482,16.780633119853615,10.682882836945103,1884.9599999999998,300.00070153049904,2600.0060799309917,54566.454567032786,12685.846140630512,-145536.39249999999,1.5210276882767864,37415.762332384649,9029.9826995266158,-149545.89249999999,1.8821846834520592,20624.281715264104,1952.7580404591922,-153471.41577411792,2.680943696864186,null,199]
["IC/ICD","IC55-250A5AC",12023,17.100000000000001,15625,24,"NA",12.9,131,405.87929240107826,73,330,32,0.96580438405967473,0.32204519672380888,0.50242607151553897,null,6.8493150684931503E-2,0.13140456683704552,0.26138112000000002,1.1190357486407188,2450.4479999999999,0,-4084.08,0,0,0,0,0,9.3625753871394934E-2,0.1210141811527905,2.2470180929134784,5.808680695333944,3.6979209820194594,1884.9599999999998,300.00070153049904,2600.0060799309917,450553.72440197191,108824.9504964739,-81774.880000000005,0.32204519672380888,309834.13884093857,77537.777228737672,-117169.038925,0.50242607151553897,171523.45365247509,16767.752825339161,-151957.30491561347,0.89362650050696746,null,574]

{"sheet":"Hilfe","index":5,"n_rows":8,"n_cols":8,"rows_kept":8,"cut":false,"hidden":true,"merged":[[0,0,0,8]]}
[]
[]
[]
[null,null,null,null,null,"Farben:"]
[]
[null,null,null,null,null,"Eingabefelder",null,"2. Fahrsatz"]
[]
[null,null,null,null,null,"Ergebnisfelder"]

{"sheet":"Help","index":6,"n_rows":8,"n_cols":8,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,0,0,8]]}
[]
[]
[]
[null,null,null,null,null,"Colours:"]
[]
[null,null,null,null,null,"Input cells",null,"2. Motion task"]
[]
[null,null,null,null,null,"result cells"]

{"sheet":"Changes","index":7,"n_rows":24,"n_cols":4,"rows_kept":24,"cut":false,"hidden":true,"merged":[]}
["Version","Date","Name","Description"]
["V1.0","2003-10-15","M. Scholz","Initial version"]
["V1.1","2003-10-15","M. Scholz","Error in Lmin Check solved\nJext/Jmot and Gext/Gmot calculation error corrected\nOther motorlinie: no motor curves displayed "]
["V1.2","2003-10-29","M. Scholz","New feature: Lmax-Check \nIrms and Ipeak calculation correction"]
["V1.3","2003-11-07","M. Scholz","KT=Mo/Io not Mn/In because In data in some datasheets not correct\nCorrection working curve with 2 motion tasks and different load\nDry friction added\nClearInput, OpenDom and SaveDim added"]
["V1.4","2003-12-02","M. Scholz","Power Calculation corrected\nMotor curve correction (nn-knee, nmax(M=0) limited by mechanical, nmax(Mmax)\nlimited by voltage)\nwL-losses in speed curve and % calculation\nInertia formula correction\nSpeed calculation only with 2% losses (prev. 15 %)\nKe Baumüler Peak->RMS"]
["V1.5","2003-12-19","M. Scholz","Calculation error Inertia2/3 Cylinder Material corrected\nLmax of SR620 wrong type (text)"]
["V1.6","2004-02-10","M. Scholz","Calculation error of Trms (^3) corrected, appeared only with 2 motion tasks.\nWorking point calculation corrected (load and dry friction and sine2)\nTrms calculation error (load and dry friction an sine2)\nAdd Goldline BH and Bautz MWF Motor series to database\nLinMotor: wL and pol pitch added\nAdd L3S LinMotorLine\nFormat 3123 -> 3.1k"]
["V1.7","2004-04-09","M. Scholz","Error if you load Dim with different Inertia type "]
["V1.7-V2.16",null,"H. Goergen","diverses"]
["V2.17","2009-10-08","R.Fetzner","AKD Drives included"]
["V2.18","2009-12-10","R.Fetzner","fieldlength"]
["V2.19","2010-06-11","R.Fetzner","AKM8 Motors added"]
["V2.20","2010-06-14","R.Fetzner","AKM8 Data corrected"]
["V2.22","2011-03-29","R.Fetzner","Kollmorgen Logo, S700 min/max motorinductance + power internal brakeresistor "]
["V2.23","2011-05-25","R.Fetzner","Cart.DDR from Motor Database V6.2 included"]
["V2.24","2011-05-26","R.Fetzner","KBM from Motor Database V6.2 included"]
["V2.25","2011-05-27","R.Fetzner","Speicherproblem active.shape gelöst"]
["V2.26","2012-03-26","A.Schwalb","Aktualisierung von Mmax "]
["V2.29","2015-03-12","N. Will","AKMH and ICH motors added, Bautz motors deleted"]
["V2.30","2015-05-16","G.Schilling","Logik, Layout, PDF, DE_EN_Texte, Userform other L+R-Motors, 100% skalierung bei Start, Motorselektion check"]
["V2.33","2015-11-09","G.Schilling","Berechnung der Massenträgheit überarbeitet, da Formelfehler"]
["V2.34","2015-11-12","G.Schilling","Inertia / Zahnstange / Formel in H14 war falsch"]
["V2.35","2016-01-28","G.Schilling","Verbesserte AKMH-Werte, PDF-Druck der Drehmomentenkurve hinzugefügt"]

{"sheet":"Calc","index":8,"n_rows":201,"n_cols":26,"rows_kept":201,"cut":false,"hidden":true,"merged":[]}
["AC-Voltage","Selected",null,null,null,null,null,null,null,null,0,{"$f":"IF(ABS(MIN($O$1:$O$100))>MAX($O$1:$O$100),O1/MIN($O$1:$O$100)*-1,O1/MAX($O$1:$O$100))","v":0},{"$f":"IF(ABS(MIN($P$1:$P$100))>MAX($P$1:$P$100),P1/MIN($P$1:$P$100)*-1,P1/MAX($P$1:$P$100))","v":1},{"$f":"IF(ABS(MIN($Q$1:$Q$100))>MAX($Q$1:$Q$100),Q1/MIN($Q$1:$Q$100)*-1,Q1/MAX($Q$1:$Q$100))","v":0},0,{"$f":"IF($A$90=TRUE,(Main!$E$46),Lspeed1)","v":2000},0,null,null,0,0,{"$f":"IF($A$90=TRUE,Main!$E$46,Lspeed1)","v":2000},{"$f":"IF(move1,IF(ABS(MIN($U$1:$U$101))>MAX($U$1:$U$101),U1/MIN($U$1:$U$101)*-1,U1/MAX($U$1:$U$101)),IF(ABS(MIN($U$1:$U$201))>MAX($U$1:$U$201),U1/MIN($U$1:$U$201)*-1,U1/MAX($U$1:$U$201)))","v":0},{"$f":"IF(move1,IF(ABS(MIN($V$1:$V$101))>MAX($V$1:$V$101),V1/MIN($V$1:$V$101)*-1,V1/MAX($V$1:$V$101)),IF(ABS(MIN($V$1:$V$201))>MAX($V$1:$V$201),V1/MIN($V$1:$V$201)*-1,V1/MAX($V$1:$V$201)))","v":1},{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W1*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W1>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W1*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W1>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W1*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W1>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W1*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W1>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W1*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W1>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W1*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W1>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":9},{"$f":"IF(move1,ABS(IF($A$90=TRUE,X1*speed,X1*MAX(ABS(Lspeed1),ABS(Lspeed2)))),ABS(IF($A$90=TRUE,X1*speed,X1*MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6)))))","v":127.32395447351627}]
[50,"400",null,null,null,null,null,null,null,null,1,{"$f":"IF(ABS(MIN($O$1:$O$100))>MAX($O$1:$O$100),O2/MIN($O$1:$O$100)*-1,O2/MAX($O$1:$O$100))","v":-0.87463256218361252},{"$f":"IF(ABS(MIN($P$1:$P$100))>MAX($P$1:$P$100),P2/MIN($P$1:$P$100)*-1,P2/MAX($P$1:$P$100))","v":0.6131352617568846},{"$f":"IF(ABS(MIN($Q$1:$Q$100))>MAX($Q$1:$Q$100),Q2/MIN($Q$1:$Q$100)*-1,Q2/MAX($Q$1:$Q$100))","v":3.7046415323823224E-2},{"$f":"IF($A$90=TRUE,(IF(K2<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K2*PI()*Main!$D$45/100/Main!$D$46))),(IF(K2<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K2<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K2-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K2<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R2)))))))),(IF(K2<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K2*PI()*Main!$D$71/100/Main!$D$72))),(IF(K2<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K2<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K2-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K2<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R2)))))))))","v":-31186.194134874277},{"$f":"IF($A$90=TRUE,(IF(K2<=(Main!$D$46/Main!$D$45*100),O2*Main!$D$45/100000+P1,IF(K2<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K2<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O2*Main!$D$45/100000+P1,IF(K2<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S2))))),(IF(K2<=(Main!$D$72/Main!$D$71*100),O2*Main!$D$71/100000+P1,IF(K2<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K2<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O2*Main!$D$71/100000+P1,IF(K2<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S2))))))","v":1226.2705235137691},{"$f":"IF($A$90=TRUE,P2*Main!$D$45/100000+Q1,P2*100+Q1)","v":30.423771688376615},{"$f":"IF($A$90=TRUE,(IF(K2<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K2-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K2<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K2<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K2-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K2<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K2-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K2<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K2<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K2-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":1765841.1398624675},{"$f":"IF($A$90=TRUE,(IF(K2<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O2*Main!$D$45/100000+P1,IF(K2<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K2<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O2*Main!$D$45/100000+P1,Main!$E$52)))),(IF(K2<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O2*Main!$D$71/100000+P1,IF(K2<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K2<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O2*Main!$D$71/100000+P1,Main!$E$78)))))","v":1226.2705235137691},9.9999999999999995E-7,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T2*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T2*PI()/50))))","v":-2.3882061557795888E-3},{"$f":"IF($A$90=TRUE,U2*2*Main!$D$46/100000*(T2-T1)+V1,U2*2*Ltime1*(T2-T1)/100000+V1)","v":1999.9999999999961},{"$f":"IF(move1,IF(ABS(MIN($U$1:$U$101))>MAX($U$1:$U$101),U2/MIN($U$1:$U$101)*-1,U2/MAX($U$1:$U$101)),IF(ABS(MIN($U$1:$U$201))>MAX($U$1:$U$201),U2/MIN($U$1:$U$201)*-1,U2/MAX($U$1:$U$201)))","v":-6.2831853071795822E-8},{"$f":"IF(move1,IF(ABS(MIN($V$1:$V$101))>MAX($V$1:$V$101),V2/MIN($V$1:$V$101)*-1,V2/MAX($V$1:$V$101)),IF(ABS(MIN($V$1:$V$201))>MAX($V$1:$V$201),V2/MIN($V$1:$V$201)*-1,V2/MAX($V$1:$V$201)))","v":0.99999999999999811},{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W2*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W2>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W2*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W2>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W2*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W2>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W2*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W2>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W2*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W2>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W2*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W2>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad))),0)","v":5.9999980623687392},{"$f":"IF(move1,ABS(IF($A$90=TRUE,X2*speed,X2*MAX(ABS(Lspeed1),ABS(Lspeed2)))),ABS(IF($A$90=TRUE,X2*speed,X2*MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6)))))","v":127.32395447351603}]
[115,null,null,null,null,null,null,null,null,null,2,-1,0.17081839068445759,4.7367480578022744E-2,{"$f":"IF($A$90=TRUE,(IF(K3<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K3*PI()*Main!$D$45/100/Main!$D$46))),(IF(K3<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K3<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K3-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K3<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R1)))))))),(IF(K3<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K3*PI()*Main!$D$71/100/Main!$D$72))),(IF(K3<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K3<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K3-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K3<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R1)))))))))","v":-35656.337853480611},{"$f":"IF($A$90=TRUE,(IF(K3<=(Main!$D$46/Main!$D$45*100),O3*Main!$D$45/100000+P2,IF(K3<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K3<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O3*Main!$D$45/100000+P2,IF(K3<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S3))))),(IF(K3<=(Main!$D$72/Main!$D$71*100),O3*Main!$D$71/100000+P2,IF(K3<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K3<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O3*Main!$D$71/100000+P2,IF(K3<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S3))))))","v":341.63678136891519},{"$f":"IF($A$90=TRUE,P3*Main!$D$45/100000+Q2,P3*100+Q2)","v":38.899780234139399},{"$f":"IF($A$90=TRUE,(IF(K3<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K3-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K3<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K3<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K3-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K3<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K3-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K3<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K3<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K3-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2920985.8080664333},{"$f":"IF($A$90=TRUE,(IF(K3<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O3*Main!$D$45/100000+P2,IF(K3<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K3<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O3*Main!$D$45/100000+P2,Main!$E$52)))),(IF(K3<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O3*Main!$D$71/100000+P2,IF(K3<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K3<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O3*Main!$D$71/100000+P2,Main!$E$78)))))","v":341.63678136891519},9.9999999999999995E-7,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T3*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T3*PI()/50))))","v":-2.3882061557795888E-3},{"$f":"IF($A$90=TRUE,U3*2*Main!$D$46/100000*(T3-T2)+V2,U3*2*Ltime1*(T3-T2)/100000+V2)","v":1999.9999999999961},-6.2831853071795822E-8,0.99999999999999811,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W3*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W3>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W3*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W3>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W3*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W3>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W3*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W3>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W3*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W3>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W3*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W3>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":5.9999980623687392},{"$f":"IF(move1,ABS(IF($A$90=TRUE,X3*speed,X3*MAX(ABS(Lspeed1),ABS(Lspeed2)))),ABS(IF($A$90=TRUE,X3*speed,X3*MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6)))))","v":127.32395447351603}]
[230,null,null,null,null,null,null,null,null,null,3,-0.26870470107056443,5.1965768064473707E-2,5.0507318630757837E-2,{"$f":"IF($A$90=TRUE,(IF(K4<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K4*PI()*Main!$D$45/100/Main!$D$46))),(IF(K4<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K4<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K4-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K4<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R4)))))))),(IF(K4<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K4*PI()*Main!$D$71/100/Main!$D$72))),(IF(K4<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K4<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K4-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K4<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R4)))))))))","v":-9581.0256041905595},{"$f":"IF($A$90=TRUE,(IF(K4<=(Main!$D$46/Main!$D$45*100),O4*Main!$D$45/100000+P3,IF(K4<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K4<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O4*Main!$D$45/100000+P3,IF(K4<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S4))))),(IF(K4<=(Main!$D$72/Main!$D$71*100),O4*Main!$D$71/100000+P3,IF(K4<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K4<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O4*Main!$D$71/100000+P3,IF(K4<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S4))))))","v":103.93153612894741},{"$f":"IF($A$90=TRUE,P4*Main!$D$45/100000+Q3,P4*100+Q3)","v":41.478321645498582},{"$f":"IF($A$90=TRUE,(IF(K4<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K4-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K4<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K4<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K4-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K4<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K4-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K4<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K4<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K4-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":3065940.0993068451},{"$f":"IF($A$90=TRUE,(IF(K4<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O4*Main!$D$45/100000+P3,IF(K4<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K4<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O4*Main!$D$45/100000+P3,Main!$E$52)))),(IF(K4<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O4*Main!$D$71/100000+P3,IF(K4<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K4<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O4*Main!$D$71/100000+P3,Main!$E$78)))))","v":103.93153612894741},1,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T4*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T4*PI()/50))))","v":-2386.635089262038},{"$f":"IF($A$90=TRUE,U4*2*Main!$D$46/100000*(T4-T3)+V3,U4*2*Ltime1*(T4-T3)/100000+V3)","v":1996.1336550217404},-6.2790519529313374E-2,0.99806682751087017,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W4*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W4>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W4*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W4>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W4*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W4>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W4*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W4>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W4*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W4>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W4*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W4>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":4.0636433975787334},127.07781530752085]
[400,null,null,null,null,null,null,null,null,null,4,0,0.02,5.171574416536729E-2,{"$f":"IF($A$90=TRUE,(IF(K5<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K5*PI()*Main!$D$45/100/Main!$D$46))),(IF(K5<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K5<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K5-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K5<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R5)))))))),(IF(K5<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K5*PI()*Main!$D$71/100/Main!$D$72))),(IF(K5<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K5<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K5-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K5<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R5)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K5<=(Main!$D$46/Main!$D$45*100),O5*Main!$D$45/100000+P4,IF(K5<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K5<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O5*Main!$D$45/100000+P4,IF(K5<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S5))))),(IF(K5<=(Main!$D$72/Main!$D$71*100),O5*Main!$D$71/100000+P4,IF(K5<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K5<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O5*Main!$D$71/100000+P4,IF(K5<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S5))))))","v":40},{"$f":"IF($A$90=TRUE,P5*Main!$D$45/100000+Q4,P5*100+Q4)","v":42.470721645498585},{"$f":"IF($A$90=TRUE,(IF(K5<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K5-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K5<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K5<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K5-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K5<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K5-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K5<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K5<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K5-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2150573.1879858854},{"$f":"IF($A$90=TRUE,(IF(K5<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O5*Main!$D$45/100000+P4,IF(K5<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K5<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O5*Main!$D$45/100000+P4,Main!$E$52)))),(IF(K5<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O5*Main!$D$71/100000+P4,IF(K5<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K5<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O5*Main!$D$71/100000+P4,Main!$E$78)))))","v":103.93153612894741},2,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T5*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T5*PI()/50))))","v":-4763.8512201766162},{"$f":"IF($A$90=TRUE,U5*2*Main!$D$46/100000*(T5-T4)+V4,U5*2*Ltime1*(T5-T4)/100000+V4)","v":1988.4162160450544},-0.12533323356430426,0.99420810802252724,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W5*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W5>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W5*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W5>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W5*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W5>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W5*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W5>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W5*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W5>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W5*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W5>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":2.1349287100300391},126.586507883061]
[480,null,null,null,null,null,null,null,null,null,5,0,0.02,5.2924169699976736E-2,{"$f":"IF($A$90=TRUE,(IF(K6<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K6*PI()*Main!$D$45/100/Main!$D$46))),(IF(K6<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K6<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K6-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K6<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R6)))))))),(IF(K6<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K6*PI()*Main!$D$71/100/Main!$D$72))),(IF(K6<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K6<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K6-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K6<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R6)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K6<=(Main!$D$46/Main!$D$45*100),O6*Main!$D$45/100000+P5,IF(K6<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K6<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O6*Main!$D$45/100000+P5,IF(K6<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S6))))),(IF(K6<=(Main!$D$72/Main!$D$71*100),O6*Main!$D$71/100000+P5,IF(K6<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K6<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O6*Main!$D$71/100000+P5,IF(K6<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S6))))))","v":40},{"$f":"IF($A$90=TRUE,P6*Main!$D$45/100000+Q5,P6*100+Q5)","v":43.463121645498589},{"$f":"IF($A$90=TRUE,(IF(K6<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K6-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K6<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K6<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K6-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K6<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K6-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K6<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K6<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K6-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":491454.5153709022},{"$f":"IF($A$90=TRUE,(IF(K6<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O6*Main!$D$45/100000+P5,IF(K6<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K6<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O6*Main!$D$45/100000+P5,Main!$E$52)))),(IF(K6<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O6*Main!$D$71/100000+P5,IF(K6<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K6<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O6*Main!$D$71/100000+P5,Main!$E$78)))))","v":40},4,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T6*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T6*PI()/50))))","v":-9452.5736608242678},{"$f":"IF($A$90=TRUE,U6*2*Main!$D$46/100000*(T6-T5)+V5,U6*2*Ltime1*(T6-T5)/100000+V5)","v":1957.7898773839838},-0.24868988716485479,0.97889493869199196,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W6*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W6>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W6*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W6>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W6*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W6>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W6*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W6>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W6*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W6>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W6*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W6>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":1.6691880968154225},124.63677460837468]
[null,null,null,null,null,null,null,null,null,null,6,0,0.02,5.4132595234586182E-2,{"$f":"IF($A$90=TRUE,(IF(K7<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K7*PI()*Main!$D$45/100/Main!$D$46))),(IF(K7<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K7<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K7-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K7<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R7)))))))),(IF(K7<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K7*PI()*Main!$D$71/100/Main!$D$72))),(IF(K7<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K7<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K7-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K7<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R7)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K7<=(Main!$D$46/Main!$D$45*100),O7*Main!$D$45/100000+P6,IF(K7<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K7<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O7*Main!$D$45/100000+P6,IF(K7<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S7))))),(IF(K7<=(Main!$D$72/Main!$D$71*100),O7*Main!$D$71/100000+P6,IF(K7<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K7<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O7*Main!$D$71/100000+P6,IF(K7<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S7))))))","v":40},{"$f":"IF($A$90=TRUE,P7*Main!$D$45/100000+Q6,P7*100+Q6)","v":44.455521645498592},{"$f":"IF($A$90=TRUE,(IF(K7<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K7-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K7<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K7<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K7-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K7<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K7-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K7<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K7<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K7-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":1337628.2223802856},{"$f":"IF($A$90=TRUE,(IF(K7<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O7*Main!$D$45/100000+P6,IF(K7<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K7<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O7*Main!$D$45/100000+P6,Main!$E$52)))),(IF(K7<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O7*Main!$D$71/100000+P6,IF(K7<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K7<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O7*Main!$D$71/100000+P6,Main!$E$78)))))","v":40},6,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T7*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T7*PI()/50))))","v":-13992.223368146919},{"$f":"IF($A$90=TRUE,U7*2*Main!$D$46/100000*(T7-T6)+V6,U7*2*Ltime1*(T7-T6)/100000+V6)","v":1912.4550736711878},-0.36812455268467792,0.95622753683559392,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W7*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W7>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W7*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W7>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W7*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W7>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W7*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W7>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W7*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W7>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W7*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W7>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":5.3523572260231997},121.75067136637776]
[null,null,null,null,null,null,null,null,null,null,7,0,0.02,5.5341020769195635E-2,{"$f":"IF($A$90=TRUE,(IF(K8<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K8*PI()*Main!$D$45/100/Main!$D$46))),(IF(K8<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K8<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K8-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K8<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R8)))))))),(IF(K8<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K8*PI()*Main!$D$71/100/Main!$D$72))),(IF(K8<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K8<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K8-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K8<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R8)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K8<=(Main!$D$46/Main!$D$45*100),O8*Main!$D$45/100000+P7,IF(K8<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K8<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O8*Main!$D$45/100000+P7,IF(K8<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S8))))),(IF(K8<=(Main!$D$72/Main!$D$71*100),O8*Main!$D$71/100000+P7,IF(K8<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K8<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O8*Main!$D$71/100000+P7,IF(K8<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S8))))))","v":40},{"$f":"IF($A$90=TRUE,P8*Main!$D$45/100000+Q7,P8*100+Q7)","v":45.447921645498596},{"$f":"IF($A$90=TRUE,(IF(K8<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K8-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K8<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K8<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K8-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K8<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K8-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K8<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K8<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K8-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2704107.1520337844},{"$f":"IF($A$90=TRUE,(IF(K8<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O8*Main!$D$45/100000+P7,IF(K8<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K8<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O8*Main!$D$45/100000+P7,Main!$E$52)))),(IF(K8<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O8*Main!$D$71/100000+P7,IF(K8<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K8<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O8*Main!$D$71/100000+P7,Main!$E$78)))))","v":40},7,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T8*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T8*PI()/50))))","v":-16183.650097940934},{"$f":"IF($A$90=TRUE,U8*2*Main!$D$46/100000*(T8-T7)+V7,U8*2*Ltime1*(T8-T7)/100000+V7)","v":1886.2375605125235},-0.42577929156507266,0.94311878025626172,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W8*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W8>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W8*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W8>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W8*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W8>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W8*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W8>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W8*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W8>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W8*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W8>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":7.1303347794627445},120.08161264046646]
["Massenträgheit",1,2,3,4,null,null,null,null,null,8,0,0.02,5.6549446303805082E-2,{"$f":"IF($A$90=TRUE,(IF(K9<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K9*PI()*Main!$D$45/100/Main!$D$46))),(IF(K9<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K9<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K9-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K9<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R9)))))))),(IF(K9<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K9*PI()*Main!$D$71/100/Main!$D$72))),(IF(K9<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K9<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K9-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K9<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R9)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K9<=(Main!$D$46/Main!$D$45*100),O9*Main!$D$45/100000+P8,IF(K9<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K9<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O9*Main!$D$45/100000+P8,IF(K9<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S9))))),(IF(K9<=(Main!$D$72/Main!$D$71*100),O9*Main!$D$71/100000+P8,IF(K9<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K9<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O9*Main!$D$71/100000+P8,IF(K9<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S9))))))","v":40},{"$f":"IF($A$90=TRUE,P9*Main!$D$45/100000+Q8,P9*100+Q8)","v":46.440321645498599},{"$f":"IF($A$90=TRUE,(IF(K9<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K9-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K9<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K9<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K9-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K9<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K9-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K9<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K9<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K9-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":3135400.7700304859},{"$f":"IF($A$90=TRUE,(IF(K9<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O9*Main!$D$45/100000+P8,IF(K9<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K9<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O9*Main!$D$45/100000+P8,Main!$E$52)))),(IF(K9<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O9*Main!$D$71/100000+P8,IF(K9<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K9<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O9*Main!$D$71/100000+P8,Main!$E$78)))))","v":40},8,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T9*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T9*PI()/50))))","v":-18311.207354404814},{"$f":"IF($A$90=TRUE,U9*2*Main!$D$46/100000*(T9-T8)+V8,U9*2*Ltime1*(T9-T8)/100000+V8)","v":1856.5734045983877},-0.48175367410171532,0.92828670229919386,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W9*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W9>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W9*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W9>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W9*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W9>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W9*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W9>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W9*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W9>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W9*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W9>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":8.8564929002071064},118.19313382191311]
[{"$f":"IF(deutsch,\"Nicht benutzt\",\"Not used\")","v":"Nicht benutzt"},"Zahnstange","Nicht benutzt","Nicht benutzt",null,null,null,null,null,null,9,0,0.02,5.7757871838414528E-2,{"$f":"IF($A$90=TRUE,(IF(K10<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K10*PI()*Main!$D$45/100/Main!$D$46))),(IF(K10<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K10<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K10-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K10<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R10)))))))),(IF(K10<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K10*PI()*Main!$D$71/100/Main!$D$72))),(IF(K10<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K10<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K10-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K10<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R10)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K10<=(Main!$D$46/Main!$D$45*100),O10*Main!$D$45/100000+P9,IF(K10<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K10<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O10*Main!$D$45/100000+P9,IF(K10<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S10))))),(IF(K10<=(Main!$D$72/Main!$D$71*100),O10*Main!$D$71/100000+P9,IF(K10<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K10<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O10*Main!$D$71/100000+P9,IF(K10<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S10))))))","v":40},{"$f":"IF($A$90=TRUE,P10*Main!$D$45/100000+Q9,P10*100+Q9)","v":47.432721645498603},{"$f":"IF($A$90=TRUE,(IF(K10<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K10-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K10<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K10<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K10-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K10<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K10-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K10<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K10<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K10-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2482350.9868799951},{"$f":"IF($A$90=TRUE,(IF(K10<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O10*Main!$D$45/100000+P9,IF(K10<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K10<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O10*Main!$D$45/100000+P9,Main!$E$52)))),(IF(K10<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O10*Main!$D$71/100000+P9,IF(K10<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K10<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O10*Main!$D$71/100000+P9,Main!$E$78)))))","v":40},9,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T10*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T10*PI()/50))))","v":-20366.498641035749},{"$f":"IF($A$90=TRUE,U10*2*Main!$D$46/100000*(T10-T9)+V9,U10*2*Ltime1*(T10-T9)/100000+V9)","v":1823.5796767999097},-0.53582679497899666,0.91178983839995487,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W10*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W10>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W10*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W10>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W10*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W10>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W10*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W10>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W10*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W10>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W10*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W10>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":10.524019230760338},116.09268787385061]
[{"$f":"IF(deutsch,\"Zylinder\",\"Cylinder\")","v":"Zylinder"},null,null,null,null,null,null,null,null,null,10,0,0.02,5.8966297373023974E-2,{"$f":"IF($A$90=TRUE,(IF(K11<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K11*PI()*Main!$D$45/100/Main!$D$46))),(IF(K11<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K11<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K11-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K11<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R11)))))))),(IF(K11<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K11*PI()*Main!$D$71/100/Main!$D$72))),(IF(K11<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K11<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K11-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K11<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R11)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K11<=(Main!$D$46/Main!$D$45*100),O11*Main!$D$45/100000+P10,IF(K11<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K11<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O11*Main!$D$45/100000+P10,IF(K11<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S11))))),(IF(K11<=(Main!$D$72/Main!$D$71*100),O11*Main!$D$71/100000+P10,IF(K11<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K11<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O11*Main!$D$71/100000+P10,IF(K11<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S11))))))","v":40},{"$f":"IF($A$90=TRUE,P11*Main!$D$45/100000+Q10,P11*100+Q10)","v":48.425121645498606},{"$f":"IF($A$90=TRUE,(IF(K11<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K11-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K11<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K11<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K11-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K11<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K11-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K11<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K11<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K11-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":970807.78952923184},{"$f":"IF($A$90=TRUE,(IF(K11<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O11*Main!$D$45/100000+P10,IF(K11<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K11<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O11*Main!$D$45/100000+P10,Main!$E$52)))),(IF(K11<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O11*Main!$D$71/100000+P10,IF(K11<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K11<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O11*Main!$D$71/100000+P10,Main!$E$78)))))","v":40},10,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T11*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T11*PI()/50))))","v":-22341.412662098679},{"$f":"IF($A$90=TRUE,U11*2*Main!$D$46/100000*(T11-T10)+V10,U11*2*Ltime1*(T11-T10)/100000+V10)","v":1787.3865882873099},-0.58778525229247314,0.89369329414365495,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W11*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W11>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W11*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W11>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W11*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W11>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W11*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W11>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W11*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W11>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W11*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W11>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":12.126332806516061},113.7885642968335]
["Block",null,null,null,null,null,null,null,null,null,11,0,0.02,6.0174722907633427E-2,{"$f":"IF($A$90=TRUE,(IF(K12<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K12*PI()*Main!$D$45/100/Main!$D$46))),(IF(K12<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K12<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K12-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K12<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R12)))))))),(IF(K12<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K12*PI()*Main!$D$71/100/Main!$D$72))),(IF(K12<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K12<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K12-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K12<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R12)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K12<=(Main!$D$46/Main!$D$45*100),O12*Main!$D$45/100000+P11,IF(K12<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K12<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O12*Main!$D$45/100000+P11,IF(K12<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S12))))),(IF(K12<=(Main!$D$72/Main!$D$71*100),O12*Main!$D$71/100000+P11,IF(K12<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K12<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O12*Main!$D$71/100000+P11,IF(K12<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S12))))))","v":40},{"$f":"IF($A$90=TRUE,P12*Main!$D$45/100000+Q11,P12*100+Q11)","v":49.41752164549861},{"$f":"IF($A$90=TRUE,(IF(K12<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K12-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K12<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K12<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K12-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K12<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K12-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K12<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K12<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K12-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":876478.4587318555},{"$f":"IF($A$90=TRUE,(IF(K12<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O12*Main!$D$45/100000+P11,IF(K12<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K12<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O12*Main!$D$45/100000+P11,Main!$E$52)))),(IF(K12<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O12*Main!$D$71/100000+P11,IF(K12<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K12<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O12*Main!$D$71/100000+P11,Main!$E$78)))))","v":40},11,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T12*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T12*PI()/50))))","v":-24228.155334204861},{"$f":"IF($A$90=TRUE,U12*2*Main!$D$46/100000*(T12-T11)+V11,U12*2*Ltime1*(T12-T11)/100000+V11)","v":1748.1369766458981},-0.63742398974868963,0.87406848832294903,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W12*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W12>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W12*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W12>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W12*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W12>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W12*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W12>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W12*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W12>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W12*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W12>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":13.657110027818209},111.28985641396635]
[{"$f":"IF(deutsch,\"Spindel\",\"Spindle\")","v":"Spindel"},null,null,null,null,null,null,null,null,null,12,0,0.02,6.1383148442242873E-2,{"$f":"IF($A$90=TRUE,(IF(K13<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K13*PI()*Main!$D$45/100/Main!$D$46))),(IF(K13<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K13<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K13-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K13<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R13)))))))),(IF(K13<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K13*PI()*Main!$D$71/100/Main!$D$72))),(IF(K13<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K13<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K13-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K13<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R13)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K13<=(Main!$D$46/Main!$D$45*100),O13*Main!$D$45/100000+P12,IF(K13<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K13<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O13*Main!$D$45/100000+P12,IF(K13<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S13))))),(IF(K13<=(Main!$D$72/Main!$D$71*100),O13*Main!$D$71/100000+P12,IF(K13<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K13<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O13*Main!$D$71/100000+P12,IF(K13<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S13))))))","v":40},{"$f":"IF($A$90=TRUE,P13*Main!$D$45/100000+Q12,P13*100+Q12)","v":50.409921645498613},{"$f":"IF($A$90=TRUE,(IF(K13<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K13-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K13<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K13<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K13-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K13<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K13-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K13<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K13<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K13-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2420644.4035018892},{"$f":"IF($A$90=TRUE,(IF(K13<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O13*Main!$D$45/100000+P12,IF(K13<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K13<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O13*Main!$D$45/100000+P12,Main!$E$52)))),(IF(K13<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O13*Main!$D$71/100000+P12,IF(K13<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K13<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O13*Main!$D$71/100000+P12,Main!$E$78)))))","v":40},12,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T13*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T13*PI()/50))))","v":-26019.280545998234},{"$f":"IF($A$90=TRUE,U13*2*Main!$D$46/100000*(T13-T12)+V12,U13*2*Ltime1*(T13-T12)/100000+V12)","v":1705.985742161381},-0.68454710592868862,0.85299287108069055,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W13*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W13>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W13*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W13>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W13*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W13>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W13*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W13>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W13*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W13>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W13*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W13>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":15.110309616319896},108.60642548371177]
[{"$f":"IF(deutsch,\"Zahnstange\",\"Rack\")","v":"Zahnstange"},null,null,null,null,null,null,null,null,null,13,0,0.02,6.2591573976852319E-2,{"$f":"IF($A$90=TRUE,(IF(K14<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K14*PI()*Main!$D$45/100/Main!$D$46))),(IF(K14<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K14<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K14-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K14<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R14)))))))),(IF(K14<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K14*PI()*Main!$D$71/100/Main!$D$72))),(IF(K14<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K14<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K14-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K14<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R14)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K14<=(Main!$D$46/Main!$D$45*100),O14*Main!$D$45/100000+P13,IF(K14<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K14<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O14*Main!$D$45/100000+P13,IF(K14<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S14))))),(IF(K14<=(Main!$D$72/Main!$D$71*100),O14*Main!$D$71/100000+P13,IF(K14<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K14<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O14*Main!$D$71/100000+P13,IF(K14<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S14))))))","v":40},{"$f":"IF($A$90=TRUE,P14*Main!$D$45/100000+Q13,P14*100+Q13)","v":51.402321645498617},{"$f":"IF($A$90=TRUE,(IF(K14<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K14-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K14<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K14<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K14-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K14<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K14-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K14<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K14<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K14-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":3127657.4679969233},{"$f":"IF($A$90=TRUE,(IF(K14<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O14*Main!$D$45/100000+P13,IF(K14<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K14<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O14*Main!$D$45/100000+P13,Main!$E$52)))),(IF(K14<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O14*Main!$D$71/100000+P13,IF(K14<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K14<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O14*Main!$D$71/100000+P13,Main!$E$78)))))","v":40},13,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T14*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T14*PI()/50))))","v":-27707.719544555115},{"$f":"IF($A$90=TRUE,U14*2*Main!$D$46/100000*(T14-T13)+V13,U14*2*Ltime1*(T14-T13)/100000+V13)","v":1661.0992364992017},-0.72896862742141155,0.83054961824960083,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W14*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W14>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W14*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W14>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W14*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W14>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W14*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W14>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W14*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W14>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W14*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W14>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":16.480196457149049},105.74886178200849]
[null,null,null,null,null,null,null,null,null,null,14,0,0.02,6.3799999511461772E-2,{"$f":"IF($A$90=TRUE,(IF(K15<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K15*PI()*Main!$D$45/100/Main!$D$46))),(IF(K15<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K15<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K15-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K15<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R15)))))))),(IF(K15<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K15*PI()*Main!$D$71/100/Main!$D$72))),(IF(K15<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K15<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K15-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K15<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R15)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K15<=(Main!$D$46/Main!$D$45*100),O15*Main!$D$45/100000+P14,IF(K15<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K15<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O15*Main!$D$45/100000+P14,IF(K15<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S15))))),(IF(K15<=(Main!$D$72/Main!$D$71*100),O15*Main!$D$71/100000+P14,IF(K15<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K15<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O15*Main!$D$71/100000+P14,IF(K15<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S15))))))","v":40},{"$f":"IF($A$90=TRUE,P15*Main!$D$45/100000+Q14,P15*100+Q14)","v":52.39472164549862},{"$f":"IF($A$90=TRUE,(IF(K15<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K15-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K15<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K15<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K15-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K15<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K15-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K15<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K15<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K15-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2753005.0660264194},{"$f":"IF($A$90=TRUE,(IF(K15<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O15*Main!$D$45/100000+P14,IF(K15<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K15<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O15*Main!$D$45/100000+P14,Main!$E$52)))),(IF(K15<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O15*Main!$D$71/100000+P14,IF(K15<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K15<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O15*Main!$D$71/100000+P14,Main!$E$78)))))","v":40},14,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T15*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T15*PI()/50))))","v":-29286.808832522605},{"$f":"IF($A$90=TRUE,U15*2*Main!$D$46/100000*(T15-T14)+V14,U15*2*Ltime1*(T15-T14)/100000+V14)","v":1613.6546061905151},-0.77051324277578925,0.80682730309525752,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W15*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W15>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W15*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W15>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W15*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W15>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W15*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W15>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W15*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W15>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W15*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W15>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":17.761364232786676},102.72844280729048]
[null,null,null,null,null,null,null,null,null,null,15,0,0.02,6.5008425046071211E-2,{"$f":"IF($A$90=TRUE,(IF(K16<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K16*PI()*Main!$D$45/100/Main!$D$46))),(IF(K16<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K16<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K16-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K16<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R16)))))))),(IF(K16<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K16*PI()*Main!$D$71/100/Main!$D$72))),(IF(K16<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K16<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K16-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K16<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R16)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K16<=(Main!$D$46/Main!$D$45*100),O16*Main!$D$45/100000+P15,IF(K16<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K16<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O16*Main!$D$45/100000+P15,IF(K16<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S16))))),(IF(K16<=(Main!$D$72/Main!$D$71*100),O16*Main!$D$71/100000+P15,IF(K16<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K16<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O16*Main!$D$71/100000+P15,IF(K16<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S16))))))","v":40},{"$f":"IF($A$90=TRUE,P16*Main!$D$45/100000+Q15,P16*100+Q15)","v":53.387121645498624},{"$f":"IF($A$90=TRUE,(IF(K16<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K16-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K16<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K16<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K16-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K16<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K16-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K16<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K16<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K16-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":1426256.5539804322},{"$f":"IF($A$90=TRUE,(IF(K16<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O16*Main!$D$45/100000+P15,IF(K16<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K16<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O16*Main!$D$45/100000+P15,Main!$E$52)))),(IF(K16<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O16*Main!$D$71/100000+P15,IF(K16<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K16<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O16*Main!$D$71/100000+P15,Main!$E$78)))))","v":40},15,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T16*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T16*PI()/50))))","v":-30750.31646589837},{"$f":"IF($A$90=TRUE,U16*2*Main!$D$46/100000*(T16-T15)+V15,U16*2*Ltime1*(T16-T15)/100000+V15)","v":1563.8390935157597},-0.80901699437494734,0.78191954675787989,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W16*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W16>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W16*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W16>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W16*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W16>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W16*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W16>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W16*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W16>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W16*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W16>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":18.948756759332209},99.557088773352774]
[null,null,null,null,null,null,null,null,null,null,16,0,0.02,6.6216850580680664E-2,{"$f":"IF($A$90=TRUE,(IF(K17<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K17*PI()*Main!$D$45/100/Main!$D$46))),(IF(K17<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K17<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K17-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K17<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R17)))))))),(IF(K17<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K17*PI()*Main!$D$71/100/Main!$D$72))),(IF(K17<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K17<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K17-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K17<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R17)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K17<=(Main!$D$46/Main!$D$45*100),O17*Main!$D$45/100000+P16,IF(K17<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K17<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O17*Main!$D$45/100000+P16,IF(K17<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S17))))),(IF(K17<=(Main!$D$72/Main!$D$71*100),O17*Main!$D$71/100000+P16,IF(K17<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K17<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O17*Main!$D$71/100000+P16,IF(K17<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S17))))))","v":40},{"$f":"IF($A$90=TRUE,P17*Main!$D$45/100000+Q16,P17*100+Q16)","v":54.379521645498627},{"$f":"IF($A$90=TRUE,(IF(K17<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K17-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K17<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K17<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K17-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K17<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K17-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K17<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K17<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K17-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":393746.8865670127},{"$f":"IF($A$90=TRUE,(IF(K17<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O17*Main!$D$45/100000+P16,IF(K17<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K17<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O17*Main!$D$45/100000+P16,Main!$E$52)))),(IF(K17<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O17*Main!$D$71/100000+P16,IF(K17<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K17<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O17*Main!$D$71/100000+P16,Main!$E$78)))))","v":40},16,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T17*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T17*PI()/50))))","v":-32092.466648666519},{"$f":"IF($A$90=TRUE,U17*2*Main!$D$46/100000*(T17-T16)+V16,U17*2*Ltime1*(T17-T16)/100000+V16)","v":1511.8492975449199},-0.84432792550201508,0.75592464877245991,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W17*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W17>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W17*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W17>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W17*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W17>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W17*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W17>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W17*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W17>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W17*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W17>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":20.037687940951436},96.247315565713464]
[null,null,null,null,null,null,null,null,null,null,17,0,0.02,6.7425276115290117E-2,{"$f":"IF($A$90=TRUE,(IF(K18<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K18*PI()*Main!$D$45/100/Main!$D$46))),(IF(K18<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K18<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K18-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K18<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R18)))))))),(IF(K18<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K18*PI()*Main!$D$71/100/Main!$D$72))),(IF(K18<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K18<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K18-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K18<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R18)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K18<=(Main!$D$46/Main!$D$45*100),O18*Main!$D$45/100000+P17,IF(K18<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K18<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O18*Main!$D$45/100000+P17,IF(K18<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S18))))),(IF(K18<=(Main!$D$72/Main!$D$71*100),O18*Main!$D$71/100000+P17,IF(K18<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K18<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O18*Main!$D$71/100000+P17,IF(K18<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S18))))))","v":40},{"$f":"IF($A$90=TRUE,P18*Main!$D$45/100000+Q17,P18*100+Q17)","v":55.371921645498631},{"$f":"IF($A$90=TRUE,(IF(K18<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K18-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K18<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K18<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K18-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K18<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K18-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K18<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K18<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K18-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2077577.3561017755},{"$f":"IF($A$90=TRUE,(IF(K18<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O18*Main!$D$45/100000+P17,IF(K18<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K18<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O18*Main!$D$45/100000+P17,Main!$E$52)))),(IF(K18<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O18*Main!$D$71/100000+P17,IF(K18<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K18<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O18*Main!$D$71/100000+P17,Main!$E$78)))))","v":40},17,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T18*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T18*PI()/50))))","v":-33307.962527225754},{"$f":"IF($A$90=TRUE,U18*2*Main!$D$46/100000*(T18-T17)+V17,U18*2*Ltime1*(T18-T17)/100000+V17)","v":1457.8903982508141},-0.87630668004386369,0.72894519912540701,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W18*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W18>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W18*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W18>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W18*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W18>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W18*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W18>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W18*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W18>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W18*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W18>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":21.023860263755829},92.812185347131575]
["Material",null,1,null,2,null,2,null,4,null,18,0,0.02,6.8633701649899556E-2,{"$f":"IF($A$90=TRUE,(IF(K19<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K19*PI()*Main!$D$45/100/Main!$D$46))),(IF(K19<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K19<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K19-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K19<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R19)))))))),(IF(K19<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K19*PI()*Main!$D$71/100/Main!$D$72))),(IF(K19<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K19<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K19-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K19<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R19)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K19<=(Main!$D$46/Main!$D$45*100),O19*Main!$D$45/100000+P18,IF(K19<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K19<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O19*Main!$D$45/100000+P18,IF(K19<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S19))))),(IF(K19<=(Main!$D$72/Main!$D$71*100),O19*Main!$D$71/100000+P18,IF(K19<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K19<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O19*Main!$D$71/100000+P18,IF(K19<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S19))))))","v":40},{"$f":"IF($A$90=TRUE,P19*Main!$D$45/100000+Q18,P19*100+Q18)","v":56.364321645498634},{"$f":"IF($A$90=TRUE,(IF(K19<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K19-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K19<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K19<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K19-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K19<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K19-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K19<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K19<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K19-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":3042900.8590005939},{"$f":"IF($A$90=TRUE,(IF(K19<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O19*Main!$D$45/100000+P18,IF(K19<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K19<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O19*Main!$D$45/100000+P18,Main!$E$52)))),(IF(K19<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O19*Main!$D$71/100000+P18,IF(K19<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K19<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O19*Main!$D$71/100000+P18,Main!$E$78)))))","v":40},18,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T19*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T19*PI()/50))))","v":-34392.007094650646},{"$f":"IF($A$90=TRUE,U19*2*Main!$D$46/100000*(T19-T18)+V18,U19*2*Ltime1*(T19-T18)/100000+V18)","v":1402.1753467574799},-0.90482705246601958,0.70108767337874001,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W19*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W19>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W19*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W19>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W19*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W19>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W19*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W19>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W19*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W19>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W19*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W19>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":21.903381756126556},89.26525500721813]
[{"$f":"IF(deutsch,\"Stahl\",\"Steel\")","v":"Stahl"},1,"Aluminium",0.33,"Aluminium",0.33,"Aluminium",0.33,null,null,19,0,0.02,6.9842127184509009E-2,{"$f":"IF($A$90=TRUE,(IF(K20<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K20*PI()*Main!$D$45/100/Main!$D$46))),(IF(K20<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K20<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K20-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K20<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R20)))))))),(IF(K20<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K20*PI()*Main!$D$71/100/Main!$D$72))),(IF(K20<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K20<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K20-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K20<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R20)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K20<=(Main!$D$46/Main!$D$45*100),O20*Main!$D$45/100000+P19,IF(K20<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K20<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O20*Main!$D$45/100000+P19,IF(K20<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S20))))),(IF(K20<=(Main!$D$72/Main!$D$71*100),O20*Main!$D$71/100000+P19,IF(K20<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K20<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O20*Main!$D$71/100000+P19,IF(K20<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S20))))))","v":40},{"$f":"IF($A$90=TRUE,P20*Main!$D$45/100000+Q19,P20*100+Q19)","v":57.356721645498638},{"$f":"IF($A$90=TRUE,(IF(K20<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K20-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K20<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K20<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K20-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K20<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K20-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K20<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K20<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K20-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2955871.0237481403},{"$f":"IF($A$90=TRUE,(IF(K20<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O20*Main!$D$45/100000+P19,IF(K20<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K20<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O20*Main!$D$45/100000+P19,Main!$E$52)))),(IF(K20<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O20*Main!$D$71/100000+P19,IF(K20<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K20<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O20*Main!$D$71/100000+P19,Main!$E$78)))))","v":40},19,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T20*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T20*PI()/50))))","v":-35340.322122286416},{"$f":"IF($A$90=TRUE,U20*2*Main!$D$46/100000*(T20-T19)+V19,U20*2*Ltime1*(T20-T19)/100000+V19)","v":1344.9240249193758},-0.92977648588825135,0.67246201245968795,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W20*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W20>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W20*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W20>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W20*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W20>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W20*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W20>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W20*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W20>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W20*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W20>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":22.67278134854838},85.620522659586442]
["Aluminium",0.33,null,null,null,null,null,null,null,null,20,0,0.02,7.1050552719118448E-2,{"$f":"IF($A$90=TRUE,(IF(K21<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K21*PI()*Main!$D$45/100/Main!$D$46))),(IF(K21<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K21<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K21-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K21<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R21)))))))),(IF(K21<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K21*PI()*Main!$D$71/100/Main!$D$72))),(IF(K21<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K21<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K21-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K21<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R21)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K21<=(Main!$D$46/Main!$D$45*100),O21*Main!$D$45/100000+P20,IF(K21<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K21<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O21*Main!$D$45/100000+P20,IF(K21<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S21))))),(IF(K21<=(Main!$D$72/Main!$D$71*100),O21*Main!$D$71/100000+P20,IF(K21<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K21<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O21*Main!$D$71/100000+P20,IF(K21<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S21))))))","v":40},{"$f":"IF($A$90=TRUE,P21*Main!$D$45/100000+Q20,P21*100+Q20)","v":58.349121645498641},{"$f":"IF($A$90=TRUE,(IF(K21<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K21-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K21<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K21<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K21-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K21<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K21-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K21<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K21<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K21-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":1846586.1486034824},{"$f":"IF($A$90=TRUE,(IF(K21<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O21*Main!$D$45/100000+P20,IF(K21<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K21<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O21*Main!$D$45/100000+P20,Main!$E$52)))),(IF(K21<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O21*Main!$D$71/100000+P20,IF(K21<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K21<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O21*Main!$D$71/100000+P20,Main!$E$78)))))","v":40},20,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T21*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T21*PI()/50))))","v":-36149.16504396293},{"$f":"IF($A$90=TRUE,U21*2*Main!$D$46/100000*(T21-T20)+V20,U21*2*Ltime1*(T21-T20)/100000+V20)","v":1286.3623775481558},-0.95105651629515353,0.64318118877407793,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W21*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W21>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W21*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W21>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W21*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W21>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W21*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W21>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W21*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W21>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W21*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W21>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":23.329022572335255},81.892372397692768]
[{"$f":"IF(deutsch,\"Kupfer\",\"Copper\")","v":"Kupfer"},1.2,null,null,null,null,null,null,null,null,21,0,0.02,7.2258978253727901E-2,{"$f":"IF($A$90=TRUE,(IF(K22<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K22*PI()*Main!$D$45/100/Main!$D$46))),(IF(K22<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K22<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K22-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K22<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R22)))))))),(IF(K22<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K22*PI()*Main!$D$71/100/Main!$D$72))),(IF(K22<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K22<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K22-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K22<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R22)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K22<=(Main!$D$46/Main!$D$45*100),O22*Main!$D$45/100000+P21,IF(K22<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K22<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O22*Main!$D$45/100000+P21,IF(K22<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S22))))),(IF(K22<=(Main!$D$72/Main!$D$71*100),O22*Main!$D$71/100000+P21,IF(K22<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K22<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O22*Main!$D$71/100000+P21,IF(K22<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S22))))))","v":40},{"$f":"IF($A$90=TRUE,P22*Main!$D$45/100000+Q21,P22*100+Q21)","v":59.341521645498645},{"$f":"IF($A$90=TRUE,(IF(K22<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K22-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K22<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K22<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K22-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K22<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K22-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K22<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K22<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K22-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-98680.040721722442},{"$f":"IF($A$90=TRUE,(IF(K22<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O22*Main!$D$45/100000+P21,IF(K22<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K22<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O22*Main!$D$45/100000+P21,Main!$E$52)))),(IF(K22<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O22*Main!$D$71/100000+P21,IF(K22<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K22<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O22*Main!$D$71/100000+P21,Main!$E$78)))))","v":40},21,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T22*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T22*PI()/50))))","v":-36815.343726193496},{"$f":"IF($A$90=TRUE,U22*2*Main!$D$46/100000*(T22-T21)+V21,U22*2*Ltime1*(T22-T21)/100000+V21)","v":1226.7215207117224},-0.96858316112863108,0.61336076035586118,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W22*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W22>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W22*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W22>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W22*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W22>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W22*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W22>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W22*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W22>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W22*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W22>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":23.869515543184992},78.095517527390996]
[{"$f":"IF(deutsch,\"Messing\",\"Brass\")","v":"Messing"},1.1000000000000001,null,null,null,null,null,null,null,null,22,0,0.02,7.3467403788337354E-2,{"$f":"IF($A$90=TRUE,(IF(K23<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K23*PI()*Main!$D$45/100/Main!$D$46))),(IF(K23<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K23<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K23-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K23<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R23)))))))),(IF(K23<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K23*PI()*Main!$D$71/100/Main!$D$72))),(IF(K23<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K23<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K23-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K23<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R23)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K23<=(Main!$D$46/Main!$D$45*100),O23*Main!$D$45/100000+P22,IF(K23<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K23<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O23*Main!$D$45/100000+P22,IF(K23<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S23))))),(IF(K23<=(Main!$D$72/Main!$D$71*100),O23*Main!$D$71/100000+P22,IF(K23<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K23<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O23*Main!$D$71/100000+P22,IF(K23<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S23))))))","v":40},{"$f":"IF($A$90=TRUE,P23*Main!$D$45/100000+Q22,P23*100+Q22)","v":60.333921645498648},{"$f":"IF($A$90=TRUE,(IF(K23<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K23-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K23<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K23<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K23-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K23<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K23-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K23<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K23<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K23-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-1683353.4591067731},{"$f":"IF($A$90=TRUE,(IF(K23<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O23*Main!$D$45/100000+P22,IF(K23<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K23<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O23*Main!$D$45/100000+P22,Main!$E$52)))),(IF(K23<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O23*Main!$D$71/100000+P22,IF(K23<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K23<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O23*Main!$D$71/100000+P22,Main!$E$78)))))","v":40},22,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T23*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T23*PI()/50))))","v":-37336.229066067448},{"$f":"IF($A$90=TRUE,U23*2*Main!$D$46/100000*(T23-T22)+V22,U23*2*Ltime1*(T23-T22)/100000+V22)","v":1166.2368296246932},-0.98228725072868861,0.58311841481234661,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W23*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W23>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W23*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W23>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W23*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W23>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W23*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W23>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W23*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W23>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W23*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W23>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":24.29212718226939},74.244942500236192]
[null,null,null,null,null,null,null,null,null,null,23,0,0.02,7.4675829322946793E-2,{"$f":"IF($A$90=TRUE,(IF(K24<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K24*PI()*Main!$D$45/100/Main!$D$46))),(IF(K24<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K24<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K24-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K24<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R24)))))))),(IF(K24<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K24*PI()*Main!$D$71/100/Main!$D$72))),(IF(K24<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K24<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K24-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K24<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R24)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K24<=(Main!$D$46/Main!$D$45*100),O24*Main!$D$45/100000+P23,IF(K24<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K24<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O24*Main!$D$45/100000+P23,IF(K24<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S24))))),(IF(K24<=(Main!$D$72/Main!$D$71*100),O24*Main!$D$71/100000+P23,IF(K24<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K24<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O24*Main!$D$71/100000+P23,IF(K24<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S24))))))","v":40},{"$f":"IF($A$90=TRUE,P24*Main!$D$45/100000+Q23,P24*100+Q23)","v":61.326321645498652},{"$f":"IF($A$90=TRUE,(IF(K24<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K24-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K24<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K24<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K24-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K24<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K24-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K24<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K24<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K24-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2883217.932049118},{"$f":"IF($A$90=TRUE,(IF(K24<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O24*Main!$D$45/100000+P23,IF(K24<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K24<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O24*Main!$D$45/100000+P23,Main!$E$52)))),(IF(K24<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O24*Main!$D$71/100000+P23,IF(K24<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K24<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O24*Main!$D$71/100000+P23,Main!$E$78)))))","v":40},23,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T24*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T24*PI()/50))))","v":-37709.765367118176},{"$f":"IF($A$90=TRUE,U24*2*Main!$D$46/100000*(T24-T23)+V23,U24*2*Ltime1*(T24-T23)/100000+V23)","v":1105.1470097299618},-0.99211470131447776,0.55257350486498091,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W24*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W24>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W24*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W24>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W24*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W24>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W24*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W24>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W24*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W24>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W24*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W24>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":24.595189634521876},70.355843776700155]
[null,null,null,null,null,null,null,null,null,null,24,0,0.02,7.5884254857556246E-2,{"$f":"IF($A$90=TRUE,(IF(K25<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K25*PI()*Main!$D$45/100/Main!$D$46))),(IF(K25<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K25<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K25-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K25<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R25)))))))),(IF(K25<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K25*PI()*Main!$D$71/100/Main!$D$72))),(IF(K25<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K25<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K25-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K25<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R25)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K25<=(Main!$D$46/Main!$D$45*100),O25*Main!$D$45/100000+P24,IF(K25<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K25<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O25*Main!$D$45/100000+P24,IF(K25<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S25))))),(IF(K25<=(Main!$D$72/Main!$D$71*100),O25*Main!$D$71/100000+P24,IF(K25<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K25<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O25*Main!$D$71/100000+P24,IF(K25<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S25))))))","v":40},{"$f":"IF($A$90=TRUE,P25*Main!$D$45/100000+Q24,P25*100+Q24)","v":62.318721645498655},{"$f":"IF($A$90=TRUE,(IF(K25<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K25-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K25<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K25<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K25-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K25<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K25-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K25<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K25<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K25-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-3085953.6268896475},{"$f":"IF($A$90=TRUE,(IF(K25<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O25*Main!$D$45/100000+P24,IF(K25<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K25<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O25*Main!$D$45/100000+P24,Main!$E$52)))),(IF(K25<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O25*Main!$D$71/100000+P24,IF(K25<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K25<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O25*Main!$D$71/100000+P24,Main!$E$78)))))","v":40},24,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T25*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T25*PI()/50))))","v":-37934.478452217932},{"$f":"IF($A$90=TRUE,U25*2*Main!$D$46/100000*(T25-T24)+V24,U25*2*Ltime1*(T25-T24)/100000+V24)","v":1043.6931546373687},-0.99802672842827145,0.52184657731868433,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W25*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W25>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W25*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W25>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W25*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W25>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W25*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W25>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W25*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W25>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W25*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W25>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":24.777506850899481},66.443569852684448]
[null,null,null,null,null,null,null,null,null,null,25,0,0.02,7.7092680392165699E-2,{"$f":"IF($A$90=TRUE,(IF(K26<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K26*PI()*Main!$D$45/100/Main!$D$46))),(IF(K26<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K26<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K26-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K26<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R26)))))))),(IF(K26<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K26*PI()*Main!$D$71/100/Main!$D$72))),(IF(K26<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K26<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K26-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K26<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R26)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K26<=(Main!$D$46/Main!$D$45*100),O26*Main!$D$45/100000+P25,IF(K26<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K26<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O26*Main!$D$45/100000+P25,IF(K26<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S26))))),(IF(K26<=(Main!$D$72/Main!$D$71*100),O26*Main!$D$71/100000+P25,IF(K26<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K26<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O26*Main!$D$71/100000+P25,IF(K26<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S26))))))","v":40},{"$f":"IF($A$90=TRUE,P26*Main!$D$45/100000+Q25,P26*100+Q25)","v":63.311121645498659},{"$f":"IF($A$90=TRUE,(IF(K26<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K26-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K26<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K26<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K26-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K26<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K26-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K26<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K26<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K26-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2221446.6637772238},{"$f":"IF($A$90=TRUE,(IF(K26<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O26*Main!$D$45/100000+P25,IF(K26<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K26<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O26*Main!$D$45/100000+P25,Main!$E$52)))),(IF(K26<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O26*Main!$D$71/100000+P25,IF(K26<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K26<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O26*Main!$D$71/100000+P25,Main!$E$78)))))","v":40},25,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T26*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T26*PI()/50))))","v":-38009.481481481482},{"$f":"IF($A$90=TRUE,U26*2*Main!$D$46/100000*(T26-T25)+V25,U26*2*Ltime1*(T26-T25)/100000+V25)","v":982.11779463736866},-1,0.49105889731868435,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W26*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W26>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W26*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W26>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W26*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W26>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W26*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W26>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W26*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W26>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W26*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W26>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":24.838359308641976},62.523560686019266]
[null,null,null,null,null,null,null,null,null,null,26,0,0.02,7.8301105926775139E-2,{"$f":"IF($A$90=TRUE,(IF(K27<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K27*PI()*Main!$D$45/100/Main!$D$46))),(IF(K27<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K27<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K27-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K27<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R27)))))))),(IF(K27<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K27*PI()*Main!$D$71/100/Main!$D$72))),(IF(K27<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K27<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K27-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K27<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R27)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K27<=(Main!$D$46/Main!$D$45*100),O27*Main!$D$45/100000+P26,IF(K27<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K27<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O27*Main!$D$45/100000+P26,IF(K27<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S27))))),(IF(K27<=(Main!$D$72/Main!$D$71*100),O27*Main!$D$71/100000+P26,IF(K27<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K27<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O27*Main!$D$71/100000+P26,IF(K27<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S27))))))","v":40},{"$f":"IF($A$90=TRUE,P27*Main!$D$45/100000+Q26,P27*100+Q26)","v":64.303521645498662},{"$f":"IF($A$90=TRUE,(IF(K27<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K27-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K27<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K27<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K27-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K27<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K27-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K27<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K27<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K27-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-588677.13790196448},{"$f":"IF($A$90=TRUE,(IF(K27<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O27*Main!$D$45/100000+P26,IF(K27<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K27<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O27*Main!$D$45/100000+P26,Main!$E$52)))),(IF(K27<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O27*Main!$D$71/100000+P26,IF(K27<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K27<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O27*Main!$D$71/100000+P26,Main!$E$78)))))","v":40},26,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T27*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T27*PI()/50))))","v":-37934.478452217932},{"$f":"IF($A$90=TRUE,U27*2*Main!$D$46/100000*(T27-T26)+V26,U27*2*Ltime1*(T27-T26)/100000+V26)","v":920.66393954477564},-0.99802672842827145,0.46033196977238783,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W27*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W27>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W27*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W27>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W27*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W27>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W27*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W27>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W27*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W27>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W27*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W27>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":24.777506850899481},58.611286762003573]
[null,null,null,null,null,null,null,null,null,null,27,0,0.02,7.9509531461384592E-2,{"$f":"IF($A$90=TRUE,(IF(K28<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K28*PI()*Main!$D$45/100/Main!$D$46))),(IF(K28<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K28<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K28-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K28<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R28)))))))),(IF(K28<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K28*PI()*Main!$D$71/100/Main!$D$72))),(IF(K28<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K28<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K28-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K28<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R28)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K28<=(Main!$D$46/Main!$D$45*100),O28*Main!$D$45/100000+P27,IF(K28<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K28<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O28*Main!$D$45/100000+P27,IF(K28<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S28))))),(IF(K28<=(Main!$D$72/Main!$D$71*100),O28*Main!$D$71/100000+P27,IF(K28<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K28<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O28*Main!$D$71/100000+P27,IF(K28<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S28))))))","v":40},{"$f":"IF($A$90=TRUE,P28*Main!$D$45/100000+Q27,P28*100+Q27)","v":65.295921645498666},{"$f":"IF($A$90=TRUE,(IF(K28<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K28-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K28<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K28<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K28-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K28<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K28-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K28<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K28<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K28-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-1247679.8132160387},{"$f":"IF($A$90=TRUE,(IF(K28<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O28*Main!$D$45/100000+P27,IF(K28<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K28<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O28*Main!$D$45/100000+P27,Main!$E$52)))),(IF(K28<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O28*Main!$D$71/100000+P27,IF(K28<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K28<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O28*Main!$D$71/100000+P27,Main!$E$78)))))","v":40},27,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T28*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T28*PI()/50))))","v":-37709.765367118176},{"$f":"IF($A$90=TRUE,U28*2*Main!$D$46/100000*(T28-T27)+V27,U28*2*Ltime1*(T28-T27)/100000+V27)","v":859.57411965004417},-0.99211470131447776,0.42978705982502208,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W28*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W28>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W28*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W28>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W28*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W28>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W28*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W28>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W28*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W28>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W28*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W28>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":24.595189634521876},54.722188038467522]
[null,null,null,null,null,null,null,null,null,null,28,0,0.02,8.0717956995994045E-2,{"$f":"IF($A$90=TRUE,(IF(K29<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K29*PI()*Main!$D$45/100/Main!$D$46))),(IF(K29<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K29<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K29-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K29<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R29)))))))),(IF(K29<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K29*PI()*Main!$D$71/100/Main!$D$72))),(IF(K29<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K29<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K29-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K29<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R29)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K29<=(Main!$D$46/Main!$D$45*100),O29*Main!$D$45/100000+P28,IF(K29<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K29<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O29*Main!$D$45/100000+P28,IF(K29<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S29))))),(IF(K29<=(Main!$D$72/Main!$D$71*100),O29*Main!$D$71/100000+P28,IF(K29<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K29<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O29*Main!$D$71/100000+P28,IF(K29<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S29))))))","v":40},{"$f":"IF($A$90=TRUE,P29*Main!$D$45/100000+Q28,P29*100+Q28)","v":66.288321645498669},{"$f":"IF($A$90=TRUE,(IF(K29<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K29-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K29<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K29<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K29-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K29<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K29-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K29<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K29<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K29-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2652540.6107558077},{"$f":"IF($A$90=TRUE,(IF(K29<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O29*Main!$D$45/100000+P28,IF(K29<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K29<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O29*Main!$D$45/100000+P28,Main!$E$52)))),(IF(K29<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O29*Main!$D$71/100000+P28,IF(K29<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K29<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O29*Main!$D$71/100000+P28,Main!$E$78)))))","v":40},28,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T29*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T29*PI()/50))))","v":-37336.229066067448},{"$f":"IF($A$90=TRUE,U29*2*Main!$D$46/100000*(T29-T28)+V28,U29*2*Ltime1*(T29-T28)/100000+V28)","v":799.08942856301485},-0.98228725072868861,0.39954471428150745,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W29*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W29>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W29*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W29>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W29*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W29>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W29*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W29>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W29*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W29>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W29*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W29>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":24.29212718226939},50.871613011312718]
["Bewegung",1.5708,null,null,null,null,null,null,null,null,29,0,0.02,8.1926382530603484E-2,{"$f":"IF($A$90=TRUE,(IF(K30<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K30*PI()*Main!$D$45/100/Main!$D$46))),(IF(K30<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K30<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K30-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K30<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R30)))))))),(IF(K30<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K30*PI()*Main!$D$71/100/Main!$D$72))),(IF(K30<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K30<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K30-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K30<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R30)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K30<=(Main!$D$46/Main!$D$45*100),O30*Main!$D$45/100000+P29,IF(K30<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K30<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O30*Main!$D$45/100000+P29,IF(K30<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S30))))),(IF(K30<=(Main!$D$72/Main!$D$71*100),O30*Main!$D$71/100000+P29,IF(K30<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K30<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O30*Main!$D$71/100000+P29,IF(K30<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S30))))))","v":40},{"$f":"IF($A$90=TRUE,P30*Main!$D$45/100000+Q29,P30*100+Q29)","v":67.280721645498673},{"$f":"IF($A$90=TRUE,(IF(K30<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K30-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K30<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K30<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K30-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K30<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K30-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K30<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K30<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K30-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-3140049.8100450626},{"$f":"IF($A$90=TRUE,(IF(K30<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O30*Main!$D$45/100000+P29,IF(K30<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K30<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O30*Main!$D$45/100000+P29,Main!$E$52)))),(IF(K30<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O30*Main!$D$71/100000+P29,IF(K30<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K30<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O30*Main!$D$71/100000+P29,Main!$E$78)))))","v":40},29,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T30*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T30*PI()/50))))","v":-36815.343726193496},{"$f":"IF($A$90=TRUE,U30*2*Main!$D$46/100000*(T30-T29)+V29,U30*2*Ltime1*(T30-T29)/100000+V29)","v":739.44857172658135},-0.96858316112863108,0.36972428586329065,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W30*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W30>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W30*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W30>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W30*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W30>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W30*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W30>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W30*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W30>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W30*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W30>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":23.869515543184992},47.074758141010932]
[true,null,null,null,null,null,null,null,null,null,30,0,0.02,8.3134808065212937E-2,{"$f":"IF($A$90=TRUE,(IF(K31<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K31*PI()*Main!$D$45/100/Main!$D$46))),(IF(K31<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K31<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K31-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K31<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R31)))))))),(IF(K31<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K31*PI()*Main!$D$71/100/Main!$D$72))),(IF(K31<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K31<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K31-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K31<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R31)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K31<=(Main!$D$46/Main!$D$45*100),O31*Main!$D$45/100000+P30,IF(K31<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K31<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O31*Main!$D$45/100000+P30,IF(K31<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S31))))),(IF(K31<=(Main!$D$72/Main!$D$71*100),O31*Main!$D$71/100000+P30,IF(K31<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K31<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O31*Main!$D$71/100000+P30,IF(K31<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S31))))))","v":40},{"$f":"IF($A$90=TRUE,P31*Main!$D$45/100000+Q30,P31*100+Q30)","v":68.273121645498676},{"$f":"IF($A$90=TRUE,(IF(K31<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K31-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K31<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K31<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K31-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K31<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K31-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K31<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K31<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K31-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2541607.789528206},{"$f":"IF($A$90=TRUE,(IF(K31<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O31*Main!$D$45/100000+P30,IF(K31<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K31<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O31*Main!$D$45/100000+P30,Main!$E$52)))),(IF(K31<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O31*Main!$D$71/100000+P30,IF(K31<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K31<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O31*Main!$D$71/100000+P30,Main!$E$78)))))","v":40},30,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T31*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T31*PI()/50))))","v":-36149.16504396293},{"$f":"IF($A$90=TRUE,U31*2*Main!$D$46/100000*(T31-T30)+V30,U31*2*Ltime1*(T31-T30)/100000+V30)","v":680.88692435536143},-0.95105651629515353,0.34044346217768073,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W31*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W31>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W31*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W31>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W31*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W31>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W31*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W31>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W31*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W31>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W31*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W31>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":23.329022572335255},43.346607879117279]
[null,null,null,null,null,null,null,null,null,null,31,0,0.02,8.4343233599822376E-2,{"$f":"IF($A$90=TRUE,(IF(K32<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K32*PI()*Main!$D$45/100/Main!$D$46))),(IF(K32<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K32<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K32-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K32<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R32)))))))),(IF(K32<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K32*PI()*Main!$D$71/100/Main!$D$72))),(IF(K32<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K32<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K32-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K32<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R32)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K32<=(Main!$D$46/Main!$D$45*100),O32*Main!$D$45/100000+P31,IF(K32<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K32<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O32*Main!$D$45/100000+P31,IF(K32<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S32))))),(IF(K32<=(Main!$D$72/Main!$D$71*100),O32*Main!$D$71/100000+P31,IF(K32<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K32<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O32*Main!$D$71/100000+P31,IF(K32<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S32))))))","v":40},{"$f":"IF($A$90=TRUE,P32*Main!$D$45/100000+Q31,P32*100+Q31)","v":69.26552164549868},{"$f":"IF($A$90=TRUE,(IF(K32<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K32-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K32<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K32<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K32-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K32<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K32-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K32<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K32<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K32-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-1064179.0502424813},{"$f":"IF($A$90=TRUE,(IF(K32<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O32*Main!$D$45/100000+P31,IF(K32<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K32<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O32*Main!$D$45/100000+P31,Main!$E$52)))),(IF(K32<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O32*Main!$D$71/100000+P31,IF(K32<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K32<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O32*Main!$D$71/100000+P31,Main!$E$78)))))","v":40},31,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T32*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T32*PI()/50))))","v":-35340.322122286423},{"$f":"IF($A$90=TRUE,U32*2*Main!$D$46/100000*(T32-T31)+V31,U32*2*Ltime1*(T32-T31)/100000+V31)","v":623.63560251725744},-0.92977648588825146,0.31181780125862874,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W32*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W32>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W32*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W32>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W32*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W32>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W32*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W32>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W32*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W32>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W32*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W32>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":22.672781348548384},39.701875531485591]
[null,null,null,null,null,null,null,null,null,null,32,0,0.02,8.5551659134431829E-2,{"$f":"IF($A$90=TRUE,(IF(K33<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K33*PI()*Main!$D$45/100/Main!$D$46))),(IF(K33<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K33<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K33-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K33<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R33)))))))),(IF(K33<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K33*PI()*Main!$D$71/100/Main!$D$72))),(IF(K33<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K33<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K33-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K33<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R33)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K33<=(Main!$D$46/Main!$D$45*100),O33*Main!$D$45/100000+P32,IF(K33<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K33<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O33*Main!$D$45/100000+P32,IF(K33<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S33))))),(IF(K33<=(Main!$D$72/Main!$D$71*100),O33*Main!$D$71/100000+P32,IF(K33<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K33<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O33*Main!$D$71/100000+P32,IF(K33<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S33))))))","v":40},{"$f":"IF($A$90=TRUE,P33*Main!$D$45/100000+Q32,P33*100+Q32)","v":70.257921645498683},{"$f":"IF($A$90=TRUE,(IF(K33<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K33-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K33<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K33<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K33-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K33<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K33-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K33<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K33<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K33-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-781284.14951992303},{"$f":"IF($A$90=TRUE,(IF(K33<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O33*Main!$D$45/100000+P32,IF(K33<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K33<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O33*Main!$D$45/100000+P32,Main!$E$52)))),(IF(K33<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O33*Main!$D$71/100000+P32,IF(K33<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K33<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O33*Main!$D$71/100000+P32,Main!$E$78)))))","v":40},32,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T33*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T33*PI()/50))))","v":-34392.007094650638},{"$f":"IF($A$90=TRUE,U33*2*Main!$D$46/100000*(T33-T32)+V32,U33*2*Ltime1*(T33-T32)/100000+V32)","v":567.92055102392339},-0.90482705246601947,0.28396027551196168,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W33*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W33>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W33*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W33>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W33*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W33>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W33*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W33>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W33*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W33>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W33*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W33>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":21.903381756126553},36.154945191572146]
[null,null,null,null,null,null,null,null,null,null,33,0,0.02,8.6760084669041282E-2,{"$f":"IF($A$90=TRUE,(IF(K34<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K34*PI()*Main!$D$45/100/Main!$D$46))),(IF(K34<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K34<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K34-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K34<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R34)))))))),(IF(K34<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K34*PI()*Main!$D$71/100/Main!$D$72))),(IF(K34<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K34<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K34-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K34<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R34)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K34<=(Main!$D$46/Main!$D$45*100),O34*Main!$D$45/100000+P33,IF(K34<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K34<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O34*Main!$D$45/100000+P33,IF(K34<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S34))))),(IF(K34<=(Main!$D$72/Main!$D$71*100),O34*Main!$D$71/100000+P33,IF(K34<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K34<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O34*Main!$D$71/100000+P33,IF(K34<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S34))))))","v":40},{"$f":"IF($A$90=TRUE,P34*Main!$D$45/100000+Q33,P34*100+Q33)","v":71.250321645498687},{"$f":"IF($A$90=TRUE,(IF(K34<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K34-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K34<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K34<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K34-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K34<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K34-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K34<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K34<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K34-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2356548.9363510283},{"$f":"IF($A$90=TRUE,(IF(K34<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O34*Main!$D$45/100000+P33,IF(K34<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K34<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O34*Main!$D$45/100000+P33,Main!$E$52)))),(IF(K34<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O34*Main!$D$71/100000+P33,IF(K34<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K34<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O34*Main!$D$71/100000+P33,Main!$E$78)))))","v":40},33,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T34*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T34*PI()/50))))","v":-33307.962527225747},{"$f":"IF($A$90=TRUE,U34*2*Main!$D$46/100000*(T34-T33)+V33,U34*2*Ltime1*(T34-T33)/100000+V33)","v":513.96165172981773},-0.87630668004386347,0.25698082586490889,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W34*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W34>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W34*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W34>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W34*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W34>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W34*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W34>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W34*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W34>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W34*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W34>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":21.023860263755822},32.719814972990271]
[true,null,null,null,null,null,null,null,null,null,34,0,0.02,8.7968510203650721E-2,{"$f":"IF($A$90=TRUE,(IF(K35<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K35*PI()*Main!$D$45/100/Main!$D$46))),(IF(K35<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K35<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K35-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K35<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R35)))))))),(IF(K35<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K35*PI()*Main!$D$71/100/Main!$D$72))),(IF(K35<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K35<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K35-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K35<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R35)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K35<=(Main!$D$46/Main!$D$45*100),O35*Main!$D$45/100000+P34,IF(K35<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K35<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O35*Main!$D$45/100000+P34,IF(K35<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S35))))),(IF(K35<=(Main!$D$72/Main!$D$71*100),O35*Main!$D$71/100000+P34,IF(K35<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K35<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O35*Main!$D$71/100000+P34,IF(K35<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S35))))))","v":40},{"$f":"IF($A$90=TRUE,P35*Main!$D$45/100000+Q34,P35*100+Q34)","v":72.24272164549869},{"$f":"IF($A$90=TRUE,(IF(K35<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K35-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K35<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K35<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K35-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K35<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K35-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K35<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K35<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K35-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-3116827.5456495485},{"$f":"IF($A$90=TRUE,(IF(K35<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O35*Main!$D$45/100000+P34,IF(K35<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K35<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O35*Main!$D$45/100000+P34,Main!$E$52)))),(IF(K35<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O35*Main!$D$71/100000+P34,IF(K35<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K35<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O35*Main!$D$71/100000+P34,Main!$E$78)))))","v":40},34,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T35*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T35*PI()/50))))","v":-32092.466648666516},{"$f":"IF($A$90=TRUE,U35*2*Main!$D$46/100000*(T35-T34)+V34,U35*2*Ltime1*(T35-T34)/100000+V34)","v":461.97185575897799},-0.84432792550201496,0.23098592787948899,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W35*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W35>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W35*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W35>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W35*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W35>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W35*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W35>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W35*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W35>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W35*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W35>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":20.037687940951432},29.410041765350968]
[null,null,null,null,null,null,null,null,null,null,35,0,0.02,8.9176935738260174E-2,{"$f":"IF($A$90=TRUE,(IF(K36<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K36*PI()*Main!$D$45/100/Main!$D$46))),(IF(K36<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K36<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K36-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K36<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R36)))))))),(IF(K36<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K36*PI()*Main!$D$71/100/Main!$D$72))),(IF(K36<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K36<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K36-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K36<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R36)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K36<=(Main!$D$46/Main!$D$45*100),O36*Main!$D$45/100000+P35,IF(K36<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K36<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O36*Main!$D$45/100000+P35,IF(K36<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S36))))),(IF(K36<=(Main!$D$72/Main!$D$71*100),O36*Main!$D$71/100000+P35,IF(K36<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K36<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O36*Main!$D$71/100000+P35,IF(K36<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S36))))))","v":40},{"$f":"IF($A$90=TRUE,P36*Main!$D$45/100000+Q35,P36*100+Q35)","v":73.235121645498694},{"$f":"IF($A$90=TRUE,(IF(K36<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K36-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K36<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K36<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K36-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K36<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K36-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K36<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K36<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K36-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2799186.0963902692},{"$f":"IF($A$90=TRUE,(IF(K36<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O36*Main!$D$45/100000+P35,IF(K36<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K36<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O36*Main!$D$45/100000+P35,Main!$E$52)))),(IF(K36<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O36*Main!$D$71/100000+P35,IF(K36<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K36<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O36*Main!$D$71/100000+P35,Main!$E$78)))))","v":40},35,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T36*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T36*PI()/50))))","v":-30750.316465898373},{"$f":"IF($A$90=TRUE,U36*2*Main!$D$46/100000*(T36-T35)+V35,U36*2*Ltime1*(T36-T35)/100000+V35)","v":412.15634308422261},-0.80901699437494745,0.2060781715421113,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W36*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W36>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W36*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W36>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W36*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W36>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W36*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W36>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W36*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W36>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W36*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W36>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":18.948756759332213},26.238687731413254]
[null,null,null,null,null,null,null,null,null,null,36,0,0.02,9.0385361272869627E-2,{"$f":"IF($A$90=TRUE,(IF(K37<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K37*PI()*Main!$D$45/100/Main!$D$46))),(IF(K37<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K37<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K37-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K37<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R37)))))))),(IF(K37<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K37*PI()*Main!$D$71/100/Main!$D$72))),(IF(K37<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K37<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K37-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K37<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R37)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K37<=(Main!$D$46/Main!$D$45*100),O37*Main!$D$45/100000+P36,IF(K37<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K37<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O37*Main!$D$45/100000+P36,IF(K37<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S37))))),(IF(K37<=(Main!$D$72/Main!$D$71*100),O37*Main!$D$71/100000+P36,IF(K37<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K37<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O37*Main!$D$71/100000+P36,IF(K37<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S37))))))","v":40},{"$f":"IF($A$90=TRUE,P37*Main!$D$45/100000+Q36,P37*100+Q36)","v":74.227521645498697},{"$f":"IF($A$90=TRUE,(IF(K37<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K37-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K37<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K37<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K37-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K37<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K37-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K37<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K37<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K37-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-1513477.3425582026},{"$f":"IF($A$90=TRUE,(IF(K37<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O37*Main!$D$45/100000+P36,IF(K37<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K37<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O37*Main!$D$45/100000+P36,Main!$E$52)))),(IF(K37<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O37*Main!$D$71/100000+P36,IF(K37<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K37<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O37*Main!$D$71/100000+P36,Main!$E$78)))))","v":40},36,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T37*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T37*PI()/50))))","v":-29286.808832522605},{"$f":"IF($A$90=TRUE,U37*2*Main!$D$46/100000*(T37-T36)+V36,U37*2*Ltime1*(T37-T36)/100000+V36)","v":364.711712775536},-0.77051324277578925,0.18235585638776799,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W37*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W37>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W37*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W37>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W37*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W37>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W37*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W37>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W37*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W37>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W37*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W37>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":17.761364232786676},23.218268756695242]
[null,null,null,null,null,null,null,null,null,null,37,0,0.02,9.1593786807479066E-2,{"$f":"IF($A$90=TRUE,(IF(K38<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K38*PI()*Main!$D$45/100/Main!$D$46))),(IF(K38<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K38<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K38-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K38<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R38)))))))),(IF(K38<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K38*PI()*Main!$D$71/100/Main!$D$72))),(IF(K38<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K38<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K38-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K38<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R38)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K38<=(Main!$D$46/Main!$D$45*100),O38*Main!$D$45/100000+P37,IF(K38<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K38<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O38*Main!$D$45/100000+P37,IF(K38<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S38))))),(IF(K38<=(Main!$D$72/Main!$D$71*100),O38*Main!$D$71/100000+P37,IF(K38<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K38<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O38*Main!$D$71/100000+P37,IF(K38<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S38))))))","v":40},{"$f":"IF($A$90=TRUE,P38*Main!$D$45/100000+Q37,P38*100+Q37)","v":75.219921645498701},{"$f":"IF($A$90=TRUE,(IF(K38<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K38-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K38<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K38<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K38-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K38<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K38-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K38<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K38<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K38-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-295650.67712107179},{"$f":"IF($A$90=TRUE,(IF(K38<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O38*Main!$D$45/100000+P37,IF(K38<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K38<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O38*Main!$D$45/100000+P37,Main!$E$52)))),(IF(K38<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O38*Main!$D$71/100000+P37,IF(K38<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K38<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O38*Main!$D$71/100000+P37,Main!$E$78)))))","v":40},37,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T38*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T38*PI()/50))))","v":-27707.719544555111},{"$f":"IF($A$90=TRUE,U38*2*Main!$D$46/100000*(T38-T37)+V37,U38*2*Ltime1*(T38-T37)/100000+V37)","v":319.82520711335673},-0.72896862742141144,0.15991260355667836,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W38*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W38>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W38*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W38>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W38*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W38>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W38*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W38>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W38*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W38>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W38*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W38>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":16.480196457149045},20.360705054991971]
[null,"bk","copy","bk","copy",null,null,null,null,null,38,0,0.02,9.2802212342088519E-2,{"$f":"IF($A$90=TRUE,(IF(K39<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K39*PI()*Main!$D$45/100/Main!$D$46))),(IF(K39<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K39<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K39-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K39<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R39)))))))),(IF(K39<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K39*PI()*Main!$D$71/100/Main!$D$72))),(IF(K39<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K39<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K39-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K39<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R39)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K39<=(Main!$D$46/Main!$D$45*100),O39*Main!$D$45/100000+P38,IF(K39<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K39<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O39*Main!$D$45/100000+P38,IF(K39<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S39))))),(IF(K39<=(Main!$D$72/Main!$D$71*100),O39*Main!$D$71/100000+P38,IF(K39<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K39<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O39*Main!$D$71/100000+P38,IF(K39<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S39))))))","v":40},{"$f":"IF($A$90=TRUE,P39*Main!$D$45/100000+Q38,P39*100+Q38)","v":76.212321645498704},{"$f":"IF($A$90=TRUE,(IF(K39<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K39-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K39<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K39<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K39-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K39<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K39-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K39<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K39<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K39-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2002531.2061941298},{"$f":"IF($A$90=TRUE,(IF(K39<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O39*Main!$D$45/100000+P38,IF(K39<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K39<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O39*Main!$D$45/100000+P38,Main!$E$52)))),(IF(K39<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O39*Main!$D$71/100000+P38,IF(K39<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K39<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O39*Main!$D$71/100000+P38,Main!$E$78)))))","v":40},38,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T39*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T39*PI()/50))))","v":-26019.280545998241},{"$f":"IF($A$90=TRUE,U39*2*Main!$D$46/100000*(T39-T38)+V38,U39*2*Ltime1*(T39-T38)/100000+V38)","v":277.67397262883958},-0.68454710592868884,0.13883698631441979,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W39*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W39>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W39*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W39>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W39*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W39>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W39*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W39>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W39*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W39>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W39*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W39>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":15.110309616319903},17.677274124737387]
[{"$f":"AND((AutoCalcRot=TRUE),(AutoCalcLin=TRUE))","v":true},81,{"$f":"time1","v":81},50,{"$f":"Ltime1","v":50},null,null,null,null,null,39,0,0.02,9.4010637876697958E-2,{"$f":"IF($A$90=TRUE,(IF(K40<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K40*PI()*Main!$D$45/100/Main!$D$46))),(IF(K40<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K40<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K40-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K40<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R40)))))))),(IF(K40<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K40*PI()*Main!$D$71/100/Main!$D$72))),(IF(K40<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K40<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K40-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K40<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R40)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K40<=(Main!$D$46/Main!$D$45*100),O40*Main!$D$45/100000+P39,IF(K40<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K40<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O40*Main!$D$45/100000+P39,IF(K40<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S40))))),(IF(K40<=(Main!$D$72/Main!$D$71*100),O40*Main!$D$71/100000+P39,IF(K40<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K40<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O40*Main!$D$71/100000+P39,IF(K40<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S40))))))","v":40},{"$f":"IF($A$90=TRUE,P40*Main!$D$45/100000+Q39,P40*100+Q39)","v":77.204721645498708},{"$f":"IF($A$90=TRUE,(IF(K40<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K40-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K40<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K40<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K40-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K40<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K40-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K40<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K40<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K40-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-3016858.6429225327},{"$f":"IF($A$90=TRUE,(IF(K40<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O40*Main!$D$45/100000+P39,IF(K40<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K40<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O40*Main!$D$45/100000+P39,Main!$E$52)))),(IF(K40<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O40*Main!$D$71/100000+P39,IF(K40<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K40<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O40*Main!$D$71/100000+P39,Main!$E$78)))))","v":40},39,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T40*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T40*PI()/50))))","v":-24228.155334204868},{"$f":"IF($A$90=TRUE,U40*2*Main!$D$46/100000*(T40-T39)+V39,U40*2*Ltime1*(T40-T39)/100000+V39)","v":238.42436098742769},-0.63742398974868986,0.11921218049371385,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W40*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W40>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W40*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W40>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W40*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W40>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W40*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W40>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W40*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W40>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W40*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W40>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":13.657110027818216},15.178566241870225]
[{"$f":"AND((ctime1=btime1),(ctime2=btime2),(ctime3=btime3),(ctime4=btime4),(ctime5=btime5),(ctime6=btime6),(ctime7=btime7),(ctime8=btime8),(cspeed1=bspeed1),(cspeed2=bspeed2),(cspeed6=bspeed6),(cinertia=bInertia),(cinertia2=binertia2),(ctorque=btorque),(ctorque2=btorque2),(cgear=bgear),(cgear_inertia=bgear_inertia),(cWirkungsgrad=bWirkungsgrad),(cULU=bULU),(cDryTorq=bDryTorq),(cDryTorq2=bDryTorq2))","v":true},2000,{"$f":"time2","v":2000},0,{"$f":"Ltime2","v":0},null,null,null,null,null,40,0,0.02,9.5219063411307411E-2,{"$f":"IF($A$90=TRUE,(IF(K41<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K41*PI()*Main!$D$45/100/Main!$D$46))),(IF(K41<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K41<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K41-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K41<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R41)))))))),(IF(K41<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K41*PI()*Main!$D$71/100/Main!$D$72))),(IF(K41<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K41<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K41-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K41<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R41)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K41<=(Main!$D$46/Main!$D$45*100),O41*Main!$D$45/100000+P40,IF(K41<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K41<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O41*Main!$D$45/100000+P40,IF(K41<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S41))))),(IF(K41<=(Main!$D$72/Main!$D$71*100),O41*Main!$D$71/100000+P40,IF(K41<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K41<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O41*Main!$D$71/100000+P40,IF(K41<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S41))))))","v":40},{"$f":"IF($A$90=TRUE,P41*Main!$D$45/100000+Q40,P41*100+Q40)","v":78.197121645498711},{"$f":"IF($A$90=TRUE,(IF(K41<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K41-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K41<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K41<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K41-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K41<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K41-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K41<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K41<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K41-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2987839.1515930486},{"$f":"IF($A$90=TRUE,(IF(K41<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O41*Main!$D$45/100000+P40,IF(K41<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K41<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O41*Main!$D$45/100000+P40,Main!$E$52)))),(IF(K41<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O41*Main!$D$71/100000+P40,IF(K41<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K41<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O41*Main!$D$71/100000+P40,Main!$E$78)))))","v":40},40,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T41*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T41*PI()/50))))","v":-22341.412662098683},{"$f":"IF($A$90=TRUE,U41*2*Main!$D$46/100000*(T41-T40)+V40,U41*2*Ltime1*(T41-T40)/100000+V40)","v":202.23127247482782},-0.58778525229247325,0.1011156362374139,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W41*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W41>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W41*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W41>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W41*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W41>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W41*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W41>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W41*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W41>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W41*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W41>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":12.126332806516064},12.87444266485312]
[{"$f":"AND((cltime1=bltime1),(cltime2=bltime2),(cltime3=bltime3),(cltime4=bltime4),(cltime5=bltime5),(cltime6=bltime6),(cltime7=bltime7),(cltime8=bltime8),(clspeed1=blspeed1),(clspeed2=blspeed2),(clspeed6=blspeed6),(cltorque=bltorque),(cltorque2=bltorque2),(cgewicht=bgewicht),(cgewicht2=bgewicht2),(clwirkungsgrad=blwirkungsgrad),(clDryTorq=blDrytorq),(clDryTorq2=blDryTorq2))","v":true},100,{"$f":"time3","v":100},30,{"$f":"Ltime3","v":30},null,null,null,null,null,41,0,0.02,9.6427488945916864E-2,{"$f":"IF($A$90=TRUE,(IF(K42<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K42*PI()*Main!$D$45/100/Main!$D$46))),(IF(K42<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K42<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K42-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K42<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R42)))))))),(IF(K42<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K42*PI()*Main!$D$71/100/Main!$D$72))),(IF(K42<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K42<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K42-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K42<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R42)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K42<=(Main!$D$46/Main!$D$45*100),O42*Main!$D$45/100000+P41,IF(K42<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K42<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O42*Main!$D$45/100000+P41,IF(K42<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S42))))),(IF(K42<=(Main!$D$72/Main!$D$71*100),O42*Main!$D$71/100000+P41,IF(K42<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K42<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O42*Main!$D$71/100000+P41,IF(K42<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S42))))))","v":40},{"$f":"IF($A$90=TRUE,P42*Main!$D$45/100000+Q41,P42*100+Q41)","v":79.189521645498715},{"$f":"IF($A$90=TRUE,(IF(K42<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K42-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K42<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K42<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K42-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K42<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K42-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K42<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K42<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K42-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-1925508.7997567549},{"$f":"IF($A$90=TRUE,(IF(K42<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O42*Main!$D$45/100000+P41,IF(K42<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K42<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O42*Main!$D$45/100000+P41,Main!$E$52)))),(IF(K42<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O42*Main!$D$71/100000+P41,IF(K42<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K42<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O42*Main!$D$71/100000+P41,Main!$E$78)))))","v":40},41,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T42*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T42*PI()/50))))","v":-20366.49864103576},{"$f":"IF($A$90=TRUE,U42*2*Main!$D$46/100000*(T42-T41)+V41,U42*2*Ltime1*(T42-T41)/100000+V41)","v":169.2375446763499},-0.53582679497899699,8.4618772338174955E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W42*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W42>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W42*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W42>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W42*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W42>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W42*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W42>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W42*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W42>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W42*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W42>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":10.524019230760345},10.773996716790625]
[null,300,{"$f":"time4","v":300},50,{"$f":"Ltime4","v":50},null,null,null,null,null,42,0,0.02,9.7635914480526304E-2,{"$f":"IF($A$90=TRUE,(IF(K43<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K43*PI()*Main!$D$45/100/Main!$D$46))),(IF(K43<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K43<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K43-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K43<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R43)))))))),(IF(K43<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K43*PI()*Main!$D$71/100/Main!$D$72))),(IF(K43<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K43<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K43-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K43<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R43)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K43<=(Main!$D$46/Main!$D$45*100),O43*Main!$D$45/100000+P42,IF(K43<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K43<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O43*Main!$D$45/100000+P42,IF(K43<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S43))))),(IF(K43<=(Main!$D$72/Main!$D$71*100),O43*Main!$D$71/100000+P42,IF(K43<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K43<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O43*Main!$D$71/100000+P42,IF(K43<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S43))))))","v":40},{"$f":"IF($A$90=TRUE,P43*Main!$D$45/100000+Q42,P43*100+Q42)","v":80.181921645498718},{"$f":"IF($A$90=TRUE,(IF(K43<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K43-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K43<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K43<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K43-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K43<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K43-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K43<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K43<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K43-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":197262.69615408761},{"$f":"IF($A$90=TRUE,(IF(K43<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O43*Main!$D$45/100000+P42,IF(K43<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K43<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O43*Main!$D$45/100000+P42,Main!$E$52)))),(IF(K43<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O43*Main!$D$71/100000+P42,IF(K43<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K43<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O43*Main!$D$71/100000+P42,Main!$E$78)))))","v":40},42,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T43*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T43*PI()/50))))","v":-18311.207354404811},{"$f":"IF($A$90=TRUE,U43*2*Main!$D$46/100000*(T43-T42)+V42,U43*2*Ltime1*(T43-T42)/100000+V42)","v":139.57338876221411},-0.48175367410171527,6.9786694381107059E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W43*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W43>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W43*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W43>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W43*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W43>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W43*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W43>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W43*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W43>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W43*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W43>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":8.8564929002071047},8.8855178982372678]
[null,127.32395447351627,{"$f":"speed1","v":127.32395447351627},0,{"$f":"Lspeed1","v":0},null,null,null,null,null,43,0,0.02,9.8844340015135757E-2,{"$f":"IF($A$90=TRUE,(IF(K44<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K44*PI()*Main!$D$45/100/Main!$D$46))),(IF(K44<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K44<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K44-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K44<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R44)))))))),(IF(K44<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K44*PI()*Main!$D$71/100/Main!$D$72))),(IF(K44<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K44<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K44-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K44<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R44)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K44<=(Main!$D$46/Main!$D$45*100),O44*Main!$D$45/100000+P43,IF(K44<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K44<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O44*Main!$D$45/100000+P43,IF(K44<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S44))))),(IF(K44<=(Main!$D$72/Main!$D$71*100),O44*Main!$D$71/100000+P43,IF(K44<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K44<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O44*Main!$D$71/100000+P43,IF(K44<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S44))))))","v":40},{"$f":"IF($A$90=TRUE,P44*Main!$D$45/100000+Q43,P44*100+Q43)","v":81.174321645498722},{"$f":"IF($A$90=TRUE,(IF(K44<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K44-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K44<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K44<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K44-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K44<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K44-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K44<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K44<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K44-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":1599204.5117206066},{"$f":"IF($A$90=TRUE,(IF(K44<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O44*Main!$D$45/100000+P43,IF(K44<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K44<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O44*Main!$D$45/100000+P43,Main!$E$52)))),(IF(K44<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O44*Main!$D$71/100000+P43,IF(K44<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K44<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O44*Main!$D$71/100000+P43,Main!$E$78)))))","v":40},43,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T44*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T44*PI()/50))))","v":-16183.650097940943},{"$f":"IF($A$90=TRUE,U44*2*Main!$D$46/100000*(T44-T43)+V43,U44*2*Ltime1*(T44-T43)/100000+V43)","v":113.35587560354978},-0.42577929156507288,5.6677937801774887E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W44*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W44>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W44*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W44>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W44*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W44>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W44*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W44>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W44*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W44>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W44*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W44>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":7.1303347794627516},7.2164591723259726]
[null,2.5464790894703255,{"$f":"speed2","v":2.5464790894703255},1,{"$f":"Lspeed2","v":1},null,null,null,null,null,44,0,0.02,0.10005276554974521,{"$f":"IF($A$90=TRUE,(IF(K45<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K45*PI()*Main!$D$45/100/Main!$D$46))),(IF(K45<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K45<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K45-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K45<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R45)))))))),(IF(K45<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K45*PI()*Main!$D$71/100/Main!$D$72))),(IF(K45<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K45<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K45-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K45<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R45)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K45<=(Main!$D$46/Main!$D$45*100),O45*Main!$D$45/100000+P44,IF(K45<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K45<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O45*Main!$D$45/100000+P44,IF(K45<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S45))))),(IF(K45<=(Main!$D$72/Main!$D$71*100),O45*Main!$D$71/100000+P44,IF(K45<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K45<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O45*Main!$D$71/100000+P44,IF(K45<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S45))))))","v":40},{"$f":"IF($A$90=TRUE,P45*Main!$D$45/100000+Q44,P45*100+Q44)","v":82.166721645498725},{"$f":"IF($A$90=TRUE,(IF(K45<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K45-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K45<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K45<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K45-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K45<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K45-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K45<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K45<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K45-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2842604.6680268347},{"$f":"IF($A$90=TRUE,(IF(K45<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O45*Main!$D$45/100000+P44,IF(K45<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K45<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O45*Main!$D$45/100000+P44,Main!$E$52)))),(IF(K45<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O45*Main!$D$71/100000+P44,IF(K45<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K45<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O45*Main!$D$71/100000+P44,Main!$E$78)))))","v":40},44,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T45*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T45*PI()/50))))","v":-13992.223368146928},{"$f":"IF($A$90=TRUE,U45*2*Main!$D$46/100000*(T45-T44)+V44,U45*2*Ltime1*(T45-T44)/100000+V44)","v":90.688473747151761},-0.36812455268467814,4.5344236873575881E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W45*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W45>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W45*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W45>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W45*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W45>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W45*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W45>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W45*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W45>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W45*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W45>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":5.3523572260232068},5.7734075513275132]
[null,112.5,{"$f":"inertia","v":112.5},5,{"$f":"Gewicht","v":5},null,null,null,null,null,45,0,0.02,0.10126119108435465,{"$f":"IF($A$90=TRUE,(IF(K46<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K46*PI()*Main!$D$45/100/Main!$D$46))),(IF(K46<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K46<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K46-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K46<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R46)))))))),(IF(K46<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K46*PI()*Main!$D$71/100/Main!$D$72))),(IF(K46<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K46<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K46-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K46<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R46)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K46<=(Main!$D$46/Main!$D$45*100),O46*Main!$D$45/100000+P45,IF(K46<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K46<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O46*Main!$D$45/100000+P45,IF(K46<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S46))))),(IF(K46<=(Main!$D$72/Main!$D$71*100),O46*Main!$D$71/100000+P45,IF(K46<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K46<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O46*Main!$D$71/100000+P45,IF(K46<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S46))))))","v":40},{"$f":"IF($A$90=TRUE,P46*Main!$D$45/100000+Q45,P46*100+Q45)","v":83.159121645498729},{"$f":"IF($A$90=TRUE,(IF(K46<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K46-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K46<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K46<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K46-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K46<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K46-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K46<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K46<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K46-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":3102921.6908134022},{"$f":"IF($A$90=TRUE,(IF(K46<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O46*Main!$D$45/100000+P45,IF(K46<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K46<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O46*Main!$D$45/100000+P45,Main!$E$52)))),(IF(K46<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O46*Main!$D$71/100000+P45,IF(K46<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K46<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O46*Main!$D$71/100000+P45,Main!$E$78)))))","v":40},46,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T46*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T46*PI()/50))))","v":-9452.5736608242842},{"$f":"IF($A$90=TRUE,U46*2*Main!$D$46/100000*(T46-T45)+V45,U46*2*Ltime1*(T46-T45)/100000+V45)","v":60.062135086081085},-0.24868988716485524,3.0031067543040541E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W46*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W46>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W46*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W46>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W46*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W46>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W46*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W46>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W46*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W46>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W46*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W46>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":1.6691880968154358},3.823674276641186]
[null,7.5,{"$f":"torque","v":7.5},0,{"$f":"Ltorque","v":0},null,null,null,null,null,46,0,0.02,0.1024696166189641,{"$f":"IF($A$90=TRUE,(IF(K47<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K47*PI()*Main!$D$45/100/Main!$D$46))),(IF(K47<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K47<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K47-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K47<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R47)))))))),(IF(K47<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K47*PI()*Main!$D$71/100/Main!$D$72))),(IF(K47<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K47<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K47-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K47<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R47)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K47<=(Main!$D$46/Main!$D$45*100),O47*Main!$D$45/100000+P46,IF(K47<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K47<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O47*Main!$D$45/100000+P46,IF(K47<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S47))))),(IF(K47<=(Main!$D$72/Main!$D$71*100),O47*Main!$D$71/100000+P46,IF(K47<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K47<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O47*Main!$D$71/100000+P46,IF(K47<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S47))))))","v":40},{"$f":"IF($A$90=TRUE,P47*Main!$D$45/100000+Q46,P47*100+Q46)","v":84.151521645498732},{"$f":"IF($A$90=TRUE,(IF(K47<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K47-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K47<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K47<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K47-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K47<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K47-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K47<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K47<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K47-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2290127.8399078851},{"$f":"IF($A$90=TRUE,(IF(K47<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O47*Main!$D$45/100000+P46,IF(K47<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K47<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O47*Main!$D$45/100000+P46,Main!$E$52)))),(IF(K47<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O47*Main!$D$71/100000+P46,IF(K47<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K47<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O47*Main!$D$71/100000+P46,Main!$E$78)))))","v":40},48,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T47*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T47*PI()/50))))","v":-4763.8512201766262},{"$f":"IF($A$90=TRUE,U47*2*Main!$D$46/100000*(T47-T46)+V46,U47*2*Ltime1*(T47-T46)/100000+V46)","v":44.627257132708813},-0.12533323356430454,2.2313628566354406E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W47*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W47>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W47*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W47>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W47*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W47>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W47*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W47>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W47*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W47>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W47*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W47>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":2.1349287100300303},2.8410594277214605]
[null,1,{"$f":"gear","v":1},1,{"$f":"LWirkungsgrad","v":1},null,null,null,null,null,47,0,0.02,0.10367804215357354,{"$f":"IF($A$90=TRUE,(IF(K48<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K48*PI()*Main!$D$45/100/Main!$D$46))),(IF(K48<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K48<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K48-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K48<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R48)))))))),(IF(K48<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K48*PI()*Main!$D$71/100/Main!$D$72))),(IF(K48<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K48<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K48-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K48<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R48)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K48<=(Main!$D$46/Main!$D$45*100),O48*Main!$D$45/100000+P47,IF(K48<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K48<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O48*Main!$D$45/100000+P47,IF(K48<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S48))))),(IF(K48<=(Main!$D$72/Main!$D$71*100),O48*Main!$D$71/100000+P47,IF(K48<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K48<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O48*Main!$D$71/100000+P47,IF(K48<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S48))))))","v":40},{"$f":"IF($A$90=TRUE,P48*Main!$D$45/100000+Q47,P48*100+Q47)","v":85.143921645498736},{"$f":"IF($A$90=TRUE,(IF(K48<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K48-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K48<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K48<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K48-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K48<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K48-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K48<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K48<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K48-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":685318.80717257073},{"$f":"IF($A$90=TRUE,(IF(K48<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O48*Main!$D$45/100000+P47,IF(K48<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K48<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O48*Main!$D$45/100000+P47,Main!$E$52)))),(IF(K48<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O48*Main!$D$71/100000+P47,IF(K48<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K48<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O48*Main!$D$71/100000+P47,Main!$E$78)))))","v":40},49,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T48*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T48*PI()/50))))","v":-2386.6350892620458},{"$f":"IF($A$90=TRUE,U48*2*Main!$D$46/100000*(T48-T47)+V47,U48*2*Ltime1*(T48-T47)/100000+V47)","v":40.760908288104297},-6.2790519529313582E-2,2.0380454144052148E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W48*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W48>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W48*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W48>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W48*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W48>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W48*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W48>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W48*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W48>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W48*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W48>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":4.0636433975787263},2.5949200155868817]
[null,0,{"$f":"gear_inertia","v":0},1,{"$f":"Ltime5","v":1},null,null,null,null,null,48,0,0.02,0.10488646768818299,{"$f":"IF($A$90=TRUE,(IF(K49<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K49*PI()*Main!$D$45/100/Main!$D$46))),(IF(K49<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K49<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K49-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K49<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R49)))))))),(IF(K49<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K49*PI()*Main!$D$71/100/Main!$D$72))),(IF(K49<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K49<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K49-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K49<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R49)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K49<=(Main!$D$46/Main!$D$45*100),O49*Main!$D$45/100000+P48,IF(K49<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K49<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O49*Main!$D$45/100000+P48,IF(K49<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S49))))),(IF(K49<=(Main!$D$72/Main!$D$71*100),O49*Main!$D$71/100000+P48,IF(K49<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K49<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O49*Main!$D$71/100000+P48,IF(K49<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S49))))))","v":40},{"$f":"IF($A$90=TRUE,P49*Main!$D$45/100000+Q48,P49*100+Q48)","v":86.136321645498739},{"$f":"IF($A$90=TRUE,(IF(K49<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K49-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K49<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K49<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K49-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K49<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K49-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K49<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K49<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K49-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":1156500.0947142974},{"$f":"IF($A$90=TRUE,(IF(K49<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O49*Main!$D$45/100000+P48,IF(K49<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K49<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O49*Main!$D$45/100000+P48,Main!$E$52)))),(IF(K49<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O49*Main!$D$71/100000+P48,IF(K49<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K49<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O49*Main!$D$71/100000+P48,Main!$E$78)))))","v":40},49.999989999999997,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T49*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T49*PI()/50))))","v":-2.3882061555603205E-2},{"$f":"IF($A$90=TRUE,U49*2*Main!$D$46/100000*(T49-T48)+V48,U49*2*Ltime1*(T49-T48)/100000+V48)","v":40.760869599551469},-6.2831853066027051E-7,2.0380434799775735E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W49*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W49>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W49*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W49>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W49*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W49>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W49*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W49>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W49*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W49>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W49*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W49>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":5.9999806236873914},2.5949175525971122]
[null,1,{"$f":"Wirkungsgrad","v":1},0,{"$f":"Ltime6","v":0},null,null,null,null,null,49,0,0.02,0.10609489322279245,{"$f":"IF($A$90=TRUE,(IF(K50<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K50*PI()*Main!$D$45/100/Main!$D$46))),(IF(K50<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K50<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K50-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K50<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R50)))))))),(IF(K50<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K50*PI()*Main!$D$71/100/Main!$D$72))),(IF(K50<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K50<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K50-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K50<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R50)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K50<=(Main!$D$46/Main!$D$45*100),O50*Main!$D$45/100000+P49,IF(K50<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K50<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O50*Main!$D$45/100000+P49,IF(K50<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S50))))),(IF(K50<=(Main!$D$72/Main!$D$71*100),O50*Main!$D$71/100000+P49,IF(K50<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K50<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O50*Main!$D$71/100000+P49,IF(K50<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S50))))))","v":40},{"$f":"IF($A$90=TRUE,P50*Main!$D$45/100000+Q49,P50*100+Q49)","v":87.128721645498743},{"$f":"IF($A$90=TRUE,(IF(K50<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K50-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K50<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K50<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K50-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K50<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K50-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K50<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K50<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K50-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2598356.3321409845},{"$f":"IF($A$90=TRUE,(IF(K50<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O50*Main!$D$45/100000+P49,IF(K50<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K50<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O50*Main!$D$45/100000+P49,Main!$E$52)))),(IF(K50<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O50*Main!$D$71/100000+P49,IF(K50<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K50<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O50*Main!$D$71/100000+P49,Main!$E$78)))))","v":40},49.999989999999997,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(T50*PI()/50))),(IF($B$30=1,laccel1,laccel1*SIN(T50*PI()/50))))","v":-2.3882061555603205E-2},{"$f":"IF($A$90=TRUE,U50*2*Main!$D$46/100000*(T50-T49)+V49,U50*2*Ltime1*(T50-T49)/100000+V49)","v":40.760869599551469},-6.2831853066027051E-7,2.0380434799775735E-2,{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W50*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W50>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W50*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W50>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W50*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W50>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W50*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W50>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W50*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W50>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W50*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W50>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad))),0)","v":5.9999806236873914},2.5949175525971122]
[null,942.47779607693792,{"$f":"ULU","v":942.47779607693792},1,{"$f":"Ltime7","v":1},null,null,null,null,null,50,0,0.02,0.10730331875740189,{"$f":"IF($A$90=TRUE,(IF(K51<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K51*PI()*Main!$D$45/100/Main!$D$46))),(IF(K51<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K51<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K51-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K51<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R51)))))))),(IF(K51<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K51*PI()*Main!$D$71/100/Main!$D$72))),(IF(K51<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K51<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K51-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K51<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R51)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K51<=(Main!$D$46/Main!$D$45*100),O51*Main!$D$45/100000+P50,IF(K51<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K51<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O51*Main!$D$45/100000+P50,IF(K51<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S51))))),(IF(K51<=(Main!$D$72/Main!$D$71*100),O51*Main!$D$71/100000+P50,IF(K51<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K51<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O51*Main!$D$71/100000+P50,IF(K51<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S51))))))","v":40},{"$f":"IF($A$90=TRUE,P51*Main!$D$45/100000+Q50,P51*100+Q50)","v":88.121121645498746},{"$f":"IF($A$90=TRUE,(IF(K51<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K51-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K51<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K51<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K51-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K51<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K51-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K51<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K51<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K51-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":3141600},{"$f":"IF($A$90=TRUE,(IF(K51<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O51*Main!$D$45/100000+P50,IF(K51<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K51<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O51*Main!$D$45/100000+P50,Main!$E$52)))),(IF(K51<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O51*Main!$D$71/100000+P50,IF(K51<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K51<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O51*Main!$D$71/100000+P50,Main!$E$78)))))","v":40},50,0,{"$f":"IF($A$90=TRUE,Main!$E$48,Lspeed2)","v":40},0,0.02,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W51*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W51>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W51*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W51>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W51*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W51>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W51*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W51>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W51*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W51>=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W51*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W51>=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":9},2.5464790894703255]
[null,1,{"$f":"time5","v":1},0,{"$f":"Ltime8","v":0},null,null,null,null,null,51,0,0.02,0.10851174429201134,{"$f":"IF($A$90=TRUE,(IF(K52<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K52*PI()*Main!$D$45/100/Main!$D$46))),(IF(K52<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K52<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K52-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K52<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R52)))))))),(IF(K52<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K52*PI()*Main!$D$71/100/Main!$D$72))),(IF(K52<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K52<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K52-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K52<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R52)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K52<=(Main!$D$46/Main!$D$45*100),O52*Main!$D$45/100000+P51,IF(K52<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K52<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O52*Main!$D$45/100000+P51,IF(K52<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S52))))),(IF(K52<=(Main!$D$72/Main!$D$71*100),O52*Main!$D$71/100000+P51,IF(K52<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K52<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O52*Main!$D$71/100000+P51,IF(K52<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S52))))))","v":40},{"$f":"IF($A$90=TRUE,P52*Main!$D$45/100000+Q51,P52*100+Q51)","v":89.11352164549875},{"$f":"IF($A$90=TRUE,(IF(K52<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K52-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K52<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K52<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K52-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K52<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K52-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K52<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K52<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K52-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2598356.332141038},{"$f":"IF($A$90=TRUE,(IF(K52<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O52*Main!$D$45/100000+P51,IF(K52<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K52<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O52*Main!$D$45/100000+P51,Main!$E$52)))),(IF(K52<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O52*Main!$D$71/100000+P51,IF(K52<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K52<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O52*Main!$D$71/100000+P51,Main!$E$78)))))","v":40},50.000000999999997,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T52-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T52-50)*PI()/50))))","v":1.9344469812974578E-3},{"$f":"IF($A$90=TRUE,U52*2*Main!$D$50*(T52-T51)/100000+V51,U52*2*Ltime3*(T52-T51)/100000+V51)","v":40.000000000003865},5.0893800859660125E-8,2.0000000000001933E-2,{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W52*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W52<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W52*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W52<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W52*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+Ltorque)/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W52*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W52<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W52*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W52<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W52*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+Ltorque)/LWirkungsgrad))),0)","v":6.0000015694813174},2.5464790894705716]
[null,0,{"$f":"time6","v":0},0,{"$f":"Lspeed6","v":0},null,null,null,null,null,52,0,0.02,0.10972016982662079,{"$f":"IF($A$90=TRUE,(IF(K53<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K53*PI()*Main!$D$45/100/Main!$D$46))),(IF(K53<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K53<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K53-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K53<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R53)))))))),(IF(K53<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K53*PI()*Main!$D$71/100/Main!$D$72))),(IF(K53<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K53<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K53-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K53<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R53)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K53<=(Main!$D$46/Main!$D$45*100),O53*Main!$D$45/100000+P52,IF(K53<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K53<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O53*Main!$D$45/100000+P52,IF(K53<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S53))))),(IF(K53<=(Main!$D$72/Main!$D$71*100),O53*Main!$D$71/100000+P52,IF(K53<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K53<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O53*Main!$D$71/100000+P52,IF(K53<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S53))))))","v":40},{"$f":"IF($A$90=TRUE,P53*Main!$D$45/100000+Q52,P53*100+Q52)","v":90.105921645498753},{"$f":"IF($A$90=TRUE,(IF(K53<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K53-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K53<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K53<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K53-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K53<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K53-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K53<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K53<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K53-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":1156500.0947143864},{"$f":"IF($A$90=TRUE,(IF(K53<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O53*Main!$D$45/100000+P52,IF(K53<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K53<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O53*Main!$D$45/100000+P52,Main!$E$52)))),(IF(K53<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O53*Main!$D$71/100000+P52,IF(K53<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K53<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O53*Main!$D$71/100000+P52,Main!$E$78)))))","v":40},50.000000999999997,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T53-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T53-50)*PI()/50))))","v":1.9344469812974578E-3},{"$f":"IF($A$90=TRUE,U53*2*Main!$D$50*(T53-T52)/100000+V52,U53*2*Ltime3*(T53-T52)/100000+V52)","v":40.000000000003865},5.0893800859660125E-8,2.0000000000001933E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W53*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W53<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W53*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W53<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W53*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W53<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W53*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W53<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W53*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W53<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W53*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W53<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":6.0000015694813174},2.5464790894705716]
[null,1,{"$f":"time7","v":1},5,{"$f":"Gewicht2","v":5},null,null,null,null,null,53,0,0.02,0.11092859536123023,{"$f":"IF($A$90=TRUE,(IF(K54<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K54*PI()*Main!$D$45/100/Main!$D$46))),(IF(K54<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K54<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K54-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K54<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R54)))))))),(IF(K54<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K54*PI()*Main!$D$71/100/Main!$D$72))),(IF(K54<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K54<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K54-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K54<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R54)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K54<=(Main!$D$46/Main!$D$45*100),O54*Main!$D$45/100000+P53,IF(K54<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K54<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O54*Main!$D$45/100000+P53,IF(K54<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S54))))),(IF(K54<=(Main!$D$72/Main!$D$71*100),O54*Main!$D$71/100000+P53,IF(K54<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K54<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O54*Main!$D$71/100000+P53,IF(K54<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S54))))))","v":40},{"$f":"IF($A$90=TRUE,P54*Main!$D$45/100000+Q53,P54*100+Q53)","v":91.098321645498757},{"$f":"IF($A$90=TRUE,(IF(K54<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K54-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K54<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K54<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K54-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K54<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K54-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K54<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K54<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K54-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":685318.80717108329},{"$f":"IF($A$90=TRUE,(IF(K54<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O54*Main!$D$45/100000+P53,IF(K54<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K54<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O54*Main!$D$45/100000+P53,Main!$E$52)))),(IF(K54<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O54*Main!$D$71/100000+P53,IF(K54<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K54<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O54*Main!$D$71/100000+P53,Main!$E$78)))))","v":40},51,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T54-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T54-50)*PI()/50))))","v":1933.1744223022508},{"$f":"IF($A$90=TRUE,U54*2*Main!$D$50*(T54-T53)/100000+V53,U54*2*Ltime3*(T54-T53)/100000+V53)","v":43.866344978259534},5.0860320818743837E-2,2.1933172489129765E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W54*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W54<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W54*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W54<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W54*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W54<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W54*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W54<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W54*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W54<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W54*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W54<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":7.5684488479612266},2.7926182554657375]
[null,0,{"$f":"time8","v":0},0,{"$f":"Ltorque2","v":0},null,null,null,null,null,54,0,0.02,0.11213702089583968,{"$f":"IF($A$90=TRUE,(IF(K55<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K55*PI()*Main!$D$45/100/Main!$D$46))),(IF(K55<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K55<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K55-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K55<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R55)))))))),(IF(K55<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K55*PI()*Main!$D$71/100/Main!$D$72))),(IF(K55<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K55<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K55-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K55<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R55)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K55<=(Main!$D$46/Main!$D$45*100),O55*Main!$D$45/100000+P54,IF(K55<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K55<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O55*Main!$D$45/100000+P54,IF(K55<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S55))))),(IF(K55<=(Main!$D$72/Main!$D$71*100),O55*Main!$D$71/100000+P54,IF(K55<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K55<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O55*Main!$D$71/100000+P54,IF(K55<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S55))))))","v":40},{"$f":"IF($A$90=TRUE,P55*Main!$D$45/100000+Q54,P55*100+Q54)","v":92.09072164549876},{"$f":"IF($A$90=TRUE,(IF(K55<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K55-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K55<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K55<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K55-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K55<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K55-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K55<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K55<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K55-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2290127.8399058636},{"$f":"IF($A$90=TRUE,(IF(K55<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O55*Main!$D$45/100000+P54,IF(K55<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K55<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O55*Main!$D$45/100000+P54,Main!$E$52)))),(IF(K55<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O55*Main!$D$71/100000+P54,IF(K55<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K55<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O55*Main!$D$71/100000+P54,Main!$E$78)))))","v":40},52,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T55-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T55-50)*PI()/50))))","v":3858.7194883430589},{"$f":"IF($A$90=TRUE,U55*2*Main!$D$50*(T55-T54)/100000+V54,U55*2*Ltime3*(T55-T54)/100000+V54)","v":51.583783954945652},0.10151991918708644,2.5791891977472826E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W55*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W55<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W55*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W55<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W55*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W55<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W55*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W55<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W55*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W55<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W55*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W55<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":9.1307077448756679},3.2839256799255994]
[null,0,{"$f":"speed6","v":0},0,{"$f":"LDryTorq","v":0},null,null,null,null,null,55,0,0.02,0.11334544643044914,{"$f":"IF($A$90=TRUE,(IF(K56<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K56*PI()*Main!$D$45/100/Main!$D$46))),(IF(K56<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K56<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K56-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K56<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R56)))))))),(IF(K56<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K56*PI()*Main!$D$71/100/Main!$D$72))),(IF(K56<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K56<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K56-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K56<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R56)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K56<=(Main!$D$46/Main!$D$45*100),O56*Main!$D$45/100000+P55,IF(K56<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K56<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O56*Main!$D$45/100000+P55,IF(K56<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S56))))),(IF(K56<=(Main!$D$72/Main!$D$71*100),O56*Main!$D$71/100000+P55,IF(K56<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K56<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O56*Main!$D$71/100000+P55,IF(K56<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S56))))))","v":40},{"$f":"IF($A$90=TRUE,P56*Main!$D$45/100000+Q55,P56*100+Q55)","v":93.083121645498764},{"$f":"IF($A$90=TRUE,(IF(K56<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K56-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K56<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K56<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K56-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K56<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K56-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K56<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K56<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K56-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":3102921.6908136108},{"$f":"IF($A$90=TRUE,(IF(K56<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O56*Main!$D$45/100000+P55,IF(K56<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K56<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O56*Main!$D$45/100000+P55,Main!$E$52)))),(IF(K56<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O56*Main!$D$71/100000+P55,IF(K56<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K56<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O56*Main!$D$71/100000+P55,Main!$E$78)))))","v":40},54,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T56-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T56-50)*PI()/50))))","v":7656.5846652676564},{"$f":"IF($A$90=TRUE,U56*2*Main!$D$50*(T56-T55)/100000+V55,U56*2*Ltime3*(T56-T55)/100000+V55)","v":82.210122616016278},0.20143880860353239,4.1105061308008138E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W56*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W56<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W56*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W56<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W56*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W56<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W56*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W56<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W56*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W56<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W56*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W56<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":12.212042358420494},5.233658954611923]
[null,112.5,{"$f":"inertia2","v":112.5},0,{"$f":"LDryTorq2","v":0},null,null,null,null,null,56,0,0.02,0.11455387196505858,{"$f":"IF($A$90=TRUE,(IF(K57<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K57*PI()*Main!$D$45/100/Main!$D$46))),(IF(K57<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K57<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K57-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K57<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R57)))))))),(IF(K57<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K57*PI()*Main!$D$71/100/Main!$D$72))),(IF(K57<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K57<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K57-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K57<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R57)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K57<=(Main!$D$46/Main!$D$45*100),O57*Main!$D$45/100000+P56,IF(K57<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K57<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O57*Main!$D$45/100000+P56,IF(K57<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S57))))),(IF(K57<=(Main!$D$72/Main!$D$71*100),O57*Main!$D$71/100000+P56,IF(K57<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K57<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O57*Main!$D$71/100000+P56,IF(K57<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S57))))))","v":40},{"$f":"IF($A$90=TRUE,P57*Main!$D$45/100000+Q56,P57*100+Q56)","v":94.075521645498767},{"$f":"IF($A$90=TRUE,(IF(K57<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K57-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K57<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K57<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K57-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K57<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K57-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K57<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K57<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K57-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2842604.668028092},{"$f":"IF($A$90=TRUE,(IF(K57<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O57*Main!$D$45/100000+P56,IF(K57<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K57<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O57*Main!$D$45/100000+P56,Main!$E$52)))),(IF(K57<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O57*Main!$D$71/100000+P56,IF(K57<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K57<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O57*Main!$D$71/100000+P56,Main!$E$78)))))","v":40},56,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T57-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T57-50)*PI()/50))))","v":11333.700928199005},{"$f":"IF($A$90=TRUE,U57*2*Main!$D$50*(T57-T56)/100000+V56,U57*2*Ltime3*(T57-T56)/100000+V56)","v":127.54492632881229},0.29818088767458911,6.3772463164406143E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W57*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W57<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W57*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W57<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W57*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W57<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W57*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W57<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W57*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W57<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W57*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W57<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":15.195409353078793},8.1197621966088409]
[null,7.5,{"$f":"torque2","v":7.5},null,null,null,null,null,null,null,57,0,0.02,0.11576229749966803,{"$f":"IF($A$90=TRUE,(IF(K58<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K58*PI()*Main!$D$45/100/Main!$D$46))),(IF(K58<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K58<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K58-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K58<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R58)))))))),(IF(K58<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K58*PI()*Main!$D$71/100/Main!$D$72))),(IF(K58<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K58<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K58-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K58<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R58)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K58<=(Main!$D$46/Main!$D$45*100),O58*Main!$D$45/100000+P57,IF(K58<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K58<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O58*Main!$D$45/100000+P57,IF(K58<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S58))))),(IF(K58<=(Main!$D$72/Main!$D$71*100),O58*Main!$D$71/100000+P57,IF(K58<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K58<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O58*Main!$D$71/100000+P57,IF(K58<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S58))))))","v":40},{"$f":"IF($A$90=TRUE,P58*Main!$D$45/100000+Q57,P58*100+Q57)","v":95.067921645498771},{"$f":"IF($A$90=TRUE,(IF(K58<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K58-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K58<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K58<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K58-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K58<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K58-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K58<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K58<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K58-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":1599204.5117219184},{"$f":"IF($A$90=TRUE,(IF(K58<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O58*Main!$D$45/100000+P57,IF(K58<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K58<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O58*Main!$D$45/100000+P57,Main!$E$52)))),(IF(K58<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O58*Main!$D$71/100000+P57,IF(K58<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K58<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O58*Main!$D$71/100000+P57,Main!$E$78)))))","v":40},57,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T58-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T58-50)*PI()/50))))","v":13108.756579332156},{"$f":"IF($A$90=TRUE,U58*2*Main!$D$50*(T58-T57)/100000+V57,U58*2*Ltime3*(T58-T57)/100000+V57)","v":153.7624394874766},0.34488122616770883,7.6881219743738294E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W58*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W58<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W58*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W58<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W58*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W58<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W58*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W58<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W58*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W58<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W58*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W58<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":16.635571171364823},9.7888209225201344]
[null,1.5,{"$f":"DryTorq","v":1.5},null,null,null,null,null,null,null,58,0,0.02,0.11697072303427747,{"$f":"IF($A$90=TRUE,(IF(K59<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K59*PI()*Main!$D$45/100/Main!$D$46))),(IF(K59<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K59<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K59-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K59<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R59)))))))),(IF(K59<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K59*PI()*Main!$D$71/100/Main!$D$72))),(IF(K59<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K59<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K59-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K59<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R59)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K59<=(Main!$D$46/Main!$D$45*100),O59*Main!$D$45/100000+P58,IF(K59<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K59<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O59*Main!$D$45/100000+P58,IF(K59<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S59))))),(IF(K59<=(Main!$D$72/Main!$D$71*100),O59*Main!$D$71/100000+P58,IF(K59<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K59<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O59*Main!$D$71/100000+P58,IF(K59<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S59))))))","v":40},{"$f":"IF($A$90=TRUE,P59*Main!$D$45/100000+Q58,P59*100+Q58)","v":96.060321645498775},{"$f":"IF($A$90=TRUE,(IF(K59<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K59-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K59<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K59<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K59-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K59<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K59-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K59<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K59<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K59-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":197262.69615399232},{"$f":"IF($A$90=TRUE,(IF(K59<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O59*Main!$D$45/100000+P58,IF(K59<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K59<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O59*Main!$D$45/100000+P58,Main!$E$52)))),(IF(K59<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O59*Main!$D$71/100000+P58,IF(K59<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K59<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O59*Main!$D$71/100000+P58,Main!$E$78)))))","v":40},58,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T59-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T59-50)*PI()/50))))","v":14832.077957067899},{"$f":"IF($A$90=TRUE,U59*2*Main!$D$50*(T59-T58)/100000+V58,U59*2*Ltime3*(T59-T58)/100000+V58)","v":183.42659540161239},0.39022047602238941,9.171329770080619E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W59*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W59<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W59*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W59<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W59*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W59<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W59*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W59<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W59*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W59<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W59*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W59<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":18.033759249167755},11.677299741073492]
[15,1.5,{"$f":"DryTorq2","v":1.5},null,null,null,null,null,null,null,59,0,0.02,0.11817914856888692,{"$f":"IF($A$90=TRUE,(IF(K60<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K60*PI()*Main!$D$45/100/Main!$D$46))),(IF(K60<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K60<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K60-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K60<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R60)))))))),(IF(K60<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K60*PI()*Main!$D$71/100/Main!$D$72))),(IF(K60<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K60<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K60-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K60<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R60)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K60<=(Main!$D$46/Main!$D$45*100),O60*Main!$D$45/100000+P59,IF(K60<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K60<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O60*Main!$D$45/100000+P59,IF(K60<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S60))))),(IF(K60<=(Main!$D$72/Main!$D$71*100),O60*Main!$D$71/100000+P59,IF(K60<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K60<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O60*Main!$D$71/100000+P59,IF(K60<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S60))))))","v":40},{"$f":"IF($A$90=TRUE,P60*Main!$D$45/100000+Q59,P60*100+Q59)","v":97.052721645498778},{"$f":"IF($A$90=TRUE,(IF(K60<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K60-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K60<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K60<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K60-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K60<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K60-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K60<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K60<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K60-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-1925508.7997544215},{"$f":"IF($A$90=TRUE,(IF(K60<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O60*Main!$D$45/100000+P59,IF(K60<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K60<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O60*Main!$D$45/100000+P59,Main!$E$52)))),(IF(K60<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O60*Main!$D$71/100000+P59,IF(K60<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K60<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O60*Main!$D$71/100000+P59,Main!$E$78)))))","v":40},59,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T60-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T60-50)*PI()/50))))","v":16496.863899238957},{"$f":"IF($A$90=TRUE,U60*2*Main!$D$50*(T60-T59)/100000+V59,U60*2*Ltime3*(T60-T59)/100000+V59)","v":216.42032320009031},0.43401970393298733,0.10821016160004515,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W60*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W60<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W60*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W60<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W60*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W60<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W60*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W60<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W60*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W60<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W60*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W60<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":19.384455576915876},13.777745689135987]
[10,null,null,null,null,null,null,null,null,null,60,0,0.02,0.11938757410349637,{"$f":"IF($A$90=TRUE,(IF(K61<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K61*PI()*Main!$D$45/100/Main!$D$46))),(IF(K61<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K61<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K61-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K61<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R61)))))))),(IF(K61<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K61*PI()*Main!$D$71/100/Main!$D$72))),(IF(K61<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K61<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K61-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K61<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R61)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K61<=(Main!$D$46/Main!$D$45*100),O61*Main!$D$45/100000+P60,IF(K61<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K61<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O61*Main!$D$45/100000+P60,IF(K61<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S61))))),(IF(K61<=(Main!$D$72/Main!$D$71*100),O61*Main!$D$71/100000+P60,IF(K61<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K61<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O61*Main!$D$71/100000+P60,IF(K61<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S61))))))","v":40},{"$f":"IF($A$90=TRUE,P61*Main!$D$45/100000+Q60,P61*100+Q60)","v":98.045121645498782},{"$f":"IF($A$90=TRUE,(IF(K61<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K61-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K61<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K61<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K61-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K61<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K61-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K61<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K61<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K61-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2987839.1515925778},{"$f":"IF($A$90=TRUE,(IF(K61<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O61*Main!$D$45/100000+P60,IF(K61<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K61<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O61*Main!$D$45/100000+P60,Main!$E$52)))),(IF(K61<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O61*Main!$D$71/100000+P60,IF(K61<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K61<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O61*Main!$D$71/100000+P60,Main!$E$78)))))","v":40},60,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T61-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T61-50)*PI()/50))))","v":18096.544256299931},{"$f":"IF($A$90=TRUE,U61*2*Main!$D$50*(T61-T60)/100000+V60,U61*2*Ltime3*(T61-T60)/100000+V60)","v":252.61341171269015},0.47610605435690329,0.12630670585634507,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W61*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W61<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W61*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W61<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W61*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W61<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W61*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W61<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W61*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W61<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W61*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W61<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":20.682329573278011},16.081869266153092]
[8,null,null,null,null,null,null,null,null,null,61,0,0.02,0.12059599963810581,{"$f":"IF($A$90=TRUE,(IF(K62<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K62*PI()*Main!$D$45/100/Main!$D$46))),(IF(K62<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K62<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K62-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K62<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R62)))))))),(IF(K62<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K62*PI()*Main!$D$71/100/Main!$D$72))),(IF(K62<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K62<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K62-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K62<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R62)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K62<=(Main!$D$46/Main!$D$45*100),O62*Main!$D$45/100000+P61,IF(K62<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K62<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O62*Main!$D$45/100000+P61,IF(K62<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S62))))),(IF(K62<=(Main!$D$72/Main!$D$71*100),O62*Main!$D$71/100000+P61,IF(K62<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K62<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O62*Main!$D$71/100000+P61,IF(K62<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S62))))))","v":40},{"$f":"IF($A$90=TRUE,P62*Main!$D$45/100000+Q61,P62*100+Q61)","v":99.037521645498785},{"$f":"IF($A$90=TRUE,(IF(K62<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K62-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K62<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K62<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K62-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K62<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K62-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K62<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K62<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K62-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-3016858.6429225593},{"$f":"IF($A$90=TRUE,(IF(K62<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O62*Main!$D$45/100000+P61,IF(K62<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K62<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O62*Main!$D$45/100000+P61,Main!$E$52)))),(IF(K62<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O62*Main!$D$71/100000+P61,IF(K62<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K62<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O62*Main!$D$71/100000+P61,Main!$E$78)))))","v":40},61,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T62-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T62-50)*PI()/50))))","v":19624.805820705937},{"$f":"IF($A$90=TRUE,U62*2*Main!$D$50*(T62-T61)/100000+V61,U62*2*Ltime3*(T62-T61)/100000+V61)","v":291.86302335410204},0.51631343169643862,0.14593151167705101,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W62*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W62<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W62*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W62<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W62*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W62<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W62*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W62<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W62*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W62<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W62*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W62<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":21.922259122532751},18.58057714902025]
[6,null,null,null,null,null,null,null,null,null,62,0,0.02,0.12180442517271527,{"$f":"IF($A$90=TRUE,(IF(K63<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K63*PI()*Main!$D$45/100/Main!$D$46))),(IF(K63<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K63<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K63-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K63<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R63)))))))),(IF(K63<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K63*PI()*Main!$D$71/100/Main!$D$72))),(IF(K63<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K63<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K63-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K63<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R63)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K63<=(Main!$D$46/Main!$D$45*100),O63*Main!$D$45/100000+P62,IF(K63<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K63<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O63*Main!$D$45/100000+P62,IF(K63<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S63))))),(IF(K63<=(Main!$D$72/Main!$D$71*100),O63*Main!$D$71/100000+P62,IF(K63<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K63<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O63*Main!$D$71/100000+P62,IF(K63<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S63))))))","v":40},{"$f":"IF($A$90=TRUE,P63*Main!$D$45/100000+Q62,P63*100+Q62)","v":100.02992164549879},{"$f":"IF($A$90=TRUE,(IF(K63<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K63-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K63<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K63<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K63-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K63<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K63-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K63<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K63<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K63-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2002531.2061953039},{"$f":"IF($A$90=TRUE,(IF(K63<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O63*Main!$D$45/100000+P62,IF(K63<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K63<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O63*Main!$D$45/100000+P62,Main!$E$52)))),(IF(K63<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O63*Main!$D$71/100000+P62,IF(K63<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K63<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O63*Main!$D$71/100000+P62,Main!$E$78)))))","v":40},62,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T63-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T63-50)*PI()/50))))","v":21075.61724225857},{"$f":"IF($A$90=TRUE,U63*2*Main!$D$50*(T63-T62)/100000+V62,U63*2*Ltime3*(T63-T62)/100000+V62)","v":334.01425783861919},0.55448315580223784,0.16700712891930961,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W63*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W63<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W63*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W63<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W63*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W63<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W63*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W63<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W63*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W63<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W63*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W63<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":23.09935078921912},21.264008079274838]
[20,null,null,null,null,null,null,null,null,null,63,0,0.02,0.12301285070732472,{"$f":"IF($A$90=TRUE,(IF(K64<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K64*PI()*Main!$D$45/100/Main!$D$46))),(IF(K64<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K64<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K64-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K64<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R64)))))))),(IF(K64<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K64*PI()*Main!$D$71/100/Main!$D$72))),(IF(K64<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K64<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K64-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K64<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R64)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K64<=(Main!$D$46/Main!$D$45*100),O64*Main!$D$45/100000+P63,IF(K64<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K64<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O64*Main!$D$45/100000+P63,IF(K64<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S64))))),(IF(K64<=(Main!$D$72/Main!$D$71*100),O64*Main!$D$71/100000+P63,IF(K64<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K64<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O64*Main!$D$71/100000+P63,IF(K64<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S64))))))","v":40},{"$f":"IF($A$90=TRUE,P64*Main!$D$45/100000+Q63,P64*100+Q63)","v":101.02232164549879},{"$f":"IF($A$90=TRUE,(IF(K64<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K64-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K64<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K64<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K64-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K64<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K64-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K64<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K64<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K64-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-295650.67712116684},{"$f":"IF($A$90=TRUE,(IF(K64<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O64*Main!$D$45/100000+P63,IF(K64<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K64<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O64*Main!$D$45/100000+P63,Main!$E$52)))),(IF(K64<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O64*Main!$D$71/100000+P63,IF(K64<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K64<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O64*Main!$D$71/100000+P63,Main!$E$78)))))","v":40},63,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T64-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T64-50)*PI()/50))))","v":22443.252831089645},{"$f":"IF($A$90=TRUE,U64*2*Main!$D$50*(T64-T63)/100000+V63,U64*2*Ltime3*(T64-T63)/100000+V63)","v":378.90076350079846},0.5904645882113434,0.18945038175039924,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W64*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W64<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W64*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W64<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W64*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W64<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W64*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W64<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W64*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W64<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W64*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W64<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":24.208959130290733},24.121571780978112]
[20,null,null,null,null,null,null,null,null,null,64,0,0.02,0.12422127624193416,{"$f":"IF($A$90=TRUE,(IF(K65<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K65*PI()*Main!$D$45/100/Main!$D$46))),(IF(K65<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K65<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K65-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K65<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R65)))))))),(IF(K65<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K65*PI()*Main!$D$71/100/Main!$D$72))),(IF(K65<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K65<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K65-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K65<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R65)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K65<=(Main!$D$46/Main!$D$45*100),O65*Main!$D$45/100000+P64,IF(K65<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K65<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O65*Main!$D$45/100000+P64,IF(K65<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S65))))),(IF(K65<=(Main!$D$72/Main!$D$71*100),O65*Main!$D$71/100000+P64,IF(K65<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K65<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O65*Main!$D$71/100000+P64,IF(K65<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S65))))))","v":40},{"$f":"IF($A$90=TRUE,P65*Main!$D$45/100000+Q64,P65*100+Q64)","v":102.0147216454988},{"$f":"IF($A$90=TRUE,(IF(K65<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K65-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K65<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K65<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K65-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K65<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K65-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K65<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K65<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K65-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-1513477.3425568668},{"$f":"IF($A$90=TRUE,(IF(K65<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O65*Main!$D$45/100000+P64,IF(K65<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K65<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O65*Main!$D$45/100000+P64,Main!$E$52)))),(IF(K65<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O65*Main!$D$71/100000+P64,IF(K65<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K65<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O65*Main!$D$71/100000+P64,Main!$E$78)))))","v":40},64,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T65-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T65-50)*PI()/50))))","v":23722.315154343312},{"$f":"IF($A$90=TRUE,U65*2*Main!$D$50*(T65-T64)/100000+V64,U65*2*Ltime3*(T65-T64)/100000+V64)","v":426.34539380948507},0.62411572664838932,0.21317269690474253,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W65*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W65<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W65*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W65<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W65*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W65<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W65*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W65<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W65*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W65<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W65*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W65<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":25.246705028557209},27.141990755696121]
[null,null,null,null,null,null,null,null,null,null,65,{"$f":"IF(ABS(MIN($O$1:$O$100))>MAX($O$1:$O$100),O66/MIN($O$1:$O$100)*-1,O66/MAX($O$1:$O$100))","v":0},{"$f":"IF(ABS(MIN($P$1:$P$100))>MAX($P$1:$P$100),P66/MIN($P$1:$P$100)*-1,P66/MAX($P$1:$P$100))","v":0.02},{"$f":"IF(ABS(MIN($Q$1:$Q$100))>MAX($Q$1:$Q$100),Q66/MIN($Q$1:$Q$100)*-1,Q66/MAX($Q$1:$Q$100))","v":0.12542970177654361},{"$f":"IF($A$90=TRUE,(IF(K66<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K66*PI()*Main!$D$45/100/Main!$D$46))),(IF(K66<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K66<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K66-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K66<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R66)))))))),(IF(K66<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K66*PI()*Main!$D$71/100/Main!$D$72))),(IF(K66<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K66<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K66-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K66<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R66)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K66<=(Main!$D$46/Main!$D$45*100),O66*Main!$D$45/100000+P65,IF(K66<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K66<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O66*Main!$D$45/100000+P65,IF(K66<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S66))))),(IF(K66<=(Main!$D$72/Main!$D$71*100),O66*Main!$D$71/100000+P65,IF(K66<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K66<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O66*Main!$D$71/100000+P65,IF(K66<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S66))))))","v":40},{"$f":"IF($A$90=TRUE,P66*Main!$D$45/100000+Q65,P66*100+Q65)","v":103.0071216454988},{"$f":"IF($A$90=TRUE,(IF(K66<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K66-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K66<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K66<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K66-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K66<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K66-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K66<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K66<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K66-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2799186.0963902259},{"$f":"IF($A$90=TRUE,(IF(K66<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O66*Main!$D$45/100000+P65,IF(K66<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K66<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O66*Main!$D$45/100000+P65,Main!$E$52)))),(IF(K66<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O66*Main!$D$71/100000+P65,IF(K66<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K66<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O66*Main!$D$71/100000+P65,Main!$E$78)))))","v":40},65,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T66-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T66-50)*PI()/50))))","v":24907.756337377679},{"$f":"IF($A$90=TRUE,U66*2*Main!$D$50*(T66-T65)/100000+V65,U66*2*Ltime3*(T66-T65)/100000+V65)","v":476.16090648424046},{"$f":"IF(move1,IF(ABS(MIN($U$1:$U$101))>MAX($U$1:$U$101),U66/MIN($U$1:$U$101)*-1,U66/MAX($U$1:$U$101)),IF(ABS(MIN($U$1:$U$201))>MAX($U$1:$U$201),U66/MIN($U$1:$U$201)*-1,U66/MAX($U$1:$U$201)))","v":0.65530376544370739},{"$f":"IF(move1,IF(ABS(MIN($V$1:$V$101))>MAX($V$1:$V$101),V66/MIN($V$1:$V$101)*-1,V66/MAX($V$1:$V$101)),IF(ABS(MIN($V$1:$V$201))>MAX($V$1:$V$201),V66/MIN($V$1:$V$201)*-1,V66/MAX($V$1:$V$201)))","v":0.23808045324212024},{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W66*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W66<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W66*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W66<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W66*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W66<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W66*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W66<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W66*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W66<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W66*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W66<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":26.208492975059094},30.313344789633835]
[null,null,null,null,null,null,null,null,null,null,66,0,0.02,0.12663812731115306,{"$f":"IF($A$90=TRUE,(IF(K67<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K67*PI()*Main!$D$45/100/Main!$D$46))),(IF(K67<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K67<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K67-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K67<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R67)))))))),(IF(K67<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K67*PI()*Main!$D$71/100/Main!$D$72))),(IF(K67<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K67<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K67-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K67<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R67)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K67<=(Main!$D$46/Main!$D$45*100),O67*Main!$D$45/100000+P66,IF(K67<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K67<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O67*Main!$D$45/100000+P66,IF(K67<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S67))))),(IF(K67<=(Main!$D$72/Main!$D$71*100),O67*Main!$D$71/100000+P66,IF(K67<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K67<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O67*Main!$D$71/100000+P66,IF(K67<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S67))))))","v":40},{"$f":"IF($A$90=TRUE,P67*Main!$D$45/100000+Q66,P67*100+Q66)","v":103.9995216454988},{"$f":"IF($A$90=TRUE,(IF(K67<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K67-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K67<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K67<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K67-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K67<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K67-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K67<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K67<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K67-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-3116827.5456493814},{"$f":"IF($A$90=TRUE,(IF(K67<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O67*Main!$D$45/100000+P66,IF(K67<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K67<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O67*Main!$D$45/100000+P66,Main!$E$52)))),(IF(K67<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O67*Main!$D$71/100000+P66,IF(K67<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K67<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O67*Main!$D$71/100000+P66,Main!$E$78)))))","v":40},66,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T67-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T67-50)*PI()/50))))","v":25994.897985419881},{"$f":"IF($A$90=TRUE,U67*2*Main!$D$50*(T67-T66)/100000+V66,U67*2*Ltime3*(T67-T66)/100000+V66)","v":528.15070245508025},0.68390561965663221,0.26407535122754011,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W67*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W67<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W67*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W67<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W67*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W67<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W67*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W67<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W67*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W67<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W67*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W67<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":27.090527232170661},{"$f":"IF(move1,ABS(IF($A$90=TRUE,X67*speed,X67*MAX(ABS(Lspeed1),ABS(Lspeed2)))),ABS(IF($A$90=TRUE,X67*speed,X67*MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6)))))","v":33.623117997273134}]
[null,null,null,null,null,null,null,null,null,null,67,0,0.02,0.12784655284576252,{"$f":"IF($A$90=TRUE,(IF(K68<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K68*PI()*Main!$D$45/100/Main!$D$46))),(IF(K68<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K68<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K68-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K68<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R68)))))))),(IF(K68<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K68*PI()*Main!$D$71/100/Main!$D$72))),(IF(K68<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K68<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K68-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K68<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R68)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K68<=(Main!$D$46/Main!$D$45*100),O68*Main!$D$45/100000+P67,IF(K68<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K68<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O68*Main!$D$45/100000+P67,IF(K68<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S68))))),(IF(K68<=(Main!$D$72/Main!$D$71*100),O68*Main!$D$71/100000+P67,IF(K68<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K68<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O68*Main!$D$71/100000+P67,IF(K68<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S68))))))","v":40},{"$f":"IF($A$90=TRUE,P68*Main!$D$45/100000+Q67,P68*100+Q67)","v":104.99192164549881},{"$f":"IF($A$90=TRUE,(IF(K68<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K68-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K68<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K68<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K68-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K68<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K68-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K68<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K68<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K68-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2356548.9363510911},{"$f":"IF($A$90=TRUE,(IF(K68<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O68*Main!$D$45/100000+P67,IF(K68<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K68<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O68*Main!$D$45/100000+P67,Main!$E$52)))),(IF(K68<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O68*Main!$D$71/100000+P67,IF(K68<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K68<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O68*Main!$D$71/100000+P67,Main!$E$78)))))","v":40},67,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T68-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T68-50)*PI()/50))))","v":26979.449647052861},{"$f":"IF($A$90=TRUE,U68*2*Main!$D$50*(T68-T67)/100000+V67,U68*2*Ltime3*(T68-T67)/100000+V67)","v":582.10960174918591},0.70980841083552959,0.29105480087459296,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W68*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W68<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W68*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W68<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W68*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W68<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W68*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W68<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W68*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W68<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W68*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W68<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":27.889326813642224},37.058248215855016]
[null,null,null,null,null,null,null,null,null,null,68,0,0.02,0.12905497838037194,{"$f":"IF($A$90=TRUE,(IF(K69<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K69*PI()*Main!$D$45/100/Main!$D$46))),(IF(K69<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K69<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K69-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K69<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R69)))))))),(IF(K69<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K69*PI()*Main!$D$71/100/Main!$D$72))),(IF(K69<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K69<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K69-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K69<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R69)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K69<=(Main!$D$46/Main!$D$45*100),O69*Main!$D$45/100000+P68,IF(K69<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K69<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O69*Main!$D$45/100000+P68,IF(K69<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S69))))),(IF(K69<=(Main!$D$72/Main!$D$71*100),O69*Main!$D$71/100000+P68,IF(K69<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K69<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O69*Main!$D$71/100000+P68,IF(K69<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S69))))))","v":40},{"$f":"IF($A$90=TRUE,P69*Main!$D$45/100000+Q68,P69*100+Q68)","v":105.98432164549881},{"$f":"IF($A$90=TRUE,(IF(K69<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K69-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K69<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K69<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K69-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K69<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K69-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K69<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K69<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K69-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-781284.14951724815},{"$f":"IF($A$90=TRUE,(IF(K69<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O69*Main!$D$45/100000+P68,IF(K69<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K69<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O69*Main!$D$45/100000+P68,Main!$E$52)))),(IF(K69<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O69*Main!$D$71/100000+P68,IF(K69<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K69<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O69*Main!$D$71/100000+P68,Main!$E$78)))))","v":40},68,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T69-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T69-50)*PI()/50))))","v":27857.525746667023},{"$f":"IF($A$90=TRUE,U69*2*Main!$D$50*(T69-T68)/100000+V68,U69*2*Ltime3*(T69-T68)/100000+V68)","v":637.82465324251996},0.73290991249747584,0.31891232662125996,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W69*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W69<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W69*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W69<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W69*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W69<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W69*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W69<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W69*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W69<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W69*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W69<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":28.601739222462506},40.605178555768454]
["AKM73M",null,null,null,null,null,null,null,null,null,69,0,0.02,0.1302634039149814,{"$f":"IF($A$90=TRUE,(IF(K70<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K70*PI()*Main!$D$45/100/Main!$D$46))),(IF(K70<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K70<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K70-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K70<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R70)))))))),(IF(K70<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K70*PI()*Main!$D$71/100/Main!$D$72))),(IF(K70<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K70<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K70-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K70<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R70)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K70<=(Main!$D$46/Main!$D$45*100),O70*Main!$D$45/100000+P69,IF(K70<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K70<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O70*Main!$D$45/100000+P69,IF(K70<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S70))))),(IF(K70<=(Main!$D$72/Main!$D$71*100),O70*Main!$D$71/100000+P69,IF(K70<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K70<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O70*Main!$D$71/100000+P69,IF(K70<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S70))))))","v":40},{"$f":"IF($A$90=TRUE,P70*Main!$D$45/100000+Q69,P70*100+Q69)","v":106.97672164549881},{"$f":"IF($A$90=TRUE,(IF(K70<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K70-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K70<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K70<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K70-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K70<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K70-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K70<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K70<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K70-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-1064179.0502423912},{"$f":"IF($A$90=TRUE,(IF(K70<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O70*Main!$D$45/100000+P69,IF(K70<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K70<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O70*Main!$D$45/100000+P69,Main!$E$52)))),(IF(K70<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O70*Main!$D$71/100000+P69,IF(K70<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K70<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O70*Main!$D$71/100000+P69,Main!$E$78)))))","v":40},69,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T70-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T70-50)*PI()/50))))","v":28625.660919051999},{"$f":"IF($A$90=TRUE,U70*2*Main!$D$50*(T70-T69)/100000+V69,U70*2*Ltime3*(T70-T69)/100000+V69)","v":695.07597508062395},0.75311895356948366,0.34753798754031195,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W70*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W70<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W70*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W70<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W70*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W70<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W70*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W70<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W70*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W70<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W70*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W70<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":29.224952892324193},44.249910903400142]
[false,null,null,null,null,null,null,null,null,null,70,0,0.02,0.13147182944959085,{"$f":"IF($A$90=TRUE,(IF(K71<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K71*PI()*Main!$D$45/100/Main!$D$46))),(IF(K71<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K71<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K71-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K71<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R71)))))))),(IF(K71<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K71*PI()*Main!$D$71/100/Main!$D$72))),(IF(K71<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K71<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K71-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K71<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R71)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K71<=(Main!$D$46/Main!$D$45*100),O71*Main!$D$45/100000+P70,IF(K71<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K71<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O71*Main!$D$45/100000+P70,IF(K71<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S71))))),(IF(K71<=(Main!$D$72/Main!$D$71*100),O71*Main!$D$71/100000+P70,IF(K71<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K71<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O71*Main!$D$71/100000+P70,IF(K71<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S71))))))","v":40},{"$f":"IF($A$90=TRUE,P71*Main!$D$45/100000+Q70,P71*100+Q70)","v":107.96912164549882},{"$f":"IF($A$90=TRUE,(IF(K71<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K71-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K71<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K71<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K71-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K71<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K71-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K71<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K71<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K71-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2541607.7895281501},{"$f":"IF($A$90=TRUE,(IF(K71<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O71*Main!$D$45/100000+P70,IF(K71<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K71<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O71*Main!$D$45/100000+P70,Main!$E$52)))),(IF(K71<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O71*Main!$D$71/100000+P70,IF(K71<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K71<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O71*Main!$D$71/100000+P70,Main!$E$78)))))","v":40},70,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T71-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T71-50)*PI()/50))))","v":29280.823685609972},{"$f":"IF($A$90=TRUE,U71*2*Main!$D$50*(T71-T70)/100000+V70,U71*2*Ltime3*(T71-T70)/100000+V70)","v":753.63762245184387},0.7703557781990743,0.37681881122592192,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W71*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W71<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W71*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W71<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W71*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W71<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W71*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W71<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W71*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W71<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W71*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W71<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":29.756508283591558},47.978061165293802]
[{"$f":"IF(A71,10,1)","v":1},null,null,null,null,null,null,null,null,null,71,0,0.02,0.1326802549842003,{"$f":"IF($A$90=TRUE,(IF(K72<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K72*PI()*Main!$D$45/100/Main!$D$46))),(IF(K72<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K72<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K72-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K72<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R72)))))))),(IF(K72<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K72*PI()*Main!$D$71/100/Main!$D$72))),(IF(K72<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K72<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K72-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K72<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R72)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K72<=(Main!$D$46/Main!$D$45*100),O72*Main!$D$45/100000+P71,IF(K72<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K72<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O72*Main!$D$45/100000+P71,IF(K72<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S72))))),(IF(K72<=(Main!$D$72/Main!$D$71*100),O72*Main!$D$71/100000+P71,IF(K72<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K72<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O72*Main!$D$71/100000+P71,IF(K72<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S72))))))","v":40},{"$f":"IF($A$90=TRUE,P72*Main!$D$45/100000+Q71,P72*100+Q71)","v":108.96152164549882},{"$f":"IF($A$90=TRUE,(IF(K72<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K72-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K72<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K72<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K72-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K72<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K72-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K72<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K72<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K72-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-3140049.8100449699},{"$f":"IF($A$90=TRUE,(IF(K72<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O72*Main!$D$45/100000+P71,IF(K72<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K72<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O72*Main!$D$45/100000+P71,Main!$E$52)))),(IF(K72<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O72*Main!$D$71/100000+P71,IF(K72<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K72<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O72*Main!$D$71/100000+P71,Main!$E$78)))))","v":40},71,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T72-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T72-50)*PI()/50))))","v":29820.428418216732},{"$f":"IF($A$90=TRUE,U72*2*Main!$D$50*(T72-T71)/100000+V71,U72*2*Ltime3*(T72-T71)/100000+V71)","v":813.27847928827737},0.78455236051419119,0.40663923964413867,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W72*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W72<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W72*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W72<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W72*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W72<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W72*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W72<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W72*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W72<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W72*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W72<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":30.194307589979843},51.774916035595581]
[null,null,null,null,null,null,null,null,null,null,72,0,0.02,0.13388868051880976,{"$f":"IF($A$90=TRUE,(IF(K73<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K73*PI()*Main!$D$45/100/Main!$D$46))),(IF(K73<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K73<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K73-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K73<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R73)))))))),(IF(K73<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K73*PI()*Main!$D$71/100/Main!$D$72))),(IF(K73<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K73<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K73-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K73<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R73)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K73<=(Main!$D$46/Main!$D$45*100),O73*Main!$D$45/100000+P72,IF(K73<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K73<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O73*Main!$D$45/100000+P72,IF(K73<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S73))))),(IF(K73<=(Main!$D$72/Main!$D$71*100),O73*Main!$D$71/100000+P72,IF(K73<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K73<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O73*Main!$D$71/100000+P72,IF(K73<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S73))))))","v":40},{"$f":"IF($A$90=TRUE,P73*Main!$D$45/100000+Q72,P73*100+Q72)","v":109.95392164549882},{"$f":"IF($A$90=TRUE,(IF(K73<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K73-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K73<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K73<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K73-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K73<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K73-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K73<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K73<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K73-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2652540.6107573896},{"$f":"IF($A$90=TRUE,(IF(K73<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O73*Main!$D$45/100000+P72,IF(K73<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K73<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O73*Main!$D$45/100000+P72,Main!$E$52)))),(IF(K73<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O73*Main!$D$71/100000+P72,IF(K73<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K73<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O73*Main!$D$71/100000+P72,Main!$E$78)))))","v":40},72,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T73-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T73-50)*PI()/50))))","v":30242.345543514632},{"$f":"IF($A$90=TRUE,U73*2*Main!$D$50*(T73-T72)/100000+V72,U73*2*Ltime3*(T73-T72)/100000+V72)","v":873.76317037530657},0.79565267309023779,0.4368815851876533,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W73*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W73<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W73*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W73<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W73*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W73<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W73*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W73<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W73*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W73<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W73*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W73<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":30.536623017638206},55.625491062750385]
[null,null,null,null,null,null,null,null,null,null,73,0,0.02,0.13509710605341918,{"$f":"IF($A$90=TRUE,(IF(K74<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K74*PI()*Main!$D$45/100/Main!$D$46))),(IF(K74<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K74<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K74-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K74<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R74)))))))),(IF(K74<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K74*PI()*Main!$D$71/100/Main!$D$72))),(IF(K74<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K74<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K74-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K74<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R74)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K74<=(Main!$D$46/Main!$D$45*100),O74*Main!$D$45/100000+P73,IF(K74<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K74<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O74*Main!$D$45/100000+P73,IF(K74<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S74))))),(IF(K74<=(Main!$D$72/Main!$D$71*100),O74*Main!$D$71/100000+P73,IF(K74<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K74<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O74*Main!$D$71/100000+P73,IF(K74<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S74))))))","v":40},{"$f":"IF($A$90=TRUE,P74*Main!$D$45/100000+Q73,P74*100+Q73)","v":110.94632164549883},{"$f":"IF($A$90=TRUE,(IF(K74<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K74-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K74<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K74<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K74-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K74<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K74-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K74<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K74<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K74-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-1247679.8132187487},{"$f":"IF($A$90=TRUE,(IF(K74<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O74*Main!$D$45/100000+P73,IF(K74<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K74<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O74*Main!$D$45/100000+P73,Main!$E$52)))),(IF(K74<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O74*Main!$D$71/100000+P73,IF(K74<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K74<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O74*Main!$D$71/100000+P73,Main!$E$78)))))","v":40},73,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T74-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T74-50)*PI()/50))))","v":30544.909947365722},{"$f":"IF($A$90=TRUE,U74*2*Main!$D$50*(T74-T73)/100000+V73,U74*2*Ltime3*(T74-T73)/100000+V73)","v":934.85299027003805},0.80361290806472707,0.46742649513501905,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W74*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W74<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W74*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W74<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W74*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W74<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W74*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W74<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W74*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W74<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W74*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W74<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":30.782103603962724},59.514589786286436]
[null,null,null,null,null,null,null,null,null,null,74,0,0.02,0.13630553158802863,{"$f":"IF($A$90=TRUE,(IF(K75<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K75*PI()*Main!$D$45/100/Main!$D$46))),(IF(K75<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K75<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K75-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K75<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R75)))))))),(IF(K75<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K75*PI()*Main!$D$71/100/Main!$D$72))),(IF(K75<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K75<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K75-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K75<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R75)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K75<=(Main!$D$46/Main!$D$45*100),O75*Main!$D$45/100000+P74,IF(K75<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K75<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O75*Main!$D$45/100000+P74,IF(K75<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S75))))),(IF(K75<=(Main!$D$72/Main!$D$71*100),O75*Main!$D$71/100000+P74,IF(K75<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K75<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O75*Main!$D$71/100000+P74,IF(K75<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S75))))))","v":40},{"$f":"IF($A$90=TRUE,P75*Main!$D$45/100000+Q74,P75*100+Q74)","v":111.93872164549883},{"$f":"IF($A$90=TRUE,(IF(K75<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K75-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K75<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K75<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K75-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K75<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K75-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K75<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K75<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K75-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-588677.13790257229},{"$f":"IF($A$90=TRUE,(IF(K75<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O75*Main!$D$45/100000+P74,IF(K75<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K75<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O75*Main!$D$45/100000+P74,Main!$E$52)))),(IF(K75<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O75*Main!$D$71/100000+P74,IF(K75<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K75<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O75*Main!$D$71/100000+P74,Main!$E$78)))))","v":40},74,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T75-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T75-50)*PI()/50))))","v":30726.927546296527},{"$f":"IF($A$90=TRUE,U75*2*Main!$D$50*(T75-T74)/100000+V74,U75*2*Ltime3*(T75-T74)/100000+V74)","v":996.30684536263107},0.8084016500268999,0.49815342268131552,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W75*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W75<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W75*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W75<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W75*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W75<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W75*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W75<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W75*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W75<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W75*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W75<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":30.929780549228582},63.426863710302122]
[null,null,null,null,null,null,null,null,null,null,75,0,0.02,0.13751395712263809,{"$f":"IF($A$90=TRUE,(IF(K76<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K76*PI()*Main!$D$45/100/Main!$D$46))),(IF(K76<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K76<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K76-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K76<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R76)))))))),(IF(K76<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K76*PI()*Main!$D$71/100/Main!$D$72))),(IF(K76<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K76<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K76-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K76<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R76)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K76<=(Main!$D$46/Main!$D$45*100),O76*Main!$D$45/100000+P75,IF(K76<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K76<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O76*Main!$D$45/100000+P75,IF(K76<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S76))))),(IF(K76<=(Main!$D$72/Main!$D$71*100),O76*Main!$D$71/100000+P75,IF(K76<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K76<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O76*Main!$D$71/100000+P75,IF(K76<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S76))))))","v":40},{"$f":"IF($A$90=TRUE,P76*Main!$D$45/100000+Q75,P76*100+Q75)","v":112.93112164549883},{"$f":"IF($A$90=TRUE,(IF(K76<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K76-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K76<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K76<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K76-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K76<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K76-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K76<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K76<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K76-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2221446.6637756405},{"$f":"IF($A$90=TRUE,(IF(K76<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O76*Main!$D$45/100000+P75,IF(K76<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K76<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O76*Main!$D$45/100000+P75,Main!$E$52)))),(IF(K76<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O76*Main!$D$71/100000+P75,IF(K76<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K76<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O76*Main!$D$71/100000+P75,Main!$E$78)))))","v":40},75,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T76-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T76-50)*PI()/50))))","v":30787.68},{"$f":"IF($A$90=TRUE,U76*2*Main!$D$50*(T76-T75)/100000+V75,U76*2*Ltime3*(T76-T75)/100000+V75)","v":1057.8822053626311},0.81,0.52894110268131556,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W76*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W76<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W76*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W76<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W76*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W76<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W76*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W76<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W76*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W76<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W76*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W76<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":30.979071040000001},67.346872876967311]
[null,null,null,null,null,null,null,null,null,null,76,0,0.02,0.13872238265724754,{"$f":"IF($A$90=TRUE,(IF(K77<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K77*PI()*Main!$D$45/100/Main!$D$46))),(IF(K77<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K77<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K77-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K77<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R77)))))))),(IF(K77<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K77*PI()*Main!$D$71/100/Main!$D$72))),(IF(K77<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K77<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K77-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K77<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R77)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K77<=(Main!$D$46/Main!$D$45*100),O77*Main!$D$45/100000+P76,IF(K77<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K77<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O77*Main!$D$45/100000+P76,IF(K77<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S77))))),(IF(K77<=(Main!$D$72/Main!$D$71*100),O77*Main!$D$71/100000+P76,IF(K77<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K77<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O77*Main!$D$71/100000+P76,IF(K77<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S77))))))","v":40},{"$f":"IF($A$90=TRUE,P77*Main!$D$45/100000+Q76,P77*100+Q76)","v":113.92352164549884},{"$f":"IF($A$90=TRUE,(IF(K77<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K77-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K77<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K77<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K77-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K77<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K77-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K77<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K77<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K77-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-3085953.6268892279},{"$f":"IF($A$90=TRUE,(IF(K77<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O77*Main!$D$45/100000+P76,IF(K77<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K77<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O77*Main!$D$45/100000+P76,Main!$E$52)))),(IF(K77<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O77*Main!$D$71/100000+P76,IF(K77<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K77<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O77*Main!$D$71/100000+P76,Main!$E$78)))))","v":40},76,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T77-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T77-50)*PI()/50))))","v":30726.927546296527},{"$f":"IF($A$90=TRUE,U77*2*Main!$D$50*(T77-T76)/100000+V76,U77*2*Ltime3*(T77-T76)/100000+V76)","v":1119.3360604552242},0.8084016500268999,0.55966803022761213,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W77*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W77<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W77*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W77<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W77*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W77<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W77*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W77<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W77*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W77<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W77*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W77<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":30.929780549228582},71.259146800983018]
[null,null,null,null,null,null,null,null,null,null,77,0,0.02,0.13993080819185699,{"$f":"IF($A$90=TRUE,(IF(K78<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K78*PI()*Main!$D$45/100/Main!$D$46))),(IF(K78<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K78<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K78-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K78<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R78)))))))),(IF(K78<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K78*PI()*Main!$D$71/100/Main!$D$72))),(IF(K78<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K78<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K78-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K78<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R78)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K78<=(Main!$D$46/Main!$D$45*100),O78*Main!$D$45/100000+P77,IF(K78<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K78<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O78*Main!$D$45/100000+P77,IF(K78<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S78))))),(IF(K78<=(Main!$D$72/Main!$D$71*100),O78*Main!$D$71/100000+P77,IF(K78<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K78<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O78*Main!$D$71/100000+P77,IF(K78<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S78))))))","v":40},{"$f":"IF($A$90=TRUE,P78*Main!$D$45/100000+Q77,P78*100+Q77)","v":114.91592164549884},{"$f":"IF($A$90=TRUE,(IF(K78<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K78-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K78<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K78<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K78-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K78<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K78-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K78<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K78<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K78-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":2883217.9320491557},{"$f":"IF($A$90=TRUE,(IF(K78<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O78*Main!$D$45/100000+P77,IF(K78<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K78<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O78*Main!$D$45/100000+P77,Main!$E$52)))),(IF(K78<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O78*Main!$D$71/100000+P77,IF(K78<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K78<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O78*Main!$D$71/100000+P77,Main!$E$78)))))","v":40},77,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T78-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T78-50)*PI()/50))))","v":30544.909947365726},{"$f":"IF($A$90=TRUE,U78*2*Main!$D$50*(T78-T77)/100000+V77,U78*2*Ltime3*(T78-T77)/100000+V77)","v":1180.4258803499556},0.80361290806472707,0.59021294017497783,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W78*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W78<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W78*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W78<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W78*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W78<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W78*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W78<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W78*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W78<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W78*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W78<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":30.782103603962724},75.148245524519055]
[null,null,null,null,null,null,null,null,null,null,78,0,0.02,0.14113923372646645,{"$f":"IF($A$90=TRUE,(IF(K79<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K79*PI()*Main!$D$45/100/Main!$D$46))),(IF(K79<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K79<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K79-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K79<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R79)))))))),(IF(K79<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K79*PI()*Main!$D$71/100/Main!$D$72))),(IF(K79<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K79<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K79-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K79<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R79)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K79<=(Main!$D$46/Main!$D$45*100),O79*Main!$D$45/100000+P78,IF(K79<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K79<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O79*Main!$D$45/100000+P78,IF(K79<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S79))))),(IF(K79<=(Main!$D$72/Main!$D$71*100),O79*Main!$D$71/100000+P78,IF(K79<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K79<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O79*Main!$D$71/100000+P78,IF(K79<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S79))))))","v":40},{"$f":"IF($A$90=TRUE,P79*Main!$D$45/100000+Q78,P79*100+Q78)","v":115.90832164549884},{"$f":"IF($A$90=TRUE,(IF(K79<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K79-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K79<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K79<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K79-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K79<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K79-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K79<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K79<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K79-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-1683353.4591068537},{"$f":"IF($A$90=TRUE,(IF(K79<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O79*Main!$D$45/100000+P78,IF(K79<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K79<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O79*Main!$D$45/100000+P78,Main!$E$52)))),(IF(K79<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O79*Main!$D$71/100000+P78,IF(K79<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K79<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O79*Main!$D$71/100000+P78,Main!$E$78)))))","v":40},78,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T79-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T79-50)*PI()/50))))","v":30242.345543514635},{"$f":"IF($A$90=TRUE,U79*2*Main!$D$50*(T79-T78)/100000+V78,U79*2*Ltime3*(T79-T78)/100000+V78)","v":1240.9105714369848},0.79565267309023791,0.6204552857184924,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W79*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W79<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W79*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W79<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W79*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W79<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W79*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W79<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W79*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W79<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W79*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W79<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":30.53662301763821},78.998820551673859]
["alle","alle",null,null,null,null,null,null,null,null,79,0,0.02,0.14234765926107587,{"$f":"IF($A$90=TRUE,(IF(K80<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K80*PI()*Main!$D$45/100/Main!$D$46))),(IF(K80<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K80<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K80-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K80<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R80)))))))),(IF(K80<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K80*PI()*Main!$D$71/100/Main!$D$72))),(IF(K80<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K80<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K80-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K80<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R80)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K80<=(Main!$D$46/Main!$D$45*100),O80*Main!$D$45/100000+P79,IF(K80<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K80<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O80*Main!$D$45/100000+P79,IF(K80<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S80))))),(IF(K80<=(Main!$D$72/Main!$D$71*100),O80*Main!$D$71/100000+P79,IF(K80<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K80<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O80*Main!$D$71/100000+P79,IF(K80<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S80))))))","v":40},{"$f":"IF($A$90=TRUE,P80*Main!$D$45/100000+Q79,P80*100+Q79)","v":116.90072164549885},{"$f":"IF($A$90=TRUE,(IF(K80<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K80-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K80<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K80<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K80-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K80<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K80-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K80<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K80<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K80-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-98680.040720199075},{"$f":"IF($A$90=TRUE,(IF(K80<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O80*Main!$D$45/100000+P79,IF(K80<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K80<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O80*Main!$D$45/100000+P79,Main!$E$52)))),(IF(K80<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O80*Main!$D$71/100000+P79,IF(K80<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K80<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O80*Main!$D$71/100000+P79,Main!$E$78)))))","v":40},79,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T80-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T80-50)*PI()/50))))","v":29820.428418216732},{"$f":"IF($A$90=TRUE,U80*2*Main!$D$50*(T80-T79)/100000+V79,U80*2*Ltime3*(T80-T79)/100000+V79)","v":1300.5514282734182},0.78455236051419119,0.65027571413670915,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W80*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W80<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W80*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W80<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W80*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W80<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W80*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W80<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W80*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W80<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W80*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W80<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":30.194307589979843},82.795675421975631]
[null,null,null,null,null,null,null,null,null,null,80,0,0.02,0.14355608479568532,{"$f":"IF($A$90=TRUE,(IF(K81<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K81*PI()*Main!$D$45/100/Main!$D$46))),(IF(K81<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K81<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K81-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K81<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R81)))))))),(IF(K81<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K81*PI()*Main!$D$71/100/Main!$D$72))),(IF(K81<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K81<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K81-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K81<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R81)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K81<=(Main!$D$46/Main!$D$45*100),O81*Main!$D$45/100000+P80,IF(K81<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K81<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O81*Main!$D$45/100000+P80,IF(K81<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S81))))),(IF(K81<=(Main!$D$72/Main!$D$71*100),O81*Main!$D$71/100000+P80,IF(K81<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K81<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O81*Main!$D$71/100000+P80,IF(K81<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S81))))))","v":40},{"$f":"IF($A$90=TRUE,P81*Main!$D$45/100000+Q80,P81*100+Q80)","v":117.89312164549885},{"$f":"IF($A$90=TRUE,(IF(K81<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K81-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K81<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K81<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K81-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K81<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K81-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K81<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K81<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K81-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":1846586.1486016717},{"$f":"IF($A$90=TRUE,(IF(K81<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O81*Main!$D$45/100000+P80,IF(K81<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K81<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O81*Main!$D$45/100000+P80,Main!$E$52)))),(IF(K81<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O81*Main!$D$71/100000+P80,IF(K81<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K81<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O81*Main!$D$71/100000+P80,Main!$E$78)))))","v":40},80,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T81-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T81-50)*PI()/50))))","v":29280.823685609976},{"$f":"IF($A$90=TRUE,U81*2*Main!$D$50*(T81-T80)/100000+V80,U81*2*Ltime3*(T81-T80)/100000+V80)","v":1359.1130756446382},0.77035577819907441,0.67955653782231906,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W81*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W81<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W81*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W81<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W81*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W81<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W81*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W81<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W81*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W81<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W81*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W81<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":29.756508283591561},86.523825683869291]
[null,null,null,null,null,null,null,null,null,null,81,0,0.02,0.14476451033029478,{"$f":"IF($A$90=TRUE,(IF(K82<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K82*PI()*Main!$D$45/100/Main!$D$46))),(IF(K82<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K82<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K82-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K82<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R82)))))))),(IF(K82<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K82*PI()*Main!$D$71/100/Main!$D$72))),(IF(K82<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K82<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K82-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K82<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R82)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K82<=(Main!$D$46/Main!$D$45*100),O82*Main!$D$45/100000+P81,IF(K82<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K82<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O82*Main!$D$45/100000+P81,IF(K82<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S82))))),(IF(K82<=(Main!$D$72/Main!$D$71*100),O82*Main!$D$71/100000+P81,IF(K82<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K82<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O82*Main!$D$71/100000+P81,IF(K82<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S82))))))","v":40},{"$f":"IF($A$90=TRUE,P82*Main!$D$45/100000+Q81,P82*100+Q81)","v":118.88552164549886},{"$f":"IF($A$90=TRUE,(IF(K82<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K82-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K82<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K82<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K82-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K82<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K82-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K82<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K82<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K82-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2955871.0237464146},{"$f":"IF($A$90=TRUE,(IF(K82<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O82*Main!$D$45/100000+P81,IF(K82<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K82<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O82*Main!$D$45/100000+P81,Main!$E$52)))),(IF(K82<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O82*Main!$D$71/100000+P81,IF(K82<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K82<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O82*Main!$D$71/100000+P81,Main!$E$78)))))","v":40},81,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T82-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T82-50)*PI()/50))))","v":28625.660919052003},{"$f":"IF($A$90=TRUE,U82*2*Main!$D$50*(T82-T81)/100000+V81,U82*2*Ltime3*(T82-T81)/100000+V81)","v":1416.3643974827423},0.75311895356948366,0.70818219874137112,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W82*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W82<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W82*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W82<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W82*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W82<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W82*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W82<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W82*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W82<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W82*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W82<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":29.224952892324193},90.168558031500979]
[null,null,null,null,null,null,null,null,null,null,82,0,0.02,0.14597293586490423,{"$f":"IF($A$90=TRUE,(IF(K83<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K83*PI()*Main!$D$45/100/Main!$D$46))),(IF(K83<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K83<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K83-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K83<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R83)))))))),(IF(K83<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K83*PI()*Main!$D$71/100/Main!$D$72))),(IF(K83<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K83<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K83-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K83<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R83)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K83<=(Main!$D$46/Main!$D$45*100),O83*Main!$D$45/100000+P82,IF(K83<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K83<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O83*Main!$D$45/100000+P82,IF(K83<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S83))))),(IF(K83<=(Main!$D$72/Main!$D$71*100),O83*Main!$D$71/100000+P82,IF(K83<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K83<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O83*Main!$D$71/100000+P82,IF(K83<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S83))))))","v":40},{"$f":"IF($A$90=TRUE,P83*Main!$D$45/100000+Q82,P83*100+Q82)","v":119.87792164549886},{"$f":"IF($A$90=TRUE,(IF(K83<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K83-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K83<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K83<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K83-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K83<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K83-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K83<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K83<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K83-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":3042900.859001861},{"$f":"IF($A$90=TRUE,(IF(K83<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O83*Main!$D$45/100000+P82,IF(K83<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K83<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O83*Main!$D$45/100000+P82,Main!$E$52)))),(IF(K83<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O83*Main!$D$71/100000+P82,IF(K83<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K83<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O83*Main!$D$71/100000+P82,Main!$E$78)))))","v":40},82,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T83-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T83-50)*PI()/50))))","v":27857.525746667019},{"$f":"IF($A$90=TRUE,U83*2*Main!$D$50*(T83-T82)/100000+V82,U83*2*Ltime3*(T83-T82)/100000+V82)","v":1472.0794489760763},0.73290991249747584,0.73603972448803812,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W83*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W83<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W83*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W83<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W83*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W83<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W83*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W83<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W83*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W83<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W83*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W83<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":28.601739222462506},93.715488371414423]
[null,null,null,null,null,null,null,null,null,null,83,0,0.02,0.14718136139951368,{"$f":"IF($A$90=TRUE,(IF(K84<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K84*PI()*Main!$D$45/100/Main!$D$46))),(IF(K84<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K84<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K84-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K84<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R84)))))))),(IF(K84<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K84*PI()*Main!$D$71/100/Main!$D$72))),(IF(K84<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K84<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K84-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K84<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R84)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K84<=(Main!$D$46/Main!$D$45*100),O84*Main!$D$45/100000+P83,IF(K84<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K84<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O84*Main!$D$45/100000+P83,IF(K84<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S84))))),(IF(K84<=(Main!$D$72/Main!$D$71*100),O84*Main!$D$71/100000+P83,IF(K84<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K84<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O84*Main!$D$71/100000+P83,IF(K84<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S84))))))","v":40},{"$f":"IF($A$90=TRUE,P84*Main!$D$45/100000+Q83,P84*100+Q83)","v":120.87032164549886},{"$f":"IF($A$90=TRUE,(IF(K84<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K84-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K84<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K84<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K84-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K84<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K84-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K84<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K84<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K84-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2077577.3561002398},{"$f":"IF($A$90=TRUE,(IF(K84<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O84*Main!$D$45/100000+P83,IF(K84<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K84<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O84*Main!$D$45/100000+P83,Main!$E$52)))),(IF(K84<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O84*Main!$D$71/100000+P83,IF(K84<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K84<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O84*Main!$D$71/100000+P83,Main!$E$78)))))","v":40},83,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T84-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T84-50)*PI()/50))))","v":26979.449647052854},{"$f":"IF($A$90=TRUE,U84*2*Main!$D$50*(T84-T83)/100000+V83,U84*2*Ltime3*(T84-T83)/100000+V83)","v":1526.038348270182},0.70980841083552937,0.76301917413509102,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W84*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W84<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W84*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W84<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W84*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W84<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W84*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W84<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W84*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W84<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W84*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W84<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":27.889326813642217},97.150618589996313]
[{"$f":"time1+time2+time3+time4","v":2481},null,null,null,null,null,null,null,null,null,84,8.2338561713211855E-2,5.6419734985591802E-2,0.15059031382013802,{"$f":"IF($A$90=TRUE,(IF(K85<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K85*PI()*Main!$D$45/100/Main!$D$46))),(IF(K85<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K85<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K85-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K85<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R85)))))))),(IF(K85<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K85*PI()*Main!$D$71/100/Main!$D$72))),(IF(K85<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K85<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K85-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K85<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R85)))))))))","v":2935.8915748159452},{"$f":"IF($A$90=TRUE,(IF(K85<=(Main!$D$46/Main!$D$45*100),O85*Main!$D$45/100000+P84,IF(K85<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K85<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O85*Main!$D$45/100000+P84,IF(K85<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S85))))),(IF(K85<=(Main!$D$72/Main!$D$71*100),O85*Main!$D$71/100000+P84,IF(K85<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K85<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O85*Main!$D$71/100000+P84,IF(K85<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S85))))))","v":112.8394699711836},{"$f":"IF($A$90=TRUE,P85*Main!$D$45/100000+Q84,P85*100+Q84)","v":123.66986889548393},{"$f":"IF($A$90=TRUE,(IF(K85<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K85-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K85<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K85<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K85-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K85<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K85-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K85<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K85<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K85-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":393746.8865656901},{"$f":"IF($A$90=TRUE,(IF(K85<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O85*Main!$D$45/100000+P84,IF(K85<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K85<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O85*Main!$D$45/100000+P84,Main!$E$52)))),(IF(K85<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O85*Main!$D$71/100000+P84,IF(K85<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K85<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O85*Main!$D$71/100000+P84,Main!$E$78)))))","v":112.8394699711836},84,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T85-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T85-50)*PI()/50))))","v":25994.897985419877},{"$f":"IF($A$90=TRUE,U85*2*Main!$D$50*(T85-T84)/100000+V84,U85*2*Ltime3*(T85-T84)/100000+V84)","v":1578.0281442410219},0.6839056196566321,0.789014072120511,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W85*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W85<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W85*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W85<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W85*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W85<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W85*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W85<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W85*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W85<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W85*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W85<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":27.090527232170658},100.46039179763562]
[{"$f":"Ltime1+Ltime2+Ltime3+Ltime4","v":130},null,null,null,null,null,null,null,null,null,85,0.6627032893679411,0.34954458038822467,0.17171024364141174,{"$f":"IF($A$90=TRUE,(IF(K86<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K86*PI()*Main!$D$45/100/Main!$D$46))),(IF(K86<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K86<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K86-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K86<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R86)))))))),(IF(K86<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K86*PI()*Main!$D$71/100/Main!$D$72))),(IF(K86<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K86<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K86-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K86<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R86)))))))))","v":23629.572382316233},{"$f":"IF($A$90=TRUE,(IF(K86<=(Main!$D$46/Main!$D$45*100),O86*Main!$D$45/100000+P85,IF(K86<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K86<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O86*Main!$D$45/100000+P85,IF(K86<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S86))))),(IF(K86<=(Main!$D$72/Main!$D$71*100),O86*Main!$D$71/100000+P85,IF(K86<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K86<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O86*Main!$D$71/100000+P85,IF(K86<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S86))))))","v":699.08916077644938},{"$f":"IF($A$90=TRUE,P86*Main!$D$45/100000+Q85,P86*100+Q85)","v":141.01427097434765},{"$f":"IF($A$90=TRUE,(IF(K86<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K86-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K86<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K86<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K86-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K86<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K86-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K86<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K86<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K86-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":1426256.5539816201},{"$f":"IF($A$90=TRUE,(IF(K86<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O86*Main!$D$45/100000+P85,IF(K86<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K86<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O86*Main!$D$45/100000+P85,Main!$E$52)))),(IF(K86<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O86*Main!$D$71/100000+P85,IF(K86<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K86<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O86*Main!$D$71/100000+P85,Main!$E$78)))))","v":699.08916077644938},85,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T86-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T86-50)*PI()/50))))","v":24907.756337377683},{"$f":"IF($A$90=TRUE,U86*2*Main!$D$50*(T86-T85)/100000+V85,U86*2*Ltime3*(T86-T85)/100000+V85)","v":1627.8436569157773},0.6553037654437075,0.81392182845788863,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W86*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W86<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W86*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W86<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W86*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W86<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W86*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W86<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W86*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W86<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W86*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W86<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":26.208492975059098},103.63174583157333]
[null,null,null,null,null,null,null,null,null,null,86,0.86044288378365419,0.73013298447994657,0.21582581074672016,{"$f":"IF($A$90=TRUE,(IF(K87<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K87*PI()*Main!$D$45/100/Main!$D$46))),(IF(K87<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K87<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K87-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K87<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R87)))))))),(IF(K87<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K87*PI()*Main!$D$71/100/Main!$D$72))),(IF(K87<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K87<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K87-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K87<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R87)))))))))","v":30680.242167813129},{"$f":"IF($A$90=TRUE,(IF(K87<=(Main!$D$46/Main!$D$45*100),O87*Main!$D$45/100000+P86,IF(K87<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K87<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O87*Main!$D$45/100000+P86,IF(K87<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S87))))),(IF(K87<=(Main!$D$72/Main!$D$71*100),O87*Main!$D$71/100000+P86,IF(K87<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K87<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O87*Main!$D$71/100000+P86,IF(K87<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S87))))))","v":1460.2659689598931},{"$f":"IF($A$90=TRUE,P87*Main!$D$45/100000+Q86,P87*100+Q86)","v":177.24346966424261},{"$f":"IF($A$90=TRUE,(IF(K87<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K87-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K87<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K87<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K87-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K87<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K87-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K87<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K87<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K87-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2753005.0660256855},{"$f":"IF($A$90=TRUE,(IF(K87<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O87*Main!$D$45/100000+P86,IF(K87<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K87<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O87*Main!$D$45/100000+P86,Main!$E$52)))),(IF(K87<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O87*Main!$D$71/100000+P86,IF(K87<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K87<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O87*Main!$D$71/100000+P86,Main!$E$78)))))","v":1460.2659689598931},86,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T87-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T87-50)*PI()/50))))","v":23722.315154343312},{"$f":"IF($A$90=TRUE,U87*2*Main!$D$50*(T87-T86)/100000+V86,U87*2*Ltime3*(T87-T86)/100000+V86)","v":1675.2882872244638},0.62411572664838932,0.83764414361223194,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W87*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W87<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W87*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W87<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W87*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W87<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W87*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W87<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W87*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W87<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W87*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W87<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":25.246705028557209},106.65216480629134]
[null,null,null,null,null,null,null,null,null,null,87,0.56138839503390237,0.97844454282771376,0.2749446792343338,{"$f":"IF($A$90=TRUE,(IF(K88<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K88*PI()*Main!$D$45/100/Main!$D$46))),(IF(K88<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K88<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K88-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K88<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R88)))))))),(IF(K88<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K88*PI()*Main!$D$71/100/Main!$D$72))),(IF(K88<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K88<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K88-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K88<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R88)))))))))","v":20017.054280352058},{"$f":"IF($A$90=TRUE,(IF(K88<=(Main!$D$46/Main!$D$45*100),O88*Main!$D$45/100000+P87,IF(K88<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K88<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O88*Main!$D$45/100000+P87,IF(K88<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S88))))),(IF(K88<=(Main!$D$72/Main!$D$71*100),O88*Main!$D$71/100000+P87,IF(K88<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K88<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O88*Main!$D$71/100000+P87,IF(K88<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S88))))))","v":1956.8890856554276},{"$f":"IF($A$90=TRUE,P88*Main!$D$45/100000+Q87,P88*100+Q87)","v":225.79388787935378},{"$f":"IF($A$90=TRUE,(IF(K88<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K88-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K88<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K88<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K88-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K88<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K88-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K88<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K88<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K88-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":3127657.4679970331},{"$f":"IF($A$90=TRUE,(IF(K88<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O88*Main!$D$45/100000+P87,IF(K88<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K88<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O88*Main!$D$45/100000+P87,Main!$E$52)))),(IF(K88<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O88*Main!$D$71/100000+P87,IF(K88<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K88<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O88*Main!$D$71/100000+P87,Main!$E$78)))))","v":1956.8890856554276},87,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T88-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T88-50)*PI()/50))))","v":22443.252831089641},{"$f":"IF($A$90=TRUE,U88*2*Main!$D$50*(T88-T87)/100000+V87,U88*2*Ltime3*(T88-T87)/100000+V87)","v":1720.1747928866432},0.59046458821134329,0.86008739644332166,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W88*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W88<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W88*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W88<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W88*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W88<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W88*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W88<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W88*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W88<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W88*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W88<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":24.208959130290729},109.50972850799462]
[null,null,null,null,null,null,null,null,null,null,88,0,1,0.33536595596480595,{"$f":"IF($A$90=TRUE,(IF(K89<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K89*PI()*Main!$D$45/100/Main!$D$46))),(IF(K89<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K89<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K89-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K89<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R89)))))))),(IF(K89<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K89*PI()*Main!$D$71/100/Main!$D$72))),(IF(K89<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K89<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K89-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K89<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R89)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K89<=(Main!$D$46/Main!$D$45*100),O89*Main!$D$45/100000+P88,IF(K89<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K89<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O89*Main!$D$45/100000+P88,IF(K89<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S89))))),(IF(K89<=(Main!$D$72/Main!$D$71*100),O89*Main!$D$71/100000+P88,IF(K89<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K89<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O89*Main!$D$71/100000+P88,IF(K89<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S89))))))","v":2000},{"$f":"IF($A$90=TRUE,P89*Main!$D$45/100000+Q88,P89*100+Q88)","v":275.41388787935375},{"$f":"IF($A$90=TRUE,(IF(K89<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K89-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K89<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K89<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K89-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K89<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K89-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K89<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K89<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K89-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2420644.4035044541},{"$f":"IF($A$90=TRUE,(IF(K89<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O89*Main!$D$45/100000+P88,IF(K89<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K89<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O89*Main!$D$45/100000+P88,Main!$E$52)))),(IF(K89<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O89*Main!$D$71/100000+P88,IF(K89<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K89<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O89*Main!$D$71/100000+P88,Main!$E$78)))))","v":1956.8890856554276},88,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T89-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T89-50)*PI()/50))))","v":21075.617242258573},{"$f":"IF($A$90=TRUE,U89*2*Main!$D$50*(T89-T88)/100000+V88,U89*2*Ltime3*(T89-T88)/100000+V88)","v":1762.3260273711603},0.55448315580223795,0.88116301368558014,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W89*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W89<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W89*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W89<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W89*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W89<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W89*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W89<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W89*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W89<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W89*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W89<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":23.099350789219123},112.1931594382492]
[true,null,null,null,null,null,null,null,null,null,89,0,1,0.39578723269527816,{"$f":"IF($A$90=TRUE,(IF(K90<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K90*PI()*Main!$D$45/100/Main!$D$46))),(IF(K90<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K90<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K90-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K90<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R90)))))))),(IF(K90<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K90*PI()*Main!$D$71/100/Main!$D$72))),(IF(K90<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K90<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K90-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K90<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R90)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K90<=(Main!$D$46/Main!$D$45*100),O90*Main!$D$45/100000+P89,IF(K90<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K90<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O90*Main!$D$45/100000+P89,IF(K90<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S90))))),(IF(K90<=(Main!$D$72/Main!$D$71*100),O90*Main!$D$71/100000+P89,IF(K90<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K90<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O90*Main!$D$71/100000+P89,IF(K90<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S90))))))","v":2000},{"$f":"IF($A$90=TRUE,P90*Main!$D$45/100000+Q89,P90*100+Q89)","v":325.03388787935376},{"$f":"IF($A$90=TRUE,(IF(K90<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K90-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K90<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K90<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K90-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K90<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K90-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K90<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K90<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K90-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":876478.45873331919},{"$f":"IF($A$90=TRUE,(IF(K90<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O90*Main!$D$45/100000+P89,IF(K90<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K90<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O90*Main!$D$45/100000+P89,Main!$E$52)))),(IF(K90<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O90*Main!$D$71/100000+P89,IF(K90<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K90<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O90*Main!$D$71/100000+P89,Main!$E$78)))))","v":2000},89,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T90-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T90-50)*PI()/50))))","v":19624.805820705944},{"$f":"IF($A$90=TRUE,U90*2*Main!$D$50*(T90-T89)/100000+V89,U90*2*Ltime3*(T90-T89)/100000+V89)","v":1801.5756390125721},0.51631343169643884,0.90078781950628606,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W90*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W90<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W90*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W90<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W90*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W90<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W90*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W90<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W90*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W90<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W90*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W90<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":21.922259122532758},114.69186732111635]
[null,null,null,null,null,null,null,null,null,null,90,0,1,0.45620850942575031,{"$f":"IF($A$90=TRUE,(IF(K91<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K91*PI()*Main!$D$45/100/Main!$D$46))),(IF(K91<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K91<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K91-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K91<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R91)))))))),(IF(K91<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K91*PI()*Main!$D$71/100/Main!$D$72))),(IF(K91<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K91<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K91-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K91<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R91)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K91<=(Main!$D$46/Main!$D$45*100),O91*Main!$D$45/100000+P90,IF(K91<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K91<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O91*Main!$D$45/100000+P90,IF(K91<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S91))))),(IF(K91<=(Main!$D$72/Main!$D$71*100),O91*Main!$D$71/100000+P90,IF(K91<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K91<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O91*Main!$D$71/100000+P90,IF(K91<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S91))))))","v":2000},{"$f":"IF($A$90=TRUE,P91*Main!$D$45/100000+Q90,P91*100+Q90)","v":374.65388787935376},{"$f":"IF($A$90=TRUE,(IF(K91<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K91-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K91<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K91<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K91-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K91<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K91-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K91<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K91<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K91-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":970807.78952812194},{"$f":"IF($A$90=TRUE,(IF(K91<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O91*Main!$D$45/100000+P90,IF(K91<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K91<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O91*Main!$D$45/100000+P90,Main!$E$52)))),(IF(K91<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O91*Main!$D$71/100000+P90,IF(K91<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K91<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O91*Main!$D$71/100000+P90,Main!$E$78)))))","v":2000},90,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T91-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T91-50)*PI()/50))))","v":18096.544256299934},{"$f":"IF($A$90=TRUE,U91*2*Main!$D$50*(T91-T90)/100000+V90,U91*2*Ltime3*(T91-T90)/100000+V90)","v":1837.7687275251719},0.47610605435690334,0.91888436376258598,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W91*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W91<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W91*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W91<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W91*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W91<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W91*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W91<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W91*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W91<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W91*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W91<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":20.682329573278011},116.99599089813346]
[null,null,null,null,null,null,null,null,null,null,91,0,1,0.51662978615622246,{"$f":"IF($A$90=TRUE,(IF(K92<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K92*PI()*Main!$D$45/100/Main!$D$46))),(IF(K92<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K92<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K92-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K92<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R92)))))))),(IF(K92<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K92*PI()*Main!$D$71/100/Main!$D$72))),(IF(K92<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K92<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K92-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K92<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R92)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K92<=(Main!$D$46/Main!$D$45*100),O92*Main!$D$45/100000+P91,IF(K92<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K92<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O92*Main!$D$45/100000+P91,IF(K92<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S92))))),(IF(K92<=(Main!$D$72/Main!$D$71*100),O92*Main!$D$71/100000+P91,IF(K92<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K92<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O92*Main!$D$71/100000+P91,IF(K92<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S92))))))","v":2000},{"$f":"IF($A$90=TRUE,P92*Main!$D$45/100000+Q91,P92*100+Q91)","v":424.27388787935377},{"$f":"IF($A$90=TRUE,(IF(K92<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K92-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K92<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K92<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K92-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K92<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K92-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K92<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K92<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K92-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2482350.9868792798},{"$f":"IF($A$90=TRUE,(IF(K92<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O92*Main!$D$45/100000+P91,IF(K92<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K92<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O92*Main!$D$45/100000+P91,Main!$E$52)))),(IF(K92<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O92*Main!$D$71/100000+P91,IF(K92<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K92<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O92*Main!$D$71/100000+P91,Main!$E$78)))))","v":2000},91,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T92-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T92-50)*PI()/50))))","v":16496.863899238968},{"$f":"IF($A$90=TRUE,U92*2*Main!$D$50*(T92-T91)/100000+V91,U92*2*Ltime3*(T92-T91)/100000+V91)","v":1870.7624553236499},0.43401970393298761,0.93538122766182497,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W92*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W92<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W92*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W92<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W92*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W92<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W92*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W92<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W92*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W92<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W92*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W92<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":19.384455576915883},119.09643684619596]
[null,null,null,null,null,null,null,null,null,null,92,0,1,0.57705106288669472,{"$f":"IF($A$90=TRUE,(IF(K93<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K93*PI()*Main!$D$45/100/Main!$D$46))),(IF(K93<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K93<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K93-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K93<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R93)))))))),(IF(K93<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K93*PI()*Main!$D$71/100/Main!$D$72))),(IF(K93<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K93<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K93-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K93<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R93)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K93<=(Main!$D$46/Main!$D$45*100),O93*Main!$D$45/100000+P92,IF(K93<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K93<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O93*Main!$D$45/100000+P92,IF(K93<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S93))))),(IF(K93<=(Main!$D$72/Main!$D$71*100),O93*Main!$D$71/100000+P92,IF(K93<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K93<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O93*Main!$D$71/100000+P92,IF(K93<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S93))))))","v":2000},{"$f":"IF($A$90=TRUE,P93*Main!$D$45/100000+Q92,P93*100+Q92)","v":473.89388787935377},{"$f":"IF($A$90=TRUE,(IF(K93<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K93-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K93<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K93<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K93-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K93<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K93-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K93<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K93<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K93-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":3135400.7700302559},{"$f":"IF($A$90=TRUE,(IF(K93<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O93*Main!$D$45/100000+P92,IF(K93<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K93<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O93*Main!$D$45/100000+P92,Main!$E$52)))),(IF(K93<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O93*Main!$D$71/100000+P92,IF(K93<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K93<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O93*Main!$D$71/100000+P92,Main!$E$78)))))","v":2000},92,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T93-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T93-50)*PI()/50))))","v":14832.077957067895},{"$f":"IF($A$90=TRUE,U93*2*Main!$D$50*(T93-T92)/100000+V92,U93*2*Ltime3*(T93-T92)/100000+V92)","v":1900.4266112377857},0.3902204760223893,0.95021330561889283,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W93*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W93<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W93*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W93<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W93*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W93<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W93*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W93<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W93*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W93<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W93*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W93<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":18.033759249167751},120.98491566474931]
[null,null,null,null,null,null,null,null,null,null,93,0,1,0.63747233961716687,{"$f":"IF($A$90=TRUE,(IF(K94<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K94*PI()*Main!$D$45/100/Main!$D$46))),(IF(K94<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K94<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K94-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K94<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R94)))))))),(IF(K94<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K94*PI()*Main!$D$71/100/Main!$D$72))),(IF(K94<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K94<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K94-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K94<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R94)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K94<=(Main!$D$46/Main!$D$45*100),O94*Main!$D$45/100000+P93,IF(K94<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K94<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O94*Main!$D$45/100000+P93,IF(K94<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S94))))),(IF(K94<=(Main!$D$72/Main!$D$71*100),O94*Main!$D$71/100000+P93,IF(K94<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K94<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O94*Main!$D$71/100000+P93,IF(K94<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S94))))))","v":2000},{"$f":"IF($A$90=TRUE,P94*Main!$D$45/100000+Q93,P94*100+Q93)","v":523.51388787935377},{"$f":"IF($A$90=TRUE,(IF(K94<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K94-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K94<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K94<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K94-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K94<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K94-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K94<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K94<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K94-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2704107.1520356508},{"$f":"IF($A$90=TRUE,(IF(K94<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O94*Main!$D$45/100000+P93,IF(K94<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K94<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O94*Main!$D$45/100000+P93,Main!$E$52)))),(IF(K94<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O94*Main!$D$71/100000+P93,IF(K94<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K94<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O94*Main!$D$71/100000+P93,Main!$E$78)))))","v":2000},93,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T94-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T94-50)*PI()/50))))","v":13108.756579332163},{"$f":"IF($A$90=TRUE,U94*2*Main!$D$50*(T94-T93)/100000+V93,U94*2*Ltime3*(T94-T93)/100000+V93)","v":1926.64412439645},0.344881226167709,0.96332206219822503,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W94*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W94<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W94*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W94<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W94*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W94<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W94*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W94<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W94*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W94<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W94*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W94<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":16.635571171364827},122.65397439066061]
[null,null,null,null,null,null,null,null,null,null,94,0,1,0.69789361634763902,{"$f":"IF($A$90=TRUE,(IF(K95<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K95*PI()*Main!$D$45/100/Main!$D$46))),(IF(K95<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K95<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K95-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K95<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R95)))))))),(IF(K95<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K95*PI()*Main!$D$71/100/Main!$D$72))),(IF(K95<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K95<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K95-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K95<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R95)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K95<=(Main!$D$46/Main!$D$45*100),O95*Main!$D$45/100000+P94,IF(K95<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K95<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O95*Main!$D$45/100000+P94,IF(K95<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S95))))),(IF(K95<=(Main!$D$72/Main!$D$71*100),O95*Main!$D$71/100000+P94,IF(K95<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K95<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O95*Main!$D$71/100000+P94,IF(K95<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S95))))))","v":2000},{"$f":"IF($A$90=TRUE,P95*Main!$D$45/100000+Q94,P95*100+Q94)","v":573.13388787935378},{"$f":"IF($A$90=TRUE,(IF(K95<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K95-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K95<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K95<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K95-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K95<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K95-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K95<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K95<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K95-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":1337628.2223808568},{"$f":"IF($A$90=TRUE,(IF(K95<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O95*Main!$D$45/100000+P94,IF(K95<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K95<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O95*Main!$D$45/100000+P94,Main!$E$52)))),(IF(K95<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O95*Main!$D$71/100000+P94,IF(K95<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K95<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O95*Main!$D$71/100000+P94,Main!$E$78)))))","v":2000},94,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T95-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T95-50)*PI()/50))))","v":11333.700928199012},{"$f":"IF($A$90=TRUE,U95*2*Main!$D$50*(T95-T94)/100000+V94,U95*2*Ltime3*(T95-T94)/100000+V94)","v":1949.3115262528481},0.29818088767458933,0.9746557631264241,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W95*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W95<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W95*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W95<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W95*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W95<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W95*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W95<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W95*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W95<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W95*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W95<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":15.1954093530788},124.09702601165908]
[null,null,null,null,null,null,null,null,null,null,95,0,1,0.75831489307811129,{"$f":"IF($A$90=TRUE,(IF(K96<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K96*PI()*Main!$D$45/100/Main!$D$46))),(IF(K96<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K96<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K96-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K96<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R96)))))))),(IF(K96<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K96*PI()*Main!$D$71/100/Main!$D$72))),(IF(K96<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K96<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K96-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K96<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R96)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K96<=(Main!$D$46/Main!$D$45*100),O96*Main!$D$45/100000+P95,IF(K96<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K96<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O96*Main!$D$45/100000+P95,IF(K96<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S96))))),(IF(K96<=(Main!$D$72/Main!$D$71*100),O96*Main!$D$71/100000+P95,IF(K96<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K96<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O96*Main!$D$71/100000+P95,IF(K96<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S96))))))","v":2000},{"$f":"IF($A$90=TRUE,P96*Main!$D$45/100000+Q95,P96*100+Q95)","v":622.75388787935378},{"$f":"IF($A$90=TRUE,(IF(K96<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K96-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K96<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K96<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K96-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K96<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K96-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K96<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K96<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K96-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":491454.51537027874},{"$f":"IF($A$90=TRUE,(IF(K96<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O96*Main!$D$45/100000+P95,IF(K96<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K96<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O96*Main!$D$45/100000+P95,Main!$E$52)))),(IF(K96<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O96*Main!$D$71/100000+P95,IF(K96<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K96<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O96*Main!$D$71/100000+P95,Main!$E$78)))))","v":2000},96,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T96-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T96-50)*PI()/50))))","v":7656.5846652676701},{"$f":"IF($A$90=TRUE,U96*2*Main!$D$50*(T96-T95)/100000+V95,U96*2*Ltime3*(T96-T95)/100000+V95)","v":1979.9378649139187},0.20143880860353275,0.98996893245695938,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W96*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W96<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W96*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W96<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W96*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W96<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W96*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W96<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W96*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W96<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W96*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W96<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":12.212042358420504},126.04675928634539]
[null,null,null,null,null,null,null,null,null,null,96,0,1,0.81873616980858344,{"$f":"IF($A$90=TRUE,(IF(K97<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K97*PI()*Main!$D$45/100/Main!$D$46))),(IF(K97<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K97<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K97-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K97<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R97)))))))),(IF(K97<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K97*PI()*Main!$D$71/100/Main!$D$72))),(IF(K97<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K97<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K97-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K97<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R97)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K97<=(Main!$D$46/Main!$D$45*100),O97*Main!$D$45/100000+P96,IF(K97<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K97<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O97*Main!$D$45/100000+P96,IF(K97<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S97))))),(IF(K97<=(Main!$D$72/Main!$D$71*100),O97*Main!$D$71/100000+P96,IF(K97<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K97<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O97*Main!$D$71/100000+P96,IF(K97<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S97))))))","v":2000},{"$f":"IF($A$90=TRUE,P97*Main!$D$45/100000+Q96,P97*100+Q96)","v":672.37388787935379},{"$f":"IF($A$90=TRUE,(IF(K97<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K97-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K97<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K97<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K97-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K97<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K97-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K97<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K97<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K97-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2150573.1879855553},{"$f":"IF($A$90=TRUE,(IF(K97<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O97*Main!$D$45/100000+P96,IF(K97<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K97<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O97*Main!$D$45/100000+P96,Main!$E$52)))),(IF(K97<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O97*Main!$D$71/100000+P96,IF(K97<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K97<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O97*Main!$D$71/100000+P96,Main!$E$78)))))","v":2000},98,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T97-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T97-50)*PI()/50))))","v":3858.7194883430675},{"$f":"IF($A$90=TRUE,U97*2*Main!$D$50*(T97-T96)/100000+V96,U97*2*Ltime3*(T97-T96)/100000+V96)","v":1995.372742867291},0.10151991918708668,0.99768637143364547,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W97*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W97<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W97*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W97<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W97*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W97<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W97*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W97<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W97*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W97<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W97*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W97<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":9.130707744875675},127.02937413526512]
[null,null,null,null,null,null,null,null,null,null,97,0,1,0.87915744653905559,{"$f":"IF($A$90=TRUE,(IF(K98<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K98*PI()*Main!$D$45/100/Main!$D$46))),(IF(K98<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K98<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K98-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K98<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R98)))))))),(IF(K98<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K98*PI()*Main!$D$71/100/Main!$D$72))),(IF(K98<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K98<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K98-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K98<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R98)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K98<=(Main!$D$46/Main!$D$45*100),O98*Main!$D$45/100000+P97,IF(K98<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K98<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O98*Main!$D$45/100000+P97,IF(K98<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S98))))),(IF(K98<=(Main!$D$72/Main!$D$71*100),O98*Main!$D$71/100000+P97,IF(K98<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K98<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O98*Main!$D$71/100000+P97,IF(K98<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S98))))))","v":2000},{"$f":"IF($A$90=TRUE,P98*Main!$D$45/100000+Q97,P98*100+Q97)","v":721.99388787935379},{"$f":"IF($A$90=TRUE,(IF(K98<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K98-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K98<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K98<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K98-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K98<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K98-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K98<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K98<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K98-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":3065940.0993067659},{"$f":"IF($A$90=TRUE,(IF(K98<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O98*Main!$D$45/100000+P97,IF(K98<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K98<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O98*Main!$D$45/100000+P97,Main!$E$52)))),(IF(K98<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O98*Main!$D$71/100000+P97,IF(K98<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K98<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O98*Main!$D$71/100000+P97,Main!$E$78)))))","v":2000},99,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T98-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T98-50)*PI()/50))))","v":1933.1744223022572},{"$f":"IF($A$90=TRUE,U98*2*Main!$D$50*(T98-T97)/100000+V97,U98*2*Ltime3*(T98-T97)/100000+V97)","v":1999.2390917118955},5.0860320818744004E-2,0.99961954585594781,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W98*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W98<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W98*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W98<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W98*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W98<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W98*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W98<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W98*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W98<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W98*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W98<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":7.568448847961232},127.27551354739971]
[null,null,null,null,null,null,null,null,null,null,98,0,1,0.93957872326952785,{"$f":"IF($A$90=TRUE,(IF(K99<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K99*PI()*Main!$D$45/100/Main!$D$46))),(IF(K99<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K99<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K99-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K99<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R99)))))))),(IF(K99<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K99*PI()*Main!$D$71/100/Main!$D$72))),(IF(K99<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K99<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K99-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K99<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R99)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K99<=(Main!$D$46/Main!$D$45*100),O99*Main!$D$45/100000+P98,IF(K99<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K99<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O99*Main!$D$45/100000+P98,IF(K99<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S99))))),(IF(K99<=(Main!$D$72/Main!$D$71*100),O99*Main!$D$71/100000+P98,IF(K99<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K99<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O99*Main!$D$71/100000+P98,IF(K99<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S99))))))","v":2000},{"$f":"IF($A$90=TRUE,P99*Main!$D$45/100000+Q98,P99*100+Q98)","v":771.6138878793538},{"$f":"IF($A$90=TRUE,(IF(K99<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K99-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K99<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K99<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K99-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K99<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K99-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K99<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K99<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K99-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":-2920985.8080665339},{"$f":"IF($A$90=TRUE,(IF(K99<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O99*Main!$D$45/100000+P98,IF(K99<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K99<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O99*Main!$D$45/100000+P98,Main!$E$52)))),(IF(K99<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O99*Main!$D$71/100000+P98,IF(K99<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K99<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O99*Main!$D$71/100000+P98,Main!$E$78)))))","v":2000},99.999999000000003,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T99-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T99-50)*PI()/50))))","v":1.9344469893987388E-3},{"$f":"IF($A$90=TRUE,U99*2*Main!$D$50*(T99-T98)/100000+V98,U99*2*Ltime3*(T99-T98)/100000+V98)","v":1999.2390955807857},5.0893801072798549E-8,0.99961954779039286,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W99*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W99<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W99*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W99<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W99*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W99<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W99*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W99<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W99*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W99<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W99*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W99<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":6.0000015694813245},127.2755137937009]
[0,112,null,null,null,null,null,null,null,null,99,0,1,1,{"$f":"IF($A$90=TRUE,(IF(K100<=(Main!$D$46/Main!$D$45*100),(IF($B$30=1,Main!$G$46,Main!$G$46*SIN(K100*PI()*Main!$D$45/100/Main!$D$46))),(IF(K100<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),0,(IF(K100<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((K100-(Main!$D$46+Main!$D$48)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$50))),(IF(K100<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),0,R100)))))))),(IF(K100<=(Main!$D$72/Main!$D$71*100),(IF($B$30=1,Main!$G$72,Main!$G$72*SIN(K100*PI()*Main!$D$71/100/Main!$D$72))),(IF(K100<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),0,(IF(K100<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),(IF($B$30=1,Main!$G$76,Main!$G$76*SIN((K100-(Main!$D$72+Main!$D$74)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$76))),(IF(K100<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),0,R100)))))))))","v":0},{"$f":"IF($A$90=TRUE,(IF(K100<=(Main!$D$46/Main!$D$45*100),O100*Main!$D$45/100000+P99,IF(K100<=((Main!$D$46+Main!$D$48)/Main!$D$45*100),Main!$E$48,IF(K100<=((Main!$D$46+Main!$D$48+Main!$D$50)/Main!$D$45*100),O100*Main!$D$45/100000+P99,IF(K100<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52)/Main!$D$45*100),Main!$E$52,S100))))),(IF(K100<=(Main!$D$72/Main!$D$71*100),O100*Main!$D$71/100000+P99,IF(K100<=((Main!$D$72+Main!$D$74)/Main!$D$71*100),Main!$E$74,IF(K100<=((Main!$D$72+Main!$D$74+Main!$D$76)/Main!$D$71*100),O100*Main!$D$71/100000+P99,IF(K100<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78)/Main!$D$71*100),Main!$E$78,S100))))))","v":2000},{"$f":"IF($A$90=TRUE,P100*Main!$D$45/100000+Q99,P100*100+Q99)","v":821.2338878793538},{"$f":"IF($A$90=TRUE,(IF(K100<=((m1time+Main!$D$55)/Main!$D$45*100),(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((K100-m1time/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$55))),(IF(K100<=((m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100),0,(IF(K100<=((m1time+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((K100-(m1time+Main!$D$55+Main!$D$57)/Main!$D$45*100)*PI()*Main!$D$45/100/Main!$D$59))),0)))))),(IF(K100<=((lm1time+Main!$D$81)/Main!$D$71*100),(IF($B$30=1,Main!$G$81,Main!$G$81*SIN((K100-lm1time/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$81))),(IF(K100<=((lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100),0,(IF(K100<=((lm1time+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),(IF($B$30=1,Main!$G$85,Main!$G$85*SIN((K100-(lm1time+Main!$D$81+Main!$D$83)/Main!$D$71*100)*PI()*Main!$D$71/100/Main!$D$85))),0)))))))","v":1765841.1398602573},{"$f":"IF($A$90=TRUE,(IF(K100<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55)/Main!$D$45*100),O100*Main!$D$45/100000+P99,IF(K100<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57)/Main!$D$45*100),Main!$E$57,IF(K100<=((Main!$D$46+Main!$D$48+Main!$D$50+Main!$D$52+Main!$D$55+Main!$D$57+Main!$D$59)/Main!$D$45*100),O100*Main!$D$45/100000+P99,Main!$E$52)))),(IF(K100<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81)/Main!$D$71*100),O100*Main!$D$71/100000+P99,IF(K100<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83)/Main!$D$71*100),Main!$E$83,IF(K100<=((Main!$D$72+Main!$D$74+Main!$D$76+Main!$D$78+Main!$D$81+Main!$D$83+Main!$D$85)/Main!$D$71*100),O100*Main!$D$71/100000+P99,Main!$E$78)))))","v":2000},99.999999000000003,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$50,Main!$G$50*SIN((T100-50)*PI()/50))),(IF($B$30=1,laccel3,laccel3*SIN((T100-50)*PI()/50))))","v":1.9344469893987388E-3},{"$f":"IF($A$90=TRUE,U100*2*Main!$D$50*(T100-T99)/100000+V99,U100*2*Ltime3*(T100-T99)/100000+V99)","v":1999.2390955807857},5.0893801072798549E-8,0.99961954779039286,{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W100*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W100<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W100*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W100<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W100*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+Ltorque)/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W100*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W100<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W100*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W100<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W100*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+Ltorque)/LWirkungsgrad))),0)","v":6.0000015694813245},127.2755137937009]
[1319.0204936359687,112,null,null,null,null,null,null,null,null,100,null,null,null,null,null,null,null,null,100,0,{"$f":"IF($A$90=TRUE,Main!$E$46,Lspeed1)","v":2000},0,1,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W101*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W101<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W101*MAX(ABS(accel1),ABS(accel3))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W101<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W101*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W101<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W101*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque+IF(W101<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad,(W101*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia/gear^2+Calc!$A$107+gear_inertia)/1000+(torque+IF(W101<=0,DryTorq,-DryTorq))/gear)/Wirkungsgrad),(W101*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht+Calc!$A$107)+(Ltorque+IF(W101<=0,LDryTorq,-LDryTorq)))/LWirkungsgrad)))","v":9},127.32395447351627]
[1849.2330490204452,31.890859332021563,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"100+T2","v":100.000001},{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T102-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T102-100)*PI()/50))))","v":-0.19739254911198548},{"$f":"IF($A$90=TRUE,U102*2*Main!$D$55*(T102-T101)/100000+V101,U102*2*Ltime5*(T102-T101)/100000+V101)","v":1999.9999999999961},-5.1932449856796039E-6,0.99999999999999811,{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W102*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W102>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W102*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W102>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W102*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W102>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W102*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W102>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W102*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W102>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W102*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W102>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad))),0)","v":5.9998398488451539},127.32395447351603]
[0,42,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"100+T3","v":100.000001},{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T103-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T103-100)*PI()/50))))","v":-0.19739254911198548},{"$f":"IF($A$90=TRUE,U103*2*Main!$D$55*(T103-T102)/100000+V102,U103*2*Ltime5*(T103-T102)/100000+V102)","v":1999.9999999999961},-5.1932449856796039E-6,0.99999999999999811,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W103*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W103>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W103*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W103>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W103*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W103>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W103*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W103>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W103*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W103>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W103*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W103>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":5.9998398488451539},127.32395447351603]
[1849.2330490204452,31.890859332021563,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,101,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T104-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T104-100)*PI()/50))))","v":-197262.69615329089},{"$f":"IF($A$90=TRUE,U104*2*Main!$D$55*(T104-T103)/100000+V103,U104*2*Ltime5*(T104-T103)/100000+V103)","v":1996.0547500221842},-5.1898286549738604,0.99802737501109207,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W104*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W104>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W104*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W104>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W104*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W104>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W104*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W104>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W104*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W104>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W104*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W104>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":154.04580081237},127.07279205923523]
[1960,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,102,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T105-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T105-100)*PI()/50))))","v":-393746.88656561828},{"$f":"IF($A$90=TRUE,U105*2*Main!$D$55*(T105-T104)/100000+V104,U105*2*Ltime5*(T105-T104)/100000+V104)","v":1988.1798122908717},-10.359175427253719,0.99408990614543591,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W105*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W105>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W105*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W105>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W105*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W105>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W105*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W105>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W105*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W105>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W105*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W105>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":313.45997396690495},126.57145795264354]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,104,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T106-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T106-100)*PI()/50))))","v":-781284.14951710787},{"$f":"IF($A$90=TRUE,U106*2*Main!$D$55*(T106-T105)/100000+V105,U106*2*Ltime5*(T106-T105)/100000+V105)","v":1956.9284463101874},-20.554980469748205,0.97846422315509374,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W106*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W106>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W106*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W106>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W106*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W106>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W106*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W106>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W106*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W106>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W106*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W106>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":627.88187330821359},124.58193420296361]
[9.1999999999999993,122,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,106,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T107-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T107-100)*PI()/50))))","v":-1156500.0947141841},{"$f":"IF($A$90=TRUE,U107*2*Main!$D$55*(T107-T106)/100000+V106,U107*2*Ltime5*(T107-T106)/100000+V106)","v":1910.6684425216199},-30.4266211912846,0.95533422126080991,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W107*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W107>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W107*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W107>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W107*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W107>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W107*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W107>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W107*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W107>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W107*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W107>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":932.30707684477466},121.63693089480348]
[42,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,107,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T108-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T108-100)*PI()/50))))","v":-1337628.2223808323},{"$f":"IF($A$90=TRUE,U108*2*Main!$D$55*(T108-T107)/100000+V107,U108*2*Ltime5*(T108-T107)/100000+V107)","v":1883.9158780740033},-35.191961853847843,0.94195793903700165,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W108*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W108>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W108*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W108>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W108*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W108>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W108*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W108>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W108*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W108>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W108*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W108>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1079.2623644249818},119.9338097459144]
[13.6,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,108,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T109-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T109-100)*PI()/50))))","v":-1513477.3425579488},{"$f":"IF($A$90=TRUE,U109*2*Main!$D$55*(T109-T108)/100000+V108,U109*2*Ltime5*(T109-T108)/100000+V108)","v":1853.6463312228443},-39.818415920651979,0.9268231656114222,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W109*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W109>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W109*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W109>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W109*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W109>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W109*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W109>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W109*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W109>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W109*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W109>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1221.9346172620158},118.00679054330895]
[33.799999999999997,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,109,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T110-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T110-100)*PI()/50))))","v":-1683353.459106016},{"$f":"IF($A$90=TRUE,U110*2*Main!$D$55*(T110-T109)/100000+V109,U110*2*Ltime5*(T110-T109)/100000+V109)","v":1819.9792620407241},-44.287724891121151,0.90998963102036201,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W110*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W110>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W110*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W110>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W110*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W110>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W110*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W110>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W110*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W110>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W110*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W110>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1359.7607731546809},115.86347835140843]
[10.903225806451612,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,110,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T111-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T111-100)*PI()/50))))","v":-1846586.1486020335},{"$f":"IF($A$90=TRUE,U111*2*Main!$D$55*(T111-T110)/100000+V110,U111*2*Ltime5*(T111-T110)/100000+V110)","v":1783.0475390686834},-48.582250444581959,0.89152376953434165,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W111*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W111>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W111*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W111>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W111*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W111>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W111*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W111>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W111*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W111>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W111*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W111>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1492.1968952324498},113.51233184424812]
[1500,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,111,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T112-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T112-100)*PI()/50))))","v":-2002531.2061944834},{"$f":"IF($A$90=TRUE,U112*2*Main!$D$55*(T112-T111)/100000+V111,U112*2*Ltime5*(T112-T111)/100000+V111)","v":1742.9969149447936},-52.685044050657005,0.87149845747239685,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W112*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W112>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W112*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W112>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W112*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W112>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W112*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W112>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W112*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W112>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W112*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W112>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1618.7203186257909},110.9626299229551]
[112,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,112,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T113-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T113-100)*PI()/50))))","v":-2150573.1879855683},{"$f":"IF($A$90=TRUE,U113*2*Main!$D$55*(T113-T112)/100000+V112,U113*2*Ltime5*(T113-T112)/100000+V112)","v":1699.9854511850822},-56.579913857371203,0.84999272559254113,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W113*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W113>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W113*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W113>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W113*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W113>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W113*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W113>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W113*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W113>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W113*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W113>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1738.8317131856243},108.22443509616471]
[6000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,113,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T114-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T114-100)*PI()/50))))","v":-2290127.8399071065},{"$f":"IF($A$90=TRUE,U114*2*Main!$D$55*(T114-T113)/100000+V113,U114*2*Ltime5*(T114-T113)/100000+V113)","v":1654.18289438694},-60.251488592994221,0.82709144719347005,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W114*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W114>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W114*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W114>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W114*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W114>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W114*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W114>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W114*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W114>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W114*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W114>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1852.0570541112991},105.30855376789606]
[0.68,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,114,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T115-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T115-100)*PI()/50))))","v":-2420644.4035044196},{"$f":"IF($A$90=TRUE,U115*2*Main!$D$55*(T115-T114)/100000+V114,U115*2*Ltime5*(T115-T114)/100000+V114)","v":1605.7700063168515},-63.685278229427482,0.80288500315842581,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W115*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W115>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W115*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W115>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W115*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W115>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W115*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W115>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W115*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W115>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W115*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W115>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1957.949492709919},102.22649358961237]
[12.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,115,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T116-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T116-100)*PI()/50))))","v":-2541607.7895283345},{"$f":"IF($A$90=TRUE,U116*2*Main!$D$55*(T116-T115)/100000+V115,U116*2*Ltime5*(T116-T115)/100000+V115)","v":1554.9378505262848},-66.867731167725239,0.77746892526314237,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W116*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W116>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W116*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W116>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W116*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W116>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W116*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W116>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W116*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W116>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W116*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W116>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2056.0911199039888},98.990418044777954]
[200,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,116,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T117-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T117-100)*PI()/50))))","v":-2652540.6107571307},{"$f":"IF($A$90=TRUE,U117*2*Main!$D$55*(T117-T116)/100000+V116,U117*2*Ltime5*(T117-T116)/100000+V116)","v":1501.8870383111423},-69.786287720064507,0.75094351915557112,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W117*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W117>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W117*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W117>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W117*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W117>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W117*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W117>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W117*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W117>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W117*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W117>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2146.0946155276188},95.613098445146022]
[640,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,117,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T118-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T118-100)*PI()/50))))","v":-2753005.0660258024},{"$f":"IF($A$90=TRUE,U118*2*Main!$D$55*(T118-T117)/100000+V117,U118*2*Ltime5*(T118-T117)/100000+V117)","v":1446.8269369906263},-72.429429677094859,0.72341346849531318,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W118*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W118>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W118*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W118>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W118*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W118>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W118*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W118>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W118*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W118>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W118*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W118>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2227.6047769022675},92.107863528225749]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,118,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T119-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T119-100)*PI()/50))))","v":-2842604.6680272473},{"$f":"IF($A$90=TRUE,U119*2*Main!$D$55*(T119-T118)/100000+V118,U119*2*Ltime5*(T119-T118)/100000+V118)","v":1389.9748436300813},-74.786725765048558,0.6949874218150407,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W119*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W119>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W119*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W119>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W119*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W119>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W119*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W119>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W119*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W119>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W119*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W119>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2300.29992065944},88.488546854844685]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,119,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T120-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T120-100)*PI()/50))))","v":-2920985.8080665306},{"$f":"IF($A$90=TRUE,U120*2*Main!$D$55*(T120-T119)/100000+V119,U120*2*Ltime5*(T120-T119)/100000+V119)","v":1331.5551274687507},-76.848872813212623,0.66577756373437535,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W120*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W120>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W120*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W120>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W120*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W120>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W120*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W120>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W120*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W120>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W120*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W120>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2363.893152277979},84.769432214404176]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,120,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T121-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T121-100)*PI()/50))))","v":-2987839.1515928544},{"$f":"IF($A$90=TRUE,U121*2*Main!$D$55*(T121-T120)/100000+V120,U121*2*Ltime5*(T121-T120)/100000+V120)","v":1271.7983444368936},-78.60773246929331,0.63589917221844683,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W121*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W121>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W121*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W121>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W121*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W121>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W121*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W121>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W121*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W121>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W121*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W121>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2418.1334983256693},80.96519725328821]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,121,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T122-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T122-100)*PI()/50))))","v":-3042900.8590017073},{"$f":"IF($A$90=TRUE,U122*2*Main!$D$55*(T122-T121)/100000+V121,U122*2*Ltime5*(T122-T121)/100000+V121)","v":1210.9403272568595},-80.056363317774611,0.60547016362842976,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W122*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W122>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W122*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W122>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W122*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W122>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W122*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W122>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W122*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W122>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W122*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W122>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2462.8068969367187},77.090855548898631]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,122,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T123-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T123-100)*PI()/50))))","v":-3085953.6268892479},{"$f":"IF($A$90=TRUE,U123*2*Main!$D$55*(T123-T122)/100000+V122,U123*2*Ltime5*(T123-T122)/100000+V122)","v":1149.2212547190745},-81.18904827451405,0.57461062735953727,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W123*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W123>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W123*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W123>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W123*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W123>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W123*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W123>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W123*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W123>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W123*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W123>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2497.7370426161428},73.161697357924339]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,123,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T124-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T124-100)*PI()/50))))","v":-3116827.5456495634},{"$f":"IF($A$90=TRUE,U124*2*Main!$D$55*(T124-T123)/100000+V123,U124*2*Ltime5*(T124-T123)/100000+V123)","v":1086.8847038060833},-82.00131714946194,0.54344235190304169,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W124*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W124>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W124*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W124>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W124*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W124>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W124*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W124>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W124*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W124>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W124*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W124>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2522.7860820370124},69.193229272683482]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,124,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T125-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T125-100)*PI()/50))))","v":-3135400.7700302578},{"$f":"IF($A$90=TRUE,U125*2*Main!$D$55*(T125-T124)/100000+V124,U125*2*Ltime5*(T125-T124)/100000+V124)","v":1024.1766884054782},-82.489964288459177,0.51208834420273908,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W125*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W125>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W125*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W125>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W125*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W125>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W125*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W125>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W125*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W125>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W125*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W125>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2537.8551580845492},65.201113023687881]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,125,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T126-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T126-100)*PI()/50))))","v":-3141600},{"$f":"IF($A$90=TRUE,U126*2*Main!$D$55*(T126-T125)/100000+V125,U126*2*Ltime5*(T126-T125)/100000+V125)","v":961.34468840547822},-82.65306122448979,0.48067234420273913,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W126*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W126>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W126*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W126>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W126*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W126>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W126*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W126>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W126*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W126>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W126*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W126>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2542.8847999999998},61.201103669947898]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,126,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T127-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T127-100)*PI()/50))))","v":-3135400.7700302578},{"$f":"IF($A$90=TRUE,U127*2*Main!$D$55*(T127-T126)/100000+V126,U127*2*Ltime5*(T127-T126)/100000+V126)","v":898.63667300487305},-82.489964288459177,0.44931833650243652,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W127*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W127>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W127*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W127>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W127*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W127>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W127*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W127>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W127*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W127>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W127*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W127>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2537.8551580845492},57.20898742095229]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,127,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T128-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T128-100)*PI()/50))))","v":-3116827.5456495639},{"$f":"IF($A$90=TRUE,U128*2*Main!$D$55*(T128-T127)/100000+V127,U128*2*Ltime5*(T128-T127)/100000+V127)","v":836.3001220918818},-82.001317149461954,0.41815006104594088,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W128*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W128>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W128*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W128>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W128*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W128>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W128*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W128>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W128*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W128>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W128*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W128>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2522.7860820370129},53.240519335711426]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,128,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T129-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T129-100)*PI()/50))))","v":-3085953.6268892484},{"$f":"IF($A$90=TRUE,U129*2*Main!$D$55*(T129-T128)/100000+V128,U129*2*Ltime5*(T129-T128)/100000+V128)","v":774.58104955409681},-81.189048274514064,0.38729052477704839,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W129*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W129>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W129*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W129>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W129*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W129>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W129*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W129>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W129*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W129>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W129*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W129>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2497.7370426161433},49.311361144737134]
[{"$f":"IF(move1,C130,C131)","v":10.075051423661446},{"$f":"IF(move1,ABS(IF(Rotativ,((time1/2+time2+time3/2)/time*(speed2-speed1)+(speed1))*gear,((Ltime1/2+Ltime2+Ltime3/2)/ltime*(Lspeed2-Lspeed1)+(Lspeed1)))),ABS(IF(Rotativ,((time1/2+time2+time3/2)/time*(ABS(speed2)-ABS(speed1))+(time5/2+time6+time7/2)/time*(ABS(speed6)-ABS(speed1))+ABS(speed1))*gear,((Ltime1/2+Ltime2+Ltime3/2)/ltime*(ABS(Lspeed2)-ABS(Lspeed1))+((Ltime5/2+Ltime6+Ltime7/2)/ltime*(ABS(Lspeed6)-ABS(Lspeed1))+ABS(Lspeed1))))))","v":22.185980958664175},{"$f":"IF($A$90=TRUE,IF($B$30=1,SQRT((D130^2*time1+D131^2*time2+D132^2*time3+D133^2*time4)/time),SQRT((((D130-D131)*2/3.1415+D131)^2*time1+D131^2*time2+((D132-D131)*2/3.145+D131)^2*time3+D133^2*time4)/time)),IF($B$30=1,SQRT((D130^2*Ltime1+D131^2*Ltime2+D132^2*Ltime3+D133^2*Ltime4)/ltime),SQRT((((D130-D131)*2/3.1415+D131)^2*Ltime1+D131^2*Ltime2+((D132-D131)*2/3.145+D131)^2*Ltime3+D133^2*Ltime4)/ltime)))","v":10.075051423661446},{"$f":"IF(Calc!$A$90,INDEX(Motor!$X$1:$X$1068,$B$107,1),INDEX(LinMotor!$V$1:$V$1355,$B$107,1))","v":-24.838359308641976},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,129,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T130-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T130-100)*PI()/50))))","v":-3042900.8590017073},{"$f":"IF($A$90=TRUE,U130*2*Main!$D$55*(T130-T129)/100000+V129,U130*2*Ltime5*(T130-T129)/100000+V129)","v":713.72303237406265},{"$f":"IF(move1,IF(ABS(MIN($U$1:$U$101))>MAX($U$1:$U$101),U130/MIN($U$1:$U$101)*-1,U130/MAX($U$1:$U$101)),IF(ABS(MIN($U$1:$U$201))>MAX($U$1:$U$201),U130/MIN($U$1:$U$201)*-1,U130/MAX($U$1:$U$201)))","v":-80.056363317774611},{"$f":"IF(move1,IF(ABS(MIN($V$1:$V$101))>MAX($V$1:$V$101),V130/MIN($V$1:$V$101)*-1,V130/MAX($V$1:$V$101)),IF(ABS(MIN($V$1:$V$201))>MAX($V$1:$V$201),V130/MIN($V$1:$V$201)*-1,V130/MAX($V$1:$V$201)))","v":0.35686151618703132},{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W130*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W130>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W130*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W130>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W130*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W130>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W130*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W130>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W130*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W130>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W130*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W130>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2462.8068969367187},45.437019440347562]
[null,null,{"$f":"IF($A$90=TRUE,IF($B$30=1,SQRT((D130^2*time1+D131^2*time2+D132^2*time3+D133^2*time4+D134^2*time5+D135^2*time6+D136^2*time7+D137^2*time8)/time),SQRT((((D130-D131)*2/3.1415+D131)^2*time1+D131^2*time2+((D132-D131)*2/3.145+D131)^2*time3+D133^2*time4+((D134-D135)*2/3.1415+D135)^2*time5+D135^2*time6+((D136-D135)*2/3.145+D135)^2*time7+D137^2*time8)/time)),IF($B$30=1,SQRT((D130^2*Ltime1+D131^2*Ltime2+D132^2*Ltime3+D133^2*Ltime4+D134^2*Ltime5+D135^2*Ltime6+D136^2*Ltime7+D137^2*Ltime8)/ltime),SQRT((((D130-D131)*2/3.1415+D131)^2*Ltime1+D131^2*Ltime2+((D132-D131)*2/3.145+D131)^2*Ltime3+D133^2*Ltime4+((D134-D135)*2/3.1415+D135)^2*Ltime5+D135^2*Ltime6+((D136-D135)*2/3.145+D135)^2*Ltime7+D137^2*Ltime8)/ltime)))","v":47.136784067966126},{"$f":"IF(Calc!$A$90,INDEX(Motor!$Y$1:$Y$1068,$B$107,1),INDEX(LinMotor!$W$1:$W$1355,$B$107,1))","v":9},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,130,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T131-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T131-100)*PI()/50))))","v":-2987839.1515928549},{"$f":"IF($A$90=TRUE,U131*2*Main!$D$55*(T131-T130)/100000+V130,U131*2*Ltime5*(T131-T130)/100000+V130)","v":653.96624934220551},-78.60773246929331,0.32698312467110274,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W131*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W131>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W131*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W131>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W131*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W131>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W131*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W131>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W131*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W131>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W131*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W131>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2418.1334983256693},{"$f":"IF(move1,ABS(IF($A$90=TRUE,X131*speed,X131*MAX(ABS(Lspeed1),ABS(Lspeed2)))),ABS(IF($A$90=TRUE,X131*speed,X131*MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6)))))","v":41.632784479231582}]
[null,null,null,{"$f":"IF(Calc!$A$90,INDEX(Motor!$Z$1:$Z$1068,$B$107,1),INDEX(LinMotor!$X$1:$X$1355,$B$107,1))","v":30.979071040000001},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,131,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T132-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T132-100)*PI()/50))))","v":-2920985.8080665306},{"$f":"IF($A$90=TRUE,U132*2*Main!$D$55*(T132-T131)/100000+V131,U132*2*Ltime5*(T132-T131)/100000+V131)","v":595.54653318087492},-76.848872813212623,0.29777326659043746,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W132*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W132>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W132*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W132>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W132*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W132>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W132*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W132>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W132*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W132>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W132*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W132>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2363.893152277979},37.91366983879108]
[null,null,null,{"$f":"IF(Calc!$A$90,INDEX(Motor!$AA$1:$AA$1068,$B$107,1),INDEX(LinMotor!$Y$1:$Y$1355,$B$107,1))","v":9},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,132,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T133-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T133-100)*PI()/50))))","v":-2842604.6680272468},{"$f":"IF($A$90=TRUE,U133*2*Main!$D$55*(T133-T132)/100000+V132,U133*2*Ltime5*(T133-T132)/100000+V132)","v":538.69443982032999},-74.786725765048544,0.26934721991016497,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W133*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W133>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W133*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W133>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W133*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W133>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W133*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W133>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W133*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W133>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W133*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W133>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2300.2999206594395},34.294353165410016]
[null,null,null,{"$f":"IF(Calc!$A$90,INDEX(Motor!$AB$1:$AB$1068,$B$107,1),INDEX(LinMotor!$Z$1:$Z$1355,$B$107,1))","v":-2542.8848000000003},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,133,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T134-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T134-100)*PI()/50))))","v":-2753005.0660258015},{"$f":"IF($A$90=TRUE,U134*2*Main!$D$55*(T134-T133)/100000+V133,U134*2*Ltime5*(T134-T133)/100000+V133)","v":483.63433849981396},-72.429429677094831,0.24181716924990698,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W134*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W134>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W134*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W134>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W134*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W134>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W134*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W134>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W134*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W134>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W134*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W134>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2227.6047769022666},30.789118248489736]
[null,null,null,{"$f":"IF(Calc!$A$90,INDEX(Motor!$AC$1:$AC$1068,$B$107,1),INDEX(LinMotor!$AA$1:$AA$1355,$B$107,1))","v":7.5},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,134,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T135-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T135-100)*PI()/50))))","v":-2652540.6107571302},{"$f":"IF($A$90=TRUE,U135*2*Main!$D$55*(T135-T134)/100000+V134,U135*2*Ltime5*(T135-T134)/100000+V134)","v":430.58352628467134},-69.786287720064507,0.21529176314233567,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W135*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W135>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W135*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W135>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W135*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W135>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W135*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W135>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W135*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W135>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W135*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W135>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2146.0946155276188},27.411798648857793]
[null,null,null,{"$f":"IF(Calc!$A$90,INDEX(Motor!$AD$1:$AD$1068,$B$107,1),INDEX(LinMotor!$AB$1:$AB$1355,$B$107,1))","v":2554.8848000000003},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,135,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T136-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T136-100)*PI()/50))))","v":-2541607.789528335},{"$f":"IF($A$90=TRUE,U136*2*Main!$D$55*(T136-T135)/100000+V135,U136*2*Ltime5*(T136-T135)/100000+V135)","v":379.75137049410466},-66.867731167725253,0.18987568524705234,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W136*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W136>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W136*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W136>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W136*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W136>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W136*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W136>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W136*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W136>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W136*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W136>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2056.0911199039892},24.175723104023398]
[null,null,null,{"$f":"IF(Calc!$A$90,INDEX(Motor!$AE$1:$AE$1068,$B$107,1),INDEX(LinMotor!$AC$1:$AC$1355,$B$107,1))","v":9},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,136,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T137-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T137-100)*PI()/50))))","v":-2420644.4035044196},{"$f":"IF($A$90=TRUE,U137*2*Main!$D$55*(T137-T136)/100000+V136,U137*2*Ltime5*(T137-T136)/100000+V136)","v":331.33848242401626},-63.685278229427482,0.16566924121200813,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W137*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W137>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W137*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W137>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W137*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W137>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W137*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W137>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W137*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W137>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W137*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W137>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1957.949492709919},21.093662925739707]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,137,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T138-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T138-100)*PI()/50))))","v":-2290127.839907106},{"$f":"IF($A$90=TRUE,U138*2*Main!$D$55*(T138-T137)/100000+V137,U138*2*Ltime5*(T138-T137)/100000+V137)","v":285.53592562587414},-60.251488592994207,0.14276796281293708,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W138*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W138>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W138*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W138>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W138*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W138>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W138*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W138>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W138*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W138>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W138*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W138>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1852.0570541112986},18.177781597471064]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,138,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T139-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T139-100)*PI()/50))))","v":-2150573.1879855688},{"$f":"IF($A$90=TRUE,U139*2*Main!$D$55*(T139-T138)/100000+V138,U139*2*Ltime5*(T139-T138)/100000+V138)","v":242.52446186616277},-56.579913857371217,0.12126223093308139,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W139*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W139>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W139*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W139>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W139*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W139>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W139*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W139>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W139*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W139>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W139*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W139>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1738.8317131856247},15.439586770680672]
["","",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,139,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T140-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T140-100)*PI()/50))))","v":-2002531.2061944841},{"$f":"IF($A$90=TRUE,U140*2*Main!$D$55*(T140-T139)/100000+V139,U140*2*Ltime5*(T140-T139)/100000+V139)","v":202.47383774227308},-52.685044050657019,0.10123691887113653,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W140*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W140>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W140*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W140>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W140*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W140>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W140*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W140>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W140*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W140>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W140*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W140>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1618.7203186257914},12.889884849387649]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,140,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T141-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T141-100)*PI()/50))))","v":-1846586.148602034},{"$f":"IF($A$90=TRUE,U141*2*Main!$D$55*(T141-T140)/100000+V140,U141*2*Ltime5*(T141-T140)/100000+V140)","v":165.54211477023239},-48.582250444581973,8.2771057385116198E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W141*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W141>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W141*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W141>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W141*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W141>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W141*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W141>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W141*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W141>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W141*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W141>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1492.1968952324503},10.538738342227337]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,141,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T142-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T142-100)*PI()/50))))","v":-1683353.4591060169},{"$f":"IF($A$90=TRUE,U142*2*Main!$D$55*(T142-T141)/100000+V141,U142*2*Ltime5*(T142-T141)/100000+V141)","v":131.87504558811204},-44.287724891121179,6.5937522794056028E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W142*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W142>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W142*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W142>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W142*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W142>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W142*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W142>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W142*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W142>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W142*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W142>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1359.7607731546818},8.3954261503268306]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,142,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T143-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T143-100)*PI()/50))))","v":-1513477.3425579485},{"$f":"IF($A$90=TRUE,U143*2*Main!$D$55*(T143-T142)/100000+V142,U143*2*Ltime5*(T143-T142)/100000+V142)","v":101.60549873695308},-39.818415920651972,5.0802749368476542E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W143*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W143>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W143*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W143>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W143*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W143>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W143*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W143>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W143*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W143>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W143*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W143>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1221.9346172620155},6.4684069477213644]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,143,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T144-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T144-100)*PI()/50))))","v":-1337628.222380833},{"$f":"IF($A$90=TRUE,U144*2*Main!$D$55*(T144-T143)/100000+V143,U144*2*Ltime5*(T144-T143)/100000+V143)","v":74.852934289336417},-35.191961853847864,3.7426467144668206E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W144*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W144>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W144*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W144>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W144*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W144>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W144*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W144>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W144*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W144>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W144*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W144>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1079.2623644249825},4.765285798832287]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,144,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T145-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T145-100)*PI()/50))))","v":-1156500.0947141848},{"$f":"IF($A$90=TRUE,U145*2*Main!$D$55*(T145-T144)/100000+V144,U145*2*Ltime5*(T145-T144)/100000+V144)","v":51.722932395052723},-30.426621191284621,2.5861466197526363E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W145*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W145>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W145*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W145>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W145*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W145>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W145*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W145>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W145*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W145>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W145*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W145>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":932.30707684477534},3.2927841447522264]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,146,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T146-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T146-100)*PI()/50))))","v":-781284.14951710927},{"$f":"IF($A$90=TRUE,U146*2*Main!$D$55*(T146-T145)/100000+V145,U146*2*Ltime5*(T146-T145)/100000+V145)","v":20.471566414368354},-20.554980469748241,1.0235783207184178E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W146*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W146>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W146*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W146>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W146*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W146>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W146*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W146>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W146*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W146>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W146*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W146>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":627.88187330821472},1.3032603950723005]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,148,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T147-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T147-100)*PI()/50))))","v":-393746.88656561915},{"$f":"IF($A$90=TRUE,U147*2*Main!$D$55*(T147-T146)/100000+V146,U147*2*Ltime5*(T147-T146)/100000+V146)","v":4.7216909517435877},-10.359175427253742,2.3608454758717937E-3,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W147*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W147>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W147*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W147>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W147*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W147>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W147*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W147>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W147*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W147>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W147*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W147>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":313.45997396690569},0.30059218188890713]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,149,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T148-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T148-100)*PI()/50))))","v":-197262.69615329156},{"$f":"IF($A$90=TRUE,U148*2*Main!$D$55*(T148-T147)/100000+V147,U148*2*Ltime5*(T148-T147)/100000+V147)","v":0.77643702867775666},-5.1898286549738781,3.8821851433887831E-4,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W148*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W148>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W148*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W148>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W148*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W148>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W148*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W148>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W148*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W148>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W148*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W148>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":154.04580081237054},4.9429516445459461E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,149.99999,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T149-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T149-100)*PI()/50))))","v":-1.9739254959223058},{"$f":"IF($A$90=TRUE,U149*2*Main!$D$55*(T149-T148)/100000+V148,U149*2*Ltime5*(T149-T148)/100000+V148)","v":0.77639755056262327},-5.1932449983144804E-5,3.8819877528131161E-4,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W149*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W149>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W149*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W149>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W149*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W149>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W149*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W149>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W149*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W149>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W149*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W149>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":5.9983984884476413},4.942700319059249E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,149.99999,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$55,Main!$G$55*SIN((T150-100)*PI()/50))),(IF($B$30=1,laccel5,laccel5*SIN((T150-100)*PI()/50))))","v":-1.9739254959223058},{"$f":"IF($A$90=TRUE,U150*2*Main!$D$55*(T150-T149)/100000+V149,U150*2*Ltime5*(T150-T149)/100000+V149)","v":0.77639755056262327},-5.1932449983144804E-5,3.8819877528131161E-4,{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W150*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W150>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W150*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W150>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W150*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W150>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W150*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W150>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W150*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W150>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W150*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W150>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad))),0)","v":5.9983984884476413},4.942700319059249E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150,0,{"$f":"IF($A$90=TRUE,Main!$E$57,Lspeed6)","v":0},0,0,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W151*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W151>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W151*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W151>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W151*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W151>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W151*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W151>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W151*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W151>=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W151*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W151>=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":9},0]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150.000001,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T152-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T152-150)*PI()/50))))","v":0.19739254911198548},{"$f":"IF($A$90=TRUE,U152*2*Main!$D$59*(T152-T151)/100000+V151,U152*2*Ltime7*(T152-T151)/100000+V151)","v":3.9478509722723438E-12},5.1932449856796039E-6,1.973925486136172E-15,{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W152*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W152<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W152*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W152<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W152*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W152<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W152*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W152<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W152*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W152<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W152*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W152<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad))),0)","v":6.0001601511548461},2.5132799873091542E-13]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,150.000001,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T153-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T153-150)*PI()/50))))","v":0.19739254911198548},{"$f":"IF($A$90=TRUE,U153*2*Main!$D$59*(T153-T152)/100000+V152,U153*2*Ltime7*(T153-T152)/100000+V152)","v":3.9478509722723438E-12},5.1932449856796039E-6,1.973925486136172E-15,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W153*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W153<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W153*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W153<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W153*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W153<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W153*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W153<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W153*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W153<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W153*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W153<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":6.0001601511548461},2.5132799873091542E-13]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,151,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T154-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T154-150)*PI()/50))))","v":197262.69615329089},{"$f":"IF($A$90=TRUE,U154*2*Main!$D$59*(T154-T153)/100000+V153,U154*2*Ltime7*(T154-T153)/100000+V153)","v":3.9452499778158527},5.1898286549738604,1.9726249889079265E-3,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W154*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W154<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W154*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W154<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W154*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W154<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W154*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W154<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W154*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W154<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W154*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W154<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":166.04580081237},0.25116241428103336]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,152,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T155-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T155-150)*PI()/50))))","v":393746.88656561828},{"$f":"IF($A$90=TRUE,U155*2*Main!$D$59*(T155-T154)/100000+V154,U155*2*Ltime7*(T155-T154)/100000+V154)","v":11.820187709128218},10.359175427253719,5.9100938545641087E-3,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W155*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W155<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W155*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W155<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W155*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W155<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W155*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W155<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W155*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W155<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W155*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W155<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":325.45997396690495},0.75249652087272889]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,154,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T156-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T156-150)*PI()/50))))","v":781284.14951710787},{"$f":"IF($A$90=TRUE,U156*2*Main!$D$59*(T156-T155)/100000+V155,U156*2*Ltime7*(T156-T155)/100000+V155)","v":43.071553689812532},20.554980469748205,2.1535776844906266E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W156*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W156<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W156*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W156<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W156*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W156<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W156*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W156<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W156*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W156<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W156*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W156<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":639.88187330821359},2.7420202705526511]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,156,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T157-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T157-150)*PI()/50))))","v":1156500.0947141841},{"$f":"IF($A$90=TRUE,U157*2*Main!$D$59*(T157-T156)/100000+V156,U157*2*Ltime7*(T157-T156)/100000+V156)","v":89.331557478379892},30.4266211912846,4.4665778739189949E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W157*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W157<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W157*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W157<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W157*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W157<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W157*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W157<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W157*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W157<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W157*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W157<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":944.30707684477466},5.6870235787127719]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,157,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T158-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T158-150)*PI()/50))))","v":1337628.2223808323},{"$f":"IF($A$90=TRUE,U158*2*Main!$D$59*(T158-T157)/100000+V157,U158*2*Ltime7*(T158-T157)/100000+V157)","v":116.08412192599654},35.191961853847843,5.8042060962998271E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W158*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W158<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W158*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W158<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W158*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W158<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W158*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W158<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W158*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W158<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W158*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W158<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1091.2623644249818},7.3901447276018475]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,158,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T159-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T159-150)*PI()/50))))","v":1513477.3425579488},{"$f":"IF($A$90=TRUE,U159*2*Main!$D$59*(T159-T158)/100000+V158,U159*2*Ltime7*(T159-T158)/100000+V158)","v":146.35366877715552},39.818415920651979,7.3176834388577763E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W159*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W159<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W159*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W159<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W159*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W159<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W159*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W159<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W159*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W159<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W159*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W159<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1233.9346172620158},9.3171639302073146]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,159,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T160-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T160-150)*PI()/50))))","v":1683353.459106016},{"$f":"IF($A$90=TRUE,U160*2*Main!$D$59*(T160-T159)/100000+V159,U160*2*Ltime7*(T160-T159)/100000+V159)","v":180.02073795927583},44.287724891121151,9.001036897963792E-2,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W160*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W160<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W160*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W160<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W160*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W160<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W160*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W160<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W160*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W160<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W160*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W160<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1371.7607731546809},11.460476122107819]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,160,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T161-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T161-150)*PI()/50))))","v":1846586.1486020335},{"$f":"IF($A$90=TRUE,U161*2*Main!$D$59*(T161-T160)/100000+V160,U161*2*Ltime7*(T161-T160)/100000+V160)","v":216.95246093131649},48.582250444581959,0.10847623046565824,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W161*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W161<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W161*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W161<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W161*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W161<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W161*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W161<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W161*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W161<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W161*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W161<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1504.1968952324498},13.811622629268129]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,161,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T162-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T162-150)*PI()/50))))","v":2002531.2061944834},{"$f":"IF($A$90=TRUE,U162*2*Main!$D$59*(T162-T161)/100000+V161,U162*2*Ltime7*(T162-T161)/100000+V161)","v":257.00308505520616},52.685044050657005,0.12850154252760307,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W162*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W162<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W162*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W162<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W162*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W162<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W162*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W162<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W162*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W162<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W162*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W162<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1630.7203186257909},16.361324550561147]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,162,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T163-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T163-150)*PI()/50))))","v":2150573.1879855683},{"$f":"IF($A$90=TRUE,U163*2*Main!$D$59*(T163-T162)/100000+V162,U163*2*Ltime7*(T163-T162)/100000+V162)","v":300.01454881491753},56.579913857371203,0.15000727440745876,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W163*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W163<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W163*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W163<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W163*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W163<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W163*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W163<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W163*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W163<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W163*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W163<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1750.8317131856243},19.099519377351541]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,163,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T164-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T164-150)*PI()/50))))","v":2290127.8399071065},{"$f":"IF($A$90=TRUE,U164*2*Main!$D$59*(T164-T163)/100000+V163,U164*2*Ltime7*(T164-T163)/100000+V163)","v":345.81710561305965},60.251488592994221,0.17290855280652984,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W164*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W164<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W164*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W164<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W164*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W164<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W164*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W164<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W164*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W164<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W164*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W164<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1864.0570541112991},22.015400705620188]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,164,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T165-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T165-150)*PI()/50))))","v":2420644.4035044196},{"$f":"IF($A$90=TRUE,U165*2*Main!$D$59*(T165-T164)/100000+V164,U165*2*Ltime7*(T165-T164)/100000+V164)","v":394.22999368314805},63.685278229427482,0.19711499684157402,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W165*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W165<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W165*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W165<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W165*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W165<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W165*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W165<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W165*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W165<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W165*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W165<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1969.949492709919},25.097460883903874]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,165,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T166-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T166-150)*PI()/50))))","v":2541607.7895283345},{"$f":"IF($A$90=TRUE,U166*2*Main!$D$59*(T166-T165)/100000+V165,U166*2*Ltime7*(T166-T165)/100000+V165)","v":445.06214947371473},66.867731167725239,0.22253107473685738,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W166*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W166<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W166*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W166<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W166*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W166<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W166*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W166<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W166*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W166<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W166*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W166<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2068.0911199039888},28.333536428738274]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"100+T67","v":166},{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T167-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T167-150)*PI()/50))))","v":2652540.6107571307},{"$f":"IF($A$90=TRUE,U167*2*Main!$D$59*(T167-T166)/100000+V166,U167*2*Ltime7*(T167-T166)/100000+V166)","v":498.11296168885735},69.786287720064507,0.24905648084442869,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W167*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W167<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W167*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W167<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W167*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W167<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W167*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W167<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W167*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W167<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W167*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W167<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2158.0946155276188},31.710856028370216]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,167,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T168-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T168-150)*PI()/50))))","v":2753005.0660258024},{"$f":"IF($A$90=TRUE,U168*2*Main!$D$59*(T168-T167)/100000+V167,U168*2*Ltime7*(T168-T167)/100000+V167)","v":553.17306300937344},72.429429677094859,0.27658653150468671,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W168*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W168<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W168*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W168<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W168*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W168<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W168*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W168<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W168*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W168<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W168*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W168<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2239.6047769022675},35.216090945290503]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,168,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T169-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T169-150)*PI()/50))))","v":2842604.6680272473},{"$f":"IF($A$90=TRUE,U169*2*Main!$D$59*(T169-T168)/100000+V168,U169*2*Ltime7*(T169-T168)/100000+V168)","v":610.02515636991836},74.786725765048558,0.30501257818495919,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W169*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W169<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W169*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W169<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W169*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W169<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W169*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W169<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W169*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W169<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W169*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W169<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2312.29992065944},38.835407618671567]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,169,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T170-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T170-150)*PI()/50))))","v":2920985.8080665306},{"$f":"IF($A$90=TRUE,U170*2*Main!$D$59*(T170-T169)/100000+V169,U170*2*Ltime7*(T170-T169)/100000+V169)","v":668.44487253124896},76.848872813212623,0.33422243626562448,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W170*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W170<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W170*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W170<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W170*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W170<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W170*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W170<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W170*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W170<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W170*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W170<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2375.893152277979},42.554522259112062]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,170,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T171-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T171-150)*PI()/50))))","v":2987839.1515928544},{"$f":"IF($A$90=TRUE,U171*2*Main!$D$59*(T171-T170)/100000+V170,U171*2*Ltime7*(T171-T170)/100000+V170)","v":728.2016555631061},78.60773246929331,0.36410082778155306,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W171*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W171<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W171*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W171<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W171*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W171<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W171*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W171<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W171*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W171<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W171*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W171<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2430.1334983256693},46.35875722022805]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,171,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T172-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T172-150)*PI()/50))))","v":3042900.8590017073},{"$f":"IF($A$90=TRUE,U172*2*Main!$D$59*(T172-T171)/100000+V171,U172*2*Ltime7*(T172-T171)/100000+V171)","v":789.05967274314025},80.056363317774611,0.39452983637157013,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W172*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W172<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W172*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W172<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W172*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W172<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W172*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W172<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W172*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W172<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W172*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W172<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2474.8068969367187},50.233098924617615]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,172,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T173-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T173-150)*PI()/50))))","v":3085953.6268892479},{"$f":"IF($A$90=TRUE,U173*2*Main!$D$59*(T173-T172)/100000+V172,U173*2*Ltime7*(T173-T172)/100000+V172)","v":850.77874528092525},81.18904827451405,0.42538937264046262,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W173*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W173<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W173*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W173<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W173*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W173<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W173*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W173<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W173*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W173<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W173*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W173<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2509.7370426161428},54.162257115591906]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,173,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T174-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T174-150)*PI()/50))))","v":3116827.5456495634},{"$f":"IF($A$90=TRUE,U174*2*Main!$D$59*(T174-T173)/100000+V173,U174*2*Ltime7*(T174-T173)/100000+V173)","v":913.11529619391649},82.00131714946194,0.45655764809695826,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W174*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W174<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W174*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W174<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W174*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W174<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W174*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W174<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W174*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W174<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W174*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W174<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2534.7860820370124},58.130725200832771]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,174,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T175-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T175-150)*PI()/50))))","v":3135400.7700302578},{"$f":"IF($A$90=TRUE,U175*2*Main!$D$59*(T175-T174)/100000+V174,U175*2*Ltime7*(T175-T174)/100000+V174)","v":975.82331159452167},82.489964288459177,0.48791165579726081,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W175*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W175<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W175*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W175<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W175*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W175<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W175*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W175<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W175*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W175<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W175*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W175<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2549.8551580845492},62.122841449828378]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,175,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T176-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T176-150)*PI()/50))))","v":3141600},{"$f":"IF($A$90=TRUE,U176*2*Main!$D$59*(T176-T175)/100000+V175,U176*2*Ltime7*(T176-T175)/100000+V175)","v":1038.6553115945217},82.65306122448979,0.51932765579726081,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W176*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W176<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W176*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W176<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W176*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W176<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W176*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W176<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W176*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W176<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W176*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W176<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2554.8847999999998},66.122850803568355]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,176,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T177-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T177-150)*PI()/50))))","v":3135400.7700302578},{"$f":"IF($A$90=TRUE,U177*2*Main!$D$59*(T177-T176)/100000+V176,U177*2*Ltime7*(T177-T176)/100000+V176)","v":1101.3633269951267},82.489964288459177,0.55068166349756331,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W177*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W177<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W177*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W177<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W177*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W177<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W177*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W177<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W177*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W177<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W177*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W177<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2549.8551580845492},70.114967052563955]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,177,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T178-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T178-150)*PI()/50))))","v":3116827.5456495639},{"$f":"IF($A$90=TRUE,U178*2*Main!$D$59*(T178-T177)/100000+V177,U178*2*Ltime7*(T178-T177)/100000+V177)","v":1163.699877908118},82.001317149461954,0.58184993895405901,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W178*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W178<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W178*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W178<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W178*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W178<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W178*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W178<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W178*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W178<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W178*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W178<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2534.7860820370129},74.083435137804827]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,178,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T179-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T179-150)*PI()/50))))","v":3085953.6268892484},{"$f":"IF($A$90=TRUE,U179*2*Main!$D$59*(T179-T178)/100000+V178,U179*2*Ltime7*(T179-T178)/100000+V178)","v":1225.418950445903},81.189048274514064,0.61270947522295149,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W179*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W179<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W179*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W179<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W179*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W179<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W179*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W179<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W179*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W179<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W179*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W179<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2509.7370426161433},78.012593328779118]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,179,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T180-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T180-150)*PI()/50))))","v":3042900.8590017073},{"$f":"IF($A$90=TRUE,U180*2*Main!$D$59*(T180-T179)/100000+V179,U180*2*Ltime7*(T180-T179)/100000+V179)","v":1286.276967625937},80.056363317774611,0.64313848381296845,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W180*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W180<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W180*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W180<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W180*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W180<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W180*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W180<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W180*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W180<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W180*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W180<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2474.8068969367187},81.886935033168669]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,180,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T181-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T181-150)*PI()/50))))","v":2987839.1515928549},{"$f":"IF($A$90=TRUE,U181*2*Main!$D$59*(T181-T180)/100000+V180,U181*2*Ltime7*(T181-T180)/100000+V180)","v":1346.0337506577941},78.60773246929331,0.67301687532889709,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W181*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W181<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W181*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W181<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W181*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W181<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W181*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W181<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W181*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W181<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W181*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W181<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2430.1334983256693},85.691169994284664]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,181,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T182-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T182-150)*PI()/50))))","v":2920985.8080665306},{"$f":"IF($A$90=TRUE,U182*2*Main!$D$59*(T182-T181)/100000+V181,U182*2*Ltime7*(T182-T181)/100000+V181)","v":1404.4534668191247},76.848872813212623,0.70222673340956232,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W182*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W182<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W182*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W182<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W182*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W182<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W182*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W182<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W182*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W182<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W182*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W182<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2375.893152277979},89.410284634725159]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,182,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T183-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T183-150)*PI()/50))))","v":2842604.6680272468},{"$f":"IF($A$90=TRUE,U183*2*Main!$D$59*(T183-T182)/100000+V182,U183*2*Ltime7*(T183-T182)/100000+V182)","v":1461.3055601796698},74.786725765048544,0.73065278008983492,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W183*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W183<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W183*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W183<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W183*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W183<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W183*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W183<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W183*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W183<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W183*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W183<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2312.2999206594395},93.029601308106237]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,183,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T184-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T184-150)*PI()/50))))","v":2753005.0660258015},{"$f":"IF($A$90=TRUE,U184*2*Main!$D$59*(T184-T183)/100000+V183,U184*2*Ltime7*(T184-T183)/100000+V183)","v":1516.3656615001858},72.429429677094831,0.75818283075009285,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W184*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W184<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W184*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W184<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W184*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W184<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W184*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W184<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W184*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W184<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W184*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W184<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2239.6047769022666},96.53483622502651]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,184,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T185-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T185-150)*PI()/50))))","v":2652540.6107571302},{"$f":"IF($A$90=TRUE,U185*2*Main!$D$59*(T185-T184)/100000+V184,U185*2*Ltime7*(T185-T184)/100000+V184)","v":1569.4164737153283},69.786287720064507,0.78470823685766411,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W185*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W185<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W185*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W185<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W185*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W185<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W185*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W185<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W185*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W185<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W185*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W185<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2158.0946155276188},99.912155824658441]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,185,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T186-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T186-150)*PI()/50))))","v":2541607.789528335},{"$f":"IF($A$90=TRUE,U186*2*Main!$D$59*(T186-T185)/100000+V185,U186*2*Ltime7*(T186-T185)/100000+V185)","v":1620.248629505895},66.867731167725253,0.81012431475294755,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W186*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W186<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W186*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W186<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W186*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W186<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W186*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W186<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W186*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W186<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W186*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W186<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":2068.0911199039892},103.14823136949286]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,186,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T187-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T187-150)*PI()/50))))","v":2420644.4035044196},{"$f":"IF($A$90=TRUE,U187*2*Main!$D$59*(T187-T186)/100000+V186,U187*2*Ltime7*(T187-T186)/100000+V186)","v":1668.6615175759835},63.685278229427482,0.83433075878799168,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W187*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W187<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W187*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W187<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W187*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W187<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W187*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W187<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W187*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W187<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W187*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W187<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1969.949492709919},106.23029154777653]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,187,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T188-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T188-150)*PI()/50))))","v":2290127.839907106},{"$f":"IF($A$90=TRUE,U188*2*Main!$D$59*(T188-T187)/100000+V187,U188*2*Ltime7*(T188-T187)/100000+V187)","v":1714.4640743741256},60.251488592994207,0.85723203718706287,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W188*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W188<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W188*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W188<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W188*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W188<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W188*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W188<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W188*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W188<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W188*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W188<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1864.0570541112986},109.1461728760452]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,188,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T189-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T189-150)*PI()/50))))","v":2150573.1879855688},{"$f":"IF($A$90=TRUE,U189*2*Main!$D$59*(T189-T188)/100000+V188,U189*2*Ltime7*(T189-T188)/100000+V188)","v":1757.4755381338371},56.579913857371217,0.87873776906691858,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W189*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W189<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W189*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W189<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W189*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W189<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W189*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W189<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W189*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W189<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W189*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W189<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1750.8317131856247},111.88436770283559]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,189,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T190-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T190-150)*PI()/50))))","v":2002531.2061944841},{"$f":"IF($A$90=TRUE,U190*2*Main!$D$59*(T190-T189)/100000+V189,U190*2*Ltime7*(T190-T189)/100000+V189)","v":1797.5261622577268},52.685044050657019,0.89876308112886338,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W190*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W190<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W190*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W190<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W190*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W190<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W190*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W190<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W190*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W190<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W190*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W190<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1630.7203186257914},114.43406962412861]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,190,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T191-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T191-150)*PI()/50))))","v":1846586.148602034},{"$f":"IF($A$90=TRUE,U191*2*Main!$D$59*(T191-T190)/100000+V190,U191*2*Ltime7*(T191-T190)/100000+V190)","v":1834.4578852297675},48.582250444581973,0.91722894261488375,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W191*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W191<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W191*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W191<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W191*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W191<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W191*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W191<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W191*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W191<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W191*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W191<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1504.1968952324503},116.78521613128892]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,191,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T192-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T192-150)*PI()/50))))","v":1683353.4591060169},{"$f":"IF($A$90=TRUE,U192*2*Main!$D$59*(T192-T191)/100000+V191,U192*2*Ltime7*(T192-T191)/100000+V191)","v":1868.1249544118878},44.287724891121179,0.93406247720594393,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W192*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W192<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W192*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W192<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W192*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W192<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W192*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W192<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W192*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W192<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W192*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W192<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1371.7607731546818},118.92852832318943]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,192,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T193-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T193-150)*PI()/50))))","v":1513477.3425579485},{"$f":"IF($A$90=TRUE,U193*2*Main!$D$59*(T193-T192)/100000+V192,U193*2*Ltime7*(T193-T192)/100000+V192)","v":1898.3945012630468},39.818415920651972,0.94919725063152338,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W193*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W193<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W193*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W193<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W193*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W193<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W193*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W193<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W193*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W193<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W193*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W193<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1233.9346172620155},120.85554752579489]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,193,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T194-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T194-150)*PI()/50))))","v":1337628.222380833},{"$f":"IF($A$90=TRUE,U194*2*Main!$D$59*(T194-T193)/100000+V193,U194*2*Ltime7*(T194-T193)/100000+V193)","v":1925.1470657106634},{"$f":"IF(move1,IF(ABS(MIN($U$1:$U$101))>MAX($U$1:$U$101),U194/MIN($U$1:$U$101)*-1,U194/MAX($U$1:$U$101)),IF(ABS(MIN($U$1:$U$201))>MAX($U$1:$U$201),U194/MIN($U$1:$U$201)*-1,U194/MAX($U$1:$U$201)))","v":35.191961853847864},{"$f":"IF(move1,IF(ABS(MIN($V$1:$V$101))>MAX($V$1:$V$101),V194/MIN($V$1:$V$101)*-1,V194/MAX($V$1:$V$101)),IF(ABS(MIN($V$1:$V$201))>MAX($V$1:$V$201),V194/MIN($V$1:$V$201)*-1,V194/MAX($V$1:$V$201)))","v":0.96257353285533165},{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W194*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W194<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W194*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W194<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W194*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W194<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W194*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W194<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W194*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W194<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W194*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W194<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":1091.2623644249825},122.55866867468396]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,194,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T195-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T195-150)*PI()/50))))","v":1156500.0947141848},{"$f":"IF($A$90=TRUE,U195*2*Main!$D$59*(T195-T194)/100000+V194,U195*2*Ltime7*(T195-T194)/100000+V194)","v":1948.277067604947},30.426621191284621,0.97413853380247351,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W195*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W195<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W195*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W195<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W195*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W195<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W195*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W195<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W195*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W195<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W195*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W195<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":944.30707684477534},{"$f":"IF(move1,ABS(IF($A$90=TRUE,X195*speed,X195*MAX(ABS(Lspeed1),ABS(Lspeed2)))),ABS(IF($A$90=TRUE,X195*speed,X195*MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6)))))","v":124.03117032876402}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,196,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T196-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T196-150)*PI()/50))))","v":781284.14951710927},{"$f":"IF($A$90=TRUE,U196*2*Main!$D$59*(T196-T195)/100000+V195,U196*2*Ltime7*(T196-T195)/100000+V195)","v":1979.5284335856313},20.554980469748241,0.98976421679281568,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W196*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W196<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W196*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W196<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W196*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W196<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W196*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W196<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W196*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W196<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W196*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W196<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":639.88187330821472},126.02069407844395]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,198,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T197-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T197-150)*PI()/50))))","v":393746.88656561915},{"$f":"IF($A$90=TRUE,U197*2*Main!$D$59*(T197-T196)/100000+V196,U197*2*Ltime7*(T197-T196)/100000+V196)","v":1995.278309048256},10.359175427253742,0.99763915452412799,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W197*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W197<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W197*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W197<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W197*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W197<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W197*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W197<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W197*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W197<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W197*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W197<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":325.45997396690569},127.02336229162734]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,199,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T198-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T198-150)*PI()/50))))","v":197262.69615329156},{"$f":"IF($A$90=TRUE,U198*2*Main!$D$59*(T198-T197)/100000+V197,U198*2*Ltime7*(T198-T197)/100000+V197)","v":1999.2235629713218},5.1898286549738781,0.99961178148566088,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W198*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W198<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W198*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W198<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W198*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W198<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W198*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W198<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W198*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W198<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W198*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W198<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":166.04580081237054},127.27452495707078]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,199.999999,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T199-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T199-150)*PI()/50))))","v":0.1973925499386468},{"$f":"IF($A$90=TRUE,U199*2*Main!$D$59*(T199-T198)/100000+V198,U199*2*Ltime7*(T199-T198)/100000+V198)","v":1999.2235669191689},5.1932450074284225E-6,0.99961178345958446,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W199*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W199<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W199*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W199<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W199*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W199<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W199*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W199<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W199*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W199<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W199*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W199<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":6.0001601511555167},127.27452520839853]
["Steuerung Rotatorisch Others",null,{"$f":"IF((SUM(Motor!O3:O12))>0,1,0)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,199.999999,{"$f":"IF($A$90=TRUE,(IF($B$30=1,Main!$G$59,Main!$G$59*SIN((T200-150)*PI()/50))),(IF($B$30=1,laccel7,laccel7*SIN((T200-150)*PI()/50))))","v":0.1973925499386468},{"$f":"IF($A$90=TRUE,U200*2*Main!$D$59*(T200-T199)/100000+V199,U200*2*Ltime7*(T200-T199)/100000+V199)","v":1999.2235669191689},5.1932450074284225E-6,0.99961178345958446,{"$f":"MAX(IF(move1,(IF($A$90=TRUE,IF($A$71=TRUE,(W200*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W200<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W200*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W200<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W200*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W200<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),(IF($A$90=TRUE,IF($A$71=TRUE,(W200*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W200<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W200*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W200<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W200*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W200<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad))),0)","v":6.0001601511555167},127.27452520839853]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,200,0,{"$f":"IF($A$90=TRUE,Main!$E$46,Lspeed1)","v":2000},0,1,{"$f":"IF(move1,ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W201*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W201<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W201*MAX(ABS(accel1),ABS(accel3))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W201<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W201*MAX(ABS(laccel1),ABS(laccel3))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W201<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)),ABS(IF($A$90=TRUE,IF($A$71=TRUE,(W201*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/10/gear^2+Calc!$A$107+gear_inertia/10)/1000+(torque2+IF(W201<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad,(W201*MAX(ABS(accel1),ABS(accel3),ABS(accel5),ABS(accel7))*gear*(inertia2/gear^2+Calc!$A$107+gear_inertia)/1000+(torque2+IF(W201<=0,DryTorq2,-DryTorq2))/gear)/Wirkungsgrad),(W201*MAX(ABS(laccel1),ABS(laccel3),ABS(laccel5),ABS(laccel7))*(Gewicht2+Calc!$A$107)+(Ltorque2+IF(W201<=0,LDryTorq2,-LDryTorq2)))/LWirkungsgrad)))","v":9},{"$f":"IF(move1,ABS(IF($A$90=TRUE,X201*speed,X201*MAX(ABS(Lspeed1),ABS(Lspeed2)))),ABS(IF($A$90=TRUE,X201*speed,X201*MAX(ABS(Lspeed1),ABS(Lspeed2),ABS(Lspeed6)))))","v":127.32395447351627}]

{"sheet":"Graphic","index":9,"n_rows":46,"n_cols":14,"rows_kept":46,"cut":false,"hidden":false,"merged":[[44,13,44,16],[43,8,43,10],[42,8,42,10],[0,0,0,18],[1,1,5,11],[1,12,5,17],[41,8,41,10],[42,13,42,16],[43,13,43,16]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Mo [Nm]",{"$f":"IF(I46=\"Linear\",Main!R71,Main!R43)","v":42},null,"Mmax[Nm]",{"$f":"IF(I46=\"Linear\",Main!R76,Main!R48)","v":112},null,"Motor",{"$f":"IFERROR(Calc!A70,\"no data\")","v":"AKM73M"}]
[null,"Io [A]",{"$f":"IF(I46=\"Linear\",Main!R72,Main!R44)","v":13.6},null,"nmax[min-1]",{"$f":"IF(I46=\"Linear\",Main!R77,Main!R49)","v":6000},null,"Drive",{"$f":"IFERROR(Drives!A2,\"no data\")","v":"S724"},null,null,null,null,"AnyDim Application Support"]
[null,"Mn [Nm]",{"$f":"IF(I46=\"Linear\",Main!R73,Main!R45)","v":33.799999999999997},null,"Ru-v [Ohm]",{"$f":"IF(I46=\"Linear\",Main!R78,Main!R50)","v":0.68},null,"Voltage",{"$f":"IFERROR(CONCATENATE(Calc!B2,\" V\"),\"no data\")","v":"400 V"},null,null,null,null,"Email: technik@kollmorgen.com"]
[null,"In [A]",{"$f":"IF(I46=\"Linear\",Main!R74,Main!R46)","v":10.903225806451612},null,"Lu-v [mH]",{"$f":"IF(I46=\"Linear\",Main!R79,Main!R51)","v":12.4},null,null,null,null,null,null,null,"Tel.: +49 (0)2102 93940"]
[null,"nn [min-1]",{"$f":"IF(I46=\"Linear\",Main!R75,Main!R47)","v":1500},null,"Ke [V/10^3]",{"$f":"IF(I46=\"Linear\",Main!R80,Main!R52)","v":200},null,"Motortype","Rotative"]