### FOLDT

sets the time constant for drive foldback. After the drive enters foldback state (FOLD=1), this variable defines how long it will take the drive to reduce the current level to ICONT. See also FOLD, FOLDD, FOLDR, FOLDMODE, FOLDTIME, MFOLD, MFOLDD, MFOLDDIS, and MFOLDR.

Firmware Versions: all
Type: variable (R/W) Range: 1 to 32767
Units: milli-seconds Default: drive data
Opmodes: all Drive Status: en/dis EEPROM: yes