### TRUN

provides a relative incremental run time counter. Error log stamps include the value of this counter at the time of the error. The clock is a very coarse counter and is incremented every 15 minutes. It is intended for use by factory Quality Assurance Program personnel. This clock has a resolution of 15 minutes.

Firmware Versions: all
Type: variable (R) and (RW) for 'TRUN = 0'
Range: 0000:00 to 9999:45
Units: hours: minutes Default: n/a
Opmodes: all Drive Status: en/dis EEPROM: yes